MAU-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       Counter32, Integer32,
       OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE,
       OBJECT-IDENTITY, mib-2
           FROM SNMPv2-SMI
       TruthValue, TEXTUAL-CONVENTION





           FROM SNMPv2-TC
       OBJECT-GROUP, MODULE-COMPLIANCE, NOTIFICATION-GROUP
           FROM SNMPv2-CONF;

   mauMod MODULE-IDENTITY
       LAST-UPDATED "9710310000Z"
       ORGANIZATION "IETF HUB MIB Working Group"
       CONTACT-INFO
           "WG E-mail: hubmib@hprnd.rose.hp.com

                Chair: Dan Romascanu
               Postal: Madge Networks (Israel) Ltd.
                       Atidim Technology Park, Bldg. 3
                       Tel Aviv 61131, Israel
                  Tel: 972-3-6458414, 6458458
                  Fax: 972-3-6487146
               E-mail: dromasca@madge.com

               Editor: Kathryn de Graaf
               Postal: 3Com Corporation
                       118 Turnpike Rd.
                       Southborough, MA  01772
                       USA
                  Tel: (508)229-1627
                  Fax: (508)490-5882
               E-mail: kdegraaf@isd.3com.com"
       DESCRIPTION
               "Management information for 802.3 MAUs.

               The following references are used throughout this
               MIB module:

               [IEEE 802.3 Std]
                  refers to IEEE 802.3/ISO 8802-3 Information
                  processing systems - Local area networks -
                  Part 3: Carrier sense multiple access with
                  collision detection (CSMA/CD) access method
                  and physical layer specifications (1993),
                  and to IEEE Std 802.3u-1995, Supplement to
                  IEEE Std 802.3, clauses 22 through 29.

               [IEEE 802.3 Mgt]
                  refers to IEEE 802.3u-1995, - 10 Mb/s &
                  100 Mb/s Management, Section 30 -
                  Supplement to IEEE Std 802.3."
       ::= { snmpDot3MauMgt 6 }







   snmpDot3MauMgt OBJECT IDENTIFIER ::= { mib-2 26 }


   -- textual conventions

   JackType ::= TEXTUAL-CONVENTION
       STATUS     current
       DESCRIPTION
               "Common enumeration values for repeater and
               interface MAU jack types."
       SYNTAX     INTEGER {
                      other(1),
                      rj45(2),
                      rj45S(3), -- rj45 shielded
                      db9(4),
                      bnc(5),
                      fAUI(6),  -- female aui
                      mAUI(7),  -- male aui
                      fiberSC(8),
                      fiberMIC(9),
                      fiberST(10),
                      telco(11)
                  }


   dot3RpMauBasicGroup         OBJECT IDENTIFIER ::= { snmpDot3MauMgt 1 }
   dot3IfMauBasicGroup         OBJECT IDENTIFIER ::= { snmpDot3MauMgt 2 }
   dot3BroadMauBasicGroup      OBJECT IDENTIFIER ::= { snmpDot3MauMgt 3 }

   dot3IfMauAutoNegGroup       OBJECT IDENTIFIER ::= { snmpDot3MauMgt 5 }

   -- object identities for MAU types
   --  (see rpMauType and ifMauType for usage)

   dot3MauType
       OBJECT IDENTIFIER ::= { snmpDot3MauMgt 4 }

   dot3MauTypeAUI OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "no internal MAU, view from AUI"
       ::= { dot3MauType 1 }

   dot3MauType10Base5 OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "thick coax MAU (per 802.3 section 8)"
       ::= { dot3MauType 2 }





   dot3MauTypeFoirl OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "FOIRL MAU (per 802.3 section 9.9)"
       ::= { dot3MauType 3 }

   dot3MauType10Base2 OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "thin coax MAU (per 802.3 section 10)"
       ::= { dot3MauType 4 }

   dot3MauType10BaseT OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "UTP MAU (per 802.3 section 14)"
       ::= { dot3MauType 5 }

   dot3MauType10BaseFP OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "passive fiber MAU (per 802.3 section 16)"
       ::= { dot3MauType 6 }

   dot3MauType10BaseFB OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "sync fiber MAU (per 802.3 section 17)"
       ::= { dot3MauType 7 }

   dot3MauType10BaseFL OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "async fiber MAU (per 802.3 section 18)"
       ::= { dot3MauType 8 }

   dot3MauType10Broad36 OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "broadband DTE MAU (per 802.3 section 11). Note
               that 10BROAD36 MAUs can be attached to interfaces
               but not to repeaters."
       ::= { dot3MauType 9 }

   ------ new since RFC 1515:

   dot3MauType10BaseTHD OBJECT-IDENTITY
       STATUS     current





       DESCRIPTION
               "UTP MAU (per 802.3 section 14), half duplex mode"
       ::= { dot3MauType 10 }

   dot3MauType10BaseTFD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "UTP MAU (per 802.3 section 14), full duplex mode"
       ::= { dot3MauType 11 }

   dot3MauType10BaseFLHD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "async fiber MAU (per 802.3 section 18), half
               duplex mode"
       ::= { dot3MauType 12 }

   dot3MauType10BaseFLFD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "async fiber MAU (per 802.3 section 18), full
               duplex mode"
       ::= { dot3MauType 13 }

   dot3MauType100BaseT4 OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "4 pair categ. 3 UTP (per 802.3 section 23)"
       ::= { dot3MauType 14 }

   dot3MauType100BaseTXHD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "2 pair categ. 5 UTP (per 802.3 section 25), half
               duplex mode"
       ::= { dot3MauType 15 }

   dot3MauType100BaseTXFD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "2 pair categ. 5 UTP (per 802.3 section 25), full
               duplex mode"
       ::= { dot3MauType 16 }

   dot3MauType100BaseFXHD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "X fiber over PMT (per 802.3 section 26), half





               duplex mode"
       ::= { dot3MauType 17 }

   dot3MauType100BaseFXFD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "X fiber over PMT (per 802.3 section 26), full
               duplex mode"
       ::= { dot3MauType 18 }

   dot3MauType100BaseT2HD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "2 pair categ. 3 UTP (per 802.3 section 32), half
               duplex mode"
       ::= { dot3MauType 19 }

   dot3MauType100BaseT2FD OBJECT-IDENTITY
       STATUS     current
       DESCRIPTION
               "2 pair categ. 3 UTP (per 802.3 section 32), full
               duplex mode"
       ::= { dot3MauType 20 }


   --
   -- The Basic Repeater MAU Table
   --

   rpMauTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF RpMauEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "Table of descriptive and status information about
               the MAU(s) attached to the ports of a repeater."
       ::= { dot3RpMauBasicGroup 1 }

   rpMauEntry OBJECT-TYPE
       SYNTAX     RpMauEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "An entry in the table, containing information
               about a single MAU."
       INDEX      { rpMauGroupIndex, rpMauPortIndex, rpMauIndex }
       ::= { rpMauTable 1 }






   RpMauEntry ::=
       SEQUENCE {
           rpMauGroupIndex
               Integer32,
           rpMauPortIndex
               Integer32,
           rpMauIndex
               Integer32,
           rpMauType
               OBJECT IDENTIFIER,
           rpMauStatus
               INTEGER,
           rpMauMediaAvailable
               INTEGER,
           rpMauMediaAvailableStateExits
               Counter32,
           rpMauJabberState
               INTEGER,
           rpMauJabberingStateEnters
               Counter32,
           rpMauFalseCarriers
               Counter32
       }

   rpMauGroupIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This variable uniquely identifies the group
               containing the port to which the MAU described by
               this entry is connected.

               Note:  In practice, a group will generally be a
               field-replaceable unit (i.e., module, card, or
               board) that can fit in the physical system
               enclosure, and the group number will correspond to
               a number marked on the physical enclosure.

               The group denoted by a particular value of this
               object is the same as the group denoted by the
               same value of rptrGroupIndex."
       ::= { rpMauEntry 1 }

   rpMauPortIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS read-only
       STATUS     current





       DESCRIPTION
               "This variable uniquely identifies the repeater
               port within group rpMauGroupIndex to which the MAU
               described by this entry is connected."
       REFERENCE
               "Reference RFC 1516, rptrPortIndex."
       ::= { rpMauEntry 2 }

   rpMauIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This variable uniquely identifies the MAU
               described by this entry from among other MAUs
               connected to the same port (rpMauPortIndex)."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.1, aMAUID."
       ::= { rpMauEntry 3 }

   rpMauType OBJECT-TYPE
       SYNTAX     OBJECT IDENTIFIER
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This object identifies the 10 or 100 Mb/s
               baseband MAU type.  An initial set of MAU types
               are defined above.  The assignment of OBJECT
               IDENTIFIERs to new types of MAUs is managed by the
               IANA.  If the MAU type is unknown, the object
               identifier

               unknownMauType OBJECT IDENTIFIER ::= { 0 0 }

               is returned.  Note that unknownMauType is a
               syntactically valid object identifier, and any
               conformant implementation of ASN.1 and the BER
               must be able to generate and recognize this
               value."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.2, aMAUType."
       ::= { rpMauEntry 4 }

   rpMauStatus OBJECT-TYPE
       SYNTAX     INTEGER {
                      other(1),
                      unknown(2),
                      operational(3),





                      standby(4),
                      shutdown(5),
                      reset(6)
                  }
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "The current state of the MAU.  This object may be
               implemented as a read-only object by those agents
               and MAUs that do not implement software control of
               the MAU state.  Some agents may not support
               setting the value of this object to some of the
               enumerated values.

               The value other(1) is returned if the MAU is in a
               state other than one of the states 2 through 6.

               The value unknown(2) is returned when the MAU's
               true state is unknown; for example, when it is
               being initialized.

               A MAU in the operational(3) state is fully
               functional, operates, and passes signals to its
               attached DTE or repeater port in accordance to its
               specification.

               A MAU in standby(4) state forces DI and CI to idle
               and the media transmitter to idle or fault, if
               supported.  Standby(4) mode only applies to link
               type MAUs.  The state of rpMauMediaAvailable is
               unaffected.

               A MAU in shutdown(5) state assumes the same
               condition on DI, CI, and the media transmitter as
               though it were powered down or not connected.  The
               MAU may return other(1) value for the
               rpMauJabberState and rpMauMediaAvailable objects
               when it is in this state.  For an AUI, this state
               will remove power from the AUI.

               Setting this variable to the value reset(6) resets
               the MAU in the same manner as a power-off, power-
               on cycle of at least one-half second would.  The
               agent is not required to return the value reset
               (6).

               Setting this variable to the value operational(3),
               standby(4), or shutdown(5) causes the MAU to





               assume the respective state except that setting a
               mixing-type MAU or an AUI to standby(4) will cause
               the MAU to enter the shutdown state."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.7, aMAUAdminState,
               30.5.1.2.2, acMAUAdminControl, and 30.5.1.2.1,
               acRESETMAU."
       ::= { rpMauEntry 5 }

   rpMauMediaAvailable OBJECT-TYPE
       SYNTAX     INTEGER {
                      other(1),
                      unknown(2),
                      available(3),
                      notAvailable(4),
                      remoteFault(5),
                      invalidSignal(6),
                      remoteJabber(7),
                      remoteLinkLoss(8),
                      remoteTest(9)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "If the MAU is a link or fiber type (FOIRL,
               10BASE-T, 10BASE-F) then this is equivalent to the
               link test fail state/low light function.  For an
               AUI or a coax (including broadband) MAU this
               indicates whether or not loopback is detected on
               the DI circuit.  The value of this attribute
               persists between packets for MAU types AUI,
               10BASE5, 10BASE2, 10BROAD36, and 10BASE-FP.

               The value other(1) is returned if the
               mediaAvailable state is not one of 2 through 6.

               The value unknown(2) is returned when the MAU's
               true state is unknown; for example, when it is
               being initialized.  At power-up or following a
               reset, the value of this attribute will be unknown
               for AUI, coax, and 10BASE-FP MAUs.  For these MAUs
               loopback will be tested on each transmission
               during which no collision is detected.  If DI is
               receiving input when DO returns to IDL after a
               transmission and there has been no collision
               during the transmission then loopback will be
               detected.  The value of this attribute will only
               change during non-collided transmissions for AUI,





               coax, and 10BASE-FP MAUs.

               For 100BASE-T4, 100BASE-TX and 100BASE-FX the
               enumerations match the states within the
               respective link integrity state diagrams, fig 23-
               12 and 24-15 of sections 23 and 24 of [2].  Any
               MAU which implements management of auto-
               negotiation will map remote fault indication to
               remote fault.

               The value available(3) indicates that the link,
               light, or loopback is normal.  The value
               notAvailable(4) indicates link loss, low light, or
               no loopback.

               The value remoteFault(5) indicates that a fault
               has been detected at the remote end of the link.
               This value applies to 10BASE-FB, 100BASE-T4 Far
               End Fault Indication and non-specified remote
               faults from a system running auto-negotiation.
               The values remoteJabber(7), remoteLinkLoss(8), and
               remoteTest(9) should be used instead of
               remoteFault(5) where the reason for remote fault
               is identified in the remote signaling protocol.

               The value invalidSignal(6) indicates that an
               invalid signal has been received from the other
               end of the link.  InvalidSignal(6) applies only to
               MAUs of type 10BASE-FB.

               Where an IEEE Std 802.3u-1995 clause 22 MII is
               present, a logic one in the remote fault bit
               (reference section 22.2.4.2.8 of that document)
               maps to the value remoteFault(5), and a logic zero
               in the link status bit (reference section
               22.2.4.2.10 of that document) maps to the value
               notAvailable(4).  The value notAvailable(4) takes
               precedence over the value remoteFault(5)."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.4, aMediaAvailable."
       ::= { rpMauEntry 6 }

   rpMauMediaAvailableStateExits OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A count of the number of times that





               rpMauMediaAvailable for this MAU instance leaves
               the state available(3)."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.5, aLoseMediaCounter."
       ::= { rpMauEntry 7 }

   rpMauJabberState OBJECT-TYPE
       SYNTAX     INTEGER {
                      other(1),
                      unknown(2),
                      noJabber(3),
                      jabbering(4)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "The value other(1) is returned if the jabber
               state is not 2, 3, or 4.  The agent must always
               return other(1) for MAU type dot3MauTypeAUI.

               The value unknown(2) is returned when the MAU's
               true state is unknown; for example, when it is
               being initialized.

               If the MAU is not jabbering the agent returns
               noJabber(3).  This is the 'normal' state.

               If the MAU is in jabber state the agent returns
               the jabbering(4) value."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.6,
               aJabber.jabberFlag."
       ::= { rpMauEntry 8 }

   rpMauJabberingStateEnters OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A count of the number of times that
               mauJabberState for this MAU instance enters the
               state jabbering(4).  For MAUs of type
               dot3MauTypeAUI, dot3MauType100BaseT4,
               dot3MauType100BaseTX, and dot3MauType100BaseFX,
               this counter will always indicate zero."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.6,
               aJabber.jabberCounter."





       ::= { rpMauEntry 9 }

   rpMauFalseCarriers OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A count of the number of false carrier events
               during IDLE in 100BASE-X links.  This counter does
               not increment at the symbol rate.  It can
               increment after a valid carrier completion at a
               maximum rate of once per 100 ms until the next
               carrier event.

               This counter increments only for MAUs of type
               dot3MauType100BaseT4, dot3MauType100BaseTX, and
               dot3MauType100BaseFX.  For all other MAU types,
               this counter will always indicate zero.

               The approximate minimum time for rollover of this
               counter is 7.4 hours."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.10, aFalseCarriers."
       ::= { rpMauEntry 10 }


   -- The rpJackTable applies to MAUs attached to repeaters
   -- which have one or more external jacks (connectors).

   rpJackTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF RpJackEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "Information about the external jacks attached to
               MAUs attached to the ports of a repeater."
       ::= { dot3RpMauBasicGroup 2 }

   rpJackEntry OBJECT-TYPE
       SYNTAX     RpJackEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "An entry in the table, containing information
               about a particular jack."

       INDEX    { rpMauGroupIndex,
                  rpMauPortIndex,





                  rpMauIndex,
                  rpJackIndex }
       ::= { rpJackTable 1 }

   RpJackEntry ::=
       SEQUENCE {
           rpJackIndex
               Integer32,
           rpJackType
               JackType
       }

   rpJackIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "This variable uniquely identifies the jack
               described by this entry from among other jacks
               attached to the same MAU (rpMauIndex)."
       ::= { rpJackEntry 1 }

   rpJackType OBJECT-TYPE
       SYNTAX     JackType
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "The jack connector type, as it appears on the
               outside of the system."
       ::= { rpJackEntry 2 }


   --
   -- The Basic Interface MAU Table
   --

   ifMauTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF IfMauEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "Table of descriptive and status information about
               MAU(s) attached to an interface."

       ::= { dot3IfMauBasicGroup 1 }

   ifMauEntry OBJECT-TYPE
       SYNTAX     IfMauEntry





       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "An entry in the table, containing information
               about a single MAU."
       INDEX      { ifMauIfIndex, ifMauIndex }
       ::= { ifMauTable 1 }

   IfMauEntry ::=
       SEQUENCE {
           ifMauIfIndex
               Integer32,
           ifMauIndex
               Integer32,
           ifMauType
               OBJECT IDENTIFIER,
           ifMauStatus
               INTEGER,
           ifMauMediaAvailable
               INTEGER,
           ifMauMediaAvailableStateExits
               Counter32,
           ifMauJabberState
               INTEGER,
           ifMauJabberingStateEnters
               Counter32,
           ifMauFalseCarriers
               Counter32,
           ifMauTypeList
               Integer32,
           ifMauDefaultType
               OBJECT IDENTIFIER,
           ifMauAutoNegSupported
               TruthValue
       }

   ifMauIfIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This variable uniquely identifies the interface
               to which the MAU described by this entry is
               connected."
       REFERENCE
               "RFC 1213, ifIndex"
       ::= { ifMauEntry 1 }






   ifMauIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This variable uniquely identifies the MAU
               described by this entry from among other MAUs
               connected to the same interface (ifMauIfIndex)."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.1, aMAUID."
       ::= { ifMauEntry 2 }

   ifMauType OBJECT-TYPE
       SYNTAX     OBJECT IDENTIFIER
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This object identifies the 10 or 100 Mb/s
               baseband or broadband MAU type.  An initial set of
               MAU types are defined above.  The assignment of
               OBJECT IDENTIFIERs to new types of MAUs is managed
               by the IANA.  If the MAU type is unknown, the
               object identifier

               unknownMauType OBJECT IDENTIFIER ::= { 0 0 }

               is returned.  Note that unknownMauType is a
               syntactically valid object identifier, and any
               conformant implementation of ASN.1 and the BER
               must be able to generate and recognize this value.

               This object represents the operational type of the
               MAU, as determined by either (1) the result of the
               auto-negotiation function or (2) if auto-
               negotiation is not enabled or is not implemented
               for this MAU, by the value of the object
               ifMauDefaultType.  In case (2), a set to the
               object ifMauDefaultType will force the MAU into
               the new operating mode."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.2, aMAUType."
       ::= { ifMauEntry 3 }

   ifMauStatus OBJECT-TYPE
       SYNTAX     INTEGER {
                      other(1),
                      unknown(2),
                      operational(3),





                      standby(4),
                      shutdown(5),
                      reset(6)
                  }
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "The current state of the MAU.  This object may be
               implemented as a read-only object by those agents
               and MAUs that do not implement software control of
               the MAU state.  Some agents may not support
               setting the value of this object to some of the
               enumerated values.

               The value other(1) is returned if the MAU is in a
               state other than one of the states 2 through 6.

               The value unknown(2) is returned when the MAU's
               true state is unknown; for example, when it is
               being initialized.

               A MAU in the operational(3) state is fully
               functional, operates, and passes signals to its
               attached DTE or repeater port in accordance to its
               specification.

               A MAU in standby(4) state forces DI and CI to idle
               and the media transmitter to idle or fault, if
               supported.  Standby(4) mode only applies to link
               type MAUs.  The state of ifMauMediaAvailable is
               unaffected.

               A MAU in shutdown(5) state assumes the same
               condition on DI, CI, and the media transmitter as
               though it were powered down or not connected.  The
               MAU may return other(1) value for the
               ifMauJabberState and ifMauMediaAvailable objects
               when it is in this state.  For an AUI, this state
               will remove power from the AUI.

               Setting this variable to the value reset(6) resets
               the MAU in the same manner as a power-off, power-
               on cycle of at least one-half second would.  The
               agent is not required to return the value reset
               (6).

               Setting this variable to the value operational(3),
               standby(4), or shutdown(5) causes the MAU to





               assume the respective state except that setting a
               mixing-type MAU or an AUI to standby(4) will cause
               the MAU to enter the shutdown state."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.7, aMAUAdminState,
               30.5.1.2.2, acMAUAdminControl, and 30.5.1.2.1,
               acRESETMAU."
       ::= { ifMauEntry 4 }

   ifMauMediaAvailable OBJECT-TYPE
       SYNTAX     INTEGER {
                      other(1),
                      unknown(2),
                      available(3),
                      notAvailable(4),
                      remoteFault(5),
                      invalidSignal(6),
                      remoteJabber(7),
                      remoteLinkLoss(8),
                      remoteTest(9)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "If the MAU is a link or fiber type (FOIRL,
               10BASE-T, 10BASE-F) then this is equivalent to the
               link test fail state/low light function.  For an
               AUI or a coax (including broadband) MAU this
               indicates whether or not loopback is detected on
               the DI circuit.  The value of this attribute
               persists between packets for MAU types AUI,
               10BASE5, 10BASE2, 10BROAD36, and 10BASE-FP.

               The value other(1) is returned if the
               mediaAvailable state is not one of 2 through 6.

               The value unknown(2) is returned when the MAU's
               true state is unknown; for example, when it is
               being initialized.  At power-up or following a
               reset, the value of this attribute will be unknown
               for AUI, coax, and 10BASE-FP MAUs.  For these MAUs
               loopback will be tested on each transmission
               during which no collision is detected.  If DI is
               receiving input when DO returns to IDL after a
               transmission and there has been no collision
               during the transmission then loopback will be
               detected.  The value of this attribute will only
               change during non-collided transmissions for AUI,





               coax, and 10BASE-FP MAUs.

               For 100BASE-T4, 100BASE-TX and 100BASE-FX the
               enumerations match the states within the
               respective link integrity state diagrams, fig 23-
               12 and 24-15 of sections 23 and 24 of [2].  Any
               MAU which implements management of auto-
               negotiation will map remote fault indication to
               remote fault.

               The value available(3) indicates that the link,
               light, or loopback is normal.  The value
               notAvailable(4) indicates link loss, low light, or
               no loopback.

               The value remoteFault(5) indicates that a fault
               has been detected at the remote end of the link.
               This value applies to 10BASE-FB, 100BASE-T4 Far
               End Fault Indication and non-specified remote
               faults from a system running auto-negotiation.
               The values remoteJabber(7), remoteLinkLoss(8), and
               remoteTest(9) should be used instead of
               remoteFault(5) where the reason for remote fault
               is identified in the remote signaling protocol.

               The value invalidSignal(6) indicates that an
               invalid signal has been received from the other
               end of the link.  InvalidSignal(6) applies only to
               MAUs of type 10BASE-FB.

               Where an IEEE Std 802.3u-1995 clause 22 MII is
               present, a logic one in the remote fault bit
               (reference section 22.2.4.2.8 of that document)
               maps to the value remoteFault(5), and a logic zero
               in the link status bit (reference section
               22.2.4.2.10 of that document) maps to the value
               notAvailable(4).  The value notAvailable(4) takes
               precedence over the value remoteFault(5)."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.4, aMediaAvailable."
       ::= { ifMauEntry 5 }

   ifMauMediaAvailableStateExits OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A count of the number of times that





               ifMauMediaAvailable for this MAU instance leaves
               the state available(3)."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.5, aLoseMediaCounter."
       ::= { ifMauEntry 6 }

   ifMauJabberState OBJECT-TYPE
       SYNTAX     INTEGER {
                      other(1),
                      unknown(2),
                      noJabber(3),
                      jabbering(4)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "The value other(1) is returned if the jabber
               state is not 2, 3, or 4.  The agent must always
               return other(1) for MAU type dot3MauTypeAUI.

               The value unknown(2) is returned when the MAU's
               true state is unknown; for example, when it is
               being initialized.

               If the MAU is not jabbering the agent returns
               noJabber(3).  This is the 'normal' state.

               If the MAU is in jabber state the agent returns
               the jabbering(4) value."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.6,
               aJabber.jabberFlag."
       ::= { ifMauEntry 7 }

   ifMauJabberingStateEnters OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A count of the number of times that
               mauJabberState for this MAU instance enters the
               state jabbering(4).  For MAUs of type
               dot3MauTypeAUI, dot3MauType100BaseT4,
               dot3MauType100BaseTX, and dot3MauType100BaseFX,
               this counter will always indicate zero."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.6,
               aJabber.jabberCounter."





       ::= { ifMauEntry 8 }

   ifMauFalseCarriers OBJECT-TYPE
       SYNTAX     Counter32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A count of the number of false carrier events
               during IDLE in 100BASE-X links.  This counter does
               not increment at the symbol rate.  It can
               increment after a valid carrier completion at a
               maximum rate of once per 100 ms until the next
               carrier event.

               This counter increments only for MAUs of type
               dot3MauType100BaseT4, dot3MauType100BaseTX, and
               dot3MauType100BaseFX.  For all other MAU types,
               this counter will always indicate zero.

               The approximate minimum time for rollover of this
               counter is 7.4 hours."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.10, aFalseCarriers."
       ::= { ifMauEntry 9 }

   ifMauTypeList OBJECT-TYPE
       SYNTAX     Integer32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A value that uniquely identifies the set of
               possible IEEE 802.3 types that the MAU could be.
               The value is a sum which initially takes the value
               zero.  Then, for each type capability of this MAU,
               2 raised to the power noted below is added to the
               sum. For example, a MAU which has the capability
               to be only 10BASE-T would have a value of 512
               (2**9).  In contrast, a MAU which supports both
               10Base-T (full duplex) and 100BASE-TX (full
               duplex) would have a value of ((2**11) + (2**16))
               or 67584.

               The powers of 2 assigned to the capabilities are
               these:

               Power  Capability
                 0      other or unknown
                 1      AUI





                 2      10BASE-5
                 3      FOIRL
                 4      10BASE-2
                 5      10BASE-T duplex mode unknown
                 6      10BASE-FP
                 7      10BASE-FB
                 8      10BASE-FL duplex mode unknown
                 9      10BROAD36
                10      10BASE-T  half duplex mode
                11      10BASE-T  full duplex mode
                12      10BASE-FL half duplex mode
                13      10BASE-FL full duplex mode
                14      100BASE-T4
                15      100BASE-TX half duplex mode
                16      100BASE-TX full duplex mode
                17      100BASE-FX half duplex mode
                18      100BASE-FX full duplex mode
                19      100BASE-T2 half duplex mode
                20      100BASE-T2 full duplex mode

               If auto-negotiation is present on this MAU, this
               object will map to ifMauAutoNegCapability."

       ::= { ifMauEntry 10 }

   ifMauDefaultType OBJECT-TYPE
       SYNTAX     OBJECT IDENTIFIER
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "This object identifies the default administrative
               10 or 100 Mb/s baseband MAU type, to be used in
               conjunction with the operational MAU type denoted
               by ifMauType.

               The set of possible values for this object is the
               same as the set defined for the ifMauType object.

               This object represents the administratively-
               configured type of the MAU.  If auto-negotiation
               is not enabled or is not implemented for this MAU,
               the value of this object determines the
               operational type of the MAU.  In this case, a set
               to this object will force the MAU into the
               specified operating mode.

               If auto-negotiation is implemented and enabled for
               this MAU, the operational type of the MAU is





               determined by auto-negotiation, and the value of
               this object denotes the type to which the MAU will
               automatically revert if/when auto-negotiation is
               later disabled.

               NOTE TO IMPLEMENTORS:  It may be necessary to
               provide for underlying hardware implementations
               which do not follow the exact behavior specified
               above.  In particular, when
               ifMauAutoNegAdminStatus transitions from enabled
               to disabled, the agent implementation must ensure
               that the operational type of the MAU (as reported
               by ifMauType) correctly transitions to the value
               specified by this object, rather than continuing
               to operate at the value earlier determined by the
               auto-negotiation function."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.1.1, aMAUID, and [IEEE
               802.3 Std], 22.2.4.1.4."
       ::= { ifMauEntry 11 }

   ifMauAutoNegSupported OBJECT-TYPE
       SYNTAX     TruthValue
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This object indicates whether or not auto-
               negotiation is supported on this MAU."
       ::= { ifMauEntry 12 }



   -- The ifJackTable applies to MAUs attached to interfaces
   -- which have one or more external jacks (connectors).

   ifJackTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF IfJackEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "Information about the external jacks attached to
               MAUs attached to an interface."
       ::= { dot3IfMauBasicGroup 2 }

   ifJackEntry OBJECT-TYPE
       SYNTAX     IfJackEntry
       MAX-ACCESS not-accessible
       STATUS     current





       DESCRIPTION
               "An entry in the table, containing information
               about a particular jack."
       INDEX    { ifMauIfIndex,
                  ifMauIndex,
                  ifJackIndex }
       ::= { ifJackTable 1 }

   IfJackEntry ::=
       SEQUENCE {
           ifJackIndex
               Integer32,
           ifJackType
               JackType
       }


   ifJackIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "This variable uniquely identifies the jack
               described by this entry from among other jacks
               attached to the same MAU."
       ::= { ifJackEntry 1 }

   ifJackType OBJECT-TYPE
       SYNTAX     JackType
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "The jack connector type, as it appears on the
               outside of the system."
       ::= { ifJackEntry 2 }


   -- The ifMauAutoNegTable applies to systems in which
   -- auto-negotiation is supported on one or more MAUs
   -- attached to interfaces.  Note that if auto-negotiation
   -- is present and enabled, the ifMauType object reflects
   -- the result of the auto-negotiation function.

   ifMauAutoNegTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF IfMauAutoNegEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION





               "Configuration and status objects for the auto-
               negotiation function of MAUs attached to
               interfaces."
       ::= { dot3IfMauAutoNegGroup 1 }

   ifMauAutoNegEntry OBJECT-TYPE
       SYNTAX     IfMauAutoNegEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "An entry in the table, containing configuration
               and status information for the auto-negotiation
               function of a particular MAU."
           INDEX     { ifMauIfIndex, ifMauIndex }
       ::= { ifMauAutoNegTable 1 }

   IfMauAutoNegEntry ::=
       SEQUENCE {
           ifMauAutoNegAdminStatus
               INTEGER,
           ifMauAutoNegRemoteSignaling
               INTEGER,
           ifMauAutoNegConfig
               INTEGER,
           ifMauAutoNegCapability
               Integer32,
           ifMauAutoNegCapAdvertised
               Integer32,
           ifMauAutoNegCapReceived
               Integer32,
           ifMauAutoNegRestart
               INTEGER

       }


   ifMauAutoNegAdminStatus OBJECT-TYPE
       SYNTAX     INTEGER {
                      enabled(1),
                      disabled(2)
                  }
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "Setting this object to enabled(1) will cause the
               interface which has the auto-negotiation signaling
               ability to be enabled.






               If the value of this object is disabled(2) then
               the interface will act as it would if it had no
               auto-negotiation signaling.  Under these
               conditions, an IEEE 802.3 MAU will immediately be
               forced to the state indicated by the value of the
               object ifMauDefaultType.

               NOTE TO IMPLEMENTORS:  When
               ifMauAutoNegAdminStatus transitions from enabled
               to disabled, the agent implementation must ensure
               that the operational type of the MAU (as reported
               by ifMauType) correctly transitions to the value
               specified by the ifMauDefaultType object, rather
               than continuing to operate at the value earlier
               determined by the auto-negotiation function."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.6.1.1.2, aAutoNegAdminState
               and 30.6.1.2.2, acAutoNegAdminControl."
       ::= { ifMauAutoNegEntry 1 }

   ifMauAutoNegRemoteSignaling OBJECT-TYPE
       SYNTAX     INTEGER {
                      detected(1),
                      notdetected(2)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A value indicating whether the remote end of the
               link is using auto-negotiation signaling. It takes
               the value detected(1) if and only if, during the
               previous link negotiation, FLP Bursts were
               received."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.6.1.1.3,
               aAutoNegRemoteSignaling."
       ::= { ifMauAutoNegEntry 2 }

   ifMauAutoNegConfig OBJECT-TYPE
       SYNTAX     INTEGER {
                      other(1),
                      configuring(2),
                      complete(3),
                      disabled(4),
                      parallelDetectFail(5)
                  }
       MAX-ACCESS read-only
       STATUS     current





       DESCRIPTION
               "A value indicating the current status of the
               auto-negotiation process.  The enumeration
               parallelDetectFail(5) maps to a failure in
               parallel detection as defined in 28.2.3.1 of [IEEE
               802.3 Std]."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.6.1.1.4,
               aAutoNegAutoConfig."
       ::= { ifMauAutoNegEntry 4 }

   ifMauAutoNegCapability OBJECT-TYPE
       SYNTAX     Integer32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A value that uniquely identifies the set of
               capabilities of the local auto-negotiation entity.
               The value is a sum which initially takes the value
               zero.  Then, for each capability of this
               interface, 2 raised to the power noted below is
               added to the sum. For example, an interface which
               has the capability to support only 100Base-TX half
               duplex would have a value of 32768 (2**15).  In
               contrast, an interface which supports both
               100Base-TX half duplex and and 100Base-TX full
               duplex would have a value of 98304 ((2**15) +
               (2**16)).

               The powers of 2 assigned to the capabilities are
               these:

               Power   Capability
                 0       other or unknown
                (1-9)    (reserved)
                10       10BASE-T  half duplex mode
                11       10BASE-T  full duplex mode
                12       (reserved)
                13       (reserved)
                14       100BASE-T4
                15       100BASE-TX half duplex mode
                16       100BASE-TX full duplex mode
                17       (reserved)
                18       (reserved)
                19      100BASE-T2 half duplex mode
                20      100BASE-T2 full duplex mode

               Note that interfaces that support this MIB may





               have capabilities that extend beyond the scope of
               this MIB."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.6.1.1.5,
               aAutoNegLocalTechnologyAbility."
       ::= { ifMauAutoNegEntry 5 }

   ifMauAutoNegCapAdvertised OBJECT-TYPE
       SYNTAX     Integer32
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "A value that uniquely identifies the set of
               capabilities advertised by the local auto-
               negotiation entity. Refer to
               ifMauAutoNegCapability for a description of the
               possible values of this object.

               Capabilities in this object that are not available
               in ifMauAutoNegCapability cannot be enabled."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.6.1.1.6,
               aAutoNegAdvertisedTechnologyAbility."
       ::= { ifMauAutoNegEntry 6 }

   ifMauAutoNegCapReceived OBJECT-TYPE
       SYNTAX     Integer32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "A value that uniquely identifies the set of
               capabilities received from the remote auto-
               negotiation entity. Refer to
               ifMauAutoNegCapability for a description of the
               possible values of this object.

               Note that interfaces that support this MIB may be
               attached to remote auto-negotiation entities which
               have capabilities beyond the scope of this MIB."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.6.1.1.7,
               aAutoNegReceivedTechnologyAbility."
       ::= { ifMauAutoNegEntry 7 }

   ifMauAutoNegRestart OBJECT-TYPE
       SYNTAX     INTEGER {
                      restart(1),
                      norestart(2)





                  }
       MAX-ACCESS read-write
       STATUS     current
       DESCRIPTION
               "If the value of this object is set to restart(1)
               then this will force auto-negotiation to begin
               link renegotiation. If auto-negotiation signaling
               is disabled, a write to this object has no effect.

               Setting the value of this object to norestart(2)
               has no effect."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.6.1.2.1,
               acAutoNegRestartAutoConfig."
       ::= { ifMauAutoNegEntry 8 }


   --
   -- The Basic Broadband MAU Table
   --

   broadMauBasicTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF BroadMauBasicEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "Table of descriptive and status information about
               the broadband MAUs connected to interfaces."
       ::= { dot3BroadMauBasicGroup 1 }

   broadMauBasicEntry OBJECT-TYPE
       SYNTAX     BroadMauBasicEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
               "An entry in the table, containing information
               about a single broadband MAU."
       INDEX     { broadMauIfIndex, broadMauIndex }
       ::= { broadMauBasicTable 1 }

   BroadMauBasicEntry ::=
       SEQUENCE {
           broadMauIfIndex
               Integer32,
           broadMauIndex
               Integer32,
           broadMauXmtRcvSplitType
               INTEGER,





           broadMauXmtCarrierFreq
               Integer32,
           broadMauTranslationFreq
               Integer32
       }

   broadMauIfIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This variable uniquely identifies the interface
               to which the MAU described by this entry is
               connected."
       REFERENCE
               "Reference RFC 1213, ifIndex."
       ::= { broadMauBasicEntry 1 }

   broadMauIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This variable uniquely identifies the MAU
               connected to interface broadMauIfIndex that is
               described by this entry."
       REFERENCE
               "Reference IEEE 802.3 MAU Mgt, 20.2.3.2, aMAUID."
       ::= { broadMauBasicEntry 2 }

   broadMauXmtRcvSplitType OBJECT-TYPE
       SYNTAX     INTEGER {
                      other(1),
                      single(2),
                      dual(3)
                  }
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This object indicates the type of frequency
               multiplexing/cabling system used to separate the
               transmit and receive paths for the 10BROAD36 MAU.

               The value other(1) is returned if the split type
               is not either single or dual.

               The value single(2) indicates a single cable
               system.  The value dual(3) indicates a dual cable





               system, offset normally zero."
       REFERENCE
               "Reference IEEE 802.3 MAU Mgt, 20.2.3.2,
               aBbMAUXmitRcvSplitType."
       ::= { broadMauBasicEntry 3 }

   broadMauXmtCarrierFreq OBJECT-TYPE
       SYNTAX     Integer32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This variable indicates the transmit carrier
               frequency of the 10BROAD36 MAU in MHz/4; that is,
               in units of 250 kHz."
       REFERENCE
               "Reference IEEE 802.3 MAU Mgt, 20.2.3.2,
               aBroadbandFrequencies.xmitCarrierFrequency."
       ::= { broadMauBasicEntry 4 }

   broadMauTranslationFreq OBJECT-TYPE
       SYNTAX     Integer32
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
               "This variable indicates the translation offset
               frequency of the 10BROAD36 MAU in MHz/4; that is,
               in units of 250 kHz."
       REFERENCE
               "Reference IEEE 802.3 MAU Mgt, 20.2.3.2,
               aBroadbandFrequencies.translationFrequency."
       ::= { broadMauBasicEntry 5 }



   -- Notifications for use by 802.3 MAUs

   rpMauJabberTrap NOTIFICATION-TYPE
       OBJECTS     { rpMauJabberState }
       STATUS      current
       DESCRIPTION
               "This trap is sent whenever a managed repeater MAU
               enters the jabber state.

               The agent must throttle the generation of
               consecutive rpMauJabberTraps so that there is at
               least a five-second gap between them."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.3.1, nJabber





               notification."
       ::= { snmpDot3MauMgt 0 1 }

   ifMauJabberTrap NOTIFICATION-TYPE
       OBJECTS     { ifMauJabberState }
       STATUS      current
       DESCRIPTION
               "This trap is sent whenever a managed interface
               MAU enters the jabber state.

               The agent must throttle the generation of
               consecutive ifMauJabberTraps so that there is at
               least a five-second gap between them."
       REFERENCE
               "[IEEE 802.3 Mgt], 30.5.1.3.1, nJabber
               notification."
       ::= { snmpDot3MauMgt 0 2 }


   -- Conformance information

   mauModConf
           OBJECT IDENTIFIER ::= { mauMod 1 }
     mauModCompls
           OBJECT IDENTIFIER ::= { mauModConf 1 }
     mauModObjGrps
           OBJECT IDENTIFIER ::= { mauModConf 2 }
     mauModNotGrps
           OBJECT IDENTIFIER ::= { mauModConf 3 }


   -- Object groups

   mauRpGrpBasic OBJECT-GROUP
       OBJECTS     { rpMauGroupIndex,
                     rpMauPortIndex,
                     rpMauIndex,
                     rpMauType,
                     rpMauStatus,
                     rpMauMediaAvailable,
                     rpMauMediaAvailableStateExits,
                     rpMauJabberState,
                     rpMauJabberingStateEnters }
       STATUS      current
       DESCRIPTION
           "Basic conformance group for MAUs attached to
           repeater ports.  This group is also the
           conformance specification for RFC 1515





           implementations."
       ::= { mauModObjGrps 1 }

   mauRpGrp100Mbs OBJECT-GROUP
       OBJECTS     { rpMauFalseCarriers }
       STATUS      current
       DESCRIPTION
           "Conformance group for MAUs attached to
           repeater ports with 100 Mb/s capability."
       ::= { mauModObjGrps 2 }

   mauRpGrpJack OBJECT-GROUP
       OBJECTS     { rpJackType }
       STATUS      current
       DESCRIPTION
           "Conformance group for MAUs attached to
           repeater ports with managed jacks."
       ::= { mauModObjGrps 3 }

   mauIfGrpBasic OBJECT-GROUP
       OBJECTS     { ifMauIfIndex,
                     ifMauIndex,
                     ifMauType,
                     ifMauStatus,
                     ifMauMediaAvailable,
                     ifMauMediaAvailableStateExits,
                     ifMauJabberState,
                     ifMauJabberingStateEnters }
       STATUS      current
       DESCRIPTION
           "Basic conformance group for MAUs attached to
           interfaces.  This group also provides a
           conformance specification for RFC 1515
           implementations."
       ::= { mauModObjGrps 4 }

   mauIfGrp100Mbs OBJECT-GROUP
       OBJECTS     { ifMauFalseCarriers,
                     ifMauTypeList,
                     ifMauDefaultType,
                     ifMauAutoNegSupported }
       STATUS      current
       DESCRIPTION
           "Conformance group for MAUs attached
           to interfaces with 100 Mb/s capability."
       ::= { mauModObjGrps 5 }

   mauIfGrpJack OBJECT-GROUP





       OBJECTS     { ifJackType }
       STATUS      current
       DESCRIPTION
           "Conformance group for MAUs attached
           to interfaces with managed jacks."
       ::= { mauModObjGrps 6 }

   mauIfGrpAutoNeg OBJECT-GROUP
       OBJECTS     { ifMauAutoNegAdminStatus,
                     ifMauAutoNegRemoteSignaling,
                     ifMauAutoNegConfig,
                     ifMauAutoNegCapability,
                     ifMauAutoNegCapAdvertised,
                     ifMauAutoNegCapReceived,
                     ifMauAutoNegRestart }
       STATUS      current
       DESCRIPTION
           "Conformance group for MAUs attached to
           interfaces with managed auto-negotiation."
       ::= { mauModObjGrps 7 }

   mauBroadBasic OBJECT-GROUP
       OBJECTS     { broadMauIfIndex,
                     broadMauIndex,
                     broadMauXmtRcvSplitType,
                     broadMauXmtCarrierFreq,
                     broadMauTranslationFreq }
       STATUS      current
       DESCRIPTION
           "Conformance group for broadband MAUs
           attached to interfaces.  This group
           provides a conformance specification
           for RFC 1515 implementations."
       ::= { mauModObjGrps 8 }

   -- Notification groups

   rpMauNotifications NOTIFICATION-GROUP
       NOTIFICATIONS { rpMauJabberTrap }
       STATUS      current
       DESCRIPTION
           "Notifications for repeater MAUs."
       ::= { mauModNotGrps 1 }

   ifMauNotifications NOTIFICATION-GROUP
       NOTIFICATIONS { ifMauJabberTrap }
       STATUS      current
       DESCRIPTION





           "Notifications for interface MAUs."
       ::= { mauModNotGrps 2 }


   -- Compliances

   mauModRpCompl MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "Compliance for MAUs attached to repeater ports."

       MODULE -- this module
           MANDATORY-GROUPS { mauRpGrpBasic }

           GROUP mauRpGrp100Mbs
           DESCRIPTION
               "Implementation of this optional group is
               recommended for MAUs which have 100Mb/s
               capability."

           GROUP mauRpGrpJack
           DESCRIPTION
               "Implementation of this optional group is
               recommended for MAUs which have one or more
               external jacks."

           GROUP rpMauNotifications
           DESCRIPTION
               "Implementation of this group is
               recommended for MAUs attached to repeater
               ports."

       ::= { mauModCompls 1 }


   mauModIfCompl MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "Compliance for MAUs attached to interfaces."

       MODULE -- this module
           MANDATORY-GROUPS { mauIfGrpBasic }

           GROUP mauIfGrp100Mbs
           DESCRIPTION
               "Implementation of this optional group is
               recommended for MAUs which have 100Mb/s
               capability."





           GROUP mauIfGrpJack
           DESCRIPTION
               "Implementation of this optional group is
               recommended for MAUs which have one or more
               external jacks."

           GROUP mauIfGrpAutoNeg
           DESCRIPTION
               "Implementation of this group is
               mandatory for MAUs which support
               managed auto-negotiation."

           GROUP mauBroadBasic
           DESCRIPTION
               "Implementation of this group is
               mandatory for broadband MAUs."

           GROUP ifMauNotifications
           DESCRIPTION
               "Implementation of this group is
               recommended for MAUs attached to
               interfaces."

       ::= { mauModCompls 2 }

   END


