MPLS-LDP-STD-MIB DEFINITIONS ::= BEGIN


     IMPORTS
         OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE,
         Integer32, Counter32, Unsigned32
             FROM SNMPv2-SMI                                -- [RFC2578]

         MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
             FROM SNMPv2-CONF                              --  [RFC2580]

         RowStatus, TimeInterval, TruthValue,
         TimeStamp, StorageType





             FROM SNMPv2-TC                                --  [RFC2579]

         InetAddressPrefixLength,
         InetAddressType,
         InetAddress,
         InetPortNumber
             FROM INET-ADDRESS-MIB                         --  [RFC3291]

         IndexInteger,
         IndexIntegerNextFree
             FROM DIFFSERV-MIB                             --  [RFC3289]

         mplsStdMIB,
         MplsLabelDistributionMethod,
         MplsLdpIdentifier,
         MplsLdpLabelType,
         MplsLspType,
         MplsLsrIdentifier,
         MplsRetentionMode
             FROM MPLS-TC-STD-MIB                          --  [RFC3811]

         MplsIndexType
             FROM MPLS-LSR-STD-MIB;                        --  [RFC3813]

     mplsLdpStdMIB MODULE-IDENTITY
         LAST-UPDATED "200406030000Z"  -- June 3, 2004
         ORGANIZATION "Multiprotocol Label Switching (mpls)
                       Working Group"
         CONTACT-INFO

             "Joan Cucchiara (jcucchiara@mindspring.com)
              Marconi Communications, Inc.

              Hans Sjostrand (hans@ipunplugged.com)
              ipUnplugged

              James V. Luciani (james_luciani@mindspring.com)
              Marconi Communications, Inc.

              Working Group Chairs:
              George Swallow,   email: swallow@cisco.com
              Loa Andersson,    email: loa@pi.se

              MPLS Working Group, email: mpls@uu.net"

         DESCRIPTION
             "Copyright (C) The Internet Society (2004). The
             initial version of this MIB module was published





             in RFC 3815. For full legal notices see the RFC
             itself or see:
             http://www.ietf.org/copyrights/ianamib.html

             This MIB contains managed object definitions for the
             'Multiprotocol Label Switching, Label Distribution
             Protocol, LDP' document."

         REVISION "200406030000Z"  -- June 3, 2004
         DESCRIPTION
            "Initial version published as part of RFC 3815."

         ::= { mplsStdMIB 4 }

     --****************************************************************

     mplsLdpNotifications OBJECT IDENTIFIER ::= { mplsLdpStdMIB 0 }
     mplsLdpObjects       OBJECT IDENTIFIER ::= { mplsLdpStdMIB 1 }
     mplsLdpConformance   OBJECT IDENTIFIER ::= { mplsLdpStdMIB 2 }

     --****************************************************************
     -- MPLS LDP Objects
     --****************************************************************

     mplsLdpLsrObjects    OBJECT IDENTIFIER ::= { mplsLdpObjects 1 }

     mplsLdpEntityObjects OBJECT IDENTIFIER ::= { mplsLdpObjects 2 }

     --
     -- The MPLS Label Distribution Protocol's
     -- Label Switching Router Objects
     --

     mplsLdpLsrId OBJECT-TYPE
         SYNTAX      MplsLsrIdentifier
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The Label Switching Router's Identifier."
         ::= { mplsLdpLsrObjects 1 }

     mplsLdpLsrLoopDetectionCapable OBJECT-TYPE
         SYNTAX      INTEGER {
                                none(1),
                                other(2),
                                hopCount(3),
                                pathVector(4),
                                hopCountAndPathVector(5)





                             }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "A indication of whether this
             Label Switching Router supports
             loop detection.

             none(1) -- Loop Detection is not supported
                        on this LSR.

             other(2) -- Loop Detection is supported but
                         by a method other than those
                         listed below.

             hopCount(3) -- Loop Detection is supported by
                            Hop Count only.

             pathVector(4) -- Loop Detection is supported by
                              Path Vector only.

             hopCountAndPathVector(5) -- Loop Detection is
                                  supported by both Hop Count
                                  And Path Vector.

             Since Loop Detection is determined during
             Session Initialization, an individual session
             may not be running with loop detection.  This
             object simply gives an indication of whether or not the
             LSR has the ability to support Loop Detection and
             which types."

         ::= { mplsLdpLsrObjects 2 }

     --
     -- The MPLS Label Distribution Protocol Entity Objects
     --

     mplsLdpEntityLastChange OBJECT-TYPE
         SYNTAX  TimeStamp
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
             "The value of sysUpTime at the time of the most
             recent addition or deletion of an entry
             to/from the mplsLdpEntityTable/mplsLdpEntityStatsTable, or
             the most recent change in value of any objects in the
             mplsLdpEntityTable.





             If no such changes have occurred since the last
             re-initialization of the local management subsystem,
             then this object contains a zero value."
         ::= { mplsLdpEntityObjects 1 }

     mplsLdpEntityIndexNext  OBJECT-TYPE
         SYNTAX      IndexIntegerNextFree
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
             "This object contains an appropriate value to
             be used for mplsLdpEntityIndex when creating
             entries in the mplsLdpEntityTable. The value
             0 indicates that no unassigned entries are
             available."
        ::= { mplsLdpEntityObjects 2 }


     mplsLdpEntityTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsLdpEntityEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "This table contains information about the
             MPLS Label Distribution Protocol Entities which
             exist on this Label Switching Router (LSR)
             or Label Edge Router (LER)."
          ::= { mplsLdpEntityObjects 3 }

      mplsLdpEntityEntry OBJECT-TYPE
          SYNTAX      MplsLdpEntityEntry
          MAX-ACCESS  not-accessible
          STATUS      current
          DESCRIPTION
              "An entry in this table represents an LDP entity.
              An entry can be created by a network administrator
              or by an SNMP agent as instructed by LDP."
          INDEX       {  mplsLdpEntityLdpId, mplsLdpEntityIndex  }
          ::= { mplsLdpEntityTable 1 }

      MplsLdpEntityEntry ::= SEQUENCE {
          mplsLdpEntityLdpId                MplsLdpIdentifier,
          mplsLdpEntityIndex                IndexInteger,
          mplsLdpEntityProtocolVersion      Unsigned32,
          mplsLdpEntityAdminStatus          INTEGER,
          mplsLdpEntityOperStatus           INTEGER,
          mplsLdpEntityTcpPort              InetPortNumber,
          mplsLdpEntityUdpDscPort           InetPortNumber,





          mplsLdpEntityMaxPduLength         Unsigned32,
          mplsLdpEntityKeepAliveHoldTimer   Unsigned32,
          mplsLdpEntityHelloHoldTimer       Unsigned32,
          mplsLdpEntityInitSessionThreshold Integer32,
          mplsLdpEntityLabelDistMethod      MplsLabelDistributionMethod,
          mplsLdpEntityLabelRetentionMode   MplsRetentionMode,
          mplsLdpEntityPathVectorLimit      Integer32,
          mplsLdpEntityHopCountLimit        Integer32,
          mplsLdpEntityTransportAddrKind    INTEGER,
          mplsLdpEntityTargetPeer           TruthValue,
          mplsLdpEntityTargetPeerAddrType   InetAddressType,
          mplsLdpEntityTargetPeerAddr       InetAddress,
          mplsLdpEntityLabelType            MplsLdpLabelType,
          mplsLdpEntityDiscontinuityTime    TimeStamp,
          mplsLdpEntityStorageType          StorageType,
          mplsLdpEntityRowStatus            RowStatus
      }

      mplsLdpEntityLdpId OBJECT-TYPE
          SYNTAX      MplsLdpIdentifier
          MAX-ACCESS  not-accessible
          STATUS      current
          DESCRIPTION
              "The LDP identifier."
         REFERENCE
             "RFC3036, LDP Specification, Section on LDP Identifiers."
         ::= { mplsLdpEntityEntry 1 }

     mplsLdpEntityIndex OBJECT-TYPE
         SYNTAX      IndexInteger
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "This index is used as a secondary index to uniquely
             identify this row.  Before creating a row in this table,
             the 'mplsLdpEntityIndexNext' object should be retrieved.
             That value should be used for the value of this index
             when creating a row in this table.  NOTE:  if a value
             of zero (0) is retrieved, that indicates that no rows
             can be created in this table at this time.

             A secondary index (this object) is meaningful to some
             but not all, LDP implementations.  For example
             an LDP implementation which uses PPP would
             use this index to differentiate PPP sub-links.

             Another way to use this index is to give this the
             value of ifIndex.  However, this is dependant





             on the implementation."
         ::= { mplsLdpEntityEntry 2 }

     mplsLdpEntityProtocolVersion OBJECT-TYPE
         SYNTAX      Unsigned32(1..65535)
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
            "The version number of the LDP protocol which will be
            used in the session initialization message.

            Section 3.5.3 in the LDP Specification specifies
            that the version of the LDP protocol is negotiated during
            session establishment. The value of this object
            represents the value that is sent in the initialization
            message."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.3 Initialization
            Message."
         DEFVAL { 1 }
         ::= { mplsLdpEntityEntry 3 }

     mplsLdpEntityAdminStatus OBJECT-TYPE
         SYNTAX      INTEGER {
                       enable(1),
                       disable(2)
                     }
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The administrative status of this LDP Entity.
             If this object is changed from 'enable' to 'disable'
             and this entity has already attempted to establish
             contact with a Peer, then all contact with that
             Peer is lost and all information from that Peer
             needs to be removed from the MIB. (This implies
             that the network management subsystem should clean
             up any related entry in the mplsLdpPeerTable.  This
             further implies that a 'tear-down' for that session
             is issued and the session and all information related
             to that session cease to exist).

             At this point the operator is able to change values
             which are related to this entity.

             When the admin status is set back to 'enable', then
             this Entity will attempt to establish a new session
             with the Peer."





         DEFVAL  { enable }
         ::= { mplsLdpEntityEntry 4 }

     mplsLdpEntityOperStatus OBJECT-TYPE
         SYNTAX      INTEGER {
                       unknown(1),
                       enabled(2),
                       disabled(3)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The operational status of this LDP Entity.

             The value of unknown(1) indicates that the
             operational status cannot be determined at
             this time.  The value of unknown should be
             a transient condition before changing
             to enabled(2) or disabled(3)."
         ::= { mplsLdpEntityEntry 5 }

     mplsLdpEntityTcpPort OBJECT-TYPE
         SYNTAX      InetPortNumber
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The TCP Port for
             LDP.  The default value is the well-known
             value of this port."
         REFERENCE
             "RFC3036, LDP Specification, Section 3.10, Well-known
              Numbers, and Section 3.10.1.  UDP and TCP Ports."
         DEFVAL { 646 }
         ::= { mplsLdpEntityEntry 6 }

     mplsLdpEntityUdpDscPort OBJECT-TYPE
         SYNTAX      InetPortNumber
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The UDP Discovery Port for
             LDP.  The default value is the
             well-known value for this port."
         REFERENCE
             "RFC3036, LDP Specification, Section 2.4.1,
             Basic Discovery Mechanism, Section 2.4.2,
             Extended Discovery Mechanism, Section
             3.10, Well-known Numbers, and Section 3.10.1.





             UDP and TCP Ports."
         DEFVAL { 646 }
         ::= { mplsLdpEntityEntry 7 }

     mplsLdpEntityMaxPduLength OBJECT-TYPE
         SYNTAX      Unsigned32 (256..65535)
         UNITS       "octets"
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
            "The maximum PDU Length that is sent in
            the Common Session Parameters of an Initialization
            Message. According to the LDP Specification [RFC3036]
            a value of 255 or less specifies the
            default maximum length of 4096 octets, this is why
            the value of this object starts at 256.  The operator
            should explicitly choose the default value (i.e., 4096),
            or some other value.

            The receiving LSR MUST calculate the maximum PDU
            length for the session by using the smaller of its and
            its peer's proposals for Max PDU Length."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.3.
            Initialization Message."
         DEFVAL { 4096 }
         ::= { mplsLdpEntityEntry 8 }

     mplsLdpEntityKeepAliveHoldTimer OBJECT-TYPE
         SYNTAX      Unsigned32 (1..65535)
         UNITS       "seconds"
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The 16-bit integer value which is the proposed keep
             alive hold timer for this LDP Entity."
         DEFVAL { 40 }
         ::= { mplsLdpEntityEntry 9 }

     mplsLdpEntityHelloHoldTimer OBJECT-TYPE
         SYNTAX      Unsigned32 (0..65535)
         UNITS       "seconds"
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The 16-bit integer value which is the proposed Hello
             hold timer for this LDP Entity. The Hello Hold time
             in seconds.





             An LSR maintains a record of Hellos received
             from potential peers.  This object represents
             the Hold Time in the Common Hello Parameters TLV of
             the Hello Message.

             A value of 0 is a default value and should be
             interpretted in conjunction with the
             mplsLdpEntityTargetPeer object.

             If the value of this object is 0: if the value of the
             mplsLdpEntityTargetPeer object is false(2), then this
             specifies that the Hold Time's actual default value is
             15 seconds (i.e., the default Hold time for Link Hellos
             is 15 seconds).  Otherwise if the value of the
             mplsLdpEntityTargetPeer object is true(1), then this
             specifies that the Hold Time's actual default value is
             45 seconds (i.e., the default Hold time for Targeted
             Hellos is 45 seconds).

             A value of 65535 means infinite (i.e., wait forever).

             All other values represent the amount of time in
             seconds to wait for a Hello Message.  Setting the
             hold time to a value smaller than 15 is not
             recommended, although not forbidden according
             to RFC3036."
         REFERENCE
             "RFC3036, LDP Specification, Section 3.5.2.,
             Hello Message."
         DEFVAL { 0 }
         ::= { mplsLdpEntityEntry 10 }

     mplsLdpEntityInitSessionThreshold OBJECT-TYPE
         SYNTAX      Integer32(0..100)
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "When attempting to establish a session with
             a given Peer, the given LDP Entity should
             send out the SNMP notification,
             'mplsLdpInitSessionThresholdExceeded', when
             the number of Session Initialization messages
             sent exceeds this threshold.

             The notification is used to notify an
             operator when this Entity and its Peer are
             possibly engaged in an endless sequence
             of messages as each NAKs the other's





             Initialization messages with Error Notification
             messages.  Setting this threshold which triggers
             the notification is one way to notify the
             operator.  The notification should be generated
             each time this threshold is exceeded and
             for every subsequent Initialization message
             which is NAK'd with an Error Notification
             message after this threshold is exceeded.

             A value of 0 (zero) for this object
             indicates that the threshold is infinity, thus
             the SNMP notification will never be generated."
         REFERENCE
             "RFC3036, LDP Specification,
             Section 2.5.3 Session Initialization."
         DEFVAL { 8 }
         ::= { mplsLdpEntityEntry 11 }

     mplsLdpEntityLabelDistMethod OBJECT-TYPE
         SYNTAX      MplsLabelDistributionMethod
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "For any given LDP session, the method of
             label distribution must be specified."
         ::= { mplsLdpEntityEntry 12 }

     mplsLdpEntityLabelRetentionMode OBJECT-TYPE
         SYNTAX      MplsRetentionMode
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The LDP Entity can be configured to use either
             conservative or liberal label retention mode.

             If the value of this object is conservative(1)
             then advertized label mappings are retained
             only if they will be used to forward packets,
             i.e., if label came from a valid next hop.

             If the value of this object is liberal(2)
             then all advertized label mappings are retained
             whether they are from a valid next hop or not."
         ::= { mplsLdpEntityEntry 13 }

     mplsLdpEntityPathVectorLimit OBJECT-TYPE
         SYNTAX      Integer32 (0..255)
         MAX-ACCESS  read-create





         STATUS      current
         DESCRIPTION
             "If the value of this object is 0 (zero) then
             Loop Detection for Path Vectors is disabled.

             Otherwise, if this object has a value greater than
             zero, then Loop Dection for Path Vectors is enabled,
             and the Path Vector Limit is this value.
             Also, the value of the object,
             'mplsLdpLsrLoopDetectionCapable', must be set to
             either 'pathVector(4)' or 'hopCountAndPathVector(5)',
             if this object has a value greater than 0 (zero),
             otherwise it is ignored."
         REFERENCE
            "RFC3036, LDP Specification, Section 2.8 Loop Dection,
            Section 3.4.5 Path Vector TLV."
         ::= { mplsLdpEntityEntry 14 }

     mplsLdpEntityHopCountLimit OBJECT-TYPE
         SYNTAX       Integer32 (0..255)
         MAX-ACCESS   read-create
         STATUS       current
         DESCRIPTION
             "If the value of this object is 0 (zero),
             then Loop Detection using Hop Counters is
             disabled.

             If the value of this object is greater than
             0 (zero) then Loop Detection using Hop
             Counters is enabled, and this object
             specifies this Entity's maximum allowable
             value for the Hop Count.
             Also, the value of the object
             mplsLdpLsrLoopDetectionCapable must be set
             to either 'hopCount(3)' or
             'hopCountAndPathVector(5)' if this object
             has a value greater than 0 (zero), otherwise
             it is ignored."
         DEFVAL { 0 }
         ::= { mplsLdpEntityEntry 15 }

     mplsLdpEntityTransportAddrKind OBJECT-TYPE
         SYNTAX     INTEGER {
                               interface(1),
                               loopback(2)
                            }
         MAX-ACCESS read-create
         STATUS     current





         DESCRIPTION
             "This specifies whether the loopback or interface
             address is to be used as the transport address
             in the transport address TLV of the
             hello message.

             If the value is interface(1), then the IP
             address of the interface from which hello
             messages are sent is used as the transport
             address in the hello message.

             Otherwise, if the value is loopback(2), then the IP
             address of the loopback interface is used as the
             transport address in the hello message."
         DEFVAL { loopback }
         ::= { mplsLdpEntityEntry 16 }

     mplsLdpEntityTargetPeer OBJECT-TYPE
         SYNTAX      TruthValue
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "If this LDP entity uses targeted peer then set
             this to true."
         DEFVAL { false }
         ::= { mplsLdpEntityEntry 17 }

     mplsLdpEntityTargetPeerAddrType OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The type of the internetwork layer address used for
             the Extended Discovery.  This object indicates how
             the value of mplsLdpEntityTargetPeerAddr is to
             be interpreted."
         ::= { mplsLdpEntityEntry 18 }

     mplsLdpEntityTargetPeerAddr OBJECT-TYPE
         SYNTAX      InetAddress
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The value of the internetwork layer address
             used for the Extended Discovery.  The value of
             mplsLdpEntityTargetPeerAddrType specifies how
             this address is to be interpreted."
        ::= { mplsLdpEntityEntry 19 }





     mplsLdpEntityLabelType OBJECT-TYPE
         SYNTAX      MplsLdpLabelType
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "Specifies the optional parameters for the LDP
             Initialization Message.

             If the value is generic(1) then no
             optional parameters will be sent in
             the LDP Initialization message associated
             with this Entity.

             If the value is atmParameters(2) then
             a row must be created in the
             mplsLdpEntityAtmTable, which
             corresponds to this entry.

             If the value is frameRelayParameters(3) then
             a row must be created in the
             mplsLdpEntityFrameRelayTable, which
             corresponds to this entry."
         REFERENCE
             "RFC3036, LDP Specification, Section 3.5.3.,
             Initialization Message."
         ::= { mplsLdpEntityEntry 20 }

     mplsLdpEntityDiscontinuityTime OBJECT-TYPE
         SYNTAX      TimeStamp
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The value of sysUpTime on the most recent occasion
             at which any one or more of this entity's counters
             suffered a discontinuity.  The relevant counters
             are the specific instances associated with this
             entity of any Counter32 object contained
             in the 'mplsLdpEntityStatsTable'.  If no such
             discontinuities have occurred since the last
             re-initialization of the local management
             subsystem, then this object contains a zero
             value."
         ::= { mplsLdpEntityEntry 21 }

     mplsLdpEntityStorageType  OBJECT-TYPE
         SYNTAX      StorageType
         MAX-ACCESS  read-create
         STATUS      current





         DESCRIPTION
             "The storage type for this conceptual row.
             Conceptual rows having the value 'permanent(4)'
             need not allow write-access to any columnar
             objects in the row."
         DEFVAL{ nonVolatile }
         ::= { mplsLdpEntityEntry 22 }

     mplsLdpEntityRowStatus OBJECT-TYPE
         SYNTAX      RowStatus
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The status of this conceptual row.  All writable
              objects in this row may be modified at any
              time, however, as described in detail in
              the section entitled, 'Changing Values After
              Session Establishment', and again described
              in the DESCRIPTION clause of the
              mplsLdpEntityAdminStatus object, if a session
              has been initiated with a Peer, changing objects
              in this table will wreak havoc with the session
              and interrupt traffic.  To repeat again:
              the recommended procedure is to
              set the mplsLdpEntityAdminStatus to down, thereby
              explicitly causing a session to be torn down. Then,
              change objects in this entry, then set
              the mplsLdpEntityAdminStatus to enable,
              which enables a new session to be initiated."
         ::= { mplsLdpEntityEntry 23 }

     --
     -- The MPLS LDP Entity Statistics Table
     --

     mplsLdpEntityStatsTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsLdpEntityStatsEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "This table is a read-only table which augments
             the mplsLdpEntityTable.  The purpose of this
             table is to keep statistical information about
             the LDP Entities on the LSR."
         ::= { mplsLdpEntityObjects 4 }

     mplsLdpEntityStatsEntry OBJECT-TYPE
         SYNTAX      MplsLdpEntityStatsEntry





         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "A row in this table contains statistical information
             about an LDP Entity.  Some counters contained in a
             row are for fatal errors received during a former
             LDP Session associated with this entry.  For example,
             an LDP PDU received on a TCP connection during an
             LDP Session contains a fatal error.  That
             error is counted here, because the
             session is terminated.

             If the error is NOT fatal (i.e., the Session
             remains), then the error is counted in the
             mplsLdpSessionStatsEntry."
         AUGMENTS       {   mplsLdpEntityEntry  }
         ::= { mplsLdpEntityStatsTable 1 }

     MplsLdpEntityStatsEntry ::= SEQUENCE {
         mplsLdpEntityStatsSessionAttempts               Counter32,
         mplsLdpEntityStatsSessionRejectedNoHelloErrors  Counter32,
         mplsLdpEntityStatsSessionRejectedAdErrors       Counter32,
         mplsLdpEntityStatsSessionRejectedMaxPduErrors   Counter32,
         mplsLdpEntityStatsSessionRejectedLRErrors       Counter32,
         mplsLdpEntityStatsBadLdpIdentifierErrors        Counter32,
         mplsLdpEntityStatsBadPduLengthErrors            Counter32,
         mplsLdpEntityStatsBadMessageLengthErrors        Counter32,
         mplsLdpEntityStatsBadTlvLengthErrors            Counter32,
         mplsLdpEntityStatsMalformedTlvValueErrors       Counter32,
         mplsLdpEntityStatsKeepAliveTimerExpErrors       Counter32,
         mplsLdpEntityStatsShutdownReceivedNotifications Counter32,
         mplsLdpEntityStatsShutdownSentNotifications     Counter32
     }

     mplsLdpEntityStatsSessionAttempts OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "A count of the Session Initialization messages
             which were sent or received by this LDP Entity and
             were NAK'd.   In other words, this counter counts
             the number of session initializations that failed.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."





         ::= { mplsLdpEntityStatsEntry 1 }

     mplsLdpEntityStatsSessionRejectedNoHelloErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "A count of the Session Rejected/No Hello Error
             Notification Messages sent or received by
             this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         ::= { mplsLdpEntityStatsEntry 2 }

     mplsLdpEntityStatsSessionRejectedAdErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "A count of the Session Rejected/Parameters
             Advertisement Mode Error Notification Messages sent
             or received by this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         ::= { mplsLdpEntityStatsEntry 3 }

     mplsLdpEntityStatsSessionRejectedMaxPduErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "A count of the Session Rejected/Parameters

             Max Pdu Length Error Notification Messages sent
             or received by this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         ::= { mplsLdpEntityStatsEntry 4 }






     mplsLdpEntityStatsSessionRejectedLRErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "A count of the Session Rejected/Parameters
             Label Range Notification Messages sent
             or received by this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         ::= { mplsLdpEntityStatsEntry 5 }

     mplsLdpEntityStatsBadLdpIdentifierErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Bad LDP Identifier
             Fatal Errors detected by the session(s)
             (past and present) associated with this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.1.2."
         ::= { mplsLdpEntityStatsEntry 6 }

     mplsLdpEntityStatsBadPduLengthErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Bad PDU Length
             Fatal Errors detected by the session(s)
             (past and present) associated with this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.1.2."
         ::= { mplsLdpEntityStatsEntry 7 }





     mplsLdpEntityStatsBadMessageLengthErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Bad Message
             Length Fatal Errors detected by the session(s)
             (past and present) associated with this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.1.2."
         ::= { mplsLdpEntityStatsEntry 8 }

     mplsLdpEntityStatsBadTlvLengthErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Bad TLV
             Length Fatal Errors detected by the session(s)
             (past and present) associated with this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.1.2."
         ::= { mplsLdpEntityStatsEntry 9 }

     mplsLdpEntityStatsMalformedTlvValueErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Malformed TLV
             Value Fatal Errors detected by the session(s)
             (past and present) associated with this
             LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."





         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.1.2."
         ::= { mplsLdpEntityStatsEntry 10 }

     mplsLdpEntityStatsKeepAliveTimerExpErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Session Keep Alive
             Timer Expired Errors detected by the session(s)
             (past and present) associated with this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.1.2."
         ::= { mplsLdpEntityStatsEntry 11 }

     mplsLdpEntityStatsShutdownReceivedNotifications OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Shutdown Notifications
             received related to session(s) (past and present)
             associated with this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpEntityDiscontinuityTime."
         ::= { mplsLdpEntityStatsEntry 12 }

     mplsLdpEntityStatsShutdownSentNotifications OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Shutdown Notfications
             sent related to session(s) (past and present) associated
             with this LDP Entity.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of





             mplsLdpEntityDiscontinuityTime."
         ::= { mplsLdpEntityStatsEntry 13 }

     --
     -- The MPLS LDP Peer Table
     --

     mplsLdpSessionObjects OBJECT IDENTIFIER ::= { mplsLdpObjects 3 }

     mplsLdpPeerLastChange OBJECT-TYPE
         SYNTAX  TimeStamp
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
             "The value of sysUpTime at the time of the most
             recent addition or deletion to/from the
             mplsLdpPeerTable/mplsLdpSessionTable."
         ::= { mplsLdpSessionObjects 1 }

     mplsLdpPeerTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsLdpPeerEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "Information about LDP peers known by Entities in
             the mplsLdpEntityTable.  The information in this table
             is based on information from the Entity-Peer interaction
             during session initialization but is not appropriate
             for the mplsLdpSessionTable, because objects in this
             table may or may not be used in session establishment."
         ::= { mplsLdpSessionObjects 2 }

     mplsLdpPeerEntry OBJECT-TYPE
         SYNTAX      MplsLdpPeerEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "Information about a single Peer which is related
             to a Session.  This table is augmented by
             the mplsLdpSessionTable."
         INDEX       { mplsLdpEntityLdpId,
                       mplsLdpEntityIndex,
                       mplsLdpPeerLdpId }
         ::= { mplsLdpPeerTable 1 }

     MplsLdpPeerEntry ::= SEQUENCE {
         mplsLdpPeerLdpId                MplsLdpIdentifier,
         mplsLdpPeerLabelDistMethod      MplsLabelDistributionMethod,





         mplsLdpPeerPathVectorLimit      Integer32,
         mplsLdpPeerTransportAddrType    InetAddressType,
         mplsLdpPeerTransportAddr        InetAddress
     }

     mplsLdpPeerLdpId OBJECT-TYPE
         SYNTAX      MplsLdpIdentifier
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "The LDP identifier of this LDP Peer."
         ::= { mplsLdpPeerEntry 1 }

     mplsLdpPeerLabelDistMethod OBJECT-TYPE
         SYNTAX      MplsLabelDistributionMethod
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "For any given LDP session, the method of
             label distribution must be specified."
         ::= { mplsLdpPeerEntry 2 }

     mplsLdpPeerPathVectorLimit OBJECT-TYPE
         SYNTAX      Integer32 (0..255)
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "If the value of this object is 0 (zero) then
             Loop Dection for Path Vectors for this Peer
             is disabled.

             Otherwise, if this object has a value greater than
             zero, then Loop Dection for Path  Vectors for this
             Peer is enabled and the Path Vector Limit is this value."
         REFERENCE
            "RFC3036, LDP Specification, Section 2.8 Loop Dection,
            Section 3.4.5 Path Vector TLV."
         ::= { mplsLdpPeerEntry 3 }

     mplsLdpPeerTransportAddrType OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The type of the Internet address for the
             mplsLdpPeerTransportAddr object.  The LDP
             specification describes this as being either
             an IPv4 Transport Address or IPv6 Transport





             Address which is used in opening the LDP session's
             TCP connection, or if the optional TLV is not
             present, then this is the IPv4/IPv6 source
             address for the UPD packet carrying the Hellos.

             This object specifies how the value of the
             mplsLdpPeerTransportAddr object should be
             interpreted."
         REFERENCE
            "RFC3036, LDP Specification, Section 2.5.2
            Transport Connection Establishment and
            Section 3.5.2.1 Hello Message Procedures."
         ::= { mplsLdpPeerEntry 4 }

     mplsLdpPeerTransportAddr OBJECT-TYPE
         SYNTAX      InetAddress
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The Internet address advertised by the peer
             in the Hello Message or the Hello source address.

             The type of this address is specified by the
             value of the mplsLdpPeerTransportAddrType
             object."
         REFERENCE
            "RFC3036, LDP Specification, Section 2.5.2
            Transport Connection Establishment and
            Section 3.5.2.1 Hello Message Procedures."
         ::= { mplsLdpPeerEntry 5 }

     --
     -- The MPLS LDP Sessions Table
     --

     mplsLdpSessionTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsLdpSessionEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "A table of Sessions between the LDP Entities
             and LDP Peers.  This table AUGMENTS the
             mplsLdpPeerTable.  Each row in this table
             represents a single session."
         ::= { mplsLdpSessionObjects 3 }

     mplsLdpSessionEntry OBJECT-TYPE
         SYNTAX      MplsLdpSessionEntry





         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "An entry in this table represents information on a
             single session between an LDP Entity and LDP Peer.
             The information contained in a row is read-only.

             Please note:  the Path Vector Limit for the
             Session is the value which is configured in
             the corresponding mplsLdpEntityEntry. The
             Peer's Path Vector Limit is in the
             mplsLdpPeerPathVectorLimit object in the
             mplsLdpPeerTable.

             Values which may differ from those configured are
             noted in the objects of this table, the
             mplsLdpAtmSessionTable and the
             mplsLdpFrameRelaySessionTable. A value will
             differ if it was negotiated between the
             Entity and the Peer.  Values may or may not
             be negotiated.  For example, if the values
             are the same then no negotiation takes place.
             If they are negotiated, then they may differ."
         AUGMENTS { mplsLdpPeerEntry }
         ::= { mplsLdpSessionTable 1 }

     MplsLdpSessionEntry ::= SEQUENCE {
         mplsLdpSessionStateLastChange       TimeStamp,
         mplsLdpSessionState                 INTEGER,
         mplsLdpSessionRole                  INTEGER,
         mplsLdpSessionProtocolVersion       Unsigned32,
         mplsLdpSessionKeepAliveHoldTimeRem  TimeInterval,
         mplsLdpSessionKeepAliveTime         Unsigned32,
         mplsLdpSessionMaxPduLength          Unsigned32,
         mplsLdpSessionDiscontinuityTime     TimeStamp
     }

     mplsLdpSessionStateLastChange OBJECT-TYPE
         SYNTAX TimeStamp
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The value of sysUpTime at the time this
             Session entered its current state as
             denoted by the mplsLdpSessionState
             object."
         ::= { mplsLdpSessionEntry 1 }






     mplsLdpSessionState OBJECT-TYPE
         SYNTAX      INTEGER {
                        nonexistent(1),
                        initialized(2),
                        openrec(3),
                        opensent(4),
                        operational(5)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The current state of the session, all of the
             states 1 to 5 are based on the state machine
             for session negotiation behavior."
         REFERENCE
             "RFC3036, LDP Specification, Section 2.5.4,
             Initialization State Machine."
         ::= { mplsLdpSessionEntry 2 }

     mplsLdpSessionRole OBJECT-TYPE
         SYNTAX      INTEGER {
                        unknown(1),
                        active(2),
                        passive(3)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "During session establishment the LSR/LER takes either
             the active role or the passive role based on address
             comparisons.  This object indicates whether this LSR/LER
             was behaving in an active role or passive role during
             this session's establishment.

             The value of unknown(1), indicates that the role is not
             able to be determined at the present time."
         REFERENCE
             "RFC3036, LDP Specification, Section 2.5.3.,
             Session Initialization"
         ::= { mplsLdpSessionEntry 3 }

     mplsLdpSessionProtocolVersion OBJECT-TYPE
         SYNTAX      Unsigned32(1..65535)
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The version of the LDP Protocol which
             this session is using.  This is the version of





             the LDP protocol which has been negotiated
             during session initialization."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.3,
            Initialization Message."
         ::= { mplsLdpSessionEntry 4 }

     mplsLdpSessionKeepAliveHoldTimeRem OBJECT-TYPE
         SYNTAX      TimeInterval
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The keep alive hold time remaining for
             this session."
         ::= { mplsLdpSessionEntry 5 }

        mplsLdpSessionKeepAliveTime OBJECT-TYPE
            SYNTAX      Unsigned32 (1..65535)
            UNITS       "seconds"
            MAX-ACCESS  read-only
            STATUS      current
            DESCRIPTION
                "The negotiated KeepAlive Time which
                represents the amount of seconds between
                keep alive messages.  The
                mplsLdpEntityKeepAliveHoldTimer
                related to this Session is the
                value that was proposed as the
                KeepAlive Time for this session.

                This value is negotiated during
                session initialization between
                the entity's proposed value
                (i.e., the value configured in
                mplsLdpEntityKeepAliveHoldTimer)
                and the peer's proposed
                KeepAlive Hold Timer value.
                This value is the smaller
                of the two proposed values."
            REFERENCE
               "RFC3036, LDP Specification, Section 3.5.3,
               Initialization Message."
            ::= { mplsLdpSessionEntry 6 }

        mplsLdpSessionMaxPduLength OBJECT-TYPE
            SYNTAX      Unsigned32 (1..65535)
            UNITS       "octets"
            MAX-ACCESS  read-only





            STATUS      current
            DESCRIPTION
                "The value of maximum allowable length for LDP PDUs for
                this session.  This value may have been negotiated
                during the Session Initialization.  This object is
                related to the mplsLdpEntityMaxPduLength object.  The
                mplsLdpEntityMaxPduLength object specifies the requested
                LDP PDU length, and this object reflects the negotiated
                LDP PDU length between the Entity and
                the Peer."
            REFERENCE
               "RFC3036, LDP Specification, Section 3.5.3,
               Initialization Message."
            ::= { mplsLdpSessionEntry 7 }

     mplsLdpSessionDiscontinuityTime OBJECT-TYPE
         SYNTAX      TimeStamp
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The value of sysUpTime on the most recent occasion
             at which any one or more of this session's counters
             suffered a discontinuity.  The relevant counters are
             the specific instances associated with this session
             of any Counter32 object contained in the
             mplsLdpSessionStatsTable.

             The initial value of this object is the value of
             sysUpTime when the entry was created in this table.

             Also, a command generator can distinguish when a session
             between a given Entity and Peer goes away and a new
             session is established.  This value would change and
             thus indicate to the command generator that this is a
             different session."
         ::= { mplsLdpSessionEntry 8 }

     --
     -- The MPLS LDP Session Statistics Table
     --

     mplsLdpSessionStatsTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsLdpSessionStatsEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "A table of statistics for Sessions between
             LDP Entities and LDP Peers.  This table AUGMENTS





             the mplsLdpPeerTable."
         ::= { mplsLdpSessionObjects 4 }

     mplsLdpSessionStatsEntry OBJECT-TYPE
         SYNTAX      MplsLdpSessionStatsEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "An entry in this table represents statistical
             information on a single session between an LDP
             Entity and LDP Peer."

         AUGMENTS       { mplsLdpPeerEntry }
         ::= { mplsLdpSessionStatsTable 1 }

     MplsLdpSessionStatsEntry ::= SEQUENCE {
         mplsLdpSessionStatsUnknownMesTypeErrors  Counter32,
         mplsLdpSessionStatsUnknownTlvErrors      Counter32
     }

     mplsLdpSessionStatsUnknownMesTypeErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Unknown Message Type
             Errors detected by this LSR/LER during this session.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpSessionDiscontinuityTime."
         ::= { mplsLdpSessionStatsEntry 1 }

     mplsLdpSessionStatsUnknownTlvErrors OBJECT-TYPE
         SYNTAX      Counter32
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This object counts the number of Unknown TLV Errors
             detected by this LSR/LER during this session.

             Discontinuities in the value of this counter can occur
             at re-initialization of the management system, and at
             other times as indicated by the value of
             mplsLdpSessionDiscontinuityTime."
         ::= { mplsLdpSessionStatsEntry 2 }






     --
     -- The MPLS LDP Hello Adjacency Table
     --

     mplsLdpHelloAdjacencyObjects OBJECT IDENTIFIER ::=
                                   { mplsLdpSessionObjects 5 }

     mplsLdpHelloAdjacencyTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsLdpHelloAdjacencyEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "A table of Hello Adjacencies for Sessions."
         ::= { mplsLdpHelloAdjacencyObjects 1 }

     mplsLdpHelloAdjacencyEntry OBJECT-TYPE
         SYNTAX      MplsLdpHelloAdjacencyEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "Each row represents a single LDP Hello Adjacency.
             An LDP Session can have one or more Hello
             Adjacencies."
              INDEX       { mplsLdpEntityLdpId,
                            mplsLdpEntityIndex,
                            mplsLdpPeerLdpId,
                            mplsLdpHelloAdjacencyIndex }
         ::= { mplsLdpHelloAdjacencyTable 1 }

     MplsLdpHelloAdjacencyEntry ::= SEQUENCE {
         mplsLdpHelloAdjacencyIndex         Unsigned32,
         mplsLdpHelloAdjacencyHoldTimeRem   TimeInterval,
         mplsLdpHelloAdjacencyHoldTime      Unsigned32,
         mplsLdpHelloAdjacencyType          INTEGER
     }

     mplsLdpHelloAdjacencyIndex OBJECT-TYPE
         SYNTAX      Unsigned32 (1..4294967295)
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "An identifier for this specific adjacency."
         ::= { mplsLdpHelloAdjacencyEntry 1 }

     mplsLdpHelloAdjacencyHoldTimeRem OBJECT-TYPE
         SYNTAX      TimeInterval
         UNITS       "seconds"
         MAX-ACCESS  read-only





         STATUS      current
         DESCRIPTION
             "If the value of this object is 65535,
             this means that the hold time is infinite
             (i.e., wait forever).

             Otherwise, the time remaining for
             this Hello Adjacency to receive its
             next Hello Message.

             This interval will change when the 'next'
             Hello Message which corresponds to this
             Hello Adjacency is received unless it
             is infinite."
         ::= { mplsLdpHelloAdjacencyEntry 2 }

     mplsLdpHelloAdjacencyHoldTime OBJECT-TYPE
         SYNTAX Unsigned32 (0..65535)
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The Hello hold time which is negotiated between
             the Entity and the Peer.  The entity associated
             with this Hello Adjacency issues a proposed
             Hello Hold Time value in the
             mplsLdpEntityHelloHoldTimer object.  The peer
             also proposes a value and this object represents
             the negotiated value.

             A value of 0 means the default,
             which is 15 seconds for Link Hellos
             and 45 seconds for Targeted Hellos.
             A value of 65535 indicates an
             infinite hold time."
         REFERENCE
            "RFC3036, LDP Specification, Section 3.5.2 Hello Message"
         ::= { mplsLdpHelloAdjacencyEntry 3 }

     mplsLdpHelloAdjacencyType OBJECT-TYPE
         SYNTAX      INTEGER {
                        link(1),
                        targeted(2)
                     }
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "This adjacency is the result of a 'link'
             hello if the value of this object is link(1).





             Otherwise, it is a result of a 'targeted'
             hello, targeted(2)."
         ::= { mplsLdpHelloAdjacencyEntry 4 }

     --
     --  Session Label (LSP) Mapping to LSR MIB's
     --  In Segment LIB Information.
     --
     --
     -- NOTE: the next 2 tables map to the
     -- MPLS-LSR-STD-MIB's MplsInSegmentTable
     -- and MplsOutSegmentTable.  The
     -- cross-connect (XC) information is not
     -- represented here as it can be gleaned
     -- from the MPLS-LSR-STD-MIB.
     --

     mplsInSegmentLdpLspTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsInSegmentLdpLspEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "A table of LDP LSP's which
             map to the mplsInSegmentTable in the
             MPLS-LSR-STD-MIB module."
         ::= { mplsLdpSessionObjects 6 }

     mplsInSegmentLdpLspEntry OBJECT-TYPE
         SYNTAX      MplsInSegmentLdpLspEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "An entry in this table represents information
             on a single LDP LSP which is represented by
             a session's index triple (mplsLdpEntityLdpId,
             mplsLdpEntityIndex, mplsLdpPeerLdpId) AND the
             index for the mplsInSegmentTable
             (mplsInSegmentLdpLspLabelIndex) from the
             MPLS-LSR-STD-MIB.

             The information contained in a row is read-only."
         INDEX       { mplsLdpEntityLdpId,
                       mplsLdpEntityIndex,
                       mplsLdpPeerLdpId,
                       mplsInSegmentLdpLspIndex
                     }
         ::= { mplsInSegmentLdpLspTable 1 }






     MplsInSegmentLdpLspEntry ::= SEQUENCE {
         mplsInSegmentLdpLspIndex                 MplsIndexType,
         mplsInSegmentLdpLspLabelType             MplsLdpLabelType,
         mplsInSegmentLdpLspType                  MplsLspType
     }

     mplsInSegmentLdpLspIndex OBJECT-TYPE
         SYNTAX        MplsIndexType
         MAX-ACCESS    not-accessible
         STATUS        current
         DESCRIPTION
             "This contains the same value as the
             mplsInSegmentIndex in the
             MPLS-LSR-STD-MIB's mplsInSegmentTable."
         ::= { mplsInSegmentLdpLspEntry 1 }

     mplsInSegmentLdpLspLabelType  OBJECT-TYPE
         SYNTAX        MplsLdpLabelType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The Layer 2 Label Type."
         ::= { mplsInSegmentLdpLspEntry 2 }

     mplsInSegmentLdpLspType OBJECT-TYPE
         SYNTAX        MplsLspType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The type of LSP connection."
         ::= { mplsInSegmentLdpLspEntry 3 }

     --
     --  Session Label (LSP) Mapping to LSR MIB's
     --  Out Segment LIB Information.
     --

     mplsOutSegmentLdpLspTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsOutSegmentLdpLspEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "A table of LDP LSP's which
             map to the mplsOutSegmentTable in the
            MPLS-LSR-STD-MIB."
         ::= { mplsLdpSessionObjects 7 }

     mplsOutSegmentLdpLspEntry OBJECT-TYPE





         SYNTAX      MplsOutSegmentLdpLspEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "An entry in this table represents information
             on a single LDP LSP which is represented by
             a session's index triple (mplsLdpEntityLdpId,
             mplsLdpEntityIndex, mplsLdpPeerLdpId) AND the
             index (mplsOutSegmentLdpLspIndex)
             for the mplsOutSegmentTable.

             The information contained in a row is read-only."
         INDEX       { mplsLdpEntityLdpId,
                       mplsLdpEntityIndex,
                       mplsLdpPeerLdpId,
                       mplsOutSegmentLdpLspIndex
                     }
         ::= { mplsOutSegmentLdpLspTable 1 }

     MplsOutSegmentLdpLspEntry ::= SEQUENCE {
         mplsOutSegmentLdpLspIndex                 MplsIndexType,
         mplsOutSegmentLdpLspLabelType             MplsLdpLabelType,
         mplsOutSegmentLdpLspType                  MplsLspType
     }

     mplsOutSegmentLdpLspIndex OBJECT-TYPE
         SYNTAX       MplsIndexType
         MAX-ACCESS   not-accessible
         STATUS       current
         DESCRIPTION
             "This contains the same value as the
             mplsOutSegmentIndex in the
             MPLS-LSR-STD-MIB's mplsOutSegmentTable."
         ::= { mplsOutSegmentLdpLspEntry 1 }

     mplsOutSegmentLdpLspLabelType  OBJECT-TYPE
         SYNTAX        MplsLdpLabelType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION
             "The Layer 2 Label Type."
         ::= { mplsOutSegmentLdpLspEntry 2 }

     mplsOutSegmentLdpLspType OBJECT-TYPE
         SYNTAX        MplsLspType
         MAX-ACCESS    read-only
         STATUS        current
         DESCRIPTION





             "The type of LSP connection."
         ::= { mplsOutSegmentLdpLspEntry 3 }

     --
     -- Mpls FEC Table
     --

     mplsFecObjects OBJECT IDENTIFIER ::=
                                { mplsLdpSessionObjects 8 }

     mplsFecLastChange OBJECT-TYPE
         SYNTAX  TimeStamp
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
             "The value of sysUpTime at the time of the most
             recent addition/deletion of an entry
             to/from the mplsLdpFectTable or
             the most recent change in values to any objects
             in the mplsLdpFecTable.

             If no such changes have occurred since the last
             re-initialization of the local management subsystem,
             then this object contains a zero value."
        ::= { mplsFecObjects 1 }

     mplsFecIndexNext  OBJECT-TYPE
         SYNTAX         IndexIntegerNextFree
         MAX-ACCESS     read-only
         STATUS         current
         DESCRIPTION
             "This object contains an appropriate value to
             be used for mplsFecIndex when creating
             entries in the mplsFecTable. The value
             0 indicates that no unassigned entries are
             available."
        ::= { mplsFecObjects 2 }

     mplsFecTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsFecEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "This table represents the FEC
             (Forwarding Equivalence Class)
             Information associated with an LSP."
         ::= { mplsFecObjects 3 }






     mplsFecEntry OBJECT-TYPE
         SYNTAX      MplsFecEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "Each row represents a single FEC Element."
         INDEX       { mplsFecIndex }
         ::= { mplsFecTable 1 }

     MplsFecEntry ::= SEQUENCE {
         mplsFecIndex               IndexInteger,
         mplsFecType                INTEGER,
         mplsFecAddrPrefixLength    InetAddressPrefixLength,
         mplsFecAddrType            InetAddressType,
         mplsFecAddr                InetAddress,
         mplsFecStorageType         StorageType,
         mplsFecRowStatus           RowStatus
     }

     mplsFecIndex OBJECT-TYPE
         SYNTAX      IndexInteger
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "The index which uniquely identifies this entry."
         ::= { mplsFecEntry 1 }

     mplsFecType  OBJECT-TYPE
         SYNTAX      INTEGER {
                        prefix(1),
                        hostAddress(2)
                     }
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The type of the FEC.  If the value of this object
             is 'prefix(1)' then the FEC type described by this
             row is an address prefix.

             If the value of this object is 'hostAddress(2)' then
             the FEC type described by this row is a host address."
         REFERENCE
             "RFC3036, Section 3.4.1. FEC TLV."
         ::= { mplsFecEntry 2 }

     mplsFecAddrType  OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  read-create





         STATUS      current
         DESCRIPTION
             "The value of this object is the type of the
             Internet address.  The value of this object,
             decides how the value of the mplsFecAddr object
             is interpreted."
         REFERENCE
             "RFC3036, Section 3.4.1. FEC TLV."
         ::= { mplsFecEntry 4 }

     mplsFecAddr     OBJECT-TYPE
         SYNTAX      InetAddress
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The value of this object is interpreted based
             on the value of the 'mplsFecAddrType' object.

             This address is then further interpretted as
             an being used with the address prefix,
             or as the host address.  This further interpretation
             is indicated by the 'mplsFecType' object.
             In other words, the FEC element is populated
             according to the Prefix FEC Element value encoding, or
             the Host Address FEC Element encoding."
         REFERENCE
             "RFC3036, Section 3.4.1 FEC TLV."
         ::= { mplsFecEntry 5 }

     mplsFecAddrPrefixLength  OBJECT-TYPE
         SYNTAX      InetAddressPrefixLength
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "If the value of the 'mplsFecType' is 'hostAddress(2)'
             then this object is undefined.

             If the value of 'mplsFecType' is 'prefix(1)'
             then the value of this object is the length in
             bits of the address prefix represented by
             'mplsFecAddr', or zero.  If the value of this
             object is zero, this indicates that the
             prefix matches all addresses.  In this case the
             address prefix MUST also be zero (i.e., 'mplsFecAddr'
             should have the value of zero.)"
         REFERENCE
             "RFC3036, Section 3.4.1. FEC TLV."
         DEFVAL { 0 }





         ::= { mplsFecEntry 3 }

     mplsFecStorageType  OBJECT-TYPE
         SYNTAX      StorageType
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The storage type for this conceptual row.
             Conceptual rows having the value 'permanent(4)'
             need not allow write-access to any columnar
             objects in the row."
         DEFVAL { nonVolatile }
         ::= { mplsFecEntry 6 }

     mplsFecRowStatus OBJECT-TYPE
         SYNTAX      RowStatus
         MAX-ACCESS  read-create
         STATUS      current
         DESCRIPTION
             "The status of this conceptual row.  If the value of this
             object is 'active(1)', then none of the writable objects
             of this entry can be modified, except to set this object
             to 'destroy(6)'.

             NOTE: if this row is being referenced by any entry in
             the mplsLdpLspFecTable, then a request to destroy
             this row, will result in an inconsistentValue error."
         ::= { mplsFecEntry 7 }

     --
     --  LDP LSP FEC Table
     --

     mplsLdpLspFecLastChange OBJECT-TYPE
        SYNTAX TimeStamp
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
             "The value of sysUpTime at the time of the most
             recent addition/deletion of an entry
             to/from the mplsLdpLspFecTable or
             the most recent change in values to any objects in the
             mplsLdpLspFecTable.

             If no such changes have occurred since the last
             re-initialization of the local management subsystem,
             then this object contains a zero value."
       ::= { mplsLdpSessionObjects 9 }





     mplsLdpLspFecTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF MplsLdpLspFecEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
           "A table which shows the relationship between
           LDP LSPs and FECs.  Each row represents
           a single LDP LSP to FEC association."
       ::= { mplsLdpSessionObjects 10 }

     mplsLdpLspFecEntry OBJECT-TYPE
        SYNTAX     MplsLdpLspFecEntry
        MAX-ACCESS not-accessible
        STATUS     current
        DESCRIPTION
           "An entry represents a LDP LSP
           to FEC association."
        INDEX       { mplsLdpEntityLdpId,
                      mplsLdpEntityIndex,
                      mplsLdpPeerLdpId,
                      mplsLdpLspFecSegment,
                      mplsLdpLspFecSegmentIndex,
                      mplsLdpLspFecIndex
                     }
        ::= { mplsLdpLspFecTable 1 }

     MplsLdpLspFecEntry ::= SEQUENCE {
        mplsLdpLspFecSegment       INTEGER,
        mplsLdpLspFecSegmentIndex  MplsIndexType,
        mplsLdpLspFecIndex         IndexInteger,
        mplsLdpLspFecStorageType   StorageType,
        mplsLdpLspFecRowStatus     RowStatus
     }

     mplsLdpLspFecSegment OBJECT-TYPE
         SYNTAX INTEGER {
                            inSegment(1),
                            outSegment(2)
                        }
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
            "If the value is inSegment(1), then this
            indicates that the following index,
            mplsLdpLspFecSegmentIndex, contains the same
            value as the mplsInSegmentLdpLspIndex.

            Otherwise, if the value of this object is





            outSegment(2),  then this
            indicates that following index,
            mplsLdpLspFecSegmentIndex, contains the same
            value as the mplsOutSegmentLdpLspIndex."
         ::= { mplsLdpLspFecEntry 1 }

     mplsLdpLspFecSegmentIndex OBJECT-TYPE
         SYNTAX      MplsIndexType
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
            "This index is interpretted by using the value
            of the mplsLdpLspFecSegment.

            If the mplsLdpLspFecSegment is inSegment(1),
            then this index has the same value as
            mplsInSegmentLdpLspIndex.

            If the mplsLdpLspFecSegment is outSegment(2),
            then this index has the same value as
            mplsOutSegmentLdpLspIndex."
         ::= { mplsLdpLspFecEntry 2 }

     mplsLdpLspFecIndex   OBJECT-TYPE
         SYNTAX      IndexInteger
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "This index identifies the FEC entry in the
             mplsFecTable associated with this session.
             In other words, the value of this index
             is the same as the value of the mplsFecIndex
             that denotes the FEC associated with this
             Session."
         ::= { mplsLdpLspFecEntry 3 }

     mplsLdpLspFecStorageType  OBJECT-TYPE
        SYNTAX      StorageType
        MAX-ACCESS  read-create
        STATUS      current
        DESCRIPTION
            "The storage type for this conceptual row.
            Conceptual rows having the value 'permanent(4)'
            need not allow write-access to any columnar
            objects in the row."
        DEFVAL { nonVolatile }
        ::= { mplsLdpLspFecEntry 4 }






     mplsLdpLspFecRowStatus  OBJECT-TYPE
        SYNTAX     RowStatus
        MAX-ACCESS read-create
        STATUS     current
        DESCRIPTION
            "The status of this conceptual row.  If the
             value of this object is 'active(1)', then
             none of the writable objects of this entry
             can be modified.

             The Agent should delete this row when
             the session ceases to exist.  If an
             operator wants to associate the session with
             a different FEC, the recommended
             procedure is (as described in detail in the section
             entitled, 'Changing Values After Session
             Establishment', and again described in the
             DESCRIPTION clause of the
             mplsLdpEntityAdminStatus object)
             is to set the mplsLdpEntityAdminStatus to
             down, thereby explicitly causing a session
             to be torn down. This will also
             cause this entry to be deleted.

             Then, set the mplsLdpEntityAdminStatus
             to enable which enables a new session to be initiated.
             Once the session is initiated, an entry may be
             added to this table to associate the new session
             with a FEC."
        ::= { mplsLdpLspFecEntry 5 }

     --
     -- Address Message/Address Withdraw Message Information
     --
     -- This information is associated with a specific Session
     -- because Label Address Messages are sent after session
     -- initialization has taken place.
     --

     mplsLdpSessionPeerAddrTable OBJECT-TYPE
         SYNTAX      SEQUENCE OF MplsLdpSessionPeerAddrEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "This table 'extends' the mplsLdpSessionTable.
             This table is used to store Label Address Information
             from Label Address Messages received by this LSR from
             Peers.  This table is read-only and should be updated





             when Label Withdraw Address Messages are received, i.e.,
             Rows should be deleted as appropriate.

             NOTE:  since more than one address may be contained
             in a Label Address Message, this table 'sparse augments',
             the mplsLdpSessionTable's information."
         ::= { mplsLdpSessionObjects 11 }

     mplsLdpSessionPeerAddrEntry OBJECT-TYPE
         SYNTAX      MplsLdpSessionPeerAddrEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "An entry in this table represents information on
             a session's single next hop address which was
             advertised in an Address Message from the LDP peer.
             The information contained in a row is read-only."
         INDEX       { mplsLdpEntityLdpId,
                       mplsLdpEntityIndex,
                       mplsLdpPeerLdpId,
                       mplsLdpSessionPeerAddrIndex
                     }
         ::= { mplsLdpSessionPeerAddrTable 1 }

     MplsLdpSessionPeerAddrEntry ::= SEQUENCE {
         mplsLdpSessionPeerAddrIndex       Unsigned32,
         mplsLdpSessionPeerNextHopAddrType InetAddressType,
         mplsLdpSessionPeerNextHopAddr     InetAddress
     }

     mplsLdpSessionPeerAddrIndex OBJECT-TYPE
         SYNTAX      Unsigned32 (1..4294967295)
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
             "An index which uniquely identifies this entry within
             a given session."
         ::= { mplsLdpSessionPeerAddrEntry 1 }

     mplsLdpSessionPeerNextHopAddrType OBJECT-TYPE
         SYNTAX      InetAddressType
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The internetwork layer address type of this Next Hop
             Address as specified in the Label Address Message
             associated with this Session. The value of this
             object indicates how to interpret the value of





             mplsLdpSessionPeerNextHopAddr."
         ::= { mplsLdpSessionPeerAddrEntry 2 }

     mplsLdpSessionPeerNextHopAddr OBJECT-TYPE
         SYNTAX      InetAddress
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
             "The next hop address.  The type of this address
             is specified by the value of the
             mplsLdpSessionPeerNextHopAddrType."
         REFERENCE
             "RFC3036, Section 2.7. LDP Identifiers
             and Next Hop Addresses"
            ::= { mplsLdpSessionPeerAddrEntry 3 }

     ---
     --- Notifications
     ---

     mplsLdpInitSessionThresholdExceeded NOTIFICATION-TYPE
          OBJECTS     {
                        mplsLdpEntityInitSessionThreshold
                      }
          STATUS      current
          DESCRIPTION
             "This notification is generated when the value of
             the 'mplsLdpEntityInitSessionThreshold' object
             is not zero, and the number of Session
             Initialization messages exceeds the value
             of the 'mplsLdpEntityInitSessionThreshold' object."
          ::= { mplsLdpNotifications 1 }

     mplsLdpPathVectorLimitMismatch NOTIFICATION-TYPE
          OBJECTS     {
                        mplsLdpEntityPathVectorLimit,
                        mplsLdpPeerPathVectorLimit
                      }
          STATUS      current
          DESCRIPTION
             "This notification is sent when the
             'mplsLdpEntityPathVectorLimit' does NOT match
             the value of the 'mplsLdpPeerPathVectorLimit' for
             a specific Entity."
          REFERENCE
             "RFC3036, LDP Specification, Section 3.5.3."
          ::= { mplsLdpNotifications 2 }






     mplsLdpSessionUp NOTIFICATION-TYPE
          OBJECTS     {
                         mplsLdpSessionState,
                         mplsLdpSessionDiscontinuityTime,
                         mplsLdpSessionStatsUnknownMesTypeErrors,
                         mplsLdpSessionStatsUnknownTlvErrors
                      }
          STATUS      current
          DESCRIPTION
             "If this notification is sent when the
             value of 'mplsLdpSessionState' enters
             the 'operational(5)' state."
          ::= { mplsLdpNotifications 3 }

     mplsLdpSessionDown NOTIFICATION-TYPE
          OBJECTS     {
                         mplsLdpSessionState,
                         mplsLdpSessionDiscontinuityTime,
                         mplsLdpSessionStatsUnknownMesTypeErrors,
                         mplsLdpSessionStatsUnknownTlvErrors

                      }
          STATUS      current
          DESCRIPTION
             "This notification is sent when the
             value of 'mplsLdpSessionState' leaves
             the 'operational(5)' state."
          ::= { mplsLdpNotifications 4 }

     --****************************************************************
     -- Module Conformance Statement
     --****************************************************************

     mplsLdpGroups
         OBJECT IDENTIFIER ::= { mplsLdpConformance 1 }

     mplsLdpCompliances
         OBJECT IDENTIFIER ::= { mplsLdpConformance 2 }

     --
     -- Full Compliance
     --

     mplsLdpModuleFullCompliance MODULE-COMPLIANCE
         STATUS current
         DESCRIPTION
             "The Module is implemented with support
             for read-create and read-write.  In other





             words, both monitoring and configuration
             are available when using this MODULE-COMPLIANCE."

         MODULE -- this module
             MANDATORY-GROUPS    { mplsLdpGeneralGroup,
                                   mplsLdpNotificationsGroup
                                 }
         GROUP mplsLdpLspGroup
         DESCRIPTION
             "This group must be supported if the LSR MIB is
             implemented, specifically the mplsInSegmentTable,
             the mplsOutSegmentTable or the mplsXCTable."

         OBJECT mplsLdpEntityTargetPeerAddrType
         SYNTAX InetAddressType { unknown(0), ipv4(1), ipv6(2) }
         DESCRIPTION
            "An implementation is only required to support
            'unknown(0)', IPv4 and globally unique IPv6 addresses."

         OBJECT mplsLdpEntityTargetPeerAddr
         SYNTAX InetAddress (SIZE(0|4|16))
         DESCRIPTION
             "An implementation is only required to support IPv4 and
             globally unique IPv6 addresses."

         OBJECT mplsLdpEntityRowStatus
         SYNTAX RowStatus { active(1) }
         WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for createAndWait and notInService is not
             required."

         OBJECT mplsFecAddrType
         SYNTAX InetAddressType { unknown(0), ipv4(1), ipv6(2) }
         DESCRIPTION
            "An implementation is only required to support
            'unknown(0)', IPv4 and globally unique IPv6 addresses."

         OBJECT mplsFecAddr
         SYNTAX InetAddress (SIZE(0|4|16))
         DESCRIPTION
             "An implementation is only required to support IPv4 and
             globally unique IPv6 addresses."

         OBJECT mplsFecRowStatus
         SYNTAX RowStatus { active(1) }
         WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
         DESCRIPTION





             "Support for createAndWait and notInService is not
             required."

         OBJECT mplsLdpLspFecRowStatus
         SYNTAX RowStatus { active(1) }
         WRITE-SYNTAX RowStatus { createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for createAndWait and notInService is not
             required."

         OBJECT mplsLdpSessionPeerNextHopAddrType
         SYNTAX InetAddressType { unknown(0), ipv4(1), ipv6(2) }
         DESCRIPTION
             "An implementation is only required to support
             'unknown(0)', IPv4 and globally unique IPv6 addresses."

         OBJECT mplsLdpSessionPeerNextHopAddr
         SYNTAX InetAddress (SIZE(0|4|16))
         DESCRIPTION
             "An implementation is only required to support IPv4
             and globally unique IPv6 addresses."

         ::= { mplsLdpCompliances 1 }

     --
     -- Read-Only Compliance
     --

     mplsLdpModuleReadOnlyCompliance MODULE-COMPLIANCE
         STATUS current
         DESCRIPTION
             "The Module is implemented with support
             for read-only.  In other words, only monitoring
             is available by implementing this MODULE-COMPLIANCE."

         MODULE -- this module
             MANDATORY-GROUPS    { mplsLdpGeneralGroup,
                                   mplsLdpNotificationsGroup
                                 }

         GROUP mplsLdpLspGroup
         DESCRIPTION
             "This group must be supported if the LSR MIB is
             implemented, specifically the mplsInSegmentTable,
             the mplsOutSegmentTable or the mplsXCTable."

         OBJECT       mplsLdpEntityProtocolVersion
         MIN-ACCESS   read-only





         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityAdminStatus
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityTcpPort
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityUdpDscPort
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityMaxPduLength
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityKeepAliveHoldTimer
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityHelloHoldTimer
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityInitSessionThreshold
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityLabelDistMethod
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityLabelRetentionMode
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."






         OBJECT       mplsLdpEntityPathVectorLimit
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityHopCountLimit
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityTransportAddrKind
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityTargetPeer
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityTargetPeerAddrType
         SYNTAX       InetAddressType { unknown(0), ipv4(1), ipv6(2) }
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required.
            An implementation is only required to support
            'unknown(0)', IPv4 and globally unique IPv6 addresses."

         OBJECT       mplsLdpEntityTargetPeerAddr
         SYNTAX       InetAddress (SIZE(0|4|16))
         MIN-ACCESS   read-only
         DESCRIPTION
             "Write access is not required.
             An implementation is only required to support IPv4 and
             globally unique IPv6 addresses."

         OBJECT       mplsLdpEntityLabelType
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsLdpEntityStorageType
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT mplsLdpEntityRowStatus
         SYNTAX RowStatus { active(1) }





         MIN-ACCESS   read-only
         DESCRIPTION
             "Write access is not required, and active is the
             only status that needs to be supported."

         OBJECT       mplsFecType
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsFecAddrPrefixLength
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT       mplsFecAddrType
         SYNTAX       InetAddressType { unknown(0), ipv4(1), ipv6(2) }
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required.
            An implementation is only required to support
            'unknown(0)', IPv4 and globally unique IPv6 addresses."

         OBJECT        mplsFecAddr
         SYNTAX        InetAddress (SIZE(0|4|16))
         MIN-ACCESS    read-only
         DESCRIPTION
             "Write access is not required.
             An implementation is only required to support IPv4 and
             globally unique IPv6 addresses."

         OBJECT       mplsFecStorageType
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."

         OBJECT mplsFecRowStatus
         SYNTAX RowStatus { active(1) }
         MIN-ACCESS   read-only
         DESCRIPTION
             "Write access is not required, and active is the
             only status that needs to be supported."

         OBJECT       mplsLdpLspFecStorageType
         MIN-ACCESS   read-only
         DESCRIPTION
            "Write access is not required."






         OBJECT mplsLdpLspFecRowStatus
         SYNTAX RowStatus { active(1) }
         MIN-ACCESS   read-only
         DESCRIPTION
             "Write access is not required, and active is the
             only status that needs to be supported."

         OBJECT mplsLdpSessionPeerNextHopAddrType
         SYNTAX InetAddressType { unknown(0), ipv4(1), ipv6(2) }
         DESCRIPTION
            "An implementation is only required to support
            'unknown(0)', IPv4 and globally unique IPv6 addresses."


         OBJECT mplsLdpSessionPeerNextHopAddr
         SYNTAX InetAddress (SIZE(0|4|16))
         DESCRIPTION
             "An implementation is only required to support IPv4
             and globally unique IPv6 addresses."

         ::= { mplsLdpCompliances 2 }

     -- units of conformance

     mplsLdpGeneralGroup OBJECT-GROUP
         OBJECTS {
         mplsLdpLsrId,
         mplsLdpLsrLoopDetectionCapable,
         mplsLdpEntityLastChange,
         mplsLdpEntityIndexNext,
         mplsLdpEntityProtocolVersion,
         mplsLdpEntityAdminStatus,
         mplsLdpEntityOperStatus,
         mplsLdpEntityTcpPort,
         mplsLdpEntityUdpDscPort,
         mplsLdpEntityMaxPduLength,
         mplsLdpEntityKeepAliveHoldTimer,
         mplsLdpEntityHelloHoldTimer,
         mplsLdpEntityInitSessionThreshold,
         mplsLdpEntityLabelDistMethod,
         mplsLdpEntityLabelRetentionMode,
         mplsLdpEntityPathVectorLimit,
         mplsLdpEntityHopCountLimit,
         mplsLdpEntityTransportAddrKind,
         mplsLdpEntityTargetPeer,
         mplsLdpEntityTargetPeerAddrType,
         mplsLdpEntityTargetPeerAddr,
         mplsLdpEntityLabelType,





         mplsLdpEntityDiscontinuityTime,
         mplsLdpEntityStorageType,
         mplsLdpEntityRowStatus,
         mplsLdpEntityStatsSessionAttempts,
         mplsLdpEntityStatsSessionRejectedNoHelloErrors,
         mplsLdpEntityStatsSessionRejectedAdErrors,
         mplsLdpEntityStatsSessionRejectedMaxPduErrors,
         mplsLdpEntityStatsSessionRejectedLRErrors,
         mplsLdpEntityStatsBadLdpIdentifierErrors,
         mplsLdpEntityStatsBadPduLengthErrors,
         mplsLdpEntityStatsBadMessageLengthErrors,
         mplsLdpEntityStatsBadTlvLengthErrors,
         mplsLdpEntityStatsMalformedTlvValueErrors,
         mplsLdpEntityStatsKeepAliveTimerExpErrors,
         mplsLdpEntityStatsShutdownReceivedNotifications,
         mplsLdpEntityStatsShutdownSentNotifications,
         mplsLdpPeerLastChange,
         mplsLdpPeerLabelDistMethod,
         mplsLdpPeerPathVectorLimit,
         mplsLdpPeerTransportAddrType,
         mplsLdpPeerTransportAddr,
         mplsLdpHelloAdjacencyHoldTimeRem,
         mplsLdpHelloAdjacencyHoldTime,
         mplsLdpHelloAdjacencyType,
         mplsLdpSessionStateLastChange,
         mplsLdpSessionState,
         mplsLdpSessionRole,
         mplsLdpSessionProtocolVersion,
         mplsLdpSessionKeepAliveHoldTimeRem,
         mplsLdpSessionKeepAliveTime,
         mplsLdpSessionMaxPduLength,
         mplsLdpSessionDiscontinuityTime,
         mplsLdpSessionStatsUnknownMesTypeErrors,
         mplsLdpSessionStatsUnknownTlvErrors,
         mplsLdpSessionPeerNextHopAddrType,
         mplsLdpSessionPeerNextHopAddr,
         mplsFecLastChange,
         mplsFecIndexNext,
         mplsFecType,
         mplsFecAddrType,
         mplsFecAddr,
         mplsFecAddrPrefixLength,
         mplsFecStorageType,
         mplsFecRowStatus
         }
         STATUS    current
         DESCRIPTION
             "Objects that apply to all MPLS LDP implementations."





         ::= { mplsLdpGroups 1 }

     mplsLdpLspGroup OBJECT-GROUP
         OBJECTS {
         mplsInSegmentLdpLspLabelType,
         mplsInSegmentLdpLspType,
         mplsOutSegmentLdpLspLabelType,
         mplsOutSegmentLdpLspType,
         mplsLdpLspFecLastChange,
         mplsLdpLspFecStorageType,
         mplsLdpLspFecRowStatus
         }
         STATUS    current
         DESCRIPTION
             "These objects are for LDP implementations
             which interface to the Label Information Base (LIB)
             in the MPLS-LSR-STD-MIB.  The LIB is
             represented in the mplsInSegmentTable,
             mplsOutSegmentTable and mplsXCTable."
         ::= { mplsLdpGroups 2 }

     mplsLdpNotificationsGroup NOTIFICATION-GROUP
         NOTIFICATIONS { mplsLdpInitSessionThresholdExceeded,
                         mplsLdpPathVectorLimitMismatch,
                         mplsLdpSessionUp,
                         mplsLdpSessionDown
                            }
         STATUS   current
         DESCRIPTION
             "The notification for an MPLS LDP implementation."
         ::= { mplsLdpGroups 3 }

     END


