RADIUS-AUTH-SERVER-MIB DEFINITIONS ::= BEGIN


   IMPORTS
          MODULE-IDENTITY, OBJECT-TYPE, OBJECT-IDENTITY,
          Counter32, Integer32,
          IpAddress, TimeTicks, mib-2      FROM SNMPv2-SMI
          SnmpAdminString                  FROM SNMP-FRAMEWORK-MIB
          InetAddressType, InetAddress     FROM INET-ADDRESS-MIB
          MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF;

   radiusAuthServMIB MODULE-IDENTITY
          LAST-UPDATED "200608210000Z"  -- 21 August 2006
          ORGANIZATION "IETF RADIUS Extensions Working Group."
          CONTACT-INFO
                 " Bernard Aboba
                   Microsoft
                   One Microsoft Way
                   Redmond, WA  98052
                   US
                   Phone: +1 425 936 6605





                   EMail: bernarda@microsoft.com"
          DESCRIPTION
                "The MIB module for entities implementing the server
                 side of the Remote Authentication Dial-In User
                 Service (RADIUS) authentication protocol.  Copyright
                 (C) The Internet Society (2006).  This version of this
                 MIB module is part of RFC 4669; see the RFC itself for
                 full legal notices."
          REVISION "200608210000Z"  -- 21 August 2006
          DESCRIPTION
                "Revised version as published in RFC 4669.  This
                 version obsoletes that of RFC 2619 by deprecating the
                 MIB table containing IPv4-only address formats and
                 defining a new table to add support for version-neutral
                 IP address formats.  The remaining MIB objects from RFC
                 2619 are carried forward into this version."
          REVISION "199906110000Z"  -- 11 Jun 1999
          DESCRIPTION "Initial version as published in RFC 2619."
          ::= { radiusAuthentication 1 }

   radiusMIB  OBJECT-IDENTITY
          STATUS  current
          DESCRIPTION
                "The OID assigned to RADIUS MIB work by the IANA."
           ::= { mib-2 67 }

   radiusAuthentication  OBJECT IDENTIFIER ::= {radiusMIB 1}

   radiusAuthServMIBObjects OBJECT IDENTIFIER
           ::= { radiusAuthServMIB 1 }

   radiusAuthServ  OBJECT IDENTIFIER
           ::= { radiusAuthServMIBObjects 1 }

   radiusAuthServIdent OBJECT-TYPE
          SYNTAX      SnmpAdminString
          MAX-ACCESS  read-only
          STATUS      current
          DESCRIPTION
                "The implementation identification string for the
                 RADIUS authentication server software in use on the
                 system, for example, 'FNS-2.1'."
          ::= {radiusAuthServ 1}

   radiusAuthServUpTime OBJECT-TYPE
          SYNTAX      TimeTicks
          MAX-ACCESS  read-only
          STATUS      current





          DESCRIPTION
                "If the server has a persistent state (e.g., a
                 process), this value will be the time elapsed (in
                 hundredths of a second) since the server process
                 was started.  For software without persistent state,
                 this value will be zero."
          ::= {radiusAuthServ 2}

   radiusAuthServResetTime OBJECT-TYPE
          SYNTAX      TimeTicks
          MAX-ACCESS  read-only
          STATUS      current
          DESCRIPTION
                "If the server has a persistent state (e.g., a process)
                 and supports a 'reset' operation (e.g., can be told to
                 re-read configuration files), this value will be the
                 time elapsed (in hundredths of a second) since the
                 server was 'reset.'  For software that does not
                 have persistence or does not support a 'reset'
                 operation, this value will be zero."
          ::= {radiusAuthServ 3}

   radiusAuthServConfigReset OBJECT-TYPE
          SYNTAX INTEGER { other(1),
                           reset(2),
                           initializing(3),
                           running(4)}
          MAX-ACCESS  read-write
          STATUS      current
          DESCRIPTION
                 "Status/action object to reinitialize any persistent
                  server state.  When set to reset(2), any persistent
                  server state (such as a process) is reinitialized as
                  if the server had just been started.  This value will
                  never be returned by a read operation.  When read,
                  one of the following values will be returned:
                      other(1) - server in some unknown state;
                      initializing(3) - server (re)initializing;
                      running(4) - server currently running."
          ::= {radiusAuthServ 4}

   radiusAuthServTotalAccessRequests OBJECT-TYPE
           SYNTAX Counter32
           UNITS "packets"
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
                  "The number of packets received on the





                   authentication port."
           REFERENCE "RFC 2865 section 4.1"
           ::= { radiusAuthServ 5}

   radiusAuthServTotalInvalidRequests OBJECT-TYPE
           SYNTAX Counter32
           UNITS "packets"
           MAX-ACCESS read-only
           STATUS current
           DESCRIPTION
                 "The number of RADIUS Access-Request packets
                  received from unknown addresses."
           REFERENCE "RFC 2865 section 4.1"
           ::= { radiusAuthServ 6 }

   radiusAuthServTotalDupAccessRequests OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                "The number of duplicate RADIUS Access-Request
                 packets received."
          REFERENCE "RFC 2865 section 4.1"
          ::= { radiusAuthServ 7 }

   radiusAuthServTotalAccessAccepts OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                "The number of RADIUS Access-Accept packets sent."
          REFERENCE "RFC 2865 section 4.2"
          ::= { radiusAuthServ 8 }

   radiusAuthServTotalAccessRejects OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Reject packets sent."
         REFERENCE "RFC 2865 section 4.3"
         ::= { radiusAuthServ 9 }

   radiusAuthServTotalAccessChallenges OBJECT-TYPE
         SYNTAX Counter32





         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Challenge packets sent."
         REFERENCE "RFC 2865 section 4.4"
         ::= { radiusAuthServ 10 }

   radiusAuthServTotalMalformedAccessRequests OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of malformed RADIUS Access-Request
                packets received.  Bad authenticators
                and unknown types are not included as
                malformed Access-Requests."
         REFERENCE "RFC 2865 section 4.1"
         ::= { radiusAuthServ 11 }

   radiusAuthServTotalBadAuthenticators OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Authentication-Request packets
                that contained invalid Message Authenticator
                attributes received."
         REFERENCE "RFC 2865 section 3"
         ::= { radiusAuthServ 12 }

   radiusAuthServTotalPacketsDropped OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of incoming packets
                silently discarded for some reason other
                than malformed, bad authenticators or
                unknown types."
         REFERENCE "RFC 2865 section 3"
         ::= { radiusAuthServ 13 }

   radiusAuthServTotalUnknownTypes OBJECT-TYPE
         SYNTAX Counter32





         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS packets of unknown type that
                were received."
         REFERENCE "RFC 2865 section 4"
         ::= { radiusAuthServ 14 }


   radiusAuthClientTable OBJECT-TYPE
          SYNTAX     SEQUENCE OF RadiusAuthClientEntry
          MAX-ACCESS not-accessible
          STATUS     deprecated
          DESCRIPTION
                "The (conceptual) table listing the RADIUS
                 authentication clients with which the server shares
                 a secret."
          ::= { radiusAuthServ 15 }


   radiusAuthClientEntry OBJECT-TYPE
          SYNTAX     RadiusAuthClientEntry
          MAX-ACCESS not-accessible
          STATUS     deprecated
          DESCRIPTION
                "An entry (conceptual row) representing a RADIUS
                 authentication client with which the server shares a
                 secret."
          INDEX      { radiusAuthClientIndex }
          ::= { radiusAuthClientTable 1 }

   RadiusAuthClientEntry ::= SEQUENCE {
          radiusAuthClientIndex                           Integer32,
          radiusAuthClientAddress                         IpAddress,
          radiusAuthClientID                        SnmpAdminString,
          radiusAuthServAccessRequests                    Counter32,
          radiusAuthServDupAccessRequests                 Counter32,
          radiusAuthServAccessAccepts                     Counter32,
          radiusAuthServAccessRejects                     Counter32,
          radiusAuthServAccessChallenges                  Counter32,
          radiusAuthServMalformedAccessRequests           Counter32,
          radiusAuthServBadAuthenticators                 Counter32,
          radiusAuthServPacketsDropped                    Counter32,
          radiusAuthServUnknownTypes                      Counter32
   }

   radiusAuthClientIndex OBJECT-TYPE





          SYNTAX     Integer32 (1..2147483647)
          MAX-ACCESS not-accessible
          STATUS     deprecated
          DESCRIPTION
                "A number uniquely identifying each RADIUS
                 authentication client with which this server
                 communicates."
          ::= { radiusAuthClientEntry 1 }

   radiusAuthClientAddress OBJECT-TYPE
          SYNTAX     IpAddress
          MAX-ACCESS read-only
          STATUS     deprecated
          DESCRIPTION
                "The NAS-IP-Address of the RADIUS authentication client
                 referred to in this table entry."
          REFERENCE "RFC 2865 section 2"
          ::= { radiusAuthClientEntry 2 }

   radiusAuthClientID OBJECT-TYPE
          SYNTAX     SnmpAdminString
          MAX-ACCESS read-only
          STATUS     deprecated
          DESCRIPTION
                "The NAS-Identifier of the RADIUS authentication client
                 referred to in this table entry.  This is not
                 necessarily the same as sysName in MIB II."
          REFERENCE "RFC 2865 section 5.32"
          ::= { radiusAuthClientEntry 3 }

   -- Server Counters

   --
   -- Responses = AccessAccepts + AccessRejects + AccessChallenges
   --
   -- Requests - DupRequests - BadAuthenticators - MalformedRequests -
   -- UnknownTypes -  PacketsDropped - Responses = Pending
   --
   -- Requests - DupRequests - BadAuthenticators - MalformedRequests -
   -- UnknownTypes - PacketsDropped = entries logged

   radiusAuthServAccessRequests OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS deprecated
          DESCRIPTION
                "The number of packets received on the authentication





                 port from this client."
          REFERENCE "RFC 2865 section 4.1"
          ::= { radiusAuthClientEntry  4 }

   radiusAuthServDupAccessRequests OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS deprecated
          DESCRIPTION
                "The number of duplicate RADIUS Access-Request
                 packets received from this client."
          REFERENCE "RFC 2865 section 4.1"
          ::= { radiusAuthClientEntry  5 }

   radiusAuthServAccessAccepts OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS deprecated
          DESCRIPTION
                "The number of RADIUS Access-Accept packets
                 sent to this client."
          REFERENCE "RFC 2865 section 4.2"
          ::= { radiusAuthClientEntry  6 }

   radiusAuthServAccessRejects OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
                "The number of RADIUS Access-Reject packets
                 sent to this client."
          REFERENCE "RFC 2865 section 4.3"
          ::= { radiusAuthClientEntry  7 }

   radiusAuthServAccessChallenges OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS deprecated
          DESCRIPTION
                "The number of RADIUS Access-Challenge packets
                 sent to this client."
          REFERENCE "RFC 2865 section 4.4"
          ::= { radiusAuthClientEntry  8 }






   radiusAuthServMalformedAccessRequests OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS deprecated
          DESCRIPTION
                "The number of malformed RADIUS Access-Request
                 packets received from this client.
                 Bad authenticators and unknown types are not included
                 as malformed Access-Requests."
          REFERENCE "RFC 2865 section 3"
          ::= { radiusAuthClientEntry  9 }

   radiusAuthServBadAuthenticators OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS deprecated
          DESCRIPTION
                "The number of RADIUS Authentication-Request packets
                 that contained invalid Message Authenticator
                 attributes received from this client."
          REFERENCE "RFC 2865 section 3"
          ::= { radiusAuthClientEntry  10 }

   radiusAuthServPacketsDropped OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
                 "The number of incoming packets from this
                  client silently discarded for some reason other
                  than malformed, bad authenticators or
                  unknown types."
          REFERENCE "RFC 2865 section 3"
          ::= { radiusAuthClientEntry  11 }

   radiusAuthServUnknownTypes OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS deprecated
          DESCRIPTION
                "The number of RADIUS packets of unknown type that
                 were received from this client."
          REFERENCE "RFC 2865 section 4"
          ::= { radiusAuthClientEntry  12 }





   -- New MIB objects added in this revision

   radiusAuthClientExtTable OBJECT-TYPE
          SYNTAX     SEQUENCE OF RadiusAuthClientExtEntry
          MAX-ACCESS not-accessible
          STATUS     current
          DESCRIPTION
                "The (conceptual) table listing the RADIUS
                 authentication clients with which the server shares
                 a secret."
          ::= { radiusAuthServ 16 }

   radiusAuthClientExtEntry OBJECT-TYPE
          SYNTAX     RadiusAuthClientExtEntry
          MAX-ACCESS not-accessible
          STATUS     current
          DESCRIPTION
                "An entry (conceptual row) representing a RADIUS
                 authentication client with which the server shares a
                 secret."
          INDEX      { radiusAuthClientExtIndex }
          ::= { radiusAuthClientExtTable 1 }

   RadiusAuthClientExtEntry ::= SEQUENCE {
          radiusAuthClientExtIndex                 Integer32,
          radiusAuthClientInetAddressType          InetAddressType,
          radiusAuthClientInetAddress              InetAddress,
          radiusAuthClientExtID                    SnmpAdminString,
          radiusAuthServExtAccessRequests          Counter32,
          radiusAuthServExtDupAccessRequests       Counter32,
          radiusAuthServExtAccessAccepts           Counter32,
          radiusAuthServExtAccessRejects           Counter32,
          radiusAuthServExtAccessChallenges        Counter32,
          radiusAuthServExtMalformedAccessRequests Counter32,
          radiusAuthServExtBadAuthenticators       Counter32,
          radiusAuthServExtPacketsDropped          Counter32,
          radiusAuthServExtUnknownTypes            Counter32,
          radiusAuthServCounterDiscontinuity       TimeTicks
   }

   radiusAuthClientExtIndex OBJECT-TYPE
          SYNTAX     Integer32 (1..2147483647)
          MAX-ACCESS not-accessible
          STATUS     current
          DESCRIPTION
                "A number uniquely identifying each RADIUS
                 authentication client with which this server
                 communicates."





          ::= { radiusAuthClientExtEntry 1 }

   radiusAuthClientInetAddressType OBJECT-TYPE
            SYNTAX     InetAddressType
            MAX-ACCESS read-only
            STATUS     current
            DESCRIPTION
                  "The type of address format used for the
                   radiusAuthClientInetAddress object."
            ::= { radiusAuthClientExtEntry 2 }

      radiusAuthClientInetAddress OBJECT-TYPE
            SYNTAX     InetAddress
            MAX-ACCESS read-only
            STATUS     current
            DESCRIPTION
                  "The IP address of the RADIUS authentication
                   client referred to in this table entry, using
                   the version-neutral IP address format."
            ::= { radiusAuthClientExtEntry 3 }


   radiusAuthClientExtID OBJECT-TYPE
          SYNTAX     SnmpAdminString
          MAX-ACCESS read-only
          STATUS     current
          DESCRIPTION
                "The NAS-Identifier of the RADIUS authentication client
                 referred to in this table entry.  This is not
                 necessarily the same as sysName in MIB II."
          REFERENCE "RFC 2865 section 5.32"
          ::= { radiusAuthClientExtEntry 4 }

   -- Server Counters

   --
   -- Responses = AccessAccepts + AccessRejects + AccessChallenges
   --
   -- Requests - DupRequests - BadAuthenticators - MalformedRequests -
   -- UnknownTypes -  PacketsDropped - Responses = Pending
   --
   -- Requests - DupRequests - BadAuthenticators - MalformedRequests -
   -- UnknownTypes - PacketsDropped = entries logged

   radiusAuthServExtAccessRequests OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only





          STATUS current
          DESCRIPTION
                "The number of packets received on the authentication
                 port from this client.  This counter may experience a
                 discontinuity when the RADIUS Server module within the
                 managed entity is reinitialized, as indicated by the
                 current value of radiusAuthServCounterDiscontinuity."
          REFERENCE "RFC 2865 section 4.1"
          ::= { radiusAuthClientExtEntry  5 }

   radiusAuthServExtDupAccessRequests OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                "The number of duplicate RADIUS Access-Request
                 packets received from this client.  This counter may
                 experience a discontinuity when the RADIUS Server
                 module within the managed entity is reinitialized, as
                 indicated by the current value of
                 radiusAuthServCounterDiscontinuity."
          REFERENCE "RFC 2865 section 4.1"
          ::= { radiusAuthClientExtEntry  6 }

   radiusAuthServExtAccessAccepts OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                "The number of RADIUS Access-Accept packets
                 sent to this client.  This counter may experience a
                 discontinuity when the RADIUS Server module within the
                 managed entity is reinitialized, as indicated by the
                 current value of radiusAuthServCounterDiscontinuity."
          REFERENCE "RFC 2865 section 4.2"
          ::= { radiusAuthClientExtEntry  7 }

   radiusAuthServExtAccessRejects OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
                "The number of RADIUS Access-Reject packets
                 sent to this client.  This counter may experience a
                 discontinuity when the RADIUS Server module within the





                 managed entity is reinitialized, as indicated by the
                 current value of radiusAuthServCounterDiscontinuity."
          REFERENCE "RFC 2865 section 4.3"
          ::= { radiusAuthClientExtEntry  8 }

   radiusAuthServExtAccessChallenges OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                "The number of RADIUS Access-Challenge packets
                 sent to this client.  This counter may experience a
                 discontinuity when the RADIUS Server module within the
                 managed entity is reinitialized, as indicated by the
                 current value of radiusAuthServCounterDiscontinuity."
          REFERENCE "RFC 2865 section 4.4"
          ::= { radiusAuthClientExtEntry  9 }

   radiusAuthServExtMalformedAccessRequests OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                "The number of malformed RADIUS Access-Request
                 packets received from this client.  Bad authenticators
                 and unknown types are not included as malformed
                 Access-Requests.  This counter may experience a
                 discontinuity when the RADIUS Server module within the
                 managed entity is reinitialized, as indicated by the
                 current value of radiusAuthServCounterDiscontinuity."
          REFERENCE "RFC 2865 sections 3, 4.1"
          ::= { radiusAuthClientExtEntry  10 }

   radiusAuthServExtBadAuthenticators OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                "The number of RADIUS Authentication-Request packets
                 that contained invalid Message Authenticator
                 attributes received from this client.  This counter
                 may experience a discontinuity when the RADIUS Server
                 module within the managed entity is reinitialized, as
                 indicated by the current value of
                 radiusAuthServCounterDiscontinuity."





          REFERENCE "RFC 2865 section 3"
          ::= { radiusAuthClientExtEntry  11 }

   radiusAuthServExtPacketsDropped OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
                "The number of incoming packets from this client
                 silently discarded for some reason other than
                 malformed, bad authenticators or unknown types.
                 This counter may experience a discontinuity when the
                 RADIUS Server module within the managed entity is
                 reinitialized, as indicated by the current value of
                 radiusAuthServCounterDiscontinuity."
          REFERENCE "RFC 2865 section 3"
          ::= { radiusAuthClientExtEntry  12 }

   radiusAuthServExtUnknownTypes OBJECT-TYPE
          SYNTAX Counter32
          UNITS "packets"
          MAX-ACCESS read-only
          STATUS current
          DESCRIPTION
                "The number of RADIUS packets of unknown type that
                 were received from this client.  This counter may
                 experience a discontinuity when the RADIUS Server
                 module within the managed entity is reinitialized, as
                 indicated by the current value of
                 radiusAuthServCounterDiscontinuity."
          REFERENCE "RFC 2865 section 4"
          ::= { radiusAuthClientExtEntry  13 }

   radiusAuthServCounterDiscontinuity OBJECT-TYPE
            SYNTAX TimeTicks
            UNITS "centiseconds"
            MAX-ACCESS read-only
            STATUS current
            DESCRIPTION
                  "The number of centiseconds since the last
                   discontinuity in the RADIUS Server counters.
                   A discontinuity may be the result of a
                   reinitialization of the RADIUS Server module
                   within the managed entity."
            ::= { radiusAuthClientExtEntry 14 }







   -- conformance information

   radiusAuthServMIBConformance  OBJECT IDENTIFIER
          ::= { radiusAuthServMIB 2 }

   radiusAuthServMIBCompliances  OBJECT IDENTIFIER
          ::= { radiusAuthServMIBConformance 1 }

   radiusAuthServMIBGroups  OBJECT IDENTIFIER
          ::= { radiusAuthServMIBConformance 2 }

   -- compliance statements

   radiusAuthServMIBCompliance MODULE-COMPLIANCE
               STATUS  deprecated
               DESCRIPTION
                     "The compliance statement for authentication
                      servers implementing the RADIUS Authentication
                      Server MIB.  Implementation of this module is for
                      IPv4-only entities, or for backwards compatibility
                      use with entities that support both IPv4 and
                      IPv6."
               MODULE  -- this module
               MANDATORY-GROUPS { radiusAuthServMIBGroup }

               OBJECT        radiusAuthServConfigReset
               WRITE-SYNTAX  INTEGER { reset(2) }
               DESCRIPTION  "The only SETable value is 'reset' (2)."

               ::= { radiusAuthServMIBCompliances 1 }


   radiusAuthServMIBExtCompliance MODULE-COMPLIANCE
               STATUS  current
               DESCRIPTION
                     "The compliance statement for authentication
                      servers implementing the RADIUS Authentication
                      Server IPv6 Extensions MIB.  Implementation of
                      this module is for entities that support IPv6,
                      or support IPv4 and IPv6."
               MODULE  -- this module
               MANDATORY-GROUPS { radiusAuthServExtMIBGroup }

               OBJECT        radiusAuthServConfigReset
               WRITE-SYNTAX  INTEGER { reset(2) }
               DESCRIPTION  "The only SETable value is 'reset' (2)."

               OBJECT radiusAuthClientInetAddressType





               SYNTAX InetAddressType { ipv4(1), ipv6(2) }
               DESCRIPTION
                 "An implementation is only required to support
                  IPv4 and globally unique IPv6 addresses."

               OBJECT radiusAuthClientInetAddress
               SYNTAX InetAddress ( SIZE (4|16) )
               DESCRIPTION
                 "An implementation is only required to support
                  IPv4 and globally unique IPv6 addresses."

               ::= { radiusAuthServMIBCompliances 2 }


   -- units of conformance

   radiusAuthServMIBGroup OBJECT-GROUP
         OBJECTS {radiusAuthServIdent,
                  radiusAuthServUpTime,
                  radiusAuthServResetTime,
                  radiusAuthServConfigReset,
                  radiusAuthServTotalAccessRequests,
                  radiusAuthServTotalInvalidRequests,
                  radiusAuthServTotalDupAccessRequests,
                  radiusAuthServTotalAccessAccepts,
                  radiusAuthServTotalAccessRejects,
                  radiusAuthServTotalAccessChallenges,
                  radiusAuthServTotalMalformedAccessRequests,
                  radiusAuthServTotalBadAuthenticators,
                  radiusAuthServTotalPacketsDropped,
                  radiusAuthServTotalUnknownTypes,
                  radiusAuthClientAddress,
                  radiusAuthClientID,
                  radiusAuthServAccessRequests,
                  radiusAuthServDupAccessRequests,
                  radiusAuthServAccessAccepts,
                  radiusAuthServAccessRejects,
                  radiusAuthServAccessChallenges,
                  radiusAuthServMalformedAccessRequests,
                  radiusAuthServBadAuthenticators,
                  radiusAuthServPacketsDropped,
                  radiusAuthServUnknownTypes
                 }
         STATUS  deprecated
         DESCRIPTION
               "The collection of objects providing management of
                a RADIUS Authentication Server."
         ::= { radiusAuthServMIBGroups 1 }





   radiusAuthServExtMIBGroup OBJECT-GROUP
         OBJECTS {radiusAuthServIdent,
                  radiusAuthServUpTime,
                  radiusAuthServResetTime,
                  radiusAuthServConfigReset,
                  radiusAuthServTotalAccessRequests,
                  radiusAuthServTotalInvalidRequests,
                  radiusAuthServTotalDupAccessRequests,
                  radiusAuthServTotalAccessAccepts,
                  radiusAuthServTotalAccessRejects,
                  radiusAuthServTotalAccessChallenges,
                  radiusAuthServTotalMalformedAccessRequests,
                  radiusAuthServTotalBadAuthenticators,
                  radiusAuthServTotalPacketsDropped,
                  radiusAuthServTotalUnknownTypes,
                  radiusAuthClientInetAddressType,
                  radiusAuthClientInetAddress,
                  radiusAuthClientExtID,
                  radiusAuthServExtAccessRequests,
                  radiusAuthServExtDupAccessRequests,
                  radiusAuthServExtAccessAccepts,
                  radiusAuthServExtAccessRejects,
                  radiusAuthServExtAccessChallenges,
                  radiusAuthServExtMalformedAccessRequests,
                  radiusAuthServExtBadAuthenticators,
                  radiusAuthServExtPacketsDropped,
                  radiusAuthServExtUnknownTypes,
                  radiusAuthServCounterDiscontinuity
                 }
         STATUS  current
         DESCRIPTION
               "The collection of objects providing management of
                a RADIUS Authentication Server."
         ::= { radiusAuthServMIBGroups 2 }

   END


