SNMPv2-TM DEFINITIONS ::= BEGIN


          IMPORTS
              snmpDomains, snmpProxys
                  FROM SNMPv2-SMI
              TEXTUAL-CONVENTION
                  FROM SNMPv2-TC;

          -- SNMPv2 over UDP

          snmpUDPDomain  OBJECT IDENTIFIER ::= { snmpDomains 1 }
          -- for a SnmpUDPAddress of length 6:
          --
          -- octets   contents        encoding
          --  1-4     IP-address      network-byte order
          --  5-6     UDP-port        network-byte order
          --
          SnmpUDPAddress ::= TEXTUAL-CONVENTION
              DISPLAY-HINT "1d.1d.1d.1d/2d"
              STATUS       current
              DESCRIPTION
                      "Represents a UDP address."
              SYNTAX       OCTET STRING (SIZE (6))

























          RFC 1449        Transport Mappings for SNMPv2       April 1993


          -- SNMPv2 over OSI

          snmpCLNSDomain OBJECT IDENTIFIER ::= { snmpDomains 2 }
          snmpCONSDomain OBJECT IDENTIFIER ::= { snmpDomains 3 }
          -- for a SnmpOSIAddress of length m:
          --
          -- octets   contents            encoding
          --    1     length of NSAP      "n" as an unsigned-integer
          --                                (either 0 or from 3 to 20)
          -- 2..(n+1) NSAP                concrete binary representation
          -- (n+2)..m TSEL                string of (up to 64) octets
          --
          SnmpOSIAddress ::= TEXTUAL-CONVENTION
              DISPLAY-HINT "*1x:/1x:"
              STATUS       current
              DESCRIPTION
                      "Represents an OSI transport-address."
              SYNTAX       OCTET STRING (SIZE (1 | 4..85))
































          RFC 1449        Transport Mappings for SNMPv2       April 1993


          -- SNMPv2 over DDP

          snmpDDPDomain  OBJECT IDENTIFIER ::= { snmpDomains 4 }
          -- for a SnmpNBPAddress of length m:
          --
          --    octets      contents         encoding
          --       1        length of object "n" as an unsigned integer
          --     2..(n+1)   object           string of (up to 32) octets
          --      n+2       length of type   "p" as an unsigned integer
          -- (n+3)..(n+2+p) type             string of (up to 32) octets
          --     n+3+p      length of zone   "q" as an unsigned integer
          -- (n+4+p)..m     zone             string of (up to 32) octets
          --
          -- for comparison purposes, strings are case-insensitive
          --
          -- all strings may contain any octet other than 255 (hex ff)
          --
          SnmpNBPAddress ::= TEXTUAL-CONVENTION
              STATUS       current
              DESCRIPTION
                      "Represents an NBP name."
              SYNTAX       OCTET STRING (SIZE (3..99))


          -- SNMPv2 over IPX

          snmpIPXDomain  OBJECT IDENTIFIER ::= { snmpDomains 5 }
          -- for a SnmpIPXAddress of length 12:
          --
          -- octets   contents            encoding
          --  1-4     network-number      network-byte order
          --  5-10    physical-address    network-byte order
          -- 11-12    socket-number       network-byte order
          --
          SnmpIPXAddress ::= TEXTUAL-CONVENTION
              DISPLAY-HINT "4x.1x:1x:1x:1x:1x:1x.2d"
              STATUS       current
              DESCRIPTION
                      "Represents an IPX address."
              SYNTAX       OCTET STRING (SIZE (12))










          RFC 1449        Transport Mappings for SNMPv2       April 1993


          -- for proxy to community-based SNMPv1 (RFC 1157)

          rfc1157Proxy   OBJECT IDENTIFIER ::= { snmpProxys 1 }

          -- uses SnmpUDPAddress
          rfc1157Domain  OBJECT IDENTIFIER ::= { rfc1157Proxy 1 }

          -- the community-based noAuth
          rfc1157noAuth  OBJECT IDENTIFIER ::= { rfc1157Proxy 2 }


          END






































          
