PARALLEL-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
       Counter32, Integer32
           FROM SNMPv2-SMI
       InterfaceIndex
           FROM IF-MIB
       transmission
           FROM RFC1213-MIB
       MODULE-COMPLIANCE, OBJECT-GROUP
           FROM SNMPv2-CONF;


   para MODULE-IDENTITY
        LAST-UPDATED "9405261700Z"
        ORGANIZATION "IETF Character MIB Working Group"
        CONTACT-INFO
               "        Bob Stewart
                Postal: Xyplex, Inc.
                        295 Foster Street
                        Littleton, MA 01460

                   Tel: 508-952-4816
                   Fax: 508-952-4887
                E-mail: rlstewart@eng.xyplex.com"





        DESCRIPTION
               "The MIB module for Parallel-printer-like hardware devices."
       ::= { transmission 34 }


   -- Generic Parallel-printer-like information

   paraNumber OBJECT-TYPE
       SYNTAX Integer32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The number of ports (regardless of their current
           state) in the Parallel-printer-like port table."
       ::= { para 1 }


   -- the Parallel-printer-like Port table

   paraPortTable OBJECT-TYPE
       SYNTAX SEQUENCE OF ParaPortEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A list of port entries.  The number of entries is
           given by the value of paraNumber."
       ::= { para 2 }

   paraPortEntry OBJECT-TYPE
       SYNTAX ParaPortEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Status and parameter values for a port."
       INDEX { paraPortIndex }
       ::= { paraPortTable 1 }

   ParaPortEntry ::=
       SEQUENCE {
           paraPortIndex
               InterfaceIndex,
           paraPortType
               INTEGER,
           paraPortInSigNumber
               Integer32,
           paraPortOutSigNumber
               Integer32
       }





   paraPortIndex OBJECT-TYPE
       SYNTAX InterfaceIndex
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The value of ifIndex for the port.  By convention
           and if possible, hardware port numbers map directly
           to external connectors.  The value for each port must
           remain constant at least from one re-initialization
           of the network management agent to the next."
       ::= { paraPortEntry 1 }

   paraPortType OBJECT-TYPE
       SYNTAX INTEGER {
           other(1),
           centronics(2),
           dataproducts(3)
       }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The port's hardware type."
       ::= { paraPortEntry 2 }

   paraPortInSigNumber OBJECT-TYPE
       SYNTAX Integer32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The number of input signals for the port in the
           input signal table (paraPortInSigTable).  The table
           contains entries only for those signals the software
           can detect and that are useful to observe."
       ::= { paraPortEntry 3 }

   paraPortOutSigNumber OBJECT-TYPE
       SYNTAX Integer32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The number of output signals for the port in the
           output signal table (paraPortOutSigTable).  The
           table contains entries only for those signals the
           software can assert and that are useful to observe."
       ::= { paraPortEntry 4 }








   -- Parallel-printer-like Input Signal Table

   paraInSigTable OBJECT-TYPE
       SYNTAX SEQUENCE OF ParaInSigEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A list of port input control signal entries."
       ::= { para 3 }

   paraInSigEntry OBJECT-TYPE
       SYNTAX ParaInSigEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Input control signal status for a hardware port."
       INDEX { paraInSigPortIndex, paraInSigName }
       ::= { paraInSigTable 1 }

   ParaInSigEntry ::=
       SEQUENCE {
           paraInSigPortIndex
               InterfaceIndex,
           paraInSigName
               INTEGER,
           paraInSigState
               INTEGER,
           paraInSigChanges
               Counter32
       }

   paraInSigPortIndex OBJECT-TYPE
       SYNTAX InterfaceIndex
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The value of paraPortIndex for the port to which
           this entry belongs."
       ::= { paraInSigEntry 1 }

   paraInSigName OBJECT-TYPE
       SYNTAX INTEGER { power(1), online(2), busy(3),
                        paperout(4), fault(5) }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Identification of a hardware signal."
       ::= { paraInSigEntry 2 }





   paraInSigState OBJECT-TYPE
       SYNTAX INTEGER { none(1), on(2), off(3) }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The current signal state."
       ::= { paraInSigEntry 3 }

   paraInSigChanges OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The number of times the signal has changed from
           'on' to 'off' or from 'off' to 'on'."
       ::= { paraInSigEntry 4 }


   -- Output Signal Table

   paraOutSigTable OBJECT-TYPE
       SYNTAX SEQUENCE OF ParaOutSigEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "A list of port output control signal entries."
       ::= { para 4 }

   paraOutSigEntry OBJECT-TYPE
       SYNTAX ParaOutSigEntry
       MAX-ACCESS not-accessible
       STATUS current
       DESCRIPTION
           "Output control signal status for a hardware port."
       INDEX { paraOutSigPortIndex, paraOutSigName }
       ::= { paraOutSigTable 1 }

   ParaOutSigEntry ::=
       SEQUENCE {
           paraOutSigPortIndex
               InterfaceIndex,
           paraOutSigName
               INTEGER,
           paraOutSigState
               INTEGER,
           paraOutSigChanges
               Counter32
       }





   paraOutSigPortIndex OBJECT-TYPE
       SYNTAX InterfaceIndex
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The value of paraPortIndex for the port to which
           this entry belongs."
       ::= { paraOutSigEntry 1 }

   paraOutSigName OBJECT-TYPE
       SYNTAX INTEGER { power(1), online(2), busy(3),
                        paperout(4), fault(5) }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "Identification of a hardware signal."
       ::= { paraOutSigEntry 2 }

   paraOutSigState OBJECT-TYPE
       SYNTAX INTEGER { none(1), on(2), off(3) }
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The current signal state."
       ::= { paraOutSigEntry 3 }

   paraOutSigChanges OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
           "The number of times the signal has changed from
           'on' to 'off' or from 'off' to 'on'."
       ::= { paraOutSigEntry 4 }


   -- conformance information

   paraConformance OBJECT IDENTIFIER ::= { para 5 }

   paraGroups      OBJECT IDENTIFIER ::= { paraConformance 1 }
   paraCompliances OBJECT IDENTIFIER ::= { paraConformance 2 }











   -- compliance statements

   paraCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for SNMPv2 entities
               which have Parallel-printer-like hardware
               interfaces."

       MODULE  -- this module
           MANDATORY-GROUPS { paraGroup }
       ::= { paraCompliances 1 }


   -- units of conformance

   paraGroup    OBJECT-GROUP
       OBJECTS { paraNumber, paraPortIndex, paraPortType,
                 paraPortInSigNumber, paraPortOutSigNumber,
                 paraInSigPortIndex, paraInSigName,
                 paraInSigState, paraInSigChanges,
                 paraOutSigPortIndex, paraOutSigName,
                 paraOutSigState, paraOutSigChanges }
       STATUS  current
       DESCRIPTION
               "A collection of objects providing information
                applicable to all Parallel-printer-like interfaces."
       ::= { paraGroups 1 }

   END


