DS3-MIB DEFINITIONS ::= BEGIN


   IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE,
        NOTIFICATION-TYPE, transmission
             FROM SNMPv2-SMI                    -- [RFC2578]
        DisplayString, TimeStamp, TruthValue
             FROM SNMPv2-TC                     -- [RFC2579]
        MODULE-COMPLIANCE, OBJECT-GROUP,
        NOTIFICATION-GROUP
             FROM SNMPv2-CONF                   -- [RFC2580]
        InterfaceIndex
             FROM IF-MIB                        -- [RFC2863]
        PerfCurrentCount, PerfIntervalCount,
        PerfTotalCount
             FROM PerfHist-TC-MIB;              -- [RFC3593]






   ds3 MODULE-IDENTITY
       LAST-UPDATED "200409080000Z"  -- September 08, 2004
       ORGANIZATION "IETF AToM MIB Working Group"
       CONTACT-INFO
         "WG charter:
            http://www.ietf.org/html.charters/atommib-charter.html

          Mailing Lists:
            General Discussion: atommib@research.telcordia.com
            To Subscribe: atommib-request@research.telcordia.com

          Editor: Orly Nicklass

          Postal: RAD Data Communications, Ltd.
                  Ziv Tower, 24 Roul Walenberg
                  Tel Aviv, Israel, 69719

                  Tel: +9723 765 9969
          E-mail: orly_n@rad.com"

       DESCRIPTION
            "The is the MIB module that describes
             DS3 and E3 interfaces objects.

             Copyright (c) The Internet Society (2004).  This
             version of this MIB module is part of RFC 3896;
             see the RFC itself for full legal notices."

       REVISION "200409080000Z"  -- September 08, 2004

        DESCRIPTION
             "The RFC 3896 version of this MIB module.
             The key changes made to this MIB module
             since its publication in RFC 2496 are as follows:

         (1) The dsx3FracIfIndex SYNTAX matches the description range.

         (2) Reference was added to Circuit Identifier object.

         (3) Usage of ifStackTable section was updated.

         (4) Align the DESCRIPTION clauses of few statistic objects with
             thenear end definition, the far end definition and with
             RFC 3593.

         (5) Add new value, dsx3M13, to dsx3LineType."

        REVISION "199808012130Z"





        DESCRIPTION
             "The RFC 2496 version of this MIB module.
             The key changes made to this MIB module
             since its publication in RFC 1407 are as follows:

            (1)  The Fractional Table has been deprecated.

            (2)  This document uses SMIv2.

            (3)  Values are given for ifTable and ifXTable.

            (4)  Example usage of ifStackTable is included.

            (5)  dsx3IfIndex has been deprecated.

            (6)  The definition of valid intervals has been clarified
                 for the case where the agent proxied for other devices.
                 In particular, the treatment of missing intervals has
                 been clarified.

           (7)  An inward loopback has been added.

           (8)  Additional lineStatus bits have been added for Near End
                in Unavailable Signal State, Carrier Equipment Out of
                Service.

           (9)  A read-write line Length object has been added.

           (10) Added a lineStatus last change, trap and enabler.

           (11) Textual Conventions for statistics objects have
                been used.

           (12) A new object, dsx3LoopbackStatus, has been introduced to
                reflect the loopbacks established on a DS3/E3 interface
                and the source to the requests.  dsx3LoopbackConfig
                continues to be the desired loopback state while
                dsx3LoopbackStatus reflects the actual state.

           (13) A dual loopback has been added to allow the setting of
                an inward loopback and a line loopback at the same time.

           (14) An object has been added to indicated whether or not
                this is a channelized DS3/E3.

           (15) A new object has been added to indicate which DS1 is to
                set for remote loopback."






       REVISION "199301252028Z"
       DESCRIPTION
            "Initial version, published as RFC 1407."
       ::= { transmission 30 }

   -- The DS3/E3 Near End Group

   -- The DS3/E3 Near End Group consists of four tables:
   --    DS3/E3 Configuration
   --    DS3/E3 Current
   --    DS3/E3 Interval
   --    DS3/E3 Total

   -- the DS3/E3 Configuration Table

   dsx3ConfigTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx3ConfigEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS3/E3 Configuration table."
        ::= { ds3 5 }

   dsx3ConfigEntry OBJECT-TYPE
        SYNTAX  Dsx3ConfigEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "An entry in the DS3/E3 Configuration table."
        INDEX   { dsx3LineIndex }
        ::= { dsx3ConfigTable 1 }

   Dsx3ConfigEntry ::=
        SEQUENCE {
            dsx3LineIndex                        InterfaceIndex,
            dsx3IfIndex                          InterfaceIndex,
            dsx3TimeElapsed                      INTEGER,
            dsx3ValidIntervals                   INTEGER,
            dsx3LineType                         INTEGER,
            dsx3LineCoding                       INTEGER,
            dsx3SendCode                         INTEGER,
            dsx3CircuitIdentifier                DisplayString,
            dsx3LoopbackConfig                   INTEGER,
            dsx3LineStatus                       INTEGER,
            dsx3TransmitClockSource              INTEGER,
            dsx3InvalidIntervals                 INTEGER,
            dsx3LineLength                       INTEGER,
            dsx3LineStatusLastChange             TimeStamp,





            dsx3LineStatusChangeTrapEnable       INTEGER,
            dsx3LoopbackStatus                   INTEGER,
            dsx3Channelization                   INTEGER,
            dsx3Ds1ForRemoteLoop                 INTEGER

   }

   dsx3LineIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index

        STATUS  current
        DESCRIPTION
               "This object should be made equal to ifIndex.  The
               next paragraph describes its previous usage.
               Making the object equal to ifIndex allows proper
               use of ifStackTable.

               Previously, this object was the identifier of a
               DS3/E3 Interface on a managed device.  If there is
               an ifEntry that is directly associated with this
               and only this DS3/E3 interface, it should have the
               same value as ifIndex.  Otherwise, number the
               dsx3LineIndices with an unique identifier
               following the rules of choosing a number that is
               greater than ifNumber and numbering the inside
               interfaces (e.g., equipment side) with even
               numbers and outside interfaces (e.g., network side)
               with odd numbers."
        ::= { dsx3ConfigEntry 1 }

   dsx3IfIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only
        STATUS  deprecated
        DESCRIPTION
               "This value for this object is equal to the value
               of ifIndex from the Interfaces table of MIB II
               (RFC 1213)."
        ::= { dsx3ConfigEntry 2 }

   dsx3TimeElapsed OBJECT-TYPE
        SYNTAX  INTEGER (0..899)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of seconds that have elapsed since the





               beginning of the near end current error-
               measurement period. If, for some reason, such as
               an adjustment in the system's time-of-day clock,
               the current interval exceeds the maximum value,
               the agent will return the maximum value."
        ::= { dsx3ConfigEntry 3 }

   dsx3ValidIntervals OBJECT-TYPE
        SYNTAX  INTEGER (0..96)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of previous near end intervals for
               which data was collected.  The value will be 96
               unless the interface was brought online within the
               last 24 hours, in which case the value will be the
               number of complete 15 minute near end intervals
               since the interface has been online.  In the case
               where the agent is a proxy, it is possible that
               some intervals are unavailable.  In this case,
               this interval is the maximum interval number for
               which data is available."
        ::= { dsx3ConfigEntry 4 }

   dsx3LineType OBJECT-TYPE
        SYNTAX  INTEGER {
                   dsx3other(1),
                   dsx3M23(2),
                   dsx3SYNTRAN(3),
                   dsx3CbitParity(4),
                   dsx3ClearChannel(5),
                   e3other(6),
                   e3Framed(7),
                   e3Plcp(8),
                   dsx3M13(9)
               }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This variable indicates the variety of DS3 C-bit
               or E3 application implementing this interface. The
               type of interface affects the interpretation of
               the usage and error statistics.  The rate of DS3
               is 44.736 Mbps and E3 is 34.368 Mbps.  The
               dsx3ClearChannel value means that the C-bits are
               not used except for sending/receiving AIS.  The
               values, in sequence, describe:






                              TITLE:          SPECIFICATION:
                              dsx3M23         ANSI T1.107-1988
                              dsx3SYNTRAN     ANSI T1.107-1988
                              dsx3CbitParity  ANSI T1.107a-1990
                              dsx3ClearChannel ANSI T1.102-1987
                              e3Framed        CCITT G.751
                              e3Plcp          ETSI T/NA(91)18
                              dsx3M13         ANSI T1.107a-1990."

       REFERENCE
               "American National Standard for telecommunications
                    - digital hierarchy -
                    formats specification, ANSI T1.107- 1988.
                    ANSI T1.107a-1990.
                American National Standard for telecommunications
                    - digital hierarchy -
                    electrical interfaces, ANSI T1.102- 1987.
                CCITT - Digital Multiplex Equipment Operating at
                    the Third Order Bit Rate of 34 368 Kbit/s and
                    the Forth Order Bit Rate of 139 264 Kbit/s
                    and Using Positive Justification, G.751
                European Telecommunications Standards Institute
                    -- ETS '34M' --
                    Metropolitan Area Network Physical
                    Convergence Layer Procedure for
                    34.368 Megabits per Second, T/NA(91)18,
                    May 1991."
        ::= { dsx3ConfigEntry 5 }

   dsx3LineCoding OBJECT-TYPE
        SYNTAX  INTEGER {
                   dsx3Other(1),
                   dsx3B3ZS(2),
                   e3HDB3(3)
               }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This variable describes the variety of Zero Code
               Suppression used on this interface, which in turn
               affects a number of its characteristics.
               dsx3B3ZS and e3HDB3 refer to the use of specified
               patterns of normal bits and bipolar violations
               which are used to replace sequences of zero bits
               of a specified length."
        ::= { dsx3ConfigEntry 6 }

   dsx3SendCode OBJECT-TYPE





        SYNTAX  INTEGER {
                  dsx3SendNoCode(1),
                  dsx3SendLineCode(2),
                  dsx3SendPayloadCode(3),
                  dsx3SendResetCode(4),
                  dsx3SendDS1LoopCode(5),
                  dsx3SendTestPattern(6)
                  }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This variable indicates what type of code is
               being sent across the DS3/E3 interface by the
               device.  (These are optional for E3 interfaces.)
               Setting this variable causes the interface to
               begin sending the code requested.
               The values mean:

                  dsx3SendNoCode
                      sending looped or normal data

                  dsx3SendLineCode
                      sending a request for a line loopback

                  dsx3SendPayloadCode
                      sending a request for a payload loopback
                      (i.e., all DS1/E1s in a DS3/E3 frame)

                  dsx3SendResetCode
                      sending a loopback deactivation request

                  dsx3SendDS1LoopCode
                      requesting to loopback a particular DS1/E1
                      within a DS3/E3 frame.  The DS1/E1 is
                      indicated in dsx3Ds1ForRemoteLoop.

                  dsx3SendTestPattern
                      sending a test pattern."
        ::= { dsx3ConfigEntry 7 }

   dsx3CircuitIdentifier OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This variable contains the transmission vendor's
               circuit identifier, for the purpose of
               facilitating troubleshooting."





        REFERENCE "ITU-T M.1400"
        ::= { dsx3ConfigEntry 8 }

   dsx3LoopbackConfig OBJECT-TYPE
        SYNTAX  INTEGER {
                    dsx3NoLoop(1),
                    dsx3PayloadLoop(2),
                    dsx3LineLoop(3),
                    dsx3OtherLoop(4),
                    dsx3InwardLoop(5),
                    dsx3DualLoop(6)
                  }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
             "This variable represents the desired loopback
             configuration of the DS3/E3 interface.
             The values mean:

             dsx3NoLoop
               Not in the loopback state.  A device that is
               not capable of performing a loopback on
               the interface shall always return this as
               its value.

             dsx3PayloadLoop
               The received signal at this interface is looped
               through the device.  Typically the received signal
               is looped back for retransmission after it has
               passed through the device's framing function.

             dsx3LineLoop
               The received signal at this interface does not
               go through the device (minimum penetration) but
               is looped back out.

             dsx3OtherLoop
               Loopbacks that are not defined here.

             dsx3InwardLoop
               The sent signal at this interface is looped back
               through the device.

             dsx3DualLoop
               Both dsx1LineLoop and dsx1InwardLoop will be
               active simultaneously."
        ::= { dsx3ConfigEntry 9 }






   dsx3LineStatus OBJECT-TYPE
        SYNTAX  INTEGER (1..4095)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "This variable indicates the Line Status of the
               interface.  It contains loopback state information
               and failure state information.  The dsx3LineStatus
               is a bit map represented as a sum, therefore, it
               can represent multiple failures and a loopback
               (see dsx3LoopbackConfig object for the type of
               loopback) simultaneously.  The dsx3NoAlarm must be
               set if and only if no other flag is set.

               If the dsx3loopbackState bit is set, the loopback
               in effect can be determined from the
               dsx3loopbackConfig object.
          The various bit positions are:
           1     dsx3NoAlarm         No alarm present
           2     dsx3RcvRAIFailure   Receiving Yellow/Remote
                                     Alarm Indication
           4     dsx3XmitRAIAlarm    Transmitting Yellow/Remote
                                     Alarm Indication
           8     dsx3RcvAIS          Receiving AIS failure state
          16     dsx3XmitAIS         Transmitting AIS
          32     dsx3LOF             Receiving LOF failure state
          64     dsx3LOS             Receiving LOS failure state
         128     dsx3LoopbackState   Looping the received signal
         256     dsx3RcvTestCode     Receiving a Test Pattern
         512     dsx3OtherFailure    any line status not defined
                                     here
        1024     dsx3UnavailSigState Near End in Unavailable
                                     Signal State
        2048     dsx3NetEquipOOS     Carrier Equipment Out of
                                     Service"
        ::= { dsx3ConfigEntry 10 }

   dsx3TransmitClockSource OBJECT-TYPE
        SYNTAX  INTEGER {
                   loopTiming(1),
                   localTiming(2),
                   throughTiming(3)
               }
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "The source of Transmit Clock.






               loopTiming indicates that the recovered receive
               clock is used as the transmit clock.

               localTiming indicates that a local clock source is
               used or that an external clock is attached to the
               box containing the interface.

               throughTiming indicates that transmit clock is
               derived from the recovered receive clock of
               another DS3 interface."
        ::= { dsx3ConfigEntry 11 }

   dsx3InvalidIntervals OBJECT-TYPE
        SYNTAX  INTEGER (0..96)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               " The number of intervals in the range from 0 to
               dsx3ValidIntervals for which no data is available.
               This object will typically be zero except in cases
               where the data for some intervals are not
               available (e.g., in proxy situations)."
        ::= { dsx3ConfigEntry 12 }

   dsx3LineLength OBJECT-TYPE
        SYNTAX  INTEGER (0..64000)
        UNITS "meters"
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "The length of the ds3 line in meters.  This
               object provides information for line build out
               circuitry if it exists and can use this object to
               adjust the line build out."
        ::= { dsx3ConfigEntry 13 }

   dsx3LineStatusLastChange OBJECT-TYPE
        SYNTAX  TimeStamp
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The value of MIB II's sysUpTime object at the
               time this DS3/E3 entered its current line status
               state.  If the current state was entered prior to
               the last re-initialization of the proxy-agent,
               then this object contains a zero value."
        ::= { dsx3ConfigEntry 14 }






   dsx3LineStatusChangeTrapEnable  OBJECT-TYPE
        SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
               "Indicates whether dsx3LineStatusChange traps
               should be generated for this interface."
        DEFVAL { disabled }
        ::= { dsx3ConfigEntry 15 }

   dsx3LoopbackStatus  OBJECT-TYPE
        SYNTAX      INTEGER (1..127)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
               "This variable represents the current state of the
               loopback on the DS3 interface.  It contains
               information about loopbacks established by a
               manager and remotely from the far end.

               The dsx3LoopbackStatus is a bit map represented as
               a sum, therefore is can represent multiple
               loopbacks simultaneously.

               The various bit positions are:
                1  dsx3NoLoopback
                2  dsx3NearEndPayloadLoopback
                4  dsx3NearEndLineLoopback
                8  dsx3NearEndOtherLoopback
               16  dsx3NearEndInwardLoopback
               32  dsx3FarEndPayloadLoopback
               64  dsx3FarEndLineLoopback"
        ::= { dsx3ConfigEntry 16 }

   dsx3Channelization  OBJECT-TYPE
        SYNTAX      INTEGER {
                       disabled(1),
                       enabledDs1(2),
                       enabledDs2(3)
                    }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
               "Indicates whether this ds3/e3 is channelized or
               unchannelized.  The value of enabledDs1 indicates





               that this is a DS3 channelized into DS1s.  The
               value of enabledDs3 indicated that this is a DS3
               channelized into DS2s.  Setting this object will
               cause the creation or deletion of DS2 or DS1
               entries in the ifTable.  "
        ::= { dsx3ConfigEntry 17 }

   dsx3Ds1ForRemoteLoop  OBJECT-TYPE
        SYNTAX      INTEGER (0..29)
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
               "Indicates which DS1/E1 on this DS3/E3 will be
               indicated in the remote ds1 loopback request.  A
               value of 0 means no DS1 will be looped.  A value
               of 29 means all DS1s/E1s will be looped."
        ::= { dsx3ConfigEntry 18 }

   -- the DS3/E3 Current Table


   dsx3CurrentTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx3CurrentEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS3/E3 current table contains various
               statistics being collected for the current 15
               minute interval."
        ::= { ds3 6 }

   dsx3CurrentEntry OBJECT-TYPE
        SYNTAX  Dsx3CurrentEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "An entry in the DS3/E3 Current table."
        INDEX   { dsx3CurrentIndex }
        ::= { dsx3CurrentTable 1 }

   Dsx3CurrentEntry ::=
        SEQUENCE {
            dsx3CurrentIndex           InterfaceIndex,
            dsx3CurrentPESs            PerfCurrentCount,
            dsx3CurrentPSESs           PerfCurrentCount,
            dsx3CurrentSEFSs           PerfCurrentCount,
            dsx3CurrentUASs            PerfCurrentCount,
            dsx3CurrentLCVs            PerfCurrentCount,





            dsx3CurrentPCVs            PerfCurrentCount,
            dsx3CurrentLESs            PerfCurrentCount,
            dsx3CurrentCCVs            PerfCurrentCount,
            dsx3CurrentCESs            PerfCurrentCount,
            dsx3CurrentCSESs           PerfCurrentCount
       }

   dsx3CurrentIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
        STATUS  current
        DESCRIPTION
               "The index value which uniquely identifies the
               DS3/E3 interface to which this entry is
               applicable.  The interface identified by a
               particular value of this index is the same
               interface as identified by the same value an
               dsx3LineIndex object instance."
        ::= { dsx3CurrentEntry 1 }

   dsx3CurrentPESs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit
               Errored Seconds."
        ::= { dsx3CurrentEntry 2 }

   dsx3CurrentPSESs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit
               Severely Errored Seconds."
        ::= { dsx3CurrentEntry 3 }

   dsx3CurrentSEFSs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of
               Severely Errored Framing Seconds."
        ::= { dsx3CurrentEntry 4 }






   dsx3CurrentUASs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of
               Unavailable Seconds."
        ::= { dsx3CurrentEntry 5 }

   dsx3CurrentLCVs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Line
               Coding Violations."
        ::= { dsx3CurrentEntry 6 }

   dsx3CurrentPCVs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit
               Coding Violations."
        ::= { dsx3CurrentEntry 7 }

   dsx3CurrentLESs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of Line Errored Seconds."
        ::= { dsx3CurrentEntry 8 }

   dsx3CurrentCCVs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of C-bit Coding Violations."
        ::= { dsx3CurrentEntry 9 }

   dsx3CurrentCESs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION





               "The number of C-bit Errored Seconds."
        ::= { dsx3CurrentEntry 10 }

   dsx3CurrentCSESs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of C-bit Severely Errored Seconds."
        ::= { dsx3CurrentEntry 11 }

   -- the DS3/E3 Interval Table

   dsx3IntervalTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx3IntervalEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS3/E3 Interval Table contains various
               statistics collected by each DS3/E3 Interface over
               the previous 24 hours of operation.  The past 24
               hours are broken into 96 completed 15 minute
               intervals.  Each row in this table represents one
               such interval (identified by dsx3IntervalNumber)
               and for one specific interface (identified by
               dsx3IntervalIndex)."
        ::= { ds3 7 }

   dsx3IntervalEntry OBJECT-TYPE
        SYNTAX  Dsx3IntervalEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "An entry in the DS3/E3 Interval table."
        INDEX   { dsx3IntervalIndex, dsx3IntervalNumber }
        ::= { dsx3IntervalTable 1 }

   Dsx3IntervalEntry ::=
        SEQUENCE {
            dsx3IntervalIndex           InterfaceIndex,
            dsx3IntervalNumber          INTEGER,
            dsx3IntervalPESs            PerfIntervalCount,
            dsx3IntervalPSESs           PerfIntervalCount,
            dsx3IntervalSEFSs           PerfIntervalCount,
            dsx3IntervalUASs            PerfIntervalCount,
            dsx3IntervalLCVs            PerfIntervalCount,
            dsx3IntervalPCVs            PerfIntervalCount,
            dsx3IntervalLESs            PerfIntervalCount,





            dsx3IntervalCCVs            PerfIntervalCount,
            dsx3IntervalCESs            PerfIntervalCount,
            dsx3IntervalCSESs           PerfIntervalCount,
            dsx3IntervalValidData       TruthValue
        }

   dsx3IntervalIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
        STATUS  current
        DESCRIPTION
               "The index value which uniquely identifies the
               DS3/E3 interface to which this entry is
               applicable.  The interface identified by a
               particular value of this index is the same
               interface as identified by the same value an
               dsx3LineIndex object instance."
        ::= { dsx3IntervalEntry 1 }

   dsx3IntervalNumber OBJECT-TYPE
        SYNTAX  INTEGER (1..96)
        MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
        STATUS  current
        DESCRIPTION
               "A number between 1 and 96, where 1 is the most
               recently completed 15 minute interval and 96 is
               the 15 minutes interval completed 23 hours and 45
               minutes prior to interval 1."
        ::= { dsx3IntervalEntry 2 }

   dsx3IntervalPESs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit
               Errored Seconds."
        ::= { dsx3IntervalEntry 3 }

   dsx3IntervalPSESs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit
               Severely Errored Seconds."





        ::= { dsx3IntervalEntry 4 }

   dsx3IntervalSEFSs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of
               Severely Errored Framing Seconds."
        ::= { dsx3IntervalEntry 5 }

   dsx3IntervalUASs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of
               Unavailable Seconds.  This object may decrease if
               the occurrence of unavailable seconds occurs across
               an interval boundary."
        ::= { dsx3IntervalEntry 6 }

   dsx3IntervalLCVs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Line
               Coding Violations."
        ::= { dsx3IntervalEntry 7 }

   dsx3IntervalPCVs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit
               Coding Violations."
        ::= { dsx3IntervalEntry 8 }

   dsx3IntervalLESs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of Line Errored  Seconds  (BPVs  or
               illegal  zero  sequences)."
        ::= { dsx3IntervalEntry 9 }





    dsx3IntervalCCVs OBJECT-TYPE
         SYNTAX  PerfIntervalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The number of C-bit Coding Violations."
         ::= { dsx3IntervalEntry 10 }

    dsx3IntervalCESs OBJECT-TYPE
         SYNTAX  PerfIntervalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The number of C-bit Errored Seconds."
         ::= { dsx3IntervalEntry 11 }

    dsx3IntervalCSESs OBJECT-TYPE
         SYNTAX  PerfIntervalCount
         MAX-ACCESS  read-only
         STATUS  current
         DESCRIPTION
                "The number of C-bit Severely Errored Seconds."
         ::= { dsx3IntervalEntry 12 }

    dsx3IntervalValidData OBJECT-TYPE
         SYNTAX  TruthValue
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
                " This variable indicates if the data for this
                interval is valid."
         ::= { dsx3IntervalEntry 13 }

   -- the DS3/E3 Total

   dsx3TotalTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx3TotalEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS3/E3 Total Table contains the cumulative
               sum of the various statistics for the 24 hour
               period preceding the current interval."
        ::= { ds3 8 }

   dsx3TotalEntry OBJECT-TYPE
        SYNTAX  Dsx3TotalEntry
        MAX-ACCESS  not-accessible





        STATUS  current
        DESCRIPTION
               "An entry in the DS3/E3 Total table."
       INDEX   { dsx3TotalIndex }
        ::= { dsx3TotalTable 1 }

   Dsx3TotalEntry ::=
        SEQUENCE {
            dsx3TotalIndex      InterfaceIndex,
            dsx3TotalPESs       PerfTotalCount,
            dsx3TotalPSESs      PerfTotalCount,
            dsx3TotalSEFSs      PerfTotalCount,
            dsx3TotalUASs       PerfTotalCount,
            dsx3TotalLCVs       PerfTotalCount,
            dsx3TotalPCVs       PerfTotalCount,
            dsx3TotalLESs       PerfTotalCount,
            dsx3TotalCCVs       PerfTotalCount,
            dsx3TotalCESs       PerfTotalCount,
            dsx3TotalCSESs      PerfTotalCount
        }

   dsx3TotalIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
        STATUS  current
        DESCRIPTION
               "The index value which uniquely identifies the
               DS3/E3 interface to which this entry is
               applicable.  The interface identified by a
               particular value of this index is the same
               interface as identified by the same value an
               dsx3LineIndex object instance."
        ::= { dsx3TotalEntry 1 }

   dsx3TotalPESs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit
               Errored Seconds, encountered by a DS3 interface in
               the previous 24 hour interval. Invalid 15 minute
               intervals count as 0."
        ::= { dsx3TotalEntry 2 }

   dsx3TotalPSESs OBJECT-TYPE
        SYNTAX  PerfTotalCount





        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit
               Severely Errored Seconds, encountered by a DS3
               interface in the previous 24 hour interval.
               Invalid 15 minute intervals count as 0."
        ::= { dsx3TotalEntry 3 }

   dsx3TotalSEFSs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of
               Severely Errored Framing Seconds, encountered by a
               DS3/E3 interface in the previous 24 hour interval.
               Invalid 15 minute intervals count as 0."
        ::= { dsx3TotalEntry 4 }

   dsx3TotalUASs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of
               Unavailable Seconds, encountered by a DS3
               interface in the previous 24 hour interval.
               Invalid 15 minute intervals count as 0."
        ::= { dsx3TotalEntry 5 }

   dsx3TotalLCVs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Line
               Coding Violations encountered by a DS3/E3
               interface in the previous 24 hour interval.
               Invalid 15 minute intervals count as 0."
        ::= { dsx3TotalEntry 6 }

   dsx3TotalPCVs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of P-bit





               Coding Violations, encountered by a DS3 interface
               in the previous 24 hour interval. Invalid 15
               minute intervals count as 0."
        ::= { dsx3TotalEntry 7 }

   dsx3TotalLESs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of Line Errored  Seconds  (BPVs  or
               illegal  zero  sequences) encountered by a DS3/E3
               interface in the previous 24 hour interval.
               Invalid 15 minute intervals count as 0."
        ::= { dsx3TotalEntry 8 }

   dsx3TotalCCVs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of C-bit Coding Violations encountered
               by a DS3 interface in the previous 24 hour
               interval. Invalid 15 minute intervals count as 0."
        ::= { dsx3TotalEntry 9 }

   dsx3TotalCESs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of C-bit Errored Seconds encountered
               by a DS3 interface in the previous 24 hour
               interval. Invalid 15 minute intervals count as 0."
        ::= { dsx3TotalEntry 10 }

   dsx3TotalCSESs OBJECT-TYPE
        SYNTAX  PerfTotalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of C-bit Severely Errored Seconds
               encountered by a DS3 interface in the previous 24
               hour interval. Invalid 15 minute intervals count
               as 0."
        ::= { dsx3TotalEntry 11 }







   -- The DS3 Far End Group

   -- The DS3 Far End Group consists of four tables :
   --   DS3 Far End Configuration
   --   DS3 Far End Current
   --   DS3 Far End Interval
   --   DS3 Far End Total

   -- The DS3 Far End Configuration Table

   dsx3FarEndConfigTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx3FarEndConfigEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS3 Far End Configuration Table contains
               configuration information reported in the C-bits
               from the remote end."
        ::= { ds3 9 }

   dsx3FarEndConfigEntry OBJECT-TYPE
        SYNTAX  Dsx3FarEndConfigEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "An entry in the DS3 Far End Configuration table."
       INDEX   { dsx3FarEndLineIndex }
        ::= { dsx3FarEndConfigTable 1 }

   Dsx3FarEndConfigEntry ::=
        SEQUENCE {
           dsx3FarEndLineIndex          InterfaceIndex,
           dsx3FarEndEquipCode           DisplayString,
           dsx3FarEndLocationIDCode      DisplayString,
           dsx3FarEndFrameIDCode         DisplayString,
           dsx3FarEndUnitCode            DisplayString,
           dsx3FarEndFacilityIDCode      DisplayString
        }

   dsx3FarEndLineIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
        STATUS  current
        DESCRIPTION
               "The index value which uniquely identifies the DS3
               interface to which this entry is applicable.  The
               interface identified by a particular value of this





               index is the same interface as identified by the
               same value an dsx3LineIndex object instance."
       ::= { dsx3FarEndConfigEntry 1 }

   dsx3FarEndEquipCode OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..10))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This is the Far End Equipment Identification code
               that describes the specific piece of equipment.
               It is sent within the Path Identification
               Message."
        ::= { dsx3FarEndConfigEntry 2 }

   dsx3FarEndLocationIDCode OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..11))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This is the Far End Location Identification code
               that describes the specific location of the
               equipment.  It is sent within the Path
               Identification Message."
        ::= { dsx3FarEndConfigEntry 3 }

   dsx3FarEndFrameIDCode OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..10))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This is the Far End Frame Identification code
               that identifies where the equipment is located
               within a building at a given location.  It is sent
               within the Path Identification Message."
        ::= { dsx3FarEndConfigEntry 4 }

   dsx3FarEndUnitCode OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..6))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This is the Far End code that identifies the
               equipment location within a bay.  It is sent
               within the Path Identification Message."
        ::= { dsx3FarEndConfigEntry 5 }

   dsx3FarEndFacilityIDCode OBJECT-TYPE





        SYNTAX  DisplayString (SIZE (0..38))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This code identifies a specific Far End DS3 path.
               It is sent within the Path Identification
               Message."
        ::= { dsx3FarEndConfigEntry 6 }

   -- The DS3 Far End Current

   dsx3FarEndCurrentTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx3FarEndCurrentEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS3 Far End Current table contains various
               statistics being collected for the current 15
               minute interval.  The statistics are collected
               from the far end block error code within the C-
               bits."
        ::= { ds3 10 }

   dsx3FarEndCurrentEntry OBJECT-TYPE
        SYNTAX  Dsx3FarEndCurrentEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "An entry in the DS3 Far End Current table."
        INDEX   { dsx3FarEndCurrentIndex }
        ::= { dsx3FarEndCurrentTable 1 }

   Dsx3FarEndCurrentEntry ::=
        SEQUENCE {
            dsx3FarEndCurrentIndex        InterfaceIndex,
            dsx3FarEndTimeElapsed         INTEGER,
            dsx3FarEndValidIntervals      INTEGER,
            dsx3FarEndCurrentCESs         PerfCurrentCount,
            dsx3FarEndCurrentCSESs        PerfCurrentCount,
            dsx3FarEndCurrentCCVs         PerfCurrentCount,
            dsx3FarEndCurrentUASs         PerfCurrentCount,
            dsx3FarEndInvalidIntervals    INTEGER
       }

    dsx3FarEndCurrentIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index





        STATUS  current
        DESCRIPTION
               "The index value which uniquely identifies the DS3
               interface to which this entry is applicable.  The
               interface identified by a particular value of this
               index is identical to the interface identified by
               the same value of dsx3LineIndex."
        ::= { dsx3FarEndCurrentEntry 1 }

   dsx3FarEndTimeElapsed OBJECT-TYPE
        SYNTAX  INTEGER (0..899)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of seconds that have elapsed since the
               beginning of the far end current error-measurement
               period. If, for some reason, such as an adjustment
               in the system's time-of-day clock, the current
               interval exceeds the maximum value, the agent will
               return the maximum value."
        ::= { dsx3FarEndCurrentEntry 2 }

   dsx3FarEndValidIntervals OBJECT-TYPE
        SYNTAX  INTEGER (0..96)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The number of previous far end intervals for
               which data was collected.  The value will be 96
               unless the interface was brought online within the
               last 24 hours, in which case the value will be the
               number of complete 15 minute far end intervals
               since the interface has been online. In the case
               where the agent is a proxy, it is possible that
               some intervals are unavailable.  In this case,
               this interval is the maximum interval number for
               which data is available."
        ::= { dsx3FarEndCurrentEntry 3 }

   dsx3FarEndCurrentCESs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Errored Seconds."
        ::= { dsx3FarEndCurrentEntry 4 }






   dsx3FarEndCurrentCSESs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Severely Errored Seconds."
        ::= { dsx3FarEndCurrentEntry 5 }

   dsx3FarEndCurrentCCVs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Coding Violations reported via the far end
               block error count."
        ::= { dsx3FarEndCurrentEntry 6 }

   dsx3FarEndCurrentUASs OBJECT-TYPE
        SYNTAX  PerfCurrentCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Far End
               unavailable seconds."
        ::= { dsx3FarEndCurrentEntry 7 }

   dsx3FarEndInvalidIntervals OBJECT-TYPE
        SYNTAX  INTEGER (0..96)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               " The number of intervals in the range from 0 to
               dsx3FarEndValidIntervals for which no data is
               available.  This object will typically be zero
               except in cases where the data for some intervals
               are not available (e.g., in proxy situations)."
        ::= { dsx3FarEndCurrentEntry 8 }

   -- The DS3 Far End Interval Table

   dsx3FarEndIntervalTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx3FarEndIntervalEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS3 Far End Interval Table contains various





               statistics collected by each DS3 interface over
               the previous 24 hours of operation.  The past 24
               hours are broken into 96 completed 15 minute
               intervals."
        ::= { ds3 11 }

   dsx3FarEndIntervalEntry OBJECT-TYPE
        SYNTAX  Dsx3FarEndIntervalEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "An entry in the DS3 Far End Interval table."
        INDEX   { dsx3FarEndIntervalIndex,
                  dsx3FarEndIntervalNumber }
        ::= { dsx3FarEndIntervalTable 1 }

   Dsx3FarEndIntervalEntry ::=
        SEQUENCE {
             dsx3FarEndIntervalIndex      InterfaceIndex,
             dsx3FarEndIntervalNumber     INTEGER,
             dsx3FarEndIntervalCESs       PerfIntervalCount,
             dsx3FarEndIntervalCSESs      PerfIntervalCount,
             dsx3FarEndIntervalCCVs       PerfIntervalCount,
             dsx3FarEndIntervalUASs       PerfIntervalCount,
             dsx3FarEndIntervalValidData  TruthValue
       }

   dsx3FarEndIntervalIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
        STATUS  current
        DESCRIPTION
               "The index value which uniquely identifies the DS3
               interface to which this entry is applicable.  The
               interface identified by a particular value of this
               index is identical to the interface identified by
               the same value of dsx3LineIndex."
        ::= { dsx3FarEndIntervalEntry 1 }

   dsx3FarEndIntervalNumber OBJECT-TYPE
       SYNTAX  INTEGER (1..96)
       MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
       STATUS  current
       DESCRIPTION
               "A number between 1 and 96, where 1 is the most
               recently completed 15 minute interval and 96 is





               the 15 minutes interval completed 23 hours and 45
               minutes prior to interval 1."
       ::= { dsx3FarEndIntervalEntry 2 }

   dsx3FarEndIntervalCESs OBJECT-TYPE
       SYNTAX  PerfIntervalCount
       MAX-ACCESS  read-only
       STATUS  current
       DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Errored Seconds encountered by a DS3
               interface in one of the previous 96, individual 15
               minute, intervals. In the case where the agent is
               a proxy and data is not available, return
               noSuchInstance."
       ::= { dsx3FarEndIntervalEntry 3 }

   dsx3FarEndIntervalCSESs OBJECT-TYPE
       SYNTAX  PerfIntervalCount
       MAX-ACCESS  read-only
       STATUS  current
       DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Severely Errored Seconds."
        ::= { dsx3FarEndIntervalEntry 4 }

   dsx3FarEndIntervalCCVs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Coding Violations reported via the far end
               block error count."
        ::= { dsx3FarEndIntervalEntry 5 }

   dsx3FarEndIntervalUASs OBJECT-TYPE
        SYNTAX  PerfIntervalCount
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "The counter associated with the number of Far End
               unavailable seconds."
        ::= { dsx3FarEndIntervalEntry 6 }

   dsx3FarEndIntervalValidData OBJECT-TYPE
        SYNTAX  TruthValue
        MAX-ACCESS  read-only





        STATUS  current
        DESCRIPTION
               " This variable indicates if the data for this
               interval is valid."
        ::= { dsx3FarEndIntervalEntry 7 }

   -- The DS3 Far End Total

   dsx3FarEndTotalTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx3FarEndTotalEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS3 Far End Total Table contains the
               cumulative sum of the various statistics for the
               24 hour period preceding the current interval."
        ::= { ds3 12 }

   dsx3FarEndTotalEntry OBJECT-TYPE
        SYNTAX  Dsx3FarEndTotalEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "An entry in the DS3 Far End Total table."
        INDEX   { dsx3FarEndTotalIndex }
        ::= { dsx3FarEndTotalTable 1 }

   Dsx3FarEndTotalEntry ::=
        SEQUENCE {
            dsx3FarEndTotalIndex       InterfaceIndex,
            dsx3FarEndTotalCESs        PerfTotalCount,
            dsx3FarEndTotalCSESs       PerfTotalCount,
            dsx3FarEndTotalCCVs        PerfTotalCount,
            dsx3FarEndTotalUASs        PerfTotalCount
        }

   dsx3FarEndTotalIndex OBJECT-TYPE
       SYNTAX  InterfaceIndex
       MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
       STATUS  current
       DESCRIPTION
               "The index value which uniquely identifies the DS3
               interface to which this entry is applicable.  The
               interface identified by a particular value of this
               index is identical to the interface identified by
               the same value of dsx3LineIndex."
       ::= { dsx3FarEndTotalEntry 1 }





   dsx3FarEndTotalCESs OBJECT-TYPE
       SYNTAX  PerfTotalCount
       MAX-ACCESS  read-only
       STATUS  current
       DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Errored Seconds encountered by a DS3
               interface in the previous 24 hour interval.
               Invalid 15 minute intervals count as 0."
       ::= { dsx3FarEndTotalEntry 2 }

   dsx3FarEndTotalCSESs OBJECT-TYPE
       SYNTAX  PerfTotalCount
       MAX-ACCESS  read-only
       STATUS  current
       DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Severely Errored Seconds encountered by a
               DS3 interface in the previous 24 hour interval.
               Invalid 15 minute intervals count as 0."
       ::= { dsx3FarEndTotalEntry 3 }

   dsx3FarEndTotalCCVs OBJECT-TYPE
       SYNTAX  PerfTotalCount
       MAX-ACCESS  read-only
       STATUS  current
       DESCRIPTION
               "The counter associated with the number of Far End
               C-bit Coding Violations reported via the far end
               block error count encountered by a DS3 interface
               in the previous 24 hour interval. Invalid 15
               minute intervals count as 0."
       ::= { dsx3FarEndTotalEntry 4 }

   dsx3FarEndTotalUASs OBJECT-TYPE
       SYNTAX  PerfTotalCount
       MAX-ACCESS  read-only
       STATUS  current
       DESCRIPTION
               "The counter associated with the number of Far End
               unavailable seconds encountered by a DS3 interface
               in the previous 24 hour interval.  Invalid 15
               minute intervals count as 0."
       ::= { dsx3FarEndTotalEntry 5 }

   -- the DS3/E3 Fractional Table

   -- This table is deprecated.





   dsx3FracTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF Dsx3FracEntry
       MAX-ACCESS  not-accessible
       STATUS  deprecated
       DESCRIPTION
               "This table is deprecated in favour of using
               ifStackTable.

               Implementation of this table was optional.  It was
               designed for those systems dividing a DS3/E3 into
               channels containing different data streams that
               are of local interest.

               The DS3/E3 fractional table identifies which
               DS3/E3 channels associated with a CSU are being
               used to support a logical interface, i.e., an
               entry in the interfaces table from the Internet-
               standard MIB.

               For example, consider a DS3 device with 4 high
               speed links carrying router traffic, a feed for
               voice, a feed for video, and a synchronous channel
               for a non-routed protocol.  We might describe the
               allocation of channels, in the dsx3FracTable, as
               follows:
               dsx3FracIfIndex.2. 1 = 3  dsx3FracIfIndex.2.15 = 4
               dsx3FracIfIndex.2. 2 = 3  dsx3FracIfIndex.2.16 = 6
               dsx3FracIfIndex.2. 3 = 3  dsx3FracIfIndex.2.17 = 6
               dsx3FracIfIndex.2. 4 = 3  dsx3FracIfIndex.2.18 = 6
               dsx3FracIfIndex.2. 5 = 3  dsx3FracIfIndex.2.19 = 6
               dsx3FracIfIndex.2. 6 = 3  dsx3FracIfIndex.2.20 = 6
               dsx3FracIfIndex.2. 7 = 4  dsx3FracIfIndex.2.21 = 6
               dsx3FracIfIndex.2. 8 = 4  dsx3FracIfIndex.2.22 = 6
               dsx3FracIfIndex.2. 9 = 4  dsx3FracIfIndex.2.23 = 6
               dsx3FracIfIndex.2.10 = 4  dsx3FracIfIndex.2.24 = 6
               dsx3FracIfIndex.2.11 = 4  dsx3FracIfIndex.2.25 = 6
               dsx3FracIfIndex.2.12 = 5  dsx3FracIfIndex.2.26 = 6
               dsx3FracIfIndex.2.13 = 5  dsx3FracIfIndex.2.27 = 6
               dsx3FracIfIndex.2.14 = 5  dsx3FracIfIndex.2.28 = 6
               For dsx3M23, dsx3 SYNTRAN, dsx3CbitParity, and
               dsx3ClearChannel  there are 28 legal channels,
               numbered 1 through 28.

               For e3Framed there are 16 legal channels, numbered
               1 through 16.  The channels (1..16) correspond
               directly to the equivalently numbered time-slots."
        ::= { ds3 13 }






   dsx3FracEntry OBJECT-TYPE
        SYNTAX  Dsx3FracEntry
        MAX-ACCESS  not-accessible
        STATUS  deprecated
        DESCRIPTION
                       "An entry in the DS3 Fractional table."
       INDEX   { dsx3FracIndex, dsx3FracNumber }
       ::= { dsx3FracTable 1 }

   Dsx3FracEntry ::=
        SEQUENCE {
            dsx3FracIndex     INTEGER,
            dsx3FracNumber    INTEGER,
            dsx3FracIfIndex   INTEGER
       }

   dsx3FracIndex OBJECT-TYPE
       SYNTAX  INTEGER (1..'7fffffff'h)
       MAX-ACCESS  read-only -- read-only since originally an
                                 -- SMIv1 index
       STATUS  deprecated
       DESCRIPTION
               "The index value which uniquely identifies  the
               DS3  interface  to which this entry is applicable
               The interface identified by a  particular value
               of  this  index is the same interface as
               identified by the same value  an  dsx3LineIndex
               object instance."
       ::= { dsx3FracEntry 1 }

   dsx3FracNumber OBJECT-TYPE
       SYNTAX  INTEGER (1..31)
       MAX-ACCESS  read-only  -- read-only since originally an
                               -- SMIv1 index
       STATUS  deprecated
       DESCRIPTION
               "The channel number for this entry."
      ::= { dsx3FracEntry 2 }

   dsx3FracIfIndex OBJECT-TYPE
      SYNTAX  INTEGER (0..'7fffffff'h)
      MAX-ACCESS  read-write
      STATUS  deprecated
      DESCRIPTION
              "An index value that uniquely identifies an
              interface.  The interface identified by a
              particular value of this index is the same
              interface as  identified by the same value an





              ifIndex object instance. If no interface is
              currently using a channel, the value should be
              zero.  If a single interface occupies more  than
              one  time slot,  that ifIndex value will be found
              in multiple time slots."
      ::= { dsx3FracEntry 3 }

    -- DS3 TRAPS

   ds3Traps OBJECT IDENTIFIER ::= { ds3 15 }

   dsx3LineStatusChange NOTIFICATION-TYPE
       OBJECTS { dsx3LineStatus,
                 dsx3LineStatusLastChange }
       STATUS  current
       DESCRIPTION
               "A dsx3LineStatusChange trap is sent when the
               value of an instance of dsx3LineStatus changes. It
               can be utilized by an NMS to trigger polls.  When
               the line status change results in a lower level
               line status change (i.e., ds1), then no traps for
               the lower level are sent."
        ::= { ds3Traps 0 1 }

   -- conformance information

   ds3Conformance OBJECT IDENTIFIER ::= { ds3 14 }
   ds3Groups      OBJECT IDENTIFIER ::= { ds3Conformance 1 }
   ds3Compliances OBJECT IDENTIFIER ::= { ds3Conformance 2 }

   -- compliance statements

   ds3Compliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for DS3/E3 interfaces."
       MODULE  -- this module
           MANDATORY-GROUPS { ds3NearEndConfigGroup,
                              ds3NearEndStatisticsGroup }

           GROUP       ds3FarEndGroup
           DESCRIPTION
               "Implementation of this group is optional for all
               systems that attach to a DS3 Interface.  However,
               only C-bit Parity and SYNTRAN DS3 applications
               have the capability (option) of providing this
               information."
           GROUP       ds3NearEndOptionalTrapGroup





           DESCRIPTION
               "Implementation of this group is optional for all
               systems that attach to a DS3 Interface.  If it is
               implemented then ds3NearEndOptionalConfigGroup
               should also be implemented."
           GROUP       ds3NearEndOptionalConfigGroup
           DESCRIPTION
               "Implementation of this group is optional for all
               systems that attach to a DS3 interface."

           OBJECT      dsx3LineType
           MIN-ACCESS  read-only
           DESCRIPTION
               "Write access for the line type is not required."

           OBJECT      dsx3LineCoding
           MIN-ACCESS  read-only
           DESCRIPTION
               "Write access for the line coding is not
               required."

           OBJECT      dsx3SendCode
           MIN-ACCESS  read-only
           DESCRIPTION
               "Write access for the send code is not required."

           OBJECT      dsx3LoopbackConfig
           MIN-ACCESS  read-only
           DESCRIPTION
               "Write access for loopbacks is not required."

           OBJECT      dsx3TransmitClockSource
           MIN-ACCESS  read-only
           DESCRIPTION
               "Write access for the transmit clock source is not
               required."

           OBJECT      dsx3LineLength
           MIN-ACCESS  read-only
           DESCRIPTION
               "Write access for the line length is not
               required."

           OBJECT      dsx3Channelization
           MIN-ACCESS  read-only
           DESCRIPTION
               "Write access for the channelization is not
               required."





       ::= { ds3Compliances 1 }

   -- units of conformance

   ds3NearEndConfigGroup  OBJECT-GROUP
       OBJECTS { dsx3LineIndex,
                 dsx3TimeElapsed,
                 dsx3ValidIntervals,
                 dsx3LineType,
                 dsx3LineCoding,
                 dsx3SendCode,
                 dsx3CircuitIdentifier,
                 dsx3LoopbackConfig,
                 dsx3LineStatus,
                 dsx3TransmitClockSource,
                 dsx3InvalidIntervals,
                 dsx3LineLength,
                 dsx3LoopbackStatus,
                 dsx3Channelization,
                 dsx3Ds1ForRemoteLoop}
       STATUS  current
       DESCRIPTION
               "A collection of objects providing configuration
               information applicable to all DS3/E3 interfaces."
       ::= { ds3Groups 1 }

   ds3NearEndStatisticsGroup OBJECT-GROUP
       OBJECTS { dsx3CurrentIndex,
                 dsx3CurrentPESs,
                 dsx3CurrentPSESs,
                 dsx3CurrentSEFSs,
                 dsx3CurrentUASs,
                 dsx3CurrentLCVs,
                 dsx3CurrentPCVs,
                 dsx3CurrentLESs,
                 dsx3CurrentCCVs,
                 dsx3CurrentCESs,
                 dsx3CurrentCSESs,
                 dsx3IntervalIndex,
                 dsx3IntervalNumber,
                 dsx3IntervalPESs,
                 dsx3IntervalPSESs,
                 dsx3IntervalSEFSs,
                 dsx3IntervalUASs,
                 dsx3IntervalLCVs,
                 dsx3IntervalPCVs,
                 dsx3IntervalLESs,
                 dsx3IntervalCCVs,





                 dsx3IntervalCESs,
                 dsx3IntervalCSESs,
                 dsx3IntervalValidData,
                 dsx3TotalIndex,
                 dsx3TotalPESs,
                 dsx3TotalPSESs,
                 dsx3TotalSEFSs,
                 dsx3TotalUASs,
                 dsx3TotalLCVs,
                 dsx3TotalPCVs,
                 dsx3TotalLESs,
                 dsx3TotalCCVs,
                 dsx3TotalCESs,
                 dsx3TotalCSESs }
       STATUS  current
       DESCRIPTION
               "A collection of objects providing statistics
               information applicable to all DS3/E3 interfaces."
       ::= { ds3Groups 2 }

   ds3FarEndGroup  OBJECT-GROUP
       OBJECTS { dsx3FarEndLineIndex,
                 dsx3FarEndEquipCode,
                 dsx3FarEndLocationIDCode,
                 dsx3FarEndFrameIDCode,
                 dsx3FarEndUnitCode,
                 dsx3FarEndFacilityIDCode,
                 dsx3FarEndCurrentIndex,
                 dsx3FarEndTimeElapsed,
                 dsx3FarEndValidIntervals,
                 dsx3FarEndCurrentCESs,
                 dsx3FarEndCurrentCSESs,
                 dsx3FarEndCurrentCCVs,
                 dsx3FarEndCurrentUASs,
                 dsx3FarEndInvalidIntervals,
                 dsx3FarEndIntervalIndex,
                 dsx3FarEndIntervalNumber,
                 dsx3FarEndIntervalCESs,
                 dsx3FarEndIntervalCSESs,
                 dsx3FarEndIntervalCCVs,
                 dsx3FarEndIntervalUASs,
                 dsx3FarEndIntervalValidData,
                 dsx3FarEndTotalIndex,
                 dsx3FarEndTotalCESs,
                 dsx3FarEndTotalCSESs,
                 dsx3FarEndTotalCCVs,
                 dsx3FarEndTotalUASs }
       STATUS  current





       DESCRIPTION
               "A collection of objects providing remote
               configuration and statistics information
               applicable to C-bit Parity and SYNTRAN DS3
               interfaces."
       ::= { ds3Groups 3 }

   ds3DeprecatedGroup OBJECT-GROUP

       OBJECTS { dsx3IfIndex,
                 dsx3FracIndex,
                 dsx3FracNumber,
                 dsx3FracIfIndex }
       STATUS  deprecated
       DESCRIPTION
               "A collection of obsolete objects that may be
               implemented for backwards compatibility."
       ::= { ds3Groups 4 }

   ds3NearEndOptionalConfigGroup OBJECT-GROUP
       OBJECTS { dsx3LineStatusLastChange,
                 dsx3LineStatusChangeTrapEnable }

       STATUS    current
       DESCRIPTION
               "A collection of objects that may be implemented
               on DS3/E3 interfaces."
       ::= { ds3Groups 5 }

   ds3NearEndOptionalTrapGroup NOTIFICATION-GROUP
       NOTIFICATIONS { dsx3LineStatusChange }
       STATUS    current
       DESCRIPTION
               "A collection of notifications that may be
               implemented on DS3/E3 interfaces."
       ::= { ds3Groups 6 }

   END














