DVB-RCS-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY,
       OBJECT-TYPE,
       Integer32,
       Unsigned32,
       transmission
           FROM SNMPv2-SMI          -- [RFC2578]
       TEXTUAL-CONVENTION,
       RowStatus
           FROM SNMPv2-TC           -- [RFC2579]
       OBJECT-GROUP,
       MODULE-COMPLIANCE
           FROM SNMPv2-CONF         -- [RFC2580]
       SnmpAdminString
           FROM SNMP-FRAMEWORK-MIB  -- [RFC3411]
       InetAddressType,
       InetAddress,
       InetAddressPrefixLength,
       InetPortNumber
           FROM INET-ADDRESS-MIB    -- [RFC4001]
       Uri
           FROM URI-TC-MIB          -- [RFC5017]
       Dscp,
       DscpOrAny
           FROM DIFFSERV-DSCP-TC    -- [RFC3289]
       ;

   dvbRcsMib MODULE-IDENTITY
       LAST-UPDATED "201002161200Z"
       ORGANIZATION "The SatLabs Group"
       CONTACT-INFO
              "The SatLabs Group
               Web:    www.satlabs.org
               E-mail: info@satlabs.org"
       DESCRIPTION
           "DVB-RCS MIB subtree.

            This MIB module applies to equipment that is a Return
            Channel Satellite Terminal (RCST), defined in the Digital
            Video Broadcasting Return Channel via Satellite system
            (DVB-RCS) standard (ETSI EN 301 790 Digital Video
            Broadcasting (DVB); Interaction Channel for Satellite
            Distribution Systems, European Telecommunications
            Standards Institute (ETSI)).





            It defines a set of MIB objects to characterize the
            behavior and performance of network-layer entities
            implementing DVB-RCS.
            This MIB module is intended to be used by DVB-RCS
            equipment following the SatLabs System Recommendations,
            defined by the SatLabs Group and available at
            www.satlabs.org.
            Note that, if not stated otherwise in the object
            DESCRIPTION clause, all writable objects are
            persistent.

            Copyright (C) The IETF Trust (2010).  This version of
            this MIB module is part of RFC 5728; see the RFC itself
            for full legal notices."
       REVISION "200907201200Z"
       DESCRIPTION
           "Revision of this MIB module, following MIB doctor review
           and adjustments based on the MIB authoring guidelines
           from the IETF."
           ::= { transmission 239 }

   --==============================================================
   -- Textual Conventions
   --==============================================================
   DvbRcsSatLabsProfileMap ::= TEXTUAL-CONVENTION
       STATUS current
       DESCRIPTION
           "This textual convention enumerates the declaration of
           the SatLabs-defined terminal profiles.  The mapping to
           the profiles is to be understood as described here.  (0)
           refers to the most significant bit.

            dvbs(0) -> DVBS profile (DVB-S support)
            dvbs2ccm(1) -> DVB-S2 CCM profile (CCM support)
            dvbs2acm(2) -> DVB-S2 ACM profile (CCM, VCM and ACM
            support)"
       REFERENCE
          "SatLabs System Recommendations, available at
          www.satlabs.org."
       SYNTAX BITS     {
               dvbs(0),
               dvbs2ccm(1),
               dvbs2acm(2),
               spare1(3),
               spare2(4),
               spare3(5),
               spare4(6),
               spare5(7),





               spare6(8),
               spare7(9),
               spare8(10),
               spare9(11),
               spare10(12),
               spare11(13),
               spare12(14),
               spare13(15),
               spare14(16),
               spare15(17),
               spare16(18),
               spare17(19),
               spare18(20),
               spare19(21),
               spare20(22),
               spare21(23),
               spare22(24),
               spare23(25),
               spare24(26),
               spare25(27),
               spare26(28),
               spare27(29),
               spare28(30),
               spare29(31)
               }

   DvbRcsSatLabsOptionMap ::= TEXTUAL-CONVENTION
       STATUS current
       DESCRIPTION
           "This textual convention enumerates the declaration of
           the SatLabs-defined options.  A value of 1 indicates
           that the respective option is supported.  The mapping
           to the options is to be understood as described here.
           (0) refers to the most significant bit.

               mpegTrf(0) -> MPEG_TRF
               coarseSync(1) -> COARSE_SYNC
               wideHop(2) -> WIDE_HOPP
               fastHop(3) -> FAST_HOPP
               dynamicMfTdma(4) -> Dynamic_MF_TDMA
               contentionSync(5) -> CONTENTION_SYNC
               qpskLow(6) -> QPSKLOW
               mod16Apsk(7) -> 16APSK
               mod32Apsk(8) -> 32APSK
               normalFec(9) -> NORMALFEC
               multiTs(10) -> MULTITS
               gsTs(11) -> GSTS
               enhQoS(12) -> ENHQOS





               pep(13) -> PEP
               http(14) -> HTTP
               ftp(15) -> FTP
               dns(16) -> DNS
               chIdStrict(17) -> CHID_STRICT
               nlid(18) -> NLID
               snmpMisc(19) -> SNMPMISC

           The support of specific options mandates the support of
           specific objects and access levels."
       REFERENCE
          "SatLabs System Recommendations, available at
          www.satlabs.org."
       SYNTAX BITS     {
               mpegTrf(0),
               coarseSync(1),
               wideHop(2),
               fastHop(3),
               dynamicMfTdma(4),
               contentionSync(5),
               qpskLow(6),
               mod16Apsk(7),
               mod32Apsk(8),
               normalFec(9),
               multiTs(10),
               gsTs(11),
               enhQoS(12),
               pep(13),
               http(14),
               ftp(15),
               dns(16),
               chIdStrict(17),
               nlid(18),
               snmpMisc(19),
               spare1(20),
               spare2(21),
               spare3(22),
               spare4(23),
               spare5(24),
               spare6(25),
               spare7(26),
               spare8(27),
               spare9(28),
               spare10(29),
               spare11(30),
               spare12(31)
               }






   DvbRcsSatLabsFeatureMap ::= TEXTUAL-CONVENTION
          STATUS current
          DESCRIPTION
              "This textual convention enumerates the declaration
              of the SatLabs-specified compatibility and
              configuration features.  A value of 1 indicates that
              the respective feature is supported.  The mapping to
              the features is to be understood as described here.
              (0) refers to the most significant bit.

                  rcstPara(0) -> RCST_PARA feature
                  installLog(1) -> INSTALL_LOG feature
                  enhClassifier(2) -> ENHCLASSIFIER feature
                  routeId(3) -> ROUTE_ID feature
                  oduList(4) -> ODULIST feature
                  extNetwork(5) -> EXTNETWORK feature
                  extControl(6) -> EXTCONTROL feature
                  extConfig(7) -> EXTCONFIG feature
                  extStatus(8) -> EXTSTATUS feature
                  mpaf(9) -> MPAF feature

           The support of specific features mandates the support of
           specific objects and access levels."
          REFERENCE
             "SatLabs System Recommendations, available at
              www.satlabs.org."
          SYNTAX BITS     {
                  rcstPara(0),
                  installLog(1),
                  enhClassifier(2),
                  routeId(3),
                  oduList(4),
                  extNetwork(5),
                  extControl(6),
                  extConfig(7),
                  extStatus(8),
                  mpaf(9),
                  spare1(10),
                  spare2(11),
                  spare3(12),
                  spare4(13),
                  spare5(14),
                  spare6(15),
                  spare7(16),
                  spare8(17),
                  spare9(18),
                  spare10(19),
                  spare11(20),





                  spare12(21),
                  spare13(22),
                  spare14(23),
                  spare15(24),
                  spare16(25),
                  spare17(26),
                  spare18(27),
                  spare19(28),
                  spare20(29),
                  spare21(30),
                  spare22(31)
                  }

   --==============================================================
   -- object type definitions
   --==============================================================
   dvbRcsMibObjects      OBJECT IDENTIFIER ::= {dvbRcsMib 1}
   dvbRcsConformance     OBJECT IDENTIFIER ::= {dvbRcsMib 2}

   dvbRcsRcst        OBJECT IDENTIFIER ::= {dvbRcsMibObjects 1}
   dvbRcsFwdLink     OBJECT IDENTIFIER ::= {dvbRcsMibObjects 2}
   dvbRcsRtnLink     OBJECT IDENTIFIER ::= {dvbRcsMibObjects 3}

   dvbRcsRcstSystem        OBJECT IDENTIFIER ::= {dvbRcsRcst 1}
   dvbRcsRcstNetwork       OBJECT IDENTIFIER ::= {dvbRcsRcst 2}
   dvbRcsRcstInstall       OBJECT IDENTIFIER ::= {dvbRcsRcst 3}
   dvbRcsRcstQos           OBJECT IDENTIFIER ::= {dvbRcsRcst 4}
   dvbRcsRcstControl       OBJECT IDENTIFIER ::= {dvbRcsRcst 5}
   dvbRcsRcstState         OBJECT IDENTIFIER ::= {dvbRcsRcst 6}

   dvbRcsFwdConfig         OBJECT IDENTIFIER ::= {dvbRcsFwdLink 1}
   dvbRcsFwdStatus         OBJECT IDENTIFIER ::= {dvbRcsFwdLink 2}

   dvbRcsRtnConfig         OBJECT IDENTIFIER ::= {dvbRcsRtnLink 1}
   dvbRcsRtnStatus         OBJECT IDENTIFIER ::= {dvbRcsRtnLink 2}

   --==============================================================
   --    dvbRcsRcstSystem sub-tree object types
   --==============================================================
   dvbRcsSystemMibRevision        OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "This object allows the SNMP agent to report the
           implemented MIB module revision.
           The supported REVISION of this module is reported."
   ::= {dvbRcsRcstSystem 1}





   --==============================================================
   -- Options declared according to the textual conventions
   --==============================================================
   dvbRcsSystemSatLabsProfilesDeclaration OBJECT-TYPE
       SYNTAX        DvbRcsSatLabsProfileMap
       MAX-ACCESS    read-only
       STATUS        current
       DESCRIPTION
           "Indicates the SatLabs profiles supported, as defined in
           the SatLabs System Recommendations."
   ::= {dvbRcsRcstSystem 2}

   dvbRcsSystemSatLabsOptionsDeclaration OBJECT-TYPE
       SYNTAX        DvbRcsSatLabsOptionMap
       MAX-ACCESS    read-only
       STATUS        current
       DESCRIPTION
           "Indicates the SatLabs options supported, as defined in
           the SatLabs System Recommendations."
   ::= {dvbRcsRcstSystem 3}

   dvbRcsSystemSatLabsFeaturesDeclaration OBJECT-TYPE
       SYNTAX        DvbRcsSatLabsFeatureMap
       MAX-ACCESS    read-only
       STATUS        current
       DESCRIPTION
           "Indicates the optional compatibility features and minor
            options supported, as defined in the SatLabs System
            Recommendations."
   ::= {dvbRcsRcstSystem 4}

   dvbRcsSystemLocation OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Physical location of the ODU antenna expressed as
            longitude, latitude, and altitude.  The string
            shall have 31 characters in the following format:
                <xxxx.xxx>,<a>,<yyyyy.yyy>,<b>,<zzzz.z>,M
            where x, y and z represents digits,
                a=N or S,
                b=E or W,
            Reading the digits from left to right:
                'x' 7 latitude digits;
                 x digits 1-2 contain the degrees,
                 x digits 3-7 contain the minutes in decimal;
                'y' 8 longitude digits;





                 y digits 1-3 contain the degrees,
                 y digits 4-8 contain the minutes in decimal;
                'z' 5 altitude digits;
                    meters above sea level in decimal;
                '.' is the decimal point;
                ',' is the field separator;
                'M' is the indicator for altitude meters.
            This format is a modified subset of the NMEA 0183
            (National Marine Electronics Association, Interface
            Standard) format for Global Positioning System Fix
            Data.
            This location and the satellite position are used to
            calculate the RCST-satellite path delay.
            Note: The system.sysLocation object of MIB-II provides
            physical location of the IDU unit."
   ::= {dvbRcsRcstSystem 5}

   dvbRcsSystemOduAntennaSize OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "cm"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Diameter of the antenna."
   ::= {dvbRcsRcstSystem 6}

   dvbRcsSystemOduAntennaGain OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x0.1 dBi"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Antenna peak gain of the ODU."
   ::= {dvbRcsRcstSystem 7}

   dvbRcsSystemOduSspa OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x0.1 W"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Power level of the Solid State Power Amplifier
           installed in the ODU."
   ::= {dvbRcsRcstSystem 8}

   dvbRcsSystemOduTxType OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-write





       STATUS              current
       DESCRIPTION
           "Type of transmitter installed in the ODU."
   ::= {dvbRcsRcstSystem 9}

   dvbRcsSystemOduRxType OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
            "Type of LNB installed in the ODU, with
            information such as vendor type, output type (single,
            twin, quad,...), etc."
   ::= {dvbRcsRcstSystem 10}

   dvbRcsSystemOduRxBand OBJECT-TYPE
       SYNTAX              INTEGER   {
                           oduHighRxBand (0),
                           oduLowRxBand  (1)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "LNB High Band / Low Band selector.  High Band corresponds
           to the emission of an 18-26 kHz tone with 0.4-0.8 Vpp in
           the Rx IFL cable:
           (0)    - High Band
           (1)    - Low Band"
   ::= {dvbRcsRcstSystem 11}

   dvbRcsSystemOduRxLO OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x100 Hz"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Frequency of LNB Local Oscillator (in 100 Hz)"
   ::= {dvbRcsRcstSystem 12}

   dvbRcsSystemOduTxLO OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x100 Hz"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Frequency of Block Up-Converter Local Oscillator
           (in 100 Hz)."
   ::= {dvbRcsRcstSystem 13}





   dvbRcsSystemIduPep OBJECT IDENTIFIER ::= {dvbRcsRcstSystem 14}

   dvbRcsTcpPep OBJECT-TYPE
       SYNTAX             INTEGER{
                             disabled (0),
                             enabled (1)
                                 }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Status and control of embedded TCP PEP.
               0 - disabled or not implemented
               1 - enabled"
   ::={dvbRcsSystemIduPep 1}

   dvbRcsHttpPep  OBJECT-TYPE
       SYNTAX              INTEGER{
                              disabled (0),
                              enabled (1)
                                  }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Status and control of embedded HTTP PEP.
               0 - disabled or not implemented
               1 - enabled"
   ::={dvbRcsSystemIduPep 2}

   --==============================================================
   -- ODU structural entities
   --==============================================================

   dvbRcsOduTx         OBJECT IDENTIFIER ::= {dvbRcsRcstSystem 15}
   dvbRcsOduRx         OBJECT IDENTIFIER ::= {dvbRcsRcstSystem 16}
   dvbRcsOduAntenna    OBJECT IDENTIFIER ::= {dvbRcsRcstSystem 17}

   --==============================================================
   -- ODU BUC
   --==============================================================

   dvbRcsOduTxTypeTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF DvbRcsOduTxTypeEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "This table contains the identification of each well-
           known BUC type supported by the IDU and provides its
           associated index."





   ::={dvbRcsOduTx 1}

   dvbRcsOduTxTypeEntry OBJECT-TYPE
       SYNTAX            DvbRcsOduTxTypeEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the BUC type table."
          INDEX   { dvbRcsOduTxTypeIndex }
   ::={dvbRcsOduTxTypeTable 1}

   DvbRcsOduTxTypeEntry ::= SEQUENCE {
                     dvbRcsOduTxTypeIndex          Unsigned32,
                     dvbRcsOduTxTypeDescription    SnmpAdminString
                     }

   dvbRcsOduTxTypeIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..32)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Index for the BUC type."
   ::={dvbRcsOduTxTypeEntry 1}

   dvbRcsOduTxTypeDescription OBJECT-TYPE
       SYNTAX     SnmpAdminString
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Text-based identification of a BUC type."
   ::={dvbRcsOduTxTypeEntry 2}

   dvbRcsOduTxType OBJECT-TYPE
       SYNTAX              Unsigned32
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Index of the selected BUC type."
   ::={dvbRcsOduTx 2}

   --==============================================================
   -- ODU LNB
   --==============================================================

   dvbRcsOduRxTypeTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF DvbRcsOduRxTypeEntry
       MAX-ACCESS not-accessible
       STATUS  current





       DESCRIPTION
           "This table contains the identification of each well-
           known LNB type supported by the IDU and provides its
           associated index."
   ::={dvbRcsOduRx 1}

   dvbRcsOduRxTypeEntry OBJECT-TYPE
       SYNTAX            DvbRcsOduRxTypeEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the LNB type table."
       INDEX   { dvbRcsOduRxTypeIndex }
    ::={dvbRcsOduRxTypeTable 1}

   DvbRcsOduRxTypeEntry ::= SEQUENCE {
                     dvbRcsOduRxTypeIndex           Unsigned32,
                     dvbRcsOduRxTypeDescription     SnmpAdminString
                     }

   dvbRcsOduRxTypeIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..32)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Index for the LNB type."
   ::={dvbRcsOduRxTypeEntry 1}

   dvbRcsOduRxTypeDescription OBJECT-TYPE
       SYNTAX     SnmpAdminString
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Text-based identification of an LNB type."
   ::={dvbRcsOduRxTypeEntry 2}

   dvbRcsOduRxType OBJECT-TYPE
       SYNTAX              Unsigned32
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Index of the selected LNB type."
   ::={dvbRcsOduRx 2}










   --==============================================================
   -- ODU Antenna
   --==============================================================

   dvbRcsOduAntennaTypeTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF DvbRcsOduAntennaTypeEntry
       MAX-ACCESS not-accessible
       STATUS  current
       DESCRIPTION
           "This table contains the identification of each well-
           known antenna type supported by the IDU and provides
           its associated index."
   ::={dvbRcsOduAntenna 1}

   dvbRcsOduAntennaTypeEntry OBJECT-TYPE
       SYNTAX            DvbRcsOduAntennaTypeEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the antenna type table."
       INDEX   { dvbRcsOduAntennaTypeIndex }
   ::={dvbRcsOduAntennaTypeTable 1}

   DvbRcsOduAntennaTypeEntry ::= SEQUENCE {
                 dvbRcsOduAntennaTypeIndex          Unsigned32,
                 dvbRcsOduAntennaTypeDescription    SnmpAdminString
                 }

   dvbRcsOduAntennaTypeIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..32)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Index for the antenna type."
   ::={dvbRcsOduAntennaTypeEntry 1}

   dvbRcsOduAntennaTypeDescription OBJECT-TYPE
       SYNTAX     SnmpAdminString
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
           "Text-based identification of an antenna type."
   ::={dvbRcsOduAntennaTypeEntry 2}

   dvbRcsOduAntennaType OBJECT-TYPE
       SYNTAX              Unsigned32
       MAX-ACCESS          read-write
       STATUS              current





       DESCRIPTION
           "Index of the selected antenna type."
   ::={dvbRcsOduAntenna 2}

   --==============================================================
   -- dvbRcsRcstNetwork sub-tree object types
   --==============================================================

   dvbRcsNetworkOamInetAddressType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The type of Internet address of
           dvbRcsNetworkOamInetAddress.
           If the terminal OAM Internet address is unassigned or
           unknown, then the value of this object is unknown(0)."
   ::= {dvbRcsRcstNetwork 1}

   dvbRcsNetworkOamInetAddress OBJECT-TYPE
       SYNTAX              InetAddress
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "OAM IP Address of the RCST.  This object is used with
           both IP and interfaces MIB-II subgroups.  It uniquely
           determines the interface through which OAM traffic
           passes.
           The OAM IP address may be statically or dynamically
           assigned.  It is system dependent whether the OAM IP
           address and the Traffic IP address are the same address.
           If the terminal has no OAM Internet address assigned or if
           this Internet address is unknown, the value of this
           object is the zero-length OCTET STRING.
           The InetAddressType is given by the
           dvbRcsNetworkOamInetAddressType object."
   ::= {dvbRcsRcstNetwork 2}

   dvbRcsNetworkOamInetAddressPrefixLength OBJECT-TYPE
       SYNTAX              InetAddressPrefixLength
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Prefix length for the OAM IP Address.  If this address
           prefix is unknown or does not apply, the value is zero."
   ::= {dvbRcsRcstNetwork 3}

   dvbRcsNetworkOamInetAddressAssign OBJECT-TYPE





       SYNTAX             INTEGER    {
                   oamInetAddressStatic    (1),
                   oamInetAddressDynamic   (2)
       }
       MAX-ACCESS         read-write
       STATUS             current
       DESCRIPTION
           "Identifies whether the OAM IP address is statically
           (1) or dynamically (2) assigned."
   ::= {dvbRcsRcstNetwork 4}

   dvbRcsNetworkLanInetAddressType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The type of Internet address of dvbRcsNetworkLanInetAddress.
           If the terminal Internet address on the LAN interface is
           unassigned or unknown, then the value of this object is
           unknown(0)."
   ::= {dvbRcsRcstNetwork 5}

   dvbRcsNetworkLanInetAddress OBJECT-TYPE
       SYNTAX              InetAddress
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "IP address of the LAN interface of the terminal.  If the
           terminal has no Internet address assigned on the LAN
           interface or if this Internet address is unknown, the
           value of this object is the zero-length OCTET STRING.
           The InetAddressType is given by the
           dvbRcsNetworkLanInetAddressType object."
   ::= {dvbRcsRcstNetwork 6}

   dvbRcsNetworkLanInetAddressPrefixLength OBJECT-TYPE
       SYNTAX              InetAddressPrefixLength
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Prefix length for the LAN IP Address of the terminal.
           If this address prefix is unknown or does not apply, the
           value is zero."
   ::= {dvbRcsRcstNetwork 7}

   dvbRcsNetworkAirInterfaceDefaultGatewayInetAddressType
   OBJECT-TYPE
       SYNTAX      InetAddressType





       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The type of Internet address of
           dvbRcsNetworkAirInterfaceDefaultGatewayInetAddress.
           If the default gateway Internet address is unassigned or
           unknown, then the value of this object is unknown(0)."
   ::= {dvbRcsRcstNetwork 8}

   dvbRcsNetworkAirInterfaceDefaultGatewayInetAddress OBJECT-TYPE
       SYNTAX              InetAddress
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "IP address of the default gateway for the air
           interface.  If the terminal has no default gateway
           assigned on the air interface or if this Internet address
           is unknown, the value of this object is the zero-length
           OCTET STRING.
           The InetAddressType is given by the
           dvbRcsNetworkAirInterfaceDefaultGatewayInetAddressType
           object."
   ::= {dvbRcsRcstNetwork 9}

   dvbRcsNetworkAirInterfaceDefaultGatewayInetAddressPrefixLength
   OBJECT-TYPE
       SYNTAX              InetAddressPrefixLength
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Prefix length for the IP address of the default gateway
           for the air interface.
           If this address prefix is unknown or does not apply, the
           value is zero."
   ::= {dvbRcsRcstNetwork 10}

   dvbRcsNetworkDnsServers OBJECT IDENTIFIER ::= {dvbRcsRcstNetwork
   11}

   dvbRcsPrimaryDnsServerInetAddressType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The type of Internet address of
           dvbRcsPrimaryDnsServerInetAddress.  If the primary DNS
           server Internet address is unassigned or unknown, then
           the value of this object is unknown(0)."





   ::= { dvbRcsNetworkDnsServers 1}

   dvbRcsPrimaryDnsServerInetAddress OBJECT-TYPE
       SYNTAX              InetAddress
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "IP address of the primary DNS server in the NCC.  If
           the terminal has no primary DNS server assigned or if this
           Internet address is unknown, the value of this object is
           the zero-length OCTET STRING.
           The InetAddressType is given by the
           dvbRcsPrimaryDnsServerInetAddressType object."
   ::= {dvbRcsNetworkDnsServers 2}

   dvbRcsPrimaryDnsServerInetAddressPrefixLength OBJECT-TYPE
       SYNTAX              InetAddressPrefixLength
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Prefix length for the IP address of the primary DNS
           server in the NCC.
           If this address prefix is unknown or does not apply, the
           value is zero."
   ::= { dvbRcsNetworkDnsServers 3}

   dvbRcsSecondaryDnsServerInetAddressType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The type of Internet address of
           dvbRcsSecondaryDnsServerInetAddress.  If the secondary
           DNS server Internet address is unassigned or unknown,
           then the value of this object is unknown(0)."
   ::= { dvbRcsNetworkDnsServers 4}

   dvbRcsSecondaryDnsServerInetAddress OBJECT-TYPE
       SYNTAX              InetAddress
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "IP address of the secondary DNS server in the NCC.  If
           the terminal has no secondary DNS server assigned or if
           this Internet address is unknown, the value of this
           object is the zero-length OCTET STRING.
           The InetAddressType is given by the
           dvbRcsSecondaryDnsServerInetAddressType object."





   ::= {dvbRcsNetworkDnsServers 5}

   dvbRcsSecondaryDnsServerInetAddressPrefixLength OBJECT-TYPE
       SYNTAX              InetAddressPrefixLength
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Prefix length for the IP address of the secondary DNS
           server in the NCC.
           If this address prefix is unknown or does not apply, the
           value is zero."
   ::= { dvbRcsNetworkDnsServers 6}

   dvbRcsNetworkNccMgtInetAddressType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The type of Internet address of
           dvbRcsNetworkNccMgtInetAddress.  If the management server
           Internet address is unassigned or unknown, then the
           value of this object is unknown(0)."
   ::= {dvbRcsRcstNetwork 12}

   dvbRcsNetworkNccMgtInetAddress OBJECT-TYPE
       SYNTAX              InetAddress
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "IP address of the management server in the NCC.  If
           the terminal has no management server assigned or if this
           Internet address is unknown, the value of this object is
           the zero-length OCTET STRING.
           The InetAddressType is given by the
           dvbRcsNetworkNccMgtInetAddressType object."
   ::= {dvbRcsRcstNetwork 13}

   dvbRcsNetworkNccMgtInetAddressPrefixLength OBJECT-TYPE
       SYNTAX              InetAddressPrefixLength
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Prefix length for the IP address of the management
           server in the NCC.
           If this address prefix is unknown or does not apply, the
           value is zero."
   ::= { dvbRcsRcstNetwork 14}






   dvbRcsNetworkConfigFileDownloadUrl OBJECT-TYPE
       SYNTAX              Uri (SIZE(0..65535))
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Full path name for the configuration file download.
           It includes the protocol type (TFTP or FTP) and the
           associated server IP address or hostname.  Hostname can
           only be used if DNS is supported by the RCST.
           The format of this parameter follows RFC 3986."
   ::= {dvbRcsRcstNetwork 15}

   dvbRcsNetworkInstallLogFileDownloadUrl OBJECT-TYPE
       SYNTAX              Uri (SIZE(0..65535))
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Full path of the installation log file to download.
           It includes the protocol type (TFTP or FTP) and the
           associated server IP address or hostname.  Hostname can
           only be used if DNS is supported by the RCST.  The
           installation log file can be created on the installer's
           computer and downloaded to the RCST.
           The format of this parameter follows RFC 3986."
   ::= {dvbRcsRcstNetwork 16}

   dvbRcsNetworkConfigFileUploadUrl OBJECT-TYPE
       SYNTAX              Uri(SIZE(0..65535))
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Full path name for the configuration file upload.
           It includes the protocol type (TFTP or FTP) and the
           associated server IP address or hostname.  Hostname can
           only be used if DNS is supported by the RCST.
           The format of this parameter follows RFC 3986."
   ::= {dvbRcsRcstNetwork 17}
















   dvbRcsNetworkLogFileUploadUrl OBJECT-TYPE
       SYNTAX              Uri(SIZE(0..65535))
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Full path of the event log file.  It includes the
           protocol type (TFTP or FTP) and the associated server IP
           address or hostname.  Hostname can only be used if DNS is
           supported by the RCST.
           The format of this parameter follows RFC 3986."
   ::= {dvbRcsRcstNetwork 18}

   dvbRcsNetworkInstallLogFileUploadUrl OBJECT-TYPE
       SYNTAX              Uri(SIZE(0..65535))
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Full path of the installation log file.  It includes the
           protocol type (TFTP or FTP) and the associated server
           IP address or hostname.  Hostname can only be used if DNS
           is supported by the RCST.  The installation log file can
           be retrieved from the RCST by the NCC or by the
           installer via the LAN.
           The format of this parameter follows RFC 3986."
   ::= {dvbRcsRcstNetwork 19}

   --==============================================================
   --    dvbRcsRcstInstall sub-tree object types
   --==============================================================
   dvbRcsInstallAntennaAlignmentState OBJECT-TYPE
       SYNTAX              INTEGER {
                   antennaAlignmentStart   (1),
                   antennaAlignmentDeny    (2),
                   antennaAlignmentContinue(3),
                   antennaAlignmentStop    (4),
                   antennaAlignmentSuccess (5),
                   antennaAlignmentFail    (6)
       }
       MAX-ACCESS          read-write
       STATUS              current













       DESCRIPTION
           "Indicates the alignment state of the antenna:
               (1)-Start;
               (2)-Deny;
               (3)-Continue;
               (4)-Stop;
               (5)-Success;
               (6)-Fail"
   ::= {dvbRcsRcstInstall 1}

   dvbRcsInstallCwFrequency OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x100 Hz"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Frequency of the transmitted Continuous Wave
           carrier (in 100 Hz).
           Minimum required precision is 1 kHz."
   ::= {dvbRcsRcstInstall 2}

   dvbRcsInstallCwMaxDuration OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "seconds"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Time after which the Continuous Wave carrier must be
           put down (in seconds)."
   ::= {dvbRcsRcstInstall 3}

   dvbRcsInstallCwPower OBJECT-TYPE
       SYNTAX              Integer32
       UNITS               "x0.1 dBm"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "IDU TX output level when the IDU is configured to send
           CW.  The resolution is 0.1 dBm and the accuracy is +/- 1
           dBm.  Reconfiguration is applied immediately to a CW."
   ::= {dvbRcsRcstInstall 4}












   dvbRcsInstallCoPolReading OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x0.1 dB"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Co-polarization measured value during installation
           procedure (in 0.1 dB)."
   ::= {dvbRcsRcstInstall 5}

   dvbRcsInstallXPolReading OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x0.1 dB"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Cross-polarization measured value during installation
           procedure (in 0.1 dB)."
   ::= {dvbRcsRcstInstall 6}

   dvbRcsInstallCoPolTarget OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x0.1 dB"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Co-polarization target value during installation
           procedure (in 0.1 dB)."
   ::= {dvbRcsRcstInstall 7}

   dvbRcsInstallXPolTarget OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x0.1 dB"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Cross-polarization target value during installation
           procedure (in 0.1 dB)."
    ::= {dvbRcsRcstInstall 8}

   dvbRcsInstallStandByDuration OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "seconds"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Time to wait in stand-by mode (in seconds)."
   ::= {dvbRcsRcstInstall 9}





   dvbRcsInstallTargetEsN0 OBJECT-TYPE
       SYNTAX              Unsigned32(0..315)
       UNITS               "x0.1 dB"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "This value describes the wanted Es/N0 value that
           enables operation of the return link with the required
           error performance.  The values shall be given in tenth of
           dB and the initial value shall be equal to 7 dB.  The
           range shall be from 0 dB to 31.5 dB, with a precision
           of 0.1 dB."
       DEFVAL        { 70 }
   ::= {dvbRcsRcstInstall 10}

   --==============================================================
   -- dvbRcsRcstQos sub-tree object types
   --==============================================================
   dvbRcsPktClassTable OBJECT-TYPE
       SYNTAX              SEQUENCE OF DvbRcsPktClassEntry
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "This table describes the packet classification used in
           the DVB-RCS terminal.  The number of entries is specified
           by dvbRcsPktClassIndex. "
   ::={dvbRcsRcstQos 1}

   dvbRcsPktClassEntry OBJECT-TYPE
       SYNTAX            DvbRcsPktClassEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the packet classification table.  One object
           type of each entry may have a value in the active range
           (a non-default value).  The other object types are then
           assumed to be set to 'inactive'.  The entry with the lowest
           index value takes precedence when classifying a packet."
       INDEX   { dvbRcsPktClassIndex }
   ::= {dvbRcsPktClassTable 1}

   DvbRcsPktClassEntry ::= SEQUENCE {
               dvbRcsPktClassIndex                 Unsigned32,
               dvbRcsPktClassDscpLow               Dscp,
               dvbRcsPktClassDscpHigh              Dscp,
               dvbRcsPktClassDscpMarkValue         DscpOrAny,
               dvbRcsPktClassIpProtocol            Unsigned32,
               dvbRcsPktClassSrcInetAddressType    InetAddressType,





               dvbRcsPktClassSrcInetAddress        InetAddress,
               dvbRcsPktClassSrcInetAddressPrefixLength
                                           InetAddressPrefixLength,
               dvbRcsPktClassDstInetAddressType    InetAddressType,
               dvbRcsPktClassDstInetAddress        InetAddress,
               dvbRcsPktClassDstInetAddressPrefixLength
                                           InetAddressPrefixLength,
               dvbRcsPktClassSrcPortLow            InetPortNumber,
               dvbRcsPktClassSrcPortHigh           InetPortNumber,
               dvbRcsPktClassDstPortLow            InetPortNumber,
               dvbRcsPktClassDstPortHigh           InetPortNumber,
               dvbRcsPktClassVlanUserPri           Integer32,
               dvbRcsPktClassPhbAssociation        Unsigned32,
               dvbRcsPktClassRowStatus             RowStatus
           }

   dvbRcsPktClassIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..64)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Index automatically incremented by one at row
           creation."
   ::={dvbRcsPktClassEntry 1}

   dvbRcsPktClassDscpLow OBJECT-TYPE
       SYNTAX              Dscp
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the low value of a range of
           Diffserv Code Point (DSCP) values to which a packet is
           compared."
       DEFVAL { 0 }
   ::={dvbRcsPktClassEntry 2}

   dvbRcsPktClassDscpHigh OBJECT-TYPE
       SYNTAX              Dscp
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the high value of a range of
           Diffserv Code Point (DSCP) values to which a packet is
           compared."
       DEFVAL { 63 }
   ::={dvbRcsPktClassEntry 3}

   dvbRcsPktClassDscpMarkValue OBJECT-TYPE





       SYNTAX              DscpOrAny
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object is the Diffserv Code Point (DSCP) value
           used to mark the packet; -1 indicates no DSCP marking.
           Possible DSCP marks values are (0..63)"
       DEFVAL { -1 }
   ::={dvbRcsPktClassEntry 4}

   dvbRcsPktClassIpProtocol OBJECT-TYPE
       SYNTAX              Unsigned32 (0..255)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the IP protocol to which a
           packet is compared.  A value of 255 means match all."
       DEFVAL { 255 }
   ::={dvbRcsPktClassEntry 5}

   dvbRcsPktClassSrcInetAddressType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The type of Internet address of
           dvbRcsPktClassSrcInetAddress.  If the packet class source
           Internet address is unassigned or unknown, then the
           value of this object is unknown(0)."
   ::= { dvbRcsPktClassEntry 6}


   dvbRcsPktClassSrcInetAddress OBJECT-TYPE
       SYNTAX              InetAddress
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the IP source address to which a
           packet is compared.  If the packet class has no source
           Internet address assigned or if this Internet address is
           unknown, the value of this object is the zero-length
           OCTET STRING.
           The InetAddressType is given by the
           dvbRcsPktClassSrcInetAddressType object."
   ::={dvbRcsPktClassEntry 7}

   dvbRcsPktClassSrcInetAddressPrefixLength OBJECT-TYPE
       SYNTAX              InetAddressPrefixLength





       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Prefix length of the IP source address that will be
           matched for this packet class.  A value of zero indicates
           that the selectivity is inactive."
       DEFVAL { 0 }
   ::={dvbRcsPktClassEntry 8}

   dvbRcsPktClassDstInetAddressType OBJECT-TYPE
       SYNTAX      InetAddressType
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The type of Internet address of
           dvbRcsPktClassDstInetAddress.  If the packet class
           destination Internet address is unassigned or unknown,
           then the value of this object is unknown(0)."
   ::= { dvbRcsPktClassEntry 9}

   dvbRcsPktClassDstInetAddress OBJECT-TYPE
       SYNTAX              InetAddress
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the IP destination address to
           which a packet is compared.  If the packet class has no
           destination Internet address assigned or if this Internet
           address is unknown, the value of this object is the
           zero-length OCTET STRING.
           The InetAddressType is given by the
           dvbRcsPktClassDstInetAddressType object."
   ::={dvbRcsPktClassEntry 10}

   dvbRcsPktClassDstInetAddressPrefixLength OBJECT-TYPE
       SYNTAX              InetAddressPrefixLength
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Prefix length of the IP source address that will be
           matched for this packet class.  A value of zero indicates
           that the selectivity is inactive."
       DEFVAL { 0 }
   ::={dvbRcsPktClassEntry 11}









   dvbRcsPktClassSrcPortLow OBJECT-TYPE
       SYNTAX              InetPortNumber
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the low range of the source
           port to which a packet is compared.  A value of 0
           indicates that the selectivity is inactive."
       DEFVAL { 0 }
   ::={dvbRcsPktClassEntry 12}

   dvbRcsPktClassSrcPortHigh OBJECT-TYPE
       SYNTAX              InetPortNumber
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the high range of the source port
           to which a packet is compared.  A value of 0 indicates
           that the selectivity is inactive."
       DEFVAL { 65535 }
   ::={dvbRcsPktClassEntry 13}

   dvbRcsPktClassDstPortLow OBJECT-TYPE
       SYNTAX              InetPortNumber
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the low range of the destination
           port to which a packet is compared.  A value of 0
           indicates that the selectivity is inactive."
       DEFVAL { 0 }
   ::={dvbRcsPktClassEntry 14}

   dvbRcsPktClassDstPortHigh OBJECT-TYPE
       SYNTAX              InetPortNumber
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object specifies the high range of the destination
           port to which a packet is compared.  A value of 0
           indicates that the selectivity is inactive."
       DEFVAL { 65535 }
   ::={dvbRcsPktClassEntry 15}

   dvbRcsPktClassVlanUserPri OBJECT-TYPE
       SYNTAX              Integer32 (-1..7)
       MAX-ACCESS          read-create
       STATUS              current





       DESCRIPTION
         "This object specifies the VLAN User Priority to which a
          packet is compared.  A value of -1 indicates that the
          selectivity is inactive."
       DEFVAL { -1 }
   ::={dvbRcsPktClassEntry 16}

   dvbRcsPktClassPhbAssociation OBJECT-TYPE
       SYNTAX              Unsigned32 (0..65535)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Associate the filter entry to a specific PHB (refer to
           dvbRcsPhbIdentifier)."
   ::={dvbRcsPktClassEntry 17}

   dvbRcsPktClassRowStatus OBJECT-TYPE
       SYNTAX              RowStatus
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "The status of this conceptual row.  All writable objects
           in this row may be modified at any time."
   ::={dvbRcsPktClassEntry 18}

   --==============================================================
   -- dvbRcsPhbMappingTable
   --==============================================================
   dvbRcsPhbMappingTable OBJECT-TYPE
       SYNTAX              SEQUENCE OF DvbRcsPhbMappingEntry
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "This table is a list of Per-Hop Behavior (PHB) MIB
           entries.
           It describes the PHB mapping to the Request Class."
   ::={dvbRcsRcstQos 2}

   dvbRcsPhbMappingEntry OBJECT-TYPE
       SYNTAX            DvbRcsPhbMappingEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the PHB mapping table."
       INDEX   {dvbRcsPhbIdentifier}
   ::= {dvbRcsPhbMappingTable 1}

   DvbRcsPhbMappingEntry ::= SEQUENCE {





                   dvbRcsPhbIdentifier               Unsigned32,
                   dvbRcsPhbName
                                                SnmpAdminString,
                   dvbRcsPhbRequestClassAssociation  Unsigned32,
                   dvbRcsPhbMappingRowStatus          RowStatus
                   }

   dvbRcsPhbIdentifier OBJECT-TYPE
       SYNTAX              Unsigned32 (0..65535)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Identification of the Per-Hop Behavior (PHB).  It
           follows the unsigned 16-bit binary encoding as specified
           in RFC 3140.  The value 0 designates the Default PHB."
   ::={dvbRcsPhbMappingEntry 1}

   dvbRcsPhbName OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "The name of the Per-Hop Behavior (PHB)."
   ::={dvbRcsPhbMappingEntry 2}

   dvbRcsPhbRequestClassAssociation OBJECT-TYPE
       SYNTAX              Unsigned32 (1..16)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "This object is an association of this Per-Hop Behavior
           (PHB) to a Request Class (by reference to a Request
           Class index)."
   ::={dvbRcsPhbMappingEntry 3}

   dvbRcsPhbMappingRowStatus OBJECT-TYPE
       SYNTAX              RowStatus
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "The status of this conceptual row.  All writable
           objects in this row may be modified at any time."
       DEFVAL { active }
   ::={dvbRcsPhbMappingEntry 4}









   --==============================================================
   --   dvbRcsRequestClassTable
   --==============================================================
   dvbRcsRequestClassTable OBJECT-TYPE
       SYNTAX              SEQUENCE OF DvbRcsRequestClassEntry
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "This table is a list of Request Class entries.  This
           class describes the layer 2 QoS objects."
   ::={dvbRcsRcstQos 3}

   dvbRcsRequestClassEntry OBJECT-TYPE
       SYNTAX            DvbRcsRequestClassEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the Request Class table."
       INDEX {dvbRcsRequestClassIndex}
   ::= {dvbRcsRequestClassTable 1}

   DvbRcsRequestClassEntry ::= SEQUENCE {
                   dvbRcsRequestClassIndex              Unsigned32,
                   dvbRcsRequestClassName
                                                   SnmpAdminString,
                   dvbRcsRequestClassChanId             Unsigned32,
                   dvbRcsRequestClassVccVpi             Unsigned32,
                   dvbRcsRequestClassVccVci             Unsigned32,
                   dvbRcsRequestClassPidPoolReference   Unsigned32,
                   dvbRcsRequestClassCra                Unsigned32,
                   dvbRcsRequestClassRbdcMax            Unsigned32,
                   dvbRcsRequestClassRbdcTimeout        Unsigned32,
                   dvbRcsRequestClassVbdcMax            Unsigned32,
                   dvbRcsRequestClassVbdcTimeout        Unsigned32,
                   dvbRcsRequestClassVbdcMaxBackLog     Unsigned32,
                   dvbRcsRequestClassRowStatus          RowStatus
                   }

   dvbRcsRequestClassIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..16)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Index of the Request Class table.  A total of 16 entries
           are supported."
   ::={dvbRcsRequestClassEntry 1}

   dvbRcsRequestClassName OBJECT-TYPE





       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Name of the Request Class."
   ::={dvbRcsRequestClassEntry 2}

   dvbRcsRequestClassChanId OBJECT-TYPE
       SYNTAX              Unsigned32 (0..15)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Channel ID of the Request Class."
   ::={dvbRcsRequestClassEntry 3}

   dvbRcsRequestClassVccVpi OBJECT-TYPE
       SYNTAX              Unsigned32 (0..255)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Defines the VPI used for the Request Class (ATM profile)."
    ::={dvbRcsRequestClassEntry 4}

   dvbRcsRequestClassVccVci OBJECT-TYPE
       SYNTAX              Unsigned32 (0..65535)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Defines the VCI used for the Request Class (ATM profile)."
   ::={dvbRcsRequestClassEntry 5}

   dvbRcsRequestClassPidPoolReference OBJECT-TYPE
       SYNTAX              Unsigned32 (1..16)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Reference to the Packet IDentifier (PID) pool
           applicable for the Request Class."
   ::={dvbRcsRequestClassEntry 6}

   dvbRcsRequestClassCra OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "bit/s"
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Defines the Continuous Rate Assignment (CRA) level for the
           Request Class in bits per second (bit/s)."





   ::={dvbRcsRequestClassEntry 7}

   dvbRcsRequestClassRbdcMax OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x2 kbit/s"
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Maximum Rate-Based Dynamic Capacity (RBDC) that can be
           requested for the Request Class, in number of 2 kbit/s."
   ::={dvbRcsRequestClassEntry 8}

   dvbRcsRequestClassRbdcTimeout OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "superframes"
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Persistence of the Rate-Based Dynamic Capacity (RBDC)
           request, expressed in superframes."
   ::={dvbRcsRequestClassEntry 9}

   dvbRcsRequestClassVbdcMax OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "ATM cells/MPEG packets"
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Maximum Volume-Based Dynamic Capacity (VBDC) that can
           be allocated to the Request Class, in payload units (one
           ATM cell or one MPEG packet) per superframe."
   ::={dvbRcsRequestClassEntry 10}

   dvbRcsRequestClassVbdcTimeout OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "superframes"
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Time after which the RCST considers that the pending
           requests are lost.  The RCST may issue new requests for
           that traffic.  Volume-Based Dynamic Capacity (VBDC)
           Timeout is expressed in superframes."
   ::={dvbRcsRequestClassEntry 11}

   dvbRcsRequestClassVbdcMaxBackLog OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "bytes"





       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Volume-Based Dynamic Capacity (VBDC) back log per
           Request Class (expressed in bytes)."
   ::={dvbRcsRequestClassEntry 12}

   dvbRcsRequestClassRowStatus OBJECT-TYPE
       SYNTAX              RowStatus
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "The status of this conceptual row.  It is not possible
           to change values in a row of this table while the row is
           active."
   ::={dvbRcsRequestClassEntry 13}

   --==============================================================
   -- The table of PID pools
   --==============================================================

   dvbRcsPidPoolTable OBJECT-TYPE
       SYNTAX              SEQUENCE OF DvbRcsPidPoolEntry
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "This table contains the Packet IDentifier (PID) pools.
           For the MPEG profile, several Request Classes may be mapped
           within a pool of several PIDs to allow Section Packing
           across several Request Classes.
           A PID value may occur in more than one PID pool.  Each
           PID value can effectively occur only once in each pool."
   ::={dvbRcsRcstQos 4}

   dvbRcsPidPoolEntry OBJECT-TYPE
       SYNTAX            DvbRcsPidPoolEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the PID pool table."
       INDEX { dvbRcsPidPoolIndex, dvbRcsPidIndex }
   ::= {dvbRcsPidPoolTable 1}

   DvbRcsPidPoolEntry ::= SEQUENCE {
           dvbRcsPidPoolIndex            Unsigned32,
           dvbRcsPidIndex                Unsigned32,
           dvbRcsPidValue                Unsigned32,
           dvbRcsPidPoolRowStatus        RowStatus





           }

   dvbRcsPidPoolIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..16)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Index of the PID pool in the PID pool table."
   ::={dvbRcsPidPoolEntry 1}

   dvbRcsPidIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..16)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Index of the PID entry within the PID pool."
   ::={dvbRcsPidPoolEntry 2}

   dvbRcsPidValue OBJECT-TYPE
       SYNTAX              Unsigned32 (0..8191)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Defines one of the PIDs to be used in a PID pool of
           dvbRcsPidPoolIndex.
           A PID value may occur in more than one PID pool.  Each
           PID value can effectively occur only once in each pool."
   ::={dvbRcsPidPoolEntry 3}

   dvbRcsPidPoolRowStatus OBJECT-TYPE
       SYNTAX              RowStatus
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "The status of this conceptual row.  All writable
           objects in this row may be modified at any time."
       DEFVAL { active }
   ::={dvbRcsPidPoolEntry 4}

   dvbRcsQosGlobalRbdcMax OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x2 kbit/s"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Global maximum RBDC that can be requested for the RCST,
           in number of 2 kbit/s."
   ::={dvbRcsRcstQos 5}





   dvbRcsQosGlobalVbdcMax OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "ATM cells/MPEG packets"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Global maximum VBDC that can be allocated to the RCST,
           in payload units (one ATM cell or one MPEG packet) per
           superframe."
   ::={dvbRcsRcstQos 6}

   dvbRcsQosGlobalVbdcMaxBackLog OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "bytes"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Global VBDC back log at the RCST level (expressed in
           bytes).  It is used only if the VBDC back log is not
           configured in the Request Class (expressed in bytes)."
   ::={dvbRcsRcstQos 7}

   dvbRcsQosChannelIdStrictDispatching OBJECT-TYPE
       SYNTAX              INTEGER {
                                   notStrict (0),
                                   strict    (1)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Indicates whether the RCST will strictly follow RC
           association when signaled through Channel_ID in the
           TBTP:
               (0)- no strict association
               (1)- strict association"
   ::={dvbRcsRcstQos 8}

   --==============================================================
   -- dvbRcsRcstControl sub-tree object types
   --==============================================================
   dvbRcsCtrlRebootCommand OBJECT-TYPE
       SYNTAX              INTEGER {
                                   idle        (1),
                                   normal      (2),
                                   alternate   (3)
       }
       MAX-ACCESS          read-write
       STATUS              current





       DESCRIPTION
           "This variable shall force the RCST to reboot:
               (1)- idle
               (2)- normal reboot (from current software load)
               (3)- reboot from alternate load (swap to alternate
                    load before reboot)"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 1}

   dvbRcsCtrlRcstTxDisable OBJECT-TYPE
       SYNTAX              INTEGER {
                                   idle        (1),
                                   disable     (2)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "This variable shall force the RCST to stop transmission
           (transmit disabled as defined in SatLabs System
            Recommendations):
               (1)- idle
               (2)- initiate Tx Disabled"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 2}

   dvbRcsCtrlUserTrafficDisable OBJECT-TYPE
       SYNTAX           INTEGER {
                                idle        (1),
                                disable     (2)
       }
       MAX-ACCESS       read-write
       STATUS           current
       DESCRIPTION
           "This variable shall disable user traffic (only RCST
           management traffic can be transmitted):
               (1)- idle
               (2)- disable user traffic"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 3}

   dvbRcsCtrlCwEnable OBJECT-TYPE
       SYNTAX           INTEGER {
                                off    (1),
                                on     (2)
       }
       MAX-ACCESS       read-write
       STATUS           current
       DESCRIPTION





           "This variable will force the RCST to start transmission
           of CW, if the RCST is first set to the installation
           state and is properly configured for CW transmission:
              (1)- off
              (2)- on"
       DEFVAL {off}
   ::={dvbRcsRcstControl 4}

   dvbRcsCtrlOduTxReferenceEnable OBJECT-TYPE
       SYNTAX           INTEGER {
                                off    (1),
                                on     (2)
       }
       MAX-ACCESS       read-write
       STATUS           current
       DESCRIPTION
           "Enables activation and deactivation of the 10 MHz reference
            clock in the Tx IFL cable:
               (1) off
               (2) on"
       DEFVAL {on}
   ::={dvbRcsRcstControl 5}

   dvbRcsCtrlOduTxDCEnable OBJECT-TYPE
       SYNTAX              INTEGER {
                                   off    (1),
                                   on     (2)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Enables activation and deactivation of DC in the Tx IFL
           cable:
             (1) off
             (2) on"
       DEFVAL {on}
   ::={dvbRcsRcstControl 6}

   dvbRcsCtrlOduRxDCEnable OBJECT-TYPE
       SYNTAX              INTEGER {
                                   off    (1),
                                   on     (2)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Enables activation and deactivation of DC in the Rx IFL
           cable:





             (1) off
             (2) on"
       DEFVAL {on}
   ::={dvbRcsRcstControl 7}

   dvbRcsCtrlDownloadFileCommand OBJECT-TYPE
       SYNTAX              INTEGER {
                                   idle            (1),
                                   config          (2),
                                   installationLog (3)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "This variable will initiate an RCST configuration file
           download process:
           (1) idle
           (2) download RCST configuration file from TFTP/FTP
               server
           (3) download RCST installation log file from TFTP/FTP
               server (INSTALL_LOG feature)"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 8}

   dvbRcsCtrlUploadFileCommand OBJECT-TYPE
       SYNTAX              INTEGER {
                                   idle              (1),
                                   config            (2),
                                   eventAlarm        (3),
                                   installationLog   (4)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "This variable will initiate an RCST upload process:
           (1) idle
           (2) upload RCST configuration file to TFTP/FTP server
           (3) upload RCST event/alarm log file to TFTP/FTP server
           (4) upload RCST installation log file to TFTP/FTP server
               (INSTALL_LOG feature)"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 9}

   dvbRcsCtrlActivateConfigFileCommand OBJECT-TYPE
       SYNTAX              INTEGER {
                                   idle            (1),
                                   activate        (2)
       }





       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Triggers the RCST to use the configuration file and
           update its parameters accordingly.  Some RCST
           implementations may require a reboot for the parameters
           to take effect (vendor specific).
           (1)    idle
           (2)    activate"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 10}

   dvbRcsCtrlRcstLogonCommand OBJECT-TYPE
       SYNTAX              INTEGER {
                                   idle           (1),
                                   logon          (2)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "This variable will initiate an RCST logon:
              (1) idle
              (2) initiate RCST logon"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 11}

   dvbRcsCtrlRcstLogoffCommand OBJECT-TYPE
       SYNTAX              INTEGER {
                                   idle      (1),
                                   logoff    (2)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "This variable will initiate an RCST logoff:
              (1) idle
              (2) initiate RCST logoff"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 12}

   dvbRcsCtrlRcstRxReacquire OBJECT-TYPE
       SYNTAX              INTEGER {
                                   idle                    (1),
                                   reacquireForwardLink    (2)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION





           "This variable will force the RCST to acquire the
           forward link and start receiving:
              (1) idle
              (2) reacquire forward link"
       DEFVAL {idle}
   ::={dvbRcsRcstControl 13}

   --==============================================================
   -- dvbRcsRcstState sub-tree object types
   --==============================================================
   dvbRcsRcstMode OBJECT-TYPE
       SYNTAX              INTEGER {
                                   installation (0),
                                   operational  (1)
       }
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
         "Identifies the current mode of the RCST and allows the RCST
         to return to the installation mode when needed.  Values for
         the RCST mode are:
             Installation (0)
             Operational (1)"
   ::={dvbRcsRcstState 1}

   dvbRcsRcstFaultStatus OBJECT-TYPE
       SYNTAX              INTEGER {
                                   nofault (0),
                                   fault   (1)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Provides the fault status of the terminal.  The fault
           status management is vendor specific.  Values for the
           fault status are:
               no fault (0)
               fault (1)"
   ::={dvbRcsRcstState 2}

   dvbRcsRcstFwdLinkStatus OBJECT-TYPE
       SYNTAX              INTEGER {
                                   notAcquired (0),
                                   acquired    (1)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION





           "Provides the status of the RCST forward link.  Values
           for the forward link status are:
             Not acquired (0)
             Acquired (1)"
   ::={dvbRcsRcstState 3}

   dvbRcsRcstRtnLinkStatus OBJECT-TYPE
       SYNTAX              INTEGER {
                                   loggedOff (0),
                                   loggedOn  (1)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Provides the status of the RCST return link.  Values for
           the return link status are:
               Logged-off (0)
               Logged-on (1)"
   ::={dvbRcsRcstState 4}

   dvbRcsRcstLogUpdated OBJECT-TYPE
       SYNTAX              INTEGER {
                                   noUpdate         (0),
                                   logfileUpdated   (1)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Indicates the existence of an updated event log file:
               No update (0)
               Event Log file updated (1)
           The RCST should remove the 'Event Log file updated'
           indication as the log file is fetched by the NCC."
   ::={dvbRcsRcstState 5}

   dvbRcsRcstCurrentSoftwareVersion OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Current RCST software version."
   ::={dvbRcsRcstState 6}

   dvbRcsRcstAlternateSoftwareVersion OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION





           "Alternate (backup/new) RCST software version."
   ::={dvbRcsRcstState 7}

   dvbRcsRcstActivatedConfigFileVersion OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Version of the most recently activated configuration
           file.
           The version is vendor specific."
   ::={dvbRcsRcstState 8}

   dvbRcsRcstDownloadedConfigFileVersion OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
         "Version of the most recently downloaded configuration
          file.
          Version is vendor specific.  If the value is different
          from dvbRcsRcstActivatedConfigFileVersion, it is pending
          for activation."
   ::={dvbRcsRcstState 9}

   --==============================================================
   -- dvbRcsFwdConfig sub-tree object types
   --==============================================================
   dvbRcsFwdStartTable OBJECT-TYPE
       SYNTAX              SEQUENCE OF DvbRcsFwdStartEntry
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Lists forward link attachment points (e.g., different
           for installation and operation).
           The table describes the forward link parameters used for
           the start-up stream with the NCC."
   ::={dvbRcsFwdConfig 1}

   dvbRcsFwdStartEntry OBJECT-TYPE
       SYNTAX            DvbRcsFwdStartEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the Forward Link Start Configuration table."
       INDEX {dvbRcsFwdStartIndex}
   ::= {dvbRcsFwdStartTable 1}






   DvbRcsFwdStartEntry ::= SEQUENCE {
                       dvbRcsFwdStartIndex         Unsigned32,
                       dvbRcsFwdStartPopId         Integer32,
                       dvbRcsFwdStartFrequency     Unsigned32,
                       dvbRcsFwdStartPolar         INTEGER,
                       dvbRcsFwdStartFormat        INTEGER,
                       dvbRcsFwdStartRolloff       INTEGER,
                       dvbRcsFwdStartSymbolRate    Unsigned32,
                       dvbRcsFwdStartInnerFec      INTEGER,
                       dvbRcsFwdStartRowStatus     RowStatus
   }

   dvbRcsFwdStartIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..8)
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "Index of the Forward Link StartConfig table."
   ::={dvbRcsFwdStartEntry 1}

   dvbRcsFwdStartPopId OBJECT-TYPE
       SYNTAX              Integer32 (-1..65535)
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Population identifier associated with the start-up
            forward link:
               -1: any (auto)
               0-65535: specific StartPopId
            If 'any' is set, the RCST will assume membership of any
            announced population ID and will commence with logon in
            accordance with this assumption."
   ::={dvbRcsFwdStartEntry 2}

   dvbRcsFwdStartFrequency OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x100 kHz"
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Frequency of the start transponder carrying a
           Network Information Table to which any RCST shall
           trigger to acquire forward link.  Its value shall be
           given in multiples of 100 kHz."
   ::={dvbRcsFwdStartEntry 3}

   dvbRcsFwdStartPolar OBJECT-TYPE
       SYNTAX              INTEGER   {





                                     linearHorizontal (0),
                                     linearVertical   (1),
                                     circularLeft     (2),
                                     circularRight    (3)
       }
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "2-bit field giving the polarization of the start
           transponder carrying a Network Information Table to
           which any RCST shall trigger to acquire forward link:
               00: linear and horizontal
               01: linear and vertical
               10: circular left
               11: circular right"
   ::={dvbRcsFwdStartEntry 4}

   dvbRcsFwdStartFormat OBJECT-TYPE
       SYNTAX              INTEGER {
                                   auto     (-1),
                                   dvbs      (0),
                                   dvbs2ccm  (1),
                                   dvbs2acm  (2)
       }
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Specifies the transmission format standard applied for
           the startup stream.  The start transport stream carries a
           Network Information Table that the RCST uses for
           acquiring the forward link signaling.  Supported values
           are:
               -1: unspecified (automatic format acquisition is
                   assumed)
                0: DVB-S (support of this value is mandatory if
                   DVB-S support is claimed)
                1: DVB-S2 with CCM (support of this value is
                   mandatory if DVB-S2 CCM support is claimed)
                2: DVB-S2 with VCM or ACM (support of this value is
                   mandatory if DVB-S2 ACM support is claimed)
           This allows the RCST to discriminate between CCM and
           VCM/ACM when selecting the forward link.
           The support of automatic format selection is optional.
           One or several of the other format selections must be
           supported, according to the claimed SatLabs profile
           support."
   ::={dvbRcsFwdStartEntry 5}






   dvbRcsFwdStartRolloff OBJECT-TYPE
       SYNTAX        INTEGER {
                             autoRolloff    (0),
                             rolloff020     (1),
                             rolloff025     (2),
                             rolloff035     (3)
       }
       MAX-ACCESS    read-create
       STATUS        current
       DESCRIPTION
           "Specifies the receive filter roll-off applied on the
           start transponder.  The start transponder carries a
           Network Information Table that the RCST uses for
           acquiring the forward link signaling.
           Supported values are:
               0: any (auto)
               1: 0.20
               2: 0.25
               3: 0.35"
   ::={dvbRcsFwdStartEntry 6}

   dvbRcsFwdStartSymbolRate OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x100 symbols/s"
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Specifies the symbol rate on the start transponder
           carrying a Network Information Table to which any RCST
           shall trigger to acquire forward link.  Its value shall
           be given in multiples of 100 symbols/s."
   ::={dvbRcsFwdStartEntry 7}

   dvbRcsFwdStartInnerFec OBJECT-TYPE
       SYNTAX              INTEGER     {
                                       autoFec     (-1),
                                       fecRate12    (0),
                                       fecRate23    (1),
                                       fecRate34    (2),
                                       fecRate56    (3),
                                       fecRate78    (4),
                                       fecRate89    (5),
                                       fecRate35    (6),
                                       fecRate45    (7),
                                       fecRate910   (8),
                                       fecRate25    (9),
                                       fecRate13   (10),
                                       fecRate14   (11),





                                       noInnerCode (12)
       }
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "Specifies the inner Forward Error Correction used on
           the start transponder carrying a Network Information
           Table to which any RCST shall trigger to acquire forward
           link.
           Supported values are:
                   autoFec      (-1),
                   fecRate1/2    (0),
                   fecRate2/3    (1),
                   fecRate3/4    (2),
                   fecRate5/6    (3),
                   fecRate7/8    (4),
                   fecRate8/9    (5),
                   fecRate3/5    (6),
                   fecRate4/5    (7),
                   fecRate9/10   (8),
                   fecRate2/5    (9),
                   fecRate1/3    (10),
                   fecRate1/4    (11),
                   noInnerCode   (12)
       The support of autoFec is optional."
   ::={dvbRcsFwdStartEntry 8}

   dvbRcsFwdStartRowStatus OBJECT-TYPE
       SYNTAX              RowStatus
       MAX-ACCESS          read-create
       STATUS              current
       DESCRIPTION
           "The status of this conceptual row.  It is not possible
           to change values in a row of this table while the row is
           active."
   ::={dvbRcsFwdStartEntry 9}

   --==============================================================
   --  dvbRcsFwdStatus sub-tree object types
   --==============================================================
   dvbRcsFwdStatusPopId OBJECT-TYPE
       SYNTAX              Unsigned32 (0..65535)
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Population identifier applied at log-on:
               0-65535: specific StartPopId
           If the RCST was allowed to logon with any population,





           the RCST will report the base number of the announced
           population ID indicated by the RCS Map Table linkage
           descriptor used at logon."
   ::={dvbRcsFwdStatus 1}

   dvbRcsFwdStatusTable OBJECT-TYPE
       SYNTAX              SEQUENCE OF DvbRcsFwdStatusEntry
       MAX-ACCESS          not-accessible
       STATUS              current
       DESCRIPTION
           "This table describes the current status of Forward Link
           interfaces."
   ::={dvbRcsFwdStatus 2}

   dvbRcsFwdStatusEntry OBJECT-TYPE
       SYNTAX            DvbRcsFwdStatusEntry
       MAX-ACCESS        not-accessible
       STATUS            current
       DESCRIPTION
           "An entry in the forward link status table.  Each entry
           is associated with a physical interface.
           An RCST shall support at least one entry."
       INDEX { dvbRcsFwdStatusIndex }
   ::= {dvbRcsFwdStatusTable 1}

   DvbRcsFwdStatusEntry ::= SEQUENCE {
                   dvbRcsFwdStatusIndex             Unsigned32,
                   dvbRcsFwdStatusIfReference       Unsigned32,
                   dvbRcsFwdStatusNetId             Unsigned32,
                   dvbRcsFwdStatusNetName
                                               SnmpAdminString,
                   dvbRcsFwdStatusFormat            INTEGER,
                   dvbRcsFwdStatusFrequency         Unsigned32,
                   dvbRcsFwdStatusPolar             INTEGER,
                   dvbRcsFwdStatusInnerFec          INTEGER,
                   dvbRcsFwdStatusSymbolRate        Unsigned32,
                   dvbRcsFwdStatusRolloff           INTEGER,
                   dvbRcsFwdStatusModulation        INTEGER,
                   dvbRcsFwdStatusFecFrame          INTEGER,
                   dvbRcsFwdStatusPilot             INTEGER,
                   dvbRcsFwdStatusBer               Integer32,
                   dvbRcsFwdStatusCnr               Integer32,
                   dvbRcsFwdStatusRxPower           Integer32
   }

   dvbRcsFwdStatusIndex OBJECT-TYPE
       SYNTAX              Unsigned32 (1..8)
       MAX-ACCESS          not-accessible





       STATUS              current
       DESCRIPTION
           "Index of the forward link status table."
   ::={dvbRcsFwdStatusEntry 1}

   dvbRcsFwdStatusIfReference OBJECT-TYPE
       SYNTAX              Unsigned32 (1..8)
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Cross reference to the interface table."
   ::={dvbRcsFwdStatusEntry 2}

   dvbRcsFwdStatusNetId OBJECT-TYPE
       SYNTAX              Unsigned32
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Interactive network identifier of the forward
           link (from the RCS Map Table)."
   ::={dvbRcsFwdStatusEntry 3}

   dvbRcsFwdStatusNetName OBJECT-TYPE
       SYNTAX              SnmpAdminString
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "The name of the interactive network of the forward
           link (from the RCS Map Table)."
   ::={dvbRcsFwdStatusEntry 4}

   dvbRcsFwdStatusFormat OBJECT-TYPE
       SYNTAX              INTEGER  {
                                    dvbs            (0),
                                    dvbs2ccm        (1),
                                    dvbs2acm        (2),
                                    reservedFormat  (3)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Specifies the transmission format applied on the
           forward link.  Supported values are (from RCS Map Table):
               0: DVB-S
               1: DVB-S2 using CCM
               2: DVB-S2 using VCM or ACM
               3: reserved"
   ::={dvbRcsFwdStatusEntry 5}





   dvbRcsFwdStatusFrequency OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x100 kHz"
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "An estimate of the frequency of the forward link.  Its
           value shall be given in multiples of 100 kHz."
   ::={dvbRcsFwdStatusEntry 6}

   dvbRcsFwdStatusPolar OBJECT-TYPE
       SYNTAX              INTEGER   {
                                     linearHorizontal (0),
                                     linearVertical   (1),
                                     circularLeft     (2),
                                     circularRight    (3)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "2-bit field giving the polarization of the forward link
           Supported values are (from RCS Map Table):
               00: linear and horizontal
               01: linear and vertical
               10: circular left
               11: circular right"
   ::={dvbRcsFwdStatusEntry 7}

   dvbRcsFwdStatusInnerFec OBJECT-TYPE
       SYNTAX              INTEGER     {
                                       unknown     (-1),
                                       fecRate12    (0),
                                       fecRate23    (1),
                                       fecRate34    (2),
                                       fecRate56    (3),
                                       fecRate78    (4),
                                       fecRate89    (5),
                                       fecRate35    (6),
                                       fecRate45    (7),
                                       fecRate910   (8),
                                       fecRate25    (9),
                                       fecRate13   (10),
                                       fecRate14   (11),
                                       noInnerCode (12)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION





           "Specifies the inner Forward Error Correction used on
           the forward link for transmission to the RCST.
           Supported values are:
                   unknown      (-1),
                   fecRate1/2    (0),
                   fecRate2/3    (1),
                   fecRate3/4    (2),
                   fecRate5/6    (3),
                   fecRate7/8    (4),
                   fecRate8/9    (5),
                   fecRate3/5    (6),
                   fecRate4/5    (7),
                   fecRate9/10   (8),
                   fecRate2/5    (9),
                   fecRate1/3    (10),
                   fecRate1/4    (11),
                   noInnerCode   (12)
           The RCST will report a value that has been used for
           transmission to the RCST within the most recent 60
           seconds.  If this is not relevant, the RCST will report
           'unknown'."
   ::={dvbRcsFwdStatusEntry 8}

   dvbRcsFwdStatusSymbolRate OBJECT-TYPE
       SYNTAX              Unsigned32
       UNITS               "x100 symbols/s"
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "An estimate of the symbol rate of the forward link.
           Its value shall be given in multiples of 100 symbols/s."
   ::={dvbRcsFwdStatusEntry 9}

   dvbRcsFwdStatusRolloff OBJECT-TYPE
       SYNTAX              INTEGER   {
                                     undefRolloff       (0),
                                     rolloff020         (1),
                                     rolloff025         (2),
                                     rolloff035         (3)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "An estimate of the roll-off applied on the forward
           link.
           Supported values are:
               0: undefined
               1: 0.20





               2: 0.25
               3: 0.35"
   ::={dvbRcsFwdStatusEntry 10}

    dvbRcsFwdStatusModulation OBJECT-TYPE
       SYNTAX              INTEGER   {
                                     unknown        (0),
                                     mBPSK          (1),
                                     mQPSK          (2),
                                     m8PSK          (3),
                                     m16APSK        (4),
                                     m32APSK        (5)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Indicates the modulation on the forward link used for
           transmission to the RCST. Supported values are:
               0: unknown
               1: BPSK
               2: QPSK
               3: 8PSK
               4: 16APSK
               5: 32APSK
           The RCST will report a value that has been used for
           transmission to the RCST within the most recent 60
           seconds.
           If this is not relevant, the RCST will report
           'unknown'."
   ::={dvbRcsFwdStatusEntry 11}

   dvbRcsFwdStatusFecFrame OBJECT-TYPE
       SYNTAX              INTEGER {
                                   unknown       (0),
                                   shortframe    (1),
                                   longframe     (2)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Indicates the frame length used on the forward link for
           transmission to the RCST.
           Supported values are:
               0: Unknown
               1: Short frame
               2: Normal frame
           The RCST will report a value that has been used for
           transmission to the RCST within the most recent 60





           seconds.
           If this is not relevant, the RCST will report
           'unknown'."
   ::={dvbRcsFwdStatusEntry 12}

   dvbRcsFwdStatusPilot OBJECT-TYPE
       SYNTAX              INTEGER {
                                   unknown      (0),
                                   pilotNotused (1),
                                   pilotUsed    (2)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Indicates whether pilots are used on the forward link
           for transmission to the RCST.
           Supported values are:
               0: Unknown
               1: Pilots are not used
               2: Pilots are used
           The RCST will report a value that has been used for
           transmission to the RCST within the most recent 60
           seconds.
           If this is not relevant, the RCST will report
           'unknown'."
   ::={dvbRcsFwdStatusEntry 13}

   dvbRcsFwdStatusBer OBJECT-TYPE
       SYNTAX              Integer32
       UNITS               "exponent of 10"
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Provides the RCST BER on the Forward Link in log10
           units."
   ::={dvbRcsFwdStatusEntry 14}

   dvbRcsFwdStatusCnr OBJECT-TYPE
       SYNTAX              Integer32
       UNITS               "0.1 dB"
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Provides the RCST CNR on the Forward Link in 0.1 dB
           units."
   ::={dvbRcsFwdStatusEntry 15}

   dvbRcsFwdStatusRxPower OBJECT-TYPE





       SYNTAX              Integer32
       UNITS               "0.1 dBm"
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Provides the power level of the forward link as
           received at the IDU, in 0.1 dBm units."
       DEFVAL { -500 }
   ::={dvbRcsFwdStatusEntry 16}

   --==============================================================
   --  dvbRcsRtnConfig sub-tree object types
   --==============================================================
   dvbRcsRtnConfigMaxEirp OBJECT-TYPE
       SYNTAX              Integer32
       UNITS               "x0.1 dBm"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
           "Max Equivalent Isotropic Radiated Power (EIRP) of the RCST,
            given in resolution of 0.1 dBm and applied when the IDU
            can, itself, set the necessary IDU TX output level, e.g.,
            when using a BUC that has a power level detector and that
            provides sufficient feedback to the IDU."
   ::= {dvbRcsRtnConfig 1}

   dvbRcsRtnConfigDefIfLevel OBJECT-TYPE
       SYNTAX              Integer32
       UNITS               "x0.1 dBm"
       MAX-ACCESS          read-write
       STATUS              current
       DESCRIPTION
            "IDU TX output level applied in case the
            dvbRcsRtnConfigMaxEirp cannot be used.  The resolution
            is 0.1 dBm and the accuracy is +/- 1 dBm."
   ::= {dvbRcsRtnConfig 2}

   --==============================================================
   --  dvbRcsRtnStatus sub-tree object types
   --==============================================================
   dvbRcsRtnStatusEbN0 OBJECT-TYPE
       SYNTAX              Integer32
       UNITS               "x0.1 dB"
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "The EbN0 value reported for the return link, referenced
           to the regular SYNC burst transmission, in 0.1 dB





           units."
   ::= {dvbRcsRtnStatus 1}

   dvbRcsRtnStatusSFDuration OBJECT-TYPE
       SYNTAX              Unsigned32 (250..7500)
       UNITS               "0.1 ms"
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "The duration of the currently applied return link
           superframe structure, in tenths of milliseconds."
   ::= {dvbRcsRtnStatus 2}

   dvbRcsRtnStatusPayloadUnit OBJECT-TYPE
       SYNTAX              INTEGER   {
                                     unitATM    (0),
                                     unitMPEG   (1)
       }
       MAX-ACCESS          read-only
       STATUS              current
       DESCRIPTION
           "Indicates if the payload unit used for the return link
           is ATM or MPEG."
   ::= {dvbRcsRtnStatus 3}

   --=============================================================
   --    conformance information
   --=============================================================
   dvbRcsRcstGroups          OBJECT IDENTIFIER ::=
   {dvbRcsConformance 1}
   dvbRcsRcstCompliances     OBJECT IDENTIFIER ::=
   {dvbRcsConformance 2}

   --=============================================================
   --    conformance statements
   --=============================================================
   dvbRcsRcstCompliance1 MODULE-COMPLIANCE
        STATUS          current
        DESCRIPTION
            "The compliance statement for DVB-RCS terminals that
            are compliant with SatLabs System Recommendations.
            Compliance is linked to the support by the terminal of
            the options or features defined in the SatLabs System
            Recommendations.
            The supported options and features of a terminal are
            declared in objects
            dvbRcsSystemSatLabsOptionsDeclaration
            and dvbRcsSystemSatLabsFeaturesDeclaration





            respectively."

       MODULE  -- this module

              MANDATORY-GROUPS    {dvbRcsRcstSystemGroup,
   dvbRcsRcstNetworkGroup, dvbRcsRcstInstallGroup,
   dvbRcsRcstQosGroup, dvbRcsRcstControlGroup,
   dvbRcsRcstStateGroup, dvbRcsFwdConfigGroup,
   dvbRcsFwdStatusGroup, dvbRcsRtnConfigGroup,
   dvbRcsRtnStatusGroup}

   GROUP dvbRcsRcstExtNetworkGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports extended
            networking management functionality.  Such RCST is qualified
            as supporting the EXTNETWORK feature, as defined in the
            SatLabs System Recommendations."

   GROUP dvbRcsRcstDnsGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports the DNS
            protocol.  Such RCST is qualified as supporting the DNS
            option, as defined in the SatLabs System Recommendations."

   GROUP dvbRcsRcstExtInstallGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports the
            installation log file.  Such RCST is qualified as supporting
            the INSTALL_LOG feature, as defined in the SatLabs System
            Recommendations."

   GROUP dvbRcsRcstEnhancedClassifierGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports the
            enhanced classifier feature.  Such RCST is qualified as
            supporting the ENHCLASSIFIER feature, as defined in the
            SatLabs System Recommendations."

   GROUP dvbRcsRcstMpegQosGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports MPEG
            traffic bursts.  Such RCST is qualified as supporting the
            MPEG_TRF option, as defined in the SatLabs System
            Recommendations."

   GROUP dvbRcsRcstGlobalQosGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports global





            RCST QoS configuration data.  Such RCST is qualified as
            supporting the RCST_PARA feature, as defined in the SatLabs
            System Recommendations."

   GROUP dvbRcsRcstStrictQosGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports strict
            channel ID dispatching.  Such RCST is qualified as
            supporting the CHID_STRICT option, as defined in the SatLabs
            System Recommendations."

   GROUP dvbRcsRcstExtControlGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports extended
            control management functionality.  Such RCST is qualified as
            supporting the EXTCONTROL feature, as defined in the SatLabs
            System Recommendations."

   GROUP dvbRcsRtnExtConfigGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports extended
            return link configuration management functionality.  Such
            RCST is qualified as supporting the EXTCONFIG feature, as
            defined in the SatLabs System Recommendations."

   GROUP dvbRcsRtnExtStatusGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports extended
            return link status report functionality.  Such RCST is
            qualified as supporting the EXTSTATUS feature, as defined in
            the SatLabs System Recommendations."

   GROUP dvbRcsRcstOduListGroup
        DESCRIPTION
            "This group is mandatory for an RCST that supports the ODU
            structural entities defined under dvbRcsOduTx, dvbRcsOduRx,
            and dvbRcsOduAntenna.  Such RCST is qualified as supporting
            the ODULIST feature, as defined in the SatLabs System
            Recommendations."

   OBJECT dvbRcsSystemOduAntennaSize
        MIN-ACCESS read-only
        DESCRIPTION
            "Write access must be supported if dvbRcsRcstOduListGroup is
            not supported."

   OBJECT dvbRcsSystemOduAntennaGain
        MIN-ACCESS read-only





        DESCRIPTION
            "Write access must be supported if dvbRcsRcstOduListGroup is
            not supported."

   OBJECT dvbRcsSystemOduSspa
        MIN-ACCESS read-only
        DESCRIPTION
            "Write access must be supported if dvbRcsRcstOduListGroup is
            not supported."

   OBJECT dvbRcsSystemOduTxType
        MIN-ACCESS read-only
        DESCRIPTION
            "Write access must be supported if dvbRcsRcstOduListGroup is
            not supported."

   OBJECT dvbRcsSystemOduRxType
        MIN-ACCESS read-only
        DESCRIPTION
            "Write access must be supported if dvbRcsRcstOduListGroup is
            not supported."

   OBJECT dvbRcsSystemOduRxBand
        MIN-ACCESS read-only
        DESCRIPTION
            "Write access must be supported if dvbRcsRcstOduListGroup is
            not supported."

   OBJECT dvbRcsSystemOduRxLO
        MIN-ACCESS read-only
        DESCRIPTION
            "Write access must be supported if dvbRcsRcstOduListGroup is
            not supported."

   OBJECT dvbRcsSystemOduTxLO
     MIN-ACCESS read-only
     DESCRIPTION
         "Write access must be supported if dvbRcsRcstOduListGroup is
         not supported."

   OBJECT dvbRcsNetworkOamInetAddressType
        SYNTAX InetAddressType { ipv4(1) }
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsNetworkOamInetAddress
        SYNTAX InetAddress (SIZE(4))





        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsNetworkLanInetAddressType
        SYNTAX InetAddressType { ipv4(1) }
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsNetworkLanInetAddress
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsNetworkAirInterfaceDefaultGatewayInetAddressType
        SYNTAX InetAddressType { ipv4(1) }
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsNetworkAirInterfaceDefaultGatewayInetAddress
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsPrimaryDnsServerInetAddressType
        SYNTAX InetAddressType { ipv4(1) }
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsPrimaryDnsServerInetAddress
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsSecondaryDnsServerInetAddressType
        SYNTAX InetAddressType { ipv4(1) }
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsSecondaryDnsServerInetAddress
         SYNTAX InetAddress (SIZE(4))





         DESCRIPTION
             "An implementation is only required to support IPv4
             addresses."

   OBJECT dvbRcsNetworkNccMgtInetAddressType
        SYNTAX InetAddressType { ipv4(1) }
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsNetworkNccMgtInetAddress
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsPktClassDscpLow
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports the
            enhanced classifier feature.  Such RCST is qualified as
            supporting the ENHCLASSIFIER feature, as defined in the
            SatLabs System Recommendations."

   OBJECT dvbRcsPktClassDscpHigh
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports the
            enhanced classifier feature.  Such RCST is qualified as
            supporting the ENHCLASSIFIER feature, as defined in the
            SatLabs System Recommendations."

   OBJECT dvbRcsPktClassDscpMarkValue
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports the
            enhanced classifier feature.  Such RCST is qualified as
            supporting the ENHCLASSIFIER feature, as defined in the
            SatLabs System Recommendations."

   OBJECT dvbRcsPktClassSrcInetAddressType
        SYNTAX InetAddressType { ipv4(1) }
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsPktClassSrcInetAddress
        SYNTAX InetAddress (SIZE(4))





        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsPktClassDstInetAddressType
        SYNTAX InetAddressType { ipv4(1) }
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsPktClassDstInetAddress
        SYNTAX InetAddress (SIZE(4))
        DESCRIPTION
            "An implementation is only required to support IPv4
            addresses."

   OBJECT dvbRcsPhbName
       MIN-ACCESS read-only
       DESCRIPTION
           "Create access only required if the RCST supports extended
           management support.  Such RCST is qualified as supporting
           the SNMPMISC option, as defined in the SatLabs System
           Recommendations."

   OBJECT dvbRcsPhbRequestClassAssociation
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support.  Such RCST is qualified as supporting
            the SNMPMISC option, as defined in the SatLabs System
            Recommendations."

   OBJECT dvbRcsPhbMappingRowStatus
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support.  Such RCST is qualified as supporting
            the SNMPMISC option, as defined in the SatLabs System
            Recommendations."

   OBJECT dvbRcsRequestClassName
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support.  Such RCST is qualified as supporting
            the SNMPMISC option, as defined in the SatLabs System
            Recommendations."






   OBJECT dvbRcsRequestClassChanId
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support.  Such RCST is qualified as supporting
            the SNMPMISC option, as defined in the SatLabs System
            Recommendations."

   OBJECT dvbRcsRequestClassVccVpi
       MIN-ACCESS read-only
       DESCRIPTION
           "Create access only required if the RCST supports extended
           management support.  Such RCST is qualified as supporting
           the SNMPMISC option, as defined in the SatLabs System
           Recommendations."

   OBJECT dvbRcsRequestClassVccVci
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support.  Such RCST is qualified as supporting
            the SNMPMISC option, as defined in the SatLabs System
            Recommendations."

   OBJECT dvbRcsRequestClassPidPoolReference
        MIN-ACCESS not-accessible
        DESCRIPTION
            "Read-only access required if the RCST supports MPEG traffic
            bursts, according to the MPEG_TRF option, as defined in the
            SatLabs System Recommendations.  Create access only required
            if the RCST also supports extended management support,
            according to the SNMPMISC option, as defined in the SatLabs
            System Recommendations."

   OBJECT dvbRcsRequestClassCra
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support, according to the SNMPMISC option, as
            defined in the SatLabs System Recommendations."

   OBJECT dvbRcsRequestClassRbdcMax
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support, according to the SNMPMISC option, as
            defined in the SatLabs System Recommendations."






   OBJECT dvbRcsRequestClassRbdcTimeout
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support, according to the SNMPMISC option, as
            defined in the SatLabs System Recommendations."

   OBJECT dvbRcsRequestClassVbdcMax
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support, according to the SNMPMISC option, as
            defined in the SatLabs System Recommendations."

   OBJECT dvbRcsRequestClassVbdcTimeout
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support, according to the SNMPMISC option, as
            defined in the SatLabs System Recommendations."

   OBJECT dvbRcsRequestClassVbdcMaxBackLog
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support, according to the SNMPMISC option, as
            defined in the SatLabs System Recommendations."

   OBJECT dvbRcsRequestClassRowStatus
        MIN-ACCESS read-only
        DESCRIPTION
            "Create access only required if the RCST supports extended
            management support, according to the SNMPMISC option, as
            defined in the SatLabs System Recommendations."

   OBJECT dvbRcsPidValue
        MIN-ACCESS not-accessible
        DESCRIPTION
            "Read-only access required if the RCST supports MPEG traffic
            bursts, according to the MPEG_TRF option, as defined in the
            SatLabs System Recommendations.  Create access only required
            if the RCST also supports extended management support,
            according to the SNMPMISC option, as defined in the SatLabs
            System Recommendations."

   OBJECT dvbRcsPidPoolRowStatus
        MIN-ACCESS not-accessible
        DESCRIPTION





            "Read-only access required if the RCST supports MPEG traffic
            bursts, according to the MPEG_TRF option, as defined in the
            SatLabs System Recommendations.  Create access only required
            if the RCST also supports extended management support,
            according to the SNMPMISC option, as defined in the SatLabs
            System Recommendations."

           ::= {dvbRcsRcstCompliances 1}

   --=============================================================
   --    units of conformance
   --=============================================================

   --=============================================================
   --    object groups for RCST system
   --=============================================================
   dvbRcsRcstSystemGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsSystemMibRevision,
           dvbRcsSystemSatLabsProfilesDeclaration,
           dvbRcsSystemSatLabsOptionsDeclaration,
           dvbRcsSystemSatLabsFeaturesDeclaration,
           dvbRcsSystemLocation,
           dvbRcsSystemOduAntennaSize,
           dvbRcsSystemOduAntennaGain,
           dvbRcsSystemOduSspa,
           dvbRcsSystemOduTxType,
           dvbRcsSystemOduRxType,
           dvbRcsSystemOduRxBand,
           dvbRcsSystemOduRxLO,
           dvbRcsSystemOduTxLO,
           dvbRcsTcpPep,
           dvbRcsHttpPep
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects providing information
           applicable for basic device management support."
   ::= {dvbRcsRcstGroups 1}

   --=============================================================
   --    object groups for RCST networking
   --=============================================================
   dvbRcsRcstNetworkGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsNetworkOamInetAddressType,
           dvbRcsNetworkOamInetAddress,
           dvbRcsNetworkOamInetAddressPrefixLength,





           dvbRcsNetworkLanInetAddressType,
           dvbRcsNetworkLanInetAddress,
           dvbRcsNetworkLanInetAddressPrefixLength,
           dvbRcsNetworkConfigFileDownloadUrl,
           dvbRcsNetworkConfigFileUploadUrl,
           dvbRcsNetworkLogFileUploadUrl
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects providing basic networking
           management support."
   ::= {dvbRcsRcstGroups 2}

   dvbRcsRcstExtNetworkGroup OBJECT-GROUP
       OBJECTS {
         dvbRcsNetworkOamInetAddressAssign,
         dvbRcsNetworkAirInterfaceDefaultGatewayInetAddressType,
         dvbRcsNetworkAirInterfaceDefaultGatewayInetAddress,
         dvbRcsNetworkAirInterfaceDefaultGatewayInetAddressPrefixLength,
         dvbRcsNetworkNccMgtInetAddressType,
         dvbRcsNetworkNccMgtInetAddress,
         dvbRcsNetworkNccMgtInetAddressPrefixLength
         }
       STATUS    current
       DESCRIPTION
           "A collection of objects providing extended networking
           management support."
   ::= {dvbRcsRcstGroups 3}

   dvbRcsRcstDnsGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsPrimaryDnsServerInetAddressType,
           dvbRcsPrimaryDnsServerInetAddress,
           dvbRcsPrimaryDnsServerInetAddressPrefixLength,
           dvbRcsSecondaryDnsServerInetAddressType,
           dvbRcsSecondaryDnsServerInetAddress,
           dvbRcsSecondaryDnsServerInetAddressPrefixLength
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects providing DNS management
           support."
   ::= {dvbRcsRcstGroups 4}










   --=============================================================
   --    object groups for RCST installation
   --=============================================================

   dvbRcsRcstInstallGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsInstallAntennaAlignmentState,
           dvbRcsInstallCwFrequency,
           dvbRcsInstallCwMaxDuration,
           dvbRcsInstallCwPower,
           dvbRcsInstallCoPolReading,
           dvbRcsInstallXPolReading,
           dvbRcsInstallCoPolTarget,
           dvbRcsInstallXPolTarget,
           dvbRcsInstallStandByDuration,
           dvbRcsInstallTargetEsN0
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects providing information
           applicable for basic installation support."
   ::= {dvbRcsRcstGroups 5}

   dvbRcsRcstExtInstallGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsNetworkInstallLogFileDownloadUrl,
           dvbRcsNetworkInstallLogFileUploadUrl
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects providing extended device
           installation support."
   ::= {dvbRcsRcstGroups 6}

   --=============================================================
   --    object groups for QoS
   --=============================================================

   dvbRcsRcstQosGroup OBJECT-GROUP
      OBJECTS {
          dvbRcsPktClassDscpLow,
          dvbRcsPktClassDscpHigh,
          dvbRcsPktClassDscpMarkValue,
          dvbRcsPktClassPhbAssociation,
          dvbRcsPktClassRowStatus,
          dvbRcsPhbName,
          dvbRcsPhbRequestClassAssociation,
          dvbRcsPhbMappingRowStatus,





          dvbRcsRequestClassName,
          dvbRcsRequestClassChanId,
          dvbRcsRequestClassVccVpi,
          dvbRcsRequestClassVccVci,
          dvbRcsRequestClassCra,
          dvbRcsRequestClassRbdcMax,
          dvbRcsRequestClassRbdcTimeout,
          dvbRcsRequestClassVbdcMax,
          dvbRcsRequestClassVbdcTimeout,
          dvbRcsRequestClassVbdcMaxBackLog,
          dvbRcsRequestClassRowStatus
          }
      STATUS    current
      DESCRIPTION
          "A collection of objects providing basic access to QoS
          configuration data."
   ::= {dvbRcsRcstGroups 7}

   dvbRcsRcstEnhancedClassifierGroup OBJECT-GROUP
      OBJECTS {
          dvbRcsPktClassIpProtocol,
          dvbRcsPktClassSrcInetAddressType,
          dvbRcsPktClassSrcInetAddress,
          dvbRcsPktClassSrcInetAddressPrefixLength,
          dvbRcsPktClassDstInetAddressType,
          dvbRcsPktClassDstInetAddress,
          dvbRcsPktClassDstInetAddressPrefixLength,
          dvbRcsPktClassSrcPortLow,
          dvbRcsPktClassSrcPortHigh,
          dvbRcsPktClassDstPortLow,
          dvbRcsPktClassDstPortHigh,
          dvbRcsPktClassVlanUserPri
          }
      STATUS    current
      DESCRIPTION
          "A collection of objects providing support for
          management of the enhanced classifier."
   ::= {dvbRcsRcstGroups 8}

   dvbRcsRcstMpegQosGroup OBJECT-GROUP
      OBJECTS {
          dvbRcsRequestClassPidPoolReference,
          dvbRcsPidValue,
          dvbRcsPidPoolRowStatus
          }
      STATUS    current
      DESCRIPTION
          "A collection of objects providing access to





          MPEG-related link QoS configuration data."

   ::= {dvbRcsRcstGroups 9}

   dvbRcsRcstGlobalQosGroup OBJECT-GROUP
      OBJECTS {
          dvbRcsQosGlobalRbdcMax,
          dvbRcsQosGlobalVbdcMax,
          dvbRcsQosGlobalVbdcMaxBackLog
          }
      STATUS    current
      DESCRIPTION
          "A collection of objects providing access to global RCST
          QoS configuration data."
   ::= {dvbRcsRcstGroups 10}

   dvbRcsRcstStrictQosGroup OBJECT-GROUP
      OBJECTS {
          dvbRcsQosChannelIdStrictDispatching
          }
      STATUS    current
      DESCRIPTION
          "A collection of objects allowing management of strict
          channel ID dispatching."
   ::= {dvbRcsRcstGroups 11}

   --=============================================================
   --    object groups for RCST control
   --=============================================================
   dvbRcsRcstControlGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsCtrlRebootCommand,
           dvbRcsCtrlUserTrafficDisable,
           dvbRcsCtrlCwEnable,
           dvbRcsCtrlDownloadFileCommand,
           dvbRcsCtrlUploadFileCommand,
           dvbRcsCtrlActivateConfigFileCommand,
           dvbRcsCtrlRcstRxReacquire
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects allowing basic RCST control."
   ::= {dvbRcsRcstGroups 12}

   dvbRcsRcstExtControlGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsCtrlRcstTxDisable,
           dvbRcsCtrlOduTxReferenceEnable,





           dvbRcsCtrlOduTxDCEnable,
           dvbRcsCtrlOduRxDCEnable,
           dvbRcsCtrlRcstLogonCommand,
           dvbRcsCtrlRcstLogoffCommand
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects allowing extended RCST
           control."
   ::= {dvbRcsRcstGroups 13}

   --=============================================================
   --    object groups for RCST state
   --=============================================================

   dvbRcsRcstStateGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsRcstMode,
           dvbRcsRcstFaultStatus,
           dvbRcsRcstFwdLinkStatus,
           dvbRcsRcstLogUpdated,
           dvbRcsRcstCurrentSoftwareVersion,
           dvbRcsRcstAlternateSoftwareVersion,
           dvbRcsRcstActivatedConfigFileVersion,
           dvbRcsRcstDownloadedConfigFileVersion
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects allowing access to RCST state."
   ::= {dvbRcsRcstGroups 14}

   --=============================================================
   --    object groups for forward link
   --=============================================================

   dvbRcsFwdConfigGroup OBJECT-GROUP
       OBJECTS {
               dvbRcsFwdStartPopId,
               dvbRcsFwdStartFrequency,
               dvbRcsFwdStartPolar,
               dvbRcsFwdStartFormat,
               dvbRcsFwdStartRolloff,
               dvbRcsFwdStartSymbolRate,
               dvbRcsFwdStartInnerFec,
               dvbRcsFwdStartRowStatus
           }
       STATUS    current
       DESCRIPTION





           "A collection of objects providing basic start forward
           link configuration support."
   ::= {dvbRcsRcstGroups 15}

   dvbRcsFwdStatusGroup OBJECT-GROUP
      OBJECTS {
          dvbRcsFwdStatusPopId,
          dvbRcsFwdStatusIfReference,
          dvbRcsFwdStatusNetId,
          dvbRcsFwdStatusNetName,
          dvbRcsFwdStatusFormat,
          dvbRcsFwdStatusFrequency,
          dvbRcsFwdStatusPolar,
          dvbRcsFwdStatusInnerFec,
          dvbRcsFwdStatusSymbolRate,
          dvbRcsFwdStatusRolloff,
          dvbRcsFwdStatusModulation,
          dvbRcsFwdStatusFecFrame,
          dvbRcsFwdStatusPilot,
          dvbRcsFwdStatusBer,
          dvbRcsFwdStatusCnr,
          dvbRcsFwdStatusRxPower
       }
      STATUS    current
      DESCRIPTION
          "A collection of objects providing forward link status."
   ::= {dvbRcsRcstGroups 16}

   --=============================================================
   --    object groups for return link
   --=============================================================
    dvbRcsRtnConfigGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsRtnConfigDefIfLevel
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects providing basic return link
           configuration support."
   ::= {dvbRcsRcstGroups 17}

   dvbRcsRtnExtConfigGroup OBJECT-GROUP
      OBJECTS {
          dvbRcsRtnConfigMaxEirp
          }
      STATUS    current
      DESCRIPTION
          "A collection of objects providing extended return link





          configuration support."
   ::= {dvbRcsRcstGroups 18}

   dvbRcsRtnStatusGroup OBJECT-GROUP
      OBJECTS {
          dvbRcsRtnStatusPayloadUnit
          }
      STATUS    current
      DESCRIPTION
          "A collection of objects allowing access to return link
          status."
   ::= {dvbRcsRcstGroups 19}

   dvbRcsRtnExtStatusGroup OBJECT-GROUP
       OBJECTS {
           dvbRcsRcstRtnLinkStatus,
           dvbRcsRtnStatusEbN0,
           dvbRcsRtnStatusSFDuration
           }
       STATUS    current
       DESCRIPTION
           "A collection of objects allowing access to extended
           return link status."
   ::= {dvbRcsRcstGroups 20}

   dvbRcsRcstOduListGroup OBJECT-GROUP
          OBJECTS {
              dvbRcsOduTxTypeDescription,
              dvbRcsOduTxType,
              dvbRcsOduRxTypeDescription,
              dvbRcsOduRxType,
              dvbRcsOduAntennaTypeDescription,
              dvbRcsOduAntennaType
              }
          STATUS    current
          DESCRIPTION
              "A collection of objects supporting flexible
              selection of ODU devices."
   ::= {dvbRcsRcstGroups 21}

   END











