DOT12-IF-MIB DEFINITIONS ::= BEGIN


          IMPORTS
              transmission, Counter32, Counter64, OBJECT-TYPE,
              MODULE-IDENTITY
                  FROM SNMPv2-SMI
              MODULE-COMPLIANCE, OBJECT-GROUP
                  FROM SNMPv2-CONF
              ifIndex
                  FROM IF-MIB;

          dot12MIB MODULE-IDENTITY
               LAST-UPDATED "9602220452Z"  -- February 22, 1996
               ORGANIZATION "IETF 100VG-AnyLAN MIB Working Group"
               CONTACT-INFO
                       "       John Flick

                       Postal: Hewlett Packard Company
                               8000 Foothills Blvd. M/S 5556
                               Roseville, CA 95747-5556
                       Tel:    +1 916 785 4018
                       Fax:    +1 916 785 3583

                       E-mail: johnf@hprnd.rose.hp.com"
               DESCRIPTION
                       "This MIB module describes objects for
                       managing IEEE 802.12 interfaces."
               ::= { transmission 45 }

          dot12MIBObjects     OBJECT IDENTIFIER ::= { dot12MIB 1 }

          dot12ConfigTable OBJECT-TYPE
              SYNTAX     SEQUENCE OF Dot12ConfigEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "Configuration information for a collection of
                      802.12 interfaces attached to a particular
                      system."
              ::= { dot12MIBObjects 1 }

          dot12ConfigEntry OBJECT-TYPE
              SYNTAX     Dot12ConfigEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION





                      "Configuration for a particular interface to an
                      802.12 medium."
              INDEX      { ifIndex }
              ::= { dot12ConfigTable 1 }

          Dot12ConfigEntry ::=
              SEQUENCE {
                  dot12CurrentFramingType         INTEGER,
                  dot12DesiredFramingType         INTEGER,
                  dot12FramingCapability          INTEGER,
                  dot12DesiredPromiscStatus       INTEGER,
                  dot12TrainingVersion            INTEGER,
                  dot12LastTrainingConfig         OCTET STRING,
                  dot12Commands                   INTEGER,
                  dot12Status                     INTEGER,
                  dot12ControlMode                INTEGER
              }

          dot12CurrentFramingType OBJECT-TYPE
              SYNTAX     INTEGER {
                             frameType88023(1),
                             frameType88025(2),
                             frameTypeUnknown(3)
                         }
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "When dot12DesiredFramingType is one of
                      'frameType88023' or 'frameType88025', this is the
                      type of framing asserted by the interface.

                      When dot12DesiredFramingType is 'frameTypeEither',
                      dot12CurrentFramingType shall be one of
                      'frameType88023' or 'frameType88025' when the
                      dot12Status is 'opened'.   When the dot12Status is
                      anything other than 'opened',
                      dot12CurrentFramingType shall take the value of
                      'frameTypeUnknown'."
              ::= { dot12ConfigEntry 1 }

          dot12DesiredFramingType OBJECT-TYPE
              SYNTAX     INTEGER {
                             frameType88023(1),
                             frameType88025(2),
                             frameTypeEither(3)
                         }
              MAX-ACCESS read-write
              STATUS     current





              DESCRIPTION
                      "The type of framing which will be requested by
                      the interface during the next interface MAC
                      initialization or open action.

                      In master mode, this is the framing mode which
                      will be granted by the interface.  Note that
                      for a master mode interface, this object must be
                      equal to 'frameType88023' or 'frameType88025',
                      since a master mode interface cannot grant
                      'frameTypeEither'."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aDesiredFramingType."
              ::= { dot12ConfigEntry 2 }

          dot12FramingCapability OBJECT-TYPE
              SYNTAX     INTEGER {
                             frameType88023(1),
                             frameType88025(2),
                             frameTypeEither(3)
                         }
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The type of framing this interface is capable of
                      supporting."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aFramingCapability."
              ::= { dot12ConfigEntry 3 }

          dot12DesiredPromiscStatus OBJECT-TYPE
              SYNTAX     INTEGER {
                             singleAddressMode(1),
                             promiscuousMode(2)
                         }
              MAX-ACCESS read-write
              STATUS     current
              DESCRIPTION
                      "This object is used to select the promiscuous
                      mode that this interface will request in the next
                      training packet issued on this interface.
                      Whether the repeater grants the requested mode
                      must be verified by examining the state of the PP
                      bits in the corresponding instance of
                      dot12LastTrainingConfig.






                      In master mode, this object controls whether or
                      not promiscuous mode will be granted by the
                      interface when requested by the lower level
                      device.

                      Note that this object indicates the desired mode
                      for the next time the interface trains.  The
                      currently active mode will be reflected in
                      dot12LastTrainingConfig and in ifPromiscuousMode."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aDesiredPromiscuousStatus."
              ::= { dot12ConfigEntry 4 }

          dot12TrainingVersion OBJECT-TYPE
              SYNTAX     INTEGER (0..7)
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The value that will be used in the version bits
                      (vvv bits) in training frames on this interface.
                      This is the highest version number supported by
                      this MAC."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aMACVersion."
              ::= { dot12ConfigEntry 5 }

          dot12LastTrainingConfig OBJECT-TYPE
              SYNTAX     OCTET STRING (SIZE(2))
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This 16 bit field contains the configuration
                      bits from the most recent error-free training
                      frame received during training on this interface.
                      Training request frames are received when in
                      master mode, while training response frames are
                      received in slave mode.  On master mode interfaces,
                      this object contains the contents of the
                      requested configuration field of the most recent
                      training request frame.  On slave mode interfaces,
                      this object contains the contents of the allowed
                      configuration field of the most recent training
                      response frame.  The format of the current version
                      of this field is described in section 3.8.  Please
                      refer to the most recent version of the IEEE
                      802.12 standard for the most up-to-date definition





                      of the format of this object."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aLastTrainingConfig."
              ::= { dot12ConfigEntry 6 }

          dot12Commands OBJECT-TYPE
              SYNTAX     INTEGER {
                             noOp(1),
                             open(2),
                             reset(3),
                             close(4)
                         }
              MAX-ACCESS read-write
              STATUS     current
              DESCRIPTION
                      "If the current value of dot12Status is 'closed',
                      setting the value of this object to 'open' will
                      change the corresponding instance of MIB-II's
                      ifAdminStatus to 'up', cause this interface to
                      enter the 'opening' state, and will cause training
                      to be initiated on this interface.  The progress
                      and success of the open is given by the values of
                      the dot12Status object.  Setting this object to
                      'open' when dot12Status has a value other than
                      'closed' has no effect.

                      Setting the corresponding instance of ifAdminStatus
                      to 'up' when the current value of dot12Status is
                      'closed' will have the same effect as setting this
                      object to 'open'.  Setting ifAdminStatus to 'up'
                      when dot12Status has a value other than 'closed'
                      has no effect.

                      Setting the value of this object to 'close' will
                      move this interface into the 'closed' state and
                      cause all transmit and receive actions to stop.
                      This object will then have to be set to 'open' in
                      order to reinitiate training.

                      Setting the corresponding instance of ifAdminStatus
                      to 'down' will have the same effect as setting this
                      object to 'close'.

                      Setting the value of this object to 'reset' when
                      the current value of dot12Status has a value other
                      than 'closed' will reset the interface.  On a
                      reset, all MIB counters should retain their values.





                      This will cause the MAC to initiate an
                      acInitializeMAC action as specified in IEEE 802.12.
                      This will cause training to be reinitiated on this
                      interface.  Setting this object to 'reset' when
                      dot12Status has a value of 'closed' has no effect.
                      Setting this object to 'reset' has no effect on the
                      corresponding instance of ifAdminStatus.

                      Setting the value of this object to 'noOp' has no
                      effect.

                      When read, this object will always have a value
                      of 'noOp'."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.2,
                      acOpen, acClose, acInitializeMAC.
                      Also, RFC1231 IEEE802.5 Token Ring MIB,
                      dot5Commands."
              ::= { dot12ConfigEntry 7 }

          dot12Status OBJECT-TYPE
              SYNTAX     INTEGER {
                             opened(1),
                             closed(2),
                             opening(3),
                             openFailure(5),
                             linkFailure(6)
                         }
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "The current interface status with respect to
                      training.  One of the following values:

                          opened      - Training has completed
                                        successfully.
                          closed      - MAC has been disabled by
                                        setting dot12Commands to
                                        'close'.
                          opening     - MAC is in training.  Training
                                        signals have been received.
                          openFailure - Passed 24 error-free packets,
                                        but there is a problem, noted
                                        in the training configuration
                                        bits (dot12LastTrainingConfig).
                          linkFailure - Training signals not received,
                                        or could not pass 24 error-free
                                        packets.





                      Whenever the dot12Commands object is set to
                      'close' or ifAdminStatus is set to 'down', the MAC
                      will go silent, dot12Status will be 'closed', and
                      ifOperStatus will be 'down'.

                      When the value of this object is equal to 'closed'
                      and the dot12Commands object is set to 'open' or
                      the ifAdminStatus object is set to 'up', training
                      will be initiated on this interface.  When the
                      value of this object is not equal to 'closed' and
                      the dot12Commands object is set to 'reset',
                      training will be reinitiated on this interface.
                      Note that sets of some other objects (e.g.
                      dot12ControlMode) or external events (e.g. MAC
                      protocol violations) may also cause training to be
                      reinitiated on this interface.

                      When training is initiated or reinitiated on an
                      interface, the end node will send Training_Up to
                      the master and initially go to the 'linkFailure'
                      state and ifOperStatus will go to 'down'.
                      When the master sends back Training_Down,
                      dot12Status will change to the 'opening' state,
                      and training packets will be transferred.

                      After all of the training packets have been
                      passed, dot12Status will change to 'linkFailure'
                      if 24 consecutive error-free packets were not
                      passed, 'opened' if 24 consecutive error-free
                      packets were passed and the training
                      configuration bits were OK, or 'openFailure' if
                      there were 24 consecutive error-free packets, but
                      there was a problem with the training
                      configuration bits.

                      When in the 'openFailure' state, the
                      dot12LastTrainingConfig object will contain the
                      configuration bits from the last training
                      packet which can be examined to determine the
                      exact reason for the training configuration
                      failure.

                      If training did not succeed (dot12Status is
                      'linkFailure' or 'openFailure), the entire
                      process will be restarted after
                      MAC_Retraining_Delay_Timer seconds.

                      If training does succeed (dot12Status changes to





                      'opened'), ifOperStatus will change to 'up'.  If
                      training does not succeed (dot12Status changes to
                      'linkFailure' or 'openFailure'), ifOperStatus will
                      remain 'down'."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aMACStatus."
              ::= { dot12ConfigEntry 8 }

          dot12ControlMode OBJECT-TYPE
              SYNTAX     INTEGER {
                             masterMode(1),
                             slaveMode(2),
                             learn(3)
                         }
              MAX-ACCESS read-write
              STATUS     current
              DESCRIPTION
                      "This object is used to configure and report
                      whether or not this interface is operating in
                      master mode.  In a Demand Priority network, end
                      node interfaces typically operate in slave mode,
                      while switch interfaces may control the Demand
                      Priority protocol and operate in master mode.

                      This object may be implemented as a read-only
                      object by those agents and interfaces that do not
                      implement software control of master mode.  In
                      particular, interfaces that cannot operate in
                      master mode, and interfaces on which master mode
                      is controlled by a pushbutton on the device,
                      should implement this object read-only.

                      Some interfaces do not require network management
                      configuration of this feature and can autosense
                      whether to use master mode or slave mode.  The
                      value 'learn' is used for that purpose.  While
                      autosense is taking place, the value 'learn' is
                      returned.

                      A network management operation which modifies the
                      value of dot12ControlMode causes the interface
                      to retrain."
              ::= { dot12ConfigEntry 9 }

          dot12StatTable OBJECT-TYPE
              SYNTAX     SEQUENCE OF Dot12StatEntry
              MAX-ACCESS not-accessible





              STATUS     current
              DESCRIPTION
                      "Statistics for a collection of 802.12 interfaces
                      attached to a particular system."
              ::= { dot12MIBObjects 2 }

          dot12StatEntry OBJECT-TYPE
              SYNTAX     Dot12StatEntry
              MAX-ACCESS not-accessible
              STATUS     current
              DESCRIPTION
                      "Statistics for a particular interface to an
                      802.12 medium.  The receive statistics in this
                      table apply only to packets received by this
                      station (i.e., packets whose destination address
                      is either the local station address, the
                      broadcast address, or a multicast address that
                      this station is receiving, unless the station is
                      in promiscuous mode)."
              INDEX      { ifIndex }
              ::= { dot12StatTable 1 }

          Dot12StatEntry ::=
              SEQUENCE {
                  dot12InHighPriorityFrames       Counter32,
                  dot12InHighPriorityOctets       Counter32,
                  dot12InNormPriorityFrames       Counter32,
                  dot12InNormPriorityOctets       Counter32,
                  dot12InIPMErrors                Counter32,
                  dot12InOversizeFrameErrors      Counter32,
                  dot12InDataErrors               Counter32,
                  dot12InNullAddressedFrames      Counter32,
                  dot12OutHighPriorityFrames      Counter32,
                  dot12OutHighPriorityOctets      Counter32,
                  dot12TransitionIntoTrainings    Counter32,
                  dot12HCInHighPriorityOctets     Counter64,
                  dot12HCInNormPriorityOctets     Counter64,
                  dot12HCOutHighPriorityOctets    Counter64
              }

          dot12InHighPriorityFrames OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of high priority frames
                      that have been received on this interface.
                      Includes both good and bad high priority frames,





                      as well as high priority training frames.  Does
                      not include normal priority frames which were
                      priority promoted."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aHighPriorityFramesReceived."
              ::= { dot12StatEntry 1 }

          dot12InHighPriorityOctets OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of the number of octets
                      contained in high priority frames that have been
                      received on this interface. This counter is
                      incremented by OctetCount for each frame received
                      on this interface which is counted by
                      dot12InHighPriorityFrames.

                      Note that this counter will roll over very
                      quickly.  It is provided for backward
                      compatibility for Network Management protocols
                      that do not support 64 bit counters (e.g. SNMP
                      version 1)."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aHighPriorityOctetsReceived."
              ::= { dot12StatEntry 2 }

          dot12InNormPriorityFrames OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of normal priority frames
                      that have been received on this interface.
                      Includes both good and bad normal priority
                      frames, as well as normal priority training
                      frames and normal priority frames which were
                      priority promoted."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aNormalPriorityFramesReceived."
              ::= { dot12StatEntry 3 }

          dot12InNormPriorityOctets OBJECT-TYPE
              SYNTAX     Counter32





              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of the number of octets
                      contained in normal priority frames that have
                      been received on this interface. This counter is
                      incremented by OctetCount for each frame received
                      on this interface which is counted by
                      dot12InNormPriorityFrames.

                      Note that this counter will roll over very
                      quickly.  It is provided for backward
                      compatibility for Network Management protocols
                      that do not support 64 bit counters (e.g. SNMP
                      version 1)."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aNormalPriorityOctetsReceived."
              ::= { dot12StatEntry 4 }

          dot12InIPMErrors OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of the number of frames
                      that have been received on this interface with an
                      invalid packet marker and no PMI errors.  A
                      repeater will write an invalid packet marker to
                      the end of a frame containing errors as it is
                      forwarded through the repeater to the other
                      ports.  This counter is incremented by one for
                      each frame received on this interface which has
                      had an invalid packet marker added to the end of
                      the frame."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aIPMFramesReceived."
              ::= { dot12StatEntry 5 }

          dot12InOversizeFrameErrors OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of oversize frames
                      received on this interface.  This counter is
                      incremented by one for each frame received on





                      this interface whose OctetCount is larger than
                      the maximum legal frame size.  The frame size
                      which causes this counter to increment is
                      dependent on the current framing type."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aOversizeFramesReceived."
              ::= { dot12StatEntry 6 }

          dot12InDataErrors OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of errored frames
                      received on this interface.  This counter is
                      incremented by one for each frame received on
                      this interface with any of the following errors:
                      bad FCS (with no IPM), PMI errors (excluding
                      frames with an IPM as the only PMI error),
                      undersize, bad start of frame delimiter, or bad
                      end of packet marker.  Does not include frames
                      counted by dot12InIPMErrors,
                      dot12InNullAddressedFrames, or
                      dot12InOversizeFrameErrors.

                      This counter indicates problems with the cable
                      directly attached to this interface, while
                      dot12InIPMErrors indicates problems with remote
                      cables."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aDataErrorFramesReceived."
              ::= { dot12StatEntry 7 }

          dot12InNullAddressedFrames OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of null addressed frames
                      received on this interface.  This counter is
                      incremented by one for each frame received on
                      this interface with a destination MAC address
                      consisting of all zero bits.  Both void and
                      training frames are included in this counter.

                      Note that since this station would normally not





                      receive null addressed frames, this counter is
                      only incremented when this station is operating
                      in promiscuous mode or in training."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aNullAddressedFramesReceived."
              ::= { dot12StatEntry 8 }

          dot12OutHighPriorityFrames OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This counter is incremented by one for each high
                      priority frame successfully transmitted out this
                      interface."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aHighPriorityFramesTransmitted."
              ::= { dot12StatEntry 9 }

          dot12OutHighPriorityOctets OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This counter is incremented by OctetCount for
                      each frame counted by dot12OutHighPriorityFrames.

                      Note that this counter will roll over very
                      quickly.  It is provided for backward
                      compatibility for Network Management protocols
                      that do not support 64 bit counters (e.g. SNMP
                      version 1)."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aHighPriorityOctetsTransmitted."
              ::= { dot12StatEntry 10 }

          dot12TransitionIntoTrainings OBJECT-TYPE
              SYNTAX     Counter32
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of the number of times
                      this interface has entered the training state.
                      This counter is incremented by one each time
                      dot12Status transitions to 'linkFailure' from any





                      state other than 'opening' or 'openFailure'."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aTransitionsIntoTraining."
              ::= { dot12StatEntry 11 }

          dot12HCInHighPriorityOctets OBJECT-TYPE
              SYNTAX     Counter64
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of the number of octets
                      contained in high priority frames that have been
                      received on this interface. This counter is
                      incremented by OctetCount for each frame received
                      on this interface which is counted by
                      dot12InHighPriorityFrames.

                      This counter is a 64 bit version of
                      dot12InHighPriorityOctets.  It should be used by
                      Network Management protocols which support 64 bit
                      counters (e.g. SNMPv2)."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aHighPriorityOctetsReceived."
              ::= { dot12StatEntry 12 }

          dot12HCInNormPriorityOctets OBJECT-TYPE
              SYNTAX     Counter64
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This object is a count of the number of octets
                      contained in normal priority frames that have
                      been received on this interface. This counter is
                      incremented by OctetCount for each frame received
                      on this interface which is counted by
                      dot12InNormPriorityFrames.

                      This counter is a 64 bit version of
                      dot12InNormPriorityOctets.  It should be used by
                      Network Management protocols which support 64 bit
                      counters (e.g. SNMPv2)."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aNormalPriorityOctetsReceived."
              ::= { dot12StatEntry 13 }






          dot12HCOutHighPriorityOctets OBJECT-TYPE
              SYNTAX     Counter64
              MAX-ACCESS read-only
              STATUS     current
              DESCRIPTION
                      "This counter is incremented by OctetCount for
                      each frame counted by dot12OutHighPriorityFrames.

                      This counter is a 64 bit version of
                      dot12OutHighPriorityOctets.  It should be used by
                      Network Management protocols which support 64 bit
                      counters (e.g. SNMPv2)."
              REFERENCE
                      "IEEE Standard 802.12-1995, 13.2.5.2.1,
                      aHighPriorityOctetsTransmitted."
             ::= { dot12StatEntry 14 }

          -- conformance information

          dot12Conformance  OBJECT IDENTIFIER ::= { dot12MIB 2 }

          dot12Compliances  OBJECT IDENTIFIER ::= { dot12Conformance 1 }
          dot12Groups       OBJECT IDENTIFIER ::= { dot12Conformance 2 }

          -- compliance statements

          dot12Compliance MODULE-COMPLIANCE
              STATUS     current
              DESCRIPTION
                         "The compliance statement for managed network
                         entities that have 802.12 interfaces."

              MODULE  -- this module
                  MANDATORY-GROUPS { dot12ConfigGroup, dot12StatsGroup }

                  OBJECT       dot12DesiredFramingType
                  MIN-ACCESS   read-only
                  DESCRIPTION
                         "Write access to this object is not required."

                  OBJECT       dot12DesiredPromiscStatus
                  MIN-ACCESS   read-only
                  DESCRIPTION
                         "Write access to this object is not required."

                  OBJECT       dot12Commands
                  MIN-ACCESS   read-only
                  DESCRIPTION





                         "Write access to this object is not required."

                  OBJECT       dot12ControlMode
                  MIN-ACCESS   read-only
                  DESCRIPTION
                         "Write access to this object is not required."
              ::= { dot12Compliances 1 }

          -- units of conformance

          dot12ConfigGroup OBJECT-GROUP
              OBJECTS    { dot12DesiredFramingType,
                           dot12FramingCapability,
                           dot12DesiredPromiscStatus,
                           dot12TrainingVersion,
                           dot12LastTrainingConfig,
                           dot12Commands, dot12Status,
                           dot12CurrentFramingType,
                           dot12ControlMode }
              STATUS     current
              DESCRIPTION
                      "A collection of objects for managing the status
                      and configuration of IEEE 802.12 interfaces."
              ::= { dot12Groups 1 }

          dot12StatsGroup OBJECT-GROUP
              OBJECTS    { dot12InHighPriorityFrames,
                           dot12InHighPriorityOctets,
                           dot12InNormPriorityFrames,
                           dot12InNormPriorityOctets,
                           dot12InIPMErrors,
                           dot12InOversizeFrameErrors,
                           dot12InDataErrors,
                           dot12InNullAddressedFrames,
                           dot12OutHighPriorityFrames,
                           dot12OutHighPriorityOctets,
                           dot12TransitionIntoTrainings,
                           dot12HCInHighPriorityOctets,
                           dot12HCInNormPriorityOctets,
                           dot12HCOutHighPriorityOctets }
              STATUS     current
              DESCRIPTION
                      "A collection of objects providing statistics for
                      IEEE 802.12 interfaces."
              ::= { dot12Groups 2 }

      END





