T11-FC-VIRTUAL-FABRIC-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE,
       Unsigned32, mib-2
                               FROM SNMPv2-SMI         -- [RFC2578]
       MODULE-COMPLIANCE, OBJECT-GROUP
                               FROM SNMPv2-CONF        -- [RFC2580]
       RowStatus, StorageType  FROM SNMPv2-TC          -- [RFC2579]
       InterfaceIndex          FROM IF-MIB             -- [RFC2863]
       fcmInstanceIndex, FcNameIdOrZero,
       fcmPortEntry, fcmSwitchEntry
                               FROM FC-MGMT-MIB        -- [RFC4044]
       T11FabricIndex          FROM T11-TC-MIB;        -- [RFC4439]

   t11FcVirtualFabricMIB  MODULE-IDENTITY
       LAST-UPDATED    "200611100000Z"
       ORGANIZATION    "IETF IMSS (Internet and Management Support
                        for Storage) Working Group"
       CONTACT-INFO
               "
                        Scott Kipp
                        McDATA Corporation
                   Tel: +1 720 558-3452
                E-mail: scott.kipp@mcdata.com
                Postal: 4 McDATA Parkway
                        Broomfield, CO USA 80021

                        G D Ramkumar
                        SnapTell, Inc.
                   Tel: +1 650-326-7627
                E-mail: gramkumar@stanfordalumni.org
                Postal: 2741 Middlefield Rd, Suite 200
                        Palo Alto, CA USA 94306

                        Keith McCloghrie
                        Cisco Systems, Inc.
                   Tel: +1 408 526-5260
                E-mail: kzm@cisco.com
                Postal: 170 West Tasman Drive
                        San Jose, CA USA 95134
               "

       DESCRIPTION
           "This module defines management information specific to
            Fibre Channel Virtual Fabrics.  A Virtual Fabric is a





            Fabric composed of partitions of switches, links and
            N_Ports with a single Fabric management domain, Fabric
            Services and independence from other Virtual Fabrics.

            Copyright (C) The IETF Trust (2006).  This version of
            this MIB module is part of RFC 4747; see the RFC itself for
            full legal notices."
       REVISION        "200611100000Z"
       DESCRIPTION
           "Initial version of this MIB module, published as RFC 4747."
       ::= { mib-2 147 }

   t11vfObjects       OBJECT IDENTIFIER ::= { t11FcVirtualFabricMIB 1 }
   t11vfConformance   OBJECT IDENTIFIER ::= { t11FcVirtualFabricMIB 2 }

   --********************************
   --  MIB object definitions
   --

   t11vfCoreSwitchTable  OBJECT-TYPE
       SYNTAX      SEQUENCE OF T11vfCoreSwitchEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table of core switches supported by the current
            management entity."
       ::= { t11vfObjects 1 }

   t11vfCoreSwitchEntry OBJECT-TYPE
       SYNTAX      T11vfCoreSwitchEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Each entry represents one core switch."
       INDEX   { fcmInstanceIndex, t11vfCoreSwitchSwitchName }
       ::= { t11vfCoreSwitchTable 1}

   T11vfCoreSwitchEntry ::=
       SEQUENCE {
          t11vfCoreSwitchSwitchName   FcNameIdOrZero,
          t11vfCoreSwitchMaxSupported Unsigned32,
         t11vfCoreSwitchStorageType  StorageType
       }

   t11vfCoreSwitchSwitchName OBJECT-TYPE
       SYNTAX      FcNameIdOrZero (SIZE(8 | 16))
       MAX-ACCESS  not-accessible
       STATUS      current





       DESCRIPTION
           "The Core Switch_Name (WWN) of this Core Switch."
       ::= { t11vfCoreSwitchEntry 1 }

   t11vfCoreSwitchMaxSupported OBJECT-TYPE
       SYNTAX      Unsigned32 (1..4095)
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "In switches that do not support Virtual Fabrics,
            this object has the value of 1.  If Virtual Fabrics
            are supported, this object is the maximum number of
            Virtual Fabrics supported by the Core Switch.  For
            the purpose of this count, the Control VF_ID is
            ignored."
       ::= { t11vfCoreSwitchEntry 2 }

   t11vfCoreSwitchStorageType OBJECT-TYPE
       SYNTAX      StorageType
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The storage type for this conceptual row.
            Conceptual rows having the value 'permanent' need not
            allow write-access to any columnar objects in the row."
       DEFVAL { nonVolatile }
       ::= { t11vfCoreSwitchEntry 3 }

   -- Virtual Switch table

   t11vfVirtualSwitchTable  OBJECT-TYPE
       SYNTAX      SEQUENCE OF T11vfVirtualSwitchEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table of Virtual Switches.  When one Core Switch
            provides switching functions for multiple Virtual Fabrics,
            that Core Switch is modeled as containing multiple
            Virtual Switches, one for each Virtual Fabric.  This table
            contains one row for every Virtual Switch on every Core
            Switch.  This table augments the basic switch information in
            the fcmSwitchTable Table in the FC-MGMT-MIB."
       REFERENCE
           "fcmSwitchTable is defined in the FC-MGMT-MIB [RFC4044]."
       ::= { t11vfObjects 2 }

   t11vfVirtualSwitchEntry OBJECT-TYPE
       SYNTAX      T11vfVirtualSwitchEntry





       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry of the Virtual Switch table.  Each row is for a
            Virtual Switch.

            This table augments the fcmSwitchTable, i.e., every entry
            in this table has a one-to-one correspondence with an
            entry in the fcmSwitchTable.  At the time when the
            fcmSwitchTable was defined, it applied to physical
            switches.  With the definition and usage of virtual
            switches, fcmSwitchTable now applies to virtual switches
            as well as physical switches, and (in contrast to physical
            switches) it is appropriate to provide the capability for
            virtual switches to be created via remote management
            applications, e.g., via SNMP.

            So, this entry contains a RowStatus object (to allow the
            creation of a virtual switch), as well as a StorageType
            object.  Obviously, if a row is created/deleted in this
            table, the corresponding row in the fcmSwitchTable will
            be created/deleted."
       REFERENCE
           "fcmSwitchEntry is defined in the FC-MGMT-MIB module
            [RFC4044]."
       AUGMENTS   { fcmSwitchEntry }
       ::= { t11vfVirtualSwitchTable 1}

   T11vfVirtualSwitchEntry ::=
       SEQUENCE {
           t11vfVirtualSwitchVfId               T11FabricIndex,
           t11vfVirtualSwitchCoreSwitchName     FcNameIdOrZero,
           t11vfVirtualSwitchRowStatus          RowStatus,
           t11vfVirtualSwitchStorageType       StorageType
       }

   t11vfVirtualSwitchVfId OBJECT-TYPE
       SYNTAX      T11FabricIndex
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The VF_ID of the Virtual Fabric for which this virtual
            switch performs its switching function.  The Control
            VF_ID is implicitly enabled and is not set.
            Communication with the Control VF_ID is required."
       REFERENCE
           "FC-SW-4, REV 7.5, section 12.2"
       ::= { t11vfVirtualSwitchEntry 1 }






   t11vfVirtualSwitchCoreSwitchName OBJECT-TYPE
       SYNTAX      FcNameIdOrZero (SIZE(8 | 16))
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The Core Switch_Name (WWN) of the Core Switch that
            contains this Virtual Switch."
       REFERENCE
           "FC-SW-4, REV 7.5, section 12.2."
       ::= { t11vfVirtualSwitchEntry 2 }

   t11vfVirtualSwitchRowStatus OBJECT-TYPE
           SYNTAX      RowStatus
           MAX-ACCESS  read-create
           STATUS      current
           DESCRIPTION
               "The status of this row."
           ::= { t11vfVirtualSwitchEntry 3 }

   t11vfVirtualSwitchStorageType OBJECT-TYPE
       SYNTAX      StorageType
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The storage type for this conceptual row.
            Conceptual rows having the value 'permanent' need not
            allow write-access to any columnar objects in the row."
       DEFVAL { nonVolatile }
       ::= { t11vfVirtualSwitchEntry 4 }

   -- Port table

   t11vfPortTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF T11vfPortEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table of Port attributes related to Virtual Fabrics."
       ::= { t11vfObjects 3 }

   t11vfPortEntry OBJECT-TYPE
       SYNTAX      T11vfPortEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Each entry represents a physical Port on a switch.
            Switches that support Virtual Fabrics would add





            these four additional columns to the fcmPortEntry
            row."
       REFERENCE
           "fcmPortEntry is defined in the FC-MGMT-MIB module."
       AUGMENTS   { fcmPortEntry }
       ::= { t11vfPortTable 1}

   T11vfPortEntry ::=
       SEQUENCE {
           t11vfPortVfId                T11FabricIndex,
           t11vfPortTaggingAdminStatus   INTEGER,
           t11vfPortTaggingOperStatus    INTEGER,
           t11vfPortStorageType        StorageType
       }

   t11vfPortVfId OBJECT-TYPE
       SYNTAX      T11FabricIndex
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The Port VF_ID assigned to this Port.  The Port VF_ID is the
            default Virtual Fabric that is assigned to untagged frames
            arriving at this Port.  The Control VF_ID is implicitly
            enabled and is not set.  Communication with the Control
            VF_ID is required."
       REFERENCE
           "FC-SW-4, REV 7.5, section 12.1"
       DEFVAL    {1}
       ::= { t11vfPortEntry 1 }

   t11vfPortTaggingAdminStatus OBJECT-TYPE
       SYNTAX INTEGER {
           off(1),
           on(2),
           auto(3)
       }
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "This object is used to configure the administrative status
            of Virtual Fabric tagging on this Port.

            SET operation   Description
            --------------  -------------------------------------------
            off(1)          To disable Virtual Fabric tagging on this
                            Port.

            on(2)           To enable Virtual Fabric tagging on this





                            Port if the attached Port doesn't
                            prohibit it.

            auto(3)         To enable Virtual Fabric tagging if the
                            peer requests it."
       REFERENCE
           "FC-SW-4, REV 7.5, section 12.4"
       ::= { t11vfPortEntry 2 }

    t11vfPortTaggingOperStatus OBJECT-TYPE
       SYNTAX INTEGER {
           off(1),
           on(2)
               }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "This object is used to report the operational status of
            Virtual Fabric tagging on this Port.

            SET operation   Description
            --------------  -------------------------------------------
            off(1)          Virtual Fabric tagging is disabled on this
                            Port.

            on(2)           Virtual Fabric tagging is enabled on this
                            Port."
       REFERENCE
           "FC-SW-4, REV 7.5, section 12.4"
       ::= { t11vfPortEntry 3 }

   t11vfPortStorageType OBJECT-TYPE
       SYNTAX      StorageType
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The storage type for this conceptual row, and for the
            corresponding row in the augmented fcmPortTable.

            Conceptual rows having the value 'permanent' need not
            allow write-access to any columnar objects in the row."
       DEFVAL { nonVolatile }
       ::= { t11vfPortEntry 4 }


   -- Locally Enabled Table

   t11vfLocallyEnabledTable OBJECT-TYPE





       SYNTAX      SEQUENCE OF T11vfLocallyEnabledEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table for assigning and reporting operational status of
            locally-enabled Virtual Fabric IDs to Ports.  The set of
            Virtual Fabrics operational on the Port is the bit-wise
            'AND' of the set of locally-enabled VF_IDs of this Port
            and the locally-enabled VF_IDs of the attached Port."
       ::= { t11vfObjects 4 }

   t11vfLocallyEnabledEntry OBJECT-TYPE
       SYNTAX      T11vfLocallyEnabledEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry for each locally-enabled VF_ID on
            each Port."
       REFERENCE
           "FC-SW-4, REV 7.5, section 12.4"
       INDEX { t11vfLocallyEnabledPortIfIndex, t11vfLocallyEnabledVfId }

       ::= { t11vfLocallyEnabledTable 1}

   T11vfLocallyEnabledEntry ::=
       SEQUENCE {
           t11vfLocallyEnabledPortIfIndex    InterfaceIndex,
           t11vfLocallyEnabledVfId           T11FabricIndex,
           t11vfLocallyEnabledOperStatus     INTEGER,
           t11vfLocallyEnabledRowStatus      RowStatus,
           t11vfLocallyEnabledStorageType    StorageType
       }

   t11vfLocallyEnabledPortIfIndex OBJECT-TYPE
       SYNTAX      InterfaceIndex
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The value of the ifIndex that identifies the Port."
       ::= { t11vfLocallyEnabledEntry 1 }

   t11vfLocallyEnabledVfId OBJECT-TYPE
       SYNTAX      T11FabricIndex
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A locally-enabled VF_ID on this Port."
       ::= { t11vfLocallyEnabledEntry 2 }






   t11vfLocallyEnabledOperStatus OBJECT-TYPE
       SYNTAX INTEGER {
           off(1),
           on(2)
               }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "This object is used to report the operational status of
            Virtual Fabric tagging on this Port.

            SET operation   Description
            --------------  -------------------------------------------
            off(1)          Virtual Fabric tagging is disabled on this
                            Port.

            on(2)           Virtual Fabric tagging is enabled on this
                            Port."
       REFERENCE
           "FC-SW-4, REV 7.3, section 12.4"
       ::= { t11vfLocallyEnabledEntry 3 }

   t11vfLocallyEnabledRowStatus OBJECT-TYPE
           SYNTAX      RowStatus
           MAX-ACCESS  read-create
           STATUS      current
           DESCRIPTION
               "The status of this conceptual row.

                When a row in this table is in 'active(1)' state,
                no object in that row can be modified except
                t11vfLocallyEnabledRowStatus and
                t11vfLocallyEnabledStorageType."
           ::= { t11vfLocallyEnabledEntry 4 }

   t11vfLocallyEnabledStorageType OBJECT-TYPE
           SYNTAX      StorageType
           MAX-ACCESS  read-create
           STATUS      current
           DESCRIPTION
               "The storage type for this conceptual row.
                Conceptual rows having the value 'permanent' need not
                allow write-access to any columnar objects in the row."
           DEFVAL { nonVolatile }
           ::= { t11vfLocallyEnabledEntry 5 }

   --********************************





   -- Conformance Section
   --

   t11vfMIBCompliances OBJECT IDENTIFIER ::= { t11vfConformance 1 }
   t11vfMIBGroups      OBJECT IDENTIFIER ::= { t11vfConformance 2 }

   t11vfMIBCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
           "Describes the requirements for compliance to the
            Fibre Channel Virtual Fabric MIB."
       MODULE  -- this module
           MANDATORY-GROUPS { t11vfGeneralGroup }

           OBJECT t11vfCoreSwitchMaxSupported
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

           OBJECT t11vfCoreSwitchStorageType
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

           OBJECT t11vfVirtualSwitchVfId
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

           OBJECT t11vfVirtualSwitchRowStatus
           SYNTAX RowStatus { active(1) }
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

           OBJECT t11vfVirtualSwitchStorageType
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

           OBJECT t11vfPortVfId
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

           OBJECT t11vfPortTaggingAdminStatus
           MIN-ACCESS read-only
           DESCRIPTION





               "Write access is not required."

           OBJECT t11vfPortStorageType
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

           OBJECT t11vfLocallyEnabledRowStatus
           SYNTAX       RowStatus { active(1) }
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

           OBJECT t11vfLocallyEnabledStorageType
           MIN-ACCESS read-only
           DESCRIPTION
               "Write access is not required."

       ::= { t11vfMIBCompliances 1 }

   -- Units of conformance

       t11vfGeneralGroup  OBJECT-GROUP
           OBJECTS { t11vfCoreSwitchMaxSupported,
                     t11vfVirtualSwitchVfId,
                     t11vfVirtualSwitchCoreSwitchName,
                     t11vfVirtualSwitchRowStatus,
                     t11vfPortVfId,
                     t11vfPortTaggingAdminStatus,
                     t11vfLocallyEnabledOperStatus,
                     t11vfPortTaggingOperStatus,
                     t11vfLocallyEnabledRowStatus,
                  t11vfCoreSwitchStorageType,
                      t11vfVirtualSwitchStorageType,
                     t11vfPortStorageType,
                     t11vfLocallyEnabledStorageType

           }
           STATUS current
           DESCRIPTION
               "A collection of objects for monitoring and
                configuring Virtual Fabrics in a Fibre Channel switch."
           ::= { t11vfMIBGroups 1 }

   END







