HPR-MIB DEFINITIONS ::= BEGIN


  IMPORTS
        DisplayString, DateAndTime, TimeStamp, TEXTUAL-CONVENTION
                FROM SNMPv2-TC

        Counter32, Gauge32, Unsigned32, TimeTicks,
        OBJECT-TYPE, MODULE-IDENTITY
                FROM SNMPv2-SMI

        MODULE-COMPLIANCE, OBJECT-GROUP
                FROM SNMPv2-CONF

        snanauMIB
                FROM SNA-NAU-MIB

        SnaControlPointName
                FROM APPN-MIB;

hprMIB MODULE-IDENTITY
        LAST-UPDATED  "970514000000Z"
        ORGANIZATION  "AIW APPN / HPR MIB SIG"
        CONTACT-INFO

                "

                        Bob Clouston
                        Cisco Systems
                        7025 Kit Creek Road
                        P.O. Box 14987
                        Research Triangle Park, NC 27709, USA
                        Tel:    1 919 472 2333
                        E-mail: clouston@cisco.com

                        Bob Moore
                        IBM Corporation
                        800 Park Offices Drive
                        RHJA/664
                        P.O. Box 12195





                        Research Triangle Park, NC 27709, USA
                        Tel:    1 919 254 4436
                        E-mail: remoore@ralvm6.vnet.ibm.com
                "
      DESCRIPTION
                "This is the MIB module for objects used to
                 manage network devices with HPR capabilities."
::= { snanauMIB 6 }
-- snanauMIB ::= { mib-2 34 }

-- *********************************************************************
-- Textual Conventions
-- *********************************************************************
-- SnaControlPointName is imported from the APPN MIB

HprNceTypes ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "A bit string identifying the set of functions provided by a
          network connection endpoint (NCE).  The following values are
          defined:

                bit 0:  control point
                bit 1:  logical unit
                bit 2:  boundary function
                bit 3:  route setup
          "

      SYNTAX BITS { controlPoint(0),
                    logicalUnit(1),
                    boundaryFunction(2),
                    routeSetup(3) }

HprRtpCounter ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
          "An object providing statistics for an RTP connection.  A
          Management Station can detect discontinuities in this counter
          by monitoring the correspondingly indexed
          hprRtpCounterDisconTime object."

      SYNTAX Counter32

-- *********************************************************************
  hprObjects         OBJECT IDENTIFIER ::= { hprMIB 1 }
-- *********************************************************************

-- *********************************************************************





hprGlobal            OBJECT IDENTIFIER ::= { hprObjects 1 }
-- *********************************************************************
-- The hprGlobal group applies to both intermediate and end nodes.
-- *********************************************************************

hprNodeCpName OBJECT-TYPE
      SYNTAX SnaControlPointName
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "Administratively assigned network name for the APPN node
          where this HPR implementation resides.  If this object has
          the same value as the appnNodeCpName object in the APPN MIB,
          then the two objects are referring to the same APPN node."

      ::= { hprGlobal 1 }

hprOperatorPathSwitchSupport  OBJECT-TYPE
      SYNTAX INTEGER {
                      notSupported(1),
                      switchTriggerSupported(2),
                      switchToPathSupported(3)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "This object indicates an implementation's level of support
          for an operator-requested path switch.

            notSupported(1)           - the agent does not support
                                        operator-requested path switches
            switchTriggerSupported(2) - the agent supports a 'switch
                                        path now' command from an
                                        operator, but not a command to
                                        switch to a specified path
            switchToPathSupported(3)  - the agent supports both a
                                        'switch path now' command and a
                                        command to switch to a specified
                                        path.  Note that the latter
                                        command is not available via
                                        this MIB; a system that supports
                                        it must do so via other means,
                                        such as a local operator
                                        interface."

      ::= { hprGlobal 2 }

-- *********************************************************************





hprAnrRouting        OBJECT IDENTIFIER ::= { hprObjects 2 }
-- *********************************************************************

hprAnrsAssigned OBJECT-TYPE
      SYNTAX Counter32
      UNITS "ANR labels"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of ANR labels assigned by this node since it was
          last re-initialized.  A Management Station can detect
          discontinuities in this counter by monitoring the
          appnNodeCounterDisconTime object in the APPN MIB."

      ::= { hprAnrRouting 1 }

hprAnrCounterState  OBJECT-TYPE
      SYNTAX INTEGER {
                      notActive(1),
                      active(2)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "This object is used for a network management station to turn
          on/off the counting of ANR packets in the hprAnrRoutingTable.
          The initial value of this object is an implementation choice.

                 notActive(1) - the counter hprAnrPacketsReceived
                                returns no meaningful value
                 active(2)    - the counter hprAnrPacketsReceived is
                                being incremented and is returning
                                meaningful values"

      ::= { hprAnrRouting 2 }

hprAnrCounterStateTime OBJECT-TYPE
      SYNTAX DateAndTime
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The time when the hprAnrCounterState object last changed its
          value.  The initial value returned by this object is the time
          at which the APPN node instrumented with this MIB was last
          brought up."

      ::= { hprAnrRouting 3 }






hprAnrRoutingTable OBJECT-TYPE
      SYNTAX SEQUENCE OF HprAnrRoutingEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The ANR Routing table provides a means of correlating an
          incoming ANR label (i.e., one assigned by this node) with the
          TG over which a packet containing the label will be forwarded.
          When the ANR label identifies a local NCE, the hprAnrOutTgDest
          and hprAnrOutTgNum objects have no meaning.  The table also
          contains an object to count the number of packets received
          with a given ANR label."

      ::= { hprAnrRouting 4 }

hprAnrRoutingEntry OBJECT-TYPE
      SYNTAX HprAnrRoutingEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The ANR label is used to index this table."

      INDEX  { hprAnrLabel }

      ::= { hprAnrRoutingTable 1 }

HprAnrRoutingEntry ::= SEQUENCE {
     hprAnrLabel             OCTET STRING,
     hprAnrType              INTEGER,
     hprAnrOutTgDest         DisplayString,
     hprAnrOutTgNum          INTEGER,
     hprAnrPacketsReceived   Counter32,
     hprAnrCounterDisconTime TimeStamp
     }

hprAnrLabel OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (1..8))
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The first ANR label in an incoming packet."

      ::= { hprAnrRoutingEntry 1 }

hprAnrType OBJECT-TYPE
      SYNTAX INTEGER {
                      nce(1),
                      tg(2)





                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "An object indicating whether an ANR label assigned by this
          node identifies a local NCE or a TG on which outgoing packets
          are forwarded.

              nce(1)  - the ANR label identifies a local NCE.  In this
                        case the hprAnrOutTgDest and hprAnrOutTgNum
                        objects have no meaning.
              tg(2)   - the ANR label identifies a TG."

      ::= { hprAnrRoutingEntry 2 }

hprAnrOutTgDest OBJECT-TYPE
      SYNTAX DisplayString (SIZE (0 | 3..17))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "Destination node for the TG over which packets with this ANR
          label are forwarded.  This is the fully qualified name of an
          APPN network node or end node, formatted according to the
          SnaControlPointName textual convention.  If the ANR label
          identifies a local NCE, then this object returns a zero-length
          string.

          This object corresponds to the appnLocalTgDest object in the
          APPN MIB."

      ::= { hprAnrRoutingEntry 3 }

hprAnrOutTgNum OBJECT-TYPE
      SYNTAX INTEGER (0..255)
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "Number of the TG over which packets with this ANR label are
          forwarded.  If the ANR label identifies a local NCE, then this
          object returns the value 0, since 0 is not a valid TG number
          for a TG that supports HPR.

          This object corresponds to the appnLocalTgNum object in the
          APPN MIB."

      ::= { hprAnrRoutingEntry 4 }

hprAnrPacketsReceived OBJECT-TYPE





      SYNTAX Counter32
      UNITS "ANR packets"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of packets received with this ANR label as their
          first label.

          A Management Station can detect discontinuities in this
          counter by monitoring the hprAnrCounterDisconTime object in
          the same row."

      ::= { hprAnrRoutingEntry 5 }

hprAnrCounterDisconTime OBJECT-TYPE
      SYNTAX TimeStamp
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The value of the sysUpTime object when the
          hprAnrPacketsReceived counter for this ANR label last
          experienced a discontinuity.  This will be the more recent of
          two times:  the time at which the ANR label was associated with
          either an outgoing TG or a local NCE, or the time at which the
          ANR counters were last turned on or off."

      ::= { hprAnrRoutingEntry 6 }

-- *********************************************************************
hprTransportUser     OBJECT IDENTIFIER ::= { hprObjects 3 }
-- *********************************************************************
-- Transport Service User (TU) Table: (RTP Connection Users)
--
-- There will be several users of the HPR transport and each HPR node
-- shall maintain a table of these users.
-- *********************************************************************

hprNceTable OBJECT-TYPE
      SYNTAX SEQUENCE OF HprNceEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The Network Connection Endpoint (NCE) table."

      ::= { hprTransportUser 1 }

hprNceEntry OBJECT-TYPE
      SYNTAX HprNceEntry





      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The NCE ID is used to index this table."

      INDEX  { hprNceId }

      ::= { hprNceTable 1 }

HprNceEntry ::= SEQUENCE {
     hprNceId            OCTET STRING,
     hprNceType          HprNceTypes,
     hprNceDefault       HprNceTypes,
     hprNceInstanceId    OCTET STRING
     }

hprNceId OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (1..8))
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The Network Connection Endpoint (NCE) ID.  NCEs identify
          Control Points (Cp), Logical Units (Lu), HPR Boundary
          Functions (Bf) and Route Setup (Rs) Functions.  A value for
          this object can be retrieved from any of the following
          objects in the APPN MIB:

               - appnLsCpCpNceId
               - appnLsRouteNceId
               - appnLsBfNceId
               - appnIsInRtpNceId
               - appnIsRtpNceId

          In each case this value identifies a row in this table
          containing information related to that in the APPN MIB."

      ::= { hprNceEntry 1 }

hprNceType OBJECT-TYPE
      SYNTAX HprNceTypes
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "A bit string identifying the function types provided by this
          Network Connection Endpoint (NCE)."

      ::= { hprNceEntry 2 }






hprNceDefault OBJECT-TYPE
      SYNTAX HprNceTypes
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "A bit string identifying the function types for which this
          Network Connection Endpoint (NCE) is the default NCE.  While
          default NCEs are not explicitly defined in the architecture,
          some implementations provide them; for such implementations,
          it is useful to make this information available to a
          Management Station."

      ::= { hprNceEntry 3 }

hprNceInstanceId   OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (4))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The NCE instance identifier (NCEII) identifying the current
          instance of this NCE.  An NCEII is used to denote different
          instances (IPLs) of an NCE component.  Each time an NCE is
          activated (IPL'd), it acquires a different, unique NCEII."

      ::= { hprNceEntry 4 }

-- *********************************************************************
hprRtp               OBJECT IDENTIFIER ::= { hprObjects 4 }
-- *********************************************************************
-- *********************************************************************
--
-- The RTP group is implemented by all managed nodes supporting the
-- HPR Transport Tower.  The group contains several scalars (simple
-- objects) and a table.
-- *********************************************************************

-- *********************************************************************
hprRtpGlobe          OBJECT IDENTIFIER ::= { hprRtp 1}
-- *********************************************************************
hprRtpGlobeConnSetups  OBJECT-TYPE
      SYNTAX Counter32
      UNITS "RTP connection setups"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of RTP connection setups in which this node has
          participated, as either sender or receiver, since it was last
          re-initialized.  Retries of a setup attempt do not cause the





          counter to be incremented.

          A Management Station can detect discontinuities in this
          counter by monitoring the appnNodeCounterDisconTime object
          in the APPN MIB."

      ::= { hprRtpGlobe 1 }

hprRtpGlobeCtrState OBJECT-TYPE
      SYNTAX INTEGER {
                      notActive(1),
                      active(2)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "This object allows a network management station to turn the
          counters in the hprRtpTable on and off.  The initial value of
          this object is an implementation choice.

                 notActive(1) - the counters in the hprRtpTable are
                                returning no meaningful values
                 active(2)    - the counters in the hprRtpTable are
                                being incremented and are returning
                                meaningful values"

      ::= { hprRtpGlobe 2 }

hprRtpGlobeCtrStateTime OBJECT-TYPE
      SYNTAX DateAndTime
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The time when the value of the hprRtpGlobeCtrState object
          last changed.  The initial value returned by this object is
          the time at which the APPN node instrumented with this MIB
          was last brought up."

      ::= { hprRtpGlobe 3 }

-- *********************************************************************
-- The RTP Connection Table
-- There may be many RTP connections on a node supporting the functions
-- specified in the RTP option set.  Each node implementing this option
-- set shall maintain a table of these RTP connections.
-- *********************************************************************

hprRtpTable OBJECT-TYPE





      SYNTAX SEQUENCE OF HprRtpEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The RTP Connection table"

      ::= { hprRtp 2 }

hprRtpEntry OBJECT-TYPE
      SYNTAX HprRtpEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The local NCE ID and local TCID are used to index this
          table."

      INDEX
             { hprRtpLocNceId,
               hprRtpLocTcid }

      ::= { hprRtpTable 1 }

HprRtpEntry ::= SEQUENCE {
     hprRtpLocNceId          OCTET STRING,       -- local nce id
     hprRtpLocTcid           OCTET STRING,       -- local tcid
     hprRtpRemCpName         SnaControlPointName,-- remote cp name
     hprRtpRemNceId          OCTET STRING,       -- remote nce id
     hprRtpRemTcid           OCTET STRING,       -- remote tcid
     hprRtpPathSwitchTrigger INTEGER,            -- trigger (read-write)
     hprRtpRscv              OCTET STRING,       -- rscv
     hprRtpTopic             DisplayString,      -- topic (cos)
     hprRtpState             INTEGER,            -- state
     hprRtpUpTime            TimeTicks,          -- up time

     hprRtpLivenessTimer     Unsigned32,         -- liveness timer
     hprRtpShortReqTimer     Unsigned32,         -- short request timer
     hprRtpPathSwTimer       Unsigned32,         -- path switch timer
     hprRtpLivenessTimeouts  HprRtpCounter,      -- liveness timeouts
     hprRtpShortReqTimeouts  HprRtpCounter,      -- short req timeouts

     hprRtpMaxSendRate       Gauge32,            -- maximum send rate
     hprRtpMinSendRate       Gauge32,            -- minimum send rate
     hprRtpCurSendRate       Gauge32,            -- current send rate

     hprRtpSmRdTripDelay     Gauge32,            -- smooth rnd trip
                                                    delay

     hprRtpSendPackets       HprRtpCounter,      -- packets sent





     hprRtpRecvPackets       HprRtpCounter,      -- packets received
     hprRtpSendBytes         HprRtpCounter,      -- bytes sent
     hprRtpRecvBytes         HprRtpCounter,      -- bytes received

     hprRtpRetrPackets       HprRtpCounter,      -- pkts re-xmitted
     hprRtpPacketsDiscarded  HprRtpCounter,      -- pkts discarded
     hprRtpDetectGaps        HprRtpCounter,      -- gaps detected
     hprRtpRateReqSends      HprRtpCounter,      -- rate req send

     hprRtpOkErrPathSws      HprRtpCounter,      -- ok  err path sws
     hprRtpBadErrPathSws     HprRtpCounter,      -- bad err path sws
     hprRtpOkOpPathSws       HprRtpCounter,      -- ok  op  path sws
     hprRtpBadOpPathSws      HprRtpCounter,      -- bad op  path sws

     hprRtpCounterDisconTime TimeStamp           -- discontinuity ind
        }

hprRtpLocNceId OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (1..8))
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The local Network Connection Endpoint (NCE) ID of this RTP
          connection.  NCEs identify CPs, LUs, Boundary Functions (BFs),
          and Route Setup (RS) components.  A value for this object can
          be retrieved from any of the following objects in the APPN
          MIB:

               - appnLsCpCpNceId
               - appnLsRouteNceId
               - appnLsBfNceId
               - appnIsInRtpNceId
               - appnIsRtpNceId

          In each case this value identifies a row in this table
          containing information related to that in the APPN MIB."

      ::= { hprRtpEntry 1 }

hprRtpLocTcid OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (8))
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The local TCID of this RTP connection.  A value for this
          object can be retrieved from either the appnIsInRtpTcid object
          or the appnIsRtpTcid object the APPN MIB; in each case this
          value identifies a row in this table containing information





          related to that in the APPN MIB."

      ::= { hprRtpEntry 2 }

hprRtpRemCpName OBJECT-TYPE
      SYNTAX SnaControlPointName
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "Administratively assigned network name for the remote node of
          this RTP connection."

      ::= { hprRtpEntry 3 }

hprRtpRemNceId OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (1..8))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The remote Network Connection Endpoint (NCE) of this RTP
          connection.  NCEs identify CPs, LUs, Boundary Functions (BFs),
          and Route Setup (RS) components."

      ::= { hprRtpEntry 4 }

hprRtpRemTcid OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (8))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The remote TCID of this RTP connection."

      ::= { hprRtpEntry 5 }

hprRtpPathSwitchTrigger OBJECT-TYPE
      SYNTAX INTEGER {
                      ready(1),
                      switchPathNow(2)
                     }
      MAX-ACCESS read-write
      STATUS current
      DESCRIPTION
          "Object by which a Management Station can trigger an operator-
          requested path switch, by setting the value to
          switchPathNow(2).  Setting this object to switchPathNow(2)
          triggers a path switch even if its previous value was already
          switchPathNow(2).






          The value ready(1) is returned on GET operations until a SET
          has been processed; after that the value received on the most
          recent SET is returned.

          This MIB module provides no support for an operator-requested
          switch to a specified path."

      ::= { hprRtpEntry 6 }

hprRtpRscv OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (0..255))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The forward Route Selection Control Vector for this RTP
          connection.  The format of this vector is described in SNA
          Formats.

          The value returned in this object during a path switch is
          implementation-dependent:  it may be the old path, the new
          path, a zero-length string, or some other valid RSCV string."

      ::= { hprRtpEntry 7 }

hprRtpTopic OBJECT-TYPE
      SYNTAX DisplayString (SIZE(8))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The topic for this RTP connection.  This is used to indicate
          the Class of Service."

      ::= { hprRtpEntry 8 }

hprRtpState OBJECT-TYPE
      SYNTAX INTEGER {
                      rtpListening(1),
                      rtpCalling(2),
                      rtpConnected(3),
                      rtpPathSwitching(4),
                      rtpDisconnecting(5),
                      other(99)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The state of the RTP connection, from the perspective of the
          local RTP protocol machine:





              rtpListening      - connection open; waiting for other end
                                  to call in
              rtpCalling        - connection opened, attempting to call
                                  out, have not yet received any data
                                  from other end
              rtpConnected      - connection is active; responded to a
                                  call-in or received other end's TCID
                                  from a call-out attempt
              rtpPathSwitching  - the path switch timer is running;
                                  attempting to find a new path for this
                                  connection.
              rtpDisconnecting  - no sessions are using this connection;
                                  in process of bringing it down
              other             - the connection is not in any of the
                                  states listed above."

      ::= { hprRtpEntry 9 }

hprRtpUpTime OBJECT-TYPE
      SYNTAX TimeTicks
      UNITS "1/100ths of a second"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The length of time the RTP connection has been up, measured
          in 1/100ths of a second."

      ::= { hprRtpEntry 10 }

hprRtpLivenessTimer OBJECT-TYPE
      SYNTAX Unsigned32
      UNITS "1/100ths of a second"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The value of the liveness (ALIVE) timer of this RTP
          connection, in units of 1/100th of a second.  When this timer
          expires and no packet has arrived from the partner since it
          was last set, packets with Status Request indicators will be
          sent to see if the RTP connection is still alive."

      ::= { hprRtpEntry 11 }

hprRtpShortReqTimer  OBJECT-TYPE
      SYNTAX Unsigned32
      UNITS "1/100ths of a second"
      MAX-ACCESS read-only
      STATUS current





      DESCRIPTION
          "The value of the RTP SHORT_REQ timer, in units of 1/100 of a
          second.  This timer represents the maximum time that a sender
          waits for a reply from a receiver."

      ::= { hprRtpEntry 12 }

hprRtpPathSwTimer OBJECT-TYPE
      SYNTAX Unsigned32
      UNITS "1/100ths of a second"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The length of time that RTP should attempt a path switch
          for a connection, in units of 1/100th of a second."

      ::= { hprRtpEntry 13 }

hprRtpLivenessTimeouts OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "liveness timeouts"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of liveness timeouts for this RTP connection."

      ::= { hprRtpEntry 14 }

hprRtpShortReqTimeouts OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "short request timeouts"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of short request timeouts for this RTP connection."

      ::= { hprRtpEntry 15 }

hprRtpMaxSendRate OBJECT-TYPE
      SYNTAX Gauge32
      UNITS "bytes per second"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The high-water mark for this RTP connection's send rate, in
          units of bytes per second.  This is the high-water mark for
          the entire life of the connection, not just the high-water
          mark for the connection's current path.





          For more details on this and other parameters related to HPR,
          see the High Performance Routing Architecture Reference."

      ::= { hprRtpEntry 16 }

hprRtpMinSendRate OBJECT-TYPE
      SYNTAX Gauge32
      UNITS "bytes per second"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The low-water mark for this RTP connection's send rate, in
          units of bytes per second.  This is the low-water mark for the
          entire life of the connection, not just the low-water mark for
          the connection's current path.

          For more details on this and other parameters related to HPR,
          see the High Performance Routing Architecture Reference."

      ::= { hprRtpEntry 17 }

hprRtpCurSendRate OBJECT-TYPE
      SYNTAX Gauge32
      UNITS "bytes per second"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The current send rate for this RTP connection, in units of
          bytes per second.

          For more details on this and other parameters related to HPR,
          see the High Performance Routing Architecture Reference."

      ::= { hprRtpEntry 18 }

hprRtpSmRdTripDelay OBJECT-TYPE
      SYNTAX Gauge32
      UNITS "1/1000ths of a second"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The smoothed round trip delay for this RTP connection, in
          units of 1/1000th of a second (ms).

          For more details on this and other parameters related to HPR,
          see the High Performance Routing Architecture Reference."

      ::= { hprRtpEntry 19 }





hprRtpSendPackets OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "RTP packets"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of packets successfully sent on this RTP
          connection."

      ::= { hprRtpEntry 20 }

hprRtpRecvPackets OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "RTP packets"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of packets received on this RTP connection.  The
          counter is incremented only once if duplicate copies of a
          packet are received."

      ::= { hprRtpEntry 21 }

hprRtpSendBytes OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "bytes"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of bytes sent on this RTP connection.  Both RTP
          Transport Header (THDR) bytes and data bytes are included in
          this count."

      ::= { hprRtpEntry 22 }

hprRtpRecvBytes OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "bytes"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of bytes received on this RTP connection.  Both RTP
          Transport Header (THDR) bytes and data bytes are included in
          this count."

      ::= { hprRtpEntry 23 }

hprRtpRetrPackets OBJECT-TYPE





      SYNTAX HprRtpCounter
      UNITS "RTP packets"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of packets retransmitted on this RTP connection."

      ::= { hprRtpEntry 24 }

hprRtpPacketsDiscarded OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "RTP packets"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of packets received on this RTP connection and then
          discarded.  A packet may be discarded because it is determined
          to be a duplicate, or for other reasons."

      ::= { hprRtpEntry 25 }

hprRtpDetectGaps OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "gaps"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of gaps detected on this RTP connection."

      ::= { hprRtpEntry 26 }

hprRtpRateReqSends OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "rate requests"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of Rate Requests sent on this RTP connection."

      ::= { hprRtpEntry 27 }

hprRtpOkErrPathSws OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "path switch attempts"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of successful path switch attempts for this RTP





          connection due to errors."

      ::= { hprRtpEntry 28 }

hprRtpBadErrPathSws OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "path switch attempts"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of unsuccessful path switches for this RTP
          connection due to errors."

      ::= { hprRtpEntry 29 }

hprRtpOkOpPathSws OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "path switches"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of successful path switches for this RTP connection
          due to operator requests."

      ::= { hprRtpEntry 30 }

hprRtpBadOpPathSws OBJECT-TYPE
      SYNTAX HprRtpCounter
      UNITS "path switches"
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The count of unsuccessful path switches for this RTP
          connection due to operator requests.  This counter is not
          incremented by an implementation that does not support
          operator-requested path switches, even if a Management Station
          requests such a path switch by setting the
          hprRtpPathSwitchTrigger object."

      ::= { hprRtpEntry 31 }

hprRtpCounterDisconTime OBJECT-TYPE
      SYNTAX TimeStamp
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The value of the sysUpTime object when the counters for this
          RTP connection last experienced a discontinuity.  This will be





          the more recent of two times:  the time at which the
          connection was established or the time at which the HPR
          counters were last turned on or off."

      ::= { hprRtpEntry 32 }

-- *********************************************************************
-- The RTP Connection Status Table
--  This table contains statistics and historical information related to
--  both successful and unsuccessful RTP path switches.  This
--  information can be important for both trend analysis and problem
--  determination.
--
--  Note the terminology here:  when RTP is triggered to find a new path
--  for a connection, this initiates a 'path switch,' which will end up
--  being either successful or unsuccessful.  During this path switch,
--  RTP will make one or more 'path switch attempts,' which are attempts
--  to find a new path for the connection and switch the connection to
--  it.  This 'new' path may be the same path that the connection was
--  using before the path switch.
--
--  It is an implementation option how many entries to keep in this
--  table, and how long to retain any individual entry.
-- *********************************************************************
hprRtpStatusTable OBJECT-TYPE
      SYNTAX SEQUENCE OF HprRtpStatusEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "RTP Connection Status Table:  This table contains historical
          information on RTP connections.  An entry is created in this
          table when a path switch is completed, either successfully or
          unsuccessfully."

      ::= { hprRtp 3 }

hprRtpStatusEntry OBJECT-TYPE
      SYNTAX HprRtpStatusEntry
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "This table is indexed by local NCE ID, local TCID, and an
          integer hprRtpStatusIndex.  Thus the primary grouping of table
          rows is by RTP connection, with the multiple entries for a
          given RTP connection ordered by time."

      INDEX
             { hprRtpStatusLocNceId,





               hprRtpStatusLocTcid,
               hprRtpStatusIndex }

      ::= { hprRtpStatusTable 1 }

  HprRtpStatusEntry ::= SEQUENCE {
     hprRtpStatusLocNceId          OCTET STRING, -- local nce id
     hprRtpStatusLocTcid           OCTET STRING, -- local tcid
     hprRtpStatusIndex             Unsigned32,   -- index
     hprRtpStatusStartTime         DateAndTime,  -- time stamp
     hprRtpStatusEndTime           DateAndTime,  -- time stamp
     hprRtpStatusRemCpName         SnaControlPointName,-- remote cp name
     hprRtpStatusRemNceId          OCTET STRING, -- remote nce id
     hprRtpStatusRemTcid           OCTET STRING, -- remote tcid
     hprRtpStatusNewRscv           OCTET STRING, -- new rscv
     hprRtpStatusOldRscv           OCTET STRING, -- old rscv
     hprRtpStatusCause             INTEGER,      -- cause
     hprRtpStatusLastAttemptResult INTEGER       -- result of last
                                          }

hprRtpStatusLocNceId OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (1..8))
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The local Network Connection Endpoint (NCE) of this RTP
          connection.  NCEs identify CPs, LUs, Boundary Functions (BFs),
          and Route Setup (RS) components."

      ::= { hprRtpStatusEntry 1 }

hprRtpStatusLocTcid OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (8))
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "The local TCID of this RTP connection."

      ::= { hprRtpStatusEntry 2 }

hprRtpStatusIndex OBJECT-TYPE
      SYNTAX Unsigned32 (1..4294967295)
      MAX-ACCESS not-accessible
      STATUS current
      DESCRIPTION
          "Table index.  This value begins at one and is incremented
          when a new entry is added to the table.  It is an
          implementation choice whether to run a single counter for





          all entries in the table, or to run a separate counter for
          the entries for each RTP connection.  In the unlikely event
          of a wrap, it is assumed that Management Stations will have
          the ability to order table entries correctly."

      ::= { hprRtpStatusEntry 3 }

hprRtpStatusStartTime OBJECT-TYPE
      SYNTAX DateAndTime
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The time when the path switch began."

      ::= { hprRtpStatusEntry 4 }

hprRtpStatusEndTime OBJECT-TYPE
      SYNTAX DateAndTime
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The time when the path switch was ended, either successfully
          or unsuccessfully."

      ::= { hprRtpStatusEntry 5 }

hprRtpStatusRemCpName OBJECT-TYPE
      SYNTAX SnaControlPointName
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "Administratively assigned network name for the remote node of
          this RTP connection."

      ::= { hprRtpStatusEntry 6 }

hprRtpStatusRemNceId OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (1..8))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The remote Network Connection Endpoint (NCE) of this RTP
          connection.  NCEs identify CPs, LUs, Boundary Functions (BFs),
          and Route Setup (RS) components."

      ::= { hprRtpStatusEntry 7 }

hprRtpStatusRemTcid OBJECT-TYPE





      SYNTAX OCTET STRING (SIZE (8))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The remote TCID of this RTP connection."

      ::= { hprRtpStatusEntry 8 }

hprRtpStatusNewRscv OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (0..255))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The new Route Selection Control Vector for this RTP
          connection.  A zero-length string indicates that no value is
          available, perhaps because the implementation does not save
          RSCVs."

      ::= { hprRtpStatusEntry 9 }

hprRtpStatusOldRscv OBJECT-TYPE
      SYNTAX OCTET STRING (SIZE (0..255))
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The old Route Selection Control Vector for this RTP
          connection.  A zero-length string indicates that no value is
          available, perhaps because the implementation does not save
          RSCVs."

      ::= { hprRtpStatusEntry 10 }

hprRtpStatusCause OBJECT-TYPE
      SYNTAX INTEGER {
                      other(1),
                      rtpConnFail(2),
                      locLinkFail(3),
                      remLinkFail(4),
                      operRequest(5)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The reason for the path switch:

               other(1)       - Reason other than those listed below,
               rtpConnFail(2) - RTP connection failure detected,
               locLinkFail(3) - Local link failure,





               remLinkFail(4) - Remote link failure (learned from TDUs),
               operRequest(5) - Operator requested path switch. "

      ::= { hprRtpStatusEntry 11 }

hprRtpStatusLastAttemptResult  OBJECT-TYPE
      SYNTAX INTEGER { successful(1),
                       initiatorMoving(2),
                       directorySearchFailed(3),
                       rscvCalculationFailed(4),
                       negativeRouteSetupReply(5),
                       backoutRouteSetupReply(6),
                       timeoutDuringFirstAttempt(7),
                       otherUnsuccessful(8)
                     }
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
          "The result of the last completed path switch attempt.  If the
          path switch is aborted in the middle of a path switch attempt
          because the path switch timer expires, the result of the
          previous path switch attempt is reported.

          The values are defined as follows:

             successful(1)                - The final path switch
                                            attempt was successful.
             initiatorMoving(2)           - The final path switch
                                            attempt failed because the
                                            initiator is mobile, and
                                            there was no active link
                                            out of this node.
             directorySearchFailed(3)     - The final path switch
                                            attempt failed because a
                                            directory search for the
                                            destination node's CP name
                                            failed.
             rscvCalculationFailed(4)     - The final path switch
                                            attempt failed because an
                                            RSCV to the node containing
                                            the remote RTP endpoint
                                            could not be calculated.
             negativeRouteSetupReply(5)   - The final path switch
                                            attempt failed because route
                                            setup failed for the new
                                            path.
             backoutRouteSetupReply(6)    - The final path switch
                                            attempt failed because the





                                            remote RTP endpoint refused
                                            to continue the RTP
                                            connection.
             timeoutDuringFirstAttempt(7) - The path switch timer
                                            expired during the first
                                            path switch attempt.
             otherUnsuccessful(8)         - The final path switch
                                            attempt failed for a reason
                                            other than those listed
                                            above."


      ::= { hprRtpStatusEntry 12 }


-- ***************************************************************
-- Conformance information
-- ***************************************************************

hprConformance       OBJECT IDENTIFIER ::= { hprMIB 2 }

hprCompliances       OBJECT IDENTIFIER ::= { hprConformance 1 }
hprGroups            OBJECT IDENTIFIER ::= { hprConformance 2 }

-- Compliance statements

hprCompliance  MODULE-COMPLIANCE
      STATUS  current
      DESCRIPTION
          "The compliance statement for the SNMPv2 entities that
          implement the HPR MIB."

      MODULE  -- this module

--    Unconditionally mandatory groups
          MANDATORY-GROUPS  {
                             hprGlobalConfGroup,
                             hprAnrRoutingConfGroup,
                             hprTransportUserConfGroup
                            }

--    Conditionally mandatory groups
          GROUP   hprRtpConfGroup
          DESCRIPTION
              "The hprRtpConfGroup is mandatory for HPR implementations
              supporting the HPR transport tower."

      ::= { hprCompliances 1 }





-- Units of conformance
hprGlobalConfGroup OBJECT-GROUP
        OBJECTS {
                 hprNodeCpName,
                 hprOperatorPathSwitchSupport
                }
      STATUS  current
      DESCRIPTION
          "A collection of objects providing the instrumentation of HPR
          general information and capabilities."

      ::= { hprGroups 1 }

hprAnrRoutingConfGroup OBJECT-GROUP
        OBJECTS {
                 hprAnrsAssigned,
                 hprAnrCounterState,
                 hprAnrCounterStateTime,
                 hprAnrType,
                 hprAnrOutTgDest,
                 hprAnrOutTgNum,
                 hprAnrPacketsReceived,
                 hprAnrCounterDisconTime
                }
      STATUS  current
      DESCRIPTION
          "A collection of objects providing instrumentation for the
          node's ANR routing."

      ::= { hprGroups 2 }

hprTransportUserConfGroup OBJECT-GROUP
        OBJECTS {
                 hprNceType,
                 hprNceDefault,
                 hprNceInstanceId
                }
      STATUS  current
      DESCRIPTION
          "A collection of objects providing information on the users of
          the HPR transport known to the node."

      ::= { hprGroups 3 }

hprRtpConfGroup  OBJECT-GROUP
        OBJECTS {
                 hprRtpGlobeConnSetups,
                 hprRtpGlobeCtrState,





                 hprRtpGlobeCtrStateTime,
                 hprRtpRemCpName,
                 hprRtpRemNceId,
                 hprRtpRemTcid,
                 hprRtpPathSwitchTrigger,
                 hprRtpRscv,
                 hprRtpTopic,
                 hprRtpState,
                 hprRtpUpTime,
                 hprRtpLivenessTimer,
                 hprRtpShortReqTimer,
                 hprRtpPathSwTimer,
                 hprRtpLivenessTimeouts,
                 hprRtpShortReqTimeouts,

                 hprRtpMaxSendRate,
                 hprRtpMinSendRate,
                 hprRtpCurSendRate,

                 hprRtpSmRdTripDelay,

                 hprRtpSendPackets,
                 hprRtpRecvPackets,
                 hprRtpSendBytes,
                 hprRtpRecvBytes,

                 hprRtpRetrPackets,
                 hprRtpPacketsDiscarded,
                 hprRtpDetectGaps,
                 hprRtpRateReqSends,

                 hprRtpOkErrPathSws,
                 hprRtpBadErrPathSws,
                 hprRtpOkOpPathSws,
                 hprRtpBadOpPathSws,
                 hprRtpCounterDisconTime,

                 hprRtpStatusStartTime,
                 hprRtpStatusEndTime,
                 hprRtpStatusRemNceId,
                 hprRtpStatusRemTcid,
                 hprRtpStatusRemCpName,
                 hprRtpStatusNewRscv,
                 hprRtpStatusOldRscv,
                 hprRtpStatusCause,
                 hprRtpStatusLastAttemptResult

                }





      STATUS  current
      DESCRIPTION
          "A collection of objects providing the instrumentation for RTP
          connection end points."

      ::= { hprGroups 4 }

-- end of conformance statement

END


