IANAPowerStateSet-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, mib-2     FROM SNMPv2-SMI
       TEXTUAL-CONVENTION         FROM SNMPv2-TC;

   ianaPowerStateSet MODULE-IDENTITY





       LAST-UPDATED "201502090000Z"    -- 9 February 2015
       ORGANIZATION "IANA"
       CONTACT-INFO "
                     Internet Assigned Numbers Authority
                     Postal: ICANN
                     12025 Waterfront Drive, Suite 300
                     Los Angeles, CA 90094
                     United States
                     Tel: +1-310-301 5800
                     EMail: iana@iana.org"

       DESCRIPTION
          "Copyright (c) 2015 IETF Trust and the persons identified as
           authors of the code.  All rights reserved.

           Redistribution and use in source and binary forms, with or
           without modification, is permitted pursuant to, and subject
           to the license terms contained in, the Simplified BSD License
           set forth in Section 4.c of the IETF Trust's Legal Provisions
           Relating to IETF Documents
           (http://trustee.ietf.org/license-info).

           This MIB module defines the PowerStateSet Textual
           Convention, which specifies the Power State Sets and
           Power State Set Values an Energy Object supports.

           The initial version of this MIB module was published in
           RFC 7460; for full legal notices see the RFC itself."

       -- revision history
       REVISION "201502090000Z"     -- 9 February 2015
       DESCRIPTION
           "Initial version of this MIB module, as published as RFC
           7460."

      ::= { mib-2 228 }

   PowerStateSet ::= TEXTUAL-CONVENTION
       STATUS current
       DESCRIPTION
           "IANAPowerState is a textual convention that describes
           Power State Sets and Power State Set Values an Energy
           Object supports.  IANA has created a registry of Power
           State supported by an Energy Object and IANA shall
           administer the list of Power State Sets and Power
           States.







           The Textual Convention assumes that Power States in a
           Power State Set are limited to 255 distinct values.  For
           a Power State Set S, the named number with the value S *
           256 is allocated to indicate the Power State Set.  For a
           Power State X in the Power State Set S, the named number
           with the value S * 256 + X + 1 is allocated to represent
           the Power State.

           Requests for new values should be made to IANA via email
           (iana@iana.org)."
       REFERENCE
          "http://www.iana.org/assignments/power-state-sets"

       SYNTAX      INTEGER {
           other(0),        -- indicates other set
           unknown(255),    -- unknown

           ieee1621(256),    -- indicates IEEE1621 set
           ieee1621Off(257),
           ieee1621Sleep(258),
           ieee1621On(259),

           dmtf(512),        -- indicates DMTF set
           dmtfOn(513),
           dmtfSleepLight(514),
           dmtfSleepDeep(515),
           dmtfOffHard(516),
           dmtfOffSoft(517),
           dmtfHibernate(518),
           dmtfPowerOffSoft(519),
           dmtfPowerOffHard(520),
           dmtfMasterBusReset(521),
           dmtfDiagnosticInterrapt(522),
           dmtfOffSoftGraceful(523),
           dmtfOffHardGraceful(524),
           dmtfMasterBusResetGraceful(525),
           dmtfPowerCycleOffSoftGraceful(526),
           dmtfPowerCycleHardGraceful(527),

           eman(1024),       -- indicates EMAN set
           emanMechOff(1025),
           emanSoftOff(1026),
           emanHibernate(1027),
           emanSleep(1028),
           emanStandby(1029),
           emanReady(1030),
           emanLowMinus(1031),
           emanLow(1032),





           emanMediumMinus(1033),
           emanMedium(1034),
           emanHighMinus(1035),
           emanHigh(1036)
                }
      END


