DS0-MIB DEFINITIONS ::= BEGIN


   IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE,
        transmission                     FROM SNMPv2-SMI
        MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF
        DisplayString, TruthValue        FROM SNMPv2-TC
        ifIndex, InterfaceIndex,
        InterfaceIndexOrZero             FROM IF-MIB;

   --  This is the MIB module for the DS0 Interface objects.

   ds0 MODULE-IDENTITY
       LAST-UPDATED "9807161630Z"
       ORGANIZATION "IETF Trunk MIB Working Group"
       CONTACT-INFO
         "        David Fowler

          Postal: Newbridge Networks Corporation
                  600 March Road
                  Kanata, Ontario, Canada K2K 2E6

                  Tel: +1 613 591 3600





                  Fax: +1 613 599 3619

          E-mail: davef@newbridge.com"
       DESCRIPTION
            "The MIB module to describe
             DS0 interfaces objects."
       REVISION "9805242010Z"
       DESCRIPTION
            "Initial version of the DS0-MIB."

       ::= { transmission 81 }

   -- The DS0 Config Group

   -- Implementation of this group is mandatory for all
   -- systems that use a DS0 Interface.

   -- The DS0 Config Group consists of two tables:
   --    DS0 Configuration Table
   --    DS0 Channel Mapping Table

   -- The DS0 Configuration Table

   dsx0ConfigTable OBJECT-TYPE
       SYNTAX  SEQUENCE OF Dsx0ConfigEntry
       MAX-ACCESS  not-accessible
       STATUS  current
       DESCRIPTION
               "The DS0 Configuration table."
       ::= { ds0 1 }

   dsx0ConfigEntry OBJECT-TYPE
       SYNTAX  Dsx0ConfigEntry
       MAX-ACCESS  not-accessible
       STATUS  current
       DESCRIPTION
               "An entry in the DS0 Configuration table.  There
               is an entry in this table for each DS0 interface."
       INDEX   { ifIndex }
       ::= { dsx0ConfigTable 1 }

   Dsx0ConfigEntry ::=
       SEQUENCE {
           dsx0Ds0ChannelNumber        INTEGER,
           dsx0RobbedBitSignalling     TruthValue,
           dsx0CircuitIdentifier       DisplayString,
           dsx0IdleCode                INTEGER,
           dsx0SeizedCode              INTEGER,





           dsx0ReceivedCode            INTEGER,
           dsx0TransmitCodesEnable     TruthValue,
           dsx0Ds0BundleMappedIfIndex  InterfaceIndexOrZero
   }

   dsx0Ds0ChannelNumber OBJECT-TYPE
       SYNTAX  INTEGER(0..31)
       MAX-ACCESS  read-only
       STATUS  current
       DESCRIPTION
               "This object indicates the channel number of the
               ds0 on its DS1/E1."
       ::= { dsx0ConfigEntry 1 }

   dsx0RobbedBitSignalling OBJECT-TYPE
       SYNTAX  TruthValue
       MAX-ACCESS  read-write
       STATUS  current
       DESCRIPTION
               "This object indicates if Robbed Bit Signalling is
               turned on or off for a given ds0.  This only
               applies to DS0s on a DS1 link.  For E1 links the
               value is always off (false)."
       ::= { dsx0ConfigEntry 2 }

   dsx0CircuitIdentifier OBJECT-TYPE
        SYNTAX  DisplayString (SIZE (0..255))
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This object contains the transmission vendor's
               circuit identifier, for the purpose of
               facilitating troubleshooting."
       ::= { dsx0ConfigEntry 3 }

   dsx0IdleCode OBJECT-TYPE
        SYNTAX  INTEGER(0..15)
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This object contains the code transmitted in the
               ABCD bits when the ds0 is not connected and
               dsx0TransmitCodesEnable is enabled.  The object is
               a bitmap and the various bit positions are:
                     1     D bit
                     2     C bit
                     4     B bit
                     8     A bit"





       ::= { dsx0ConfigEntry 4 }

   dsx0SeizedCode OBJECT-TYPE
        SYNTAX  INTEGER(0..15)
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This object contains the code transmitted in the
               ABCD bits when the ds0 is connected and
               dsx0TransmitCodesEnable is enabled.  The object is
               a bitmap and the various bit positions are:
                     1     D bit
                     2     C bit
                     4     B bit
                     8     A bit"
       ::= { dsx0ConfigEntry 5 }

   dsx0ReceivedCode OBJECT-TYPE
        SYNTAX  INTEGER(0..15)
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "This object contains the code being received in
               the ABCD bits.  The object is a bitmap and the
               various bit positions are:
                     1     D bit
                     2     C bit
                     4     B bit
                     8     A bit"
       ::= { dsx0ConfigEntry 6 }

   dsx0TransmitCodesEnable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS  read-write
        STATUS  current
        DESCRIPTION
               "This object determines if the idle and seized
               codes are transmitted. If the value of this object
               is true then the codes are transmitted."
       ::= { dsx0ConfigEntry 7 }

   dsx0Ds0BundleMappedIfIndex OBJECT-TYPE
        SYNTAX InterfaceIndexOrZero
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "This object indicates the ifIndex value assigned
               by the agent for the ds0Bundle(82) ifEntry to





               which the given ds0(81) ifEntry may belong.

               If the given ds0(81) ifEntry does not belong to
               any ds0Bundle(82) ifEntry, then this object has a
               value of zero.

               While this object provides information that can
               also be found in the ifStackTable, it provides
               this same information with a single table lookup,
               rather than by walking the ifStackTable to find
               the possibly non-existent ds0Bundle(82) ifEntry
               that may be stacked above the given ds0(81)
               ifTable entry."
       ::= { dsx0ConfigEntry 8 }

   -- The DS0 Channel Mapping Table

   dsx0ChanMappingTable OBJECT-TYPE
        SYNTAX  SEQUENCE OF Dsx0ChanMappingEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "The DS0 Channel Mapping table.  This table maps a
               DS0 channel number on a particular DS1/E1 into an
               ifIndex."
        ::= { ds0 3 }

   dsx0ChanMappingEntry OBJECT-TYPE
        SYNTAX  Dsx0ChanMappingEntry
        MAX-ACCESS  not-accessible
        STATUS  current
        DESCRIPTION
               "An entry in the DS0 Channel Mapping table.  There
               is an entry in this table corresponding to each
               ds0 ifEntry within any interface that is
               channelized to the individual ds0 ifEntry level.

               This table is intended to facilitate mapping from
               channelized interface / channel number to DS0
               ifEntry.  (e.g. mapping (DS1 ifIndex, DS0 Channel
               Number) -> ifIndex)

               While this table provides information that can
               also be found in the ifStackTable and
               dsx0ConfigTable, it provides this same information
               with a single table lookup, rather than by walking
               the ifStackTable to find the various constituent
               ds0 ifTable entries, and testing various





               dsx0ConfigTable entries to check for the entry
               with the applicable DS0 channel number."
        INDEX   { ifIndex, dsx0Ds0ChannelNumber }
        ::= { dsx0ChanMappingTable 1 }

   Dsx0ChanMappingEntry ::=
        SEQUENCE {
            dsx0ChanMappedIfIndex  InterfaceIndex
   }

   dsx0ChanMappedIfIndex OBJECT-TYPE
        SYNTAX  InterfaceIndex
        MAX-ACCESS  read-only
        STATUS  current
        DESCRIPTION
               "This object indicates the ifIndex value assigned
               by the agent for the individual ds0 ifEntry that
               corresponds to the given DS0 channel number
               (specified by the INDEX element
               dsx0Ds0ChannelNumber) of the given channelized
               interface (specified by INDEX element ifIndex)."
        ::= { dsx0ChanMappingEntry 1 }

   -- conformance information

   ds0Conformance OBJECT IDENTIFIER ::= { ds0 2 }

   ds0Groups      OBJECT IDENTIFIER ::= { ds0Conformance 1 }
   ds0Compliances OBJECT IDENTIFIER ::= { ds0Conformance 2 }



   -- compliance statements

   ds0Compliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
               "The compliance statement for DS0 interfaces."
       MODULE  -- this module
           MANDATORY-GROUPS { ds0ConfigGroup }

           OBJECT dsx0RobbedBitSignalling
           MIN-ACCESS read-only
           DESCRIPTION
               "The ability to set RBS is not required."
           OBJECT dsx0CircuitIdentifier
           MIN-ACCESS read-only
           DESCRIPTION





               "The ability to set the circuit identifier is not
               required."

           OBJECT dsx0IdleCode
           MIN-ACCESS read-only
           DESCRIPTION
               "The ability to set the idle code is not
               required."

           OBJECT dsx0SeizedCode
           MIN-ACCESS read-only
           DESCRIPTION
               "The ability to set the seized code is not
               required."

           OBJECT dsx0TransmitCodesEnable
           MIN-ACCESS read-only
           DESCRIPTION
               "The ability to enable and disable the
               transmitting of idle and seized codes is not
               required."

       ::= { ds0Compliances 1 }

   -- units of conformance

   ds0ConfigGroup  OBJECT-GROUP
       OBJECTS { dsx0Ds0ChannelNumber,
                 dsx0RobbedBitSignalling,
                 dsx0CircuitIdentifier,
                 dsx0IdleCode,
                 dsx0SeizedCode,
                 dsx0ReceivedCode,
                 dsx0TransmitCodesEnable,
                 dsx0Ds0BundleMappedIfIndex,
                 dsx0ChanMappedIfIndex }
       STATUS  current
       DESCRIPTION
               "A collection of objects providing configuration
               information applicable to all DS0 interfaces."
       ::= { ds0Groups 1 }

   END









