EtherLike-MIB DEFINITIONS ::= BEGIN


      IMPORTS
          Counter, Gauge         FROM RFC1155-SMI
          ifIndex, transmission  FROM RFC1213-MIB
          OBJECT-TYPE            FROM RFC-1212;

       -- This MIB module uses the extended OBJECT-TYPE macro as
       -- defined in RFC-1212.

      dot3    OBJECT IDENTIFIER ::= { transmission 7 }

      -- the Ethernet-like Statistics group

       dot3StatsTable  OBJECT-TYPE
            SYNTAX     SEQUENCE OF Dot3StatsEntry
            ACCESS     not-accessible
            STATUS     mandatory
            DESCRIPTION
             "Statistics for a collection of ethernet-like
             interfaces attached to a particular system."
            ::= { dot3 2 }


       dot3StatsEntry   OBJECT-TYPE
            SYNTAX      Dot3StatsEntry
            ACCESS      not-accessible
            STATUS      mandatory
            DESCRIPTION
              "Statistics for a particular interface to an
              ethernet-like medium."
            INDEX     { dot3StatsIndex }
            ::= { dot3StatsTable 1 }





       Dot3StatsEntry ::= SEQUENCE {
            dot3StatsIndex                      INTEGER,
            dot3StatsAlignmentErrors            Counter,
            dot3StatsFCSErrors                  Counter,
            dot3StatsSingleCollisionFrames      Counter,
            dot3StatsMultipleCollisionFrames    Counter,
            dot3StatsSQETestErrors              Counter,
            dot3StatsDeferredTransmissions      Counter,
            dot3StatsLateCollisions             Counter,
            dot3StatsExcessiveCollisions        Counter,
            dot3StatsInternalMacTransmitErrors  Counter,
            dot3StatsCarrierSenseErrors         Counter,
            dot3StatsFrameTooLongs              Counter,
            dot3StatsInternalMacReceiveErrors   Counter,
            dot3StatsEtherChipSet               OBJECT IDENTIFIER
       }

       dot3StatsIndex   OBJECT-TYPE
            SYNTAX      INTEGER
            ACCESS      read-only
            STATUS      mandatory
            DESCRIPTION
              "An index value that uniquely identifies an
              interface to an ethernet-like medium.  The
              interface identified by a particular value of
              this index is the same interface as identified
              by the same value of ifIndex."
            ::= { dot3StatsEntry 1 }

       dot3StatsAlignmentErrors   OBJECT-TYPE
            SYNTAX     Counter
            ACCESS     read-only
            STATUS     mandatory
            DESCRIPTION
             "A count of frames received on a particular
             interface that are not an integral number of
             octets in length and do not pass the FCS check.

             The count represented by an instance of this
             object is incremented when the alignmentError
             status is returned by the MAC service to the
             LLC (or other MAC user). Received frames for
             which multiple error conditions obtain are,
             according to the conventions of IEEE 802.3
             Layer Management, counted exclusively according
             to the error status presented to the LLC."
            REFERENCE
            "IEEE 802.3 Layer Management"





            ::= { dot3StatsEntry 2 }

       dot3StatsFCSErrors   OBJECT-TYPE
            SYNTAX      Counter
            ACCESS      read-only
            STATUS      mandatory
            DESCRIPTION
            "A count of frames received on a particular
            interface that are an integral number of octets
            in length but do not pass the FCS check.

            The count represented by an instance of this
            object is incremented when the frameCheckError
            status is returned by the MAC service to the
            LLC (or other MAC user). Received frames for
            which multiple error conditions obtain are,
            according to the conventions of IEEE 802.3
            Layer Management, counted exclusively according
            to the error status presented to the LLC."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 3 }

       dot3StatsSingleCollisionFrames   OBJECT-TYPE
            SYNTAX      Counter
            ACCESS      read-only
            STATUS      mandatory
            DESCRIPTION
            "A count of successfully transmitted frames on
            a particular interface for which transmission
            is inhibited by exactly one collision.

            A frame that is counted by an instance of this
            object is also counted by the corresponding
            instance of either the ifOutUcastPkts,
            ifOutMulticastPkts, or ifOutBroadcastPkts,
            and is not counted by the corresponding
            instance of the dot3StatsMultipleCollisionFrames
            object."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 4 }

       dot3StatsMultipleCollisionFrames   OBJECT-TYPE
            SYNTAX      Counter
            ACCESS      read-only
            STATUS      mandatory
            DESCRIPTION





            "A count of successfully transmitted frames on
            a particular interface for which transmission
             is inhibited by more than one collision.

            A frame that is counted by an instance of this
            object is also counted by the corresponding
            instance of either the ifOutUcastPkts,
            ifOutMulticastPkts, or ifOutBroadcastPkts,
            and is not counted by the corresponding
            instance of the dot3StatsSingleCollisionFrames
            object."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 5 }

       dot3StatsSQETestErrors   OBJECT-TYPE
            SYNTAX     Counter
            ACCESS     read-only
            STATUS     mandatory
            DESCRIPTION
            "A count of times that the SQE TEST ERROR
            message is generated by the PLS sublayer for a
            particular interface. The SQE TEST ERROR
            message is defined in section 7.2.2.2.4 of
            ANSI/IEEE 802.3-1985 and its generation is
            described in section 7.2.4.6 of the same
            document."
            REFERENCE
            "ANSI/IEEE Std 802.3-1985 Carrier Sense
            Multiple Access with Collision Detection Access
            Method and Physical Layer Specifications"
            ::= { dot3StatsEntry 6 }

       dot3StatsDeferredTransmissions   OBJECT-TYPE
            SYNTAX      Counter
            ACCESS      read-only
            STATUS      mandatory
            DESCRIPTION
            "A count of frames for which the first
            transmission attempt on a particular interface
            is delayed because the medium is busy.

            The count represented by an instance of this
            object does not include frames involved in
            collisions."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 7 }





       dot3StatsLateCollisions   OBJECT-TYPE
            SYNTAX      Counter
            ACCESS      read-only
            STATUS      mandatory
            DESCRIPTION
            "The number of times that a collision is
            detected on a particular interface later than
            512 bit-times into the transmission of a
            packet.

            Five hundred and twelve bit-times corresponds
            to 51.2 microseconds on a 10 Mbit/s system. A
            (late) collision included in a count
            represented by an instance of this object is
            also considered as a (generic) collision for
            purposes of other collision-related
            statistics."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 8 }

       dot3StatsExcessiveCollisions   OBJECT-TYPE
            SYNTAX    Counter
            ACCESS    read-only
            STATUS    mandatory
            DESCRIPTION
            "A count of frames for which transmission on a
            particular interface fails due to excessive
            collisions."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 9 }


       dot3StatsInternalMacTransmitErrors   OBJECT-TYPE
            SYNTAX    Counter
            ACCESS    read-only
            STATUS    mandatory
            DESCRIPTION
            "A count of frames for which transmission on a
            particular interface fails due to an internal
            MAC sublayer transmit error. A frame is only
            counted by an instance of this object if it is
            not counted by the corresponding instance of
            either the dot3StatsLateCollisions object, the
            dot3StatsExcessiveCollisions object, or the
            dot3StatsCarrierSenseErrors object.






            The precise meaning of the count represented by
            an instance of this object is implementation-
            specific.  In particular, an instance of this
            object may represent a count of transmission
            errors on a particular interface that are not
            otherwise counted."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 10 }

       dot3StatsCarrierSenseErrors   OBJECT-TYPE
            SYNTAX    Counter
            ACCESS    read-only
            STATUS    mandatory
            DESCRIPTION
            "The number of times that the carrier sense
            condition was lost or never asserted when
            attempting to transmit a frame on a particular
            interface.

            The count represented by an instance of this
            object is incremented at most once per
            transmission attempt, even if the carrier sense
            condition fluctuates during a transmission
            attempt."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 11 }

       -- { dot3StatsEntry 12 } is not assigned

       dot3StatsFrameTooLongs   OBJECT-TYPE
            SYNTAX    Counter
            ACCESS    read-only
            STATUS    mandatory
            DESCRIPTION
            "A count of frames received on a particular
            interface that exceed the maximum permitted
            frame size.

            The count represented by an instance of this
            object is incremented when the frameTooLong
            status is returned by the MAC service to the
            LLC (or other MAC user). Received frames for
            which multiple error conditions obtain are,
            according to the conventions of IEEE 802.3
            Layer Management, counted exclusively according
            to the error status presented to the LLC."





            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 13 }

       -- { dot3StatsEntry 14 } is not assigned

       -- { dot3StatsEntry 15 } is not assigned

       dot3StatsInternalMacReceiveErrors   OBJECT-TYPE
            SYNTAX    Counter
            ACCESS    read-only
            STATUS    mandatory
            DESCRIPTION
            "A count of frames for which reception on a
            particular interface fails due to an internal
            MAC sublayer receive error. A frame is only
            counted by an instance of this object if it is
            not counted by the corresponding instance of
            either the dot3StatsFrameTooLongs object, the
            dot3StatsAlignmentErrors object, or the
            dot3StatsFCSErrors object.

            The precise meaning of the count represented by
            an instance of this object is implementation-
            specific.  In particular, an instance of this
            object may represent a count of receive errors
            on a particular interface that are not
            otherwise counted."
            REFERENCE
            "IEEE 802.3 Layer Management"
            ::= { dot3StatsEntry 16 }

       dot3StatsEtherChipSet   OBJECT-TYPE
            SYNTAX        OBJECT IDENTIFIER
            ACCESS        read-only
            STATUS        mandatory
            DESCRIPTION
            "This object contains an OBJECT IDENTIFIER
            which identifies the chipset used to
            realize the interface. Ethernet-like
            interfaces are typically built out of
            several different chips. The MIB implementor
            is presented with a decision of which chip
            to identify via this object. The implementor
            should identify the chip which is usually
            called the Medium Access Control chip.
            If no such chip is easily identifiable,
            the implementor should identify the chip





            which actually gathers the transmit
            and receive statistics and error
            indications. This would allow a
            manager station to correlate the
            statistics and the chip generating
            them, giving it the ability to take
            into account any known anomalies
            in the chip."
            ::= { dot3StatsEntry 17 }

       -- the Ethernet-like Collision Statistics group

       -- Implementation of this group is optional; it is appropriate
       -- for all systems which have the necessary metering

       dot3CollTable  OBJECT-TYPE
            SYNTAX    SEQUENCE OF Dot3CollEntry
            ACCESS    not-accessible
            STATUS    mandatory
            DESCRIPTION
            "A collection of collision histograms for a
            particular set of interfaces."
            ::= { dot3 5 }


       dot3CollEntry  OBJECT-TYPE
            SYNTAX    Dot3CollEntry
            ACCESS    not-accessible
            STATUS    mandatory
            DESCRIPTION
            "A cell in the histogram of per-frame
            collisions for a particular interface.  An
            instance of this object represents the
            frequency of individual MAC frames for which
            the transmission (successful or otherwise) on a
            particular interface is accompanied by a
            particular number of media collisions."
            INDEX     { ifIndex, dot3CollCount }
            ::= { dot3CollTable 1 }

       Dot3CollEntry ::= SEQUENCE {
            dot3CollCount        INTEGER,
            dot3CollFrequencies  Counter
       }

       -- { dot3CollEntry 1 } is no longer in use

       dot3CollCount  OBJECT-TYPE





            SYNTAX    INTEGER (1..16)
            ACCESS    not-accessible
            STATUS    mandatory
            DESCRIPTION
            "The number of per-frame media collisions for
            which a particular collision histogram cell
            represents the frequency on a particular
            interface."
            ::= { dot3CollEntry 2 }


       dot3CollFrequencies   OBJECT-TYPE
            SYNTAX    Counter
            ACCESS    read-only
            STATUS    mandatory
            DESCRIPTION
            "A count of individual MAC frames for which the
            transmission (successful or otherwise) on a
            particular interface occurs after the
            frame has experienced exactly the number
            of collisions in the associated
            dot3CollCount object.

            For example, a frame which is transmitted
            on interface 77 after experiencing
            exactly 4 collisions would be indicated
            by incrementing only dot3CollFrequencies.77.4.
            No other instance of dot3CollFrequencies would
            be incremented in this example."
            ::= { dot3CollEntry 3 }

       --  802.3 Tests

       dot3Tests   OBJECT IDENTIFIER ::= { dot3 6 }

       dot3Errors  OBJECT IDENTIFIER ::= { dot3 7 }


       --  TDR Test

       -- The Time-Domain Reflectometry (TDR) test is specific
       -- to ethernet-like interfaces with the exception of
       -- 10BaseT and 10BaseF. The TDR value may be useful
       -- in determining the approximate distance to a cable fault.
       -- It is advisable to repeat this test to check for a
       -- consistent resulting TDR value, to verify that there
       -- is a fault.






       dot3TestTdr OBJECT IDENTIFIER ::= { dot3Tests 1 }

       -- A TDR test returns as its result the time interval,
       -- measured in 10 MHz ticks or 100 nsec units, between
       -- the start of TDR test transmission and the subsequent
       -- detection of a collision or deassertion of carrier.  On
       -- successful completion of a TDR test, the result is
       -- stored as the value of the appropriate instance of the
       -- MIB object dot3TestTdrValue, and the OBJECT IDENTIFIER
       -- of that instanceis stored in the corresponding instance
       -- of ifExtnsTestCode (thereby indicating where the
       -- result has been stored).


       -- Loopback Test

       -- Another test is the full-duplex loopback test.
       -- This test configures the MAC chip and executes
       -- an internal loopback test of memory, data paths,
       -- and the MAC chip logic.  This loopback test can
       -- only be executed if the interface is offline.
       -- Once the test has completed, the MAC chip should
       -- be reinitialized for network operation, but it
       -- should remain offline.

       dot3TestLoopBack OBJECT IDENTIFIER ::= { dot3Tests 2 }

       -- If an error occurs during a test, the object
       -- ifTestResult (defined in RFC1573) will be set
       -- to failed(7).  The following two OBJECT
       -- IDENTIFIERs may be used to provided more
       -- information as values for ifTestCode.

                -- couldn't initialize MAC chip for test
       dot3ErrorInitError     OBJECT IDENTIFIER ::= { dot3Errors 1 }

                -- expected data not received (or not
                -- received correctly) in loopback test
       dot3ErrorLoopbackError OBJECT IDENTIFIER ::= { dot3Errors 2 }

       -- RFC1573 does away with the interface chipset object.
       -- The following OBJECT IDENTIFIER definitions are
       -- retained for purposes of backwards compatibility
       -- with pre-RFC1573 systems.
       --  802.3 Hardware Chipsets

       -- The object ifExtnsChipSet is provided in RFC1229 to
       -- identify the MAC hardware used to communcate on an





       -- interface.  The following hardware chipsets are
       -- provided for 802.3:

       dot3ChipSets          OBJECT IDENTIFIER ::= { dot3 8 }
       dot3ChipSetAMD        OBJECT IDENTIFIER ::= { dot3ChipSets 1 }
       dot3ChipSetAMD7990    OBJECT IDENTIFIER ::= { dot3ChipSetAMD 1 }
       dot3ChipSetAMD79900   OBJECT IDENTIFIER ::= { dot3ChipSetAMD 2 }
       dot3ChipSetAMD79C940  OBJECT IDENTIFIER ::= { dot3ChipSetAMD 3 }

       dot3ChipSetIntel      OBJECT IDENTIFIER ::= { dot3ChipSets 2 }
       dot3ChipSetIntel82586 OBJECT IDENTIFIER ::= { dot3ChipSetIntel 1 }
       dot3ChipSetIntel82596 OBJECT IDENTIFIER ::= { dot3ChipSetIntel 2 }

       dot3ChipSetSeeq       OBJECT IDENTIFIER ::= { dot3ChipSets 3 }
       dot3ChipSetSeeq8003   OBJECT IDENTIFIER ::= { dot3ChipSetSeeq 1 }

       dot3ChipSetNational      OBJECT IDENTIFIER ::= { dot3ChipSets 4 }
       dot3ChipSetNational8390  OBJECT IDENTIFIER ::=
                                  { dot3ChipSetNational 1 }
       dot3ChipSetNationalSonic OBJECT IDENTIFIER ::=
                                  { dot3ChipSetNational 2 }

       dot3ChipSetFujitsu       OBJECT IDENTIFIER ::= { dot3ChipSets 5 }
       dot3ChipSetFujitsu86950  OBJECT IDENTIFIER ::=
                                  { dot3ChipSetFujitsu 1 }

       dot3ChipSetDigital       OBJECT IDENTIFIER ::= { dot3ChipSets 6 }
       dot3ChipSetDigitalDC21040  OBJECT IDENTIFIER ::=
                                  { dot3ChipSetDigital 1 }

       -- For those chipsets not represented above, OBJECT IDENTIFIER
       -- assignment is required in other documentation, e.g., assignment
       -- within that part of the registration tree delegated to
       -- individual enterprises (see RFC1155).

   END


