FourBSD-ISODE   DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-CONFORMANCE
           FROM RFC-1303
       -- everything --
           FROM RFCxxxx-MIB
       -- everything --
           FROM RFC1213-MIB
       -- everything --
           FROM UNIX-MIB
       -- everything --
           FROM EVAL-MIB;

   fourBSD-isode-support MODULE-CONFORMANCE
       LAST-UPDATED        "9201252354Z"
       PRODUCT-RELEASE     "ISODE 7.0 + 'Secure' SNMP
                            upgrade for SunOS 4.1"
       DESCRIPTION         "4BSD/ISODE 'Secure' SNMP"

       SUPPORTS            RFCxxxx-MIB -- SNMP Party MIB --
           INCLUDES        { partyPublic, partyPrivate }

       SUPPORTS            RFC1213-MIB
           INCLUDES        { system, interfaces, at, ip, icmp,
                             tcp, udp, snmp }

           VARIATION       atEntry
               CREATION-REQUIRES { atPhysAddress }
               DESCRIPTION "Address mappings on 4BSD require
                            both protocol and media addresses"

           VARIATION       ifAdminStatus





               SYNTAX      INTEGER { up(1), down(2) }
               DESCRIPTION "Unable to set test mode on 4BSD"

           VARIATION       ifOperStatus
               SYNTAX      INTEGER { up(1), down(2) }
               DESCRIPTION "Information limited on 4BSD"

           VARIATION       ipDefaultTTL
               SYNTAX      INTEGER { maxttl(255) }
               DESCRIPTION "Hard-wired on 4BSD"

           VARIATION       ipInAddrErrors
               ACCESS      not-accessible
               DESCRIPTION "Information not available on 4BSD"

           VARIATION       ipInDiscards
               ACCESS      not-accessible
               DESCRIPTION "Information not available on 4BSD"

           VARIATION       ipRouteEntry
               CREATION-REQUIRES { ipRouteNextHop }
               DESCRIPTION "Routes on 4BSD require both
                            destination and next-hop"

           VARIATION       ipRouteType
               SYNTAX       INTEGER { direct(3), indirect(4) }
               WRITE-SYNTAX INTEGER { invalid(2), direct(3),
                                      indirect(4) }
               DESCRIPTION "Information limited on 4BSD"

           VARIATION       ipRouteProto
               SYNTAX      INTEGER { other(1), icmp (4) }
               DESCRIPTION "Information limited on 4BSD"

           VARIATION       ipRouteAge
               ACCESS      not-accessible
               DESCRIPTION "Information not available on 4BSD"

           VARIATION       ipNetToMediaEntry
               CREATION-REQUIRES { ipNetToMediaPhysAddress }
               DESCRIPTION "Address mappings on 4BSD require
                            both protocol and media addresses"

           VARIATION       ipNetToMediaType
               SYNTAX       INTEGER { dynamic(3), static(4) }
               WRITE-SYNTAX INTEGER { invalid(2), dynamic(3),
                                      static(4) }
               DESCRIPTION "Information limited on 4BSD"





           VARIATION       tcpConnState
               ACCESS      read-only
               DESCRIPTION "Unable to set this on 4BSD"

           VARIATION       tcpInErrs
               ACCESS      not-accessible
               DESCRIPTION "Information not available on 4BSD"

           VARIATION       tcpOutRsts
               ACCESS      not-accessible
               DESCRIPTION "Information not available on 4BSD"

       SUPPORTS            UNIX-MIB
           INCLUDES        { agents, mbuf, netstat }

       SUPPORTS            EVAL-MIB
           INCLUDES        { functions, expressions }

       ::= { fourBSD-isode 6 6 }

   END

   
