VDSL-LINE-EXT-MCM-MIB DEFINITIONS ::= BEGIN


   IMPORTS
   MODULE-IDENTITY,
   OBJECT-TYPE,
   transmission,
   Unsigned32                      FROM SNMPv2-SMI         -- [RFC2578]
   RowStatus                       FROM SNMPv2-TC          -- [RFC2579]
   MODULE-COMPLIANCE,
   OBJECT-GROUP                    FROM SNMPv2-CONF        -- [RFC2580]
   vdslLineConfProfileName         FROM VDSL-LINE-MIB;     -- [RFC3728]

   vdslExtMCMMIB MODULE-IDENTITY
      LAST-UPDATED "200504280000Z" --    April 28, 2005
      ORGANIZATION "ADSLMIB Working Group"
      CONTACT-INFO "WG-email:  adslmib@ietf.org
            Info:      https://www1.ietf.org/mailman/listinfo/adslmib

            Chair:     Mike Sneed
                       Sand Channel Systems
            Postal:    P.O. Box 37324
                       Raleigh NC 27627-732
            Email:     sneedmike@hotmail.com
            Phone:     +1 206 600 7022

            Co-Chair/Co-editor:
                       Bob Ray
                       PESA Switching Systems, Inc.
            Postal:    330-A Wynn Drive
                       Huntsville, AL 35805
                       USA
            Email:     rray@pesa.com
            Phone:     +1 256 726 9200 ext.  142






            Co-editor: Menachem Dodge
                       ECI Telecom Ltd.
            Postal:    30 hasivim St.
                       Petach Tikva 49517,
                       Israel.
            Email:     mbdodge@ieee.org
            Phone:     +972 3 926 8421
           "

   DESCRIPTION
       "The VDSL-LINE-MIB found in RFC 3728 defines objects for
       the management of a pair of VDSL transceivers at each end of
       the VDSL line.  The VDSL-LINE-MIB configures and monitors the
       line code independent parameters (TC layer) of the VDSL line.
       This MIB module is an optional extension of the VDSL-LINE-MIB
       and defines objects for configuration and monitoring of the
       line code specific (LCS) elements (PMD layer) for VDSL lines
       using MCM coding.  The objects in this extension MIB MUST NOT
       be used for VDSL lines using Single Carrier Modulation (SCM)
       line coding.  If an object in this extension MIB is referenced
       by a line which does not use MCM, it has no effect on the
       operation of that line.

       Naming Conventions:
           Vtuc -- (VTUC) transceiver at near (Central) end of line
           Vtur -- (VTUR) transceiver at Remote end of line
           Vtu  -- One of either Vtuc or Vtur
           Curr -- Current
           LCS  -- Line Code Specific
           Max  -- Maximum
           PSD  -- Power Spectral Density
           Rx   -- Receive
           Tx   -- Transmit

       Copyright (C) The Internet Society (2005).  This version
       of this MIB module is part of RFC 4070: see the RFC
       itself for full legal notices."
           REVISION "200504280000Z" --    April 28, 2005
           DESCRIPTION "Initial version, published as RFC 4070."
       ::= { transmission 229 }

   vdslLineExtMCMMib OBJECT IDENTIFIER ::= { vdslExtMCMMIB 1 }
   vdslLineExtMCMMibObjects OBJECT IDENTIFIER ::= {vdslLineExtMCMMib 1}

   --
   -- Multiple carrier modulation (MCM) configuration profile tables
   --






   vdslLineMCMConfProfileTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VdslLineMCMConfProfileEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "This table contains additional information on multiple
           carrier VDSL lines.  One entry in this table reflects a
           profile defined by a manager which can be used to
           configure the VDSL line.

           If an entry in this table is referenced by a line which
           does not use MCM, it has no effect on the operation of that
           line.

           All read-create-objects defined in this table SHOULD be
           stored persistently."

       ::= { vdslLineExtMCMMibObjects  1 }

   vdslLineMCMConfProfileEntry OBJECT-TYPE
       SYNTAX       VdslLineMCMConfProfileEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "Each entry consists of a list of parameters that
           represents the configuration of a multiple carrier
           modulation VDSL modem."
       INDEX { vdslLineConfProfileName }
       ::= { vdslLineMCMConfProfileTable 1 }

   VdslLineMCMConfProfileEntry ::=
       SEQUENCE
           {
           vdslLineMCMConfProfileTxWindowLength       Unsigned32,
           vdslLineMCMConfProfileRowStatus            RowStatus
           }

   vdslLineMCMConfProfileTxWindowLength OBJECT-TYPE
       SYNTAX       Unsigned32 (1..255)
       UNITS        "samples"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "Specifies the length of the transmit window, counted
           in samples at the sampling rate corresponding to the
           negotiated value of N."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileEntry 1 }





   vdslLineMCMConfProfileRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "This object is used to create a new row or modify or
           delete an existing row in this table.

           A profile is activated by setting this object to `active'.
           When `active' is set, the system will validate the profile.

           None of the columns in this row may be modified while the
           row is in the 'active' state.

           Before a profile can be deleted or taken out of
           service, (by setting this object to `destroy' or
           `notInService') it must first be unreferenced
           from all associated lines."
       ::= { vdslLineMCMConfProfileEntry 2 }

   vdslLineMCMConfProfileTxBandTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VdslLineMCMConfProfileTxBandEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "This table contains transmit band descriptor configuration
           information for a VDSL line.  Each entry in this table
           reflects the configuration for one of possibly many bands
           with a multiple carrier modulation (MCM) VDSL line.
           These entries are defined by a manager and can be used to
           configure the VDSL line.

           If an entry in this table is referenced by a line which
           does not use MCM, it has no effect on the operation of that
           line.

           All read-create-objects defined in this table SHOULD be
           stored persistently."
       ::= { vdslLineExtMCMMibObjects  2 }

   vdslLineMCMConfProfileTxBandEntry OBJECT-TYPE
       SYNTAX       VdslLineMCMConfProfileTxBandEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "Each entry consists of a transmit band descriptor, which
           is defined by a start and a stop tone index."
       INDEX { vdslLineConfProfileName,





               vdslLineMCMConfProfileTxBandNumber }
       ::= { vdslLineMCMConfProfileTxBandTable 1 }

   VdslLineMCMConfProfileTxBandEntry ::=
       SEQUENCE
           {
           vdslLineMCMConfProfileTxBandNumber           Unsigned32,
           vdslLineMCMConfProfileTxBandStart            Unsigned32,
           vdslLineMCMConfProfileTxBandStop             Unsigned32,
           vdslLineMCMConfProfileTxBandRowStatus        RowStatus
           }

   vdslLineMCMConfProfileTxBandNumber OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "The index for this band descriptor entry."
       ::= { vdslLineMCMConfProfileTxBandEntry 1 }

   vdslLineMCMConfProfileTxBandStart OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "Start tone index for this band."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileTxBandEntry 2 }

   vdslLineMCMConfProfileTxBandStop OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "Stop tone index for this band."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileTxBandEntry 3 }

   vdslLineMCMConfProfileTxBandRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "This object is used to create a new row or modify or
           delete an existing row in this table.
           A profile is activated by setting this object to `active'.
           When `active' is set, the system will validate the profile.






           Each entry must be internally consistent, the Stop Tone must
           be greater than the Start Tone.  Each entry must also be
           externally consistent, all entries indexed by a specific
           profile must not overlap.  Validation of the profile will
           check both internal and external consistency.

           None of the columns in this row may be modified while the
           row is in the 'active' state.

           Before a profile can be deleted or taken out of
           service, (by setting this object to `destroy' or
           `notInService') it must be first unreferenced
           from all associated lines."
       ::= { vdslLineMCMConfProfileTxBandEntry 4 }

   vdslLineMCMConfProfileRxBandTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VdslLineMCMConfProfileRxBandEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "This table contains receive band descriptor configuration
           information for a VDSL line.  Each entry in this table
           reflects the configuration for one of possibly many bands
           with a multiple carrier modulation (MCM) VDSL line.
           These entries are defined by a manager and can be used to
           configure the VDSL line.

           If an entry in this table is referenced by a line which
           does not use MCM, it has no effect on the operation of that
           line.

           All read-create-objects defined in this table SHOULD be
           stored persistently."
       ::= { vdslLineExtMCMMibObjects 3 }

   vdslLineMCMConfProfileRxBandEntry OBJECT-TYPE
       SYNTAX       VdslLineMCMConfProfileRxBandEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "Each entry consists of a transmit band descriptor, which
           is defined by a start and a stop tone index."

       INDEX { vdslLineConfProfileName,
               vdslLineMCMConfProfileRxBandNumber }
       ::= { vdslLineMCMConfProfileRxBandTable 1 }

   VdslLineMCMConfProfileRxBandEntry ::=





       SEQUENCE
           {
           vdslLineMCMConfProfileRxBandNumber           Unsigned32,
           vdslLineMCMConfProfileRxBandStart            Unsigned32,
           vdslLineMCMConfProfileRxBandStop             Unsigned32,
           vdslLineMCMConfProfileRxBandRowStatus        RowStatus
           }

   vdslLineMCMConfProfileRxBandNumber OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "The index for this band descriptor entry."
       ::= { vdslLineMCMConfProfileRxBandEntry 1 }

   vdslLineMCMConfProfileRxBandStart OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "Start tone index for this band."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileRxBandEntry 2 }


   vdslLineMCMConfProfileRxBandStop OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "Stop tone index for this band."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileRxBandEntry 3 }

   vdslLineMCMConfProfileRxBandRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "This object is used to create a new row or modify or
           delete an existing row in this table.

           A profile is activated by setting this object to `active'.
           When `active' is set, the system will validate the profile.
           Each entry must be internally consistent, the Stop Tone must
           be greater than the Start Tone.  Each entry must also be
           externally consistent, all entries indexed by a specific





           profile must not overlap.  Validation of the profile will
           check both internal and external consistency.

           None of the columns in this row may be modified while the
           row is in the 'active' state.

           Before a profile can be deleted or taken out of
           service, (by setting this object to `destroy' or
           `notInService') it must be first unreferenced
           from all associated lines."
       ::= { vdslLineMCMConfProfileRxBandEntry 4 }

   vdslLineMCMConfProfileTxPSDTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VdslLineMCMConfProfileTxPSDEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "This table contains transmit PSD mask descriptor
           configuration information for a VDSL line.  Each entry in
           this table reflects the configuration for one tone within
           a multiple carrier modulation (MCM) VDSL line.  These
           entries are defined by a manager and can be used to
           configure the VDSL line.

           If an entry in this table is referenced by a line which
           does not use MCM, it has no effect on the operation of that
           line.

           All read-create-objects defined in this table SHOULD be
           stored persistently."
       ::= { vdslLineExtMCMMibObjects 4 }

   vdslLineMCMConfProfileTxPSDEntry OBJECT-TYPE
       SYNTAX       VdslLineMCMConfProfileTxPSDEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "Each entry consists of a transmit PSD mask descriptor,
           which defines the power spectral density (PSD) for a tone."

       INDEX { vdslLineConfProfileName,
               vdslLineMCMConfProfileTxPSDNumber }
       ::= { vdslLineMCMConfProfileTxPSDTable 1 }

   VdslLineMCMConfProfileTxPSDEntry ::=
       SEQUENCE
           {
           vdslLineMCMConfProfileTxPSDNumber            Unsigned32,





           vdslLineMCMConfProfileTxPSDTone              Unsigned32,
           vdslLineMCMConfProfileTxPSDPSD               Unsigned32,
           vdslLineMCMConfProfileTxPSDRowStatus         RowStatus
           }

   vdslLineMCMConfProfileTxPSDNumber OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "The index for this mask descriptor entry."
       ::= { vdslLineMCMConfProfileTxPSDEntry 1 }

   vdslLineMCMConfProfileTxPSDTone OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "The tone index for which the PSD is being specified."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileTxPSDEntry 2 }

   vdslLineMCMConfProfileTxPSDPSD OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "0.5dBm/Hz"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "Power Spectral Density level in steps of 0.5dBm/Hz with
           an offset of -140dBm/Hz."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileTxPSDEntry 3 }

       vdslLineMCMConfProfileTxPSDRowStatus OBJECT-TYPE
           SYNTAX       RowStatus
           MAX-ACCESS   read-create
           STATUS       current
           DESCRIPTION
               "This object is used to create a new row or modify or
           delete an existing row in this table.

           A profile is activated by setting this object to `active'.
           When `active' is set, the system will validate the profile.

           None of the columns in this row may be modified while the
           row is in the 'active' state.

           Before a profile can be deleted or taken out of





           service, (by setting this object to `destroy' or
           `notInService') it must be first unreferenced
           from all associated lines."
       ::= { vdslLineMCMConfProfileTxPSDEntry 4 }

   vdslLineMCMConfProfileMaxTxPSDTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VdslLineMCMConfProfileMaxTxPSDEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "This table contains transmit maximum PSD mask descriptor
           configuration information for a VDSL line.  Each entry in
           this table reflects the configuration for one tone within
           a multiple carrier modulation (MCM) VDSL modem.  These
           entries are defined by a manager and can be used to
           configure the VDSL line.

           If an entry in this table is referenced by a line which
           does not use MCM, it has no effect on the operation of that
           line.

           All read-create-objects defined in this table SHOULD be
           stored persistently."
       ::= { vdslLineExtMCMMibObjects 5 }

   vdslLineMCMConfProfileMaxTxPSDEntry OBJECT-TYPE
       SYNTAX       VdslLineMCMConfProfileMaxTxPSDEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "Each entry consists of a transmit PSD mask descriptor,
           which defines the maximum power spectral density (PSD)
           for a tone."
       INDEX { vdslLineConfProfileName,
               vdslLineMCMConfProfileMaxTxPSDNumber }
       ::= { vdslLineMCMConfProfileMaxTxPSDTable 1 }

   VdslLineMCMConfProfileMaxTxPSDEntry ::=
       SEQUENCE
           {
           vdslLineMCMConfProfileMaxTxPSDNumber            Unsigned32,
           vdslLineMCMConfProfileMaxTxPSDTone              Unsigned32,
           vdslLineMCMConfProfileMaxTxPSDPSD               Unsigned32,
           vdslLineMCMConfProfileMaxTxPSDRowStatus         RowStatus
           }

   vdslLineMCMConfProfileMaxTxPSDNumber OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)





       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "The index for this band descriptor entry."
       ::= { vdslLineMCMConfProfileMaxTxPSDEntry 1 }

   vdslLineMCMConfProfileMaxTxPSDTone OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "The tone index for which the PSD is being specified.
            There must not be multiple rows defined, for a particular
            profile, with the same value for this field."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileMaxTxPSDEntry 2 }

   vdslLineMCMConfProfileMaxTxPSDPSD OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "0.5dBm/Hz"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "Power Spectral Density level in steps of 0.5dBm/Hz with
           an offset of -140dBm/Hz."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileMaxTxPSDEntry 3 }

   vdslLineMCMConfProfileMaxTxPSDRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "This object is used to create a new row or modify or
           delete an existing row in this table.
           A profile is activated by setting this object to `active'.
           When `active' is set, the system will validate the profile.
           There must be only one entry in this table for each tone
           associated with a specific profile.  This will be checked
           during the validation process.

           None of the columns in this row may be modified while the
           row is in the 'active' state.

           Before a profile can be deleted or taken out of
           service, (by setting this object to `destroy' or
           `notInService') it must be first unreferenced
           from all associated lines."





       ::= { vdslLineMCMConfProfileMaxTxPSDEntry 4 }

   vdslLineMCMConfProfileMaxRxPSDTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF VdslLineMCMConfProfileMaxRxPSDEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "This table contains maximum receive PSD mask descriptor
           configuration information for a VDSL line.  Each entry in
           this table reflects the configuration for one tone within
           a multiple carrier modulation (MCM) VDSL modem.  These
           entries are defined by a manager and can be used to
           configure the VDSL line.

           If an entry in this table is referenced by a line which
           does not use MCM, it has no effect on the operation of that
           line.

           All read-create-objects defined in this table SHOULD be
           stored persistently."
       ::= { vdslLineExtMCMMibObjects 6 }

   vdslLineMCMConfProfileMaxRxPSDEntry OBJECT-TYPE
       SYNTAX       VdslLineMCMConfProfileMaxRxPSDEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
           "Each entry consists of a transmit PSD mask descriptor,
           which defines the power spectral density (PSD) for a
           tone."

       INDEX { vdslLineConfProfileName,
               vdslLineMCMConfProfileMaxRxPSDNumber }
       ::= { vdslLineMCMConfProfileMaxRxPSDTable 1 }

   VdslLineMCMConfProfileMaxRxPSDEntry ::=
       SEQUENCE
           {
           vdslLineMCMConfProfileMaxRxPSDNumber            Unsigned32,
           vdslLineMCMConfProfileMaxRxPSDTone              Unsigned32,
           vdslLineMCMConfProfileMaxRxPSDPSD               Unsigned32,
           vdslLineMCMConfProfileMaxRxPSDRowStatus         RowStatus
           }

   vdslLineMCMConfProfileMaxRxPSDNumber OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   not-accessible
       STATUS       current





       DESCRIPTION
           "The index for this band descriptor entry."
       ::= { vdslLineMCMConfProfileMaxRxPSDEntry 1 }

   vdslLineMCMConfProfileMaxRxPSDTone OBJECT-TYPE
       SYNTAX       Unsigned32 (1..4096)
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "The tone index for which the PSD is being specified.
            There must not be multiple rows defined, for a particular
            profile, with the same value for this field."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileMaxRxPSDEntry 2 }

   vdslLineMCMConfProfileMaxRxPSDPSD OBJECT-TYPE
       SYNTAX       Unsigned32
       UNITS        "0.5dBm/Hz"
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "Power Spectral Density level in steps of 0.5dBm/Hz with
           an offset of -140dBm/Hz."
       REFERENCE    "T1E1.4/2000-013R4"    -- Part 3, MCM
       ::= { vdslLineMCMConfProfileMaxRxPSDEntry 3 }

   vdslLineMCMConfProfileMaxRxPSDRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "This object is used to create a new row or modify or
           delete an existing row in this table.

           A profile is activated by setting this object to `active'.
           When `active' is set, the system will validate the profile.
           There must be only one entry in this table for each tone
           associated with a specific profile.  This will be checked
           during the validation process.

           None of the columns in this row may be modified while the
           row is in the 'active' state.

           Before a profile can be deleted or taken out of
           service, (by setting this object to `destroy' or
           `notInService') it must be first unreferenced
           from all associated lines."
       ::= { vdslLineMCMConfProfileMaxRxPSDEntry 4 }





   -- conformance information

   vdslLineExtMCMConformance OBJECT IDENTIFIER ::=
                    { vdslLineExtMCMMib 2 }
   vdslLineExtMCMGroups OBJECT IDENTIFIER ::=
                    { vdslLineExtMCMConformance 1 }
   vdslLineExtMCMCompliances OBJECT IDENTIFIER ::=
                    { vdslLineExtMCMConformance 2 }

   vdslLineExtMCMMibCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
           "The compliance statement for SNMP entities which
           manage VDSL interfaces."
       MODULE  -- this module
       MANDATORY-GROUPS
       {
           vdslLineExtMCMGroup
       }

       ::= { vdslLineExtMCMCompliances 1 }

   -- units of conformance

       vdslLineExtMCMGroup OBJECT-GROUP
           OBJECTS
               {
               vdslLineMCMConfProfileTxWindowLength,
               vdslLineMCMConfProfileRowStatus,
               vdslLineMCMConfProfileTxBandStart,
               vdslLineMCMConfProfileTxBandStop,
               vdslLineMCMConfProfileTxBandRowStatus,
               vdslLineMCMConfProfileRxBandStart,
               vdslLineMCMConfProfileRxBandStop,
               vdslLineMCMConfProfileRxBandRowStatus,
               vdslLineMCMConfProfileTxPSDTone,
               vdslLineMCMConfProfileTxPSDPSD,
               vdslLineMCMConfProfileTxPSDRowStatus,
               vdslLineMCMConfProfileMaxTxPSDTone,
               vdslLineMCMConfProfileMaxTxPSDPSD,
               vdslLineMCMConfProfileMaxTxPSDRowStatus,
               vdslLineMCMConfProfileMaxRxPSDTone,
               vdslLineMCMConfProfileMaxRxPSDPSD,
               vdslLineMCMConfProfileMaxRxPSDRowStatus
               }
            STATUS     current
            DESCRIPTION
                "A collection of objects providing configuration





                information for a VDSL line based upon multiple
                carrier modulation modem."
        ::= { vdslLineExtMCMGroups 1 }

   END


