OSPF-TRAP-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE, IpAddress
                    FROM SNMPv2-SMI
       MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
                    FROM SNMPv2-CONF
       ospfRouterId, ospfIfIpAddress, ospfAddressLessIf, ospfIfState,
       ospfVirtIfAreaId, ospfVirtIfNeighbor, ospfVirtIfState,
       ospfNbrIpAddr, ospfNbrAddressLessIndex, ospfNbrRtrId,
       ospfNbrState, ospfVirtNbrArea, ospfVirtNbrRtrId,
       ospfVirtNbrState, ospfLsdbType, ospfLsdbLsid, ospfLsdbRouterId,
       ospfLsdbAreaId, ospfExtLsdbLimit, ospf, ospfAreaId,
       ospfAreaNssaTranslatorState, ospfRestartStatus,
       ospfRestartInterval, ospfRestartExitReason,
       ospfNbrRestartHelperStatus, ospfNbrRestartHelperAge,
       ospfNbrRestartHelperExitReason, ospfVirtNbrRestartHelperStatus,
       ospfVirtNbrRestartHelperAge, ospfVirtNbrRestartHelperExitReason
                    FROM OSPF-MIB;

     ospfTrap MODULE-IDENTITY

          LAST-UPDATED "200611100000Z" -- November 10, 2006 00:00:00 EST
          ORGANIZATION "IETF OSPF Working Group"
          CONTACT-INFO
          "WG E-Mail: ospf@ietf.org

           WG Chairs: acee@cisco.com
                      rohit@gmail.com

           Editors:   Dan Joyal
                      Nortel
                      600 Technology Park Drive
                      Billerica, MA  01821
                      djoyal@nortel.com

                      Piotr Galecki
                      Airvana
                      19 Alpha Road
                      Chelmsford, MA 01824
                      pgalecki@airvana.com

                      Spencer Giacalone
                      CSFB
                      Eleven Madison Ave
                      New York, NY 10010-3629





                      spencer.giacalone@gmail.com"

          DESCRIPTION
             "The MIB module to describe traps for the OSPF
             Version 2 Protocol.

             Copyright (C) The IETF Trust (2006).
             This version of this MIB module is part of
             RFC 4750;  see the RFC itself for full legal
             notices."

          REVISION "200611100000Z" -- November 10, 2006 00:00:00 EST
          DESCRIPTION
             "Updated for latest changes to OSPFv2:
              -added graceful restart related traps
              -added new config error types
              -added ospfNssaTranslatorStatusChange trap.
              See Appendix B of RFC 4750 for more details.

             This version published as part of RFC 4750"

          REVISION "199501201225Z" -- Fri Jan 20 12:25:50 PST 1995
          DESCRIPTION
             "The initial SMIv2 revision of this MIB module, published
             in RFC 1850."

          ::= { ospf 16 }

   --  Trap Support Objects

   --  The following are support objects for the OSPF traps.

     ospfTrapControl OBJECT IDENTIFIER ::= { ospfTrap 1 }
     ospfTraps OBJECT IDENTIFIER ::= { ospfTrap 2 }

     ospfSetTrap OBJECT-TYPE
          SYNTAX       OCTET STRING (SIZE(4))
          MAX-ACCESS   read-write
          STATUS       current
          DESCRIPTION
             "A 4-octet string serving as a bit map for
             the trap events defined by the OSPF traps.  This
             object is used to enable and disable specific
             OSPF traps where a 1 in the bit field
             represents enabled.  The right-most bit (least
             significant) represents trap 0.

             This object is persistent and when written





             the entity SHOULD save the change to non-volatile
             storage."
           ::= { ospfTrapControl 1 }

     ospfConfigErrorType OBJECT-TYPE
          SYNTAX       INTEGER {
                          badVersion (1),
                          areaMismatch (2),
                          unknownNbmaNbr (3), -- Router is DR eligible
                          unknownVirtualNbr (4),
                          authTypeMismatch(5),
                          authFailure (6),
                          netMaskMismatch (7),
                          helloIntervalMismatch (8),
                          deadIntervalMismatch (9),
                          optionMismatch (10),
                          mtuMismatch (11),
                          duplicateRouterId (12),
                          noError (13) }
          MAX-ACCESS   read-only
          STATUS   current
          DESCRIPTION
             "Potential types of configuration conflicts.
             Used by the ospfConfigError and
             ospfConfigVirtError traps.  When the last value
             of a trap using this object is needed, but no
             traps of that type have been sent, this value
             pertaining to this object should be returned as
             noError."
          ::= { ospfTrapControl 2 }

     ospfPacketType OBJECT-TYPE
          SYNTAX       INTEGER {
                          hello (1),
                          dbDescript (2),
                          lsReq (3),
                          lsUpdate (4),
                          lsAck (5),
                          nullPacket (6) }
          MAX-ACCESS   read-only
          STATUS       current
          DESCRIPTION
             "OSPF packet types.  When the last value of a trap
             using this object is needed, but no traps of
             that type have been sent, this value pertaining
             to this object should be returned as nullPacket."
          ::= { ospfTrapControl 3 }






     ospfPacketSrc OBJECT-TYPE
          SYNTAX       IpAddress
          MAX-ACCESS   read-only
          STATUS       current
          DESCRIPTION
             "The IP address of an inbound packet that cannot
             be identified by a neighbor instance.  When
             the last value of a trap using this object is
             needed, but no traps of that type have been sent,
             this value pertaining to this object should
             be returned as 0.0.0.0."
          ::= { ospfTrapControl 4 }

   --  Traps

     ospfVirtIfStateChange NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfVirtIfAreaId,
             ospfVirtIfNeighbor,
             ospfVirtIfState  -- The new state
             }
          STATUS       current
          DESCRIPTION
             "An ospfVirtIfStateChange trap signifies that there
             has been a change in the state of an OSPF virtual
             interface.

             This trap should be generated when the interface
             state regresses (e.g., goes from Point-to-Point to Down)
             or progresses to a terminal state
             (i.e., Point-to-Point)."
          ::= { ospfTraps 1 }

     ospfNbrStateChange NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfNbrIpAddr,
             ospfNbrAddressLessIndex,
             ospfNbrRtrId,
             ospfNbrState  -- The new state
             }
          STATUS       current
          DESCRIPTION
             "An ospfNbrStateChange trap signifies that
             there has been a change in the state of a
             non-virtual OSPF neighbor.  This trap should be
             generated when the neighbor state regresses
             (e.g., goes from Attempt or Full to 1-Way or
             Down) or progresses to a terminal state (e.g.,





             2-Way or Full).  When an neighbor transitions
             from or to Full on non-broadcast multi-access
             and broadcast networks, the trap should be
             generated by the designated router.  A designated
             router transitioning to Down will be noted by
             ospfIfStateChange."
          ::= { ospfTraps 2 }

     ospfVirtNbrStateChange NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfVirtNbrArea,
             ospfVirtNbrRtrId,
             ospfVirtNbrState  -- The new state
             }
          STATUS       current
          DESCRIPTION
             "An ospfVirtNbrStateChange trap signifies that there
             has been a change in the state of an OSPF virtual
             neighbor.  This trap should be generated
             when the neighbor state regresses (e.g., goes
             from Attempt or Full to 1-Way or Down) or
             progresses to a terminal state (e.g., Full)."
          ::= { ospfTraps 3 }

     ospfIfConfigError NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfIfIpAddress,
             ospfAddressLessIf,
             ospfPacketSrc,  -- The source IP address
             ospfConfigErrorType, -- Type of error
             ospfPacketType
             }
          STATUS       current
          DESCRIPTION
             "An ospfIfConfigError trap signifies that a
             packet has been received on a non-virtual
             interface from a router whose configuration
             parameters conflict with this router's
             configuration parameters.  Note that the event
             optionMismatch should cause a trap only if it
             prevents an adjacency from forming."
          ::= { ospfTraps 4 }

     ospfVirtIfConfigError NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfVirtIfAreaId,
             ospfVirtIfNeighbor,
             ospfConfigErrorType, -- Type of error





             ospfPacketType
             }
          STATUS       current
          DESCRIPTION
             "An ospfVirtIfConfigError trap signifies that a
             packet has been received on a virtual interface
             from a router whose configuration parameters
             conflict with this router's configuration
             parameters.  Note that the event optionMismatch
             should cause a trap only if it prevents an
             adjacency from forming."
          ::= { ospfTraps 5 }

     ospfIfAuthFailure NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfIfIpAddress,
             ospfAddressLessIf,
             ospfPacketSrc,  -- The source IP address
             ospfConfigErrorType, -- authTypeMismatch or
                                  -- authFailure
             ospfPacketType
             }
          STATUS       current
          DESCRIPTION
             "An ospfIfAuthFailure trap signifies that a
             packet has been received on a non-virtual
             interface from a router whose authentication key
             or authentication type conflicts with this
             router's authentication key or authentication
             type."
          ::= { ospfTraps 6 }

     ospfVirtIfAuthFailure NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfVirtIfAreaId,
             ospfVirtIfNeighbor,
             ospfConfigErrorType, -- authTypeMismatch or
                                  -- authFailure
             ospfPacketType
             }
          STATUS       current
          DESCRIPTION
             "An ospfVirtIfAuthFailure trap signifies that a
             packet has been received on a virtual interface
             from a router whose authentication key or
             authentication type conflicts with this router's
             authentication key or authentication type."






          ::= { ospfTraps 7 }

     ospfIfRxBadPacket NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfIfIpAddress,
             ospfAddressLessIf,
             ospfPacketSrc,  -- The source IP address
             ospfPacketType
             }
          STATUS       current
          DESCRIPTION
             "An ospfIfRxBadPacket trap signifies that an
             OSPF packet has been received on a non-virtual
             interface that cannot be parsed."
          ::= { ospfTraps 8 }

     ospfVirtIfRxBadPacket NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
            ospfVirtIfAreaId,
            ospfVirtIfNeighbor,
            ospfPacketType
            }
          STATUS       current
          DESCRIPTION
             "An ospfVirtIfRxBadPacket trap signifies that an OSPF
             packet has been received on a virtual interface
             that cannot be parsed."
          ::= { ospfTraps 9 }

     ospfTxRetransmit NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfIfIpAddress,
             ospfAddressLessIf,
             ospfNbrRtrId, -- Destination
             ospfPacketType,
             ospfLsdbType,
             ospfLsdbLsid,
             ospfLsdbRouterId
             }
           STATUS       current
           DESCRIPTION
              "An ospfTxRetransmit trap signifies than an
              OSPF packet has been retransmitted on a
              non-virtual interface.  All packets that may be
              retransmitted are associated with an LSDB entry.
              The LS type, LS ID, and Router ID are used to
              identify the LSDB entry."
           ::= { ospfTraps 10 }





     ospfVirtIfTxRetransmit NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfVirtIfAreaId,
             ospfVirtIfNeighbor,
             ospfPacketType,
             ospfLsdbType,
             ospfLsdbLsid,
             ospfLsdbRouterId
             }
          STATUS       current
          DESCRIPTION
             "An ospfVirtIfTxRetransmit trap signifies than an
             OSPF packet has been retransmitted on a virtual
             interface.  All packets that may be retransmitted
             are associated with an LSDB entry.  The LS
             type, LS ID, and Router ID are used to identify
             the LSDB entry."
          ::= { ospfTraps 11 }

     ospfOriginateLsa NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfLsdbAreaId,  -- 0.0.0.0 for AS Externals
             ospfLsdbType,
             ospfLsdbLsid,
             ospfLsdbRouterId
             }
          STATUS       current
          DESCRIPTION
             "An ospfOriginateLsa trap signifies that a new
             LSA has been originated by this router.  This
             trap should not be invoked for simple refreshes
             of LSAs (which happens every 30 minutes), but
             instead will only be invoked when an LSA is
             (re)originated due to a topology change.
             Additionally, this trap does not include LSAs that
             are being flushed because they have reached
             MaxAge."
          ::= { ospfTraps 12 }

     ospfMaxAgeLsa NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfLsdbAreaId,  -- 0.0.0.0 for AS Externals
             ospfLsdbType,
             ospfLsdbLsid,
             ospfLsdbRouterId
             }
          STATUS       current
          DESCRIPTION





             "An ospfMaxAgeLsa trap signifies that one of
             the LSAs in the router's link state database has
             aged to MaxAge."
          ::= { ospfTraps 13 }

     ospfLsdbOverflow NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfExtLsdbLimit
             }

          STATUS       current
          DESCRIPTION
             "An ospfLsdbOverflow trap signifies that the
             number of LSAs in the router's link state
             database has exceeded ospfExtLsdbLimit."
          ::= { ospfTraps 14 }

     ospfLsdbApproachingOverflow NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfExtLsdbLimit
             }
          STATUS       current
          DESCRIPTION
             "An ospfLsdbApproachingOverflow trap signifies
             that the number of LSAs in the router's
             link state database has exceeded ninety percent of
             ospfExtLsdbLimit."
          ::= { ospfTraps 15 }

     ospfIfStateChange NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
             ospfIfIpAddress,
             ospfAddressLessIf,
             ospfIfState   -- The new state
             }
          STATUS       current
          DESCRIPTION
             "An ospfIfStateChange trap signifies that there
             has been a change in the state of a non-virtual
             OSPF interface.  This trap should be generated
             when the interface state regresses (e.g., goes
             from Dr to Down) or progresses to a terminal
             state (i.e., Point-to-Point, DR Other, Dr, or
             Backup)."
          ::= { ospfTraps 16 }

     ospfNssaTranslatorStatusChange NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap





             ospfAreaId,
             ospfAreaNssaTranslatorState -- The current translation
                                         -- status
             }
          STATUS       current
          DESCRIPTION
             "An ospfNssaTranslatorStatusChange trap indicates that
             there has been a change in the router's ability to
             translate OSPF type-7 LSAs into OSPF type-5 LSAs.
             This trap should be generated when the translator
             status transitions from or to any defined status on
             a per-area basis."
          ::= { ospfTraps 17 }

     ospfRestartStatusChange NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
                    ospfRestartStatus,
                    ospfRestartInterval,
                    ospfRestartExitReason
                  }
          STATUS       current
          DESCRIPTION
             "An ospfRestartStatusChange trap signifies that
             there has been a change in the graceful restart
             state for the router.  This trap should be
             generated when the router restart status
             changes."
          ::= { ospfTraps 18 }

     ospfNbrRestartHelperStatusChange NOTIFICATION-TYPE
          OBJECTS { ospfRouterId, -- The originator of the trap
                    ospfNbrIpAddr,
                    ospfNbrAddressLessIndex,
                    ospfNbrRtrId,
                    ospfNbrRestartHelperStatus,
                    ospfNbrRestartHelperAge,
                    ospfNbrRestartHelperExitReason
                  }
          STATUS       current
          DESCRIPTION
             "An ospfNbrRestartHelperStatusChange trap signifies that
             there has been a change in the graceful restart
             helper state for the neighbor.  This trap should be
             generated when the neighbor restart helper status
             transitions for a neighbor."
          ::= { ospfTraps 19 }

     ospfVirtNbrRestartHelperStatusChange NOTIFICATION-TYPE





          OBJECTS { ospfRouterId, -- The originator of the trap
                    ospfVirtNbrArea,
                    ospfVirtNbrRtrId,
                    ospfVirtNbrRestartHelperStatus,
                    ospfVirtNbrRestartHelperAge,
                    ospfVirtNbrRestartHelperExitReason
                  }
          STATUS       current
          DESCRIPTION
             "An ospfVirtNbrRestartHelperStatusChange trap signifies
             that there has been a change in the graceful restart
             helper state for the virtual neighbor.  This trap should
             be generated when the virtual neighbor restart helper
             status transitions for a virtual neighbor."
          ::= { ospfTraps 20 }

   --  conformance information

   ospfTrapConformance OBJECT IDENTIFIER ::= { ospfTrap 3 }
   ospfTrapGroups      OBJECT IDENTIFIER ::= { ospfTrapConformance 1 }
   ospfTrapCompliances OBJECT IDENTIFIER ::= { ospfTrapConformance 2 }

   --  compliance statements

   ospfTrapCompliance MODULE-COMPLIANCE
        STATUS       obsolete
        DESCRIPTION
           "The compliance statement."
        MODULE       -- this module
        MANDATORY-GROUPS { ospfTrapControlGroup }

        GROUP       ospfTrapControlGroup
        DESCRIPTION
           "This group is optional but recommended for all
           OSPF systems."
        ::= { ospfTrapCompliances 1 }

   ospfTrapCompliance2 MODULE-COMPLIANCE
        STATUS       current
        DESCRIPTION
           "The compliance statement."
        MODULE       -- this module
        MANDATORY-GROUPS { ospfTrapControlGroup, ospfTrapEventGroup }
        OBJECT       ospfConfigErrorType
        MIN-ACCESS   accessible-for-notify
        DESCRIPTION
           "This object is only required to be supplied within
           notifications."





        OBJECT       ospfPacketType
        MIN-ACCESS   accessible-for-notify
        DESCRIPTION
           "This object is only required to be supplied within
           notifications."
        OBJECT       ospfPacketSrc
        MIN-ACCESS   accessible-for-notify
        DESCRIPTION
           "This object is only required to be supplied within
           notifications."
        ::= { ospfTrapCompliances 2 }

   --  units of conformance

     ospfTrapControlGroup    OBJECT-GROUP
          OBJECTS { ospfSetTrap,
                    ospfConfigErrorType,
                    ospfPacketType,
                    ospfPacketSrc }
          STATUS       current
          DESCRIPTION
             "These objects are required to control traps
             from OSPF systems."
          ::= { ospfTrapGroups 1 }

     ospfTrapEventGroup       NOTIFICATION-GROUP
          NOTIFICATIONS {
             ospfVirtIfStateChange,
             ospfNbrStateChange,
             ospfVirtNbrStateChange,
             ospfIfConfigError,
             ospfVirtIfConfigError,
             ospfIfAuthFailure,
             ospfVirtIfAuthFailure,
             ospfIfRxBadPacket,
             ospfVirtIfRxBadPacket,
             ospfTxRetransmit,
             ospfVirtIfTxRetransmit,
             ospfOriginateLsa,
             ospfMaxAgeLsa,
             ospfLsdbOverflow,
             ospfLsdbApproachingOverflow,
             ospfIfStateChange,
             ospfNssaTranslatorStatusChange,
             ospfRestartStatusChange,
             ospfNbrRestartHelperStatusChange,
             ospfVirtNbrRestartHelperStatusChange
             }





          STATUS        current
          DESCRIPTION
             "A grouping of OSPF trap events, as specified
             in NOTIFICATION-TYPE constructs."
          ::= { ospfTrapGroups 2 }

   END


