T11-FC-NAME-SERVER-MIB DEFINITIONS ::= BEGIN


-- The MIB for management of the Fibre Channel functionality which
-- implements the Name Server function.

IMPORTS
    MODULE-IDENTITY,OBJECT-TYPE,
    NOTIFICATION-TYPE, Unsigned32,
    Counter32, Integer32, mib-2   FROM SNMPv2-SMI         -- [RFC2578]
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP            FROM SNMPv2-CONF        -- [RFC2580]
    SnmpAdminString               FROM SNMP-FRAMEWORK-MIB -- [RFC3411]
    TruthValue, TEXTUAL-CONVENTION,
    TimeStamp                     FROM SNMPv2-TC          -- [RFC2579]
    fcmInstanceIndex, FcPortType,
    FcAddressIdOrZero, FcClasses,
    FcNameIdOrZero                FROM FC-MGMT-MIB        -- [FC-MGMT]
    T11FabricIndex                FROM T11-TC-MIB      -- [FC-FAM-MIB]
    t11FamLocalSwitchWwn
                      FROM T11-FC-FABRIC-ADDR-MGR-MIB; -- [FC-FAM-MIB]

t11FcNameServerMIB  MODULE-IDENTITY
    LAST-UPDATED "200603020000Z"
    ORGANIZATION "T11"
    CONTACT-INFO
            "     Claudio DeSanti
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA 95134 USA
                  Phone: +1 408 853-9172
                  EMail: cds@cisco.com

                  Keith McCloghrie
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA USA 95134
                  Phone: +1 408-526-5260
                  EMail: kzm@cisco.com"
    DESCRIPTION
           "The MIB module for the management of the functionality,
           which realizes the FC-GS-4 requirements for Name
           Server (NS).

           Copyright (C) The Internet Society (2006).  This version of
           this MIB module is part of RFC 4438; see the RFC itself for
           full legal notices."





    REVISION    "200603020000Z"
    DESCRIPTION
           "Initial version of this MIB module, published as RFC 4438."
    ::= { mib-2 135 }

t11NsNotifications    OBJECT IDENTIFIER ::= { t11FcNameServerMIB 0 }
t11NsMIBObjects       OBJECT IDENTIFIER ::= { t11FcNameServerMIB 1 }
t11NsMIBConformance   OBJECT IDENTIFIER ::= { t11FcNameServerMIB 2 }
t11NsStatus           OBJECT IDENTIFIER ::= { t11NsMIBObjects 1 }
t11NsStatistics       OBJECT IDENTIFIER ::= { t11NsMIBObjects 2 }

-- Textual Conventions

T11NsGs4RejectReasonCode ::= TEXTUAL-CONVENTION
    STATUS    current
    DESCRIPTION
        "The FC-GS-4 reject reason code for a request.

         none(1)
             - no error.
         invalidCmdCode(2)
             - request contained an invalid command code.
         invalidVerLevel(3)
             - request contained an invalid version number.
         logicalError(4)
             - there was a logical error.
         invalidIUSize(5)
             - the CT_IU (Information Unit) size was invalid.
         logicalBusy(6)
             - the module is busy.
         protocolError(7)
             - there was a protocol error.
         unableToPerformCmdReq(8)
             - the command specified in the req could not be
               executed.  The details of exactly what failed
               will be in the corresponding reason code
               explanation.
         cmdNotSupported(9)
             - the command is not supported.
         serverNotAvailable(10)
             - the identified server was not available.
         couldNotEstabSession(11)
             - a server session could not be established.
         vendorError(12)
             - a vendor-specific error."
    REFERENCE
          "ANSI INCITS 387-2004, Fibre Channel - Generic
           Services-4 (FC-GS-4), section 4.4.3."





    SYNTAX  INTEGER {
              none(1),
              invalidCmdCode(2),
              invalidVerLevel(3),
              logicalError(4),
              invalidIUSize(5),
              logicalBusy(6),
              protocolError(7),
              unableToPerformCmdReq(8),
              cmdNotSupported(9),
              serverNotAvailable(10),
              couldNotEstabSession(11),
              vendorError(12)
            }

T11NsRejReasonCodeExpl ::= TEXTUAL-CONVENTION
    STATUS    current
    DESCRIPTION
        "The reject reason code explanation:

         noAdditionalExplanation(1)
             - no additional explanation.
         portIdentifierNotRegistered(2)
             - Port Identifier not registered.
         portNameNotRegistered(3)
             - Port Name not registered.
         nodeNameNotRegistered(4)
             - Node Name not registered.
         classOfServiceNotRegistered(5)
             - Class of Service not registered.
         nodeIpAddressNotRegistered(6)
             - 'IP Address (Node)' value not registered.
         ipaNotRegistered(7)
             - Initial Process Associator (IPA) not registered.
         fc4TypeNotRegistered(8)
             - FC-4 TYPEs not registered.
         symbolicPortNameNotRegistered(9)
             - Symbolic Port Name not registered.
         symbolicNodeNameNotRegistered(10)
             - Symbolic Node Name not registered.
         portTypeNotRegistered(11)
             - 'Port Type' not registered.
         portIpAddressNotRegistered(12)
             - 'IP Address (Port)' value not registered.
         fabricPortNameNotRegistered(13)
             - Fabric Port Name not registered.
         hardAddressNotRegistered(14)
             - 'Hard Address' not registered.





         fc4DescriptorNotRegistered(15)
             - FC-4 Descriptor not registered.
         fc4FeaturesNotRegistered(16)
             - FC-4 Features not registered.
         accessDenied(17)
             - Access denied.
         unacceptablePortIdentifier(18)
             - Unacceptable Port Identifier.
         databaseEmpty(19)
             - Database is empty.
         noObjectRegInSpecifiedScope(20)
             - no object has been registered in the specified
               scope.
         domainIdNotPresent(21)
             - Domain ID not present.
         portIdNotPresent(22)
             - Port number not present.
         noDeviceAttached(23)
             - No device attached.
         authorizationException(24)
             - Authorization Exception.
         authenticationException(25)
             - Authentication Exception.
         databaseFull(26)
             - Database full."
    REFERENCE
          "ANSI INCITS 387-2004, Fibre Channel - Generic
           Services-4 (FC-GS-4), sections 4.4.4 and 5.2.4"
    SYNTAX  INTEGER {
              noAdditionalExplanation(1),
              portIdentifierNotRegistered(2),
              portNameNotRegistered(3),
              nodeNameNotRegistered(4),
              classOfServiceNotRegistered(5),
              nodeIpAddressNotRegistered(6),
              ipaNotRegistered(7),
              fc4TypeNotRegistered(8),
              symbolicPortNameNotRegistered(9),
              symbolicNodeNameNotRegistered(10),
              portTypeNotRegistered(11),
              portIpAddressNotRegistered(12),
              fabricPortNameNotRegistered(13),
              hardAddressNotRegistered(14),
              fc4DescriptorNotRegistered(15),
              fc4FeaturesNotRegistered(16),
              accessDenied(17),
              unacceptablePortIdentifier(18),
              databaseEmpty(19),





              noObjectRegInSpecifiedScope(20),
              domainIdNotPresent(21),
              portIdNotPresent(22),
              noDeviceAttached(23),
              authorizationException(24),
              authenticationException(25),
              databaseFull(26)
           }

--
-- Information about a Name Server Information Subset
--

t11NsInfoSubsetTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF T11NsInfoSubsetEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "This table contains one entry for each Name Server
           Information Subset within each Fibre Channel
           management instance."
    ::= { t11NsStatus 1 }

t11NsInfoSubsetEntry OBJECT-TYPE
    SYNTAX        T11NsInfoSubsetEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "This entry contains information about operations
           on a particular Name Server Information Subset
           within the Fibre Channel management instance
           identified by fcmInstanceIndex."
    INDEX { fcmInstanceIndex, t11NsInfoSubsetIndex }
    ::= { t11NsInfoSubsetTable 1 }

T11NsInfoSubsetEntry ::= SEQUENCE {
    t11NsInfoSubsetIndex                 Unsigned32,
    t11NsInfoSubsetSwitchIndex           Unsigned32,
    t11NsInfoSubsetTableLastChange       TimeStamp,
    t11NsInfoSubsetNumRows               Integer32,
    t11NsInfoSubsetTotalRejects          Counter32,
    t11NsInfoSubsetRejReqNotfyEnable     TruthValue
}

t11NsInfoSubsetIndex OBJECT-TYPE
    SYNTAX        Unsigned32 (1..4294967295)
    MAX-ACCESS    not-accessible
    STATUS        current





    DESCRIPTION
           "An arbitrary integer value that uniquely identifies
           this Name Server Information Subset amongst all others
           within the same Fibre Channel management instance.

           It is mandatory to keep this value constant between
           restarts of the agent and to make every possible
           effort to keep it constant across such restarts."
    ::= { t11NsInfoSubsetEntry 1 }

t11NsInfoSubsetSwitchIndex OBJECT-TYPE
    SYNTAX        Unsigned32 (0..4294967295)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The value of this object is zero when operations
           upon this Name Server Information Subset do not occur
           at a local Fibre Channel switch; otherwise, it is
           non-zero and identifies the local switch.

           The switch identified by a non-zero value of this
           object is the same switch as is identified by the
           same value of fcmSwitchIndex."
    REFERENCE
           "fcmSwitchIndex is defined in the FC-MGMT-MIB module"
    ::= { t11NsInfoSubsetEntry 2 }

t11NsInfoSubsetTableLastChange OBJECT-TYPE
    SYNTAX        TimeStamp
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The value of sysUpTime at the time of the last update
           to any entry in the t11NsRegTable with the same values
           of fcmInstanceIndex and t11NsInfoSubsetIndex.  This
           includes creation of an entry, deletion of an entry, or
           modification of an existing entry.  If no such update
           has taken place since the last re-initialization of the
           local network management subsystem, then this object
           contains a zero value."
    ::= { t11NsInfoSubsetEntry 3 }

t11NsInfoSubsetNumRows OBJECT-TYPE
    SYNTAX        Integer32 (0..2147483647)
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The number of Nx_Ports currently registered in this





           Name Server Information Subset, i.e., the number of
           rows in the t11NsRegTable with the same values of
           fcmInstanceIndex and t11NsInfoSubsetIndex."
    ::= { t11NsInfoSubsetEntry 4 }

t11NsInfoSubsetTotalRejects OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The total number of (CT_IU) Requests for Name Server
           functions that were rejected for inclusion in this
           Name Server Information Subset, across all Fabrics
           for which it contains information.

           This counter has no discontinuities other than those
           that all Counter32s have when sysUpTime=0."
    ::= { t11NsInfoSubsetEntry 5 }

t11NsInfoSubsetRejReqNotfyEnable OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
           "This object indicates whether 't11NsRejectRegNotify'
           notifications are generated by rejections of requests
           to register information in this Name Server Information
           Subset.

           If value of this object is 'true', then the
           notification is generated when a request is rejected.
           If it is 'false', the notification is not generated.

           The persistence of values of this object across an
           agent reboot is implementation-dependent."
    DEFVAL { false }
    ::= { t11NsInfoSubsetEntry 6 }

--
-- Registered Port Information
--

t11NsRegTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF T11NsRegEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "This table contains entries for all Nx_Ports registered





           in the identified Name Server Information Subsets across
           all Fabrics for which such subsets contain information."
    ::= { t11NsStatus 2 }

t11NsRegEntry OBJECT-TYPE
    SYNTAX T11NsRegEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "An entry containing information about an Nx_Port
           represented by t11NsRegPortIdentifier that is registered
           with a Name Server Information Subset (identified by
           t11NsInfoSubsetIndex) within the Fibre Channel management
           instance (identified by fcmInstanceIndex) on the Fabric
           (identified by t11NsRegFabricIndex)."
    INDEX { fcmInstanceIndex, t11NsInfoSubsetIndex,
            t11NsRegFabricIndex, t11NsRegPortIdentifier }
    ::= { t11NsRegTable 1 }

T11NsRegEntry ::= SEQUENCE {
    t11NsRegFabricIndex            T11FabricIndex,
    t11NsRegPortIdentifier         FcAddressIdOrZero,
    t11NsRegPortName               FcNameIdOrZero,
    t11NsRegNodeName               FcNameIdOrZero,
    t11NsRegClassOfSvc             FcClasses,
    t11NsRegNodeIpAddress          OCTET STRING,
    t11NsRegProcAssoc              OCTET STRING,
    t11NsRegFc4Type                OCTET STRING,
    t11NsRegPortType               FcPortType,
    t11NsRegPortIpAddress          OCTET STRING,
    t11NsRegFabricPortName         FcNameIdOrZero,
    t11NsRegHardAddress            FcAddressIdOrZero,
    t11NsRegSymbolicPortName       SnmpAdminString,
    t11NsRegSymbolicNodeName       SnmpAdminString,
    t11NsRegFc4Features            OCTET STRING
    }

t11NsRegFabricIndex OBJECT-TYPE
    SYNTAX               T11FabricIndex
    MAX-ACCESS           not-accessible
    STATUS               current
    DESCRIPTION
           "A unique index value that uniquely identifies a
           particular Fabric.

           In a Fabric conformant to SW-3, only a single Fabric can
           operate within a single physical infrastructure, and thus,
           the value of this Fabric Index will always be 1.





           However, it is possible that future standards will define
           how multiple Fabrics, each with its own management
           instrumentation, could operate within one (or more) physical
           infrastructures.  To allow for this future possibility, this
           index value is used to uniquely identify a particular
           Fabric within a physical infrastructure."
    ::= { t11NsRegEntry 1 }

t11NsRegPortIdentifier OBJECT-TYPE
    SYNTAX               FcAddressIdOrZero
    MAX-ACCESS           not-accessible
    STATUS               current
    DESCRIPTION
           "The Fibre Channel Address Identifier of this Nx_Port.
           If no Port Identifier has been registered, then the
           value of this object is the zero-length string."
    ::= { t11NsRegEntry 2 }

t11NsRegPortName OBJECT-TYPE
    SYNTAX        FcNameIdOrZero
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The Port_Name (WWN) of this Nx_Port.
           If this object has not been registered, then its value
           is the zero-length string."
    DEFVAL {''H}
    ::= { t11NsRegEntry 3 }

t11NsRegNodeName OBJECT-TYPE
    SYNTAX        FcNameIdOrZero
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The Node_Name (WWN) of this Nx_Port.
           If this object has not been registered, then its value
           is the zero-length string."
    DEFVAL {''H}
    ::= { t11NsRegEntry 4 }

t11NsRegClassOfSvc OBJECT-TYPE
    SYNTAX        FcClasses
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The class of service indicator.  This object is an
           array of bits that contain a bit map of the classes of
           service supported by the associated port.  If a bit in





           this object is 1, it indicates that the class of
           service is supported by the associated port.  When a
           bit is set to 0, it indicates that no class of service
           is supported by this Nx_Port.

           If this object has not been not registered for a port,
           then the instance for that port is not instantiated."
    ::= { t11NsRegEntry 5 }

t11NsRegNodeIpAddress OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE (0 | 16))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The IP address of the node of this Nx_Port, in
           network-byte order, either as a 32-bit IPv4 address or
           a 128-bit IPv6 address.  For the former, the leftmost 96 bits
           (12 bytes) should contain x'00 00 00 00 00 00 00 00 00 00 FF
           FF', and the IPv4 address should be present in the rightmost
           32 bits.

           Note that the value of this object is the IP address value
           that is received in the FC-GS-4 message Register IP address
           (Node) RIP_NN.  It is not validated against any IP address
           format.

           If no 'IP address (Node)' has been registered, then the
           value of this object is the zero-length string."
    REFERENCE
          "ANSI INCITS 387-2004, Fibre Channel - Generic
           Services-4 (FC-GS-4)"
    DEFVAL  { ''H }
    ::= { t11NsRegEntry 6 }

t11NsRegProcAssoc OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE (0 | 8))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The Fibre Channel Initial Process Associator (IPA).

           If no 'Initial Process Associator' has been registered,
           then the value of this object is the zero-length string."
    REFERENCE
          "ANSI INCITS 387-2004, Fibre Channel - Generic
           Services-4 (FC-GS-4)"
    DEFVAL  { ''H }
    ::= { t11NsRegEntry 7 }





t11NsRegFc4Type OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE (0 | 32))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The FC-4 protocol types supported by this Nx_Port.
           This is an array of 256 bits.  Each bit in the array
           corresponds to a Type value as defined by Fibre Channel
           standards and contained in the Type field of the frame
           header.  The order of the bits in the 256-bit (32-byte)
           value is the same as defined in FC-GS-4, section 5.2.3.8,
           and represented in network-byte order.

           If no 'FC-4 TYPEs' has been registered, then the
           value of this object is the zero-length string."
    REFERENCE
           "ANSI INCITS 387-2004, Fibre Channel - Generic
           Services-4 (FC-GS-4), section 5.2.3.8."
    DEFVAL  { ''H }
    ::= { t11NsRegEntry 8 }

t11NsRegPortType OBJECT-TYPE
    SYNTAX        FcPortType
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The port type of this port.

           If no 'Port Type' has been registered, then the value
           of this object is unidentified and is represented by
           the value 'unknown'."
    DEFVAL  { 1 }                -- 'unknown', see [FC-MGMT]
    ::= { t11NsRegEntry 9 }

t11NsRegPortIpAddress OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE (0 | 16))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The value that Fibre Channel calls an 'IP Address (Port)'
           that represents the IP address of the associated port.
           The value is either in 32-bit IPv4 format or 128-bit IPv6
           format, in network-byte order.  When this object contains an
           IPv4 address, the leftmost 96 bits (12 bytes) should contain
           x'00 00 00 00 00 00 00 00 00 00 FF FF'.  The IPv4 address
           should be present in the rightmost 32 bits.

           Note that the value of this object is the IP address value





           that is received in the FC-GS-4 message Register IP address
           (Port) RIPP_ID.  It is not validated against any IP address
           format.

           If no 'IP address (Port)' has been registered, then the
           value of this object is the zero-length string."
    REFERENCE
           "ANSI INCITS 387-2004, Fibre Channel - Generic
           Services-4, (FC-GS-4)"
    DEFVAL {''H}
    ::= { t11NsRegEntry 10 }

t11NsRegFabricPortName OBJECT-TYPE
    SYNTAX        FcNameIdOrZero
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The Fabric Port Name (WWN) of the Fx_Port to which
           this Nx_Port is attached.

           If no 'Fabric Port Name' has been registered, then the
           value of this object is the zero-length string."
    DEFVAL {''H}
    ::= { t11NsRegEntry 11 }

t11NsRegHardAddress OBJECT-TYPE
    SYNTAX        FcAddressIdOrZero
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The format of this object is identical to the format
           of Hard Address defined in the Discover Address (ADISC)
           Extended Link Service (FC-FS).

           Hard Address is the 24-bit NL_Port identifier that
           consists of:
             - the 8-bit Domain_ID in the most significant byte
             - the 8-bit Area_ID in the next most significant
               byte
             - the 8-bit AL-PA (Arbitrated Loop Physical Address)
               which an NL_Port attempts acquire during FC-AL
               initialization in the least significant byte.

           If the port is not an NL_Port, or if it is an NL_Port
           but does not have a hard address, then all bits are
           reported as zeros.

           If no 'Hard Address' has been registered, then the





           value of this object is the zero-length string."
    DEFVAL {''H}
    ::= { t11NsRegEntry 12 }

t11NsRegSymbolicPortName OBJECT-TYPE
    SYNTAX        SnmpAdminString (SIZE (0..255))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The user-defined name of this port.

           If no 'Symbolic Port Name' has been registered, then
           the value of this object is the zero-length string."
    DEFVAL {''H}
    ::= { t11NsRegEntry 13 }

t11NsRegSymbolicNodeName OBJECT-TYPE
    SYNTAX        SnmpAdminString (SIZE (0..255))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The user-defined name of the node of this port.

           If no 'Symbolic Node Name' has been registered, then
           the value of this object is the zero-length string."
    DEFVAL {''H}
    ::= { t11NsRegEntry 14 }


t11NsRegFc4Features OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE (0 | 128))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The FC-4 Features associated with FC-4 Types on this
           port encoded as a 128-byte value in network-byte order,
           or the zero-length string if no 'FC-4 Features' have been
           registered.

           Section 5.2.3.15 of FC-GS-4 is the authoritative
           definition of the format of the 128-byte value,
           i.e., if different, FC-GS-4 takes precedence over the
           following description:

           The 128-byte value is an array of 4-bit values, one for
           each FC-4 Type value, positioned as follows: the 5 most
           significant bits of a Type value identify where it appears
           within the 128-byte value, specifically, within which word:





                 - Word 0 (of the 128-byte value) contains information
                   related to Types '00' through '07';
                 - Word 1 contains information related to Types
                   '08' through 0F';
                 - and so forth, up to Word 31, which contains
                   information related to Types 'F8' through 'FF'.

           The least significant of the eight 4-bit values in each
           Word represents an FC-4 Type with 000 as its 3 least
           significant bits, and most significant 4-bit value in
           each Word represents an FC-4 Type with 111 as its 3 least
           significant bits."
    REFERENCE
           "ANSI INCITS 387-2004, Fibre Channel - Generic
           Services-4 (FC-GS-4), section 5.2.3.15."
    DEFVAL {''H}
    ::= { t11NsRegEntry 15 }


--
-- Registered FC-4 Descriptors
--

t11NsRegFc4DescriptorTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF T11NsRegFc4DescriptorEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "This table contains entries for all FC-4 Descriptors
           registered in the identified Name Server Information
           Subsets across all Fabrics for which such subsets
           contain information."
    ::= { t11NsStatus 3 }

t11NsRegFc4DescriptorEntry OBJECT-TYPE
    SYNTAX        T11NsRegFc4DescriptorEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "An entry in the t11NsRegFc4DescriptorTable,
           containing information about an FC-4 Descriptor
           that is associated with a particular FC-4 Type
           value.  The particular FC-4 Descriptor was
           registered by an Nx_Port (identified by
           t11NsRegPortIdentifier) in a Name Server Information
           Subset (identified by t11NsInfoSubsetIndex) within
           the Fibre Channel management instance (identified by
           fcmInstanceIndex) on the Fabric (identified by





           t11NsRegFabricIndex).

           If no FC-4 Descriptors have been registered
           for a particular port, then there will be no
           entries in this table for that port."
    INDEX { fcmInstanceIndex, t11NsInfoSubsetIndex,
            t11NsRegFabricIndex, t11NsRegPortIdentifier,
            t11NsRegFc4TypeValue }
    ::= { t11NsRegFc4DescriptorTable 1 }

T11NsRegFc4DescriptorEntry ::= SEQUENCE {
    t11NsRegFc4TypeValue           Unsigned32,
    t11NsRegFc4Descriptor          OCTET STRING
}

t11NsRegFc4TypeValue OBJECT-TYPE
    SYNTAX          Unsigned32 (0..255)
    MAX-ACCESS      not-accessible
    STATUS          current
    DESCRIPTION
           "An integer value that identifies an FC-4 Type value
           (representing a particular protocol type, as specified
           in FC-FS) for which an FC-4 Descriptor has been
           registered.

           An instance of this object contains a 'Type value'
           that corresponds to a '1' bit in the value of the
           t11NsRegFc4Type registered for the same port;
           this correspondence is as specified in FC-GS-4."
    REFERENCE
           "ANSI INCITS 387-2004, Fibre Channel - Generic
              Services-4 (FC-GS-4), section 5.2.3.8, and
           ANSI INCITS 373-2003, Fibre Channel - Framing and
              Signaling (FC-FS), section 9.6, Table 29."
    ::= { t11NsRegFc4DescriptorEntry 1 }

t11NsRegFc4Descriptor OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE (0..255))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The FC-4 Descriptor value that has been registered
           for the particular port on the particular Fabric, and
           for the FC-4 Type represented by the corresponding
           value of t11NsRegFc4TypeIndex.

           The format of an FC-4 Descriptor is dependent on the
           corresponding FC-4 Type value, but is represented in





           network-byte order."
    REFERENCE
           "ANSI INCITS 387-2004, Fibre Channel - Generic
           Services-4 (FC-GS-4), section 5.2.5.42"
    ::= { t11NsRegFc4DescriptorEntry 2 }


--
-- Name Server per-Fabric Statistics
--

t11NsStatsTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF T11NsStatsEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "This table contains per-Fabric state and statistics
           for operations upon the identified Name Server
           Information Subsets."
    ::= { t11NsStatistics 1 }

t11NsStatsEntry OBJECT-TYPE
    SYNTAX        T11NsStatsEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "An entry in this table contains state and statistics
           for operations upon a Name Server Information Subset
           (identified by t11NsInfoSubsetIndex) within the Fibre
           Channel management instance (identified by
           fcmInstanceIndex) on the Fabric (identified by
           t11NsRegFabricIndex)."
    INDEX { fcmInstanceIndex, t11NsInfoSubsetIndex,
            t11NsRegFabricIndex }
    ::= { t11NsStatsTable 1 }

T11NsStatsEntry ::=  SEQUENCE {
    t11NsInGetReqs                Counter32,
    t11NsOutGetReqs               Counter32,
    t11NsInRegReqs                Counter32,
    t11NsInDeRegReqs              Counter32,
    t11NsInRscns                  Counter32,
    t11NsOutRscns                 Counter32,
    t11NsRejects                  Counter32,
    t11NsDatabaseFull             TruthValue
 }

t11NsInGetReqs OBJECT-TYPE





    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The total number of (CT_IU) Get Requests
           received requesting information from this Name
           Server Information Subset on this Fabric.

           This counter has no discontinuities other than those
           that all Counter32s have when sysUpTime=0."
    ::= { t11NsStatsEntry 1 }

t11NsOutGetReqs OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The total number of (CT_IU) Get Requests sent in
           order to obtain information needed in this Name Server
           Information Subset on this Fabric.

           This counter has no discontinuities other than those
           that all Counter32s have when sysUpTime=0."
    ::= { t11NsStatsEntry 2 }

t11NsInRegReqs OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The total number of (CT_IU) Registration Requests
           received to register information in the Name Server
           Information Subset on this Fabric.

           This counter has no discontinuities other than those
           that all Counter32s have when sysUpTime=0."
    ::= { t11NsStatsEntry 3 }

t11NsInDeRegReqs OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The total number of (CT_IU) De-registration Requests
           received to de-register information from this Name Server
           Information Subset on this Fabric.

           This counter has no discontinuities other than those





           that all Counter32s have when sysUpTime=0."
    ::= { t11NsStatsEntry 4 }

t11NsInRscns OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The total number of received RSCNs, indicating
           Name Server-related changes relating to this Name
           Server Information Subset on this Fabric.

           This counter has no discontinuities other than those
           that all Counter32s have when sysUpTime=0."
    ::= { t11NsStatsEntry 5 }

t11NsOutRscns OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The total number of transmitted RSCNs, indicating
           Name Server-related changes relating to this Name
           Server Information Subset on this Fabric.

           This counter has no discontinuities other than those
           that all Counter32s have when sysUpTime=0."
    ::= { t11NsStatsEntry 6 }

t11NsRejects OBJECT-TYPE
    SYNTAX        Counter32
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The total number of CT_IU Requests for Name
           Server functions on this Name Server Information
           Subset on this Fabric that were rejected.

           This counter has no discontinuities other than those
           that all Counter32s have when sysUpTime=0."
    ::= { t11NsStatsEntry 7 }

t11NsDatabaseFull OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "An indication of whether the database containing this





           Name Server Information Subset is full.  This object is
           set to 'true' only if the Name Server is unable to allocate
           space for a new entry for the corresponding Fabric, and it is
           set to 'false' whenever an existing entry is deleted for the
           corresponding Fabric."
    ::= { t11NsStatsEntry 8 }

--
-- Reject information objects
--

t11NsRejectTable OBJECT-TYPE
    SYNTAX        SEQUENCE OF T11NsRejectEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "This table contains information about the most recent
           Name Server Registration Request failures for various
           ports on various Fabrics.

           If no information is available about the most recent
           rejection of a Registration Request on a particular port
           on a particular Fabric, then there will no entry in this
           table for that port and Fabric.

           When a t11NsRejectRegNotify notification is sent for
           such a Registration Request failure, the values of the
           objects in the relevant entry of this table are updated
           immediately prior to generating the notification."
    ::= { t11NsStatus 4 }

t11NsRejectEntry OBJECT-TYPE
    SYNTAX T11NsRejectEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
           "An entry containing information about the most recent
           rejection of a request to register information in the Name
           Server Information Subset (identified by
           t11NsInfoSubsetIndex) within the Fibre Channel management
           instance (identified by fcmInstanceIndex) for a particular
           port (identified by t11NsRegPortIdentifier) on a particular
           Fabric (identified by t11NsRegFabricIndex)."
    INDEX { fcmInstanceIndex, t11NsInfoSubsetIndex,
            t11NsRegFabricIndex, t11NsRegPortIdentifier }
    ::= { t11NsRejectTable 1 }

T11NsRejectEntry ::= SEQUENCE {





    t11NsRejectCtCommandString   OCTET STRING,
    t11NsRejectReasonCode        T11NsGs4RejectReasonCode,
    t11NsRejReasonCodeExp        T11NsRejReasonCodeExpl,
    t11NsRejReasonVendorCode     OCTET STRING
}

t11NsRejectCtCommandString OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE (0..255))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "The binary content of the Registration Request,
           formatted as an octet string (in network byte
           order) containing the CT_IU, as described in
           Table 2 of [FC-GS-4] (including the preamble),
           which was most recently rejected for the particular
           Name Server Information Subset on the particular port
           on the particular Fabric.

           This object contains the zero-length string
           if and when the CT-IU's content is unavailable.

           When the length of this object is 255 octets, it
           contains the first 255 octets of the CT-IU (in
           network-byte order)."
    ::= { t11NsRejectEntry 1 }

t11NsRejectReasonCode OBJECT-TYPE
    SYNTAX        T11NsGs4RejectReasonCode
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "A registration reject reason code.  This object
           contains the reason code of the most recent Name
           Server Registration Request failure for the
           particular port on the particular Fabric."
    ::= { t11NsRejectEntry 2 }

t11NsRejReasonCodeExp OBJECT-TYPE
    SYNTAX        T11NsRejReasonCodeExpl
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "A registration reject reason code explanation.  This
           object contains the reason code explanation of the most
           recent Name Server Registration Request failure for the
           particular port on the particular Fabric."
    ::= { t11NsRejectEntry 3 }





t11NsRejReasonVendorCode OBJECT-TYPE
    SYNTAX        OCTET STRING (SIZE(1))
    MAX-ACCESS    read-only
    STATUS        current
    DESCRIPTION
           "A registration reject vendor-specific code.  This
           object contains the vendor-specific code of the most
           recent Name Server Registration Request failure for the
           particular port on the particular Fabric."
    ::= { t11NsRejectEntry 4 }


--
-- Notifications
--

t11NsRejectRegNotify NOTIFICATION-TYPE
    OBJECTS   { t11FamLocalSwitchWwn,
                t11NsRegPortName, t11NsRejectCtCommandString,
                t11NsRejectReasonCode, t11NsRejReasonCodeExp,
                t11NsRejReasonVendorCode }
    STATUS    current
    DESCRIPTION
           "This notification is generated whenever a request to
           register information in a Name Server Information
           Subset (for which the corresponding instance of
           t11NsInfoSubsetRejReqNotfyEnable is 'true') is
           rejected on a particular Fabric for a particular Nx_Port.

           The value of t11FamLocalSwitchWwn indicates the
           WWN of the switch that received the request.
           (If the WWN is unavailable, the value is set to
           the zero-length string.)

           The value of t11NsRejectCtCommandString indicates
           the rejected request, and the values of
           t11NsRejectReasonCode, t11NsRejReasonCodeExp, and
           t11NsRejReasonVendorCode indicate the reason for
           the rejection.

           The value of t11NsRegPortName represents the Port Name
           if it is able to be extracted out of the Registration
           Request, or otherwise the value as currently registered
           on the port."
    ::= { t11NsNotifications 1 }

--
-- Conformance





--

t11NsMIBCompliances OBJECT IDENTIFIER ::= {t11NsMIBConformance 1}
t11NsMIBGroups      OBJECT IDENTIFIER ::= {t11NsMIBConformance 2}

t11NsMIBCompliance MODULE-COMPLIANCE
    STATUS    current
    DESCRIPTION
           "The compliance statement for entities that
           implement the Fibre Channel Name Server."
    MODULE MANDATORY-GROUPS {t11NsDBGroup,
                             t11NsNotifyControlGroup,
                             t11NsNotifyGroup}

      OBJECT t11NsInfoSubsetRejReqNotfyEnable
      MIN-ACCESS read-only
      DESCRIPTION
             "Write access is not required."

      GROUP t11NsRequestStatsGroup
      DESCRIPTION
             "This group is mandatory only for an implementation
             that captures statistics related to Name Server
             requests."

      GROUP t11NsRscnStatsGroup
      DESCRIPTION
             "This group is mandatory only for an implementation
             that captures statistics related to Name
             Server-related RSCNs."

      GROUP t11NsRejectStatsGroup
      DESCRIPTION
             "This group is mandatory only for an implementation
             that captures statistics related to Name Server
             rejects."

    ::= { t11NsMIBCompliances 1 }

-- Units of conformance

t11NsDBGroup        OBJECT-GROUP
    OBJECTS { t11NsInfoSubsetSwitchIndex,
              t11NsInfoSubsetTableLastChange,
              t11NsInfoSubsetNumRows,
              t11NsRegPortName,
              t11NsRegNodeName,
              t11NsRegClassOfSvc,





              t11NsRegNodeIpAddress,
              t11NsRegProcAssoc,
              t11NsRegFc4Type,
              t11NsRegPortType,
              t11NsRegPortIpAddress,
              t11NsRegFabricPortName,
              t11NsRegHardAddress,
              t11NsRegSymbolicPortName,
              t11NsRegSymbolicNodeName,
              t11NsRegFc4Features,
              t11NsRegFc4Descriptor }
    STATUS current
    DESCRIPTION
           "A collection of objects for monitoring the information
           registered in a Name Server Information Subset."
    ::= { t11NsMIBGroups 1 }

t11NsRequestStatsGroup OBJECT-GROUP
    OBJECTS { t11NsInGetReqs,
              t11NsOutGetReqs,
              t11NsInRegReqs,
              t11NsInDeRegReqs,
              t11NsDatabaseFull}
    STATUS current
    DESCRIPTION
           "A collection of objects for displaying Name
           Server statistics and state for Name Server requests."
    ::= { t11NsMIBGroups 2 }

t11NsRscnStatsGroup OBJECT-GROUP
    OBJECTS { t11NsInRscns,
              t11NsOutRscns }
    STATUS current
    DESCRIPTION
           "A collection of objects for displaying Name
           Server statistics for Name Server-related RSCNs."
    ::= { t11NsMIBGroups 3 }

t11NsRejectStatsGroup OBJECT-GROUP
    OBJECTS { t11NsInfoSubsetTotalRejects,
              t11NsRejects }
    STATUS current
    DESCRIPTION
           "A collection of objects for displaying Name
           Server statistics for rejects."
    ::= { t11NsMIBGroups 4 }

t11NsNotifyControlGroup  OBJECT-GROUP





    OBJECTS { t11NsRejectCtCommandString,
              t11NsRejectReasonCode,
              t11NsRejReasonCodeExp,
              t11NsRejReasonVendorCode,
              t11NsInfoSubsetRejReqNotfyEnable }
    STATUS current
    DESCRIPTION
           "A collection of notification control and
           notification information objects for monitoring
           rejections of Name Server registrations."
    ::= { t11NsMIBGroups 5 }

t11NsNotifyGroup        NOTIFICATION-GROUP
    NOTIFICATIONS {t11NsRejectRegNotify }
    STATUS current
    DESCRIPTION
           "A collection of notifications for monitoring
           rejections of Name Server registrations."
    ::= { t11NsMIBGroups 6 }

END


