OLSRv2-MIB DEFINITIONS ::= BEGIN


   IMPORTS

      MODULE-IDENTITY, OBJECT-TYPE, Counter32, Counter64,
      Integer32, Unsigned32, mib-2, TimeTicks,
      NOTIFICATION-TYPE
               FROM SNMPv2-SMI -- RFC 2578

      TEXTUAL-CONVENTION, TimeStamp, TruthValue
               FROM SNMPv2-TC -- RFC 2579

      MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
               FROM SNMPv2-CONF -- STD 58

      InetAddressType, InetAddress,
      InetAddressPrefixLength
               FROM INET-ADDRESS-MIB -- RFC 4001

      nhdpInterfaceEntry,
      nhdpIibLinkSetEntry, nhdpIib2HopSetEntry,
      nhdpNibNeighborSetEntry, nhdpInterfacePerfEntry
               FROM NHDP-MIB -- RFC 6779

      IANAolsrv2LinkMetricTypeTC
               FROM IANA-OLSRv2-LINK-METRIC-TYPE-MIB
      ;

   manetOlsrv2MIB MODULE-IDENTITY
      LAST-UPDATED "201404090000Z"   -- 09 April 2014
      ORGANIZATION "IETF MANET Working Group"
      CONTACT-INFO
         "WG E-Mail: manet@ietf.org

          WG Chairs: sratliff@cisco.com
                     jmacker@nrl.navy.mil

          Editors:   Ulrich Herberg
                     Fujitsu Laboratories of America
                     1240 East Arques Avenue
                     Sunnyvale, CA 94085
                     USA






                     Email: ulrich@herberg.name
                     URI: http://www.herberg.name/

                     Thomas Heide Clausen
                     Ecole Polytechnique
                     LIX
                     91128 Palaiseau Cedex
                     France
                     Email: T.Clausen@computer.org
                     URI: http://www.thomasclausen.org/

                     Robert G. Cole
                     US Army CERDEC
                     Space and Terrestrial Communications
                     6010 Frankford Street
                     Bldg 6010, Room 453H
                     Aberdeen Proving Ground, MD 21005
                     USA
                     Phone: +1 443 395-8744
                     Email: robert.g.cole@us.army.mil
                     URI: http://www.cs.jhu.edu/~rgcole"

      DESCRIPTION
         "This OLSRv2-MIB module is applicable to routers
          implementing the Optimized Link State Routing
          Protocol version 2 (OLSRv2) defined in RFC 7181.

          Copyright (c) 2014 IETF Trust and the persons
          identified as authors of the code.  All rights reserved.

          Redistribution and use in source and binary forms, with
          or without modification, is permitted pursuant to, and
          subject to the license terms contained in, the Simplified
          BSD License set forth in Section 4.c of the IETF Trust's
          Legal Provisions Relating to IETF Documents
          (http://trustee.ietf.org/license-info).

          This version of this MIB module is part of RFC 7184; see
          the RFC itself for full legal notices."

        -- Revision History
        REVISION    "201404090000Z"   -- 09 April 2014
        DESCRIPTION
         "Initial version of this MIB module,
          published as RFC 7184."

        ::= { mib-2 219 }






--
-- TEXTUAL CONVENTIONS
--

Olsrv2MetricValueCompressedFormTC ::= TEXTUAL-CONVENTION
   DISPLAY-HINT "d"
   STATUS      current
   DESCRIPTION
      "OLSRv2 Metrics are expressed in terms of a Link Metric
       Compressed Form within the OLSRv2 protocol.  This textual
       convention defines the syntax of the metric objects
       consistent with the definitions of the OLSRv2 Link
       Metric Compressed Form in Section 6.2 of RFC 7181.

       The 12-bit compressed form of a link metric uses a modified
       form of a representation with an 8-bit mantissa (denoted a)
       and a 4-bit exponent (denoted b).  Note that if represented
       as the 12-bit value 256b+a, then the ordering of those 12-bit
       values is identical to the ordering of the represented values.

       The value so represented is (257+a)2^b - 256, where ^ denotes
       exponentiation.  This has a minimum value
       (when a = 0 and b = 0) of MINIMUM_METRIC = 1 and a maximum
       value (when a = 255 and b = 15) of MAXIMUM_METRIC = 2^24 - 256.

       Hence, the metric values so represented range from 1 to
       16776960.  The special value of 0 is reserved for the
       UNKNOWN_METRIC value.

       If a network manager sets the metric value 'm' through the
       MIB module, then the OLSRv2 code can both use this value
       and derive a compressed representation of 'm' (as used in
       messages) as specified in Section 6.2 of RFC7181.
       The value 'm' is persistently stored by the MIB module.
       If the MIB module is pulling this metric's value from some other
       source, e.g., the protocol instance, then this value is stored
       as is."
   SYNTAX  Unsigned32 (0..16776960)

Olsrv2TimeValueCompressedForm32TC ::= TEXTUAL-CONVENTION
   DISPLAY-HINT "x"
   STATUS      current
   DESCRIPTION
      "OLSRv2 time values may be expressed in terms of a compressed
       form within the OLSRv2 protocol.  This textual convention
       defines the syntax of the time objects defined in terms of
       an integer number of milliseconds, consistent with the
       definitions of the 8-bit exponent-mantissa compressed form





       defined in Section 5 of RFC 5497.  Time values with this
       representation are defined in terms of a constant C, which
       is represented in terms of seconds.  The constant C
       (time granularity) is used as specified in RFC 5497.
       It MUST be the same as is used by NHDP (RFC 6130).

       The 8-bit compressed form of a time value uses a modified
       form of a representation with a 3-bit mantissa (denoted a)
       and a 5-bit exponent (denoted b).  Note that if represented
       as the 8-bit value 8b+a, then the ordering of those 8-bit
       values is identical to the ordering of the represented values.

       The minimum time value that can be represented in this manner
       is C.  The maximum time value that can be represented in
       this manner is 15 * 2^28 * C, 15*268,435,456 * C,
       4,026,531,840 * C, or about 45 days if, for example,
       C = 1/1024 second.

       This TEXTUAL-CONVENTION limits the maximum value of the
       time granularity constant C to be no greater than 1/1024
       seconds due to its use of the Unsigned32 syntax limiting
       the maximum number of milliseconds to no more than
       3932160000.

       When OLSRv2 uses this 8-bit exponent-mantissa compressed
       form, this object value MUST be translated from the
       integer form represented in this MIB module into the
       exponent-mantissa form for the OLSRv2 protocol to use
       according to the algorithm defined in Section 5 of
       RFC 5497 for finding the next larger time value within
       the exponent-mantissa format.

       If a network manager sets the time value 't' through the
       MIB module, then the OLSRv2 code can derive
       'compressed_t' = T(a,b) according to the algorithm
       in RFC 5497 and 'compressed_t' is the value represented
       in the OLSRv2 messages.  But, the value 't' is persistently
       stored by the MIB module.  If the MIB module is pulling
       this time parameter from some other source that is using
       the compressed form, i.e., the protocol instance, then
       this value is stored as is, after converting from
       number of time constants C into number of milliseconds."
   SYNTAX  Unsigned32 (1..3932160000)

Olsrv2StatusTC ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Controls the operation of the OLSRv2





       protocol on the device or a specific interface.
       For example, for an interface, 'enabled' indicates
       that OLSRv2 is permitted to operate,
       and 'disabled' indicates that it is not."
   SYNTAX  INTEGER {
      enabled (1),
      disabled (2)
   }

WillingnessTC ::= TEXTUAL-CONVENTION
   DISPLAY-HINT "x"
   STATUS    current
   DESCRIPTION
      "A willingness value that evaluates to the
       device's interest in participating in
       a particular function, process, or behavior.

       The willingness ranges from a low value of
       WILL_NEVER(0) to a high value of
       WILL_ALWAYS(15).  For each parameter x,
       there is an associated willingness value
       W(x) such that WILL_NEVER < W(x) <= WILL_ALWAYS."
   SYNTAX   Unsigned32 (0..15)


--
-- Top-Level Object Identifier Assignments
--

olsrv2MIBNotifications OBJECT IDENTIFIER ::= { manetOlsrv2MIB 0 }
olsrv2MIBObjects       OBJECT IDENTIFIER ::= { manetOlsrv2MIB 1 }
olsrv2MIBConformance   OBJECT IDENTIFIER ::= { manetOlsrv2MIB 2 }

--
-- olsrv2ConfigurationGroup
--

--    Contains the OLSRv2 objects that configure specific
--    options that determine the overall performance and operation
--    of the OLSRv2 routing process.

olsrv2ConfigurationGroup OBJECT IDENTIFIER ::= {olsrv2MIBObjects 1}


   olsrv2AdminStatus  OBJECT-TYPE
      SYNTAX      Olsrv2StatusTC
      MAX-ACCESS  read-write
      STATUS      current





      DESCRIPTION
         "The configured status of the OLSRv2 process
          on this device.  'enabled(1)' means that
          OLSRv2 is configured to run on this device.
          'disabled(2)' mean that the OLSRv2 process
          is configured off.

          Operation of the OLSRv2 protocol
          requires the operation of the Neighborhood
          Discovery Protocol (RFC 6130).  Hence, this
          object cannot have a status of 'enabled'
          unless at least one interface on the device
          is a MANET interface with NHDP enabled on that
          interface.  If a network manager attempts to
          set this object to 'enabled' when no interfaces
          on this device have NHDP enabled, the device
          MUST fail the set with inconsistentValue.
          If all device interfaces running NHDP become
          disabled or removed, then the
          olsrv2AdminStatus MUST be 'disabled'.

          If the network manager, or other means, sets
          this object to 'disabled', then the associated
          interface specific objects, i.e., the
          olsrv2InterfaceAdminStatus objects MUST all
          be 'disabled'.

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      DEFVAL { disabled }
   ::= { olsrv2ConfigurationGroup 1 }

   olsrv2InterfaceTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF Olsrv2InterfaceEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The olsrv2InterfaceTable describes the OLSRv2
          status on the NHDP interfaces of this router.
          As such, this table augments the nhdpInterfaceTable
          defined in the NHDP-MIB (RFC 6779).  NHDP interfaces
          are explicitly defined by network management, command
          line interface (CLI) or other means for interfaces on
          the device that are intended to run MANET protocols.
          The olsrv2InterfaceTable contains a single object: the
          olsrv2InterfaceAdminStatus object.  This
          object is set by network management, or by





          other means, e.g., CLI.

          A conceptual row in this table exists if and only
          if a corresponding entry in the nhdpInterfaceTable
          exists.  If the corresponding entry with nhdpIfIndex
          value is deleted from the nhdpInterfaceTable, then
          the entry in this table is automatically deleted and
          OLSRv2 is disabled on this interface,
          and all configuration and state information
          related to this interface is to be removed
          from memory.

          The olsrv2InterfaceAdminStatus can only be
          'enabled' if the corresponding olsrv2AdminStatus
          object is also set to 'enabled'."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2ConfigurationGroup 2 }

   olsrv2InterfaceEntry OBJECT-TYPE
      SYNTAX      Olsrv2InterfaceEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The olsrv2InterfaceEntry describes one OLSRv2
          local interface configuration as indexed by
          its nhdpIfIndex, as defined in the
          NHDP-MIB (RFC 6779).

          The objects in this table are persistent, and when
          written, the device SHOULD save the change to
          non-volatile storage.  For further information
          on the storage behavior for these objects, refer
          to the description for the nhdpIfRowStatus
          object in the NHDP-MIB (RFC6779)."
      REFERENCE
         "RFC 6779 - Definition of Managed Objects for
          the Neighborhood Discovery Protocol,
          Herberg, U., Cole, R.G., and I. Chakeres,
          October 2012"
      AUGMENTS { nhdpInterfaceEntry }
   ::= { olsrv2InterfaceTable 1 }

   Olsrv2InterfaceEntry ::=
      SEQUENCE {
         olsrv2InterfaceAdminStatus





            Olsrv2StatusTC
      }

   olsrv2InterfaceAdminStatus OBJECT-TYPE
      SYNTAX      Olsrv2StatusTC
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The OLSRv2 interface's administrative status.
          The value 'enabled(1)' denotes that the interface
          is permitted to participate in the OLSRv2 routing
          process.  The value 'disabled(2)' denotes that
          the interface is not permitted to participate
          in the OLSRv2 routing process.

          The configuration objects for the OLSRv2 routing
          process, other than the administrative status objects,
          are common to all interfaces on this device.
          As such, the OLSRv2 configuration objects are globally
          defined for the device and are not contained within
          the olsrv2InterfaceTable."
      DEFVAL { disabled }
   ::= { olsrv2InterfaceEntry 1 }

   olsrv2OrigIpAddrType  OBJECT-TYPE
       SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
          "The type of the olsrv2OrigIpAddr, as defined
           in the InetAddress MIB module (RFC 4001).

           Only the values 'ipv4(1)' and
           'ipv6(2)' are supported."
       REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2ConfigurationGroup 3 }

   olsrv2OrigIpAddr  OBJECT-TYPE
       SYNTAX      InetAddress (SIZE(4|16))
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
          "The router's originator address.  An address that
           is unique (within the MANET) to this router.






           This object is persistent, and when written,
           the entity SHOULD save the change to
           non-volatile storage."
       REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2ConfigurationGroup 4 }

   --
   -- Local History Times
   --

   olsrv2OHoldTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2OHoldTime corresponds to
         O_HOLD_TIME of OLSRv2, and represents the
         time for which a recently used and replaced
         originator address is used to recognize the router's
         own messages.

         Guidance for setting this object may be found
         in Section 5 of the OLSRv2 specification (RFC 7181),
         which indicates that:
             o  olsrv2OHoldTime > 0

         This object is persistent, and when written,
         the entity SHOULD save the change to
         non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 30000 }
   ::= { olsrv2ConfigurationGroup 5 }


   --
   -- Message intervals
   --

   olsrv2TcInterval  OBJECT-TYPE
      SYNTAX      Olsrv2TimeValueCompressedForm32TC





      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2TcInterval corresponds to
         TC_INTERVAL of OLSRv2 and represents the
         maximum time between the transmission of
         two successive TC messages by this router.

         Guidance for setting this object may be found
         in Section 5 of the OLSRv2 specification (RFC 7181),
         which indicates that:

             o olsrv2TcInterval > 0
             o olsrv2TcInterval >= olsrv2TcMinInterval

         This object is persistent, and when written,
         the entity SHOULD save the change to
         non-volatile storage."
      REFERENCE
         "Section 5 on Representing Time.
          RFC 5497 - Representing Multi-Value Time in
          Mobile Ad Hoc Networks (MANETs),
          Clausen, T. and C. Dearlove, March 2009.

          and

          Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 5000 }
   ::= { olsrv2ConfigurationGroup 6 }

   olsrv2TcMinInterval  OBJECT-TYPE
      SYNTAX      Olsrv2TimeValueCompressedForm32TC
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2TcMinInterval corresponds to
         TC_MIN_INTERVAL of OLSRv2 and represents
         the minimum interval between transmission of
         two successive TC messages by this router.

         Guidance for setting this object may be found
         in Section 5 of the OLSRv2 specification (RFC 7181),
         which indicates that:





             o olsrv2TcInterval >= olsrv2TcMinInterval

         The OLSRv2 protocol may choose to represent this
         time interval in terms of the 8-bit exponent-mantissa
         form defined in Section 5 of RFC 5497.  When this
         is the case, this object value MUST be translated
         from the integer form represented in this
         MIB module into the exponent-mantissa form for the
         OLSRv2 protocol to use according to the algorithm
         defined in Section 5 of RFC 5497 for finding the
         next larger time value within the exponent-mantissa
         format.

         This object is persistent, and when written,
         the entity SHOULD save the change to
         non-volatile storage."
      REFERENCE
         "Section 5 on Representing Time.
          RFC 5497 - Representing Multi-Value Time in
          Mobile Ad Hoc Networks (MANETs),
          Clausen, T. and C. Dearlove, March 2009.

          and

          Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 1250 }
   ::= { olsrv2ConfigurationGroup 7 }


   --
   -- Advertised information validity times
   --

   olsrv2THoldTime  OBJECT-TYPE
      SYNTAX      Olsrv2TimeValueCompressedForm32TC
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2THoldTime corresponds to
         T_HOLD_TIME of OLSRv2 and is used as the
         minimum value in the TLV with
         Type = VALIDITY_TIME included in all
         TC messages sent by this router.






         Guidance for setting this object may be found
         in Section 5 of the OLSRv2 specification (RFC 7181),
         which indicates that:
             o olsrv2THoldTime >= olsrv2TcInterval
             o If TC messages can be lost, then
               olsrv2THoldTime SHOULD be
               significantly greater than olsrv2TcInterval;
               a value >= 3 x olsrv2TcInterval is RECOMMENDED.

         This object is persistent, and when written,
         the entity SHOULD save the change to
         non-volatile storage."
      REFERENCE
         "Section 5 on Representing Time.
          RFC 5497 - Representing Multi-Value Time in
          Mobile Ad Hoc Networks (MANETs),
          Clausen, T. and C. Dearlove, March 2009.

          and

          Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 15000 }
   ::= { olsrv2ConfigurationGroup 8 }

   olsrv2AHoldTime  OBJECT-TYPE
      SYNTAX      Olsrv2TimeValueCompressedForm32TC
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2AHoldTime corresponds to
         A_HOLD_TIME of OLSRv2 and represents
         the period during which TC messages are sent
         after they no longer have any advertised
         information to report, but are sent in order
         to accelerate outdated information removal by other
         routers.

         Guidance for setting this object may be found
         in Section 5 of the OLSRv2 specification (RFC 7181),
         which indicates that:
            o If TC messages can be lost, then
              olsrv2AHoldTime SHOULD be
              significantly greater than olsrv2TcInterval;
              a value >= 3 x olsrv2TcInterval is





              RECOMMENDED.

         This object is persistent, and when written,
         the entity SHOULD save the change to
         non-volatile storage."
      REFERENCE
         "Section 5 on Representing Time.
          RFC 5497 - Representing Multi-Value Time in
          Mobile Ad Hoc Networks (MANETs),
          Clausen, T. and C. Dearlove, March 2009.

          and

          Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 15000 }
   ::= { olsrv2ConfigurationGroup 9 }

   --
   -- Received message validity times
   --

   olsrv2RxHoldTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2RxHoldTime corresponds to
          RX_HOLD_TIME of OLSRv2 and represents the period
          after receipt of a message by the appropriate OLSRv2
          interface of this router for which that information
          is recorded, in order that the message is recognized
          as having been previously received on this OLSRv2
          interface.

          Guidance for setting this object may be found
          in Section 5 of the OLSRv2 specification (RFC 7181),
          which indicates that:
             o olsrv2RxHoldTime > 0
             o This parameter SHOULD be greater
               than the maximum difference in time that a
               message may take to traverse the MANET,
               taking into account any message forwarding
               jitter as well as propagation, queuing,
               and processing delays.





          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 30000 }
   ::= { olsrv2ConfigurationGroup 10 }

   olsrv2PHoldTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2PHoldTime corresponds to
          P_HOLD_TIME of OLSRv2 and represents the period
          after receipt of a message that is processed by
          this router for which that information is recorded,
          in order that the message is not processed again
          if received again.

          Guidance for setting this object may be found
          in Section 5 of the OLSRv2 specification (RFC 7181),
          which indicates that:
             o olsrv2PHoldTime > 0
             o This parameter SHOULD be greater
               than the maximum difference in time that a
               message may take to traverse the MANET,
               taking into account any message forwarding
               jitter as well as propagation, queuing,
               and processing delays.

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 30000 }
   ::= { olsrv2ConfigurationGroup 11 }

   olsrv2FHoldTime  OBJECT-TYPE
      SYNTAX      Unsigned32





      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2FHoldTime corresponds to
          F_HOLD_TIME of OLSRv2 and represents the period
          after receipt of a message that is forwarded by this
          router for which that information is recorded, in order
          that the message is not forwarded again if received again.

          Guidance for setting this object may be found
          in Section 5 of the OLSRv2 specification (RFC 7181),
          which indicates that:
             o olsrv2FHoldTime > 0
             o This parameter SHOULD be greater
               than the maximum difference in time that a
               message may take to traverse the MANET,
               taking into account any message forwarding
               jitter as well as propagation, queuing,
               and processing delays.

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 30000 }
   ::= { olsrv2ConfigurationGroup 12 }

   --
   -- Jitter times
   --

   olsrv2TpMaxJitter  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2TpMaxJitter corresponds to
          TP_MAXJITTER of OLSRv2 and represents the value
          of MAXJITTER used in RFC 5148 for periodically
          generated TC messages sent by this router.

          For constraints on these parameters, see RFC 5148.





          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 500 }
   ::= { olsrv2ConfigurationGroup 13 }

   olsrv2TtMaxJitter  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2TtMaxJitter corresponds to
          TT_MAXJITTER of OLSRv2 and represents the value
          of MAXJITTER used in RFC 5148 for externally
          triggered TC messages sent by this router.

          For constraints on these parameters, see RFC 5148.

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 500 }
   ::= { olsrv2ConfigurationGroup 14 }

   olsrv2FMaxJitter  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2FMaxJitter corresponds to
          F_MAXJITTER of OLSRv2 and represents the
          default value of MAXJITTER used in RFC 5148 for
          messages forwarded by this router.

          For constraints on these parameters, see RFC 5148.






          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 500 }
   ::= { olsrv2ConfigurationGroup 15 }

   --
   -- Hop limits
   --

   olsrv2TcHopLimit  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..255)
      UNITS       "hops"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2TcHopLimit corresponds to
          TC_HOP_LIMIT of OLSRv2.

          Guidance for setting this object may be found
          in Section 5 of the OLSRv2 specification (RFC 7181),
          which indicates that:
             o The maximum value of
               olsrv2TcHopLimit >= the network diameter
               in hops, a value of 255 is RECOMMENDED.
             o olsrv2TcHopLimit >= 2.

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
       REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
       DEFVAL { 255 }
   ::= { olsrv2ConfigurationGroup 16 }

   --
   -- Willingness
   --

   olsrv2WillRouting  OBJECT-TYPE





      SYNTAX      WillingnessTC
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2WillRouting corresponds to
          WILL_ROUTING of OLSRv2.

          Guidance for setting this object may be found
          in Section 5 of the OLSRv2 specification (RFC 7181),
          which indicates that:
             o WILL_NEVER (0) <= olsrv2WillRouting <=
                                  WILL_ALWAYS (15)

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 7 }
   ::= { olsrv2ConfigurationGroup 17 }

   olsrv2WillFlooding     OBJECT-TYPE
      SYNTAX      WillingnessTC
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2WillFlooding corresponds to
          WILL_FLOODING of OLSRv2.

          Guidance for setting this object may be found
          in Section 5 of the OLSRv2 specification (RFC 7181),
          which indicates that:
             o WILL_NEVER (0) <= olsrv2WillFlooding <=
                                  WILL_ALWAYS (15)

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { 7 }
   ::= { olsrv2ConfigurationGroup 18 }





   olsrv2LinkMetricType  OBJECT-TYPE
      SYNTAX      IANAolsrv2LinkMetricTypeTC
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2LinkMetricType corresponds to
          LINK_METRIC_TYPE of OLSRv2.

          If olsrv2LinkMetricType changes, then all
          link metric information recorded by this router
          is invalid.  The router MUST take the
          actions described in Section 5.5.
          'Parameter Change Constraints' and
          Section 17 'Information Base Changes'
          in RFC 7181.

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters.
          RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      DEFVAL { unknown }
   ::= { olsrv2ConfigurationGroup 19 }

--
-- olsrv2StateGroup
--

--
-- Contains information describing the current state of
-- the OLSRv2 process.
--

olsrv2StateGroup  OBJECT IDENTIFIER ::= { olsrv2MIBObjects 2 }

   --
   -- Interface Information Base (IIB)
   --

   --
   -- Link Set from RFC 6130, extended by L_in_metric,
   -- L_out_metric, and L_mpr_selector entries for each tuple
   --

   olsrv2IibLinkSetTable OBJECT-TYPE





      SYNTAX       SEQUENCE OF Olsrv2IibLinkSetEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
         "A Link Set of an interface records all links
          from other routers that are, or recently
          were, 1-hop neighbors."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 1 }

   olsrv2IibLinkSetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2IibLinkSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A Link Set consists of Link Tuples, each
          representing a single link indexed by the
          local and remote interface pair.  Each Link Set
          from NHDP is extended by OLSRv2 by the following
          fields:

          (L_in_metric (olsrv2IibLinkSetInMetricValue),
           L_out_metric (olsrv2IibLinkSetOutMetricValue),
           L_mpr_selector (olsrv2IibLinkSetMprSelector))"
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      AUGMENTS { nhdpIibLinkSetEntry }
   ::= { olsrv2IibLinkSetTable 1 }

   Olsrv2IibLinkSetEntry ::=
      SEQUENCE {
         olsrv2IibLinkSetInMetricValue
            Olsrv2MetricValueCompressedFormTC,
         olsrv2IibLinkSetOutMetricValue
            Olsrv2MetricValueCompressedFormTC,
         olsrv2IibLinkSetMprSelector
            TruthValue
      }

   olsrv2IibLinkSetInMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current





      DESCRIPTION
         "olsrv2IibLinkSetInMetricValue is the metric of the link
          from the OLSRv2 interface with addresses
          L_neighbor_iface_addr_list to this OLSRv2 interface.
          The L_neighbor_iface_addr_list is identified by
          the nhdpDiscIfIndex, which is an index to the
          nhdpIibLinkSetTable, which this table augments."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2IibLinkSetEntry 1 }

   olsrv2IibLinkSetOutMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "olsrv2IibLinkSetOutMetricValue is the metric of the
          link to the OLSRv2 interface with addresses
          L_neighbor_iface_addr_list from this OLSRv2 interface.
          The L_neighbor_iface_addr_list is identified by
          the nhdpDiscIfIndex, which is an index to the
          nhdpIibLinkSetTable, which this table augments."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2IibLinkSetEntry 2 }

   olsrv2IibLinkSetMprSelector  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "olsrv2IibLinkSetMprSelector is a boolean flag,
          recording whether this neighbor has selected this router
          as a flooding MPR, i.e., is a flooding MPR selector
          of this router."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2IibLinkSetEntry 3 }

   --
   -- 2-Hop Set; from RFC 6130, extended by OLSRv2 by the
   -- following fields: N2_in_metric, N2_out_metric





   --

   olsrv2Iib2HopSetTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF Olsrv2Iib2HopSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A 2-Hop Set of an interface records network
          addresses of symmetric 2-hop neighbors, and
          the symmetric links to symmetric 1-hop neighbors
          through which these symmetric 2-hop neighbors
          can be reached.  It consists of 2-Hop Tuples."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 2 }

   olsrv2Iib2HopSetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2Iib2HopSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "olsrv2Iib2HopSetTable consists of 2-Hop Tuples,
          each representing a single network address of
          a symmetric 2-hop neighbor and a single MANET
          interface of a symmetric 1-hop neighbor.
          Each 2-Hop Set from NHDP is extended by
          OLSRv2 by the following fields:

          (N2_in_metric (olsrv2Iib2HopSetInMetricValue),
           N2_out_metric (olsrv2Iib2HopSetOutMetricValue))"
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      AUGMENTS { nhdpIib2HopSetEntry }
   ::= { olsrv2Iib2HopSetTable 1 }

   Olsrv2Iib2HopSetEntry ::=
      SEQUENCE {
         olsrv2Iib2HopSetInMetricValue
            Olsrv2MetricValueCompressedFormTC,
         olsrv2Iib2HopSetOutMetricValue
            Olsrv2MetricValueCompressedFormTC
      }

   olsrv2Iib2HopSetInMetricValue  OBJECT-TYPE





      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "olsrv2Iib2HopSetInMetricValue is the neighbor
          metric from the router with address
          N2_2hop_iface_addr to the router
          with OLSRv2 interface addresses
          N2_neighbor_iface_addr_list.

          The N2_2hop_iface_addr is identified by the
          (nhdpIib2HopSetIpAddressType,
          nhdpIib2HopSetIpAddress) pair from the
          nhdpIibLinkSetTable, which this table augments.

          The N2_neighbor_iface_addr_list is defined by
          the nhdpDiscIfIndex, which is an index of the
          nhdpIibLinkSetTable, which this table augments."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014.

          and

          RFC 6779 - Definition of Managed Objects for the
          Neighborhood Discovery Process, Herberg, U.,
          Cole, R., and I. Chakeres, October 2012."
   ::= { olsrv2Iib2HopSetEntry 1 }

   olsrv2Iib2HopSetOutMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "olsrv2Iib2HopSetOutMetricValue is the neighbor metric
          to the router with address N2_2hop_iface_addr
          from the router with OLSRv2 interface addresses
          N2_neighbor_iface_addr_list.

          The N2_2hop_iface_addr is identified by the
          (nhdpIib2HopSetIpAddressType,
          nhdpIib2HopSetIpAddress) pair from the
          nhdpIibLinkSetTable, which this table augments.

          The N2_neighbor_iface_addr_list is defined by
          the nhdpDiscIfIndex, which is an index of the
          nhdpIibLinkSetTable, which this table augments."





      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014.

          and

          RFC 6779 - Definition of Managed Objects for the
          Neighborhood Discovery Process, Herberg, U.,
          Cole, R., and I. Chakeres, October 2012."
   ::= { olsrv2Iib2HopSetEntry 2 }

   --
   -- Local Information Base  - as defined in RFC 6130,
   -- extended by the addition of an Originator Set,
   -- defined in Section 6.1 and a Local Attached
   -- Network Set, defined in Section 6.2.
   --

   --
   -- Originator Set
   --

   olsrv2LibOrigSetTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF Olsrv2LibOrigSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Originator Set records addresses
          that were recently used as originator addresses
          by this router."
       REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 3 }

   olsrv2LibOrigSetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2LibOrigSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Originator Set consists of
          Originator Tuples:

          (O_orig_addr (olsrv2LibOrigSetIpAddrType
           and olsrv2LibOrigSetIpAddr),
           O_time (olsrv2LibOrigSetExpireTime))."





      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      INDEX { olsrv2LibOrigSetIpAddrType,
              olsrv2LibOrigSetIpAddr }
   ::= { olsrv2LibOrigSetTable 1 }

   Olsrv2LibOrigSetEntry ::=
      SEQUENCE {
         olsrv2LibOrigSetIpAddrType
            InetAddressType,
         olsrv2LibOrigSetIpAddr
            InetAddress,
         olsrv2LibOrigSetExpireTime
            TimeStamp
      }

   olsrv2LibOrigSetIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2LibOrigSetIpAddr,
          as defined in the InetAddress MIB (RFC4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2LibOrigSetEntry 1 }

   olsrv2LibOrigSetIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "An originator address recently employed
          by this router."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2LibOrigSetEntry 2 }

   olsrv2LibOrigSetExpireTime  OBJECT-TYPE





      SYNTAX      TimeStamp
      UNITS      "centiseconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "olsrv2LibOrigSetExpireTime specifies the value
          of sysUptime when this entry SHOULD expire and be
          removed from the olsrv2LibOrigSetTable.  This time
          is determined at the time the entry is added,
          derived from the following expression:

             O_time := current time + O_HOLD_TIME

          where O_time is olsrv2LibOrigSetExpireTime,
          current_time is current sysUptime, and
          O_HOLD_TIME is a parameter of the OLSRv2
          protocol.  In the event that the
          O_HOLD_TIME is changed, the
          olsrv2LibOrigSetExpireTime needs to be
          recomputed for each of the entries in this table."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2LibOrigSetEntry 3 }

   --
   -- Local Attached Network Set
   --

   olsrv2LibLocAttNetSetTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF Olsrv2LibLocAttNetSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Local Attached Network Set records
          its local non-OLSRv2 interfaces via which it
          can act as a gateway to other networks."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 4 }

   olsrv2LibLocAttNetSetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2LibLocAttNetSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current





      DESCRIPTION
         "The entries include the Local Attached
          Network Tuples:

          (AL_net_addr (olsrv2LibLocAttNetSetIpAddr),
           AL_dist (olsrv2LibLocAttNetSetDistance),
           AL_metric (olsrv2LibLocAttNetSetMetricValue)
          )

          where:

             AL_net_addr is the network address
             of an attached network that can
             be reached via this router.  The
             AL_net_addr is defined in this MIB
             module by the tuple
             (olsrv2LibLocAttNetSetIpAddrType,
              olsrv2LibLocAttNetSetIpAddr,
              olsrv2LibLocAttNetSetIpAddrPrefixLen).

             AL_dist is the number of hops to
             the network with address AL_net_addr
             from this router.  The AL_dist is
             defined in this MIB module by the
             olsrv2LibLocAttNetSetDistance object.

             AL_metric is the metric of the link to
             the attached network with address
             AL_net_addr from this router.  The
             AL_metric is defined in this MIB module
             by the olsrv2LibLocAttNetSetMetricValue
             object.

          OLSRv2 (RFC 7181) defines the rules for managing
          entries within this table, e.g., populating
          and purging entries.  Specific instructions for the
          olsrv2LibLocAttNetSetEntry(s) are found in
          Sections 7.2 and 17 of OLSRv2 (RFC 7181)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      INDEX { olsrv2LibLocAttNetSetIpAddrType,
              olsrv2LibLocAttNetSetIpAddr,
              olsrv2LibLocAttNetSetIpAddrPrefixLen }
   ::= { olsrv2LibLocAttNetSetTable 1 }

   Olsrv2LibLocAttNetSetEntry ::=





      SEQUENCE {
         olsrv2LibLocAttNetSetIpAddrType
            InetAddressType,
         olsrv2LibLocAttNetSetIpAddr
            InetAddress,
         olsrv2LibLocAttNetSetIpAddrPrefixLen
            InetAddressPrefixLength,
         olsrv2LibLocAttNetSetDistance
            Unsigned32,
         olsrv2LibLocAttNetSetMetricValue
            Olsrv2MetricValueCompressedFormTC
      }

   olsrv2LibLocAttNetSetIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2LibLocAttNetSetIpAddr, as defined
          in the InetAddress MIB (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2LibLocAttNetSetEntry 1 }

   olsrv2LibLocAttNetSetIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This is the network address of an attached
          network that can be reached via this router."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2LibLocAttNetSetEntry 2 }

   olsrv2LibLocAttNetSetIpAddrPrefixLen  OBJECT-TYPE
      SYNTAX      InetAddressPrefixLength
      UNITS       "bits"
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION





         "Indicates the number of leading one bits that form the
          mask to be logically ANDed with the destination address
          before being compared to the value in the
          olsrv2LibLocAttNetSetIpAddr field."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2LibLocAttNetSetEntry 3 }

   olsrv2LibLocAttNetSetDistance  OBJECT-TYPE
      SYNTAX      Unsigned32 (1..255)
      UNITS       "hops"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object specifies the number of hops
          to the network with address
          olsrv2LibLocAttNetSetIpAddr from this router."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2LibLocAttNetSetEntry 4 }

   olsrv2LibLocAttNetSetMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object specifies the metric of the
          link to the attached network with
          address AL_net_addr from this router.  The
          AL_net_addr is defined by the tuple
          (olsrv2LibLocAttNetSetIpAddrType,
           olsrv2LibLocAttNetSetIpAddr,
           olsrv2LibLocAttNetSetIpAddrPrefixLen)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2LibLocAttNetSetEntry 5 }

   --
   -- Neighbor Information Base
   --

   --





   -- Neighbor Set - as defined in RFC 6130,
   -- extended by OLSRv2 by the addition of the following
   -- elements to each Neighbor Tuple:
   --     N_orig_addr (olsrv2NibNeighborSetNOrigIpAddrType,
   --                  olsrv2NibNeighborSetNOrigIpAddr)
   --     N_in_metric (olsrv2NibNeighborSetNInMetricValue)
   --     N_out_metric (olsrv2NibNeighborSetNOutMetricValue)
   --     N_will_flooding (olsrv2NibNeighborSetNWillFlooding)
   --     N_will_routing (olsrv2NibNeighborSetNWillRouting)
   --     N_flooding_mpr (olsrv2NibNeighborSetNFloodingMpr)
   --     N_routing_mpr (olsrv2NibNeighborSetNRoutingMpr)
   --     N_mpr_selector (olsrv2NibNeighborSetNMprSelector)
   --     N_advertised (olsrv2NibNeighborSetNAdvertised)
   --

   olsrv2NibNeighborSetTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF Olsrv2NibNeighborSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Neighbor Set records all network
          addresses of each 1-hop neighbor.  It consists
          of Neighbor Tuples, each representing a single
          1-hop neighbor."
       REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
    ::= { olsrv2StateGroup 5 }

    olsrv2NibNeighborSetEntry  OBJECT-TYPE
       SYNTAX      Olsrv2NibNeighborSetEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
          "Each Neighbor Tuple in the Neighbor Set, defined
           in RFC 6130, has these additional elements:
              N_orig_addr (olsrv2NibNeighborSetNOrigIpAddrType,
                           olsrv2NibNeighborSetNOrigIpAddr)
              N_in_metric (olsrv2NibNeighborSetNInMetricValue)
              N_out_metric (olsrv2NibNeighborSetNOutMetricValue)
              N_will_flooding (olsrv2NibNeighborSetNWillFlooding)
              N_will_routing (olsrv2NibNeighborSetNWillRouting)
              N_flooding_mpr (olsrv2NibNeighborSetNFloodingMpr)
              N_routing_mpr (olsrv2NibNeighborSetNRoutingMpr)
              N_mpr_selector (olsrv2NibNeighborSetNMprSelector)
              N_advertised (olsrv2NibNeighborSetNAdvertised)
           defined here as extensions."





       REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
       AUGMENTS { nhdpNibNeighborSetEntry }
   ::= { olsrv2NibNeighborSetTable 1 }

   Olsrv2NibNeighborSetEntry ::=
      SEQUENCE {
         olsrv2NibNeighborSetNOrigIpAddrType
            InetAddressType,
         olsrv2NibNeighborSetNOrigIpAddr
            InetAddress,
         olsrv2NibNeighborSetNInMetricValue
            Olsrv2MetricValueCompressedFormTC,
         olsrv2NibNeighborSetNOutMetricValue
            Olsrv2MetricValueCompressedFormTC,
         olsrv2NibNeighborSetNWillFlooding
            WillingnessTC,
         olsrv2NibNeighborSetNWillRouting
            WillingnessTC,
         olsrv2NibNeighborSetNFloodingMpr
            TruthValue,
         olsrv2NibNeighborSetNRoutingMpr
            TruthValue,
         olsrv2NibNeighborSetNMprSelector
            TruthValue,
         olsrv2NibNeighborSetNAdvertised
            TruthValue
      }

   olsrv2NibNeighborSetNOrigIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2NibNeighborSetNOrigIpAddr, as defined
          in the InetAddress MIB module (RFC4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 1 }

   olsrv2NibNeighborSetNOrigIpAddr  OBJECT-TYPE





      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This is the originator IP address of the neighbor
          represented by this table entry."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 2 }

   olsrv2NibNeighborSetNInMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is the neighbor metric of any
          link from this neighbor to an OLSRv2 interface
          of this router, i.e., the minimum of all corresponding
          L_in_metric (olsrv2IibLinkSetInMetricValue)
          with L_status = SYMMETRIC and
          L_in_metric (olsrv2IibLinkSetInMetricValue) != UNKNOWN_METRIC,
          UNKNOWN_METRIC if there are no such Link Tuples.
          UNKNOWN_METRIC has a value of 0."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 3 }

   olsrv2NibNeighborSetNOutMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is the neighbor metric of any
          link from an OLSRv2 interface of this router
          to this neighbor, i.e., the minimum of all
          corresponding L_out_metric
          (olsrv2IibLinkSetOutMetricValue) with L_status =
          SYMMETRIC and L_out_metric
          (olsrv2IibLinkSetOutMetricValue) != UNKNOWN_METRIC,
          UNKNOWN_METRIC if there are no such Link Tuples.
          UNKNOWN_METRIC has a value of 0."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,





          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 4 }

   olsrv2NibNeighborSetNWillFlooding  OBJECT-TYPE
      SYNTAX      WillingnessTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is the neighbor's willingness to be
          selected as a flooding MPR, in the range from
          WILL_NEVER to WILL_ALWAYS, both inclusive, taking
          the value WILL_NEVER if no OLSRv2 specific
          information is received from this neighbor."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 5 }

   olsrv2NibNeighborSetNWillRouting  OBJECT-TYPE
      SYNTAX      WillingnessTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is the neighbor's willingness to be
          selected as a routing MPR, in the range from
          WILL_NEVER to WILL_ALWAYS, both inclusive, taking
          the value WILL_NEVER if no OLSRv2 specific
          information is received from this neighbor."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 6 }

   olsrv2NibNeighborSetNFloodingMpr  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is a boolean flag, recording whether
          this neighbor is selected as a flooding MPR
          by this router."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 7 }





   olsrv2NibNeighborSetNRoutingMpr  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is a boolean flag, recording whether
          this neighbor is selected as a routing MPR
          by this router."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 8 }

   olsrv2NibNeighborSetNMprSelector  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is a boolean flag,
          recording whether this neighbor has selected this router
          as a routing MPR, i.e., is a routing MPR
          selector of this router.

          When set to 'true', then this router is selected as
          a routing MPR by the neighbor router.
          When set to 'false',
          then this router is not selected by the neighbor
          as a routing MPR."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NibNeighborSetEntry 9 }

   olsrv2NibNeighborSetNAdvertised  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object, N_mpr_selector
          (olsrv2NibNeighborSetNMprSelector), is a boolean flag,
          recording whether this router has elected to
          advertise a link to this neighbor in its TC messages."
       REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."





   ::= { olsrv2NibNeighborSetEntry 10 }

   olsrv2NibNeighborSetTableAnsn OBJECT-TYPE
      SYNTAX      Unsigned32 (0..65535)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Advertised Neighbor Sequence Number (ANSN), is
          a variable, whose value is included in TC messages to
          indicate the freshness of the information transmitted."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 6 }

   --
   -- Topology Information Base - this Information
   -- Base is specific to OLSRv2 and is defined in
   -- Section 10 of RFC 7181.
   --

   --
   -- Advertising Remote Router Set
   --

   olsrv2TibAdRemoteRouterSetTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF Olsrv2TibAdRemoteRouterSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Advertising Remote Router Set records
          information describing each remote router in the
          network that transmits TC messages."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 7 }

   olsrv2TibAdRemoteRouterSetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2TibAdRemoteRouterSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Advertised Neighbor Set Table entry
          consists of Advertising Remote Router Tuples:






          (AR_orig_addr (olsrv2TibAdRemoteRouterSetIpAddrType,
                         olsrv2TibAdRemoteRouterSetIpAddr),
           AR_seq_number (olsrv2TibAdRemoteRouterSetMaxSeqNo),
           AR_time (olsrv2TibAdRemoteRouterSetExpireTime).

          Addresses associated with this router are
          found in the NHDP-MIB module's nhdpDiscIfSetTable.

          OLSRv2 (RFC 7181) defines the rules for managing
          entries within this table, e.g., populating
          and purging entries.  Specific instructions for the
          olsrv2TibAdRemoteRouterSetEntry(s) are found in
          Section 10.1 and Section 17 of OLSRv2 (RFC 7181)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      INDEX { olsrv2TibAdRemoteRouterSetIpAddrType,
              olsrv2TibAdRemoteRouterSetIpAddr }
   ::= { olsrv2TibAdRemoteRouterSetTable 1 }

   Olsrv2TibAdRemoteRouterSetEntry ::=
      SEQUENCE {
         olsrv2TibAdRemoteRouterSetIpAddrType
            InetAddressType,
         olsrv2TibAdRemoteRouterSetIpAddr
            InetAddress,
         olsrv2TibAdRemoteRouterSetMaxSeqNo
            Unsigned32,
         olsrv2TibAdRemoteRouterSetExpireTime
            TimeStamp
      }

   olsrv2TibAdRemoteRouterSetIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibAdRemoteRouterSetIpAddr,
          as defined in the InetAddress MIB module (RFC4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAdRemoteRouterSetEntry 1 }





   olsrv2TibAdRemoteRouterSetIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This is the originator address of a received
          TC message."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAdRemoteRouterSetEntry 2 }

   olsrv2TibAdRemoteRouterSetMaxSeqNo  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..65535)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This is the greatest Advertised Neighbor Sequence
          Number (ANSN) in any TC message
          received that originated from the router
          with originator address
          olsrv2TibAdRemoteRouterSetIpAddr.

          Sequence numbers are used in the OLSRv2 protocol
          for the purpose of discarding 'old' information,
          i.e., messages received out of order.  However,
          with a limited number of bits for representing
          sequence numbers, wraparound (that the sequence
          number is incremented from the maximum possible
          value to zero) will occur.  To prevent this from
          interfering with the operation of this protocol,
          OLSRv2 implementations observe the following when
          determining the ordering of sequence numbers.

          In OLSRv2, MAXVALUE designates one more than the
          largest possible value for a sequence number.
          For a 16-bit sequence number, MAXVALUE is 65536.

          The sequence number S1 is said to be 'greater than'
          the sequence number S2 if:

             o  S1 > S2 AND S1 - S2 < MAXVALUE/2 OR

             o  S2 > S1 AND S2 - S1 > MAXVALUE/2

          When sequence numbers S1 and S2 differ by MAXVALUE/2,
          their ordering cannot be determined.  In this case,





          which should not occur, either ordering may be
          assumed.

          Thus, when comparing two messages, it is possible
          - even in the presence of wraparound - to determine
          which message contains the most recent information."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAdRemoteRouterSetEntry 3 }

   olsrv2TibAdRemoteRouterSetExpireTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      UNITS       "centiseconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "olsrv2TibAdRemoteRouterSetExpireTime specifies the value
          of sysUptime when this entry SHOULD expire and be
          removed from the olsrv2TibAdRemoteRouterSetTable."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAdRemoteRouterSetEntry 4 }

   --
   -- Router Topology Set
   --

   olsrv2TibRouterTopologySetTable OBJECT-TYPE
      SYNTAX       SEQUENCE OF Olsrv2TibRouterTopologySetEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
         "A router's Router Topology Set records topology
          information about the network."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 8 }

   olsrv2TibRouterTopologySetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2TibRouterTopologySetEntry
      MAX-ACCESS  not-accessible
      STATUS      current





      DESCRIPTION
         "It consists of Router Topology Tuples:

          (TR_from_orig_addr
             (olsrv2TibRouterTopologySetFromOrigIpAddrType,
              olsrv2TibRouterTopologySetFromOrigIpAddr),
           TR_to_orig_addr
             (olsrv2TibRouterTopologySetToOrigIpAddrType,
              olsrv2TibRouterTopologySetToOrigIpAddr),
           TR_seq_number (olsrv2TibRouterTopologySetSeqNo),
           TR_metric (olsrv2TibRouterTopologySetMetricValue),
           TR_time (olsrv2TibRouterTopologySetExpireTime)).

          OLSRv2 (RFC 7181) defines the rules for managing
          entries within this table, e.g., populating
          and purging entries.  Specific instructions for the
          olsrv2TibRouterTopologySetEntry(s) are found in
          Section 10.2 and Section 17 of OLSRv2 (RFC 7181)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      INDEX { olsrv2TibRouterTopologySetFromOrigIpAddrType,
              olsrv2TibRouterTopologySetFromOrigIpAddr,
              olsrv2TibRouterTopologySetToOrigIpAddrType,
              olsrv2TibRouterTopologySetToOrigIpAddr }
   ::= { olsrv2TibRouterTopologySetTable 1 }

   Olsrv2TibRouterTopologySetEntry ::=
      SEQUENCE {
         olsrv2TibRouterTopologySetFromOrigIpAddrType
            InetAddressType,
         olsrv2TibRouterTopologySetFromOrigIpAddr
            InetAddress,
         olsrv2TibRouterTopologySetToOrigIpAddrType
            InetAddressType,
         olsrv2TibRouterTopologySetToOrigIpAddr
            InetAddress,
         olsrv2TibRouterTopologySetSeqNo
            Unsigned32,
         olsrv2TibRouterTopologySetMetricValue
            Olsrv2MetricValueCompressedFormTC,
         olsrv2TibRouterTopologySetExpireTime
            TimeStamp
      }

   olsrv2TibRouterTopologySetFromOrigIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }





      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibRouterTopologySetFromOrigIpAddr,
          as defined in the InetAddress MIB module (RFC4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRouterTopologySetEntry 1 }

   olsrv2TibRouterTopologySetFromOrigIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This is the originator address of a router that can
          reach the router with originator address TR_to_orig_addr
          in one hop."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRouterTopologySetEntry 2 }

   olsrv2TibRouterTopologySetToOrigIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibRouterTopologySetToOrigIpAddr,
          as defined in the InetAddress MIB module (RFC4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRouterTopologySetEntry 3 }

   olsrv2TibRouterTopologySetToOrigIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current





      DESCRIPTION
         "This is the originator address of a router that can be
          reached by the router with originator address
          TR_to_orig_addr in one hop."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRouterTopologySetEntry 4 }

   olsrv2TibRouterTopologySetSeqNo  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..65535)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This is the greatest Advertised Neighbor Sequence
          Number (ANSN) in any TC message
          received that originated from the router
          with originator address TR_from_orig_addr,
          i.e., that contributed to the information
          contained in this Tuple and that is defined by the
          objects:
             (olsrv2TibRouterTopologySetFromOrigIpAddrType,
              olsrv2TibRouterTopologySetFromOrigIpAddr).

          Sequence numbers are used in the OLSRv2 protocol
          for the purpose of discarding 'old' information,
          i.e., messages received out of order.  However,
          with a limited number of bits for representing
          sequence numbers, wraparound (that the sequence
          number is incremented from the maximum possible
          value to zero) will occur.  To prevent this from
          interfering with the operation of this protocol,
          OLSRv2 implementations observe the following when
          determining the ordering of sequence numbers.

          In OLSRv2, MAXVALUE designates one more than the
          largest possible value for a sequence number.
          For a 16-bit sequence number, MAXVALUE is 65536.

          The sequence number S1 is said to be 'greater than'
          the sequence number S2 if:

             o  S1 > S2 AND S1 - S2 < MAXVALUE/2 OR

             o  S2 > S1 AND S2 - S1 > MAXVALUE/2

          When sequence numbers S1 and S2 differ by MAXVALUE/2,





          their ordering cannot be determined.  In this case,
          which should not occur, either ordering may be
          assumed.

          Thus, when comparing two messages, it is possible
          - even in the presence of wraparound - to determine
          which message contains the most recent information."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRouterTopologySetEntry 5 }

   olsrv2TibRouterTopologySetMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This is the neighbor metric from the router
          with originator address TR_from_orig_addr
          (olsrv2TibRouterTopologySetFromOrigIpAddrType,
          olsrv2TibRouterTopologySetFromOrigIpAddr) to
          the router with originator address TR_to_orig_addr
          (olsrv2TibRouterTopologySetToOrigIpAddrType,
          olsrv2TibRouterTopologySetToOrigIpAddr)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRouterTopologySetEntry 6 }

   olsrv2TibRouterTopologySetExpireTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      UNITS       "centiseconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "olsrv2TibRouterTopologySetExpireTime specifies the value
          of sysUptime when this entry SHOULD expire and be
          removed from the olsrv2TibRouterTopologySetTable."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRouterTopologySetEntry 7 }

   --
   -- Routable Address Topology Set





   --

   olsrv2TibRoutableAddressTopologySetTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF Olsrv2TibRoutableAddressTopologySetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Routable Address Topology Set records topology
          information about the routable addresses within the MANET,
          including via which routers they may be reached."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 9 }

   olsrv2TibRoutableAddressTopologySetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2TibRoutableAddressTopologySetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "It consists of Router Topology Tuples:

          (TA_from_orig_addr
               (olsrv2TibRoutableAddressTopologySetFromOrigIpAddrType
                olsrv2TibRoutableAddressTopologySetFromOrigIpAddr),
           TA_dest_addr
               (olsrv2TibRoutableAddressTopologySetFromDestIpAddrType
                olsrv2TibRoutableAddressTopologySetFromDestIpAddr),
           TA_seq_number (olsrv2TibRoutableAddressTopologySetSeqNo)
           TA_metric (olsrv2TibRoutableAddressTopologySetMetricValue)
           TA_time (olsrv2TibRoutableAddressTopologySetExpireTime)
          )

          OLSRv2 (RFC 7181) defines the rules for managing
          entries within this table, e.g., populating
          and purging entries.  Specific instructions for the
          olsrv2TibRoutableAddressTopologySetEntry(s) are found
          in Section 10.3 and Section 17 of OLSRv2 (RFC 7181)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      INDEX { olsrv2TibRoutableAddressTopologySetFromOrigIpAddrType,
              olsrv2TibRoutableAddressTopologySetFromOrigIpAddr,
              olsrv2TibRoutableAddressTopologySetDestIpAddrType,
              olsrv2TibRoutableAddressTopologySetDestIpAddr }
   ::= { olsrv2TibRoutableAddressTopologySetTable 1 }





    Olsrv2TibRoutableAddressTopologySetEntry ::=
       SEQUENCE {
          olsrv2TibRoutableAddressTopologySetFromOrigIpAddrType
            InetAddressType,
          olsrv2TibRoutableAddressTopologySetFromOrigIpAddr
            InetAddress,
          olsrv2TibRoutableAddressTopologySetDestIpAddrType
            InetAddressType,
          olsrv2TibRoutableAddressTopologySetDestIpAddr
            InetAddress,
          olsrv2TibRoutableAddressTopologySetSeqNo
            Unsigned32,
          olsrv2TibRoutableAddressTopologySetMetricValue
            Olsrv2MetricValueCompressedFormTC,
          olsrv2TibRoutableAddressTopologySetExpireTime
            TimeStamp
       }

   olsrv2TibRoutableAddressTopologySetFromOrigIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the
          olsrv2TibRoutableAddressTopologySetFromOrigIpAddr,
          as defined in the InetAddress MIB module (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutableAddressTopologySetEntry 1 }

   olsrv2TibRoutableAddressTopologySetFromOrigIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This is the originator address of a router that can
          reach the router with routable address TA_dest_addr
          in one hop."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutableAddressTopologySetEntry 2 }





   olsrv2TibRoutableAddressTopologySetDestIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibRouterTopologySetToOrigIpAddr,
          as defined in the InetAddress MIB module (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutableAddressTopologySetEntry 3 }

   olsrv2TibRoutableAddressTopologySetDestIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This is a routable address of a router that can be
          reached by the router with originator address
          TA_from_orig_addr in one hop.  The TA_from_orig_addr
          is defined by the tuple
          (olsrv2TibRoutableAddressTopologySetFromOrigIpAddrType
           olsrv2TibRoutableAddressTopologySetFromOrigIpAddr)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutableAddressTopologySetEntry 4 }

   olsrv2TibRoutableAddressTopologySetSeqNo  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..65535)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This is the greatest Advertised Neighbor Sequence
          Number (ANSN) in any TC message
          received that originated from the router
          with originator address TA_from_orig_addr,
          i.e., that contributed to the information
          contained in this Tuple.  The TA_from_orig_addr
          is defined by the tuple
          (olsrv2TibRoutableAddressTopologySetFromOrigIpAddrType
           olsrv2TibRoutableAddressTopologySetFromOrigIpAddr)."
      REFERENCE





         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutableAddressTopologySetEntry 5 }

   olsrv2TibRoutableAddressTopologySetMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This is the neighbor metric from the router
          with originator address TA_from_orig_addr (defined
          by the tuple
          (olsrv2TibRoutableAddressTopologySetFromOrigIpAddrType
           olsrv2TibRoutableAddressTopologySetFromOrigIpAddr))
          to the router with OLSRv2 interface address TA_dest_addr
          (defined by the tuple
          (olsrv2TibRoutableAddressTopologySetFromDestIpAddrType
           olsrv2TibRoutableAddressTopologySetFromDestIpAddr))."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutableAddressTopologySetEntry 6 }

   olsrv2TibRoutableAddressTopologySetExpireTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      UNITS       "centiseconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "olsrv2TibRoutableAddressTopologySetExpireTime
          specifies the value of sysUptime when this entry
          SHOULD expire and be removed from the
          olsrv2TibRoutableAddressTopologySetTable."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutableAddressTopologySetEntry 7 }

   --
   -- Attached Network Set
   --

   olsrv2TibAttNetworksSetTable OBJECT-TYPE
      SYNTAX       SEQUENCE OF Olsrv2TibAttNetworksSetEntry
      MAX-ACCESS   not-accessible





      STATUS       current
      DESCRIPTION
         "A router's Attached Network Set records information
          about networks (which may be outside the MANET)
          attached to other routers and their routable addresses."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 10 }

   olsrv2TibAttNetworksSetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2TibAttNetworksSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "It consists of Attached Network Tuples:

          (AN_orig_addr
             (olsrv2TibAttNetworksSetOrigIpAddrType,
              olsrv2TibAttNetworksSetOrigIpAddr),
           AN_net_addr
             (olsrv2TibAttNetworksSetNetIpAddrType,
              olsrv2TibAttNetworksSetNetIpAddr,
              olsrv2TibAttNetworksSetNetIpAddrPrefixLen),
           AN_seq_number (olsrv2TibAttNetworksSetSeqNo),
           AN_dist (olsrv2TibAttNetworksSetDist),
           AN_metric (olsrv2TibAttNetworksSetMetricValue),
           AN_time (olsrv2TibAttNetworksSetExpireTime)
          )

          OLSRv2 (RFC 7181) defines the rules for managing
          entries within this table, e.g., populating
          and purging entries.  Specific instructions for the
          olsrv2TibRoutableAddressTopologySetEntry(s) are found
          in Section 10.4 and Section 17 of OLSRv2 (RFC 7181)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
      INDEX { olsrv2TibAttNetworksSetOrigIpAddrType,
              olsrv2TibAttNetworksSetOrigIpAddr,
              olsrv2TibAttNetworksSetNetIpAddrType,
              olsrv2TibAttNetworksSetNetIpAddr,
              olsrv2TibAttNetworksSetNetIpAddrPrefixLen }
   ::= { olsrv2TibAttNetworksSetTable 1 }

   Olsrv2TibAttNetworksSetEntry ::=





      SEQUENCE {
         olsrv2TibAttNetworksSetOrigIpAddrType
            InetAddressType,
         olsrv2TibAttNetworksSetOrigIpAddr
            InetAddress,
         olsrv2TibAttNetworksSetNetIpAddrType
            InetAddressType,
         olsrv2TibAttNetworksSetNetIpAddr
            InetAddress,
         olsrv2TibAttNetworksSetNetIpAddrPrefixLen
            InetAddressPrefixLength,
         olsrv2TibAttNetworksSetSeqNo
            Unsigned32,
         olsrv2TibAttNetworksSetDist
            Unsigned32,
         olsrv2TibAttNetworksSetMetricValue
            Olsrv2MetricValueCompressedFormTC,
         olsrv2TibAttNetworksSetExpireTime
            TimeStamp
      }

   olsrv2TibAttNetworksSetOrigIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibAttNetworksSetOrigIpAddr,
          as defined in the InetAddress MIB module (RFC4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAttNetworksSetEntry 1 }

   olsrv2TibAttNetworksSetOrigIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This is the originator address, of type
          olsrv2TibAttNetworksSetOrigIpAddrType, of a
          router that can act as gateway to the
          network with address AN_net_addr.  The
          AN_net_addr is defined by the tuple
             (olsrv2TibAttNetworksSetNetIpAddrType,





              olsrv2TibAttNetworksSetNetIpAddr,
              olsrv2TibAttNetworksSetNetIpAddrPrefixLen)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAttNetworksSetEntry 2 }

   olsrv2TibAttNetworksSetNetIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibAttNetworksSetNetIpAddr,
          as defined in the InetAddress MIB module (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAttNetworksSetEntry 3 }

   olsrv2TibAttNetworksSetNetIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This is the network address, of type
          olsrv2TibAttNetworksSetNetIpAddrType, of an
          attached network, that may be reached via
          the router with originator address AN_orig_addr.
          The AN_orig_addr is defined by the tuple
             (olsrv2TibAttNetworksSetOrigIpAddrType,
              olsrv2TibAttNetworksSetOrigIpAddr)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAttNetworksSetEntry 4 }

   olsrv2TibAttNetworksSetNetIpAddrPrefixLen  OBJECT-TYPE
      SYNTAX      InetAddressPrefixLength
      UNITS       "bits"
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION





         "Indicates the number of leading one bits that form the
          mask to be logically ANDed with the destination address
          before being compared to the value in the
          olsrv2TibAttNetworksSetNetIpAddr field."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAttNetworksSetEntry 5 }

   olsrv2TibAttNetworksSetSeqNo  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..65535)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This is the greatest Advertised Neighbor Sequence
          Number (ANSN) in any TC message received
          that originated from the router
          with originator address AN_orig_addr
          (i.e., that contributed to the information
          contained in this Tuple).  The AN_orig_addr
          is defined by the tuple
             (olsrv2TibAttNetworksSetOrigIpAddrType,
              olsrv2TibAttNetworksSetOrigIpAddr).

          Sequence numbers are used in the OLSRv2 protocol
          for the purpose of discarding 'old' information,
          i.e., messages received out of order.  However,
          with a limited number of bits for representing
          sequence numbers, wraparound (that the sequence
          number is incremented from the maximum possible
          value to zero) will occur.  To prevent this from
          interfering with the operation of this protocol,
          the following MUST be observed when determining
          the ordering of sequence numbers.

          The term MAXVALUE designates in the following one
          more than the largest possible value for a sequence
          number.  For a 16-bit sequence number (as are those
          defined in this specification), MAXVALUE is 65536.

          The sequence number S1 is said to be 'greater than'
          the sequence number S2 if:

             o  S1 > S2 AND S1 - S2 < MAXVALUE/2 OR

             o  S2 > S1 AND S2 - S1 > MAXVALUE/2






          When sequence numbers S1 and S2 differ by MAXVALUE/2,
          their ordering cannot be determined.  In this case,
          which should not occur, either ordering may be
          assumed.

          Thus, when comparing two messages, it is possible
          - even in the presence of wraparound - to determine
          which message contains the most recent information."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAttNetworksSetEntry 6 }

   olsrv2TibAttNetworksSetDist  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..255)
      UNITS       "hops"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The number of hops to the network
          with address AN_net_addr from the router with
          originator address AN_orig_addr.
          The AN_orig_addr is defined by the tuple
             (olsrv2TibAttNetworksSetOrigIpAddrType,
              olsrv2TibAttNetworksSetOrigIpAddr)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAttNetworksSetEntry 7 }

   olsrv2TibAttNetworksSetMetricValue  OBJECT-TYPE
      SYNTAX      Olsrv2MetricValueCompressedFormTC
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The metric of the link from the router with
          originator address AN_orig_addr to the attached
          network with address AN_net_addr.
          The AN_net_addr is defined by the tuple
            (olsrv2TibAttNetworksSetNetIpAddrType,
             olsrv2TibAttNetworksSetNetIpAddr,
             olsrv2TibAttNetworksSetNetIpAddrPrefixLen)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."





   ::= { olsrv2TibAttNetworksSetEntry 9 }

   olsrv2TibAttNetworksSetExpireTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      UNITS       "centiseconds"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "olsrv2TibAttNetworksSetExpireTime
          specifies the value of sysUptime when this
          entry SHOULD expire and be removed from the
          olsrv2TibAttNetworksSetTable."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibAttNetworksSetEntry 10 }

   --
   -- Routing Set
   --

   olsrv2TibRoutingSetTable OBJECT-TYPE
      SYNTAX       SEQUENCE OF Olsrv2TibRoutingSetEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
         "A router's Routing Set records the first hop along a
          selected path to each destination for which any such
          path is known."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2StateGroup 11 }

   olsrv2TibRoutingSetEntry  OBJECT-TYPE
      SYNTAX      Olsrv2TibRoutingSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "It consists of Routing Tuples:

           (R_dest_addr, R_next_iface_addr,
            R_local_iface_addr, R_dist, R_metric)"
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,





          and U. Herberg, April 2014."
      INDEX { olsrv2TibRoutingSetDestIpAddrType,
              olsrv2TibRoutingSetDestIpAddr,
              olsrv2TibRoutingSetDestIpAddrPrefixLen }
   ::= { olsrv2TibRoutingSetTable 1 }

   Olsrv2TibRoutingSetEntry ::=
      SEQUENCE {
         olsrv2TibRoutingSetDestIpAddrType
            InetAddressType,
         olsrv2TibRoutingSetDestIpAddr
            InetAddress,
         olsrv2TibRoutingSetDestIpAddrPrefixLen
            InetAddressPrefixLength,
         olsrv2TibRoutingSetNextIfIpAddrType
            InetAddressType,
         olsrv2TibRoutingSetNextIfIpAddr
            InetAddress,
         olsrv2TibRoutingSetLocalIfIpAddrType
            InetAddressType,
         olsrv2TibRoutingSetLocalIfIpAddr
            InetAddress,
         olsrv2TibRoutingSetDist
            Unsigned32,
         olsrv2TibRoutingSetMetricValue
            Unsigned32
      }

   olsrv2TibRoutingSetDestIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibRoutingSetDestIpAddr,
          as defined in the InetAddress MIB module (RFC 4001).

          Only the values 'ipv4(1)' and 'ipv6(2)' are
          supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 1 }

   olsrv2TibRoutingSetDestIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current





      DESCRIPTION
         "This is the address of the destination,
          either the address of an interface of
          a destination router or the network
          address of an attached network."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 2 }

   olsrv2TibRoutingSetDestIpAddrPrefixLen  OBJECT-TYPE
      SYNTAX      InetAddressPrefixLength
      UNITS       "bits"
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "Indicates the number of leading one bits that form the
          mask to be logically ANDed with the destination address
          before being compared to the value in the
          olsrv2TibRoutingSetDestIpAddr field.

          Note: This definition needs to be consistent
          with the current forwarding table MIB module description.
          Specifically, it SHOULD allow for longest prefix
          matching of network addresses."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 3 }

   olsrv2TibRoutingSetNextIfIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibRoutingSetNextIfIpAddr,
          as defined in the InetAddress MIB module (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 4 }






   olsrv2TibRoutingSetNextIfIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is the OLSRv2 interface address of the
          next hop on the selected path to the
          destination."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 5 }

   olsrv2TibRoutingSetLocalIfIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType { ipv4(1) , ipv6(2) }
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2TibRoutingSetLocalIfIpAddr
          and olsrv2TibRoutingSetNextIfIpAddr,
          as defined in the InetAddress MIB module (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 6 }

   olsrv2TibRoutingSetLocalIfIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is the address of the local OLSRv2
          interface over which a packet must be
          sent to reach the destination by the
          selected path."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 7 }

   olsrv2TibRoutingSetDist  OBJECT-TYPE
      SYNTAX      Unsigned32 (0..255)





      UNITS       "hops"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is the number of hops on the selected
          path to the destination."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 8 }

   olsrv2TibRoutingSetMetricValue  OBJECT-TYPE
      SYNTAX      Unsigned32(0..4294901760)
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object is the metric of the route
          to the destination with address R_dest_addr.
          The maximum value of this object can be
          256 times MAXIMUM_METRIC,
          as represented in Olsrv2MetricValueCompressedFormTC, i.e.,
          4294901760."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2TibRoutingSetEntry 9 }

--
-- OLSRv2 Performance Group
--

--
--    Contains objects that help to characterize the
--    performance of the OLSRv2 routing process.
--

olsrv2PerformanceObjGrp  OBJECT IDENTIFIER ::= {olsrv2MIBObjects 3}

    --
    -- Objects per local interface
    --

   olsrv2InterfacePerfTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF Olsrv2InterfacePerfEntry
      MAX-ACCESS  not-accessible
      STATUS      current





      DESCRIPTION
         "This table summarizes performance objects that are
          measured per each active local OLSRv2 interface.
          If the olsrv2InterfaceAdminStatus of the interface
          changes to 'disabled', then the row associated with this
          interface SHOULD be removed from this table."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2PerformanceObjGrp 1 }

   olsrv2InterfacePerfEntry OBJECT-TYPE
      SYNTAX      Olsrv2InterfacePerfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A single entry contains performance counters for
          each active local OLSRv2 interface."
      AUGMENTS { nhdpInterfacePerfEntry }
   ::= { olsrv2InterfacePerfTable 1 }

   Olsrv2InterfacePerfEntry ::=
      SEQUENCE {
         olsrv2IfTcMessageXmits
            Counter32,
         olsrv2IfTcMessageRecvd
            Counter32,
         olsrv2IfTcMessageXmitAccumulatedSize
            Counter64,
         olsrv2IfTcMessageRecvdAccumulatedSize
            Counter64,
         olsrv2IfTcMessageTriggeredXmits
            Counter32,
         olsrv2IfTcMessagePeriodicXmits
            Counter32,
         olsrv2IfTcMessageForwardedXmits
            Counter32,
         olsrv2IfTcMessageXmitAccumulatedMPRSelectorCount
            Counter32
      }

   olsrv2IfTcMessageXmits  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION





         "A counter is incremented each time a TC
          message has been transmitted on that interface."
   ::= { olsrv2InterfacePerfEntry 1 }

   olsrv2IfTcMessageRecvd  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented each time a
          TC message has been received on that interface.
          This excludes all messages that are ignored due to
          OLSRv2 protocol procedures, such as messages
          considered invalid for processing by this router,
          as defined in Section 16.3.1 of OLSRv2 (RFC 7181)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2InterfacePerfEntry 2 }

   olsrv2IfTcMessageXmitAccumulatedSize  OBJECT-TYPE
      SYNTAX      Counter64
      UNITS       "octets"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented by the number of octets in
          a TC message each time a TC message has been sent."
   ::= { olsrv2InterfacePerfEntry 3 }

   olsrv2IfTcMessageRecvdAccumulatedSize  OBJECT-TYPE
      SYNTAX      Counter64
      UNITS       "octets"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented by the number of octets in
          a TC message each time a TC message has been received.
          This excludes all messages that are ignored due to
          OLSRv2 protocol procedures, such as messages
          considered invalid for processing by this router,
          as defined in Section 16.3.1 of OLSRv2 (RFC 7181)."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."





   ::= { olsrv2InterfacePerfEntry 4 }

   olsrv2IfTcMessageTriggeredXmits  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented each time a triggered
          TC message has been sent."
   ::= { olsrv2InterfacePerfEntry 5 }

   olsrv2IfTcMessagePeriodicXmits  OBJECT-TYPE
      SYNTAX      Counter32
       UNITS      "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented each time a periodic
          TC message has been sent."
   ::= { olsrv2InterfacePerfEntry 6 }

   olsrv2IfTcMessageForwardedXmits  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented each time a
          TC message has been forwarded."
   ::= { olsrv2InterfacePerfEntry 7 }

   olsrv2IfTcMessageXmitAccumulatedMPRSelectorCount OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "advertised MPR selectors"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented by the number of advertised
          MPR selectors in a TC each time a TC
          message has been sent."
   ::= { olsrv2InterfacePerfEntry 8 }

   --
   -- Objects concerning the Routing Set
   --

   olsrv2RoutingSetRecalculationCount  OBJECT-TYPE





      SYNTAX      Counter32
      UNITS       "recalculations"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This counter increments each time the Routing Set has
          been recalculated."
   ::= { olsrv2PerformanceObjGrp 2 }

   --
   -- Objects concerning the MPR set
   --

   olsrv2MPRSetRecalculationCount  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "recalculations"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This counter increments each time the MPRs
          of this router have been recalculated for
          any of its interfaces."
   ::= { olsrv2PerformanceObjGrp 3 }

--
-- Notifications
--

olsrv2NotificationsObjects OBJECT IDENTIFIER ::=
                                     { olsrv2MIBNotifications 0 }
olsrv2NotificationsControl OBJECT IDENTIFIER ::=
                                     { olsrv2MIBNotifications 1 }
olsrv2NotificationsStates  OBJECT IDENTIFIER ::=
                                     { olsrv2MIBNotifications 2 }


   -- olsrv2NotificationsObjects

   olsrv2RouterStatusChange NOTIFICATION-TYPE
       OBJECTS { olsrv2OrigIpAddrType, -- The address type of
                                       --    the originator of
                                       --    the notification.
                 olsrv2OrigIpAddr,     -- The originator of
                                       --    the notification.
                 olsrv2AdminStatus     -- The new state.
       }
       STATUS      current
       DESCRIPTION





          "olsrv2RouterStatusChange is a notification generated
           when the OLSRv2 router changes it status.
           The router status is maintained in the
           olsrv2AdminStatus object."
   ::= { olsrv2NotificationsObjects 1 }

   olsrv2OrigIpAddrChange NOTIFICATION-TYPE
      OBJECTS { olsrv2OrigIpAddrType, -- The address type of
                                      --    the originator of
                                      --    the notification.
                olsrv2OrigIpAddr,     -- The originator of
                                      --    the notification.
                olsrv2PreviousOrigIpAddrType, -- The address
                                      -- type of the previous
                                      -- address of
                                      -- the originator of
                                      -- the notification.
                olsrv2PreviousOrigIpAddr  -- The previous
                                      -- address of the
                                      -- originator of
                                      -- the notification.
      }
      STATUS      current
      DESCRIPTION
         "olsrv2OrigIpAddrChange is a notification generated when
          the OLSRv2 router changes it originator IP address.
          The notification includes the new and the previous
          originator IP address of the OLSRv2 router."
   ::= { olsrv2NotificationsObjects 2 }

   olsrv2RoutingSetRecalculationCountChange NOTIFICATION-TYPE
      OBJECTS { olsrv2OrigIpAddrType, -- The address type of
                                      --   the originator of
                                      --   the notification.
                olsrv2OrigIpAddr,     -- The originator of
                                      --   the notification.
                olsrv2RoutingSetRecalculationCount  -- Number
                                          -- of the
                                          -- Routing Set
                                          -- recalculations.
      }
      STATUS       current
      DESCRIPTION
         "The olsrv2RoutingSetRecalculationCountChange
          notification is generated when a significant number of
          Routing Set recalculations have occurred in a short time.
          This notification SHOULD be generated no more than once
          per olsrv2RoutingSetRecalculationCountWindow.





          The network administrator SHOULD select
          appropriate values for 'significant number of
          Routing Set recalculations' and 'short time' through
          the settings of the
          olsrv2RoutingSetRecalculationCountThreshold
          and olsrv2RoutingSetRecalculationCountWindow objects."
   ::= { olsrv2NotificationsObjects 3 }

   olsrv2MPRSetRecalculationCountChange NOTIFICATION-TYPE
      OBJECTS { olsrv2OrigIpAddrType, -- The address type of
                                      --   the originator of
                                      --   the notification.
                olsrv2OrigIpAddr,     -- The originator of
                                      --   the notification.
                olsrv2MPRSetRecalculationCount  -- Number of
                                      --   MPR set
                                      --   recalculations.
      }
      STATUS       current
      DESCRIPTION
         "The olsrv2MPRSetRecalculationCountChange
          notification is generated when a significant
          number of MPR set recalculations occur in
          a short period of time.  This notification
          SHOULD be generated no more than once
          per olsrv2MPRSetRecalculationCountWindow.
          The network administrator SHOULD select
          appropriate values for 'significant number of
          MPR set recalculations' and 'short period of
          time' through the settings of the
          olsrv2MPRSetRecalculationCountThreshold and
          olsrv2MPRSetRecalculationCountWindow objects."
   ::= { olsrv2NotificationsObjects 4 }

   -- olsrv2NotificationsControl

   olsrv2RoutingSetRecalculationCountThreshold OBJECT-TYPE
      SYNTAX      Integer32 (0..255)
      UNITS       "recalculations"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "A threshold value for the
          olsrv2RoutingSetRecalculationCount object.
          If the number of occurrences exceeds this
          threshold within the previous
          olsrv2RoutingSetRecalculationCountWindow,
          then the olsrv2RoutingSetRecalculationCountChange





          notification is to be generated.

          It is RECOMMENDED that the value of this
          threshold be set to at least 20 and higher
          in dense topologies with frequent expected
          topology changes."
      DEFVAL { 20 }
   ::= { olsrv2NotificationsControl 1 }

   olsrv2RoutingSetRecalculationCountWindow OBJECT-TYPE
      SYNTAX      TimeTicks
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "This object is used to determine whether to generate
          an olsrv2RoutingSetRecalculationCountChange notification.
          This object represents an interval from the present moment,
          extending into the past, expressed in hundredths of
          a second.  If the change in the value of the
          olsrv2RoutingSetRecalculationCount object during
          this interval has exceeded the value of
          olsrv2RoutingSetRecalculationCountThreshold, then
          an olsrv2RoutingSetRecalculationCountChange notification
          is generated.

          It is RECOMMENDED that the value for this
          window be set to at least 5 times the
          nhdpHelloInterval (whose default value is
          2 seconds."
      DEFVAL { 1000 }
   ::= { olsrv2NotificationsControl 2 }

   olsrv2MPRSetRecalculationCountThreshold OBJECT-TYPE
      SYNTAX      Integer32 (0..255)
      UNITS       "recalculations"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "A threshold value for the
          olsrv2MPRSetRecalculationCount object.
          If the number of occurrences exceeds this
          threshold within the previous
          olsrv2MPRSetRecalculationCountWindow,
          then the
          olsrv2MPRSetRecalculationCountChange
          notification is to be generated.

          It is RECOMMENDED that the value of this





          threshold be set to at least 20 and higher
          in dense topologies with frequent expected
          topology changes."
      DEFVAL { 20 }
   ::= { olsrv2NotificationsControl 3 }

   olsrv2MPRSetRecalculationCountWindow OBJECT-TYPE
      SYNTAX       TimeTicks
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
         "This object is used to determine whether to generate
          an olsrv2MPRSetRecalculationCountChange notification.
          This object represents an interval from the present moment,
          extending into the past, expressed in hundredths of
          a second.  If the change in the value of the
          olsrv2MPRSetRecalculationCount object during
          that interval has exceeded the value of
          olsrv2MPRSetRecalculationCountThreshold, then the
          an olsrv2MPRSetRecalculationCountChange notification
          is generated.

          It is RECOMMENDED that the value for this
          window be set to at least 5 times the
          nhdpHelloInterval."
      DEFVAL { 1000 }
   ::= { olsrv2NotificationsControl 4 }

   olsrv2PreviousOrigIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType  { ipv4(1) , ipv6(2) }
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The type of the olsrv2PreviousOrigIpAddr,
          as defined in the InetAddress MIB module (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported.

          This object MUST have the same persistence
          characteristics as olsrv2PreviousOrigIpAddr."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NotificationsStates 1 }

   olsrv2PreviousOrigIpAddr  OBJECT-TYPE





      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The previous origination IP address
          of this OLSRv2 router.

          This object SHOULD be updated each time
          the olsrv2OrigIpAddr is modified.

          This object is persistent, and when written,
          the entity SHOULD save the change to
          non-volatile storage."
      REFERENCE
         "RFC 7181 - The Optimized Link State Routing Protocol
          Version 2, Clausen, T., Dearlove, C., Jacquet, P.,
          and U. Herberg, April 2014."
   ::= { olsrv2NotificationsStates 2 }

   --
   -- Compliance Statements
   --

   olsrv2Compliances  OBJECT IDENTIFIER ::= { olsrv2MIBConformance 1 }
   olsrv2MIBGroups    OBJECT IDENTIFIER ::= { olsrv2MIBConformance 2 }

   olsrv2BasicCompliance  MODULE-COMPLIANCE
      STATUS current
      DESCRIPTION
         "The basic implementation requirements for
          managed network entities that implement
          the OLSRv2 routing process."
      MODULE  -- this module
      MANDATORY-GROUPS { olsrv2ConfigObjectsGroup }
   ::= { olsrv2Compliances 1 }

   olsrv2FullCompliance MODULE-COMPLIANCE
      STATUS current
      DESCRIPTION
         "The full implementation requirements for
          managed network entities that implement
          the OLSRv2 routing process."
      MODULE  -- this module
      MANDATORY-GROUPS { olsrv2ConfigObjectsGroup,
                         olsrv2StateObjectsGroup,
                         olsrv2PerfObjectsGroup,
                         olsrv2NotificationsObjectsGroup,
                         olsrv2NotificationsGroup }





   ::= { olsrv2Compliances 2 }

   --
   -- Units of Conformance
   --

   olsrv2ConfigObjectsGroup OBJECT-GROUP
      OBJECTS {
         olsrv2AdminStatus,
         olsrv2InterfaceAdminStatus,
         olsrv2OrigIpAddrType,
         olsrv2OrigIpAddr,
         olsrv2OHoldTime,
         olsrv2TcInterval,
         olsrv2TcMinInterval,
         olsrv2THoldTime,
         olsrv2AHoldTime,
         olsrv2RxHoldTime,
         olsrv2PHoldTime,
         olsrv2FHoldTime,
         olsrv2TpMaxJitter,
         olsrv2TtMaxJitter,
         olsrv2FMaxJitter,
         olsrv2TcHopLimit,
         olsrv2WillFlooding,
         olsrv2WillRouting,
         olsrv2LinkMetricType
      }
      STATUS      current
      DESCRIPTION
         "Objects to permit configuration of OLSRv2.
          All of these SHOULD be backed by non-volatile
          storage."
   ::= { olsrv2MIBGroups 1 }

   olsrv2StateObjectsGroup  OBJECT-GROUP
      OBJECTS {
         olsrv2LibOrigSetExpireTime,
         olsrv2LibLocAttNetSetDistance,
         olsrv2LibLocAttNetSetMetricValue,
         olsrv2IibLinkSetInMetricValue,
         olsrv2IibLinkSetOutMetricValue,
         olsrv2IibLinkSetMprSelector,
         olsrv2Iib2HopSetInMetricValue,
         olsrv2Iib2HopSetOutMetricValue,
         olsrv2NibNeighborSetNOrigIpAddrType,
         olsrv2NibNeighborSetNOrigIpAddr,
         olsrv2NibNeighborSetNInMetricValue,





         olsrv2NibNeighborSetNOutMetricValue,
         olsrv2NibNeighborSetNWillFlooding,
         olsrv2NibNeighborSetNWillRouting,
         olsrv2NibNeighborSetNFloodingMpr,
         olsrv2NibNeighborSetNRoutingMpr,
         olsrv2NibNeighborSetNMprSelector,
         olsrv2NibNeighborSetNAdvertised,
         olsrv2NibNeighborSetTableAnsn,
         olsrv2TibAdRemoteRouterSetMaxSeqNo,
         olsrv2TibAdRemoteRouterSetExpireTime,
         olsrv2TibRouterTopologySetSeqNo,
         olsrv2TibRouterTopologySetMetricValue,
         olsrv2TibRouterTopologySetExpireTime,
         olsrv2TibRoutableAddressTopologySetExpireTime,
         olsrv2TibRoutableAddressTopologySetSeqNo,
         olsrv2TibRoutableAddressTopologySetMetricValue,
         olsrv2TibAttNetworksSetSeqNo,
         olsrv2TibAttNetworksSetDist,
         olsrv2TibAttNetworksSetMetricValue,
         olsrv2TibAttNetworksSetExpireTime,
         olsrv2TibRoutingSetNextIfIpAddrType,
         olsrv2TibRoutingSetNextIfIpAddr,
         olsrv2TibRoutingSetLocalIfIpAddrType,
         olsrv2TibRoutingSetLocalIfIpAddr,
         olsrv2TibRoutingSetDist,
         olsrv2TibRoutingSetMetricValue
      }
      STATUS      current
      DESCRIPTION
         "Objects to permit monitoring of OLSRv2 state."
   ::= { olsrv2MIBGroups 2 }

   olsrv2PerfObjectsGroup  OBJECT-GROUP
      OBJECTS {
         olsrv2IfTcMessageXmits,
         olsrv2IfTcMessageRecvd,
         olsrv2IfTcMessageXmitAccumulatedSize,
         olsrv2IfTcMessageRecvdAccumulatedSize,
         olsrv2IfTcMessageTriggeredXmits,
         olsrv2IfTcMessagePeriodicXmits,
         olsrv2IfTcMessageForwardedXmits,
         olsrv2IfTcMessageXmitAccumulatedMPRSelectorCount,
         olsrv2RoutingSetRecalculationCount,
         olsrv2MPRSetRecalculationCount
      }
      STATUS      current
      DESCRIPTION
         "Objects to support monitoring of OLSRv2 performance."





   ::= { olsrv2MIBGroups 3 }

   olsrv2NotificationsObjectsGroup OBJECT-GROUP
      OBJECTS {
         olsrv2RoutingSetRecalculationCountThreshold,
         olsrv2RoutingSetRecalculationCountWindow,
         olsrv2MPRSetRecalculationCountThreshold,
         olsrv2MPRSetRecalculationCountWindow,
         olsrv2PreviousOrigIpAddrType,
         olsrv2PreviousOrigIpAddr
      }
      STATUS      current
      DESCRIPTION
         "Objects to support the notification types in the
          olsrv2NotificationsGroup.  Some of these appear in
          notification payloads, others serve to control
          notification generation."
   ::= { olsrv2MIBGroups 4 }


   olsrv2NotificationsGroup NOTIFICATION-GROUP
      NOTIFICATIONS {
         olsrv2RouterStatusChange,
         olsrv2OrigIpAddrChange,
         olsrv2RoutingSetRecalculationCountChange,
         olsrv2MPRSetRecalculationCountChange
      }
      STATUS current
      DESCRIPTION
          "Notification types to support management of OLSRv2."
   ::= { olsrv2MIBGroups 5 }

END



