IPV6-ICMP-MIB DEFINITIONS ::= BEGIN


    IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE,
        Counter32, mib-2                 FROM SNMPv2-SMI
        MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF
        ipv6IfEntry                      FROM IPV6-MIB;

    ipv6IcmpMIB MODULE-IDENTITY
        LAST-UPDATED "201702220000Z"
        ORGANIZATION "IETF IPv6 Working Group"
        CONTACT-INFO
          "           Dimitry Haskin

              Postal: Bay Networks, Inc.
                      660 Technology Park Drive.
                      Billerica, MA  01821
                      US

                 Tel: +1-978-916-8124
              E-mail: dhaskin@baynetworks.com











                      Steve Onishi

              Postal: Bay Networks, Inc.
                      3 Federal Street
                      Billerica, MA 01821
                      US

                 Tel: +1-978-916-3816
              E-mail: sonishi@baynetworks.com"
        DESCRIPTION
          "The obsolete MIB module for entities implementing
           the ICMPv6.  Use the IP-MIB instead.

           Copyright (c) 2017 IETF Trust and the persons
           identified as authors of the code.  All rights
           reserved.

           Redistribution and use in source and binary
           forms, with or without modification, is permitted
           pursuant to, and subject to the license terms contained
           in, the Simplified BSD License set forth in Section
           4.c of the IETF Trust's Legal Provisions Relating to
           IETF Documents
           (http://trustee.ietf.org/license-info)."
        REVISION "201702220000Z"
        DESCRIPTION
          "Obsoleting this MIB module; it has been replaced by
          the revised IP-MIB (RFC 4293)."
        REVISION "9801082155Z"
        DESCRIPTION
          "First revision, published as RFC 2466"
        ::= { mib-2 56 }

    -- the ICMPv6 group

    ipv6IcmpMIBObjects OBJECT IDENTIFIER ::= { ipv6IcmpMIB  1 }

    -- Per-interface ICMPv6 statistics table

    ipv6IfIcmpTable OBJECT-TYPE
        SYNTAX     SEQUENCE OF Ipv6IfIcmpEntry
        MAX-ACCESS not-accessible
        STATUS     obsolete
        DESCRIPTION
         "IPv6 ICMP statistics.  This table contains statistics
         of ICMPv6 messages that are received and sourced by
         the entity.






         This table is obsolete because systems were found
         not to maintain these statistics per-interface."
        ::= { ipv6IcmpMIBObjects 1 }

    ipv6IfIcmpEntry OBJECT-TYPE
        SYNTAX     Ipv6IfIcmpEntry
        MAX-ACCESS not-accessible
        STATUS     obsolete
        DESCRIPTION
         "An ICMPv6 statistics entry containing
         objects at a particular IPv6 interface.

         Note that a receiving interface is
         the interface to which a given ICMPv6 message
         is addressed which may not be necessarily
         the input interface for the message.

         Similarly, the sending interface is
         the interface that sources a given
         ICMP message which is usually but not
         necessarily the output interface for the message.

         This table is obsolete because systems were found
         not to maintain these statistics per-interface."
        AUGMENTS { ipv6IfEntry }
        ::= { ipv6IfIcmpTable 1 }

    Ipv6IfIcmpEntry ::= SEQUENCE {
            ipv6IfIcmpInMsgs
                  Counter32      ,
            ipv6IfIcmpInErrors
                  Counter32      ,
            ipv6IfIcmpInDestUnreachs
                  Counter32      ,
            ipv6IfIcmpInAdminProhibs
                  Counter32      ,
            ipv6IfIcmpInTimeExcds
                  Counter32      ,
            ipv6IfIcmpInParmProblems
                  Counter32      ,
            ipv6IfIcmpInPktTooBigs
                  Counter32      ,
            ipv6IfIcmpInEchos
                  Counter32      ,
            ipv6IfIcmpInEchoReplies
                  Counter32      ,
            ipv6IfIcmpInRouterSolicits
                  Counter32      ,





            ipv6IfIcmpInRouterAdvertisements
                  Counter32      ,
            ipv6IfIcmpInNeighborSolicits
                  Counter32      ,
            ipv6IfIcmpInNeighborAdvertisements
                  Counter32      ,
            ipv6IfIcmpInRedirects
                  Counter32      ,
            ipv6IfIcmpInGroupMembQueries
                  Counter32      ,
            ipv6IfIcmpInGroupMembResponses
                  Counter32      ,
            ipv6IfIcmpInGroupMembReductions
                  Counter32      ,
            ipv6IfIcmpOutMsgs
                  Counter32      ,
            ipv6IfIcmpOutErrors
                  Counter32      ,
            ipv6IfIcmpOutDestUnreachs
                  Counter32      ,
            ipv6IfIcmpOutAdminProhibs
                  Counter32      ,
            ipv6IfIcmpOutTimeExcds
                  Counter32      ,
            ipv6IfIcmpOutParmProblems
                  Counter32      ,
            ipv6IfIcmpOutPktTooBigs
                  Counter32      ,
            ipv6IfIcmpOutEchos
                  Counter32      ,
            ipv6IfIcmpOutEchoReplies
                  Counter32      ,
            ipv6IfIcmpOutRouterSolicits
                  Counter32      ,
            ipv6IfIcmpOutRouterAdvertisements
                  Counter32      ,
            ipv6IfIcmpOutNeighborSolicits
                  Counter32      ,
            ipv6IfIcmpOutNeighborAdvertisements
                  Counter32      ,
            ipv6IfIcmpOutRedirects
                  Counter32      ,
            ipv6IfIcmpOutGroupMembQueries
                  Counter32      ,
            ipv6IfIcmpOutGroupMembResponses
                  Counter32      ,
            ipv6IfIcmpOutGroupMembReductions
                  Counter32





        }

    ipv6IfIcmpInMsgs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The total number of ICMP messages received
         by the interface which includes all those
         counted by ipv6IfIcmpInErrors.  Note that this
         interface is the interface to which the
         ICMP messages were addressed which may not be
         necessarily the input interface for the messages.

         This object has been obsoleted by IP-MIB::icmpStatsInMsgs."
        ::= { ipv6IfIcmpEntry 1 }

    ipv6IfIcmpInErrors OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP messages which the interface
         received but determined as having ICMP-specific
         errors (bad ICMP checksums, bad length, etc.).

         This object has been obsoleted by IP-MIB::icmpStatsInErrors."
        ::= { ipv6IfIcmpEntry 2 }

    ipv6IfIcmpInDestUnreachs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Destination Unreachable
         messages received by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 3 }

    ipv6IfIcmpInAdminProhibs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP destination
         unreachable/communication administratively





         prohibited messages received by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 4 }

    ipv6IfIcmpInTimeExcds OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Time Exceeded messages
          received by the interface.

          This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
          in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 5 }

    ipv6IfIcmpInParmProblems OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Parameter Problem messages
          received by the interface.

          This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
          in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 6 }

    ipv6IfIcmpInPktTooBigs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Packet Too Big messages
         received by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 7 }

    ipv6IfIcmpInEchos OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Echo (request) messages





          received by the interface.

          This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
          in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 8 }

    ipv6IfIcmpInEchoReplies OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Echo Reply messages received
         by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 9 }

    ipv6IfIcmpInRouterSolicits OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Router Solicit messages
          received by the interface.

          This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
          in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 10 }

    ipv6IfIcmpInRouterAdvertisements OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Router Advertisement messages
         received by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 11 }

    ipv6IfIcmpInNeighborSolicits OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Neighbor Solicit messages





          received by the interface.

          This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
          in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 12 }

    ipv6IfIcmpInNeighborAdvertisements OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Neighbor Advertisement
         messages received by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 13 }

    ipv6IfIcmpInRedirects OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of Redirect messages received
         by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 14 }

    ipv6IfIcmpInGroupMembQueries OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMPv6 Group Membership Query
         messages received by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 15}

    ipv6IfIcmpInGroupMembResponses OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMPv6 Group Membership Response messages





         received by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 16}

     ipv6IfIcmpInGroupMembReductions OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMPv6 Group Membership Reduction messages
         received by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsInPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 17}

    ipv6IfIcmpOutMsgs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The total number of ICMP messages which this
         interface attempted to send.  Note that this counter
         includes all those counted by icmpOutErrors.

         This object has been obsoleted by IP-MIB::icmpStatsOutMsgs."
        ::= { ipv6IfIcmpEntry 18 }

    ipv6IfIcmpOutErrors OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP messages which this interface did
         not send due to problems discovered within ICMP
         such as a lack of buffers.  This value should not
         include errors discovered outside the ICMP layer
         such as the inability of IPv6 to route the resultant
         datagram.  In some implementations there may be no
         types of error which contribute to this counter's
         value.

         This object has been obsoleted by IP-MIB::icmpStatsOutErrors."
        ::= { ipv6IfIcmpEntry 19 }

    ipv6IfIcmpOutDestUnreachs OBJECT-TYPE





        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Destination Unreachable
         messages sent by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 20 }

    ipv6IfIcmpOutAdminProhibs OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
          "Number of ICMP dest unreachable/communication
          administratively prohibited messages sent.

          This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
          in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 21 }

    ipv6IfIcmpOutTimeExcds OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Time Exceeded messages sent
         by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 22 }

    ipv6IfIcmpOutParmProblems OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Parameter Problem messages
         sent by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 23 }

    ipv6IfIcmpOutPktTooBigs OBJECT-TYPE





        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Packet Too Big messages sent
         by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 24 }

    ipv6IfIcmpOutEchos OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Echo (request) messages sent
         by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 25 }

    ipv6IfIcmpOutEchoReplies OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Echo Reply messages sent
         by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 26 }

    ipv6IfIcmpOutRouterSolicits OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Router Solicitation messages
          sent by the interface.

          This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
          in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 27 }

    ipv6IfIcmpOutRouterAdvertisements OBJECT-TYPE





        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Router Advertisement messages
         sent by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 28 }

    ipv6IfIcmpOutNeighborSolicits OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Neighbor Solicitation
          messages sent by the interface.

          This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
          in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 29 }

    ipv6IfIcmpOutNeighborAdvertisements OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMP Neighbor Advertisement
         messages sent by the interface.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 30 }

    ipv6IfIcmpOutRedirects OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of Redirect messages sent.  For
         a host, this object will always be zero,
         since hosts do not send redirects.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 31 }






    ipv6IfIcmpOutGroupMembQueries OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMPv6 Group Membership Query
         messages sent.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 32}

    ipv6IfIcmpOutGroupMembResponses OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMPv6 Group Membership Response
         messages sent.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 33}

    ipv6IfIcmpOutGroupMembReductions OBJECT-TYPE
        SYNTAX     Counter32
        MAX-ACCESS read-only
        STATUS     obsolete
        DESCRIPTION
         "The number of ICMPv6 Group Membership Reduction
         messages sent.

         This object has been obsoleted by IP-MIB::icmpMsgStatsOutPkts
         in the row corresponding to this message type."
        ::= { ipv6IfIcmpEntry 34}

   -- conformance information

   ipv6IcmpConformance OBJECT IDENTIFIER ::= { ipv6IcmpMIB 2 }

   ipv6IcmpCompliances
           OBJECT IDENTIFIER ::= { ipv6IcmpConformance 1 }
   ipv6IcmpGroups
           OBJECT IDENTIFIER ::= { ipv6IcmpConformance 2 }

   -- compliance statements

   ipv6IcmpCompliance MODULE-COMPLIANCE





       STATUS  obsolete
       DESCRIPTION
         "The compliance statement for SNMPv2 entities which
         implement ICMPv6.

         This compliance statement has been obsoleted by
         IP-MIB::ipMIBCompliance2."
       MODULE  -- this module
           MANDATORY-GROUPS { ipv6IcmpGroup }
       ::= { ipv6IcmpCompliances 1 }

   ipv6IcmpGroup OBJECT-GROUP
       OBJECTS   {
                   ipv6IfIcmpInMsgs,
                   ipv6IfIcmpInErrors,
                   ipv6IfIcmpInDestUnreachs,
                   ipv6IfIcmpInAdminProhibs,
                   ipv6IfIcmpInTimeExcds,
                   ipv6IfIcmpInParmProblems,
                   ipv6IfIcmpInPktTooBigs,
                   ipv6IfIcmpInEchos,
                   ipv6IfIcmpInEchoReplies,
                   ipv6IfIcmpInRouterSolicits,
                   ipv6IfIcmpInRouterAdvertisements,
                   ipv6IfIcmpInNeighborSolicits,
                   ipv6IfIcmpInNeighborAdvertisements,
                   ipv6IfIcmpInRedirects,
                   ipv6IfIcmpInGroupMembQueries,
                   ipv6IfIcmpInGroupMembResponses,
                   ipv6IfIcmpInGroupMembReductions,
                   ipv6IfIcmpOutMsgs,
                   ipv6IfIcmpOutErrors,
                   ipv6IfIcmpOutDestUnreachs,
                   ipv6IfIcmpOutAdminProhibs,
                   ipv6IfIcmpOutTimeExcds,
                   ipv6IfIcmpOutParmProblems,
                   ipv6IfIcmpOutPktTooBigs,
                   ipv6IfIcmpOutEchos,
                   ipv6IfIcmpOutEchoReplies,
                   ipv6IfIcmpOutRouterSolicits,
                   ipv6IfIcmpOutRouterAdvertisements,
                   ipv6IfIcmpOutNeighborSolicits,
                   ipv6IfIcmpOutNeighborAdvertisements,
                   ipv6IfIcmpOutRedirects,
                   ipv6IfIcmpOutGroupMembQueries,
                   ipv6IfIcmpOutGroupMembResponses,
                   ipv6IfIcmpOutGroupMembReductions
                 }





       STATUS    obsolete
       DESCRIPTION
            "The ICMPv6 group of objects providing information
             specific to ICMPv6.

             This group has been obsoleted by IP-MIB::icmpStatsGroup."
       ::= { ipv6IcmpGroups 1 }

    END


