ADSL2-LINE-TC-MIB DEFINITIONS ::= BEGIN


   IMPORTS
      MODULE-IDENTITY,
      transmission
         FROM SNMPv2-SMI

      TEXTUAL-CONVENTION
         FROM SNMPv2-TC;

   adsl2TCMIB MODULE-IDENTITY
      LAST-UPDATED "200610040000Z" -- October 4th, 2006
      ORGANIZATION "ADSLMIB Working Group"
      CONTACT-INFO "WG-email:  adslmib@ietf.org
      Info:      https://www1.ietf.org/mailman/listinfo/adslmib

                Chair:     Mike Sneed
                           Sand Channel Systems
                Postal:    P.O. Box 37324
                           Raleigh NC 27627-732
                Email:     sneedmike@hotmail.com
                Phone:     +1 206 600 7022

                Co-Chair & Co-editor:
                           Menachem Dodge
                           ECI Telecom Ltd.
                Postal:    30 Hasivim St.
                           Petach Tikva 49517,
                           Israel.
                Email:     mbdodge@ieee.org
                Phone:     +972 3 926 8421








                Co-editor: Moti Morgenstern
                           ECI Telecom Ltd.
                Postal:    30 Hasivim St.
                           Petach Tikva 49517,
                           Israel.
                Email:     moti.morgenstern@ecitele.com
                Phone:     +972 3 926 6258

                Co-editor: Scott Baillie
                           NEC Australia
                Postal:    649-655 Springvale Road,
                           Mulgrave, Victoria 3170,
                           Australia.
                Email:     scott.baillie@nec.com.au
                Phone:     +61 3 9264 3986

                Co-editor: Umberto Bonollo
                           NEC Australia
                Postal:    649-655 Springvale Road,
                           Mulgrave, Victoria 3170,
                           Australia.
                Email:     umberto.bonollo@nec.com.au
                Phone:     +61 3 9264 3385
               "
      DESCRIPTION
           "This MIB Module provides Textual Conventions to be
            used by the ADSL2-LINE-MIB module for the purpose of
            managing ADSL, ADSL2, and ADSL2+ lines.

           Copyright (C) The Internet Society (2006).  This version of
           this MIB module is part of RFC 4706: see the RFC itself for
           full legal notices."

      REVISION "200610040000Z" -- October 4th, 2006
      DESCRIPTION "Initial version, published as RFC 4706."
         ::= { transmission 238 2 } -- adsl2MIB 2

   ------------------------------------------------
   --          Textual Conventions               --
   ------------------------------------------------

   Adsl2Unit ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Identifies a transceiver as being either an ATU-C or
          an ATU-R.  An ADSL line consists of two transceivers, an ATU-C
          and an ATU-R.  Attributes with this syntax reference the two
          sides of a line.  Specified as an INTEGER, the two values





          are:

           atuc(1)  -- Central office ADSL terminal unit (ATU-C).
           atur(2)  -- Remote ADSL terminal unit (ATU-R)."
      SYNTAX      INTEGER {
                     atuc(1),
                     atur(2)
                  }

   Adsl2Direction ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
           "Identifies the direction of a band as being
            either upstream or downstream.  Specified as an INTEGER,
            the two values are:
             upstream(1), and
             downstream(2)."
        SYNTAX INTEGER {
          upstream(1),
          downstream(2)
       }



   Adsl2TransmissionModeType ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "A set of ADSL2 line transmission modes, with one bit
          per mode.  The notes (F) and (L) denote Full-Rate
          and Lite/splitterless, respectively:
             Bit 00 : Regional Std. (ANSI T1.413) (F)
             Bit 01 : Regional Std. (ETSI DTS/TM06006) (F)
             Bit 02 : G.992.1 POTS non-overlapped (F)
             Bit 03 : G.992.1 POTS overlapped (F)
             Bit 04 : G.992.1 ISDN non-overlapped (F)
             Bit 05 : G.992.1 ISDN overlapped (F)
             Bit 06 : G.992.1 TCM-ISDN non-overlapped (F)
             Bit 07 : G.992.1 TCM-ISDN overlapped (F)
             Bit 08 : G.992.2 POTS non-overlapped (L)
             Bit 09 : G.992.2 POTS overlapped (L)
             Bit 10 : G.992.2 with TCM-ISDN non-overlapped (L)
             Bit 11 : G.992.2 with TCM-ISDN overlapped (L)
             Bit 12 : G.992.1 TCM-ISDN symmetric (F) -- not in G.997.1
             Bit 13-17: Reserved
             Bit 18 : G.992.3 POTS non-overlapped (F)
             Bit 19 : G.992.3 POTS overlapped (F)
             Bit 20 : G.992.3 ISDN non-overlapped (F)
             Bit 21 : G.992.3 ISDN overlapped (F)





             Bit 22-23: Reserved
             Bit 24 : G.992.4 POTS non-overlapped (L)
             Bit 25 : G.992.4 POTS overlapped (L)
             Bit 26-27: Reserved
             Bit 28 : G.992.3 Annex I All-Digital non-overlapped (F)
             Bit 29 : G.992.3 Annex I All-Digital overlapped (F)
             Bit 30 : G.992.3 Annex J All-Digital non-overlapped (F)
             Bit 31 : G.992.3 Annex J All-Digital overlapped (F)
             Bit 32 : G.992.4 Annex I All-Digital non-overlapped (L)
             Bit 33 : G.992.4 Annex I All-Digital overlapped (L)
             Bit 34 : G.992.3 Annex L POTS non-overlapped, mode 1,
                                      wide U/S (F)
             Bit 35 : G.992.3 Annex L POTS non-overlapped, mode 2,
                                      narrow U/S(F)
             Bit 36 : G.992.3 Annex L POTS overlapped, mode 3,
                                      wide U/S (F)
             Bit 37 : G.992.3 Annex L POTS overlapped, mode 4,
                                      narrow U/S (F)
             Bit 38 : G.992.3 Annex M POTS non-overlapped (F)
             Bit 39 : G.992.3 Annex M POTS overlapped (F)
             Bit 40 : G.992.5 POTS non-overlapped (F)
             Bit 41 : G.992.5 POTS overlapped (F)
             Bit 42 : G.992.5 ISDN non-overlapped (F)
             Bit 43 : G.992.5 ISDN overlapped (F)
             Bit 44-45: Reserved
             Bit 46 : G.992.5 Annex I All-Digital non-overlapped (F)
             Bit 47 : G.992.5 Annex I All-Digital overlapped (F)
             Bit 48 : G.992.5 Annex J All-Digital non-overlapped (F)
             Bit 49 : G.992.5 Annex J All-Digital overlapped (F)
             Bit 50 : G.992.5 Annex M POTS non-overlapped (F)
             Bit 51 : G.992.5 Annex M POTS overlapped (F)
             Bit 52-55: Reserved"
      SYNTAX      BITS {
                     ansit1413(0),
                     etsi(1),
                     g9921PotsNonOverlapped(2),
                     g9921PotsOverlapped(3),
                     g9921IsdnNonOverlapped(4),
                     g9921isdnOverlapped(5),
                     g9921tcmIsdnNonOverlapped(6),
                     g9921tcmIsdnOverlapped(7),
                     g9922potsNonOverlapped(8),
                     g9922potsOverlapped(9),
                     g9922tcmIsdnNonOverlapped(10),
                     g9922tcmIsdnOverlapped(11),
                     g9921tcmIsdnSymmetric(12),
                     reserved1(13),
                     reserved2(14),





                     reserved3(15),
                     reserved4(16),
                     reserved5(17),
                     g9923PotsNonOverlapped(18),
                     g9923PotsOverlapped(19),
                     g9923IsdnNonOverlapped(20),
                     g9923isdnOverlapped(21),
                     reserved6(22),
                     reserved7(23),
                     g9924potsNonOverlapped(24),
                     g9924potsOverlapped(25),
                     reserved8(26),
                     reserved9(27),
                     g9923AnnexIAllDigNonOverlapped(28),
                     g9923AnnexIAllDigOverlapped(29),
                     g9923AnnexJAllDigNonOverlapped(30),
                     g9923AnnexJAllDigOverlapped(31),
                     g9924AnnexIAllDigNonOverlapped(32),
                     g9924AnnexIAllDigOverlapped(33),
                     g9923AnnexLMode1NonOverlapped(34),
                     g9923AnnexLMode2NonOverlapped(35),
                     g9923AnnexLMode3Overlapped(36),
                     g9923AnnexLMode4Overlapped(37),
                     g9923AnnexMPotsNonOverlapped(38),
                     g9923AnnexMPotsOverlapped(39),
                     g9925PotsNonOverlapped(40),
                     g9925PotsOverlapped(41),
                     g9925IsdnNonOverlapped(42),
                     g9925isdnOverlapped(43),
                     reserved10(44),
                     reserved11(45),
                     g9925AnnexIAllDigNonOverlapped(46),
                     g9925AnnexIAllDigOverlapped(47),
                     g9925AnnexJAllDigNonOverlapped(48),
                     g9925AnnexJAllDigOverlapped(49),
                     g9925AnnexMPotsNonOverlapped(50),
                     g9925AnnexMPotsOverlapped(51),
                     reserved12(52),
                     reserved13(53),
                     reserved14(54),
                     reserved15(55)
                  }

   Adsl2RaMode ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Specifies the rate adaptation behavior for the line.
          The three possible behaviors are:





           manual(1)    - No Rate-Adaptation.  The initialization
                          process attempts to synchronize to a
                          specified rate.
           raInit(2)    - Rate-Adaptation during initialization process
                          only, which attempts to synchronize to a rate
                          between minimum and maximum specified values.
           dynamicRa(3) - Dynamic Rate-Adaptation during initialization
                          process as well as during SHOWTIME."
      SYNTAX      INTEGER {
                     manual(1),
                     raInit(2),
                     dynamicRa(3)
                  }

   Adsl2InitResult ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Specifies the result of a full initialization attempt; the
          six possible result values are:
           noFail(0)            - Successful initialization.
           configError(1)       - Configuration failure.
           configNotFeasible(2) - Configuration details not supported.
           commFail(3)          - Communication failure.
           noPeerAtu(4)         - Peer ATU not detected.
           otherCause(5)        - Other initialization failure reason.

          The values used are as defined in ITU-T G.997.1,
          paragraph 7.5.1.3"

      SYNTAX      INTEGER {
                     noFail(0),
                     configError(1),
                     configNotFeasible(2),
                     commFail(3),
                     noPeerAtu(4),
                     otherCause(5)
                  }

   Adsl2OperationModes ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "The ADSL2 management model specified includes an ADSL Mode
          attribute that identifies an instance of ADSL Mode-Specific
          PSD Configuration object in the ADSL Line Profile.  The
          following classes of ADSL operating mode are defined.
          The notes (F) and (L) denote Full-Rate and Lite/splitterless
          respectively:






          +-------+--------------------------------------------------+
          | Value |         ADSL operation mode description          |
          +-------+--------------------------------------------------+

              1   - The default/generic PSD configuration.  Default
                    configuration will be used when no other matching
                    mode-specific configuration can be found.
              2   - ADSL family.  The attributes included in the Mode-
                    Specific PSD Configuration are irrelevant for
                    ITU-T G.992.1 and G.992.2 ADSL modes.  Hence, it
                    is possible to map those modes to this generic
                    class.
             3-7  - Unused. Reserved for future ITU-T specification.
              8   - G.992.3 POTS non-overlapped (F)
              9   - G.992.3 POTS overlapped (F)
             10   - G.992.3 ISDN non-overlapped (F)
             11   - G.992.3 ISDN overlapped (F)
           12-13  - Unused. Reserved for future ITU-T specification.
             14   - G.992.4 POTS non-overlapped (L)
             15   - G.992.4 POTS overlapped (L)
           16-17  - Unused. Reserved for future ITU-T specification.
             18   - G.992.3 Annex I All-Digital non-overlapped (F)
             19   - G.992.3 Annex I All-Digital overlapped (F)
             20   - G.992.3 Annex J All-Digital non-overlapped (F)
             21   - G.992.3 Annex J All-Digital overlapped (F)
             22   - G.992.4 Annex I All-Digital non-overlapped (L)
             23   - G.992.4 Annex I All-Digital overlapped (L)
             24   - G.992.3 Annex L POTS non-overlapped, mode 1,
                    wide U/S (F)
             25   - G.992.3 Annex L POTS non-overlapped, mode 2,
                    narrow U/S(F)
             26   - G.992.3 Annex L POTS overlapped, mode 3,
                    wide U/S (F)
             27   - G.992.3 Annex L POTS overlapped, mode 4,
                    narrow U/S (F)
             28   - G.992.3 Annex M POTS non-overlapped (F)
             29   - G.992.3 Annex M POTS overlapped (F)
             30   - G.992.5 POTS non-overlapped (F)
             31   - G.992.5 POTS overlapped (F)
             32   - G.992.5 ISDN non-overlapped (F)
             33   - G.992.5 ISDN overlapped (F)
           34-35  - Unused. Reserved for future ITU-T specification.
             36   - G.992.5 Annex I All-Digital non-overlapped (F)
             37   - G.992.5 Annex I All-Digital overlapped (F)
             38   - G.992.5 Annex J All-Digital non-overlapped (F)
             39   - G.992.5 Annex J All-Digital overlapped (F)
             40   - G.992.5 Annex M POTS non-overlapped (F)
             41   - G.992.5 Annex M POTS overlapped (F)





         "
      SYNTAX      INTEGER {
                     defMode (1),
                     adsl(2),
                     g9923PotsNonOverlapped(8),
                     g9923PotsOverlapped(9),
                     g9923IsdnNonOverlapped(10),
                     g9923isdnOverlapped(11),
                     g9924potsNonOverlapped(14),
                     g9924potsOverlapped(15),
                     g9923AnnexIAllDigNonOverlapped(18),
                     g9923AnnexIAllDigOverlapped(19),
                     g9923AnnexJAllDigNonOverlapped(20),
                     g9923AnnexJAllDigOverlapped(21),
                     g9924AnnexIAllDigNonOverlapped(22),
                     g9924AnnexIAllDigOverlapped(23),
                     g9923AnnexLMode1NonOverlapped(24),
                     g9923AnnexLMode2NonOverlapped(25),
                     g9923AnnexLMode3Overlapped(26),
                     g9923AnnexLMode4Overlapped(27),
                     g9923AnnexMPotsNonOverlapped(28),
                     g9923AnnexMPotsOverlapped(29),
                     g9925PotsNonOverlapped(30),
                     g9925PotsOverlapped(31),
                     g9925IsdnNonOverlapped(32),
                     g9925isdnOverlapped(33),
                     g9925AnnexIAllDigNonOverlapped(36),
                     g9925AnnexIAllDigOverlapped(37),
                     g9925AnnexJAllDigNonOverlapped(38),
                     g9925AnnexJAllDigOverlapped(39),
                     g9925AnnexMPotsNonOverlapped(40),
                     g9925AnnexMPotsOverlapped(41)
                  }


   Adsl2PowerMngState ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Attributes with this syntax uniquely identify each power
          management state defined for the ADSL/ADSL2 or ADSL2+ link.
          The possible values are:
            l0(1) - L0 - Full power management state.
            l1(2) - L1 - Low power management state (for G.992.2).
            l2(3) - L2 - Low power management state (for G.992.3,
                         G.992.4, and G.992.5).
            l3(4) - L3 - Idle power management state."

      SYNTAX      INTEGER {





                     l0(1),
                     l1(2),
                     l2(3),
                     l3(4)
                  }

   Adsl2ConfPmsForce ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Attributes with this syntax are configuration parameters
          that reference the desired power management state for the
          ADSL/ADSL2 or ADSL2+ link:
            l3toL0(0)          - Perform a transition from L3 to L0
                                 (Full power management state).
            l0toL2(2)          - Perform a transition from L0 to L2
                                 (Low power management state).
            l0orL2toL3(3)      - Perform a transition into L3 (Idle
                                 power management state).

          The values used are as defined in ITU-T G.997.1,
          paragraph 7.3.1.1.3"

      SYNTAX      INTEGER {
                     l3toL0(0),
                     l0toL2(2),
                     l0orL2toL3(3)
                  }

   Adsl2LConfProfPmMode ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
         "Attributes with this syntax are configuration parameters
          that reference the power modes/states into which the ATU-C or
          ATU-R may autonomously transit.

          It is a BITS structure that allows control of the following
          transit options:
           allowTransitionsToIdle(0)     - XTU may autonomously transit
                                           to idle (L3) state.
           allowTransitionsToLowPower(1) - XTU may autonomously transit
                                           to low-power (L2) state."

      SYNTAX BITS {
          allowTransitionsToIdle(0),
          allowTransitionsToLowPower(1)
        }

   Adsl2LineLdsf ::= TEXTUAL-CONVENTION





      STATUS current
      DESCRIPTION
         "Attributes with this syntax are configuration parameters
          that control the Loop Diagnostic mode for the ADSL/ADSL2 or
          ADSL2+ link.  The possible values are:
            inhibit(0)  - Inhibit Loop Diagnostic mode.
            force(1)    - Force/Initiate Loop Diagnostic mode.

          The values used are as defined in ITU-T G.997.1,
          paragraph 7.3.1.1.8"

      SYNTAX INTEGER {
          inhibit(0),
          force(1)
        }

   Adsl2LdsfResult ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
           "Possible failure reasons associated with performing
            a Dual Ended Loop Test (DELT) on a DSL line.
            Possible values are:
             none(1)         - The default value in case LDSF was never
                               requested for the associated line.
             success(2)      - The recent command completed
                               successfully.
             inProgress(3)   - The Loop Diagnostics process is in
                               progress.
             unsupported(4)  - The NE or the line card doesn't support
                               LDSF.
             cannotRun(5)    - The NE cannot initiate the command, due
                               to a nonspecific reason.
             aborted(6)      - The Loop Diagnostics process aborted.
             failed(7)       - The Loop Diagnostics process failed.
             illegalMode(8)  - The NE cannot initiate the command, due
                               to the specific mode of the relevant
                               line.
             adminUp(9)      - The NE cannot initiate the command, as
                               the relevant line is administratively
                               'Up'.
             tableFull(10)   - The NE cannot initiate the command, due
                               to reaching the maximum number of rows
                               in the results table.
             noResources(11) - The NE cannot initiate the command, due
                               to lack of internal memory resources."
        SYNTAX INTEGER {
             none(1),
             success(2),





             inProgress(3),
             unsupported(4),
             cannotRun(5),
             aborted(6),
             failed(7),
             illegalMode(8),
             adminUp(9),
             tableFull(10),
             noResources(11)
        }

   Adsl2SymbolProtection ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Attributes with this syntax are configuration parameters
          that reference the minimum-length impulse noise protection
          (INP) in terms of number of symbols.  The possible values are:
          noProtection (i.e., INP not required), halfSymbol (i.e., INP
          length is 1/2 symbol), and 1-16 symbols in steps of 1 symbol."

      SYNTAX      INTEGER {
                  noProtection(1),
                  halfSymbol(2),
                  singleSymbol(3),
                  twoSymbols(4),
                  threeSymbols(5),
                  fourSymbols(6),
                  fiveSymbols(7),
                  sixSymbols(8),
                  sevenSymbols(9),
                  eightSymbols(10),
                  nineSymbols(11),
                  tenSymbols(12),
                  elevenSymbols(13),
                  twelveSymbols(14),
                  thirteeSymbols(15),
                  fourteenSymbols(16),
                  fifteenSymbols(17),
                  sixteenSymbols(18)
                }
   Adsl2MaxBer ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Attributes with this syntax are configuration parameters
          that reference the maximum Bit Error Rate (BER).
          The possible values are:

            eminus3(1)   - Maximum BER=E^-3





            eminus5(2)   - Maximum BER=E^-5
            eminus7(3)   - Maximum BER=E^-7"
      SYNTAX      INTEGER {
                     eminus3(1),
                     eminus5(2),
                     eminus7(3)
                  }

   Adsl2ScMaskDs ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Each one of the 512 bits in this OCTET
          STRING array represents the corresponding bin
          in the downstream direction.  A value of one
          indicates that the bin is not in use."
      SYNTAX      OCTET STRING (SIZE(0..64))

   Adsl2ScMaskUs ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Each one of the 64 bits in this OCTET
         STRING array represents the corresponding bin
         in the upstream direction.  A value of one
         indicates that the bin is not in use."
      SYNTAX      OCTET STRING (SIZE(0..8))

   Adsl2RfiDs ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "Each one of the 512 bits in this OCTET
         STRING array represents the corresponding bin
         in the downstream direction.  A value of one
         indicates that the bin is part of a notch
         filter."
      SYNTAX      OCTET STRING (SIZE(0..64))

   Adsl2PsdMaskDs ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "This is a structure that represents up to
         32 PSD Mask breakpoints.
         Each breakpoint occupies 3 octets: The first
         two octets hold the index of the sub-carrier
         associated with the breakpoint.  The third octet
         holds the PSD reduction at the breakpoint from 0
         (0 dBm/Hz) to 255 (-127.5 dBm/Hz) using units of
         0.5 dBm/Hz."
      SYNTAX      OCTET STRING (SIZE(0..96))





   Adsl2PsdMaskUs ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "This is a structure that represents up to
         4 PSD Mask breakpoints.
         Each breakpoint occupies 3 octets: The first
         two octets hold the index of the sub-carrier
         associated with the breakpoint.  The third octet
         holds the PSD reduction at the breakpoint from 0
         (0 dBm/Hz) to 255 (-127.5 dBm/Hz) using units of
         0.5 dBm/Hz."
      SYNTAX      OCTET STRING (SIZE(0..12))

   Adsl2Tssi ::= TEXTUAL-CONVENTION
      STATUS      current
      DESCRIPTION
         "This is a structure that represents up to
         32 transmit spectrum shaping (TSSi) breakpoints.
         Each breakpoint occupies 3 octets: The first
         two octets hold the index of the sub-carrier
         associated with the breakpoint.  The third octet
         holds the shaping parameter at the breakpoint.  It
         is a value from 0 to 127 (units of -0.5 dB).  The
         special value 127 indicates that the sub-carrier
         is not transmitted."
      SYNTAX      OCTET STRING (SIZE(0..96))

   Adsl2LastTransmittedState ::= TEXTUAL-CONVENTION
        STATUS current
        DESCRIPTION
           "This parameter represents the last successfully
            transmitted initialization state in the last full
            initialization performed on the line.  States are
            per the specific xDSL technology and are numbered
            from 0 (if G.994.1 is used) or 1 (if G.994.1 is
            not used) up to Showtime."
        SYNTAX      INTEGER {
          atucG9941(0),
          atucQuiet1(1),
          atucComb1(2),
          atucQuiet2(3),
          atucComb2(4),
          atucIcomb1(5),
          atucLineprob(6),
          atucQuiet3(7),
          atucComb3(8),
          atucIComb2(9),
          atucMsgfmt(10),





          atucMsgpcb(11),
          atucQuiet4(12),
          atucReverb1(13),
          atucTref1(14),
          atucReverb2(15),
          atucEct(16),
          atucReverb3(17),
          atucTref2(18),
          atucReverb4(19),
          atucSegue1(20),
          atucMsg1(21),
          atucReverb5(22),
          atucSegue2(23),
          atucMedley(24),
          atucExchmarker(25),
          atucMsg2(26),
          atucReverb6(27),
          atucSegue3(28),
          atucParams(29),
          atucReverb7(30),
          atucSegue4(31),
          atucShowtime(32),
          --
          aturG9941(100),
          aturQuiet1(101),
          aturComb1(102),
          aturQuiet2(103),
          aturComb2(104),
          aturIcomb1(105),
          aturLineprob(106),
          aturQuiet3(107),
          aturComb3(108),
          aturIcomb2(109),
          aturMsgfmt(110),
          aturMsgpcb(111),
          aturReverb1(112),
          aturQuiet4(113),
          aturReverb2(114),
          aturQuiet5(115),
          aturReverb3(116),
          aturEct(117),
          aturReverb4(118),
          aturSegue1(119),
          aturReverb5(120),
          aturSegue2(121),
          aturMsg1(122),
          aturMedley(123),
          aturExchmarker(124),





          aturMsg2(125),
          aturReverb6(126),
          aturSegue3(127),
          aturParams(128),
          aturReverb7(129),
          aturSegue4(130),
          aturShowtime(131)
        }

   Adsl2LineStatus ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
         "Attributes with this syntax are status parameters
          that reflect the failure status for a given endpoint of
          ADSL/ADSL2 or ADSL2+ link.

          This BITS structure can report the following failures:

           noDefect(0)       - This bit position positively reports
                               that no defect or failure exists.
           lossOfFrame(1)    - Loss of frame synchronization.
           lossOfSignal(2)   - Loss of signal.
           lossOfPower(3)    - Loss of power.  Usually this failure may
                               be reported for ATU-Rs only.
           initFailure(4)    - Recent initialization process failed.
                               Never active on ATU-R."

      SYNTAX BITS {
          noDefect(0),
          lossOfFrame(1),
          lossOfSignal(2),
          lossOfPower(3),
          initFailure(4)
        }

   Adsl2ChAtmStatus ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
        "Attributes with this syntax are status parameters that
         reflect the failure status for Transmission Convergence (TC)
         layer of a given ATM interface (data path over an ADSL/ADSL2
         or ADSL2+ link).

         This BITS structure can report the following failures:
          noDefect(0)              - This bit position positively
                                     reports that no defect or failure
                                     exists.
          noCellDelineation(1)     - The link was successfully





                                     initialized, but cell delineation
                                     was never acquired on the
                                     associated ATM data path.
          lossOfCellDelineation(2) - Loss of cell delineation on the
                                     associated ATM data path."

      SYNTAX BITS {
          noDefect(0),
          noCellDelineation(1),
          lossOfCellDelineation(2)
        }

   Adsl2ChPtmStatus ::= TEXTUAL-CONVENTION
      STATUS current
      DESCRIPTION
        "Attributes with this syntax are status parameters that
         reflect the failure status for a given PTM interface (packet
         data path over an ADSL/ADSL2 or ADSL2+ link).

         This BITS structure can report the following failures:
             noDefect(0)     - This bit position positively
                               reports that no defect or failure exists.
             outOfSync(1)    - Out of synchronization."

         SYNTAX BITS {
             noDefect(0),
             outOfSync(1)
        }

   END






















