NHDP-MIB DEFINITIONS ::= BEGIN


-- This MIB module defines objects for the management of
-- NHDP (RFC 6130) - Mobile Ad Hoc Network (MANET)
-- Neighborhood Discovery Protocol (NHDP),
-- Clausen, T., Dearlove, C., and J. Dean, January 2011.

IMPORTS

    MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
    Counter32, Counter64, Integer32, Unsigned32, mib-2,
                 TimeTicks
                 FROM SNMPv2-SMI  -- RFC 2578

    TEXTUAL-CONVENTION, TruthValue, TimeStamp,
                 RowStatus
                 FROM SNMPv2-TC  -- RFC 2579

    MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
                 FROM SNMPv2-CONF  -- STD 58

    SnmpAdminString
                 FROM SNMP-FRAMEWORK-MIB  -- RFC 3411








    InetAddressType, InetAddress,
    InetAddressPrefixLength
                 FROM INET-ADDRESS-MIB  -- RFC 4001

    InterfaceIndex
                 FROM IF-MIB  -- RFC 2863

    Float32TC
                 FROM FLOAT-TC-MIB  -- RFC 6340
    ;

nhdpMIB MODULE-IDENTITY
       LAST-UPDATED "201607120000Z" -- 12 July 2016
       ORGANIZATION "IETF MANET Working Group"
       CONTACT-INFO
       "WG Email: manet@ietf.org
        WG web page: https://datatracker.ietf.org/wg/manet

        Editors:   Ulrich Herberg
                   United States of America
                   ulrich@herberg.name
                   http://www.herberg.name/

                   Robert G. Cole
                   US Army CERDEC
                   Space and Terrestrial Communications
                   6010 Frankford Street
                   Aberdeen Proving Ground, Maryland 21005
                   United States of America
                   +1 443 395-8744
                   robert.g.cole@us.army.mil
                   http://www.cs.jhu.edu/~rgcole/

                   Ian D Chakeres
                   Delvin
                   Ellicott City, Maryland 21042
                   United States of America
                   ian.chakeres@gmail.com
                   http://www.ianchak.com/

                   Thomas Heide Clausen
                   Ecole Polytechnique
                   LIX
                   91128 Palaiseau Cedex
                   France
                   Email: T.Clausen@computer.org
                   URI: http://www.thomasclausen.org/"






       DESCRIPTION
           "This NHDP-MIB module is applicable to routers
            implementing the Mobile Ad Hoc Network (MANET)
            Neighborhood Discovery Protocol (NHDP)
            defined in RFC 6130.

            Copyright (c) 2016 IETF Trust and the persons identified
            as authors of the code.  All rights reserved.

            Redistribution and use in source and binary forms, with
            or without modification, is permitted pursuant to, and
            subject to the license terms contained in, the Simplified
            BSD License set forth in Section 4.c of the IETF Trust's
            Legal Provisions Relating to IETF Documents
            (http://trustee.ietf.org/license-info)."

       -- revision
       REVISION "201607120000Z" -- 12 July 2016
       DESCRIPTION
            "Updated version of this MIB module,
             including updates made to NHDP by
             RFC 7466, published as RFC 7939."
       REVISION "201210221000Z" -- 22 October 2012
       DESCRIPTION
            "Initial version of this MIB module,
             published as RFC 6779."
       ::= { mib-2 213 }

--
-- Top-Level Components of this MIB Module
--
nhdpNotifications OBJECT IDENTIFIER ::= { nhdpMIB 0 }
nhdpObjects       OBJECT IDENTIFIER ::= { nhdpMIB 1 }
nhdpConformance   OBJECT IDENTIFIER ::= { nhdpMIB 2 }

--
-- TEXTUAL-CONVENTIONs
--
   -- Two new TEXTUAL-CONVENTIONs have been defined in
   -- this MIB module for indexing into the following
   -- tables and indexing into other tables in other MIB modules.
   -- This was necessary because NHDP manages and
   -- indexes based upon dynamic address tuples, i.e.,
   -- address sets, while SMI requires statically
   -- defined indexes for accessing its table rows.
   -- The NeighborIfIndex defines a unique (to the local router)
   -- index referencing a discovered virtual interface on another
   -- neighbor within the MANET.  The NeighborRouterIndex defines a





   -- unique (to the local router) index referencing a discovered
   -- virtual neighbor within the MANET.
   --
   -- Due to the nature of NHDP,
   -- different indexes may be related to common neighbor
   -- interfaces or common neighbor routers, but the information
   -- obtained through NHDP has not allowed the local router
   -- to relate these virtual objects (i.e., interfaces or routers)
   -- at this point in time.  As more topology information
   -- is gathered by the local router, it may associate
   -- virtual interfaces or routers and collapse these
   -- indexes appropriately.

   -- Multiple addresses can be associated with a
   -- given NeighborIfIndex.  Each NeighborIfIndex is
   -- associated with a NeighborRouterIndex.  Throughout
   -- the nhdpStateObjGroup, the
   -- NeighborIfIndex and the NeighborRouterIndex are used
   -- to define the set of IP Addresses related to a virtual
   -- neighbor interface or virtual neighbor under discussion.


NeighborIfIndex ::= TEXTUAL-CONVENTION
   DISPLAY-HINT "d"
   STATUS       current
   DESCRIPTION
      "An arbitrary, locally unique identifier associated with a
       virtual interface of a discovered NHDP neighbor.
       Due to the nature of NHDP, the local router
       may not know if two distinct addresses belong to the
       same interface of a neighbor or to two different
       interfaces.  As the local router gains more
       knowledge of its neighbors, its local view may change, and
       this table will be updated to reflect the local router's
       current understanding, associating address sets to neighbor
       interfaces.  The local router identifies a virtual neighbor
       interface through the receipt of address lists advertised
       through an NHDP HELLO message.

       All objects of type NeighborIfIndex are assigned by the agent
       out of a common number space.

       The value for each discovered virtual neighbor
       interface may not remain constant from
       one re-initialization of the entity's network management
       agent to the next re-initialization.  If the
       local router gains information associating two virtual
       interfaces on a neighbor as a common interface,





       then the agent MUST aggregate the two address sets to
       a single index chosen from the set of aggregated indexes,
       and it MUST update all tables in this
       MIB module that are indexed by indexes
       of type NeighborIfIndex.  It MAY then reuse freed
       index values following the next agent restart.

       The specific value is meaningful only within a given SNMP
       entity."
    SYNTAX       Unsigned32 (1..2147483647)

NeighborRouterIndex ::= TEXTUAL-CONVENTION
   DISPLAY-HINT "d"
   STATUS       current
   DESCRIPTION
      "An arbitrary, locally unique identifier associated with a
       virtual discovered neighbor (one or two hop).  Due to the
       nature of NHDP, the local router may identify
       multiple virtual neighbors that, in fact, are one and
       the same.  Neighbors that are two hops away with more than
       one advertised address will exhibit this behavior.  As the
       local router's knowledge of its neighbors' topology
       increases, the local router will be able to associate
       multiple virtual neighbor indexes into a single virtual
       neighbor index chosen from the set of aggregated indexes;
       it MUST update all tables in this MIB module indexed by these
       indexes, and it MAY reuse the freed indexes following the
       next agent re-initialization.

       All objects of type NeighborRouterIndex are assigned by
       the agent out of a common number space.

       The NeighborRouterIndex defines a discovered NHDP peer
       virtual neighbor of the local router.
       The value for each discovered virtual neighbor index MUST
       remain constant at least from one re-initialization of
       the entity's network management agent to the next
       re-initialization, except if an application is deleted
       and re-created.

       The specific value is meaningful only within a given SNMP
       entity.  A NeighborRouterIndex value MUST NOT be reused
       until the next agent restart."
    SYNTAX       Unsigned32 (1..2147483647)









--
-- nhdpObjects
--

--    1) Configuration Objects Group
--    2) State Objects Group
--    3) Performance Objects Group
--
-- nhdpConfigurationObjGrp
--

-- Contains the NHDP objects that configure specific options
-- that determine the overall performance and operation of
-- NHDP.


nhdpConfigurationObjGrp  OBJECT IDENTIFIER ::= { nhdpObjects 1 }

   nhdpInterfaceTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpInterfaceEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The nhdpInterfaceTable describes the
          configuration of the interfaces of this router
          that are intended to use MANET control protocols.
          As such, this table 'sparse augments' the ifTable
          specifically when NHDP is to be configured to
          operate over this interface.  The interface is
          identified by the ifIndex from the Interfaces
          Group defined in the Interfaces Group MIB module.

          A conceptual row in this table exists if and only
          if the row has been administratively created
          or there is an interface on the managed device
          that supports and runs NHDP.

          A row can be administratively created by setting
          rowStatus to 'createAndGo' or 'createAndWait'.
          During the row creation, objects having associated
          DEFVAL clauses are automatically defined by
          the agent if not explicitly administratively defined.

          For each entry in the nhdpInterfaceTable, there is a
          corresponding entry in the Interface Table where
          nhdpIfIndex and ifIndex are equal.  If that corresponding
          entry in the Interface Table is deleted, then the entry in
          the nhdpInterfaceTable is automatically deleted,





          NHDP is disabled on this interface, and all configuration
          and state information related to this interface is to be
          removed from memory."
      REFERENCE
         "RFC 2863 - The Interfaces Group MIB, McCloghrie,
          K., and F. Kastenholtz, June 2000"
   ::= { nhdpConfigurationObjGrp 1 }

   nhdpInterfaceEntry  OBJECT-TYPE
      SYNTAX      NhdpInterfaceEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The nhdpInterfaceEntry describes one NHDP
          local interface configuration as indexed by
          its ifIndex as defined in the Standard MIB II
          Interface Table (RFC 2863).

          The objects in this table are persistent, and when
          written, the device SHOULD save the change to
          nonvolatile storage.  For further information
          on the storage behavior for these objects, refer
          to the description for the nhdpIfRowStatus
          object."
      INDEX { nhdpIfIndex }
   ::= { nhdpInterfaceTable 1 }

   NhdpInterfaceEntry ::=
      SEQUENCE {
         nhdpIfIndex
            InterfaceIndex,
         nhdpIfName
            SnmpAdminString,
         nhdpIfStatus
            TruthValue,
         nhdpHelloInterval
            Unsigned32,
         nhdpHelloMinInterval
            Unsigned32,
         nhdpRefreshInterval
            Unsigned32,
         nhdpLHoldTime
            Unsigned32,
         nhdpHHoldTime
            Unsigned32,
         nhdpHystAcceptQuality
            Float32TC,






         nhdpHystRejectQuality
            Float32TC,
         nhdpInitialQuality
            Float32TC,
         nhdpInitialPending
            TruthValue,
         nhdpHpMaxJitter
            Unsigned32,
         nhdpHtMaxJitter
            Unsigned32,
         nhdpIfRowStatus
            RowStatus
      }

   nhdpIfIndex  OBJECT-TYPE
      SYNTAX      InterfaceIndex
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This value MUST correspond to an ifIndex referring
          to a valid entry in the Interfaces Table."
      REFERENCE
         "RFC 2863 - The Interfaces Group MIB, McCloghrie, K.,
          and F. Kastenholtz, June 2000"
   ::= { nhdpInterfaceEntry 1 }

   nhdpIfName  OBJECT-TYPE
      SYNTAX      SnmpAdminString
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The textual name of the interface.  The value of this
          object SHOULD be the name of the interface as assigned by
          the local device.  This can be a text-name, such as 'le0'
          or a simple port number, such as '1',
          depending on the interface-naming syntax of the device.

          If there is no local name or this object is otherwise not
          applicable, then this object contains a zero-length string."
   ::= { nhdpInterfaceEntry 2 }

   nhdpIfStatus  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-create
      STATUS      current








      DESCRIPTION
         "nhdpIfStatus indicates whether this interface is
          currently running NHDP.  A value of 'true(1)' indicates
          that NHDP is running on this interface.
          A value of 'false(2)' indicates that NHDP is not
          currently running on this interface.  This corresponds
          to the I_manet parameter in the Local Interface Set
          of NHDP."
      DEFVAL { false }
   ::= { nhdpInterfaceEntry 3 }

   --
   -- Interface Parameters - Message Intervals
   --


   nhdpHelloInterval  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpHelloInterval corresponds to
          HELLO_INTERVAL of NHDP and represents the
          maximum time between the transmission of two
          successive HELLO messages on this MANET interface.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),
          which indicates that:
             o nhdpHelloInterval > 0
             o nhdpHelloInterval >= nhdpHelloMinInterval"
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc
          Network (MANET) Neighborhood Discovery
          Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      DEFVAL { 2000 }
   ::= { nhdpInterfaceEntry 4 }

   nhdpHelloMinInterval  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current







      DESCRIPTION
         "nhdpHelloMinInterval corresponds to
          HELLO_MIN_INTERVAL of NHDP and represents
          the minimum interval between transmission
          of two successive HELLO messages on this
          MANET interface.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),
          which indicates that:
             o nhdpHelloMinInterval <= nhdpHelloInterval"
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
      DEFVAL { 500 }
   ::= { nhdpInterfaceEntry 5 }

   nhdpRefreshInterval  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpRefreshInterval corresponds to
          REFRESH_INTERVAL of NHDP and represents the
          maximum interval between advertisements of
          each 1-hop neighbor network address and its
          status.  Each advertisement is in a HELLO
          message on this MANET interface.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),
          which indicates that:
             o nhdpRefreshInterval >= nhdpHelloInterval"
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
      DEFVAL { 2000 }
   ::= { nhdpInterfaceEntry 6 }

   --
   -- Interface Parameters - Information Validity times
   --






   nhdpLHoldTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpLHoldTime corresponds to
          L_HOLD_TIME of NHDP and represents the period
          of advertisement, on this MANET interface, of
          former 1-hop neighbor network addresses as lost
          in HELLO messages, allowing recipients of these
          HELLO messages to accelerate removal of this
          information from their Link Sets.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),
          which indicates that it should be assigned a
          value significantly greater than the refresh
          interval held by nhdpRefreshInterval."
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
      DEFVAL { 6000 }
   ::= { nhdpInterfaceEntry 7 }

   nhdpHHoldTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpHHoldTime corresponds to
          H_HOLD_TIME of NHDP and is used as the value
          in the VALIDITY_TIME Message TLV included in all
          HELLO messages on this MANET interface.  It is then
          used by each router receiving such a HELLO message
          to indicate the validity of the information taken
          from that HELLO message and recorded in the receiving
          router's Information Bases.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),
          which indicates that it should be assigned a
          value significantly greater than the refresh interval
          held by nhdpRefreshInterval and must be representable
          as described in RFC 5497."





      REFERENCE
         "RFC 5497 - Representing Multi-Value Time in Mobile Ad
          Hoc Networks (MANETs), Clausen, T., and C. Dearlove,
          March 2009.

          Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
      DEFVAL { 6000 }
   ::= { nhdpInterfaceEntry 8 }

   --
   -- Interface Parameters - Link Quality
   --

   nhdpHystAcceptQuality  OBJECT-TYPE
      SYNTAX      Float32TC
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpHystAcceptQuality corresponds to
          HYST_ACCEPT of NHDP and represents the link
          quality threshold at or above which a link becomes
          usable, if it was not already so.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),
          which indicates that:
             o 0 <= nhdpHystRejectQuality
                 <= nhdpHystAcceptQuality <= 1.0

          The default value for this object is 1.0. According to
          RFC 6340:
             Since these textual conventions are defined in terms
             of the OCTET STRING type, the SMI's mechanisms for
             formally setting range constraints are not available.
             MIB designers using these textual conventions will need
             to use DESCRIPTION clauses to spell out any applicable
             range constraints beyond those implied by the underlying
             IEEE types.
          Therefore, this object does not have a DEFVAL clause."
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
--    DEFVAL { 1.0 }   see DESCRIPTION





   ::= { nhdpInterfaceEntry 9 }

   nhdpHystRejectQuality  OBJECT-TYPE
      SYNTAX      Float32TC
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpHystRejectQuality corresponds to
          HYST_REJECT of NHDP and represents the
          link quality threshold below which a
          link becomes unusable, if it was not
          already so.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),
          which indicates that:
             o 0 <= nhdpHystRejectQuality
                 <= nhdpHystAcceptQuality <= 1.0

          The default value for this object is 0.0. According to
          RFC 6340:
             Since these textual conventions are defined in terms
             of the OCTET STRING type, the SMI's mechanisms for
             formally setting range constraints are not available.
             MIB designers using these textual conventions will need
             to use DESCRIPTION clauses to spell out any applicable
             range constraints beyond those implied by the underlying
             IEEE types.
          Therefore, this object does not have a DEFVAL clause."
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
--    DEFVAL { 0.0 }   see DESCRIPTION
   ::= { nhdpInterfaceEntry 10 }

   nhdpInitialQuality  OBJECT-TYPE
      SYNTAX      Float32TC
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpInitialQuality corresponds to
          INITIAL_QUALITY of NHDP and represents the
          initial quality of a newly identified link.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),





          which indicates that:
             o 0 <= nhdpInitialQuality <= 1.0

          The default value for this object is 1.0. According to
          RFC 6340:
             Since these textual conventions are defined in terms
             of the OCTET STRING type, the SMI's mechanisms for
             formally setting range constraints are not available.
             MIB designers using these textual conventions will need
             to use DESCRIPTION clauses to spell out any applicable
             range constraints beyond those implied by the underlying
             IEEE types.
          Therefore, this object does not have a DEFVAL clause."
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
--    DEFVAL { 1.0 }   see DESCRIPTION
   ::= { nhdpInterfaceEntry 11 }

   nhdpInitialPending  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpInitialPending corresponds to
          INITIAL_PENDING of NHDP.  If the value of this object
          is 'true(1)', then a newly identified link is considered
          pending and is not usable until the link quality
          has reached or exceeded the nhdpHystAcceptQuality
          threshold.

          Guidance for setting this object may be found
          in Section 5 of the NHDP specification (RFC 6130),
          which indicates that:
             o If nhdpInitialQuality >= nhdpHystAcceptQuality,
               then nhdpInitialPending := false(2).
             o If nhdpInitialQuality < nhdpHystRejectQuality,
               then nhdpInitialPending := true(1)."
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
      DEFVAL { false }
   ::= { nhdpInterfaceEntry 12 }






   --
   -- Interface Parameters - Jitter
   --
   nhdpHpMaxJitter  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpHpMaxJitter corresponds to
          HP_MAXJITTER of NHDP and represents the
          value of MAXJITTER used in RFC 5148 for
          periodically generated HELLO messages on
          this MANET interface.

          Guidance for setting this object may be found
          in Section 5 of RFC 5148, which indicates that:
             o nhdpHpMaxJitter <= nhdpHelloInterval / 2
             o nhdpHpMaxJitter should not be greater
               than nhdpHelloInterval / 4
             o If nhdpMinHelloInterval > 0, then
               nhdpHpMaxJitter <= nhdpHelloMinInterval; and
               nhdpHpMaxJitter should not be greater than
               nhdpHelloMinInterval / 2"
      REFERENCE
         "Section 5 of RFC 5148 - Jitter Considerations in
          Mobile Ad Hoc Networks (MANETs),
          Clausen, T., Dearlove, C., and B. Adamson, February 2008"
      DEFVAL { 500 }
   ::= { nhdpInterfaceEntry 13 }


   nhdpHtMaxJitter  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpHtMaxJitter corresponds to
          HT_MAXJITTER of NHDP and represents the
          value of MAXJITTER used in RFC 5148 for
          externally triggered HELLO messages on this
          MANET interface.

          Guidance for setting this object may be found
          in Section 5 of RFC 5148, which indicates that:
             o nhdpHtMaxJitter <= nhdpHelloInterval / 2






             o nhdpHtMaxJitter should not be greater
               than nhdpHelloInterval / 4
             o If nhdpMinHelloInterval > 0, then
               nhdpHtMaxJitter <= nhdpHelloMinInterval; and
               nhdpHtMaxJitter should not be greater than
               nhdpHelloMinInterval / 2"
      REFERENCE
         "Section 5 of RFC 5148 - Jitter Considerations in
          Mobile Ad Hoc Networks (MANETs),
          Clausen, T., Dearlove, C., and B. Adamson, February 2008"
      DEFVAL { 500 }
   ::= { nhdpInterfaceEntry 14 }

   nhdpIfRowStatus  OBJECT-TYPE
      SYNTAX      RowStatus
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "This object permits management of the table
          by facilitating actions such as row creation,
          construction, and destruction.  The value of
          this object has no effect on whether other
          objects in this conceptual row can be
          modified.

          An entry may not exist in the 'active(1)' state unless all
          objects in the entry have a defined appropriate value.  For
          objects with DEFVAL clauses, the management station
          does not need to specify the value of this object in order
          for the row to transit to the 'active(1)' state; the default
          value for this object is used.  For objects that do not
          have DEFVAL clauses, the value of this object prior
          to this row transitioning to the 'active(1)' state MUST be
          administratively specified.


          When this object transitions to 'active(1)', all objects
          in this row SHOULD be written to nonvolatile (stable)
          storage.  Read-create objects in this row MAY be modified.
          When an object in a row with nhdpIfRowStatus of 'active(1)'
          is changed, then the updated value MUST be reflected in NHDP,
          and this new object value MUST be written to nonvolatile
          storage.

          If the value of this object is not equal to 'active(1)',
          all associated entries in the nhdpLibLocalIfSetTable,
          nhdpInterfaceStateTable, nhdpIibLinkSetTable, and
          nhdpInterfacePerfTable MUST be deleted."





      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      DEFVAL { active }
   ::= { nhdpInterfaceEntry 15 }


   --
   -- Router Parameters - Information Validity Time
   --
   nhdpNHoldTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "nhdpNHoldTime corresponds to
          N_HOLD_TIME of NHDP and is used as the period
          during which former 1-hop neighbor network
          addresses are advertised as lost in HELLO
          messages, allowing recipients of these HELLO
          messages to accelerate removal of this information
          from their 2-Hop Sets.

          This object is persistent, and when written,
          the entity SHOULD save the change to
          nonvolatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
      DEFVAL { 6000 }
   ::= { nhdpConfigurationObjGrp 2 }

   nhdpIHoldTime  OBJECT-TYPE
      SYNTAX      Unsigned32
      UNITS       "milliseconds"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "nhdpIHoldTime corresponds to
          I_HOLD_TIME of NHDP and represents the period
          for which a recently used local interface network
          address is recorded.







          This object is persistent, and when written,
          the entity SHOULD save the change to
          nonvolatile storage."
      REFERENCE
         "Section 5 on Protocol Parameters and
          Constraints of RFC 6130 - Mobile Ad Hoc Network
          (MANET) Neighborhood Discovery Protocol (NHDP),
          Clausen, T., Dearlove, C., and J. Dean, April 2011"
      DEFVAL { 6000 }
   ::= { nhdpConfigurationObjGrp 3 }


   -- A router's Local Information Base (LIB)
   --
   -- Local Interface Set Table
   --

   nhdpLibLocalIfSetTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpLibLocalIfSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Local Interface Set records all
          network addresses that are defined as local
          MANET interface network addresses.
          As such, this table 'sparse augments' the
          nhdpInterfaceTable when network addresses are
          being defined for the interfaces existing within
          the nhdpInterfaceTable.  The local interface
          is defined by the nhdpIfIndex.

          The Local Interface Set consists of Local Interface
          Address Tuples per MANET interface and their prefix
          lengths (in order to determine the network addresses
          related to the interface).

          A conceptual row in this table exists if and only
          if one has been administratively created.  This can be done
          by setting rowStatus to 'createAndGo' or 'createAndWait'.

          Further guidance on the addition or removal of
          local addresses and network addresses is found
          in Section 9 of RFC 6130."
      REFERENCE
          "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
           Discovery Protocol (NHDP), Clausen, T., Dearlove,
           C., and J. Dean, April 2011"
   ::= { nhdpConfigurationObjGrp 4 }





   nhdpLibLocalIfSetEntry  OBJECT-TYPE
      SYNTAX      NhdpLibLocalIfSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Local Interface Set consists
          of Local Interface Tuples for each network
          interface.

          The objects in this table are persistent, and when
          written, the device SHOULD save the change to
          nonvolatile storage.  For further information
          on the storage behavior for these objects, refer
          to the description for the nhdpLibLocalIfSetRowStatus
          object."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpLibLocalIfSetIndex }
   ::= { nhdpLibLocalIfSetTable 1 }

   NhdpLibLocalIfSetEntry ::=
      SEQUENCE {
         nhdpLibLocalIfSetIndex
            Integer32,
         nhdpLibLocalIfSetIfIndex
            InterfaceIndex,
         nhdpLibLocalIfSetIpAddrType
            InetAddressType,
         nhdpLibLocalIfSetIpAddr
            InetAddress,
         nhdpLibLocalIfSetIpAddrPrefixLen
            InetAddressPrefixLength,
         nhdpLibLocalIfSetRowStatus
            RowStatus
      }

   nhdpLibLocalIfSetIndex  OBJECT-TYPE
      SYNTAX      Integer32 (0..65535)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The index for this table.  Necessary
          because multiple addresses may be associated
          with a given nhdpIfIndex."







      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibLocalIfSetEntry 1 }

   nhdpLibLocalIfSetIfIndex  OBJECT-TYPE
      SYNTAX      InterfaceIndex
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Specifies the local nhdpIfIndex for which this
          IP address was added."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibLocalIfSetEntry 2 }

   nhdpLibLocalIfSetIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "The type of the nhdpLibLocalIfSetIpAddr
          in the InetAddress MIB (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibLocalIfSetEntry 3 }

   nhdpLibLocalIfSetIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "nhdpLibLocalIfSetIpAddr is an
          address of an interface of
          this router.

          This object is interpreted according to
          the setting of nhdpLibLocalIfSetIpAddrType."







      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
         C., and J. Dean, April 2011"
   ::= { nhdpLibLocalIfSetEntry 4 }

   nhdpLibLocalIfSetIpAddrPrefixLen  OBJECT-TYPE
      SYNTAX      InetAddressPrefixLength
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "Indicates the number of leading one bits that
          form the mask.  The mask is logically ANDed
          to the nhdpLibLocalIfSetIpAddr to determine
          the address prefix.  A row match is true
          if the address used as an index falls within
          the network address range defined by the
          address prefix."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibLocalIfSetEntry 5 }

   nhdpLibLocalIfSetRowStatus  OBJECT-TYPE
      SYNTAX      RowStatus
      MAX-ACCESS  read-create
      STATUS      current
      DESCRIPTION
         "This object permits management of the table
          by facilitating actions such as row creation,
          construction, and destruction.  The value of
          this object has no effect on whether other
          objects in this conceptual row can be
          modified.

          An entry may not exist in the 'active(1)' state unless all
          read-create objects in the entry have a defined
          appropriate value.  As no objects in this table have
          DEFVAL clauses, the management station MUST specify
          the values of all read-create objects prior to this row
          transitioning to the 'active(1)' state.

          When this object transitions to 'active(1)', all objects
          in this row SHOULD be written to nonvolatile (stable)
          storage.  Read-create objects in this row MAY be modified.
          When an object in a row with nhdpIfRowStatus of 'active(1)'
          is changed, then the updated value MUST be reflected in NHDP,





          and this new object value MUST be written to nonvolatile
          storage."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      DEFVAL { notReady }
    ::= { nhdpLibLocalIfSetEntry 6 }



   --
   -- Removed Interface Addr Set Table
   --

   nhdpLibRemovedIfAddrSetTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpLibRemovedIfAddrSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Removed Interface Address Set records
          network addresses that were recently used as local
          interface network addresses.  If a router's interface
          network addresses are immutable, then the Removed
          Interface Address Set is always empty and may be omitted.
          It consists of Removed Interface Address Tuples, one
          per network address."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpConfigurationObjGrp 5 }

   nhdpLibRemovedIfAddrSetEntry  OBJECT-TYPE
      SYNTAX      NhdpLibRemovedIfAddrSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Removed Interface Address Set consists
          of Removed Interface Address Tuples, one per network
          address:

          (IR_local_iface_addr, IR_time)

          The association between these addresses and the
          router's Interface is found in RFC 4293 (ipAddressTable)"







      REFERENCE
         "RFC 4293 - Management Information Base for the Internet
          Protocol (IP), S. Routhier, Ed., April 2006.

          RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpLibRemovedIfAddrSetIndex }
   ::= { nhdpLibRemovedIfAddrSetTable 1 }

   NhdpLibRemovedIfAddrSetEntry ::=
      SEQUENCE {
         nhdpLibRemovedIfAddrSetIndex
            Integer32,
         nhdpLibRemovedIfAddrSetIpAddrType
            InetAddressType,
         nhdpLibRemovedIfAddrSetIpAddr
            InetAddress,
         nhdpLibRemovedIfAddrSetIpAddrPrefixLen
            InetAddressPrefixLength,
         nhdpLibRemovedIfAddrSetIfIndex
            InterfaceIndex,
         nhdpLibRemovedIfAddrSetIRTime
            TimeStamp
      }

   nhdpLibRemovedIfAddrSetIndex  OBJECT-TYPE
      SYNTAX      Integer32 (0..65535)
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The index for this table.  Necessary
          because multiple addresses may be associated
          with a given nhdpIfIndex."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibRemovedIfAddrSetEntry 1 }

   nhdpLibRemovedIfAddrSetIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The type of the nhdpLibRemovedIfAddrSetIpAddr
          in the InetAddress MIB (RFC 4001).






          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibRemovedIfAddrSetEntry 2 }

   nhdpLibRemovedIfAddrSetIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpLibRemovedIfAddrSetIpAddr is a
          recently used address of an interface of
          this router."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibRemovedIfAddrSetEntry 3 }

   nhdpLibRemovedIfAddrSetIpAddrPrefixLen  OBJECT-TYPE
      SYNTAX      InetAddressPrefixLength
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Indicates the number of leading one bits that
          form the mask.  The mask is logically ANDed
          to the nhdpLibRemovedIfAddrSetIpAddr to determine
          the address prefix.  A row match is true
          if the address used as an index falls within
          the network address range defined by the
          address prefix."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibRemovedIfAddrSetEntry 4 }

   nhdpLibRemovedIfAddrSetIfIndex  OBJECT-TYPE
      SYNTAX      InterfaceIndex
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Specifies the local IfIndex from which this
          IP address was recently removed."






      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibRemovedIfAddrSetEntry 5 }

   nhdpLibRemovedIfAddrSetIRTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpLibRemovedIfAddrSetIRTime specifies the value
          of sysUpTime when this entry should expire and be
          removed from the nhdpLibRemovedIfAddrSetTable."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpLibRemovedIfAddrSetEntry 6 }

--
-- nhdpStateObjGrp
--

-- Contains information describing the current state of the NHDP
-- process on this router.

nhdpStateObjGrp  OBJECT IDENTIFIER ::= { nhdpObjects 2 }

   nhdpUpTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The value of sysUpTime at the time the current NHDP
          process was initialized."
   ::= { nhdpStateObjGrp 1 }

   nhdpInterfaceStateTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpInterfaceStateEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "nhdpInterfaceStateTable lists state information
          related to specific interfaces of this router.
          The value of nhdpIfIndex is an ifIndex from the
          Interfaces Group defined in the Interfaces Group
          MIB.





          The objects in this table are persistent, and when
          written, the entity SHOULD save the change to
          nonvolatile storage."
      REFERENCE
         "RFC 2863 - The Interfaces Group MIB, McCloghrie,
          K., and F. Kastenholtz, June 2000"
   ::= { nhdpStateObjGrp 2 }

   nhdpInterfaceStateEntry  OBJECT-TYPE
      SYNTAX      NhdpInterfaceStateEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "nhdpInterfaceStateEntry describes one NHDP
          local interface state as indexed by
          its nhdpIfIndex."
      INDEX { nhdpIfIndex }
   ::= { nhdpInterfaceStateTable 1 }

   NhdpInterfaceStateEntry ::=
      SEQUENCE {
         nhdpIfStateUpTime
            TimeStamp
         }

   nhdpIfStateUpTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The value of the sysUpTime when
          NHDP was last initialized on this
          MANET interface."
   ::= { nhdpInterfaceStateEntry 1 }


   --
   -- This table allows for the mapping between discovered
   -- remote interfaces and routers and their addresses.
   --

   nhdpDiscIfSetTable OBJECT-TYPE
      SYNTAX       SEQUENCE OF NhdpDiscIfSetEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
         "A router's set of discovered interfaces on
          neighboring routers."





      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpStateObjGrp 3 }

   nhdpDiscIfSetEntry  OBJECT-TYPE
      SYNTAX      NhdpDiscIfSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The entries include the nhdpDiscRouterIndex of
          the discovered router, the nhdpDiscIfIndex
          of the discovered interface, and the
          current set of addresses associated
          with this neighbor interface.  The
          nhdpDiscIfIndex uniquely identifies
          the remote interface address sets
          through this table.  It does not need
          to be unique across the MANET but MUST
          be locally unique within this router."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpDiscIfSetIndex }
   ::= { nhdpDiscIfSetTable 1 }

   NhdpDiscIfSetEntry ::=
      SEQUENCE {
         nhdpDiscIfSetIndex
            Integer32,
         nhdpDiscIfIndex
            NeighborIfIndex,
         nhdpDiscRouterIndex
            NeighborRouterIndex,
         nhdpDiscIfSetIpAddrType
            InetAddressType,
         nhdpDiscIfSetIpAddr
            InetAddress,
         nhdpDiscIfSetIpAddrPrefixLen
            InetAddressPrefixLength
      }

   nhdpDiscIfSetIndex  OBJECT-TYPE
      SYNTAX      Integer32 (0..65535)
      MAX-ACCESS  not-accessible
      STATUS      current





      DESCRIPTION
         "The index for this table.  Necessary
          because multiple addresses may be associated
          with a given nhdpDiscIfIndex."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscIfSetEntry 1 }

   nhdpDiscIfIndex  OBJECT-TYPE
      SYNTAX      NeighborIfIndex
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The NHDP interface index (locally created)
          of a neighbor's interface.  Used for cross-
          indexing into other NHDP tables and other
          MIB modules."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscIfSetEntry 2 }

   nhdpDiscRouterIndex  OBJECT-TYPE
      SYNTAX      NeighborRouterIndex
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The NHDP neighbor index (locally created)
          of a neighboring router.  Used for cross-
          indexing into other NHDP tables and other
          MIB modules."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscIfSetEntry 3 }

   nhdpDiscIfSetIpAddrType  OBJECT-TYPE
      SYNTAX      InetAddressType
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The type of the nhdpDiscIfSetIpAddr
          in the InetAddress MIB (RFC 4001).






          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscIfSetEntry 4 }

   nhdpDiscIfSetIpAddr  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The nhdpDiscIfSetIpAddr is a
          recently used address of a neighbor
          of this router."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscIfSetEntry 5 }

   nhdpDiscIfSetIpAddrPrefixLen  OBJECT-TYPE
      SYNTAX      InetAddressPrefixLength
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Indicates the number of leading one bits that
          form the mask.  The mask is logically ANDed
          to the nhdpDiscIfSetIpAddr to determine
          the address prefix.  A row match is true
          if the address used as an index falls within
          the network address range defined by the
          address prefix."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscIfSetEntry 6 }


   -- Interface Information Base (IIB)

   --
   -- Link Set
   --







   nhdpIibLinkSetTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpIibLinkSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A Link Set of an interface records all links
          from other routers that are, or recently
          were, 1-hop neighbors."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpStateObjGrp 4 }

   nhdpIibLinkSetEntry  OBJECT-TYPE
      SYNTAX      NhdpIibLinkSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A Link Set consists of Link Tuples, each
          representing a single link indexed by the
          local and remote interface pair:

          (L_neighbor_iface_addr_list, L_HEARD_time,
           L_SYM_time, L_quality, L_pending,
           L_lost, L_time).

          The local interface is indexed via the
          nhdpIfIndex.  The 1-hop interface is
          indexed via the nhdpDiscIfIndex.  There
          SHOULD be an entry in this table for each
          local interface and associated 1-hop
          neighbor reachable on this local interface.

          Note that L_quality is not included in the
          entries below, because updates may be
          required too frequently."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpIfIndex,
              nhdpDiscIfIndex }
   ::= { nhdpIibLinkSetTable 1 }









   NhdpIibLinkSetEntry ::=
      SEQUENCE {
         nhdpIibLinkSetLHeardTime
            TimeStamp,
         nhdpIibLinkSetLSymTime
            TimeStamp,
         nhdpIibLinkSetLPending
            TruthValue,
         nhdpIibLinkSetLLost
            TruthValue,
         nhdpIibLinkSetLTime
            TimeStamp
      }

   nhdpIibLinkSetLHeardTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpIibLinkSetLHeardTime corresponds
          to L_HEARD_time of NHDP and represents the
          time up to which the MANET interface of the
          1-hop neighbor would be considered heard if
          not considering link quality."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIibLinkSetEntry 1 }

   nhdpIibLinkSetLSymTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpIibLinkSetLSymTime corresponds
          to L_SYM_time of NHDP and represents the time
          up to which the link to the 1-hop neighbor
          would be considered symmetric if not considering
          link quality."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIibLinkSetEntry 2 }








   nhdpIibLinkSetLPending  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpIibLinkSetLPending corresponds
          to L_pending of NHDP and is a boolean flag,
          describing if a link is considered pending
          (i.e., a candidate, but not yet established,
          link)."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIibLinkSetEntry 3 }

   nhdpIibLinkSetLLost  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpIibLinkSetLLost corresponds
          to L_lost of NHDP and is a boolean flag,
          describing if a link is considered lost due
          to low link quality."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIibLinkSetEntry 4 }

   nhdpIibLinkSetLTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpIibLinkSetLTime specifies the value
          of sysUpTime when this entry should expire and be
          removed from the nhdpIibLinkSetTable."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIibLinkSetEntry 5 }









   --
   -- 2-Hop Set
   --
   nhdpIib2HopSetTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpIib2HopSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A 2-Hop Set of an interface records network
          addresses of symmetric 2-hop neighbors and
          the symmetric links to symmetric 1-hop neighbors
          through which these symmetric 2-hop neighbors
          can be reached.  It consists of 2-Hop Tuples."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpStateObjGrp 5 }

   nhdpIib2HopSetEntry  OBJECT-TYPE
      SYNTAX      NhdpIib2HopSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "nhdpIib2HopSetTable consists of 2-Hop Tuples, each
          representing a single network address of a symmetric
          2-hop neighbor and a single MANET interface of a
          symmetric 1-hop neighbor.

          (N2_neighbor_iface_addr_list,
           N2_2hop_addr, N2_lost, N2_time).

          The entries include:
            - the 2-hop neighbor addresses
              ('N2_neighbor_iface_addr_list'), which
              act as the table index,
            - the associated symmetric 1-hop
              neighbor address set ('N2_2hop_addr'), designated
              through nhdpDiscIfIndex,
            - a flag indicating if the 1-hop neighbor
              through which this 2-hop neighbor is reachable
              ('N2_lost') is considered lost due to link quality,
              or not,
            - and the expiration time ('N2_time').

          The nhdpIfIndex in the INDEX is the interface index of
          the local interface through which these 2-hop addresses
          are accessible.  The nhdpDiscIfIndex in the INDEX





          represents the 1-hop neighbor interface through which
          these 2-hop neighbor addresses are reachable."

      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011
          and
          RFC 7466 - An Optimization for the Mobile Ad Hoc
          Network (MANET) Neighborhood Discovery Protocol (NHDP),
          Dearlove, C., and T. Clausen, March 2015"
      INDEX { nhdpIfIndex,
              nhdpDiscIfIndex,
              nhdpIib2HopSetIpAddressType,
              nhdpIib2HopSetIpAddress
      }
   ::= { nhdpIib2HopSetTable 1 }

   NhdpIib2HopSetEntry ::=
      SEQUENCE {
         nhdpIib2HopSetIpAddressType
            InetAddressType,
         nhdpIib2HopSetIpAddress
            InetAddress,
         nhdpIib2HopSetIpAddrPrefixLen
            InetAddressPrefixLength,
         nhdpIib2HopSet1HopIfIndex
            NeighborIfIndex,
         nhdpIib2HopSetN2Time
            TimeStamp,
         nhdpIib2HopSetN2Lost
            TruthValue
      }

   nhdpIib2HopSetIpAddressType  OBJECT-TYPE
      SYNTAX      InetAddressType
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The type of the nhdpIib2HopSetIpAddress
          in the InetAddress MIB module (RFC 4001).

          Only the values 'ipv4(1)' and
          'ipv6(2)' are supported."









      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIib2HopSetEntry 1 }

   nhdpIib2HopSetIpAddress  OBJECT-TYPE
      SYNTAX      InetAddress (SIZE(4|16))
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "nhdpIib2HopSetIpAddr corresponds
          to N2_2hop_addr of NHDP and is a network
          address of a symmetric 2-hop neighbor that
          has a symmetric link (using any MANET
          interface) to the indicated symmetric
          1-hop neighbor."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIib2HopSetEntry 2 }

   nhdpIib2HopSetIpAddrPrefixLen  OBJECT-TYPE
      SYNTAX      InetAddressPrefixLength
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "Indicates the number of leading one bits that
          form the mask.  The mask is logically ANDed
          to the nhdpIib2HopSetIpAddress to determine
          the address prefix.  A row match is true
          if the address used as an index falls within
          the network address range defined by the
          address prefix."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIib2HopSetEntry 3 }

   nhdpIib2HopSet1HopIfIndex  OBJECT-TYPE
      SYNTAX      NeighborIfIndex
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpIib2HopSet1HopIfIndex is
          nhdpDiscIfIndex of the 1-hop





          neighbor that communicated the ipAddress
          of the 2-hop neighbor in this row entry."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIib2HopSetEntry 4 }

   nhdpIib2HopSetN2Time  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpIib2HopSetN2Time specifies the value
          of sysUpTime when this entry should expire and be
          removed from the nhdpIib2HopSetTable."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIib2HopSetEntry 5 }


      nhdpIib2HopSetN2Lost OBJECT-TYPE
      SYNTAX          TruthValue
      MAX-ACCESS      read-only
      STATUS          current
      DESCRIPTION
         "nhdpIib2HopSetN2Lost corresponds to N2_lost of NHDP and
          is a boolean flag, describing if for a 2-Hop Tuple, the
          corresponding Link Tuple currently is considered lost
          due to link quality."

      REFERENCE
         "RFC 7466 - An Optimization for the Mobile Ad Hoc
          Network (MANET) Neighborhood Discovery Protocol (NHDP),
          Dearlove, C., and T. Clausen, March 2015"
   ::= {nhdpIib2HopSetEntry 6}


   --
   -- Neighbor Information Base (NIB)
   --
   -- Each router maintains a Neighbor Information Base
   -- that records information about addresses of
   -- current and recently symmetric 1-hop neighbors.







   --
   -- Neighbor Set
   --
   --     The Neighbor Set Table is small because
   --     most of the corresponding information is found
   --     in the nhdpDiscoveredIfTable above.
   --

   nhdpNibNeighborSetTable  OBJECT-TYPE
      SYNTAX       SEQUENCE OF NhdpNibNeighborSetEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
         "A router's Neighbor Set records all
          network addresses of each 1-hop
          neighbor."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpStateObjGrp 6 }

   nhdpNibNeighborSetEntry  OBJECT-TYPE
      SYNTAX      NhdpNibNeighborSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Neighbor Set consists
          of Neighbor Tuples, each representing
          a single 1-hop neighbor:

          (N_neighbor_addr_list, N_symmetric)"
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpDiscRouterIndex }
   ::= { nhdpNibNeighborSetTable 1 }

   NhdpNibNeighborSetEntry ::=
      SEQUENCE {
         nhdpNibNeighborSetNSymmetric
            TruthValue
      }

   nhdpNibNeighborSetNSymmetric  OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-only





      STATUS      current
      DESCRIPTION
         "nhdpNibNeighborNSymmetric corresponds
          to N_symmetric of NHDP and is a boolean flag,
          describing if this is a symmetric 1-hop neighbor."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpNibNeighborSetEntry 1 }


   --
   -- Lost Neighbor Set
   --
   nhdpNibLostNeighborSetTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpNibLostNeighborSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Lost Neighbor Set records network
          addresses of routers that were recently
          symmetric 1-hop neighbors but are now
          advertised as lost."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpStateObjGrp 7 }

   nhdpNibLostNeighborSetEntry  OBJECT-TYPE
      SYNTAX      NhdpNibLostNeighborSetEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A router's Lost Neighbor Set consists of
          Lost Neighbor Tuples, each representing a
          single such network address:

          (NL_neighbor_addr, NL_time)"
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpDiscRouterIndex }
   ::= { nhdpNibLostNeighborSetTable 1 }







   NhdpNibLostNeighborSetEntry ::=
      SEQUENCE {
         nhdpNibLostNeighborSetNLTime
            TimeStamp
      }

   nhdpNibLostNeighborSetNLTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "nhdpNibLostNeighborSetNLTime
          specifies the value of sysUpTime when this entry
          should expire and be removed from the
          nhdpNibLostNeighborSetTable."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpNibLostNeighborSetEntry 1 }


--
-- nhdpPerformanceObjGrp
--
-- Contains objects that help to characterize the performance of
-- the NHDP process, typically counters.
--
nhdpPerformanceObjGrp  OBJECT IDENTIFIER ::= { nhdpObjects 3 }

  --
  -- Objects per local interface
  --

  nhdpInterfacePerfTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpInterfacePerfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This table summarizes performance objects that are
          measured per local NHDP interface.
          nhdpIfPerfCounterDiscontinuityTime indicates
          the most recent occasion at which any one or more
          of this interface's counters listed in this table
          suffered a discontinuity."








      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpPerformanceObjGrp 1 }

   nhdpInterfacePerfEntry  OBJECT-TYPE
      SYNTAX      NhdpInterfacePerfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "A single entry contains performance counters for
          a local NHDP interface."
      INDEX { nhdpIfIndex }
   ::= { nhdpInterfacePerfTable 1 }

   NhdpInterfacePerfEntry ::=
      SEQUENCE {
         nhdpIfHelloMessageXmits
            Counter32,
         nhdpIfHelloMessageRecvd
            Counter32,
         nhdpIfHelloMessageXmitAccumulatedSize
            Counter64,
         nhdpIfHelloMessageRecvdAccumulatedSize
            Counter64,
         nhdpIfHelloMessageTriggeredXmits
            Counter32,
         nhdpIfHelloMessagePeriodicXmits
            Counter32,
         nhdpIfHelloMessageXmitAccumulatedSymmetricNeighborCount
            Counter32,
         nhdpIfHelloMessageXmitAccumulatedHeardNeighborCount
            Counter32,
         nhdpIfHelloMessageXmitAccumulatedLostNeighborCount
            Counter32,
         nhdpIfPerfCounterDiscontinuityTime
            TimeStamp
      }

   nhdpIfHelloMessageXmits  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented each time a HELLO
          message has been transmitted on that interface."





   ::= { nhdpInterfacePerfEntry 1 }

   nhdpIfHelloMessageRecvd  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented each time a HELLO
          message has been received on that interface."
   ::= { nhdpInterfacePerfEntry 2 }

   nhdpIfHelloMessageXmitAccumulatedSize  OBJECT-TYPE
      SYNTAX      Counter64
      UNITS       "octets"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented by the number of octets in
          a HELLO message each time a HELLO message has been sent."
   ::= { nhdpInterfacePerfEntry 3 }

   nhdpIfHelloMessageRecvdAccumulatedSize  OBJECT-TYPE
      SYNTAX      Counter64
      UNITS       "octets"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented by the number of octets in
          a HELLO message each time a HELLO message has been received."
   ::= { nhdpInterfacePerfEntry 4 }

   nhdpIfHelloMessageTriggeredXmits  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented each time a triggered
          HELLO message has been sent."
   ::= { nhdpInterfacePerfEntry 5 }

   nhdpIfHelloMessagePeriodicXmits  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "messages"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION





         "A counter is incremented each time a periodic
          HELLO message has been sent."
   ::= { nhdpInterfacePerfEntry 6 }

   nhdpIfHelloMessageXmitAccumulatedSymmetricNeighborCount  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "neighbors"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented by the number of advertised
          symmetric neighbors in a HELLO each time a HELLO
          message has been sent."
   ::= { nhdpInterfacePerfEntry 7 }

   nhdpIfHelloMessageXmitAccumulatedHeardNeighborCount  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "neighbors"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented by the number of advertised
          heard neighbors in a HELLO each time a HELLO
          message has been sent."
   ::= { nhdpInterfacePerfEntry 8 }

   nhdpIfHelloMessageXmitAccumulatedLostNeighborCount  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "neighbors"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "A counter is incremented by the number of advertised
          lost neighbors in a HELLO each time a HELLO
          message has been sent."
   ::= { nhdpInterfacePerfEntry 9 }

   nhdpIfPerfCounterDiscontinuityTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "The value of sysUpTime on the most recent occasion at which
          any one or more of this interface's counters suffered a
          discontinuity.  If no such discontinuities have occurred
          since the last reinitialization of the local management
          subsystem, then this object contains a zero value."
   ::= { nhdpInterfacePerfEntry 10 }





   --
   -- Objects per discovered neighbor interface
   --
   nhdpDiscIfSetPerfTable OBJECT-TYPE
      SYNTAX       SEQUENCE OF NhdpDiscIfSetPerfEntry
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
         "A router's set of performance properties for
          each discovered interface of a neighbor."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpPerformanceObjGrp 2 }

   nhdpDiscIfSetPerfEntry  OBJECT-TYPE
      SYNTAX      NhdpDiscIfSetPerfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "There is an entry for each discovered
          interface of a neighbor."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpDiscIfIndex }
   ::= { nhdpDiscIfSetPerfTable 1 }

   NhdpDiscIfSetPerfEntry ::=
      SEQUENCE {
         nhdpDiscIfRecvdPackets
            Counter32,
         nhdpDiscIfExpectedPackets
            Counter32
      }

   nhdpDiscIfRecvdPackets  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "packets"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This counter increments each
          time this router receives a packet from that interface
          of the neighbor."
      REFERENCE





         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
         C., and J. Dean, April 2011"
   ::= { nhdpDiscIfSetPerfEntry 1 }

   nhdpDiscIfExpectedPackets  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "packets"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This counter increments by the number
          of missed packets from this neighbor based
          on the packet sequence number each time this
          router receives a packet from that interface
          of the neighbor."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscIfSetPerfEntry 2 }


   --
   -- Objects concerning the Neighbor Set
   --
   nhdpNibNeighborSetChanges  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "changes"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This counter increments each time the Neighbor Set changes.
          A change occurs whenever a new Neighbor Tuple has been
          added, a Neighbor Tuple has been removed, or any entry of
          a Neighbor Tuple has been modified."
   ::= { nhdpPerformanceObjGrp 3 }


   --
   -- Objects per discovered neighbor
   --
   nhdpDiscNeighborSetPerfTable OBJECT-TYPE
      SYNTAX       SEQUENCE OF NhdpDiscNeighborSetPerfEntry
      MAX-ACCESS   not-accessible
      STATUS       current







      DESCRIPTION
         "A router's set of discovered neighbors and
          their properties."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpPerformanceObjGrp 4 }

   nhdpDiscNeighborSetPerfEntry  OBJECT-TYPE
      SYNTAX      NhdpDiscNeighborSetPerfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The entries include the nhdpDiscRouterIndex of
          the discovered router as well as performance
          objects related to changes of the Neighbor
          Set."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpDiscRouterIndex }
   ::= { nhdpDiscNeighborSetPerfTable 1 }

   NhdpDiscNeighborSetPerfEntry ::=
      SEQUENCE {
         nhdpDiscNeighborNibNeighborSetChanges
            Counter32,
         nhdpDiscNeighborNibNeighborSetUpTime
            TimeStamp,
         nhdpDiscNeighborNibNeighborSetReachableLinkChanges
            Counter32
      }

   nhdpDiscNeighborNibNeighborSetChanges  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "changes"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object returns the number of changes
          to the given Neighbor Tuple."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscNeighborSetPerfEntry 1 }





   nhdpDiscNeighborNibNeighborSetUpTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object returns the sysUpTime when a new
          nhdpNibNeighborSetEntry has been created for a
          particular nhdpNibNeighborSetRouterIndex."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscNeighborSetPerfEntry 2 }

   nhdpDiscNeighborNibNeighborSetReachableLinkChanges  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "changes"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object counts each time the neighbor changes
          the interface(s) over which it is reachable.
          A change in the set of Link Tuples corresponding
          to the appropriate Neighbor Tuple is registered,
          i.e., a corresponding Link Tuple is added or removed
          from the set of all corresponding Link Tuples."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpDiscNeighborSetPerfEntry 3 }


   --
   -- Objects per discovered 2-hop neighbor
   --
   nhdpIib2HopSetPerfTable  OBJECT-TYPE
      SYNTAX      SEQUENCE OF NhdpIib2HopSetPerfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "This table contains performance objects per
          discovered 2-hop neighbor."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpPerformanceObjGrp 5 }





   nhdpIib2HopSetPerfEntry  OBJECT-TYPE
      SYNTAX      NhdpIib2HopSetPerfEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
         "The entries contain performance objects per
          discovered 2-hop neighbor."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
      INDEX { nhdpDiscRouterIndex }
   ::= { nhdpIib2HopSetPerfTable 1 }

   NhdpIib2HopSetPerfEntry ::=
      SEQUENCE {
         nhdpIib2HopSetPerfChanges
            Counter32,
         nhdpIib2HopSetPerfUpTime
            TimeStamp
      }

   nhdpIib2HopSetPerfChanges  OBJECT-TYPE
      SYNTAX      Counter32
      UNITS       "changes"
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object counts the changes of the union of all
          N2_neighbor_iface_addr_list of 2-Hop Tuples with an
          N2_2hop_addr equal to one of the given 2-hop
          neighbor's addresses."
      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIib2HopSetPerfEntry 1 }

   nhdpIib2HopSetPerfUpTime  OBJECT-TYPE
      SYNTAX      TimeStamp
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "This object returns the sysUpTime
          when the 2-Hop Tuple
          corresponding to the given 2-hop neighbor IP address
          was registered in the nhdpIib2HopSetTable."






      REFERENCE
         "RFC 6130 - Mobile Ad Hoc Network (MANET) Neighborhood
          Discovery Protocol (NHDP), Clausen, T., Dearlove,
          C., and J. Dean, April 2011"
   ::= { nhdpIib2HopSetPerfEntry 2 }


--
-- nhdpNotifications
--

nhdpNotificationsObjects OBJECT IDENTIFIER ::= { nhdpNotifications 0 }
nhdpNotificationsControl OBJECT IDENTIFIER ::= { nhdpNotifications 1 }
nhdpNotificationsStates  OBJECT IDENTIFIER ::= { nhdpNotifications 2 }

   -- nhdpNotificationsObjects

   nhdpNbrStateChange  NOTIFICATION-TYPE
      OBJECTS { nhdpIfName,  -- The originator of the notification.
               nhdpNbrState  -- The new state
      }
      STATUS       current
      DESCRIPTION
         "nhdpNbrStateChange is a notification sent when
          more than nhdpNbrStateChangeThreshold neighbors change
          their status (i.e., 'down(0)', 'asymmetric(1)', or
          'symmetric(2)') within a time window of
          nhdpNbrStateChangeWindow."
   ::= { nhdpNotificationsObjects 1 }

   nhdp2HopNbrStateChange  NOTIFICATION-TYPE
      OBJECTS { nhdpIfName,      -- The originator
                                 -- of the notification
               nhdp2HopNbrState  -- The new state
      }
      STATUS      current
      DESCRIPTION
         "nhdp2HopNbrStateChange is a notification sent
          when more than nhdp2HopNbrStateChangeThreshold 2-hop
          neighbors change their nhdp2HopNbrState
          within a time window of
          nhdp2HopNbrStateChangeWindow."
   ::= { nhdpNotificationsObjects 2 }










   nhdpIfStateChange  NOTIFICATION-TYPE
      OBJECTS { nhdpIfName,  -- The local interface
               nhdpIfStatus  -- The new status
      }
      STATUS       current
      DESCRIPTION
         "nhdpIfStateChange is a notification sent when
          nhdpIfStatus has changed on this interface."
   ::= { nhdpNotificationsObjects 3 }

   -- nhdpNotificationsControl

   nhdpNbrStateChangeThreshold  OBJECT-TYPE
      SYNTAX      Integer32 (0..255)
      UNITS       "changes"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "A threshold value for the
          nhdpNbrStateChange object.  If the
          number of occurrences exceeds this threshold
          within the previous nhdpNbrStateChangeWindow,
          then the nhdpNbrStateChange notification
          is to be sent.

          It is recommended that the value of this
          threshold be set to at least 10 and higher
          in dense topologies with frequent expected
          topology changes."
      DEFVAL { 10 }
   ::= { nhdpNotificationsControl 1 }

   nhdpNbrStateChangeWindow  OBJECT-TYPE
      SYNTAX      TimeTicks
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "A time window for the
          nhdpNbrStateChange object.  If the
          number of occurrences exceeds the
          nhdpNbrStateChangeThreshold
          within the previous nhdpNbrStateChangeWindow,
          then the nhdpNbrStateChange notification
          is to be sent.

          It is recommended that the value for this
          window be set to at least 5 times the
          nhdpHelloInterval.





          This object represents the time in hundredths
          of a second."
      DEFVAL { 1000 }
   ::= { nhdpNotificationsControl 2 }

   nhdp2HopNbrStateChangeThreshold  OBJECT-TYPE
      SYNTAX      Integer32 (0..255)
      UNITS       "changes"
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "A threshold value for the
          nhdp2HopNbrStateChange object.  If the
          number of occurrences exceeds this threshold
          within the previous nhdp2HopNbrStateChangeWindow,
          then the nhdp2HopNbrStateChange notification
          is to be sent.

          It is recommended that the value of this
          threshold be set to at least 10 and higher
          when topologies are expected to be highly dynamic."
      DEFVAL { 10 }
   ::= { nhdpNotificationsControl 3 }

   nhdp2HopNbrStateChangeWindow  OBJECT-TYPE
      SYNTAX      TimeTicks
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
         "A time window for the
          nhdp2HopNbrStateChange object.  If the
          number of occurrences exceeds the
          nhdp2HopNbrStateChangeThreshold
          within the previous nhdp2HopNbrStateChangeWindow,
          then the nhdp2HopNbrStateChange notification
          is to be sent.

          It is recommended that the value for this
          window be set to at least 5 times
          nhdpHelloInterval.

          This object represents the time in hundredths
          of a second."
      DEFVAL { 1000 }
   ::= { nhdpNotificationsControl 4 }








    -- nhdpNotificationStates

   nhdpNbrState OBJECT-TYPE
      SYNTAX      INTEGER {
                     down(0),
                     asymmetric(1),
                     symmetric(2)
                  }
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
         "NHDP neighbor states.  In NHDP, it is not
          necessary to remove Protocol Tuples from Protocol Sets
          at the exact time indicated, only to behave as if the
          Protocol Tuples were removed at that time.  This case is
          indicated here as 'down(0)', all other cases being
          indicated as 'asymmetric(1)' or 'symmetric(2)'.  If 'down(0)',
          the direct neighbor is also added to the
          nhdpNibLostNeighborSetTable."
   ::= { nhdpNotificationsStates 1 }

  nhdp2HopNbrState  OBJECT-TYPE
     SYNTAX      INTEGER {
                    down(0),
                    up(1),
                    notconsidered(2)
                 }
     MAX-ACCESS  read-only
     STATUS      current
     DESCRIPTION
        "NHDP 2-hop neighbor states.  In NHDP, it is not necessary
         to remove Protocol Tuples from Protocol Sets at the
         exact time indicated, only to behave as if the Protocol
         Tuples were removed at that time.  This case is indicated
         here as 'down(0)'; otherwise, it is either 'up(1)', if
         N2_lost for the 2-Hop Tuple is equal to false, or
         'notconsidered(2)' otherwise."
     ::= { nhdpNotificationsStates 2 }

--
-- nhdpConformance information
--

nhdpCompliances       OBJECT IDENTIFIER ::= { nhdpConformance 1 }
nhdpMIBGroups         OBJECT IDENTIFIER ::= { nhdpConformance 2 }








   -- Compliance Statements
   nhdpBasicCompliance  MODULE-COMPLIANCE
      STATUS      current
      DESCRIPTION
         "The basic implementation requirements for
          managed network entities that implement
          NHDP."
      MODULE -- this module
      MANDATORY-GROUPS { nhdpConfigurationGroup }
   ::= { nhdpCompliances 1 }

   nhdpFullCompliance2  MODULE-COMPLIANCE
      STATUS      current
      DESCRIPTION
         "The full implementation requirements for
          managed network entities that implement
          NHDP."
      MODULE -- this module
      MANDATORY-GROUPS { nhdpConfigurationGroup,
                         nhdpStateGroup2,
                         nhdpNotificationObjectGroup,
                         nhdpNotificationGroup,
                         nhdpPerformanceGroup
      }
   ::= { nhdpCompliances 3 }


--
-- Units of Conformance
--

   nhdpConfigurationGroup  OBJECT-GROUP
      OBJECTS {
         nhdpIfName,
         nhdpIfStatus,
         nhdpHelloInterval,
         nhdpHelloMinInterval,
         nhdpRefreshInterval,
         nhdpLHoldTime,
         nhdpHHoldTime,
         nhdpHystAcceptQuality,
         nhdpHystRejectQuality,
         nhdpInitialQuality,
         nhdpInitialPending,
         nhdpHpMaxJitter,
         nhdpHtMaxJitter,
         nhdpNHoldTime,
         nhdpIHoldTime,





         nhdpIfRowStatus,
         nhdpLibLocalIfSetIfIndex,
         nhdpLibLocalIfSetIpAddrType,
         nhdpLibLocalIfSetIpAddr,
         nhdpLibLocalIfSetIpAddrPrefixLen,
         nhdpLibLocalIfSetRowStatus,
         nhdpLibRemovedIfAddrSetIpAddrType,
         nhdpLibRemovedIfAddrSetIpAddr,
         nhdpLibRemovedIfAddrSetIpAddrPrefixLen,
         nhdpLibRemovedIfAddrSetIfIndex,
         nhdpLibRemovedIfAddrSetIRTime
      }
      STATUS      current
      DESCRIPTION
         "Set of NHDP configuration objects implemented
          in this module."
   ::= { nhdpMIBGroups 2 }

   nhdpPerformanceGroup  OBJECT-GROUP
      OBJECTS {
         nhdpIfHelloMessageXmits,
         nhdpIfHelloMessageRecvd,
         nhdpIfHelloMessageXmitAccumulatedSize,
         nhdpIfHelloMessageRecvdAccumulatedSize,
         nhdpIfHelloMessageTriggeredXmits,
         nhdpIfHelloMessagePeriodicXmits,
         nhdpIfHelloMessageXmitAccumulatedSymmetricNeighborCount,
         nhdpIfHelloMessageXmitAccumulatedHeardNeighborCount,
         nhdpIfHelloMessageXmitAccumulatedLostNeighborCount,
         nhdpIfPerfCounterDiscontinuityTime,
         nhdpDiscIfRecvdPackets,
         nhdpDiscIfExpectedPackets,
         nhdpNibNeighborSetChanges,
         nhdpDiscNeighborNibNeighborSetChanges,
         nhdpDiscNeighborNibNeighborSetUpTime,
         nhdpDiscNeighborNibNeighborSetReachableLinkChanges,
         nhdpIib2HopSetPerfChanges,
         nhdpIib2HopSetPerfUpTime
      }
      STATUS      current
      DESCRIPTION
         "Set of NHDP performance objects implemented
          in this module."
   ::= { nhdpMIBGroups 4 }









   nhdpNotificationObjectGroup  OBJECT-GROUP
      OBJECTS {
         nhdpNbrStateChangeThreshold,
         nhdpNbrStateChangeWindow,
         nhdp2HopNbrStateChangeThreshold,
         nhdp2HopNbrStateChangeWindow,
         nhdpNbrState,
         nhdp2HopNbrState
      }
      STATUS      current
      DESCRIPTION
         "Set of NHDP notification objects implemented
          in this module."
   ::= { nhdpMIBGroups 5 }

   nhdpNotificationGroup  NOTIFICATION-GROUP
      NOTIFICATIONS {
         nhdpNbrStateChange,
         nhdp2HopNbrStateChange,
         nhdpIfStateChange
      }
      STATUS      current
      DESCRIPTION
         "Set of NHDP notifications implemented
          in this module."
   ::= { nhdpMIBGroups 6 }

   nhdpStateGroup2  OBJECT-GROUP
      OBJECTS {
         nhdpUpTime,
         nhdpIfStateUpTime,
         nhdpDiscRouterIndex,
         nhdpDiscIfIndex,
         nhdpDiscIfSetIpAddrType,
         nhdpDiscIfSetIpAddr,
         nhdpDiscIfSetIpAddrPrefixLen,
         nhdpIibLinkSetLHeardTime,
         nhdpIibLinkSetLSymTime,
         nhdpIibLinkSetLPending,
         nhdpIibLinkSetLLost,
         nhdpIibLinkSetLTime,
         nhdpIib2HopSetIpAddrPrefixLen,
         nhdpIib2HopSet1HopIfIndex,
         nhdpIib2HopSetN2Time,
         nhdpIib2HopSetN2Lost,
         nhdpNibNeighborSetNSymmetric,
         nhdpNibLostNeighborSetNLTime
      }





      STATUS      current
      DESCRIPTION
         "Set of NHDP state objects implemented
          in this module."
   ::= { nhdpMIBGroups 7 }


--
-- Deprecated compliance statements and groups
--

   nhdpFullCompliance  MODULE-COMPLIANCE
      STATUS      deprecated
      DESCRIPTION
         "The full implementation requirements for
          managed network entities that implement
          NHDP.

          For version-independence, this compliance statement
          is deprecated in favor of nhdpFullCompliance2."
      MODULE -- this module
      MANDATORY-GROUPS { nhdpConfigurationGroup,
                         nhdpStateGroup,
                         nhdpNotificationObjectGroup,
                         nhdpNotificationGroup,
                         nhdpPerformanceGroup
      }
   ::= { nhdpCompliances 2 }

   nhdpStateGroup  OBJECT-GROUP
      OBJECTS {
         nhdpUpTime,
         nhdpIfStateUpTime,
         nhdpDiscRouterIndex,
         nhdpDiscIfIndex,
         nhdpDiscIfSetIpAddrType,
         nhdpDiscIfSetIpAddr,
         nhdpDiscIfSetIpAddrPrefixLen,
         nhdpIibLinkSetLHeardTime,
         nhdpIibLinkSetLSymTime,
         nhdpIibLinkSetLPending,
         nhdpIibLinkSetLLost,
         nhdpIibLinkSetLTime,
         nhdpIib2HopSetIpAddrPrefixLen,
         nhdpIib2HopSet1HopIfIndex,
         nhdpIib2HopSetN2Time,
         nhdpNibNeighborSetNSymmetric,
         nhdpNibLostNeighborSetNLTime





      }
      STATUS      deprecated
      DESCRIPTION
         "Set of NHDP state objects implemented
          in this module.

          For version-independence, this compliance statement
          is deprecated in favor of nhdpStateGroup2."
   ::= { nhdpMIBGroups 3 }


END


