IGMP-STD-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, mib-2, Counter32, Gauge32,
    Unsigned32, IpAddress, TimeTicks FROM SNMPv2-SMI
    RowStatus, TruthValue            FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF
    InterfaceIndexOrZero,
    InterfaceIndex                   FROM IF-MIB;

igmpStdMIB MODULE-IDENTITY
    LAST-UPDATED "200009280000Z" -- September 28, 2000
    ORGANIZATION "IETF IDMR Working Group."
    CONTACT-INFO
            " Dave Thaler
              Microsoft Corporation
              One Microsoft Way
              Redmond, WA  98052-6399
              US

              Phone: +1 425 703 8835
              EMail: dthaler@microsoft.com"
    DESCRIPTION
            "The MIB module for IGMP Management."
    REVISION     "200009280000Z" -- September 28, 2000





    DESCRIPTION
            "Initial version, published as RFC 2933."
    ::= { mib-2 85 }


igmpMIBObjects     OBJECT IDENTIFIER ::= { igmpStdMIB 1 }

--
--  The IGMP Interface Table
--

igmpInterfaceTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF IgmpInterfaceEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The (conceptual) table listing the interfaces on which IGMP
            is enabled."
    ::= { igmpMIBObjects 1 }

igmpInterfaceEntry OBJECT-TYPE
    SYNTAX     IgmpInterfaceEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "An entry (conceptual row) representing an interface on
            which IGMP is enabled."
    INDEX      { igmpInterfaceIfIndex }
    ::= { igmpInterfaceTable 1 }

IgmpInterfaceEntry ::= SEQUENCE {
    igmpInterfaceIfIndex               InterfaceIndex,
    igmpInterfaceQueryInterval         Unsigned32,
    igmpInterfaceStatus                RowStatus,
    igmpInterfaceVersion               Unsigned32,
    igmpInterfaceQuerier               IpAddress,
    igmpInterfaceQueryMaxResponseTime  Unsigned32,
    igmpInterfaceQuerierUpTime         TimeTicks,
    igmpInterfaceQuerierExpiryTime     TimeTicks,
    igmpInterfaceVersion1QuerierTimer  TimeTicks,
    igmpInterfaceWrongVersionQueries   Counter32,
    igmpInterfaceJoins                 Counter32,
    igmpInterfaceProxyIfIndex          InterfaceIndexOrZero,
    igmpInterfaceGroups                Gauge32,
    igmpInterfaceRobustness            Unsigned32,
    igmpInterfaceLastMembQueryIntvl    Unsigned32
}






igmpInterfaceIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The ifIndex value of the interface for which IGMP is
            enabled."
    ::= { igmpInterfaceEntry 1 }

igmpInterfaceQueryInterval OBJECT-TYPE
    SYNTAX     Unsigned32
    UNITS      "seconds"
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The frequency at which IGMP Host-Query packets are
            transmitted on this interface."
    DEFVAL     { 125 }
    ::= { igmpInterfaceEntry 2 }

igmpInterfaceStatus OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The activation of a row enables IGMP on the interface.  The
            destruction of a row disables IGMP on the interface."
    ::= { igmpInterfaceEntry 3 }

igmpInterfaceVersion OBJECT-TYPE
    SYNTAX     Unsigned32
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The version of IGMP which is running on this interface.
            This object can be used to configure a router capable of
            running either value.  For IGMP to function correctly, all
            routers on a LAN must be configured to run the same version
            of IGMP on that LAN."
    DEFVAL     { 2 }
    ::= { igmpInterfaceEntry 4 }

igmpInterfaceQuerier OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The address of the IGMP Querier on the IP subnet to which





            this interface is attached."
    ::= { igmpInterfaceEntry 5 }

igmpInterfaceQueryMaxResponseTime OBJECT-TYPE
    SYNTAX     Unsigned32 (0..255)
    UNITS      "tenths of seconds"
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The maximum query response time advertised in IGMPv2
            queries on this interface."
    DEFVAL     { 100 }
    ::= { igmpInterfaceEntry 6 }

igmpInterfaceQuerierUpTime OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The time since igmpInterfaceQuerier was last changed."
    ::= { igmpInterfaceEntry 7 }

igmpInterfaceQuerierExpiryTime OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The amount of time remaining before the Other Querier
            Present Timer expires.  If the local system is the querier,
            the value of this object is zero."
    ::= { igmpInterfaceEntry 8 }

igmpInterfaceVersion1QuerierTimer OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The time remaining until the host assumes that there are no
            IGMPv1 routers present on the interface.  While this is non-
            zero, the host will reply to all queries with version 1
            membership reports."
    ::= { igmpInterfaceEntry 9 }

igmpInterfaceWrongVersionQueries OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION





            "The number of queries received whose IGMP version does not
            match igmpInterfaceVersion, over the lifetime of the row
            entry.  IGMP requires that all routers on a LAN be
            configured to run the same version of IGMP.  Thus, if any
            queries are received with the wrong version, this indicates
            a configuration error."
    ::= { igmpInterfaceEntry 10 }

igmpInterfaceJoins OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of times a group membership has been added on
            this interface; that is, the number of times an entry for
            this interface has been added to the Cache Table.  This
            object gives an indication of the amount of IGMP activity
            over the lifetime of the row entry."
    ::= { igmpInterfaceEntry 11 }

igmpInterfaceProxyIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndexOrZero
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "Some devices implement a form of IGMP proxying whereby
            memberships learned on the interface represented by this
            row, cause IGMP Host Membership Reports to be sent on the
            interface whose ifIndex value is given by this object.  Such
            a device would implement the igmpV2RouterMIBGroup only on
            its router interfaces (those interfaces with non-zero
            igmpInterfaceProxyIfIndex).  Typically, the value of this
            object is 0, indicating that no proxying is being done."
    DEFVAL     { 0 }
    ::= { igmpInterfaceEntry 12 }

igmpInterfaceGroups OBJECT-TYPE
    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The current number of entries for this interface in the
            Cache Table."
    ::= { igmpInterfaceEntry 13 }

igmpInterfaceRobustness OBJECT-TYPE
    SYNTAX     Unsigned32 (1..255)
    MAX-ACCESS read-create





    STATUS     current
    DESCRIPTION
            "The Robustness Variable allows tuning for the expected
            packet loss on a subnet.  If a subnet is expected to be
            lossy, the Robustness Variable may be increased.  IGMP is
            robust to (Robustness Variable-1) packet losses."
    DEFVAL     { 2 }
    ::= { igmpInterfaceEntry 14 }

igmpInterfaceLastMembQueryIntvl OBJECT-TYPE
    SYNTAX     Unsigned32 (0..255)
    UNITS      "tenths of seconds"
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The Last Member Query Interval is the Max Response Time
            inserted into Group-Specific Queries sent in response to
            Leave Group messages, and is also the amount of time between
            Group-Specific Query messages.  This value may be tuned to
            modify the leave latency of the network.  A reduced value
            results in reduced time to detect the loss of the last
            member of a group.  The value of this object is irrelevant
            if igmpInterfaceVersion is 1."
    DEFVAL     { 10 }
    ::= { igmpInterfaceEntry 15 }

--
--  The IGMP Cache Table
--

igmpCacheTable OBJECT-TYPE
    SYNTAX     SEQUENCE OF IgmpCacheEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The (conceptual) table listing the IP multicast groups for
            which there are members on a particular interface."
    ::= { igmpMIBObjects 2 }

igmpCacheEntry OBJECT-TYPE
    SYNTAX     IgmpCacheEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "An entry (conceptual row) in the igmpCacheTable."
    INDEX      { igmpCacheAddress, igmpCacheIfIndex }
    ::= { igmpCacheTable 1 }






IgmpCacheEntry ::= SEQUENCE {
    igmpCacheAddress            IpAddress,
    igmpCacheIfIndex            InterfaceIndex,
    igmpCacheSelf               TruthValue,
    igmpCacheLastReporter       IpAddress,
    igmpCacheUpTime             TimeTicks,
    igmpCacheExpiryTime         TimeTicks,
    igmpCacheStatus             RowStatus,
    igmpCacheVersion1HostTimer  TimeTicks
}

igmpCacheAddress OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The IP multicast group address for which this entry
            contains information."
    ::= { igmpCacheEntry 1 }

igmpCacheIfIndex OBJECT-TYPE
    SYNTAX     InterfaceIndex
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "The interface for which this entry contains information for
            an IP multicast group address."
    ::= { igmpCacheEntry 2 }

igmpCacheSelf OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "An indication of whether the local system is a member of
            this group address on this interface."
    DEFVAL     { true }
    ::= { igmpCacheEntry 3 }

igmpCacheLastReporter OBJECT-TYPE
    SYNTAX     IpAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The IP address of the source of the last membership report
            received for this IP Multicast group address on this
            interface.  If no membership report has been received, this
            object has the value 0.0.0.0."





    ::= { igmpCacheEntry 4 }

igmpCacheUpTime OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The time elapsed since this entry was created."
    ::= { igmpCacheEntry 5 }

igmpCacheExpiryTime OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The minimum amount of time remaining before this entry will
            be aged out.  A value of 0 indicates that the entry is only
            present because igmpCacheSelf is true and that if the router
            left the group, this entry would be aged out immediately.
            Note that some implementations may process membership
            reports from the local system in the same way as reports
            from other hosts, so a value of 0 is not required."
    ::= { igmpCacheEntry 6 }

igmpCacheStatus OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The status of this entry."
    ::= { igmpCacheEntry 7 }

igmpCacheVersion1HostTimer OBJECT-TYPE
    SYNTAX     TimeTicks
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The time remaining until the local router will assume that
            there are no longer any IGMP version 1 members on the IP
            subnet attached to this interface.  Upon hearing any IGMPv1
            Membership Report, this value is reset to the group
            membership timer.  While this time remaining is non-zero,
            the local router ignores any IGMPv2 Leave messages for this
            group that it receives on this interface."
    ::= { igmpCacheEntry 8 }

-- conformance information






igmpMIBConformance
               OBJECT IDENTIFIER ::= { igmpStdMIB 2 }
igmpMIBCompliances
               OBJECT IDENTIFIER ::= { igmpMIBConformance 1 }
igmpMIBGroups  OBJECT IDENTIFIER ::= { igmpMIBConformance 2 }


-- compliance statements

igmpV1HostMIBCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for hosts running IGMPv1 and
            implementing the IGMP MIB."
    MODULE  -- this module
    MANDATORY-GROUPS { igmpBaseMIBGroup }

    OBJECT     igmpInterfaceStatus
    MIN-ACCESS read-only
    DESCRIPTION
             "Write access is not required."

    OBJECT     igmpCacheStatus
    MIN-ACCESS read-only
    DESCRIPTION
             "Write access is not required."

    ::= { igmpMIBCompliances 1 }

igmpV1RouterMIBCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for routers running IGMPv1 and
            implementing the IGMP MIB."
    MODULE  -- this module
      MANDATORY-GROUPS { igmpBaseMIBGroup,
                       igmpRouterMIBGroup
                     }

    OBJECT     igmpInterfaceStatus
    MIN-ACCESS read-only
    DESCRIPTION
             "Write access is not required."
    OBJECT     igmpCacheStatus
    MIN-ACCESS read-only
    DESCRIPTION
             "Write access is not required."






    ::= { igmpMIBCompliances 2 }

igmpV2HostMIBCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for hosts running IGMPv2 and
            implementing the IGMP MIB."
    MODULE  -- this module
    MANDATORY-GROUPS { igmpBaseMIBGroup,
                       igmpV2HostMIBGroup
                     }

    OBJECT     igmpInterfaceStatus
    MIN-ACCESS read-only
    DESCRIPTION
             "Write access is not required."

    OBJECT     igmpCacheStatus
    MIN-ACCESS read-only
    DESCRIPTION
             "Write access is not required."

    ::= { igmpMIBCompliances 3 }

igmpV2RouterMIBCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for routers running IGMPv2 and
            implementing the IGMP MIB."
    MODULE  -- this module
    MANDATORY-GROUPS { igmpBaseMIBGroup,
                       igmpRouterMIBGroup,
                       igmpV2RouterMIBGroup
                     }

    OBJECT     igmpInterfaceStatus
    MIN-ACCESS read-only
    DESCRIPTION
             "Write access is not required."
    OBJECT     igmpCacheStatus
    MIN-ACCESS read-only
    DESCRIPTION
             "Write access is not required."

    ::= { igmpMIBCompliances 4 }


-- units of conformance





igmpBaseMIBGroup OBJECT-GROUP
    OBJECTS { igmpCacheSelf,
              igmpCacheStatus, igmpInterfaceStatus
            }
    STATUS  current
    DESCRIPTION
            "The basic collection of objects providing management of
            IGMP version 1 or 2."
    ::= { igmpMIBGroups 1 }


igmpRouterMIBGroup OBJECT-GROUP
    OBJECTS { igmpCacheUpTime, igmpCacheExpiryTime,
              igmpInterfaceJoins, igmpInterfaceGroups,
              igmpCacheLastReporter, igmpInterfaceQuerierUpTime,
              igmpInterfaceQuerierExpiryTime,
              igmpInterfaceQueryInterval
            }
    STATUS  current
    DESCRIPTION
            "A collection of additional objects for management of IGMP
            version 1 or 2 in routers."
    ::= { igmpMIBGroups 2 }


igmpV2HostMIBGroup OBJECT-GROUP
    OBJECTS { igmpInterfaceVersion1QuerierTimer }
    STATUS  current
    DESCRIPTION
            "A collection of additional objects for management of IGMP
            version 2 in hosts."
    ::= { igmpMIBGroups 3 }

igmpHostOptMIBGroup OBJECT-GROUP
    OBJECTS { igmpCacheLastReporter, igmpInterfaceQuerier }
    STATUS  current
    DESCRIPTION
            "A collection of optional objects for IGMP hosts.
            Supporting this group can be especially useful in an
            environment with a router which does not support the IGMP
            MIB."
    ::= { igmpMIBGroups 4 }

igmpV2RouterMIBGroup OBJECT-GROUP
    OBJECTS { igmpInterfaceVersion, igmpInterfaceQuerier,
              igmpInterfaceQueryMaxResponseTime,
              igmpInterfaceRobustness,
              igmpInterfaceWrongVersionQueries,





              igmpInterfaceLastMembQueryIntvl,
              igmpCacheVersion1HostTimer
            }
    STATUS  current
    DESCRIPTION
            "A collection of additional objects for management of IGMP
            version 2 in routers."
    ::= { igmpMIBGroups 5 }

igmpV2ProxyMIBGroup OBJECT-GROUP
    OBJECTS { igmpInterfaceProxyIfIndex }
    STATUS  current
    DESCRIPTION
            "A collection of additional objects for management of IGMP
            proxy devices."
    ::= { igmpMIBGroups 6 }

END


