SNMP-FRAMEWORK-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE,
       OBJECT-IDENTITY,
       snmpModules                           FROM SNMPv2-SMI
       TEXTUAL-CONVENTION                    FROM SNMPv2-TC
       MODULE-COMPLIANCE, OBJECT-GROUP       FROM SNMPv2-CONF;

   snmpFrameworkMIB MODULE-IDENTITY
       LAST-UPDATED "9711200000Z"            -- 20 November 1997
       ORGANIZATION "SNMPv3 Working Group"
       CONTACT-INFO "WG-email:   snmpv3@tis.com
                     Subscribe:  majordomo@tis.com
                                 In message body:  subscribe snmpv3

                     Chair:      Russ Mundy
                                 Trusted Information Systems
                     postal:     3060 Washington Rd
                                 Glenwood MD 21738
                                 USA
                     email:      mundy@tis.com
                     phone:      +1 301-854-6889

                     Co-editor   Dave Harrington
                                 Cabletron Systems, Inc.
                     postal:     Post Office Box 5005
                                 Mail Stop: Durham
                                 35 Industrial Way
                                 Rochester, NH 03867-5005
                                 USA
                     email:      dbh@ctron.com
                     phone:      +1 603-337-7357

                     Co-editor   Randy Presuhn
                                 BMC Software, Inc.
                     postal:     1190 Saratoga Avenue
                                 Suite 130
                                 San Jose, CA 95129
                                 USA
                     email:      rpresuhn@bmc.com
                     phone:      +1 408-556-0720

                     Co-editor:  Bert Wijnen
                                 IBM T.J. Watson Research
                     postal:     Schagen 33





                                 3461 GL Linschoten
                                 Netherlands
                     email:      wijnen@vnet.ibm.com
                     phone:      +31 348-432-794
                    "
       DESCRIPTION  "The SNMP Management Architecture MIB"
       ::= { snmpModules 2 }

   -- Textual Conventions used in the SNMP Management Architecture ***

   SnmpEngineID ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION "An SNMP engine's administratively-unique identifier.

                    The value for this object may not be all zeros or
                    all 'ff'H or the empty (zero length) string.

                    The initial value for this object may be configured
                    via an operator console entry or via an algorithmic
                    function.  In the latter case, the following
                    example algorithm is recommended.

                    In cases where there are multiple engines on the
                    same system, the use of this algorithm is NOT
                    appropriate, as it would result in all of those
                    engines ending up with the same ID value.

                    1) The very first bit is used to indicate how the
                       rest of the data is composed.

                       0 - as defined by enterprise using former methods
                           that existed before SNMPv3. See item 2 below.

                       1 - as defined by this architecture, see item 3
                           below.

                       Note that this allows existing uses of the
                       engineID (also known as AgentID [RFC1910]) to
                       co-exist with any new uses.

                    2) The snmpEngineID has a length of 12 octets.

                       The first four octets are set to the binary
                       equivalent of the agent's SNMP management
                       private enterprise number as assigned by the
                       Internet Assigned Numbers Authority (IANA).
                       For example, if Acme Networks has been assigned
                       { enterprises 696 }, the first four octets would





                       be assigned '000002b8'H.

                       The remaining eight octets are determined via
                       one or more enterprise-specific methods. Such
                       methods must be designed so as to maximize the
                       possibility that the value of this object will
                       be unique in the agent's administrative domain.
                       For example, it may be the IP address of the SNMP
                       entity, or the MAC address of one of the
                       interfaces, with each address suitably padded
                       with random octets.  If multiple methods are
                       defined, then it is recommended that the first
                       octet indicate the method being used and the
                       remaining octets be a function of the method.

                    3) The length of the octet strings varies.

                       The first four octets are set to the binary
                       equivalent of the agent's SNMP management
                       private enterprise number as assigned by the
                       Internet Assigned Numbers Authority (IANA).
                       For example, if Acme Networks has been assigned
                       { enterprises 696 }, the first four octets would
                       be assigned '000002b8'H.

                       The very first bit is set to 1. For example, the
                       above value for Acme Networks now changes to be
                       '800002b8'H.

                       The fifth octet indicates how the rest (6th and
                       following octets) are formatted. The values for
                       the fifth octet are:

                         0     - reserved, unused.

                         1     - IPv4 address (4 octets)
                                 lowest non-special IP address

                         2     - IPv6 address (16 octets)
                                 lowest non-special IP address

                         3     - MAC address (6 octets)
                                 lowest IEEE MAC address, canonical
                                 order

                         4     - Text, administratively assigned
                                 Maximum remaining length 27






                         5     - Octets, administratively assigned
                                 Maximum remaining length 27

                         6-127 - reserved, unused

                       127-255 - as defined by the enterprise
                                 Maximum remaining length 27
                   "
       SYNTAX       OCTET STRING (SIZE(1..32))

   SnmpSecurityModel ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION "An identifier that uniquely identifies a
                    securityModel of the Security Subsystem within the
                    SNMP Management Architecture.

                    The values for securityModel are allocated as
                    follows:

                    - The zero value is reserved.
                    - Values between 1 and 255, inclusive, are reserved
                      for standards-track Security Models and are
                      managed by the Internet Assigned Numbers Authority
                      (IANA).
                    - Values greater than 255 are allocated to
                      enterprise-specific Security Models.  An
                      enterprise-specific securityModel value is defined
                      to be:

                      enterpriseID * 256 + security model within
                      enterprise

                      For example, the fourth Security Model defined by
                      the enterprise whose enterpriseID is 1 would be
                      260.

                    This scheme for allocation of securityModel
                    values allows for a maximum of 255 standards-
                    based Security Models, and for a maximum of
                    255 Security Models per enterprise.

                    It is believed that the assignment of new
                    securityModel values will be rare in practice
                    because the larger the number of simultaneously
                    utilized Security Models, the larger the
                    chance that interoperability will suffer.
                    Consequently, it is believed that such a range
                    will be sufficient.  In the unlikely event that





                    the standards committee finds this number to be
                    insufficient over time, an enterprise number
                    can be allocated to obtain an additional 255
                    possible values.

                    Note that the most significant bit must be zero;
                    hence, there are 23 bits allocated for various
                    organizations to design and define non-standard
                    securityModels.  This limits the ability to
                    define new proprietary implementations of Security
                    Models to the first 8,388,608 enterprises.

                    It is worthwhile to note that, in its encoded
                    form, the securityModel value will normally
                    require only a single byte since, in practice,
                    the leftmost bits will be zero for most messages
                    and sign extension is suppressed by the encoding
                    rules.

                    As of this writing, there are several values
                    of securityModel defined for use with SNMP or
                    reserved for use with supporting MIB objects.
                    They are as follows:

                        0  reserved for 'any'
                        1  reserved for SNMPv1
                        2  reserved for SNMPv2c
                        3  User-Based Security Model (USM)
                   "
       SYNTAX       INTEGER(0..2147483647)

   SnmpMessageProcessingModel ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION "An identifier that uniquely identifies a Message
                    Processing Model of the Message Processing
                    Subsystem within a SNMP Management Architecture.

                    The values for messageProcessingModel are
                    allocated as follows:

                    - Values between 0 and 255, inclusive, are
                      reserved for standards-track Message Processing
                      Models and are managed by the Internet Assigned
                      Numbers Authority (IANA).
                    - Values greater than 255 are allocated to
                      enterprise-specific Message Processing Models.
                      An enterprise messageProcessingModel value is
                      defined to be:





                      enterpriseID * 256 +
                           messageProcessingModel within enterprise

                      For example, the fourth Message Processing Model
                      defined by the enterprise whose enterpriseID
                      is 1 would be 260.

                    This scheme for allocation of securityModel
                    values allows for a maximum of 255 standards-
                    based Message Processing Models, and for a
                    maximum of 255 Message Processing Models per
                    enterprise.

                    It is believed that the assignment of new
                    messageProcessingModel values will be rare
                    in practice because the larger the number of
                    simultaneously utilized Message Processing Models,
                    the larger the chance that interoperability
                    will suffer. It is believed that such a range
                    will be sufficient.  In the unlikely event that
                    the standards committee finds this number to be
                    insufficient over time, an enterprise number
                    can be allocated to obtain an additional 256
                    possible values.

                    Note that the most significant bit must be zero;
                    hence, there are 23 bits allocated for various
                    organizations to design and define non-standard
                    messageProcessingModels.  This limits the ability
                    to define new proprietary implementations of
                    Message Processing Models to the first 8,388,608
                    enterprises.

                    It is worthwhile to note that, in its encoded
                    form, the securityModel value will normally
                    require only a single byte since, in practice,
                    the leftmost bits will be zero for most messages
                    and sign extension is suppressed by the encoding
                    rules.

                    As of this writing, there are several values of
                    messageProcessingModel defined for use with SNMP.
                    They are as follows:

                        0  reserved for SNMPv1
                        1  reserved for SNMPv2c
                        2  reserved for SNMPv2u and SNMPv2*
                        3  reserved for SNMPv3





                   "
       SYNTAX       INTEGER(0..2147483647)

   SnmpSecurityLevel ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION "A Level of Security at which SNMP messages can be
                    sent or with which operations are being processed;
                    in particular, one of:

                      noAuthNoPriv - without authentication and
                                     without privacy,
                      authNoPriv   - with authentication but
                                     without privacy,
                      authPriv     - with authentication and
                                     with privacy.

                    These three values are ordered such that
                    noAuthNoPriv is less than authNoPriv and
                    authNoPriv is less than authPriv.
                   "
       SYNTAX       INTEGER { noAuthNoPriv(1),
                              authNoPriv(2),
                              authPriv(3)
                            }

   SnmpAdminString ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "255a"
       STATUS       current
       DESCRIPTION "An octet string containing administrative
                    information, preferably in human-readable form.

                    To facilitate internationalization, this
                    information is represented using the ISO/IEC
                    IS 10646-1 character set, encoded as an octet
                    string using the UTF-8 transformation format
                    described in [RFC2044].

                    Since additional code points are added by
                    amendments to the 10646 standard from time
                    to time, implementations must be prepared to
                    encounter any code point from 0x00000000 to
                    0x7fffffff.

                    The use of control codes should be avoided.

                    When it is necessary to represent a newline,
                    the control code sequence CR LF should be used.






                    The use of leading or trailing white space should
                    be avoided.

                    For code points not directly supported by user
                    interface hardware or software, an alternative
                    means of entry and display, such as hexadecimal,
                    may be provided.

                    For information encoded in 7-bit US-ASCII,
                    the UTF-8 encoding is identical to the
                    US-ASCII encoding.

                    Note that when this TC is used for an object that
                    is used or envisioned to be used as an index, then
                    a SIZE restriction must be specified so that the
                    number of sub-identifiers for any object instance
                    does not exceed the limit of 128, as defined by
                    [RFC1905].
                   "
       SYNTAX       OCTET STRING (SIZE (0..255))


   -- Administrative assignments ***************************************

   snmpFrameworkAdmin
       OBJECT IDENTIFIER ::= { snmpFrameworkMIB 1 }
   snmpFrameworkMIBObjects
       OBJECT IDENTIFIER ::= { snmpFrameworkMIB 2 }
   snmpFrameworkMIBConformance
       OBJECT IDENTIFIER ::= { snmpFrameworkMIB 3 }

   -- the snmpEngine Group ********************************************

   snmpEngine OBJECT IDENTIFIER ::= { snmpFrameworkMIBObjects 1 }

   snmpEngineID     OBJECT-TYPE
       SYNTAX       SnmpEngineID
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "An SNMP engine's administratively-unique identifier.
                   "
       ::= { snmpEngine 1 }

   snmpEngineBoots  OBJECT-TYPE
       SYNTAX       INTEGER (1..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of times that the SNMP engine has





                    (re-)initialized itself since its initial
                    configuration.
                   "
       ::= { snmpEngine 2 }

   snmpEngineTime   OBJECT-TYPE
       SYNTAX       INTEGER (0..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The number of seconds since the SNMP engine last
                    incremented the snmpEngineBoots object.
                   "
       ::= { snmpEngine 3 }

   snmpEngineMaxMessageSize OBJECT-TYPE
       SYNTAX       INTEGER (484..2147483647)
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION "The maximum length in octets of an SNMP message
                    which this SNMP engine can send or receive and
                    process, determined as the minimum of the maximum
                    message size values supported among all of the
                    transports available to and supported by the engine.
                   "
       ::= { snmpEngine 4 }


   -- Registration Points for Authentication and Privacy Protocols **

   snmpAuthProtocols OBJECT-IDENTITY
       STATUS        current
       DESCRIPTION  "Registration point for standards-track
                     authentication protocols used in SNMP Management
                     Frameworks.
                    "
       ::= { snmpFrameworkAdmin 1 }

   snmpPrivProtocols OBJECT-IDENTITY
       STATUS        current
       DESCRIPTION  "Registration point for standards-track privacy
                     protocols used in SNMP Management Frameworks.
                    "
       ::= { snmpFrameworkAdmin 2 }

   -- Conformance information ******************************************

   snmpFrameworkMIBCompliances
                  OBJECT IDENTIFIER ::= {snmpFrameworkMIBConformance 1}





   snmpFrameworkMIBGroups
                  OBJECT IDENTIFIER ::= {snmpFrameworkMIBConformance 2}

   -- compliance statements

   snmpFrameworkMIBCompliance MODULE-COMPLIANCE
       STATUS       current
       DESCRIPTION "The compliance statement for SNMP engines which
                    implement the SNMP Management Framework MIB.
                   "
       MODULE    -- this module
           MANDATORY-GROUPS { snmpEngineGroup }

       ::= { snmpFrameworkMIBCompliances 1 }

   -- units of conformance

   snmpEngineGroup OBJECT-GROUP
       OBJECTS {
                 snmpEngineID,
                 snmpEngineBoots,
                 snmpEngineTime,
                 snmpEngineMaxMessageSize
               }
       STATUS       current
       DESCRIPTION "A collection of objects for identifying and
                    determining the configuration and current timeliness
                    values of an SNMP engine.
                   "
       ::= { snmpFrameworkMIBGroups 1 }

   END


