RFC1243-MIB DEFINITIONS ::= BEGIN


          IMPORTS
                  Counter, IpAddress
                          FROM RFC1155-SMI
                  DisplayString, mib-2
                      FROM RFC1213-MIB
                  OBJECT-TYPE
                          FROM RFC-1212;

          --  This MIB module uses the extended OBJECT-TYPE macro as
          --  defined in [9]


          --  AppleTalk MIB





                  appletalk    OBJECT IDENTIFIER ::= { mib-2 13 }


                  DdpAddress ::=  -- 2 octets of net number
                                  -- 1 octet of node number
                          OCTET STRING (SIZE (3))
                  -- This data type is used for encoding a DDP protocol
                  -- address.  The format of this address is a serial
                  -- encoding of the two octets of network number in
                  -- network byte order, followed by the 1 octet node
                  -- number.

                  llap     OBJECT IDENTIFIER ::= { appletalk 1 }
                  aarp     OBJECT IDENTIFIER ::= { appletalk 2 }
                  atport   OBJECT IDENTIFIER ::= { appletalk 3 }
                  ddp      OBJECT IDENTIFIER ::= { appletalk 4 }
                  rtmp     OBJECT IDENTIFIER ::= { appletalk 5 }
                  kip      OBJECT IDENTIFIER ::= { appletalk 6 }
                  zip      OBJECT IDENTIFIER ::= { appletalk 7 }
                  nbp      OBJECT IDENTIFIER ::= { appletalk 8 }
                  atecho   OBJECT IDENTIFIER ::= { appletalk 9 }


          -- The LLAP Group

          llapTable OBJECT-TYPE
                  SYNTAX SEQUENCE OF LlapEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "The list of LLAP entries."
                  ::= { llap 1 }
          llapEntry OBJECT-TYPE
                  SYNTAX LlapEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "An LLAP entry containing objects for the
                      LocalTalk Link Access Protocol for a particular
                      LocalTalk interface."
                  INDEX { llapIfIndex }
                  ::= { llapTable 1 }

          LlapEntry ::= SEQUENCE {
                  llapIfIndex             INTEGER,
                  llapInPkts              Counter,
                  llapOutPkts             Counter,
                  llapInNoHandlers        Counter,





                  llapInLengthErrors      Counter,
                  llapInBads              Counter,
                  llapCollisions          Counter,
                  llapDefers              Counter,
                  llapNoDataErrors        Counter,
                  llapRandomCTSErrors     Counter,
                  llapFCSErrors           Counter
          }
          llapIfIndex OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The LLAP interface to which this entry pertains.
                      The interface identified by a particular value of
                      this index is the same interface as identified
                      by the same value of ifIndex."
                  ::= { llapEntry 1 }

          llapInPkts OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of good packets received on this
                      LocalTalk interface."
                  ::= { llapEntry 2 }

          llapOutPkts OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of packets transmitted on this
                      LocalTalk interface."
                  ::= { llapEntry 3 }

          llapInNoHandlers OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of good packets received on this
                      LocalTalk interface for which there was no
                      protocol handler."
                  ::= { llapEntry 4 }







          llapInLengthErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of packets received on this
                      LocalTalk interface whose actual length did not
                      match the length in the header."
                  ::= { llapEntry 5 }

          llapInErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of packets containing errors
                      received on this LocalTalk interface."
                  ::= { llapEntry 6 }

          llapCollisions OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of collisions assumed on this
                      LocalTalk interface due to the lack of a lapCTS
                      reply."
                  ::= { llapEntry 7 }

          llapDefers OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of times this LocalTalk
                      interface deferred to other packets."
                  ::= { llapEntry 8 }

          llapNoDataErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of times this LocalTalk
                      interface received a lapRTS packet and expected
                      a data packet, but did not receive any data
                      packet."
                  ::= { llapEntry 9 }





          llapRandomCTSErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of times this LocalTalk
                      interface received a lapCTS packet that was
                      not solicited by a lapRTS packet."
                  ::= { llapEntry 10 }

          llapFCSErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of times this LocalTalk
                      interface received a packet with an FCS
                      (Frame Check Sequence) error."
                  ::= { llapEntry 11 }


          -- The AARP Group
          aarpTable OBJECT-TYPE
                  SYNTAX SEQUENCE OF AarpEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "The AppleTalk Address Translation Table
                      contains an equivalence of AppleTalk Network
                      Addresses to the link layer physical address."
                  ::= { aarp 1 }

          aarpEntry OBJECT-TYPE
                  SYNTAX AarpEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "Each entry contains one AppleTalk Network
                      Address to physical address equivalence."
                  INDEX { aarpIfIndex, aarpNetAddress }
                  ::= { aarpTable 1 }

          AarpEntry ::= SEQUENCE {
                  aarpIfIndex     INTEGER,
                  aarpPhysAddress OCTET STRING,
                  aarpNetAddress  DdpAddress
          }






          aarpIfIndex OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The interface on which this entry's equivalence
                      is effective.  The interface identified by a
                      particular value of this index is the same
                      interface as identified by the same value of
                      ifIndex."
                  ::= { aarpEntry 1 }

          aarpPhysAddress OBJECT-TYPE
                  SYNTAX OCTET STRING
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The media-dependent physical address"
                  ::= { aarpEntry 2 }

          aarpNetAddress OBJECT-TYPE
                  SYNTAX DdpAddress
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The AppleTalk Network Address corresponding to
                      the media-dependent physical address."
                  ::= { aarpEntry 3 }


          -- The ATPort Group

          atportTable OBJECT-TYPE
                  SYNTAX SEQUENCE OF AtportEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "A list of AppleTalk ports for this entity."
                  ::= { atport 1 }

          atportEntry OBJECT-TYPE
                  SYNTAX AtportEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "The description of one of the AppleTalk
                      ports on this entity."
                  INDEX { atportIndex }





                  ::= { atportTable 1 }

          AtportEntry ::= SEQUENCE {
                  atportIndex               INTEGER,
                  atportDescr               DisplayString,
                  atportType                INTEGER,
                  atportNetStart            OCTET STRING (SIZE(2)),
                  atportNetEnd              OCTET STRING (SIZE(2)),
                  atportNetAddress          DdpAddress,
                  atportStatus              INTEGER,
                  atportNetConfig           INTEGER,
                  atportZoneConfig          INTEGER,
                  atportZone                OCTET STRING,
                  atportIfIndex             INTEGER
          }

          atportIndex OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "A unique value for each AppleTalk port.
                      Its value is between 1 and the total number of
                      AppleTalk ports.  The value for each port must
                      remain constant at least from the
                      re-initialization of the entity's network
                      management system to the next
                      re-initialization."
                  ::= { atportEntry 1 }

          atportDescr OBJECT-TYPE
                  SYNTAX DisplayString
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "A text string containing information about the
                      port.  This string is intended for presentation
                      to a human; it must not contain anything but
                      printable ASCII characters."
                  ::= { atportEntry 2 }

          atportType OBJECT-TYPE
                  SYNTAX INTEGER {
                       other(1),       -- none of the following
                       localtalk(2),
                       ethertalk1(3),
                       ethertalk2(4),
                       tokentalk(5),





                       iptalk(6),
                       serial-ppp(7),
                       serial-nonstandard(8),
                       virtual(9)
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The type of port, distinguished by the protocol
                      immediately below DDP in the protocol stack."
                  ::= { atportEntry 3 }

          atportNetStart OBJECT-TYPE
                  SYNTAX OCTET STRING (SIZE(2))
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The first AppleTalk network address in the range
                      configured for this port.  This is a two octet
                      DDP network address in network byte order."
                  ::= { atportEntry 4 }

          atportNetEnd OBJECT-TYPE
                  SYNTAX OCTET STRING (SIZE(2))
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The last AppleTalk network address in the range
                      configured for this port.  This is a two octet
                      DDP network address in network byte order.  If the
                      network to which this AppleTalk port is
                      connected is a Phase 1 network or a non-extended
                      network, the value for atportNetEnd shall be two
                      octets of zero."
                  ::= { atportEntry 5 }

          atportNetAddress OBJECT-TYPE
                  SYNTAX DdpAddress
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The AppleTalk network address configured for this
                      port."
                  ::= { atportEntry 6 }

          atportStatus OBJECT-TYPE
                  SYNTAX INTEGER {
                       operational(1),





                       unconfigured(2),
                       off(3),
                       invalid(4)
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The configuration status of this port.

                      Setting this object to the value invalid(4)
                      has the effect of invalidating the corresponding
                      entry in the atportTable.  That is, it
                      effectively disassociates the mapping identified
                      with said entry.  It is an
                      implementation-specific matter as to whether the
                      agent removes an invalidated entry from the table.
                      Accordingly, management stations must be
                      prepared to receive from agents tabular
                      information corresponding to entries not
                      currently in use.  Proper interpretation of such
                      entries requires examination of the relevant
                      atportStatus object."
                          ::= { atportEntry 7 }

          atportNetConfig OBJECT-TYPE
                  SYNTAX INTEGER {
                      configured(1),  -- explicit configuration.
                      garnered(2),    -- assumed from inspection of net.
                      guessed(3),     -- a "random" configuration.
                      unconfigured(4)
                  }
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The configuration status of this port."
                  ::= { atportEntry 8 }

          atportZoneConfig OBJECT-TYPE
                  SYNTAX INTEGER {
                      configured(1),  -- explicit configuration
                      garnered(2),    -- assumed from inspection of net.
                      guessed(3),     -- a "random" configuration.
                      unconfigured(4)
                  }
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The configuration status of the zone information





                      for this port."
                  ::= { atportEntry 9 }

          atportZone OBJECT-TYPE
                  SYNTAX OCTET STRING
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The zone name configured for this AppleTalk
                      port."
                  ::= { atportEntry 10 }

          atportIfIndex OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The physical interface associated with this
                      AppleTalk port.  The interface identified by a
                      particular value of this index is the same
                      interface as identified by the same value of
                      ifIndex."
                  ::= { atportEntry 11 }


          -- The DDP Group

          ddpOutRequests OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of DDP datagrams which were
                      supplied to DDP by local DDP clients in requests
                      for transmission.  Note that this counter does
                      not include any datagrams counted in
                      ddpForwRequests."
                  ::= { ddp 1 }

          ddpOutShorts OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of short DDP datagrams which
                      were transmitted from this entity."
                  ::= { ddp 2 }






          ddpOutLongs OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of long DDP datagrams which were
                      transmitted from this entity."
                  ::= { ddp 3 }

          ddpInReceives OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of input datagrams received by
                      DDP, including those received in error."
                  ::= { ddp 4 }

          ddpForwRequests OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The number of input datagrams for which this
                      entity was not their final DDP destination, as
                      a result of which an attempt was made to find a
                      route to forward them to that final destination."
                  ::= { ddp 5 }

          ddpInLocalDatagrams OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of input DDP datagrams for
                      which this entity was their final DDP
                      destination."
                  ::= { ddp 6 }

          ddpNoProtocolHandlers OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of DDP datagrams addressed to
                      this entity that were addressed to an upper
                      layer protocol for which no protocol handler
                      existed."





                  ::= { ddp 7 }

          ddpOutNoRoutes OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of DDP datagrams dropped
                      because a route could not be found to their
                      final destination."
                  ::= { ddp 8 }

          ddpTooShortErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of input DDP datagrams dropped
                      because the received data length was less than
                      the data length specified in the DDP header or
                      the received data length was less than the
                      length of the expected DDP header."
                  ::= { ddp 9 }

          ddpTooLongErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of input DDP datagrams dropped
                      because the received data length was greater
                      than the data length specified in the DDP header
                      or because they exceeded the maximum DDP
                      datagram size."
                  ::= { ddp 10 }

          ddpBroadcastErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of input DDP datagrams dropped
                      because this entity was not their final
                      destination and they were addressed to the link
                      level broadcast."
                  ::= { ddp 11 }







          ddpShortDDPErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of input DDP datagrams dropped
                      because this entity was not their final
                      destination and their type was short DDP."
                  ::= { ddp 12 }

          ddpHopCountErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of input DDP datagrams dropped
                      because this entity was not their final
                      destination and their hop count would exceed 15."
                  ::= { ddp 13 }

          ddpChecksumErrors OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The total number of input DDP datagrams dropped
                      because of a checksum error."
                  ::= { ddp 14 }


          -- The RTMP Group

          rtmpTable OBJECT-TYPE
                  SYNTAX SEQUENCE OF RtmpEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "A list of Routing Table Maintenance Protocol
                      entries for this entity."
                  ::= { rtmp 1 }

          rtmpEntry OBJECT-TYPE
                  SYNTAX RtmpEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "The route entry to a particular network range."
                  INDEX { rtmpRangeStart }





                  ::= { rtmpTable 1 }

          RtmpEntry ::= SEQUENCE {
                  rtmpRangeStart  OCTET STRING (SIZE(2)),
                  rtmpRangeEnd    OCTET STRING (SIZE(2)),
                  rtmpNextHop     OCTET STRING,
                  rtmpType        INTEGER,
                  rtmpPort        INTEGER,
                  rtmpHops        INTEGER,
                  rtmpState       INTEGER
          }

          rtmpRangeStart OBJECT-TYPE
                  SYNTAX OCTET STRING (SIZE(2))
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The first DDP network address in the network
                      range to which this routing entry pertains.
                      This is a two octet DDP network address in
                      network byte order."
                  ::= { rtmpEntry 1 }

          rtmpRangeEnd OBJECT-TYPE
                  SYNTAX OCTET STRING (SIZE(2))
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The last DDP network address in the network range
                      to which this routing entry pertains.  This is a
                      two octet DDP network address in network byte
                      order.  If the network to which this routing
                      entry pertains is a Phase 1 network or a
                      non-extended network, the value for rtmpRangeEnd
                      shall be two octets of zero."
                  ::= { rtmpEntry 2 }

          rtmpNextHop OBJECT-TYPE
                  SYNTAX OCTET STRING
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The next hop in the route to this entry's
                      destination network.  If the type of this route
                      is Appletalk, this address takes the same form
                      as DdpAddress."
                  ::= { rtmpEntry 3 }






          rtmpType OBJECT-TYPE
                  SYNTAX INTEGER {
                          other(1),
                          appletalk(2),
                          serial-ppp(3),
                          serial-nonstandard(4)
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The type of network over which this route
                      points."
                  ::= { rtmpEntry 4 }

          rtmpPort OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The index of the AppleTalk port over which
                      this route points."
                  ::= { rtmpEntry 5 }

          rtmpHops OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The number of hops required to reach the
                      destination network to which this routing
                      entry pertains."
                  ::= { rtmpEntry 6 }

          rtmpState OBJECT-TYPE
                  SYNTAX INTEGER {
                      good(1),
                      suspect(2),
                      goingBad(3),
                      bad(4) -- may be removed from table
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The status of the information contained in this
                      route entry.

                      Setting this object to the value bad(4) has the
                      effect of invalidating the corresponding entry





                      in the rtmpTable.  That is, it  effectively
                      disassociates the mapping identified with said
                      entry.  It is an implementation-specific matter
                      as to whether the agent removes an invalidated
                      entry from the table.  Accordingly, management
                      stations must be prepared to receive from agents
                      tabular information corresponding to entries not
                      currently in use.  Proper interpretation of such
                      entries requires examination of the relevant
                      rtmpState object."
                  ::= { rtmpEntry 7 }


          -- The KIP Group

          kipTable OBJECT-TYPE
                  SYNTAX SEQUENCE OF KipEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "The table of routing information for KIP
                      networks."
                  ::= { kip 1 }

          kipEntry OBJECT-TYPE
                  SYNTAX KipEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "An entry in the routing table for KIP networks."
                  INDEX { kipNetStart }
                  ::= { kipTable 1 }

          KipEntry ::= SEQUENCE {
                  kipNetStart     OCTET STRING (SIZE(2)),
                  kipNetEnd       OCTET STRING (SIZE(2)),
                  kipNextHop      IpAddress,
                  kipHopCount     INTEGER,
                  kipBCastAddr    IpAddress,
                  kipCore         INTEGER,
                  kipType         INTEGER,
                  kipState        INTEGER,
                  kipShare        INTEGER
          }

          kipNetStart OBJECT-TYPE
                  SYNTAX OCTET STRING (SIZE(2))
                  ACCESS read-write





                  STATUS mandatory
                  DESCRIPTION
                      "The first AppleTalk network address in the
                      range for this routing entry.  This address is a
                      two octet DDP network address in network byte
                      order."
                  ::= { kipEntry 1 }

          kipNetEnd OBJECT-TYPE
                  SYNTAX OCTET STRING (SIZE(2))
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The last AppleTalk network address in the range
                      for this routing entry.  This address is a two
                      octet DDP network address in network byte order.
                      If the network to which this AppleTalk port is
                      connected is a Phase 1 network or a non-extended
                      network, the value for kipNetEnd shall be two
                      octets of zero."
                  ::= { kipEntry 2 }

          kipNextHop OBJECT-TYPE
                  SYNTAX IpAddress
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The IP address of the next hop in the route to
                      this entry's destination network."
                  ::= { kipEntry 3 }

          kipHopCount OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The number of hops required to reach the
                      destination network to which this entry pertains."
                  ::= { kipEntry 4 }

          kipBCastAddr OBJECT-TYPE
                  SYNTAX IpAddress
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The form of the IP address used to broadcast on
                      this network."
                  ::= { kipEntry 5 }





          kipCore OBJECT-TYPE
                  SYNTAX INTEGER {
                       core(1),
                       notcore(2)
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The status of this network as a Kip Core
                      network."
                  ::= { kipEntry 6 }

          kipType OBJECT-TYPE
                  SYNTAX INTEGER {
                       kipRouter(1),
                       net(2),
                       host(3),
                       other(4)
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The type of the entity that this route points
                      to."
                  ::= { kipEntry 7 }

          kipState OBJECT-TYPE
                  SYNTAX INTEGER {
                       configured(1),
                       learned(2),
                       invalid(3)
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The state of this network entry.

                      Setting this object to the value invalid(3) has
                      the effect of invalidating the corresponding
                      entry in the kipTable.  That is, it effectively
                      disassociates the mapping identified with said
                      entry.  It is an implementation-specific matter
                      as to whether the agent removes an invalidated
                      entry from the table.
                      Accordingly, management stations must be
                      prepared to receive from agents tabular
                      information corresponding to entries not
                      currently in use.  Proper interpretation of such





                      entries requires examination of the relevant
                      kipState object."
                  ::= { kipEntry 8 }

          kipShare OBJECT-TYPE
                  SYNTAX INTEGER {
                       shared(1),
                       private(2)
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "If the information in this entry is propagated
                      to other routers as part of a routing protocol,
                      the value of this variable is equal to
                      shared(1).  Otherwise its value is private(2)."
                  ::= { kipEntry 9 }


          -- The ZIP Group

          zipTable OBJECT-TYPE
                  SYNTAX SEQUENCE OF ZipEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "The table of zone information for reachable
                      AppleTalk networks."
                  ::= { zip 1 }

          zipEntry OBJECT-TYPE
                  SYNTAX ZipEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "An entry of zone information for a particular
                      zone and network combination."
                  INDEX { zipZoneNetStart, zipZoneIndex }
                  ::= { zipTable 1 }

          ZipEntry ::= SEQUENCE {
                  zipZoneName     OCTET STRING,
                  zipZoneIndex    INTEGER,
                  zipZoneNetStart OCTET STRING (SIZE(2)),
                  zipZoneNetEnd   OCTET STRING (SIZE(2)),
                  zipZoneState    INTEGER
          }






          zipZoneName OBJECT-TYPE
                  SYNTAX OCTET STRING
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The ASCII zone name of this entry."
                  ::= { zipEntry 1 }

          zipZoneIndex OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "An integer that is unique to the zipZoneName
                      that is present in this entry.  For any given
                      zone name, every zipEntry that has an equal zone
                      name will have the same zipZoneIndex."
                  ::= { zipEntry 2 }

          zipZoneNetStart OBJECT-TYPE
                  SYNTAX OCTET STRING (SIZE(2))
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The network that starts the range for this
                      entry.  This address is a two octet DDP network
                      address in network byte order."
                  ::= { zipEntry 3 }

          zipZoneNetEnd OBJECT-TYPE
                  SYNTAX OCTET STRING (SIZE(2))
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The network that ends the range for this
                      entry.  This address is a two octet DDP network
                      address in network byte order.  If the network
                      to which this zip entry pertains is a Phase 1
                      network or a non-extended network, the value for
                      zipZoneNetEnd shall be two bytes of zero."
                  ::= { zipEntry 4 }

          zipZoneState OBJECT-TYPE
                  SYNTAX INTEGER {
                          valid(1),
                          invalid(2)
                  }
                  ACCESS read-write





                  STATUS mandatory
                  DESCRIPTION
                      "The state of this zip entry.

                      Setting this object to the value invalid(2) has
                      the effect of invalidating the corresponding
                      entry in the zipTable.  That is, it effectively
                      disassociates the mapping identified with said
                      entry.  It is an implementation-specific matter
                      as to whether the agent removes an invalidated
                      entry from the table.
                      Accordingly, management stations must be
                      prepared to receive from agents tabular
                      information corresponding to entries not
                      currently in use.  Proper interpretation of
                      such entries requires examination of the
                      relevant zipZoneState object."
                  ::= { zipEntry 5 }


          -- The NBP Group

          nbpTable OBJECT-TYPE
                  SYNTAX SEQUENCE OF NbpEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "The table of NBP services registered on this
                      entity."
                  ::= { nbp 1 }

          nbpEntry OBJECT-TYPE
                  SYNTAX NbpEntry
                  ACCESS not-accessible
                  STATUS mandatory
                  DESCRIPTION
                      "The description of an NBP service registered on
                      this entity."
                  INDEX { nbpIndex }
                  ::= { nbpTable  1 }

           NbpEntry ::= SEQUENCE {
                  nbpIndex        INTEGER,
                  nbpObject       OCTET STRING,
                  nbpType         OCTET STRING,
                  nbpZone         OCTET STRING,
                  nbpState        INTEGER
           }





          nbpIndex OBJECT-TYPE
                  SYNTAX INTEGER
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The index of this NBP entry.  This value ranges
                      from 1 to the number of NBP entries currently
                      registered on this entity."
                  ::= { nbpEntry 1 }

          nbpObject OBJECT-TYPE
                  SYNTAX OCTET STRING
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The name of the service described by this
                      entity."
                  ::= { nbpEntry 2 }

          nbpType OBJECT-TYPE
                  SYNTAX OCTET STRING
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The type of the service described by this
                      entity."
                  ::= { nbpEntry 3 }

          nbpZone OBJECT-TYPE
                  SYNTAX OCTET STRING
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The zone the service described by this entity is
                      registered in."
                  ::= { nbpEntry 4 }

          nbpState OBJECT-TYPE
                  SYNTAX INTEGER {
                          valid(1),
                          invalid(2)
                  }
                  ACCESS read-write
                  STATUS mandatory
                  DESCRIPTION
                      "The state of this NBP entry.

                      Setting this object to the value invalid(2) has





                      the effect of invalidating the corresponding
                      entry in the nbpTable.  That is, it effectively
                      disassociates the mapping identified with said
                      entry.  It is an implementation-specific matter
                      as to whether the agent removes an invalidated
                      entry from the table.
                      Accordingly, management stations must be
                      prepared to receive from agents tabular
                      information corresponding to entries not
                      currently in use.  Proper interpretation of
                      such entries requires examination of the
                      relevant nbpState object."
                  ::= { nbpEntry 5 }


          -- The ATEcho Group

          atechoRequests OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The number of AppleTalk echo requests received."
                  ::= { atecho 1 }

          atechoReplies OBJECT-TYPE
                  SYNTAX Counter
                  ACCESS read-only
                  STATUS mandatory
                  DESCRIPTION
                      "The number of AppleTalk echo replies sent."
                  ::= { atecho 2 }
          END


