PMIPV6-TC-MIB DEFINITIONS ::= BEGIN

       IMPORTS
         MODULE-IDENTITY, mib-2, Unsigned32
                    FROM SNMPv2-SMI                   -- [RFC2578]
         TEXTUAL-CONVENTION
                    FROM SNMPv2-TC;                   -- [RFC2579]

       pmip6TCMIB  MODULE-IDENTITY
          LAST-UPDATED "201205070000Z"     --  7th May, 2012
          ORGANIZATION "IETF NETLMM Working Group"
          CONTACT-INFO
          "                 Glenn Mansfield Keeni
                    Postal: Cyber Solutions, Inc.
                            6-6-3, Minami Yoshinari
                            Aoba-ku, Sendai, Japan 989-3204.
                       Tel: +81-22-303-4012
                       Fax: +81-22-303-4015
                     EMail: glenn@cysols.com

                            Sri Gundavelli
                    Postal: Cisco Systems
                            170 W.Tasman Drive,
                            San Jose, CA 95134
                            USA
                       Tel: +1-408-527-6109
                     EMail: sgundave@cisco.com









                            Kazuhide Koide
                    Postal: KDDI Corporation
                            GARDEN AIR TOWER 3-10-10, Iidabashi
                            Chiyoda-ku, Tokyo 102-8460, Japan.
                       Tel: +81-3-6678-3378
                     EMail: ka-koide@kddi.com

                            Ryuji Wakikawa
                    Postal: TOYOTA InfoTechnology Center, U.S.A., Inc.
                            465 Bernardo Avenue
                            Mountain View, CA
                            94043
                            USA
                     EMail: ryuji@us.toyota-itc.com
           Support Group EMail: netlmm@ietf.org
           "

        DESCRIPTION
            "This MIB module provides textual conventions for
             Proxy Mobile IPv6 Management information.

             Copyright (c) 2012 IETF Trust and the persons
             identified as authors of the code.  All rights
             reserved.

             Redistribution and use in source and binary forms,
             with or without modification, is permitted pursuant
             to, and subject to the license terms contained in,
             the Simplified BSD License set forth in Section 4.c
             of the IETF Trust's Legal Provisions Relating to IETF
             Documents (http://trustee.ietf.org/license-info).
            "

        REVISION "201205070000Z"     --  7th May, 2012
        DESCRIPTION
            "The initial version, published as RFC 6475."
        ::= { mib-2 205 }

    -- -------------------------------------------------------------
    -- Textual Conventions
    -- -------------------------------------------------------------
       Pmip6TimeStamp64  ::=  TEXTUAL-CONVENTION
           DISPLAY-HINT "6d:2d"
           STATUS  current
           DESCRIPTION
               "A 64-bit unsigned integer field containing a timestamp.
                The value indicates the elapsed time since January 1,
                1970, 00:00 UTC, by using a fixed-point format.  In this





                format, the integer number of seconds is contained in
                the first 48 bits of the field, and the remaining 16
                bits indicate the number of 1/65536 fractions of a
                second.
               "
           REFERENCE
               "RFC 5213: Section 8.8"
           SYNTAX  OCTET STRING (SIZE (8))

       Pmip6MnIdentifier  ::=  TEXTUAL-CONVENTION
           DISPLAY-HINT "255a"
           STATUS  current
           DESCRIPTION
               "The identity of a mobile node in the Proxy Mobile IPv6
                domain.  This is the stable identifier of a mobile node
                that the mobility entities in a Proxy Mobile IPv6 domain
                can always acquire and use for predictably identifying
                a mobile node.  Various forms of identifiers can be used
                to identify a mobile node (MN).  Two examples are a
                Network Access Identifier (NAI) and an opaque
                identifier applicable to a particular application.
               "
           REFERENCE
               "RFC 4283: Section 3"
           SYNTAX  OCTET STRING (SIZE (0..255))
       Pmip6MnLLIdentifier ::=  TEXTUAL-CONVENTION
           DISPLAY-HINT "255a"
           STATUS  current
           DESCRIPTION
               "An identifier that identifies the attached interface of
                a mobile node.
               "
           REFERENCE
               "RFC 5213: Section 8.6"
           SYNTAX  OCTET STRING (SIZE (0..255))

       Pmip6MnIndex ::= TEXTUAL-CONVENTION
           DISPLAY-HINT "d"
           STATUS       current
           DESCRIPTION
               "A unique integer value, greater than zero, assigned to
                each mobile node that is currently attached to the
                Proxy Mobile IPv6 domain by the management system.
                It is recommended that the values are assigned in a
                monotonically increasing order starting from 1.  It may
                wrap after reaching its maximum value.  The value for
                each mobile node must remain constant at least from one
                re-initialization of the entity's network management





                system to the next re-initialization.
               "
           SYNTAX       Unsigned32 (1..4294967295)
       Pmip6MnLLIndex ::= TEXTUAL-CONVENTION
           DISPLAY-HINT "d"
           STATUS       current
           DESCRIPTION
               "A unique integer value, greater than zero, assigned to
                each interface of a mobile node that is currently
                attached to the Proxy Mobile IPv6 domain by the
                management system.
                It is recommended that the values are assigned in a
                monotonically increasing order starting from 1.  It may
                wrap after reaching its maximum value.  The value for
                each interface of a mobile node must remain constant at
                least from one re-initialization of the entity's network
                management system to the next re-initialization.
               "
           SYNTAX       Unsigned32 (1..4294967295)
       Pmip6MnInterfaceATT ::=  TEXTUAL-CONVENTION
           STATUS  current
           DESCRIPTION
               "The object specifies the access technology that
                connects the mobile node to the access link on the
                mobile access gateway.
                The enumerated values and the corresponding access
                technology are as follows:
                 reserved                (0): Reserved (Not used)
                 logicalNetworkInterface (1): Logical network interface
                 pointToPointInterface   (2): Point-to-point interface
                 ethernet                (3): Ethernet interface
                 wirelessLan             (4): Wireless LAN interface
                 wimax                   (5): Wimax interface
                 threeGPPGERAN           (6): 3GPP GERAN
                 threeGPPUTRAN           (7): 3GPP UTRAN
                 threeGPPEUTRAN          (8): 3GPP E-UTRAN
                 threeGPP2eHRPD          (9): 3GPP2 eHRPD
                 threeGPP2HRPD          (10): 3GPP2 HRPD
                 threeGPP21xRTT         (11): 3GPP2 1xRTT
                 threeGPP2UMB           (12): 3GPP2 UMB
               "
           REFERENCE
               "RFC 5213: Section 8.5,
                Mobile IPv6 parameters registry on
                http://www.iana.org/mobility-parameters"

           SYNTAX INTEGER
           {





                reserved               (0),
                logicalNetworkInterface(1),
                pointToPointInterface  (2),
                ethernet               (3),
                wirelessLan            (4),
                wimax                  (5),
                threeGPPGERAN          (6),
                threeGPPUTRAN          (7),
                threeGPPEUTRAN         (8),
                threeGPP2eHRPD         (9),
                threeGPP2HRPD          (10),
                threeGPP21xRTT         (11),
                threeGPP2UMB           (12)
           }
    END


