T11-FC-SP-ZONING-MIB  DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    NOTIFICATION-TYPE, mib-2,
    Counter32
                        FROM SNMPv2-SMI                -- [RFC2578]
    TruthValue          FROM SNMPv2-TC                 -- [RFC2579]
    MODULE-COMPLIANCE, OBJECT-GROUP,
    NOTIFICATION-GROUP
                        FROM SNMPv2-CONF               -- [RFC2580]
    ifIndex             FROM IF-MIB                    -- [RFC2863]
    t11ZsServerEntry,
    t11ZsStatsEntry,
    t11ZsNotifyControlEntry,
    t11ZsFabricIndex    FROM T11-FC-ZONE-SERVER-MIB    -- [RFC4936]
    T11FcSpPolicyHashValue,
    T11FcSpPolicyHashFormat,
    T11FcSpHashCalculationStatus
                        FROM T11-FC-SP-TC-MIB;

t11FcSpZoningMIB  MODULE-IDENTITY
    LAST-UPDATED  "200808200000Z"





    ORGANIZATION  "This MIB module was developed through the
                  coordinated effort of two organizations:
                  T11 began the development and the IETF (in
                  the IMSS Working Group) finished it."
    CONTACT-INFO
            "     Claudio DeSanti
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA 95134 USA
                  EMail: cds@cisco.com

                  Keith McCloghrie
                  Cisco Systems, Inc.
                  170 West Tasman Drive
                  San Jose, CA 95134 USA
                  Email: kzm@cisco.com"
    DESCRIPTION
           "This MIB module specifies the extensions to the
           T11-FC-ZONE-SERVER-MIB module that are necessary for the
           management of Fibre Channel's FC-SP Zoning Servers, as
           defined in the FC-SP specification.

           The persistence of values written to these MIB objects is
           the same as the persistence of the objects they extend,
           i.e., it is given by the value of the relevant instance of
           t11ZsServerDatabaseStorageType (defined in the
           T11-FC-ZONE-SERVER-MIB module).

           Copyright (C) The IETF Trust (2008).  This version
           of this MIB module is part of RFC 5324;  see the RFC
           itself for full legal notices."
    REVISION  "200808200000Z"
    DESCRIPTION
           "Initial version of this MIB module, published as RFC 5324."
    ::= { mib-2 177 }

t11FcSpZsMIBNotifications  OBJECT IDENTIFIER ::= { t11FcSpZoningMIB 0 }
t11FcSpZsMIBObjects        OBJECT IDENTIFIER ::= { t11FcSpZoningMIB 1 }
t11FcSpZsMIBConformance    OBJECT IDENTIFIER ::= { t11FcSpZoningMIB 2 }
t11FcSpZsConfiguration  OBJECT IDENTIFIER ::= { t11FcSpZsMIBObjects 1 }
t11FcSpZsStatistics     OBJECT IDENTIFIER ::= { t11FcSpZsMIBObjects 2 }

--
-- Augmenting the table of Zone Servers
--

t11FcSpZsServerTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FcSpZsServerEntry





    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "A table which provides FC-SP-specific information about
           the Zone Servers on each Fabric in one or more Switches."
    ::= { t11FcSpZsConfiguration 1 }

t11FcSpZsServerEntry OBJECT-TYPE
    SYNTAX       T11FcSpZsServerEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "Each entry contains information relevant to FC-SP
           for a particular Zone Server for a particular Fabric
           on a particular Switch.  The Fabric and Switch are
           identified in the same manner as in t11ZsServerEntry."
    AUGMENTS   { t11ZsServerEntry }
    ::= { t11FcSpZsServerTable 1 }

T11FcSpZsServerEntry ::= SEQUENCE {
    t11FcSpZsServerCapabilityObject      BITS,
    t11FcSpZsServerEnabled               TruthValue,
    t11FcSpZoneSetHashStatus             T11FcSpHashCalculationStatus,
    t11FcSpActiveZoneSetHashType         T11FcSpPolicyHashFormat,
    t11FcSpActiveZoneSetHash             T11FcSpPolicyHashValue,
    t11FcSpZoneSetDatabaseHashType       T11FcSpPolicyHashFormat,
    t11FcSpZoneSetDatabaseHash           T11FcSpPolicyHashValue
}

t11FcSpZsServerCapabilityObject OBJECT-TYPE
    SYNTAX       BITS {
                     fcSpZoning(0)
                 }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "Capabilities of the Zone Server for the particular Fabric
           on the particular Switch, with respect to FC-SP Zoning:

               fcSpZoning -- set to 1 to indicate the Switch is
                             capable of supporting FC-SP Zoning.
           "
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, Table 184."
    ::= { t11FcSpZsServerEntry 1 }






t11FcSpZsServerEnabled OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "This object indicates whether the Zone Server for the
           particular Fabric on the particular Switch, is operating in
           FC-SP Zoning mode."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, Table 185."
    ::= { t11FcSpZsServerEntry 2 }

t11FcSpZoneSetHashStatus OBJECT-TYPE
    SYNTAX       T11FcSpHashCalculationStatus
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "When read, the value of this object is either:

             correct -- the corresponding instances of both
                        t11FcSpActiveZoneSetHash and
                        t11FcSpZoneSetDatabaseHash contain
                        the correct hash values; or
             stale   -- the corresponding instances of
                        t11FcSpActiveZoneSetHash and
                        t11FcSpZoneSetDatabaseHash contain
                        stale (possibly incorrect) values;

           Writing a value of 'calculate' is a request to re-calculate
           and update the values of the corresponding instances of both
           t11FcSpActiveZoneSetHash and t11FcSpZoneSetDatabaseHash.
           Writing a value of 'correct' or 'stale' to this object
           is an error (e.g., 'wrongValue').

           When the Active Zone Set and/or the Zone Set Database are
           updated, it is common that multiple changes need to be made
           at the same time.  In such circumstances, the use of this
           object allows the hash values to be updated only once after
           all changes, rather than repeatedly/after each individual
           change.

           If and when the corresponding instance of
           t11ZsServerDatabaseStorageType has the value 'permanent(4)',
           then if write access is supported to any instance of a
           read-write object in any row of any table governed by the
           'permanent' value of t11ZsServerDatabaseStorageType, then





           write access to the corresponding instance of this object
           must also be supported."
    REFERENCE
           "t11ZsServerDatabaseStorageType in
           'Fibre Channel Zone Server MIB', RFC 4936, August 2007."
    DEFVAL      { stale }
    ::= { t11FcSpZsServerEntry 3 }

t11FcSpActiveZoneSetHashType OBJECT-TYPE
    SYNTAX       T11FcSpPolicyHashFormat
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The format used for the hash value contained in the
           corresponding instance of t11FcSpActiveZoneSetHash."
    ::= { t11FcSpZsServerEntry 4 }

t11FcSpActiveZoneSetHash OBJECT-TYPE
    SYNTAX       T11FcSpPolicyHashValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The value of the hash for the current Active Zone Set.
            The format of this value is given by the corresponding
            instance of t11FcSpActiveZoneSetHashType."
    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, Table 187."
    ::= { t11FcSpZsServerEntry 5 }

t11FcSpZoneSetDatabaseHashType OBJECT-TYPE
    SYNTAX       T11FcSpPolicyHashFormat
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The format used for the hash value contained in the
           corresponding instance of t11FcSpZoneSetDatabaseHash."
    ::= { t11FcSpZsServerEntry 6 }

t11FcSpZoneSetDatabaseHash OBJECT-TYPE
    SYNTAX       T11FcSpPolicyHashValue
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The value of the hash for the current Zone Set Database.
            The format of this value is given by the corresponding
            instance of t11FcSpZoneSetDatabaseHashType."





    REFERENCE
           "- ANSI INCITS 426-2007, T11/Project 1570-D,
              Fibre Channel - Security Protocols (FC-SP),
              February 2007, Table 187."
    ::= { t11FcSpZsServerEntry 7 }

--
-- Additional Statistics for FC-SP Zoning
--

t11FcSpZsStatsTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FcSpZsStatsEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "A table of statistics specific to FC-SP that are
           maintained by Zone Servers."
    ::= { t11FcSpZsStatistics 1 }

t11FcSpZsStatsEntry OBJECT-TYPE
    SYNTAX       T11FcSpZsStatsEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "A set of statistics specific to FC-SP for a particular
           Zone Server for a particular Fabric on a particular Switch.
           The Fabric and Switch are identified in the same manner as
           in t11ZsStatsEntry."
    AUGMENTS   { t11ZsStatsEntry }
    ::= { t11FcSpZsStatsTable 1 }

T11FcSpZsStatsEntry ::= SEQUENCE {
    t11FcSpZsSPCMITrequestsSent       Counter32,
    t11FcSpZsSPCMITrequestsAccepted   Counter32,
    t11FcSpZsSPCMITrequestsRejected   Counter32,
    t11FcSpZsZcpRequestsSent          Counter32,
    t11FcSpZsZcpRequestsAccepted      Counter32,
    t11FcSpZsZcpRequestsRejected      Counter32,
    t11FcSpZsZirRequestsAccepted      Counter32,
    t11FcSpZsZirRequestsRejected      Counter32
}

t11FcSpZsSPCMITrequestsSent OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of SP Commit Zone Changes (SPCMIT) operation





           requests sent by the Zone Server.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    ::= { t11FcSpZsStatsEntry 1 }

t11FcSpZsSPCMITrequestsAccepted OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of SP Commit Zone Changes (SPCMIT) operation
           requests received and accepted by the Zone Server.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    ::= { t11FcSpZsStatsEntry 2 }

t11FcSpZsSPCMITrequestsRejected OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of SP Commit Zone Changes (SPCMIT) operation
           requests received but rejected by the Zone Server.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    ::= { t11FcSpZsStatsEntry 3 }

t11FcSpZsZcpRequestsSent OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of Zoning Check Protocol (ZCP) requests sent
           by the Zone Server.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    ::= { t11FcSpZsStatsEntry 4 }

t11FcSpZsZcpRequestsAccepted OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of Zoning Check Protocol (ZCP) requests received





           and accepted by the Zone Server.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    ::= { t11FcSpZsStatsEntry 5 }

t11FcSpZsZcpRequestsRejected OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of Zoning Check Protocol (ZCP) requests received
           but rejected by the Zone Server.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    ::= { t11FcSpZsStatsEntry 6 }

t11FcSpZsZirRequestsAccepted OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of Zoning Information Request (ZIR) requests
           received and accepted by the Zone Server.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    ::= { t11FcSpZsStatsEntry 7 }

t11FcSpZsZirRequestsRejected OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
           "The number of Zoning Information Request (ZIR) requests
           received but rejected by the Zone Server.

           This counter has no discontinuities other than those
           that all Counter32's have when sysUpTime=0."
    ::= { t11FcSpZsStatsEntry 8 }

--
--  Enable/Disable for Notifications
--

t11FcSpZsNotifyControlTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF T11FcSpZsNotifyControlEntry





    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "A table of control information for notifications
           generated due to Zone Server events related to
           FC-SP Zoning."
    ::= { t11FcSpZsConfiguration 2 }

t11FcSpZsNotifyControlEntry OBJECT-TYPE
    SYNTAX       T11FcSpZsNotifyControlEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
           "Each entry is an augmentation of the notification control
           information for a Zone Server for a particular Fabric on a
           particular Switch.  The Fabric and Switch are identified in
           the same manner as in t11ZsNotifyControlEntry."
    AUGMENTS   { t11ZsNotifyControlEntry }
    ::= { t11FcSpZsNotifyControlTable 1 }

T11FcSpZsNotifyControlEntry ::= SEQUENCE {
     t11FcSpZsNotifyJoinSuccessEnable    TruthValue,
     t11FcSpZsNotifyJoinFailureEnable    TruthValue
}

t11FcSpZsNotifyJoinSuccessEnable OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "This object specifies whether
           t11FcSpZsFabricJoinFailureNotify notifications should be
           generated by the Zone Server for this Fabric."
    ::= { t11FcSpZsNotifyControlEntry 1 }

t11FcSpZsNotifyJoinFailureEnable OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
           "This object specifies whether
           t11FcSpZsFabricJoinSuccessNotify notifications should be
           generated by the Zone Server for this Fabric."
    ::= { t11FcSpZsNotifyControlEntry 2 }

--
-- Notifications
--





t11FcSpZsFabricJoinSuccessNotify NOTIFICATION-TYPE
    OBJECTS      { ifIndex, t11ZsFabricIndex }
    STATUS       current
    DESCRIPTION
           "This notification indicates that a Switch that is part
           of one Fabric (indicated by the value of t11ZsFabricIndex)
           has successfully joined (on the interface indicated by the
           value of ifIndex) with a Switch that is part of another
           Fabric.

           If multiple Virtual Fabrics are configured on an interface,
           and all are successfully joined at the same time, and if
           the agent so chooses, then it can generate just one
           notification in which t11ZsFabricIndex has the value 4096."
    ::= { t11FcSpZsMIBNotifications 1 }

t11FcSpZsFabricJoinFailureNotify NOTIFICATION-TYPE
    OBJECTS      { ifIndex, t11ZsFabricIndex }
    STATUS       current
    DESCRIPTION
           "This notification indicates that an E_Port on the local
           Switch has entered the Isolated state because a join
           between two Fabrics failed.  The failure occurred on the
           local Fabric indicated by the value of t11ZsFabricIndex,
           on the interface indicated by the value of ifIndex.

           If multiple Virtual Fabrics are configured on an interface,
           and all have a failure to join at the same time, and if the
           agent so chooses, then it can generate just one notification
           in which t11ZsFabricIndex has the value 4096."
    ::= { t11FcSpZsMIBNotifications 2 }

--
-- Conformance
--

t11FcSpZsMIBCompliances
                    OBJECT IDENTIFIER ::= { t11FcSpZsMIBConformance 1 }
t11FcSpZsMIBGroups  OBJECT IDENTIFIER ::= { t11FcSpZsMIBConformance 2 }

t11FcSpZsMIBCompliance MODULE-COMPLIANCE
    STATUS       current
    DESCRIPTION
           "The compliance statement for entities that
           implement the extensions specified in FC-SP for
           Fibre Channel's Zone Server."

    MODULE  -- this module





        MANDATORY-GROUPS { t11FcSpZsObjectsGroup,
                           t11FcSpZsNotificationControlGroup,
                           t11FcSpZsNotificationGroup }

        GROUP        t11FcSpZsStatisticsGroup
        DESCRIPTION
            "These counters, containing Zone Server statistics,
            are mandatory only for those systems that count
            such events."

-- Write access is not required for any objects in this MIB module:

        OBJECT       t11FcSpZsServerEnabled
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       t11FcSpZoneSetHashStatus
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       t11FcSpZsNotifyJoinSuccessEnable
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       t11FcSpZsNotifyJoinFailureEnable
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

    ::= { t11FcSpZsMIBCompliances 1 }

-- Units of Conformance

t11FcSpZsObjectsGroup OBJECT-GROUP
    OBJECTS  { t11FcSpZsServerCapabilityObject,
               t11FcSpZsServerEnabled,
               t11FcSpZoneSetHashStatus,
               t11FcSpActiveZoneSetHashType,
               t11FcSpActiveZoneSetHash,
               t11FcSpZoneSetDatabaseHashType,
               t11FcSpZoneSetDatabaseHash
             }
    STATUS   current
    DESCRIPTION
           "A collection of objects for Zone configuration





           information of a Zone Server capable of
           operating in FC-SP Zoning mode."
    ::= { t11FcSpZsMIBGroups 1 }

t11FcSpZsNotificationControlGroup OBJECT-GROUP
    OBJECTS  { t11FcSpZsNotifyJoinSuccessEnable,
               t11FcSpZsNotifyJoinFailureEnable
             }
    STATUS   current
    DESCRIPTION
           "A collection of notification control objects for
           monitoring Zone Server failures specific to FC-SP."
    ::= { t11FcSpZsMIBGroups 2 }

t11FcSpZsStatisticsGroup OBJECT-GROUP
    OBJECTS  { t11FcSpZsSPCMITrequestsSent,
               t11FcSpZsSPCMITrequestsAccepted,
               t11FcSpZsSPCMITrequestsRejected,
               t11FcSpZsZcpRequestsSent,
               t11FcSpZsZcpRequestsAccepted,
               t11FcSpZsZcpRequestsRejected,
               t11FcSpZsZirRequestsAccepted,
               t11FcSpZsZirRequestsRejected
             }
    STATUS   current
    DESCRIPTION
           "A collection of objects for collecting Zone Server
            statistics which are specific to FC-SP."
    ::= { t11FcSpZsMIBGroups 3 }

t11FcSpZsNotificationGroup NOTIFICATION-GROUP
    NOTIFICATIONS { t11FcSpZsFabricJoinSuccessNotify,
                    t11FcSpZsFabricJoinFailureNotify
                  }
    STATUS        current
    DESCRIPTION
           "A collection of notification(s) for monitoring
           Zone Server events that are specific to FC-SP."
    ::= { t11FcSpZsMIBGroups 4 }

END











