ITU-ALARM-MIB DEFINITIONS ::= BEGIN


   IMPORTS
      MODULE-IDENTITY, OBJECT-TYPE,
      Gauge32, mib-2
          FROM SNMPv2-SMI                -- [RFC2578]
      AutonomousType, RowPointer
          FROM SNMPv2-TC                 -- [RFC2579]
      SnmpAdminString
          FROM SNMP-FRAMEWORK-MIB        -- [RFC3411]
      alarmListName, alarmModelIndex,
      alarmActiveDateAndTime, alarmActiveIndex
          FROM ALARM-MIB                 -- [RFC3877]
      ItuPerceivedSeverity,
      ItuTrendIndication
          FROM ITU-ALARM-TC-MIB          -- [RFC3877]
      IANAItuProbableCause,
      IANAItuEventType
          FROM IANA-ITU-ALARM-TC-MIB     -- [RFC3877]
      MODULE-COMPLIANCE, OBJECT-GROUP
          FROM SNMPv2-CONF               -- [RFC2580]
      ZeroBasedCounter32
          FROM RMON2-MIB;                -- [RFC2021]

     ituAlarmMIB MODULE-IDENTITY
         LAST-UPDATED "200409090000Z"  -- September 09, 2004
         ORGANIZATION "IETF Distributed Management Working Group"
         CONTACT-INFO
              "WG EMail: disman@ietf.org
              Subscribe: disman-request@ietf.org
              http://www.ietf.org/html.charters/disman-charter.html

              Chair:     Randy Presuhn
                         randy_presuhn@mindspring.com

              Editors:   Sharon Chisholm
                         Nortel Networks
                         PO Box 3511 Station C
                         Ottawa, Ont.  K1Y 4H7
                         Canada
                         schishol@nortelnetworks.com

                         Dan Romascanu
                         Avaya
                         Atidim Technology Park, Bldg. #3
                         Tel Aviv, 61131





                         Israel
                         Tel: +972-3-645-8414
                         Email: dromasca@avaya.com"
         DESCRIPTION
                 "The MIB module describes ITU Alarm information
                 as defined in ITU Recommendation M.3100 [M.3100],
                 X.733 [X.733] and X.736 [X.736].

                 Copyright (C) The Internet Society (2004).  The
                 initial version of this MIB module was published
                 in RFC 3877.  For full legal notices see the RFC
                 itself.  Supplementary information may be available on:
                 http://www.ietf.org/copyrights/ianamib.html"
         REVISION    "200409090000Z"  -- September 09, 2004
         DESCRIPTION
             "Initial version, published as RFC 3877."
         ::= { mib-2 121 }

   ituAlarmObjects OBJECT IDENTIFIER ::= { ituAlarmMIB 1 }

   ituAlarmModel OBJECT IDENTIFIER ::= { ituAlarmObjects 1 }

   ituAlarmActive  OBJECT IDENTIFIER ::= { ituAlarmObjects 2 }

   ituAlarmTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ItuAlarmEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "A table of ITU Alarm information for possible alarms
          on the system."
      ::= { ituAlarmModel 1 }

   ituAlarmEntry OBJECT-TYPE
      SYNTAX      ItuAlarmEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "Entries appear in this table whenever an entry is created
           in the alarmModelTable with a value of alarmModelState in
           the range from 1 to 6.  Entries disappear from this table
           whenever the corresponding entries are deleted from the
           alarmModelTable, including in cases where those entries
           have been deleted due to local system action.  The value of
           alarmModelSpecificPointer has no effect on the creation
           or deletion of entries in this table.  Values of
           alarmModelState map to values of ituAlarmPerceivedSeverity
           as follows:





             alarmModelState -> ituAlarmPerceivedSeverity
                    1        ->         clear (1)
                    2        ->         indeterminate (2)
                    3        ->         warning (6)
                    4        ->         minor (5)
                    5        ->         major (4)
                    6        ->         critical (3)

           All other values of alarmModelState MUST NOT appear
           in this table.

           This table MUST be persistent across system reboots."
      INDEX       { alarmListName, alarmModelIndex,
                   ituAlarmPerceivedSeverity }
      ::= { ituAlarmTable 1 }

   ItuAlarmEntry ::= SEQUENCE {
      ituAlarmPerceivedSeverity     ItuPerceivedSeverity,
      ituAlarmEventType             IANAItuEventType,
      ituAlarmProbableCause         IANAItuProbableCause,
      ituAlarmAdditionalText        SnmpAdminString,
      ituAlarmGenericModel          RowPointer }

   ituAlarmPerceivedSeverity OBJECT-TYPE
      SYNTAX  ItuPerceivedSeverity
      MAX-ACCESS   not-accessible
      STATUS       current
      DESCRIPTION
               "ITU perceived severity values."
       REFERENCE
           "ITU Recommendation M.3100, 'Generic Network Information
               Model', 1995
            ITU Recommendation X.733, 'Information Technology - Open
               Systems Interconnection - System Management: Alarm
               Reporting Function', 1992"
       ::= { ituAlarmEntry 1 }

   ituAlarmEventType OBJECT-TYPE
      SYNTAX       IANAItuEventType
      MAX-ACCESS   read-write
      STATUS       current
      DESCRIPTION
               "Represents the event type values for the alarms"
       REFERENCE
           "ITU Recommendation M.3100, 'Generic Network Information
               Model', 1995
            ITU Recommendation X.733, 'Information Technology - Open
               Systems Interconnection - System Management: Alarm





               Reporting Function', 1992
            ITU Recommendation X.736, 'Information Technology - Open
               Systems Interconnection - System Management: Security
               Alarm Reporting Function', 1992"
       ::= { ituAlarmEntry 2 }

   ituAlarmProbableCause OBJECT-TYPE
      SYNTAX      IANAItuProbableCause
      MAX-ACCESS  read-write
      STATUS       current
      DESCRIPTION
               "ITU probable cause values."
       REFERENCE
           "ITU Recommendation M.3100, 'Generic Network Information
               Model', 1995
            ITU Recommendation X.733, 'Information Technology - Open
               Systems Interconnection - System Management: Alarm
               Reporting Function', 1992
            ITU Recommendation X.736, 'Information Technology - Open
               Systems Interconnection - System Management: Security
               Alarm Reporting Function', 1992"
       ::= { ituAlarmEntry 3 }

   ituAlarmAdditionalText OBJECT-TYPE
      SYNTAX  SnmpAdminString
      MAX-ACCESS read-write
      STATUS     current
      DESCRIPTION
               "Represents the additional text field for the alarm."
       REFERENCE
           "ITU Recommendation M.3100, 'Generic Network Information
               Model', 1995
            ITU Recommendation X.733, 'Information Technology - Open
               Systems Interconnection - System Management: Alarm
               Reporting Function', 1992"
       ::= { ituAlarmEntry 4}

   ituAlarmGenericModel OBJECT-TYPE
      SYNTAX     RowPointer
      MAX-ACCESS read-write
      STATUS     current
      DESCRIPTION
      "This object points to the corresponding
       row in the alarmModelTable for this alarm severity.

       This corresponding entry to alarmModelTable could also
       be derived by performing the reverse of the mapping
       from alarmModelState to ituAlarmPerceivedSeverity defined





       in the description of ituAlarmEntry to determine the
       appropriate { alarmListName, alarmModelIndex, alarmModelState }
       for this { alarmListName, alarmModelIndex,
       ituAlarmPerceivedSeverity }."
      ::= { ituAlarmEntry 5 }

   -- ITU Active Alarm Table --

   ituAlarmActiveTable OBJECT-TYPE
      SYNTAX      SEQUENCE OF ItuAlarmActiveEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "A table of ITU information for active alarms entries."
      ::= { ituAlarmActive 1 }

   ituAlarmActiveEntry OBJECT-TYPE
      SYNTAX      ItuAlarmActiveEntry
      MAX-ACCESS  not-accessible
      STATUS      current
      DESCRIPTION
          "Entries appear in this table when alarms are active.  They
          are removed when the alarm is no longer occurring."
      INDEX       { alarmListName, alarmActiveDateAndTime,
                   alarmActiveIndex }
      ::= { ituAlarmActiveTable 1 }

   ItuAlarmActiveEntry ::= SEQUENCE {
       ituAlarmActiveTrendIndication       ItuTrendIndication,
       ituAlarmActiveDetector              AutonomousType,
       ituAlarmActiveServiceProvider       AutonomousType,
       ituAlarmActiveServiceUser           AutonomousType
       }

   ituAlarmActiveTrendIndication OBJECT-TYPE
      SYNTAX      ItuTrendIndication
      MAX-ACCESS  read-only
      STATUS       current
      DESCRIPTION
               "Represents the trend indication values for the alarms."
       REFERENCE
           "ITU Recommendation M.3100, 'Generic Network Information
               Model', 1995
            ITU Recommendation X.733, 'Information Technology - Open
               Systems Interconnection - System Management: Alarm
               Reporting Function', 1992"
       ::= { ituAlarmActiveEntry 1 }






   ituAlarmActiveDetector OBJECT-TYPE
      SYNTAX AutonomousType
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
         "Represents the SecurityAlarmDetector object."
       REFERENCE
           "ITU Recommendation X.736, 'Information Technology - Open
               Systems Interconnection - System Management: Security
               Alarm Reporting Function', 1992"
      ::= { ituAlarmActiveEntry 2 }

   ituAlarmActiveServiceProvider OBJECT-TYPE
      SYNTAX AutonomousType
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
         "Represents the ServiceProvider object."
       REFERENCE
           "ITU Recommendation X.736, 'Information Technology - Open
               Systems Interconnection - System Management: Security
               Alarm Reporting Function', 1992"
      ::= { ituAlarmActiveEntry 3 }

   ituAlarmActiveServiceUser OBJECT-TYPE
      SYNTAX AutonomousType
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
         "Represents the ServiceUser object."
       REFERENCE
           "ITU Recommendation X.736, 'Information Technology - Open
               Systems Interconnection - System Management: Security
               Alarm Reporting Function', 1992"
      ::= { ituAlarmActiveEntry 4 }

   -- Statistics and Counters

   ituAlarmActiveStatsTable  OBJECT-TYPE
         SYNTAX  SEQUENCE OF ItuAlarmActiveStatsEntry
         MAX-ACCESS  not-accessible
         STATUS  current
         DESCRIPTION
            "This table represents the ITU alarm statistics
            information."
     ::= { ituAlarmActive 2 }







   ituAlarmActiveStatsEntry OBJECT-TYPE
         SYNTAX  ItuAlarmActiveStatsEntry
         MAX-ACCESS  not-accessible
         STATUS  current
         DESCRIPTION
            "Statistics on the current active ITU alarms."
         INDEX   { alarmListName }

     ::= {  ituAlarmActiveStatsTable 1 }

   ItuAlarmActiveStatsEntry ::=
    SEQUENCE {
      ituAlarmActiveStatsIndeterminateCurrent Gauge32,
      ituAlarmActiveStatsCriticalCurrent      Gauge32,
      ituAlarmActiveStatsMajorCurrent         Gauge32,
      ituAlarmActiveStatsMinorCurrent         Gauge32,
      ituAlarmActiveStatsWarningCurrent       Gauge32,
      ituAlarmActiveStatsIndeterminates       ZeroBasedCounter32,
      ituAlarmActiveStatsCriticals            ZeroBasedCounter32,
      ituAlarmActiveStatsMajors               ZeroBasedCounter32,
      ituAlarmActiveStatsMinors               ZeroBasedCounter32,
      ituAlarmActiveStatsWarnings             ZeroBasedCounter32
    }

   ituAlarmActiveStatsIndeterminateCurrent OBJECT-TYPE
      SYNTAX      Gauge32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the current number of active alarms with a
           ituAlarmPerceivedSeverity of indeterminate."
      ::= { ituAlarmActiveStatsEntry 1 }

   ituAlarmActiveStatsCriticalCurrent OBJECT-TYPE
      SYNTAX      Gauge32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the current number of active alarms with a
           ituAlarmPerceivedSeverity of critical."
      ::= { ituAlarmActiveStatsEntry 2 }

   ituAlarmActiveStatsMajorCurrent OBJECT-TYPE
      SYNTAX      Gauge32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the current number of active alarms with a





           ituAlarmPerceivedSeverity of major."
      ::= { ituAlarmActiveStatsEntry 3 }

   ituAlarmActiveStatsMinorCurrent OBJECT-TYPE
      SYNTAX      Gauge32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the current number of active alarms with a
           ituAlarmPerceivedSeverity of minor."
      ::= { ituAlarmActiveStatsEntry 4 }

   ituAlarmActiveStatsWarningCurrent OBJECT-TYPE
      SYNTAX      Gauge32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the current number of active alarms with a
           ituAlarmPerceivedSeverity of warning."
      ::= { ituAlarmActiveStatsEntry 5 }

   ituAlarmActiveStatsIndeterminates OBJECT-TYPE
      SYNTAX      ZeroBasedCounter32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the total number of active alarms with a
           ituAlarmPerceivedSeverity of indeterminate since system
           restart."
      ::= { ituAlarmActiveStatsEntry 6 }

   ituAlarmActiveStatsCriticals OBJECT-TYPE
      SYNTAX      ZeroBasedCounter32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the total number of active alarms with a
           ituAlarmPerceivedSeverity of critical since system restart."
      ::= { ituAlarmActiveStatsEntry 7 }

   ituAlarmActiveStatsMajors OBJECT-TYPE
      SYNTAX      ZeroBasedCounter32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the total number of active alarms with a
           ituAlarmPerceivedSeverity of major since system restart."
      ::= { ituAlarmActiveStatsEntry 8 }





   ituAlarmActiveStatsMinors OBJECT-TYPE
      SYNTAX      ZeroBasedCounter32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the total number of active alarms with a
           ituAlarmPerceivedSeverity of minor since system restart."
      ::= { ituAlarmActiveStatsEntry 9 }

   ituAlarmActiveStatsWarnings OBJECT-TYPE
      SYNTAX      ZeroBasedCounter32
      MAX-ACCESS  read-only
      STATUS      current
      DESCRIPTION
          "A count of the total number of active alarms with a
           ituAlarmPerceivedSeverity of warning since system restart."
      ::= { ituAlarmActiveStatsEntry 10 }

   -- Conformance

   ituAlarmConformance OBJECT IDENTIFIER ::= { ituAlarmMIB 2 }
   ituAlarmCompliances  OBJECT IDENTIFIER ::= { ituAlarmConformance 1 }

   ituAlarmCompliance MODULE-COMPLIANCE
      STATUS  current
      DESCRIPTION
             "The compliance statement for systems supporting
             the ITU Alarm MIB."
      MODULE -- this module
          MANDATORY-GROUPS {
              ituAlarmGroup
              }
      GROUP       ituAlarmServiceUserGroup
          DESCRIPTION
              "This group is optional."
      GROUP       ituAlarmSecurityGroup
          DESCRIPTION
              "This group is optional."
      GROUP       ituAlarmStatisticsGroup
          DESCRIPTION
              "This group is optional."
     ::= { ituAlarmCompliances 1 }

   ituAlarmGroups OBJECT IDENTIFIER ::= { ituAlarmConformance 2 }

   ituAlarmGroup OBJECT-GROUP
    OBJECTS {
              ituAlarmEventType,





              ituAlarmProbableCause,
              ituAlarmGenericModel
            }
    STATUS   current
    DESCRIPTION
                  "ITU alarm details list group."
    ::= { ituAlarmGroups 1}

   ituAlarmServiceUserGroup OBJECT-GROUP
    OBJECTS {
              ituAlarmAdditionalText,
              ituAlarmActiveTrendIndication
            }
    STATUS current
    DESCRIPTION
            "The use of these parameters is a service-user option."
    ::= { ituAlarmGroups 2 }

   ituAlarmSecurityGroup OBJECT-GROUP
     OBJECTS {
             ituAlarmActiveDetector,
             ituAlarmActiveServiceProvider,
             ituAlarmActiveServiceUser
            }
     STATUS current
     DESCRIPTION
            "Security Alarm Reporting Function"
       REFERENCE
           "ITU Recommendation X.736, 'Information Technology - Open
               Systems Interconnection - System Management: Security
               Alarm Reporting Function', 1992"
     ::= { ituAlarmGroups 3 }

   ituAlarmStatisticsGroup OBJECT-GROUP
     OBJECTS {
            ituAlarmActiveStatsIndeterminateCurrent,
            ituAlarmActiveStatsCriticalCurrent,
            ituAlarmActiveStatsMajorCurrent,
            ituAlarmActiveStatsMinorCurrent,
            ituAlarmActiveStatsWarningCurrent,
            ituAlarmActiveStatsIndeterminates,
            ituAlarmActiveStatsCriticals,
            ituAlarmActiveStatsMajors,
            ituAlarmActiveStatsMinors,
            ituAlarmActiveStatsWarnings
             }
     STATUS current
     DESCRIPTION





       "ITU Active Alarm Statistics."
     ::= { ituAlarmGroups 4 }

   END


