NEMO-MIB DEFINITIONS ::= BEGIN

      IMPORTS
        MODULE-IDENTITY,  mib-2, Unsigned32, Counter32,
        Gauge32,
        OBJECT-TYPE, NOTIFICATION-TYPE
                   FROM SNMPv2-SMI
        TEXTUAL-CONVENTION,
        TruthValue, DateAndTime, TimeStamp
                   FROM SNMPv2-TC
        SnmpAdminString
                   FROM SNMP-FRAMEWORK-MIB
        MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
                   FROM SNMPv2-CONF
        InetAddressType, InetAddress, InetAddressPrefixLength
                   FROM INET-ADDRESS-MIB
        InterfaceIndex
                   FROM IF-MIB
        mip6BindingHomeAddressType, mip6BindingHomeAddress,
        mip6MnBLEntry, mip6BindingCacheEntry,
        mip6MnBLCOAType, mip6MnBLCOA
                   FROM MOBILEIPV6-MIB
        ;

     nemoMIB MODULE-IDENTITY
         LAST-UPDATED "200903100000Z"      -- 10 March 2009
         ORGANIZATION "IETF MEXT Working Group"






         CONTACT-INFO
            "           Sri Gundavelli
                Postal: Cisco
                        170 W.Tasman Drive,
                        San Jose, CA 95134
                        USA
                   Tel: +1-408-527-6109
                 Email: sgundave@cisco.com

                        Glenn Mansfield Keeni
                Postal: Cyber Solutions Inc.
                        6-6-3, Minami Yoshinari
                        Aoba-ku, Sendai, Japan 989-3204.
                   Tel: +81-22-303-4012
                   Fax: +81-22-303-4015
                E-mail: glenn@cysols.com

                        Kenichi Nagami
                Postal: INTEC NetCore Inc.
                        1-3-3, Shin-suna
                        Koto-ku, Tokyo, 135-0075
                        Japan
                   Tel: +81-3-5665-5069
                E-mail: nagami@inetcore.com

                        Kazuhide Koide
                Postal: KDDI CORPORATION
                        GARDEN AIR TOWER 3-10-10, Iidabashi
                        Chiyoda-ku, Tokyo, 102-8460 Japan
                   Tel: +81-3-6678-3378
                E-mail: ka-koide@kddi.com

            Support Group E-mail: mext@ietf.org
            "

            DESCRIPTION
             "Copyright (c) 2009 IETF Trust and the persons identified
              as authors of the code.  All rights reserved.

              Redistribution and use in source and binary forms, with
              or without modification, are permitted provided that the
              following conditions are met:

              - Redistributions of source code must retain the above
                copyright notice, this list of conditions and the
                following disclaimer.







              - Redistributions in binary form must reproduce the
                above copyright notice, this list of conditions and
                the following disclaimer in the documentation and/or
                other materials provided with the distribution.

              - Neither the name of Internet Society, IETF or IETF
                Trust, nor the names of specific contributors, may be
                used to endorse or promote products derived from this
                software without specific prior written permission.

             THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
             CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED
             WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
             WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A
             PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE
             COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT,
             INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
             CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
             PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
             DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
             CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
             CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE
             OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
             SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH
             DAMAGE.

             This version of this MIB module is part of RFC 5488;
             see the RFC itself for full legal notices."

             REVISION    "200903100000Z"      -- 10 March 2009
             DESCRIPTION "Initial version, published as RFC 5488."

                  ::= { mib-2  184 }

      -- The NEMO MIB has the following primary groups

      nemoNotifications        OBJECT IDENTIFIER ::= { nemoMIB 0 }
      nemoObjects              OBJECT IDENTIFIER ::= { nemoMIB 1 }
      nemoConformance          OBJECT IDENTIFIER ::= { nemoMIB 2 }
      nemoCore                 OBJECT IDENTIFIER ::= { nemoObjects 1 }
      nemoMr                   OBJECT IDENTIFIER ::= { nemoObjects 2 }
      nemoCn                   OBJECT IDENTIFIER ::= { nemoObjects 3 }
      nemoHa                   OBJECT IDENTIFIER ::= { nemoObjects 4 }

       -- The sub groups

      nemoSystem               OBJECT IDENTIFIER ::= { nemoCore 1 }
      nemoBindings             OBJECT IDENTIFIER ::= { nemoCore 2 }





      nemoConfiguration        OBJECT IDENTIFIER ::= { nemoCore 3 }
      nemoStats                OBJECT IDENTIFIER ::= { nemoCore 4 }

      nemoMrSystem             OBJECT IDENTIFIER ::= { nemoMr 1 }
      nemoMrConf               OBJECT IDENTIFIER ::= { nemoMr 2 }
      nemoMrRegistration       OBJECT IDENTIFIER ::= { nemoMr 3 }
      nemoMrGlobalStats        OBJECT IDENTIFIER ::= { nemoMr 4 }

      nemoHaAdvertisement      OBJECT IDENTIFIER ::= { nemoHa 1 }
      nemoHaStats              OBJECT IDENTIFIER ::= { nemoHa 2 }
      nemoHaRegistration       OBJECT IDENTIFIER ::= { nemoHa 3 }
      nemoHaGlobalStats        OBJECT IDENTIFIER ::= { nemoHaStats 1 }

      -- Textual Conventions
    NemoBURequestRejectionCode ::= TEXTUAL-CONVENTION
           STATUS        current
           DESCRIPTION
                   "The value of the status field in the Binding
                    Acknowledgment message when the Binding Update
                    was rejected for NEMO-specific reasons.
                   "
           REFERENCE
                   "RFC 3963: Section 4.2"
           SYNTAX  INTEGER {
                   mobileRouterOperationNotPermitted (140),
                   invalidPrefix                     (141),
                   notAuthorizedForPrefix            (142),
                   forwardingSetupFailed             (143)
                  }

      --
      --
      -- nemoSystem group
      --
      --

      nemoCapabilities OBJECT-TYPE
          SYNTAX      BITS {
                           mobileRouter       (0),
                           homeAgentSupport   (1)
                      }
          MAX-ACCESS  read-only
          STATUS      current










          DESCRIPTION
                  "This object indicates the NEMO functions that
                   are supported by this managed entity.  Multiple
                   NEMO functions may be supported by a single
                   entity.
                  "
          REFERENCE
                  "RFC 3963: Section 3"
          ::= { nemoSystem 1 }

      nemoStatus OBJECT-TYPE
          SYNTAX      INTEGER { enabled(1), disabled(2) }
          MAX-ACCESS  read-write
          STATUS      current
          DESCRIPTION
                  "This object indicates whether the NEMO
                   function is enabled for the managed entity.  If it
                   is enabled, the agent discovery and registration
                   functions will be operational.

                   Changing the status from enabled(1) to disabled(2)
                   will terminate the agent discovery and registration
                   functions.  On the other hand, changing the status
                   from disabled(2) to enabled(1) will start the agent
                   discovery and registration functions.

                   The value of this object MUST remain unchanged
                   across reboots of the managed entity.
                  "
          ::= { nemoSystem 2 }

     nemoCounterDiscontinuityTime OBJECT-TYPE
        SYNTAX      TimeStamp
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The value of sysUpTime on the most recent occasion at
                 which any one or more of this NEMO entity's counters,
                 viz., counters with OID prefix 'nemoMrConf',
                 'nemoMrRegnCounters', 'nemoMrGlobalStats', or
                 'nemoHaGlobalStats', suffered a discontinuity.  If
                 no such discontinuities have occurred since the last
                 re-initialization of the local management subsystem,
                 then this object will have a zero value.
                "
        ::= { nemoStats 1 }
     --
     --





     --   nemoConfiguration group
     --
     --

    nemoMrBLTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF NemoMrBLEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "This table corresponds to the Binding Update List
                 (BL) that includes NEMO-related information and that
                 is maintained by the mobile router.  The table
                 holds a row for every binding that the mobile
                 router has established or is trying to establish.
                 Entries from the table are deleted as the lifetime
                 of the binding expires.
                "
        REFERENCE
                "RFC 3775: Sections 4.5, 11.1
                 RFC 3963: Section 5.2"
        ::= { nemoMrRegistration 1 }

    nemoMrBLEntry  OBJECT-TYPE
        SYNTAX      NemoMrBLEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry pertaining to NEMO-related information
                 contained in a Binding Update sent by a NEMO-enabled
                 mobile router to its home agent.
                "
        AUGMENTS {mip6MnBLEntry}
    ::= { nemoMrBLTable 1 }

    NemoMrBLEntry ::= SEQUENCE {
        nemoMrBLMode     INTEGER,
        nemoMrBLMrFlag   TruthValue,
        nemoMrBLHomeAddressPrefixLength   InetAddressPrefixLength,
        nemoMrBLCareofAddressPrefixLength InetAddressPrefixLength,
        nemoMrBLActiveEgressIfIndex       InterfaceIndex,
        nemoMrBLEstablishedHomeTunnelIfIndex InterfaceIndex
        }
    nemoMrBLMode OBJECT-TYPE
        SYNTAX      INTEGER {
          implicitMode (1),
          explicitMode (2)
                    }
        MAX-ACCESS  read-only





        STATUS      current
        DESCRIPTION
                "implicitMode(1): the Mobile Network Prefix Option
                 is not included in the Binding Update by the mobile
                 router.

                 explicitMode(2): the mobile router included one or
                 more Mobile Network Prefix Options in the Binding
                 Update.
                "
        REFERENCE
                "RFC 3963: Section 5.2"
        ::= { nemoMrBLEntry 1 }

    nemoMrBLMrFlag OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "true(1): the mobile router sent the Binding Update
                 with Mobile Router Flag set.

                 false(2): the mobile router did not send the Binding
                 Update with Mobile Router Flag set.  This implies that
                 the mobile router is acting as a mobile node.
                "
        REFERENCE
                "RFC 3963: Sections 4.1, 5.1"
        ::= { nemoMrBLEntry 2 }

    nemoMrBLHomeAddressPrefixLength  OBJECT-TYPE
        SYNTAX      InetAddressPrefixLength
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The prefix length of the mobile router's home network.
                "
        REFERENCE
            "RFC 3963: Section 3"
        ::= { nemoMrBLEntry 3 }

    nemoMrBLCareofAddressPrefixLength  OBJECT-TYPE
        SYNTAX      InetAddressPrefixLength
        MAX-ACCESS  read-only
        STATUS      current








        DESCRIPTION
                "The prefix length of the care-of address of the
                 mobile router.
                "
        REFERENCE
            "RFC 3963: Section 3"
        ::= { nemoMrBLEntry 4 }

    nemoMrBLActiveEgressIfIndex OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The interface index of the currently active
                 egress interface.
                "
        REFERENCE
            "RFC 3963: Section 5.5"
        ::= { nemoMrBLEntry 5 }

    nemoMrBLEstablishedHomeTunnelIfIndex  OBJECT-TYPE
        SYNTAX      InterfaceIndex
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The interface index of the tunnel established
                 between the mobile router and the home agent
                 for NEMO traffic.
                "
        REFERENCE
            "RFC 3963: Section 5.5"
        ::= { nemoMrBLEntry 6 }

    -- Mobile Router Registration Group Counters

    nemoMrRegnCounters OBJECT IDENTIFIER ::= { nemoMrRegistration 2 }

    nemoMrMobilityMessagesSent OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of mobility messages, i.e., IPv6
                 datagrams with Mobility Header, sent by the mobile
                 node.  This will include Binding Updates sent by a
                 mobile router with the Mobile Router Flag set.







                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3775: Sections 4.2, 6.1
                 RFC 3963: Section 4.1"
        ::= {  nemoMrRegnCounters 1 }

    nemoMrMobilityMessagesRecd OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of mobility messages, i.e., IPv6
                 datagrams with Mobility Header, received by the
                 mobile node.  This will include Binding
                 Acknowledgements with Mobile Router Flag set that
                 are sent to a mobile router.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3775: Sections 4.2, 6.1
                 RFC 3963: Sections 4.1, 4.2"
        ::= {  nemoMrRegnCounters 2 }

    nemoMrPrefixRegMode OBJECT-TYPE
        SYNTAX INTEGER {
                  implicitMode       (1),
                  explicitMode       (2)
               }
        MAX-ACCESS  read-write
        STATUS      current
        DESCRIPTION
                "This object indicates the mode in which the mobile
                 network prefixes will be registered with the home
                 agent.

                 implicitMode(1): the Mobile Network Prefix Option will
                 not be included in the Binding Update by the mobile
                 router.







                 explicitMode(2): the mobile router will include one or
                 more Mobile Network Prefix Options in the Binding
                 Update.

                 The value of this object MUST remain unchanged
                 across reboots of the managed entity.
                "
        REFERENCE
                "RFC 3963: Section 5.2"

        ::= { nemoMrRegistration 3 }

    nemoHaMobileNetworkPrefixTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF NemoHaMobileNetworkPrefixEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "This table contains the mobile network prefixes
                 that the home agent maintains for the mobile router.
                 The mobile network prefixes in this table are
                 registered by Binding Updates or are manually
                 pre-configured.
                "
        REFERENCE
                "RFC 3963: Section 6.1.2"
        ::= { nemoHaRegistration 1 }

    nemoHaMobileNetworkPrefixEntry OBJECT-TYPE
        SYNTAX      NemoHaMobileNetworkPrefixEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry for a mobile network prefix.

                 The instances of the columnar objects in this entry
                 pertain to an interface for a particular value of
                 mip6BindingHomeAddressType, mip6BindingHomeAddress,
                 and nemoHaMobileNetworkPrefixSeqNo.

                 The nemoHaMobileNetworkPrefixSeqNo object is used to
                 distinguish between multiple instances of
                 the mobile network prefix in the same Binding Update
                 for the same set of mip6BindingHomeAddressType and
                 mip6BindingHomeAddress.

                 There is no upper-bound on the maximum number of
                 mobile network prefixes in a Binding Update but, for
                 practical purposes, the upper bound of the value





                 nemoHaMobileNetworkPrefixSeqNo is set to 1024.

                 Implementers need to be aware that if the total
                 number of octets in mip6BindingHomeAddress
                 exceeds 112, then OIDs of column
                 instances in this row will have more than 128
                 sub-identifiers and cannot be accessed using
                 SNMPv1, SNMPv2c, or SNMPv3.
                "
        INDEX  { mip6BindingHomeAddressType,
                 mip6BindingHomeAddress,
                 nemoHaMobileNetworkPrefixSeqNo
    }
    ::= { nemoHaMobileNetworkPrefixTable 1 }

    NemoHaMobileNetworkPrefixEntry ::= SEQUENCE {
        nemoHaMobileNetworkPrefixSeqNo       Unsigned32,
        nemoHaMobileNetworkPrefixType        InetAddressType,
        nemoHaMobileNetworkPrefix            InetAddress,
        nemoHaMobileNetworkPrefixLength      Unsigned32,
        nemoHaMobileNetworkPrefixSource      INTEGER
    }

    nemoHaMobileNetworkPrefixSeqNo OBJECT-TYPE
        SYNTAX      Unsigned32 (1..1024)
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "A Binding Update may have multiple mobile network
                 prefixes.

                 This object, along with mip6BindingHomeAddressType
                 and mip6BindingHomeAddress, uniquely identifies a
                 row containing a single mobile network prefix for
                 a mobile router in this table.
                "
        REFERENCE
                "RFC 3963: Sections 2, 6.1, 6.2"
        ::= { nemoHaMobileNetworkPrefixEntry 1 }

    nemoHaMobileNetworkPrefixType OBJECT-TYPE
        SYNTAX      InetAddressType
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The address type for the mobile network prefix
                 that follows.
                "





        ::= { nemoHaMobileNetworkPrefixEntry 2 }

    nemoHaMobileNetworkPrefix OBJECT-TYPE
        SYNTAX      InetAddress
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "A mobile network prefix related to the
                 corresponding Binding Update.

                 The type of the address represented by this object
                 is specified by the corresponding
                 nemoHaMobileNetworkPrefixType object.
                "
        REFERENCE
                "RFC 3963: Sections 2, 6.1, 6.2"
        ::= { nemoHaMobileNetworkPrefixEntry 3 }

    nemoHaMobileNetworkPrefixLength OBJECT-TYPE
        SYNTAX      Unsigned32 (0..128)
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The length of the prefix specified by the corresponding
                 nemoHaMobileNetworkPrefix object.
                "
        REFERENCE
                "RFC 3963: Sections 4.3, 6.1, 6.2"
        ::= { nemoHaMobileNetworkPrefixEntry 4 }


    nemoHaMobileNetworkPrefixSource OBJECT-TYPE
        SYNTAX      INTEGER {
                 configured    (1),
                 bindingUpdate (2)
                 }

        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The information source of the mobile network prefix
                 configured with the Binding Update.

                 configured(1): indicates that the mobile network prefix
                 has been manually pre-configured.

                 bindingUpdate(2): indicates that the information is
                 introduced to the home agent by the Mobile Network





                 Prefix Option in the Binding Updates received by the
                 home agent.
                "
        REFERENCE
                "RFC 3963: Sections 4.3, 6.1, 6.2"
        ::= { nemoHaMobileNetworkPrefixEntry 5 }

    nemoBindingCacheTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF NemoBindingCacheEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
               "This table models the Binding Cache that includes
                NEMO-related information and that is maintained by the
                home agent.  Entries in this table are not required
                to survive a reboot of the home agent.
               "
        REFERENCE
                "RFC 3775: Sections 4.5, 9.1, 10.1,
                 RFC 3963: Section 6.1"
        ::= { nemoBindings 1 }

    nemoBindingCacheEntry  OBJECT-TYPE
        SYNTAX      NemoBindingCacheEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "An entry containing additional information related
                 to NEMO-enabled entries in the Binding Cache table
                 of the home agent.
                "
        AUGMENTS {mip6BindingCacheEntry}
    ::= { nemoBindingCacheTable 1 }

    NemoBindingCacheEntry ::= SEQUENCE {
         nemoBindingMrFlag     TruthValue,
         nemoBindingMrMode     INTEGER
        }

    nemoBindingMrFlag OBJECT-TYPE
        SYNTAX      TruthValue
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "true(1): indicates that the Binding Cache entry is from
                 an entity acting as a mobile router.







                 false(2): implies that the Binding Cache entry is from
                 an entity acting as a mobile node.
                "
        REFERENCE
                "RFC 3963: Sections 6.1.1, 6.2"
        ::= { nemoBindingCacheEntry 1 }

    nemoBindingMrMode OBJECT-TYPE
        SYNTAX      INTEGER {
          implicitMode(1),
          explicitMode(2)
                    }
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "implicitMode(1): the Mobile Network Prefix Option is
                 not included in the Binding Update by the mobile
                 router.

                 explicitMode(2): the mobile router included one or
                 more Mobile Network Prefix Options in the Binding
                 Update.
                "
        REFERENCE
                "RFC 3963: Sections 5.2, 6.1.1, 6.2"
        ::= { nemoBindingCacheEntry 2 }

    --
    -- nemoMrEgressIfTable
    --
    nemoMrEgressIfTable        OBJECT-TYPE
         SYNTAX      SEQUENCE OF NemoMrEgressIfEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                 "A table representing the egress interfaces that
                  will be used by the mobile router for roaming to
                  foreign networks.  Each entry in this table
                  represents a configured egress interface.
                 "
         ::= { nemoMrSystem 1 }

    nemoMrEgressIfEntry OBJECT-TYPE
         SYNTAX      NemoMrEgressIfEntry
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                 "An entry in the egress interface table.  It





                  represents a single egress interface entry.
                 "
         INDEX  { nemoMrEgressIfIndex }
         ::= { nemoMrEgressIfTable 1 }

    NemoMrEgressIfEntry ::=
         SEQUENCE {
          nemoMrEgressIfIndex             InterfaceIndex,
          nemoMrEgressIfPriority          Unsigned32,
          nemoMrEgressIfDescription       SnmpAdminString,
          nemoMrEgressIfRoamHoldDownTime  Gauge32
         }

    nemoMrEgressIfIndex  OBJECT-TYPE
         SYNTAX      InterfaceIndex
         MAX-ACCESS  not-accessible
         STATUS      current
         DESCRIPTION
                 "The index of the interface on the mobile router.
                 "
         ::= { nemoMrEgressIfEntry 1 }

    nemoMrEgressIfPriority   OBJECT-TYPE
         SYNTAX      Unsigned32 (0..255)
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                 "The priority configured to the egress interface.
                  This value will be configured to a value between 0
                  and 255.
                 "
         ::= { nemoMrEgressIfEntry 2 }

    nemoMrEgressIfDescription   OBJECT-TYPE
         SYNTAX      SnmpAdminString
         MAX-ACCESS  read-only
         STATUS      current
         DESCRIPTION
                 "A human-readable textual description of the egress
                  interface on the mobile router.
                 "
         ::= { nemoMrEgressIfEntry 3 }

    nemoMrEgressIfRoamHoldDownTime  OBJECT-TYPE
         SYNTAX      Gauge32
         UNITS       "seconds"
         MAX-ACCESS  read-only
         STATUS      current





         DESCRIPTION
                 "This object indicates the time for which the
                  egress interface will be held down during roaming
                  to avoid interface flapping.
                 "
         ::= { nemoMrEgressIfEntry 4 }

    nemoMrDiscoveryRequests OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Total number of Modified Dynamic Home Agent Address
                 Discovery Requests, with Mobile Router Support Flag
                 set, sent by the mobile router.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3775: Sections 10.5, 11.4.1
                 RFC 3963: Section 7.1"
           ::= { nemoMrConf 1 }

    nemoMrDiscoveryReplies OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Total number of Modified Dynamic Home Agent Address
                 Discovery Replies, with Mobile Router Support Flag
                 set, received by the mobile router.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3775: Sections 10.5, 11.4.1
                 RFC 3963: Section 7.2"
           ::= { nemoMrConf 2 }

    nemoMrDiscoveryRepliesRouterFlagZero OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only





        STATUS      current
        DESCRIPTION
                "Total number of Modified Dynamic Home Agent Address
                 Discovery Replies, with Mobile Router Support Flag set
                 to 0 although the flag in the corresponding request
                 is set to 1.  It implies that there is no home agent
                 that supports mobile router functionality in the home
                 network.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3775: Sections 10.5, 11.4.1
                 RFC 3963: Section 7.2"
           ::= { nemoMrConf 3 }

    nemoMrMovedHome OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Number of times the mobile router has detected
                 movement from a foreign network to its home
                 network.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
            "RFC 3963: Section 3"
            ::= { nemoMrConf 4 }

    nemoMrMovedOutofHome OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Number of times the mobile router has detected
                 movement to a foreign network from the home
                 network, has acquired a care-of address, and
                 has initiated the care-of address registration
                 process.






                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
            "RFC 3963: Section 3"
            ::= { nemoMrConf 5 }

    nemoMrMovedFNtoFN OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Number of times the mobile router has detected
                 movement to/from a foreign network from/to another
                 foreign network.  Note that 'movement' implies
                 movement in layer 3, i.e., the mobile router's care-of
                 address changed, and it initiated the care-of address
                 registration process.

                 If there are multiple egress interfaces, this counter
                 counts the total number of movements.  The movement
                 as a mobile node of the mobile entity is not counted.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 3"
            ::= { nemoMrConf 6 }

    nemoMrBetterIfDetected OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Number of times the NEMO entity has found an egress
                 interface with better priority.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
            ::= { nemoMrConf 7 }





    --
    -- nemoStats:nemoMrGlobalStats
    --

    nemoMrBindingAcksWONemoSupport  OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Acknowledgements without
                 NEMO support received by the mobile router.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 5.3"
            ::= { nemoMrGlobalStats 1 }

    nemoMrBindingAcksRegTypeChangeDisallowed  OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Acknowledgements
                 received by the mobile router with status code
                 indicating 'Registration type change disallowed'
                 (Code 139).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3775: Section 9.5.1
                 RFC 3963: Section 6.2"
            ::= { nemoMrGlobalStats 2 }

    nemoMrBindingAcksOperationNotPermitted  OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Acknowledgements
                 received by the mobile router with status code





                 indicating 'Mobile Router Operation not permitted'
                 (Code 140).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 6.6"
            ::= { nemoMrGlobalStats 3 }

    nemoMrBindingAcksInvalidPrefix  OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Acknowledgements
                 received by the mobile router with status code
                 indicating 'Invalid Prefix' (Code 141).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 6.6"
            ::= { nemoMrGlobalStats 4 }

    nemoMrBindingAcksNotAuthorizedForPrefix OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Acknowledgements
                 received by the mobile router with status code
                 indicating 'Not Authorized for Prefix' (Code 142).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963 : Section 6.6"
            ::= { nemoMrGlobalStats 5 }






    nemoMrBindingAcksForwardingSetupFailed OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Acknowledgements
                 received by the mobile router with status code
                 indicating 'Forwarding Setup failed' (Code 143).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 6.6"
            ::= { nemoMrGlobalStats 6 }

    nemoMrBindingAcksOtherError OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Acknowledgements
                 received by the mobile router (Mobile Router Flag is
                 set) with status code other than:

                 successfully processed                  --(Code 0  )
                 mobileRouterOperationNotPermitted (140) --(Code 140)
                 invalidPrefix                     (141) --(Code 141)
                 notAuthorizedForPrefix            (142) --(Code 142)
                 forwardingSetupFailed             (143) --(Code 143)

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963 : Section 6.6"
            ::= { nemoMrGlobalStats 7 }

    --
    -- nemoStats:nemoHaGlobalStats
    --

    nemoHaBUAcksWONemoSupport  OBJECT-TYPE
        SYNTAX      Counter32





        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Acknowledgements
                 without NEMO support sent by the home agent.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 5.3"
            ::= { nemoHaGlobalStats 1 }

    nemoHaBUAcksRegTypeChangeDisallowed  OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Update requests
                 rejected by the home agent with status code
                 in the Binding Acknowledgement indicating
                 'Registration type change disallowed' (Code 139).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3775: Section 9.5.1
                 RFC 3963: Section 6.2"
            ::= { nemoHaGlobalStats 2 }

    nemoHaBUAcksOperationNotPermitted  OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Update requests
                 rejected by the home agent with status code in
                 the Binding Acknowledgement indicating 'Mobile
                 Router Operation not permitted' (Code 140).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of





                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 6.6"
            ::= { nemoHaGlobalStats 3 }

    nemoHaBUAcksInvalidPrefix  OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Update requests
                 rejected by the home agent with status code in
                 the Binding Acknowledgement indicating 'Invalid
                 Prefix' (Code 141).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 6.6"
            ::= { nemoHaGlobalStats 4 }

    nemoHaBUAcksNotAuthorizedForPrefix OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Update requests
                 rejected by the home agent with status code in
                 the Binding Acknowledgement indicating 'Not
                 Authorized for Prefix' (Code 142).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 6.6"
            ::= { nemoHaGlobalStats 5 }

    nemoHaBUAcksForwardingSetupFailed OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current





        DESCRIPTION
                "The total number of Binding Update requests
                 rejected by the home agent with status code in
                 the Binding Acknowledgement indicating 'Forwarding
                 Setup failed' (Code 143).

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 6.6"
            ::= { nemoHaGlobalStats 6 }

    nemoHaBUAcksOtherError OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The total number of Binding Update requests
                 from mobile routers (Mobile Router Flag is set)
                 rejected by the home agent with status code
                 other than:

                 mobileRouterOperationNotPermitted (140)
                 invalidPrefix                     (141)
                 notAuthorizedForPrefix            (142)
                 forwardingSetupFailed             (143)

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoCounterDiscontinuityTime.
                "
        REFERENCE
                "RFC 3963: Section 6.6"
            ::= { nemoHaGlobalStats 7 }

    nemoHaCounterTable OBJECT-TYPE
        SYNTAX      SEQUENCE OF NemoHaCounterEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "A table containing registration statistics for all
                 mobile routers registered with the home agent.
                "
        ::= { nemoHaStats 2 }





    nemoHaCounterEntry  OBJECT-TYPE
        SYNTAX      NemoHaCounterEntry
        MAX-ACCESS  not-accessible
        STATUS      current
        DESCRIPTION
                "Home agent registration statistics for a mobile
                 router.

                 Implementers need to be aware that if the total
                 number of octets in mip6BindingHomeAddress
                 exceeds 113, then OIDs of column instances in
                 this row will have more than 128 sub-identifiers and
                 cannot be accessed using SNMPv1, SNMPv2c, or SNMPv3.
                "
        INDEX   { mip6BindingHomeAddressType,
                  mip6BindingHomeAddress
                }
        ::= { nemoHaCounterTable 1 }

    NemoHaCounterEntry      ::= SEQUENCE {
        nemoHaBURequestsAccepted       Counter32,
        nemoHaBURequestsDenied         Counter32,
        nemoHaBCEntryCreationTime      DateAndTime,
        nemoHaBUAcceptedTime           DateAndTime,
        nemoHaBURejectionTime          DateAndTime,
        nemoHaRecentBURejectionCode    NemoBURequestRejectionCode,
        nemoHaCtrDiscontinuityTime     TimeStamp
        }

    nemoHaBURequestsAccepted OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "Total number of Binding Update requests from the
                 mobile router accepted by the home agent.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoHaCtrDiscontinuityTime.
                "
        ::= { nemoHaCounterEntry 1 }

    nemoHaBURequestsDenied   OBJECT-TYPE
        SYNTAX      Counter32
        MAX-ACCESS  read-only
        STATUS      current





        DESCRIPTION
                "Total number of Binding Update requests from the
                 mobile router rejected by the home agent.

                 Discontinuities in the value of this counter can
                 occur at re-initialization of the management system,
                 and at other times as indicated by the value of
                 nemoHaCtrDiscontinuityTime.
                "
        ::= { nemoHaCounterEntry 2 }

    nemoHaBCEntryCreationTime   OBJECT-TYPE
        SYNTAX      DateAndTime (SIZE (11))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The time when the current Binding Cache entry was
                 created for the mobile router.  An implementation
                 MUST return all 11 bytes of the DateAndTime
                 textual-convention so that a manager may retrieve
                 the offset from GMT time.
                "
        ::= { nemoHaCounterEntry 3 }

    nemoHaBUAcceptedTime  OBJECT-TYPE
        SYNTAX      DateAndTime (SIZE (11))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The time at which the last Binding Update was
                 accepted by the home agent for this mobile router.
                 An implementation MUST return all 11 bytes of the
                 DateAndTime textual-convention so that a manager
                 may retrieve the offset from GMT time.
                "
        ::= { nemoHaCounterEntry 4 }

    nemoHaBURejectionTime  OBJECT-TYPE
        SYNTAX      DateAndTime (SIZE (11))
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The time at which the last Binding Update was
                 rejected by the home agent for this mobile router.
                 If there have been no rejections, then this object
                 will be inaccessible.  An implementation MUST return
                 all 11 bytes of the DateAndTime textual-convention
                 so that a manager may retrieve the offset from GMT





                 time.
                "
        ::= { nemoHaCounterEntry 5 }

    nemoHaRecentBURejectionCode  OBJECT-TYPE
        SYNTAX      NemoBURequestRejectionCode
        MAX-ACCESS  read-only
        STATUS      current
        DESCRIPTION
                "The Status code (>= 128) in the latest Binding
                 Acknowledgment indicating a rejection, sent to this
                 mobile router.

                 If a Binding Update request is rejected and a Binding
                 Acknowledgment is not sent to this mobile router,
                 then this will be the value of the Status code that
                 corresponds to the reason of the rejection.  If there
                 have been no Binding Update request rejections, then
                 this object will be inaccessible.
                "
        ::= { nemoHaCounterEntry 6 }

    nemoHaCtrDiscontinuityTime OBJECT-TYPE
       SYNTAX      TimeStamp
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
               "The value of sysUpTime on the most recent occasion
                at which any one or more of the counters in this row,
                viz., instances of 'nemoHaBURequestsAccepted' and
                'nemoHaBURequestsDenied', suffered a discontinuity.
                If no such discontinuity has occurred since the
                last re-initialization of the local management
                subsystem, then this object will have a zero value.
               "
       ::= { nemoHaCounterEntry 7 }

    --
    --
    -- nemoNotifications
    --
    --

    nemoHomeTunnelEstablished NOTIFICATION-TYPE
        OBJECTS   {
                    nemoMrBLActiveEgressIfIndex,
                    nemoMrBLEstablishedHomeTunnelIfIndex,
                    mip6MnBLCOAType,





                    mip6MnBLCOA,
                    nemoMrBLHomeAddressPrefixLength,
                    nemoMrBLCareofAddressPrefixLength
                  }

        STATUS    current
        DESCRIPTION
                "This notification is sent by the mobile router
                 every time the tunnel is established between the
                 home agent and the mobile router.
                "
        REFERENCE
                "RFC 3963: Section 5.5"
            ::= { nemoNotifications 1 }

    nemoHomeTunnelReleased NOTIFICATION-TYPE
        OBJECTS {
                    nemoMrBLActiveEgressIfIndex,
                    nemoMrBLEstablishedHomeTunnelIfIndex,
                    mip6MnBLCOAType,
                    mip6MnBLCOA,
                    nemoMrBLHomeAddressPrefixLength,
                    nemoMrBLCareofAddressPrefixLength
                }
        STATUS    current
        DESCRIPTION
                "This notification is sent by the mobile router
                 every time the tunnel is deleted between the home
                 agent and the mobile router.
                "
        REFERENCE
                "RFC 3963: Section 5.5"
            ::= { nemoNotifications 2}

    -- Conformance information
    nemoGroups      OBJECT IDENTIFIER ::= { nemoConformance 1 }
    nemoCompliances OBJECT IDENTIFIER ::= { nemoConformance 2 }

    -- Units of conformance
    nemoSystemGroup    OBJECT-GROUP
         OBJECTS {
                   nemoCapabilities,
                   nemoStatus
        }
         STATUS  current
         DESCRIPTION
                 "A collection of objects for basic NEMO
                  monitoring.





                 "
         ::= { nemoGroups 1 }

    nemoBindingCacheGroup    OBJECT-GROUP
         OBJECTS {
                   nemoBindingMrFlag,
                   nemoBindingMrMode
        }
         STATUS  current
         DESCRIPTION
                 "A collection of objects for monitoring the
                  NEMO extensions of the Binding Cache.
                 "
         ::= { nemoGroups 2 }

    nemoStatsGroup    OBJECT-GROUP
         OBJECTS {
                   nemoCounterDiscontinuityTime
        }
         STATUS  current
         DESCRIPTION
                 "A collection of objects for
                  monitoring NEMO statistics.
                 "
         ::= { nemoGroups 3 }

    nemoMrConfGroup   OBJECT-GROUP
         OBJECTS {
                   nemoMrEgressIfPriority,
                   nemoMrEgressIfDescription,
                   nemoMrEgressIfRoamHoldDownTime,
                   nemoMrDiscoveryRequests,
                   nemoMrDiscoveryReplies,
                   nemoMrDiscoveryRepliesRouterFlagZero,
                   nemoMrMovedHome,
                   nemoMrMovedOutofHome,
                   nemoMrMovedFNtoFN,
                   nemoMrBetterIfDetected
        }
         STATUS  current
         DESCRIPTION
                 "A collection of objects for monitoring
                  the configuration-related information on
                  the mobile router.
                 "
         ::= { nemoGroups 4 }

    nemoMrRegistrationGroup  OBJECT-GROUP





         OBJECTS {
                   nemoMrBLMode,
                   nemoMrBLMrFlag,
                   nemoMrBLHomeAddressPrefixLength,
                   nemoMrBLCareofAddressPrefixLength,
                   nemoMrBLActiveEgressIfIndex,
                   nemoMrBLEstablishedHomeTunnelIfIndex,
                   nemoMrMobilityMessagesSent,
                   nemoMrMobilityMessagesRecd,
                   nemoMrPrefixRegMode,
                   nemoMrBindingAcksWONemoSupport,
                   nemoMrBindingAcksRegTypeChangeDisallowed,
                   nemoMrBindingAcksOperationNotPermitted,
                   nemoMrBindingAcksInvalidPrefix,
                   nemoMrBindingAcksNotAuthorizedForPrefix,
                   nemoMrBindingAcksForwardingSetupFailed,
                   nemoMrBindingAcksOtherError
        }
         STATUS  current
         DESCRIPTION
                 "A collection of objects for monitoring
                  the registration details and statistics for
                  the mobile router.
                 "
         ::= { nemoGroups 5 }

    nemoHaSystemGroup    OBJECT-GROUP
        OBJECTS {
                  nemoHaMobileNetworkPrefixType,
                  nemoHaMobileNetworkPrefix,
                  nemoHaMobileNetworkPrefixLength,
                  nemoHaMobileNetworkPrefixSource
       }
        STATUS  current
        DESCRIPTION
                "A collection of objects for basic NEMO
                 configuration monitoring at the home agent.
                "
        ::= { nemoGroups 6 }

    nemoHaStatsGroup   OBJECT-GROUP
        OBJECTS {
                  nemoHaBURequestsAccepted,
                  nemoHaBURequestsDenied,
                  nemoHaBCEntryCreationTime,
                  nemoHaBUAcceptedTime,
                  nemoHaBURejectionTime,
                  nemoHaRecentBURejectionCode,





                  nemoHaCtrDiscontinuityTime
       }
        STATUS  current
        DESCRIPTION
                "A collection of objects for monitoring NEMO
                 registration-related statistics pertaining to
                 the mobile routers registered with the home agent.
                "
        ::= { nemoGroups 7 }

    nemoHaGlobalStatsGroup   OBJECT-GROUP
        OBJECTS {
                  nemoHaBUAcksWONemoSupport,
                  nemoHaBUAcksRegTypeChangeDisallowed,
                  nemoHaBUAcksOperationNotPermitted,
                  nemoHaBUAcksInvalidPrefix,
                  nemoHaBUAcksNotAuthorizedForPrefix,
                  nemoHaBUAcksForwardingSetupFailed,
                  nemoHaBUAcksOtherError
       }
        STATUS  current
        DESCRIPTION
                "A collection of objects for monitoring basic
                 NEMO advertisement and registration statistics
                 on a home agent.
                "
        ::= { nemoGroups 8 }

    nemoNotificationGroup   NOTIFICATION-GROUP
        NOTIFICATIONS {
                 nemoHomeTunnelEstablished,
                 nemoHomeTunnelReleased
       }
        STATUS  current
        DESCRIPTION
                "A collection of notifications from a home agent
                 or correspondent node to the manager about the
                 tunnel status of the mobile router.
                "
        ::= { nemoGroups 9 }

    -- Compliance statements
    nemoCoreCompliance MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities
                 that implement the NEMO-MIB.
                 "





         MODULE  -- this module
             MANDATORY-GROUPS { nemoSystemGroup
                              }
         ::= { nemoCompliances 1 }

    nemoCompliance2 MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities that
                 implement the NEMO-MIB and support monitoring of
                 the Binding Cache.

                 There are a number of INDEX objects that cannot be
                 represented in the form of OBJECT clauses in SMIv2,
                 but for which there are compliance requirements,
                 expressed in OBJECT-clause form in this description:

                 -- OBJECT      mip6BindingHomeAddressType
                 -- SYNTAX      InetAddressType { ipv6(2) }
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6BindingHomeAddress
                 --     object.
                 --
                 -- OBJECT      mip6BindingHomeAddress
                 -- SYNTAX      InetAddress (SIZE(16))
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6BindingHomeAddress
                 --     object.
                 --
                 "
         MODULE  -- this module
             MANDATORY-GROUPS { nemoSystemGroup,
                                nemoBindingCacheGroup
                              }
         ::= { nemoCompliances 2 }

    nemoCoreReadOnlyCompliance MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities
                 that implement the NEMO-MIB without support
                 for read-write (i.e., in read-only mode).
                 "
         MODULE  -- this module
             MANDATORY-GROUPS { nemoSystemGroup
                              }





         OBJECT      nemoStatus
         MIN-ACCESS  read-only
         DESCRIPTION
                "Write access is not required."
         ::= { nemoCompliances 3 }

    nemoReadOnlyCompliance2 MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities that
                 implement the NEMO-MIB without support for read-write
                 (i.e., in read-only mode) and with support for
                 monitoring of the Binding Cache.

                 There are a number of INDEX objects that cannot be
                 represented in the form of OBJECT clauses in SMIv2,
                 but for which there are compliance requirements,
                 expressed in OBJECT-clause form in this description:

                 -- OBJECT      mip6BindingHomeAddressType
                 -- SYNTAX      InetAddressType { ipv6(2) }
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6BindingHomeAddress
                 --     object.
                 --
                 -- OBJECT      mip6BindingHomeAddress
                 -- SYNTAX      InetAddress (SIZE(16))
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6BindingHomeAddress
                 --     object.
                 --
                 "
         MODULE  -- this module
             MANDATORY-GROUPS { nemoSystemGroup,
                                nemoBindingCacheGroup
                              }
         OBJECT      nemoStatus
         MIN-ACCESS  read-only
         DESCRIPTION
                "Write access is not required."
         ::= { nemoCompliances 4 }

    nemoMrCompliance MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities that





                 implement the NEMO-MIB for monitoring configuration-
                 related information, registration details, and
                 statistics on a mobile router.

                 There are a number of INDEX objects that cannot be
                 represented in the form of OBJECT clauses in SMIv2,
                 but for which there are compliance requirements,
                 expressed in OBJECT-clause form in this description:

                 -- OBJECT      mip6MnHomeAddressType
                 -- SYNTAX      InetAddressType { ipv6(2) }
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6MnHomeAddress
                 --     object.
                 --
                 -- OBJECT      mip6MnHomeAddress
                 -- SYNTAX      InetAddress (SIZE(16))
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6MnHomeAddress
                 --     object.
                 --
                 -- OBJECT      mip6MnBLNodeAddressType
                 -- SYNTAX      InetAddressType { ipv6(2) }
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6MnBLNodeAddress
                 --     object.
                 --
                 -- OBJECT      mip6MnBLNodeAddress
                 -- SYNTAX      InetAddress (SIZE(16))
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6MnBLNodeAddress
                 --     object.
                 "
         MODULE  -- this module
             MANDATORY-GROUPS { nemoStatsGroup,
                                nemoMrConfGroup,
                                nemoMrRegistrationGroup
                              }
         ::= { nemoCompliances 5 }

    nemoMrReadOnlyCompliance2 MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities that





                 implement the NEMO-MIB without support for read-
                 write (i.e., in read-only mode) and with support for
                 monitoring of configuration-related information,
                 registration details, and statistics on a mobile
                 router.

                 There are a number of INDEX objects that cannot be
                 represented in the form of OBJECT clauses in SMIv2,
                 but for which there are compliance requirements,
                 expressed in OBJECT-clause form in this description:

                 -- OBJECT      mip6MnHomeAddressType
                 -- SYNTAX      InetAddressType { ipv6(2) }
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6MnHomeAddress
                 --     object.
                 --
                 -- OBJECT      mip6MnHomeAddress
                 -- SYNTAX      InetAddress (SIZE(16))
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6MnHomeAddress
                 --     object.
                 --
                 -- OBJECT      mip6MnBLNodeAddressType
                 -- SYNTAX      InetAddressType { ipv6(2) }
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6MnBLNodeAddress
                 --     object.
                 --
                 -- OBJECT      mip6MnBLNodeAddress
                 -- SYNTAX      InetAddress (SIZE(16))
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6MnBLNodeAddress
                 --     object.
                 "
         MODULE  -- this module
             MANDATORY-GROUPS { nemoStatsGroup,
                                nemoMrConfGroup,
                                nemoMrRegistrationGroup
                              }

         OBJECT      nemoMrPrefixRegMode
         MIN-ACCESS  read-only
         DESCRIPTION





                "Write access is not required."
         ::= { nemoCompliances 6 }


    nemoHaCoreCompliance MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities that
                 implement the NEMO-MIB for configuration monitoring
                 at the home agent.

                 There are a number of INDEX objects that cannot be
                 represented in the form of OBJECT clauses in SMIv2,
                 but for which there are compliance requirements,
                 expressed in OBJECT-clause form in this description:

                 -- OBJECT      mip6BindingHomeAddressType
                 -- SYNTAX      InetAddressType { ipv6(2) }
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6BindingHomeAddress
                 --     object.
                 --
                 -- OBJECT      mip6BindingHomeAddress
                 -- SYNTAX      InetAddress (SIZE(16))
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6BindingHomeAddress
                 --     object.
                 --
                 "
         MODULE  -- this module
             MANDATORY-GROUPS { nemoHaSystemGroup
                              }
         ::= { nemoCompliances 7 }

    nemoHaCompliance2 MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities that
                 implement the NEMO-MIB with support for monitoring
                 of the home agent functionality, specifically the
                 home-agent-registration-related statistics.

                 There are a number of INDEX objects that cannot be
                 represented in the form of OBJECT clauses in SMIv2,
                 but for which there are compliance requirements,
                 expressed in OBJECT-clause form in this description:





                 -- OBJECT      mip6BindingHomeAddressType
                 -- SYNTAX      InetAddressType { ipv6(2) }
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6BindingHomeAddress
                 --     object.
                 --
                 -- OBJECT      mip6BindingHomeAddress
                 -- SYNTAX      InetAddress (SIZE(16))
                 -- DESCRIPTION
                 --     This MIB module requires support for global
                 --     IPv6 addresses for the mip6BindingHomeAddress
                 --     object.
                 --
                 "
         MODULE  -- this module
             MANDATORY-GROUPS { nemoHaSystemGroup,
                                nemoHaStatsGroup,
                                nemoHaGlobalStatsGroup
                              }
         ::= { nemoCompliances 8 }

    nemoNotificationCompliance MODULE-COMPLIANCE
         STATUS  current
         DESCRIPTION
                "The compliance statement for SNMP entities that
                 implement the NEMO-MIB and support Notification
                 from the home agent.
                 "
         MODULE  -- this module
             MANDATORY-GROUPS { nemoNotificationGroup
                              }
         ::= { nemoCompliances 9 }

    END

















