RADIUS-DYNAUTH-SERVER-MIB DEFINITIONS ::= BEGIN


IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE,
       Counter32, Integer32, mib-2,
       TimeTicks         FROM SNMPv2-SMI             -- [RFC2578]
       SnmpAdminString   FROM SNMP-FRAMEWORK-MIB     -- [RFC3411]
       InetAddressType,
       InetAddress       FROM INET-ADDRESS-MIB       -- [RFC4001]
       MODULE-COMPLIANCE,
       OBJECT-GROUP  FROM SNMPv2-CONF;               -- [RFC2580]

radiusDynAuthServerMIB MODULE-IDENTITY
       LAST-UPDATED "200608290000Z" -- 29 August 2006
       ORGANIZATION "IETF RADEXT Working Group"
       CONTACT-INFO
              " Stefaan De Cnodder
                Alcatel
                Francis Wellesplein 1
                B-2018 Antwerp
                Belgium

                Phone: +32 3 240 85 15
                EMail: stefaan.de_cnodder@alcatel.be

                Nagi Reddy Jonnala
                Cisco Systems, Inc.
                Divyasree Chambers, B Wing,
                O'Shaugnessy Road,
                Bangalore-560027, India.

                Phone: +91 94487 60828
                EMail: njonnala@cisco.com

                Murtaza Chiba
                Cisco Systems, Inc.
                170 West Tasman Dr.
                San Jose CA, 95134

                Phone: +1 408 525 7198
                EMail: mchiba@cisco.com "
       DESCRIPTION
           "The MIB module for entities implementing the server
            side of the Dynamic Authorization Extensions to the
            Remote Authentication Dial-In User Service (RADIUS)
            protocol.  Copyright (C) The Internet Society (2006).





            Initial version as published in RFC 4673; for full
            legal notices see the RFC itself."

       REVISION "200608290000Z" -- 29 August 2006
       DESCRIPTION "Initial version as published in RFC 4673."
       ::= { mib-2 146 }

radiusDynAuthServerMIBObjects OBJECT IDENTIFIER ::=
                                      { radiusDynAuthServerMIB 1 }

radiusDynAuthServerScalars    OBJECT IDENTIFIER ::=
                               { radiusDynAuthServerMIBObjects 1 }

radiusDynAuthServerDisconInvalidClientAddresses OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of Disconnect-Request packets received from
             unknown addresses.  This counter may experience a
             discontinuity when the DAS module (re)starts, as
             indicated by the value of
             radiusDynAuthServerCounterDiscontinuity."
      ::= { radiusDynAuthServerScalars 1 }

radiusDynAuthServerCoAInvalidClientAddresses OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of CoA-Request packets received from unknown
             addresses.  This counter may experience a discontinuity
             when the DAS module (re)starts, as indicated by the
             value of radiusDynAuthServerCounterDiscontinuity."
      ::= { radiusDynAuthServerScalars 2 }

radiusDynAuthServerIdentifier OBJECT-TYPE
      SYNTAX SnmpAdminString
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The NAS-Identifier of the RADIUS Dynamic Authorization
              Server.  This is not necessarily the same as sysName in
              MIB II."
      REFERENCE
             "RFC 2865, Section 5.32, NAS-Identifier."
      ::= { radiusDynAuthServerScalars 3 }






radiusDynAuthClientTable OBJECT-TYPE
      SYNTAX SEQUENCE OF RadiusDynAuthClientEntry
      MAX-ACCESS not-accessible
      STATUS     current
      DESCRIPTION
            "The (conceptual) table listing the RADIUS Dynamic
             Authorization Clients with which the server shares a
             secret."
      ::= { radiusDynAuthServerMIBObjects 2 }

radiusDynAuthClientEntry OBJECT-TYPE
       SYNTAX     RadiusDynAuthClientEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
             "An entry (conceptual row) representing one Dynamic
              Authorization Client with which the server shares a
              secret."
       INDEX      { radiusDynAuthClientIndex }
       ::= { radiusDynAuthClientTable 1 }

RadiusDynAuthClientEntry ::= SEQUENCE {
       radiusDynAuthClientIndex                     Integer32,
       radiusDynAuthClientAddressType               InetAddressType,
       radiusDynAuthClientAddress                   InetAddress,
       radiusDynAuthServDisconRequests              Counter32,
       radiusDynAuthServDisconAuthOnlyRequests      Counter32,
       radiusDynAuthServDupDisconRequests           Counter32,
       radiusDynAuthServDisconAcks                  Counter32,
       radiusDynAuthServDisconNaks                  Counter32,
       radiusDynAuthServDisconNakAuthOnlyRequests   Counter32,
       radiusDynAuthServDisconNakSessNoContext      Counter32,
       radiusDynAuthServDisconUserSessRemoved       Counter32,
       radiusDynAuthServMalformedDisconRequests     Counter32,
       radiusDynAuthServDisconBadAuthenticators     Counter32,
       radiusDynAuthServDisconPacketsDropped        Counter32,
       radiusDynAuthServCoARequests                 Counter32,
       radiusDynAuthServCoAAuthOnlyRequests         Counter32,
       radiusDynAuthServDupCoARequests              Counter32,
       radiusDynAuthServCoAAcks                     Counter32,
       radiusDynAuthServCoANaks                     Counter32,
       radiusDynAuthServCoANakAuthOnlyRequests      Counter32,
       radiusDynAuthServCoANakSessNoContext         Counter32,
       radiusDynAuthServCoAUserSessChanged          Counter32,
       radiusDynAuthServMalformedCoARequests        Counter32,
       radiusDynAuthServCoABadAuthenticators        Counter32,
       radiusDynAuthServCoAPacketsDropped           Counter32,
       radiusDynAuthServUnknownTypes                Counter32,





       radiusDynAuthServerCounterDiscontinuity      TimeTicks
}


radiusDynAuthClientIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
             "A number uniquely identifying each RADIUS Dynamic
              Authorization Client with which this Dynamic
              Authorization Server communicates.  This number is
              allocated by the agent implementing this MIB module
              and is unique in this context."
       ::= { radiusDynAuthClientEntry 1 }

radiusDynAuthClientAddressType OBJECT-TYPE
       SYNTAX     InetAddressType
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The type of IP address of the RADIUS Dynamic
              Authorization Client referred to in this table entry."
       ::= { radiusDynAuthClientEntry 2 }

radiusDynAuthClientAddress OBJECT-TYPE
       SYNTAX     InetAddress
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The IP address value of the RADIUS Dynamic
              Authorization Client referred to in this table entry,
              using the version neutral IP address format.  The type
              of this address is determined by the value of
              the radiusDynAuthClientAddressType object."
       ::= { radiusDynAuthClientEntry 3 }

radiusDynAuthServDisconRequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS Disconnect-Requests received
              from this Dynamic Authorization Client.  This also
              includes the RADIUS Disconnect-Requests that have a
              Service-Type attribute with value 'Authorize Only'.
              This counter may experience a discontinuity when the





              DAS module (re)starts as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM)."
       ::= { radiusDynAuthClientEntry 4 }

radiusDynAuthServDisconAuthOnlyRequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS Disconnect-Requests that include
              a Service-Type attribute with value 'Authorize Only'
              received from this Dynamic Authorization Client.  This
              counter may experience a discontinuity when the DAS
              module (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM)."
       ::= { radiusDynAuthClientEntry 5 }

radiusDynAuthServDupDisconRequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of duplicate RADIUS Disconnect-Request
              packets received from this Dynamic Authorization
              Client.  This counter may experience a discontinuity
              when the DAS module (re)starts, as indicated by the
              value of radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM)."
       ::= { radiusDynAuthClientEntry 6 }

radiusDynAuthServDisconAcks  OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "replies"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS Disconnect-ACK packets sent to
              this Dynamic Authorization Client.  This counter may
              experience a discontinuity when the DAS module
              (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."





       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM)."
       ::= { radiusDynAuthClientEntry 7 }

radiusDynAuthServDisconNaks OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "replies"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS Disconnect-NAK packets
              sent to this Dynamic Authorization Client.  This
              includes the RADIUS Disconnect-NAK packets sent
              with a Service-Type attribute with value 'Authorize
              Only' and the RADIUS Disconnect-NAK packets sent
              because no session context was found.  This counter
              may experience a discontinuity when the DAS module
              (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM)."
       ::= { radiusDynAuthClientEntry 8 }

radiusDynAuthServDisconNakAuthOnlyRequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "replies"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS Disconnect-NAK packets that
              include a Service-Type attribute with value
              'Authorize Only' sent to this Dynamic Authorization
              Client.  This counter may experience a discontinuity
              when the DAS module (re)starts, as indicated by the
              value of radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM)."
       ::= { radiusDynAuthClientEntry 9 }

radiusDynAuthServDisconNakSessNoContext OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "replies"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS Disconnect-NAK packets
              sent to this Dynamic Authorization Client
              because no session context was found.  This counter may





              experience a discontinuity when the DAS module
              (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM)."
       ::= { radiusDynAuthClientEntry 10 }

radiusDynAuthServDisconUserSessRemoved OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "sessions"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of user sessions removed for the
              Disconnect-Requests received from this
              Dynamic Authorization Client.  Depending on site-
              specific policies, a single Disconnect request
              can remove multiple user sessions.  In cases where
              this Dynamic Authorization Server has no
              knowledge of the number of user sessions that
              are affected by a single request, each such
              Disconnect-Request will count as a single
              affected user session only.  This counter may experience
              a discontinuity when the DAS module (re)starts, as
              indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM)."
       ::= { radiusDynAuthClientEntry 11 }

radiusDynAuthServMalformedDisconRequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of malformed RADIUS Disconnect-Request
              packets received from this Dynamic Authorization
              Client.  Bad authenticators and unknown types are not
              included as malformed Disconnect-Requests.  This counter
              may experience a discontinuity when the DAS module
              (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM), and
              Section 2.3, Packet Format."
       ::= { radiusDynAuthClientEntry 12 }






radiusDynAuthServDisconBadAuthenticators OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS Disconnect-Request packets
              that contained an invalid Authenticator field
              received from this Dynamic Authorization Client.  This
              counter may experience a discontinuity when the DAS
              module (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM), and
              Section 2.3, Packet Format."
       ::= { radiusDynAuthClientEntry 13 }

radiusDynAuthServDisconPacketsDropped OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of incoming Disconnect-Requests
              from this Dynamic Authorization Client silently
              discarded by the server application for some reason
              other than malformed, bad authenticators, or unknown
              types.  This counter may experience a discontinuity
              when the DAS module (re)starts, as indicated by the
              value of radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.1, Disconnect Messages (DM), and
              Section 2.3, Packet Format."
       ::= { radiusDynAuthClientEntry 14 }

radiusDynAuthServCoARequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS CoA-requests received from this
              Dynamic Authorization Client.  This also includes
              the CoA requests that have a Service-Type attribute
              with value 'Authorize Only'.  This counter may
              experience a discontinuity when the DAS module
              (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."





       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA)."
       ::= { radiusDynAuthClientEntry 15 }

radiusDynAuthServCoAAuthOnlyRequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS CoA-requests that include a
              Service-Type attribute with value 'Authorize Only'
              received from this Dynamic Authorization Client.  This
              counter may experience a discontinuity when the DAS
              module (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA)."
       ::= { radiusDynAuthClientEntry 16 }


radiusDynAuthServDupCoARequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of duplicate RADIUS CoA-Request packets
              received from this Dynamic Authorization Client.  This
              counter may experience a discontinuity when the DAS
              module (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA)."
       ::= { radiusDynAuthClientEntry 17 }

radiusDynAuthServCoAAcks  OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "replies"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS CoA-ACK packets sent to this
              Dynamic Authorization Client.  This counter may
              experience a discontinuity when the DAS module





              (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA)."
       ::= { radiusDynAuthClientEntry 18 }

radiusDynAuthServCoANaks OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "replies"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS CoA-NAK packets sent to
              this Dynamic Authorization Client.  This includes
              the RADIUS CoA-NAK packets sent with a Service-Type
              attribute with value 'Authorize Only' and the RADIUS
              CoA-NAK packets sent because no session context was
              found.  This counter may experience a discontinuity
              when the DAS module (re)starts, as indicated by the
              value of radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA)."
       ::= { radiusDynAuthClientEntry 19 }

radiusDynAuthServCoANakAuthOnlyRequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "replies"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS CoA-NAK packets that include a
              Service-Type attribute with value 'Authorize Only'
              sent to this Dynamic Authorization Client.  This counter
              may experience a discontinuity when the DAS module
              (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA)."
       ::= { radiusDynAuthClientEntry 20 }

radiusDynAuthServCoANakSessNoContext OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "replies"
       MAX-ACCESS read-only
       STATUS     current





       DESCRIPTION
             "The number of RADIUS CoA-NAK packets sent to this
              Dynamic Authorization Client because no session context
              was found.  This counter may experience a discontinuity
              when the DAS module (re)starts, as indicated by the
              value of radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA)."
       ::= { radiusDynAuthClientEntry 21 }

radiusDynAuthServCoAUserSessChanged OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "sessions"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of user sessions authorization
              changed for the CoA-Requests received from this
              Dynamic Authorization Client.  Depending on site-
              specific policies, a single CoA request can change
              multiple user sessions' authorization.  In cases where
              this Dynamic Authorization Server has no knowledge of
              the number of user sessions that are affected by a
              single request, each such CoA-Request will
              count as a single affected user session only.  This
              counter may experience a discontinuity when the DAS
              module (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA)."
       ::= { radiusDynAuthClientEntry 22 }

radiusDynAuthServMalformedCoARequests OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of malformed RADIUS CoA-Request packets
              received from this Dynamic Authorization Client.  Bad
              authenticators and unknown types are not included as
              malformed CoA-Requests.  This counter may experience a
              discontinuity when the DAS module (re)starts, as
              indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE





             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA), and Section 2.3, Packet Format."
       ::= { radiusDynAuthClientEntry  23 }

radiusDynAuthServCoABadAuthenticators OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of RADIUS CoA-Request packets that
              contained an invalid Authenticator field received
              from this Dynamic Authorization Client.  This counter
              may experience a discontinuity when the DAS module
              (re)starts, as indicated by the value of
                radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA), and Section 2.3, Packet Format."
       ::= { radiusDynAuthClientEntry 24 }

radiusDynAuthServCoAPacketsDropped OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of incoming CoA packets from this
              Dynamic Authorization Client silently discarded
              by the server application for some reason other than
              malformed, bad authenticators, or unknown types.  This
              counter may experience a discontinuity when the DAS
              module (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.2, Change-of-Authorization
              Messages (CoA), and Section 2.3, Packet Format."
       ::= { radiusDynAuthClientEntry 25 }

radiusDynAuthServUnknownTypes OBJECT-TYPE
       SYNTAX     Counter32
       UNITS      "requests"
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The number of incoming packets of unknown types that
              were received on the Dynamic Authorization port.  This
              counter may experience a discontinuity when the DAS





              module (re)starts, as indicated by the value of
              radiusDynAuthServerCounterDiscontinuity."
       REFERENCE
             "RFC 3576, Section 2.3, Packet Format."
       ::= { radiusDynAuthClientEntry 26 }

radiusDynAuthServerCounterDiscontinuity OBJECT-TYPE
       SYNTAX TimeTicks
       UNITS  "hundredths of a second"
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The time (in hundredths of a second) since the
              last counter discontinuity.  A discontinuity may
              be the result of a reinitialization of the DAS
              module within the managed entity."
       ::= { radiusDynAuthClientEntry 27 }


-- conformance information

radiusDynAuthServerMIBConformance
       OBJECT IDENTIFIER ::= { radiusDynAuthServerMIB 2 }
radiusDynAuthServerMIBCompliances
       OBJECT IDENTIFIER ::= { radiusDynAuthServerMIBConformance 1 }
radiusDynAuthServerMIBGroups
       OBJECT IDENTIFIER ::= { radiusDynAuthServerMIBConformance 2 }

-- compliance statements

radiusAuthServerMIBCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
             "The compliance statement for entities implementing
              the RADIUS Dynamic Authorization Server.  Implementation
              of this module is for entities that support IPv4 and/or
              IPv6."
       MODULE  -- this module
       MANDATORY-GROUPS { radiusDynAuthServerMIBGroup }

       OBJECT             radiusDynAuthClientAddressType
       SYNTAX             InetAddressType { ipv4(1), ipv6(2) }
       DESCRIPTION
           "An implementation is only required to support IPv4 and
            globally unique IPv6 addresses."

       OBJECT             radiusDynAuthClientAddress
       SYNTAX             InetAddress (SIZE(4|16))





       DESCRIPTION
           "An implementation is only required to support IPv4 and
            globally unique IPv6 addresses."

       GROUP              radiusDynAuthServerAuthOnlyGroup
       DESCRIPTION
             "Only required for Dynamic Authorization Clients that
              are supporting Service-Type attributes with value
              'Authorize-Only'."


       GROUP              radiusDynAuthServerNoSessGroup
       DESCRIPTION
             "This group is not required if the Dynamic
              Authorization Server cannot easily determine whether
              a session exists (e.g., in case of a RADIUS
              proxy)."

       ::= { radiusDynAuthServerMIBCompliances 1 }

-- units of conformance

radiusDynAuthServerMIBGroup OBJECT-GROUP
       OBJECTS { radiusDynAuthServerDisconInvalidClientAddresses,
                 radiusDynAuthServerCoAInvalidClientAddresses,
                 radiusDynAuthServerIdentifier,
                 radiusDynAuthClientAddressType,
                 radiusDynAuthClientAddress,
                 radiusDynAuthServDisconRequests,
                 radiusDynAuthServDupDisconRequests,
                 radiusDynAuthServDisconAcks,
                 radiusDynAuthServDisconNaks,
                 radiusDynAuthServDisconUserSessRemoved,
                 radiusDynAuthServMalformedDisconRequests,
                 radiusDynAuthServDisconBadAuthenticators,
                 radiusDynAuthServDisconPacketsDropped,
                 radiusDynAuthServCoARequests,
                 radiusDynAuthServDupCoARequests,
                 radiusDynAuthServCoAAcks,
                 radiusDynAuthServCoANaks,
                 radiusDynAuthServCoAUserSessChanged,
                 radiusDynAuthServMalformedCoARequests,
                 radiusDynAuthServCoABadAuthenticators,
                 radiusDynAuthServCoAPacketsDropped,
                 radiusDynAuthServUnknownTypes,
                 radiusDynAuthServerCounterDiscontinuity
               }
       STATUS  current





       DESCRIPTION
             "The collection of objects providing management of
              a RADIUS Dynamic Authorization Server."
       ::= { radiusDynAuthServerMIBGroups 1 }

radiusDynAuthServerAuthOnlyGroup OBJECT-GROUP
       OBJECTS { radiusDynAuthServDisconAuthOnlyRequests,
                 radiusDynAuthServDisconNakAuthOnlyRequests,
                 radiusDynAuthServCoAAuthOnlyRequests,
                 radiusDynAuthServCoANakAuthOnlyRequests
               }
       STATUS  current
       DESCRIPTION
             "The collection of objects supporting the RADIUS
              messages including Service-Type attribute with
              value 'Authorize Only'."
       ::= { radiusDynAuthServerMIBGroups 2 }

radiusDynAuthServerNoSessGroup OBJECT-GROUP
       OBJECTS { radiusDynAuthServDisconNakSessNoContext,
                 radiusDynAuthServCoANakSessNoContext
               }
       STATUS  current
       DESCRIPTION
             "The collection of objects supporting the RADIUS
              messages that are referring to non-existing sessions."
       ::= { radiusDynAuthServerMIBGroups 3 }


END






















