ATM2-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
       Gauge32, Counter32, Integer32
           FROM SNMPv2-SMI
       TruthValue, RowStatus, TimeStamp
           FROM SNMPv2-TC
       MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
           FROM SNMPv2-CONF
       SnmpAdminString
           FROM SNMP-FRAMEWORK-MIB
       InterfaceIndex, InterfaceIndexOrZero, ifIndex
           FROM IF-MIB
       atmMIBObjects, atmInterfaceConfEntry,
       atmVplEntry, atmVplVpi,
       atmVclEntry, atmVclVpi, atmVclVci,





       atmVpCrossConnectEntry, atmVcCrossConnectEntry
           FROM ATM-MIB
       AtmAddr, AtmSigDescrParamIndex,
       AtmInterfaceType, AtmIlmiNetworkPrefix,
       AtmVcIdentifier, AtmVpIdentifier,
       AtmTrafficDescrParamIndex
           FROM ATM-TC-MIB;

   atm2MIB MODULE-IDENTITY
       LAST-UPDATED "200309230000Z"
       ORGANIZATION "IETF AToMMIB Working Group"
       CONTACT-INFO
         "AToMMIB WG
             http://www.ietf.org/html.charters/atommib-charter.html
           Editors:
                    Faye Ly
           Postal:  Pedestal Networks
                    6503 Dumbarton Circle
                    Fremont, CA 94555
                    USA
           Tel:     +1 510 896 2908
           E-Mail:  faye@pedestalnetworks.com

                    Michael Noto
           Postal:  Cisco Systems
                    170 W. Tasman Drive
                    San Jose, CA 95134-1706
                    USA

           E-mail:  mnoto@cisco.com

                    Andrew Smith
           Postal:  Consultant

           E-Mail:  ah_smith@acm.org

                    Ethan Mickey Spiegel
           Postal:  Cisco Systems
                    170 W. Tasman Drive
                    San Jose, CA 95134-1706
                    USA
           Tel:     +1 408 526 6408
           Fax:     +1 408 526 6488
           E-Mail:  mspiegel@cisco.com

                    Kaj Tesink
           Postal:  Telcordia Technologies
                    331 Newman Springs Road





                    Red Bank, NJ 07701
                    USA
           Tel:     +1 732 758 5254
           E-mail:  kaj@research.telcordia.com"
       DESCRIPTION
         "Copyright (C) The Internet Society (2003). This version of
         this MIB module is part of RFC 3606; see the RFC itself for
         full legal notices.

         This MIB Module is a supplement to the ATM-MIB
         defined in RFC 2515."
       REVISION "200309230000Z"
       DESCRIPTION
         "Initial version of this MIB, published as RFC 3606."

         ::= { atmMIBObjects 14 }

   atm2MIBObjects  OBJECT IDENTIFIER ::= {atm2MIB 1}

   atm2MIBTraps OBJECT IDENTIFIER ::= {atm2MIB 2}

   -- This ATM2-MIB Module consists of the following tables,
   -- plus ATM trap support:
   --      1. atmSvcVpCrossConnectTable
   --      2. atmSvcVcCrossConnectTable
   --      3. atmSigStatTable
   --      4. atmSigSupportTable
   --      5. atmSigDescrParamTable
   --      6. atmIfRegisteredAddrTable
   --      7. atmVclAddrTable
   --      8. atmAddrVclTable
   --      9. atmVplStatTable
   --      10. atmVplLogicalPortTable
   --      11. atmVclStatTable
   --      12. atmAal5VclStatTable
   --      13. atmVclGenTable
   --      14. atmInterfaceExtTable
   --      15. atmIlmiSrvcRegTable
   --      16. atmIlmiNetworkPrefixTable
   --      17. atmSwitchAddressTable
   --      18. atmVpCrossConnectXTable
   --      19. atmVcCrossConnectXTable
   --      20. atmCurrentlyFailingPVplTable
   --      21. atmCurrentlyFailingPVclTable

   -- 1. ATM VPL SVC Cross-Connect Table

   atmSvcVpCrossConnectTable OBJECT-TYPE





       SYNTAX       SEQUENCE OF
                    AtmSvcVpCrossConnectEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
         "The ATM SVPC Cross-Connect table.  A
         bi-directional VP cross-connect between two
         switched VPLs is modeled as one entry in this
         table.  A Soft PVPC cross-connect, between a
         soft permanent VPL and a switched VPL, is
         also modeled as one entry in this table."
       ::= { atm2MIBObjects 1 }

   atmSvcVpCrossConnectEntry OBJECT-TYPE
       SYNTAX       AtmSvcVpCrossConnectEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
         "An entry in the ATM SVPC Cross-Connect table.
         This entry is used to model a bi-directional
         ATM VP cross-connect between two VPLs."
       INDEX { atmSvcVpCrossConnectIndex,
               atmSvcVpCrossConnectLowIfIndex,
               atmSvcVpCrossConnectLowVpi,
               atmSvcVpCrossConnectHighIfIndex,
               atmSvcVpCrossConnectHighVpi }
       ::= { atmSvcVpCrossConnectTable 1 }

   AtmSvcVpCrossConnectEntry ::= SEQUENCE {
       atmSvcVpCrossConnectIndex           INTEGER,
       atmSvcVpCrossConnectLowIfIndex      InterfaceIndex,
       atmSvcVpCrossConnectLowVpi          AtmVpIdentifier,
       atmSvcVpCrossConnectHighIfIndex     InterfaceIndex,
       atmSvcVpCrossConnectHighVpi         AtmVpIdentifier,
       atmSvcVpCrossConnectCreationTime    TimeStamp,
       atmSvcVpCrossConnectRowStatus       RowStatus
                     }

   atmSvcVpCrossConnectIndex OBJECT-TYPE
       SYNTAX       INTEGER (1..2147483647)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
         "A unique value to identify this SVPC
         cross-connect.  For each VP associated
         with this cross-connect, the agent reports
         this cross-connect index value in the
         atmVplCrossConnectIdentifer attribute of the





         corresponding atmVplTable entries."
       ::= { atmSvcVpCrossConnectEntry 1 }

   atmSvcVpCrossConnectLowIfIndex OBJECT-TYPE
       SYNTAX       InterfaceIndex
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
         "The value of this object is equal to the
         ifIndex value of the ATM interface port for this
         SVPC cross-connect.  The term low implies
         that this ATM interface has the numerically lower
         ifIndex value than the other ATM interface
         identified in the same atmSvcVpCrossConnectEntry."
       ::= { atmSvcVpCrossConnectEntry 2 }

   atmSvcVpCrossConnectLowVpi OBJECT-TYPE
       SYNTAX       AtmVpIdentifier
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
         "The value of this object is equal to the VPI
         value associated with the SVPC cross-connect
         at the ATM interface that is identified by
         atmSvcVpCrossConnectLowIfIndex.  The VPI value
         cannot exceed the number supported by the
         atmInterfaceCurrentMaxSvpcVpi at the low ATM interface
         port."
       ::= { atmSvcVpCrossConnectEntry 3 }

   atmSvcVpCrossConnectHighIfIndex OBJECT-TYPE
       SYNTAX       InterfaceIndex
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "The value of this object is equal to the
         ifIndex value of the ATM interface port for
         this SVC VP cross-connect.  The term high
         implies that this ATM interface has the
         numerically higher ifIndex value than the
         other ATM interface identified in the same
         atmSvcVpCrossConnectEntry."
       ::= { atmSvcVpCrossConnectEntry 4 }

   atmSvcVpCrossConnectHighVpi OBJECT-TYPE
       SYNTAX       AtmVpIdentifier
       MAX-ACCESS   not-accessible
       STATUS       current





       DESCRIPTION
        "The value of this object is equal to the VPI
         value associated with the SVPC cross-connect
         at the ATM interface that is identified by
         atmSvcVpCrossConnectHighIfIndex.  The VPI value
         cannot exceed the number supported by the
         atmInterfaceCurrentMaxSvpcVpi at the high ATM interface
         port."
       ::= { atmSvcVpCrossConnectEntry 5 }

   atmSvcVpCrossConnectCreationTime OBJECT-TYPE
       SYNTAX       TimeStamp
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "The value of the sysUpTime object
         at the time this bi-directional SVPC
         cross-connect was created.  If the current
         state was entered prior to the last
         re-initialization of the agent, then this
         object contains a zero value."
       ::= { atmSvcVpCrossConnectEntry 6 }

   atmSvcVpCrossConnectRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
           "This object is used to delete rows in the
            atmSvcVpCrossConnectTable."
       ::= { atmSvcVpCrossConnectEntry 7 }

   -- 2. ATM VCL SVC Cross-Connect Table

   atmSvcVcCrossConnectTable OBJECT-TYPE
       SYNTAX       SEQUENCE OF AtmSvcVcCrossConnectEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "The ATM SVCC Cross-Connect table.  A
         bi-directional VC cross-connect between two
         switched VCLs is modeled as one entry in
         this table.  A Soft PVCC cross-connect,
         between a soft permanent VCL and a switched
         VCL, is also modeled as one entry in this
         table."
       ::= { atm2MIBObjects 2 }






   atmSvcVcCrossConnectEntry OBJECT-TYPE
       SYNTAX       AtmSvcVcCrossConnectEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "An entry in the ATM SVCC Cross-Connect table.
         This entry is used to model a bi-directional ATM
         VC cross-connect between two VCLs."
       INDEX { atmSvcVcCrossConnectIndex,
               atmSvcVcCrossConnectLowIfIndex,
               atmSvcVcCrossConnectLowVpi,
               atmSvcVcCrossConnectLowVci,
               atmSvcVcCrossConnectHighIfIndex,
               atmSvcVcCrossConnectHighVpi,
               atmSvcVcCrossConnectHighVci }
       ::= { atmSvcVcCrossConnectTable 1 }

   AtmSvcVcCrossConnectEntry ::= SEQUENCE {
       atmSvcVcCrossConnectIndex           INTEGER,
       atmSvcVcCrossConnectLowIfIndex      InterfaceIndex,
       atmSvcVcCrossConnectLowVpi          AtmVpIdentifier,
       atmSvcVcCrossConnectLowVci          AtmVcIdentifier,
       atmSvcVcCrossConnectHighIfIndex     InterfaceIndex,
       atmSvcVcCrossConnectHighVpi         AtmVpIdentifier,
       atmSvcVcCrossConnectHighVci         AtmVcIdentifier,
       atmSvcVcCrossConnectCreationTime    TimeStamp,
       atmSvcVcCrossConnectRowStatus       RowStatus
               }

   atmSvcVcCrossConnectIndex OBJECT-TYPE
       SYNTAX       INTEGER (1..2147483647)
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "A unique value to identify this SVCC cross-connect.
         For each VP associated with this cross-connect, the
         agent reports this cross-connect index value in the
         atmVclCrossConnectIdentifier attribute of the
         corresponding atmVplTable entries."
       ::= { atmSvcVcCrossConnectEntry 1 }

   atmSvcVcCrossConnectLowIfIndex OBJECT-TYPE
       SYNTAX       InterfaceIndex
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "The value of this object is equal to the
         ifIndex value of the ATM interface port for this





         SVCC cross-connect.  The term low implies that
         this ATM interface has the numerically lower
         ifIndex value than the other ATM interface
         identified in the same atmSvcVcCrossConnectEntry."
       ::= { atmSvcVcCrossConnectEntry 2 }

   atmSvcVcCrossConnectLowVpi OBJECT-TYPE
       SYNTAX       AtmVpIdentifier
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "The value of this object is equal to the VPI
         value associated with the SVCC cross-connect
         at the ATM interface that is identified by
         atmSvcVcCrossConnectLowIfIndex.  The VPI value
         cannot exceed the number supported by the
         atmInterfaceCurrentMaxSvccVpi at the low ATM interface
         port."
       ::= { atmSvcVcCrossConnectEntry 3 }

   atmSvcVcCrossConnectLowVci OBJECT-TYPE
       SYNTAX       AtmVcIdentifier
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "The value of this object is equal to the VCI
         value associated with the SVCC cross-connect
         at the ATM interface that is identified by
         atmSvcVcCrossConnectLowIfIndex.  The VCI value
         cannot exceed the number supported by the
         atmInterfaceCurrentMaxSvccVci at the low ATM interface
         port."
       ::= { atmSvcVcCrossConnectEntry 4 }

   atmSvcVcCrossConnectHighIfIndex OBJECT-TYPE
       SYNTAX       InterfaceIndex
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "The value of this object is equal to the
         ifIndex value for the ATM interface port for
         this SVCC cross-connect.  The term high implies
         that this ATM interface has the numerically
         higher ifIndex value than the other ATM interface
         identified in the same atmSvcVcCrossConnectEntry."
       ::= { atmSvcVcCrossConnectEntry 5 }

   atmSvcVcCrossConnectHighVpi OBJECT-TYPE





       SYNTAX       AtmVpIdentifier
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "The value of this object is equal to the VPI
         value associated with the SVCC cross-connect
         at the ATM interface that is identified by
         atmSvcVcCrossConnectHighIfIndex.  The VPI value
         cannot exceed the number supported by the
         atmInterfaceCurrentMaxSvccVpi at the high ATM interface
         port."
       ::= { atmSvcVcCrossConnectEntry 6 }

   atmSvcVcCrossConnectHighVci OBJECT-TYPE
       SYNTAX       AtmVcIdentifier
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "The value of this object is equal to the VCI
         value associated with the SVCC cross-connect
         at the ATM interface that is identified by
         atmSvcVcCrossConnectHighIfIndex.  The VCI value
         cannot exceed the number supported by the
         atmInterfaceMaxVciBits at the high ATM interface
         port."
       ::= { atmSvcVcCrossConnectEntry 7 }

   atmSvcVcCrossConnectCreationTime OBJECT-TYPE
       SYNTAX       TimeStamp
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
        "The value of the sysUpTime object
         at the time this bi-directional SVCC
         cross-connect was created.  If the current
         state was entered prior to the last
         re-initialization of the agent, then this
         object contains a zero value."
       ::= { atmSvcVcCrossConnectEntry 8 }

   atmSvcVcCrossConnectRowStatus OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-write
       STATUS       current
       DESCRIPTION
           "This object is used to delete rows in the
            atmSvcVcCrossConnectTable."
       ::= { atmSvcVcCrossConnectEntry 9 }





   -- 3. ATM Interface Signalling Statistics Table --

   atmSigStatTable       OBJECT-TYPE
       SYNTAX       SEQUENCE OF AtmSigStatEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This table contains ATM interface signalling
        statistics, one entry per ATM signalling
        interface."
       ::= { atm2MIBObjects 3 }

   atmSigStatEntry         OBJECT-TYPE
       SYNTAX       AtmSigStatEntry
       MAX-ACCESS   not-accessible
       STATUS       current
       DESCRIPTION
        "This list contains signalling statistics variables."
       INDEX { ifIndex }
       ::= { atmSigStatTable  1}

   AtmSigStatEntry    ::= SEQUENCE  {
       atmSigSSCOPConEvents            Counter32,
       atmSigSSCOPErrdPdus             Counter32,
       atmSigDetectSetupAttempts       Counter32,
       atmSigEmitSetupAttempts         Counter32,
       atmSigDetectUnavailRoutes       Counter32,
       atmSigEmitUnavailRoutes         Counter32,
       atmSigDetectUnavailResrcs       Counter32,
       atmSigEmitUnavailResrcs         Counter32,
       atmSigDetectCldPtyEvents        Counter32,
       atmSigEmitCldPtyEvents          Counter32,
       atmSigDetectMsgErrors           Counter32,
       atmSigEmitMsgErrors             Counter32,
       atmSigDetectClgPtyEvents        Counter32,
       atmSigEmitClgPtyEvents          Counter32,
       atmSigDetectTimerExpireds       Counter32,
       atmSigEmitTimerExpireds         Counter32,
       atmSigDetectRestarts            Counter32,
       atmSigEmitRestarts              Counter32,
       atmSigInEstabls                 Counter32,
       atmSigOutEstabls                Counter32
            }

   atmSigSSCOPConEvents   OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current





       DESCRIPTION
           "SSCOP Connection Events Counter.  This counter counts
            the sum of the following errors:

            1) SSCOP Connection Disconnect Counter

                The abnormal occurrence of this event is
                characterized by the expiry of Timer_NO_RESPONSE.
                (This event is communicated to the layer management
                with MAA-ERROR code P.  See ITU-T Q.2110.)

             2) SSCOP Connection Initiation Failure

                This condition indicates the inability to establish
                an SSCOP connection.  This event occurs whenever the
                number of expiries of the connection control timer
                (Timer_CC) equals or exceeds the MaxCC, or upon
                receipt of a connection reject message BGREJ PDU.
                (This event is communicated to layer management with
                MAA-ERROR code O.  See ITU-T Q.2110.)

             3) SSCOP Connection Re-Establ/Resynch

                This event occurs upon receipt of a BGN PDU or
                RS PDU."
       REFERENCE
           "ITU-T Recommendation Q.2110, Broadband
            Integrated Services Digital Network
            (B-ISDN) - ATM Adaptation Layer - Service
            Specific Connection Oriented Protocol (SSCOP)
            Specification, July 1994."
       ::= { atmSigStatEntry 1}

   atmSigSSCOPErrdPdus   OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "SSCOP Errored PDUs Counter.  This counter counts the
           sum of the following errors:

           1) Invalid PDUs.
              These are defined in SSCOP and consist of PDUs
              with an incorrect length (MAA-ERROR code U), an
              undefined PDU type code, or that are not 32-bit
              aligned.

           2) PDUs that result in MAA-ERROR codes and are





              discarded.

           See MAA-ERROR codes A-D, F-M, and Q-T defined in
           ITU-T Q.2110."
       REFERENCE
           "ITU-T Recommendation Q.2110, Broadband
            Integrated Services Digital Network
            (B-ISDN) - ATM Adaptation Layer - Service
            Specific Connection Oriented Protocol (SSCOP)
            Specification, July 1994."
       ::= { atmSigStatEntry 2 }

   atmSigDetectSetupAttempts    OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "Call Setup Attempts Counter.  This counter counts
           the number of call setup attempts (both successful
           and unsuccessful) detected on this interface."
       ::= { atmSigStatEntry 3 }

   atmSigEmitSetupAttempts    OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "Call Setup Attempts Counter.  This counter counts
           the number of call setup attempts (both successful
           and unsuccessful) transmitted on this interface."
       ::= { atmSigStatEntry 4 }

   atmSigDetectUnavailRoutes    OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "Number of Route Unavailability detected on this interface.
           This counter is incremented when a RELEASE, RELEASE COMPLETE
           (only when not preceded by a RELEASE message for the same
           call), ADD PARTY REJECT, or STATUS message that
           contains one of the following cause code values is
           received (Note: These cause values
           apply to both UNI3.0 and UNI3.1):

           Cause Value            Meaning







              1            unallocated (unassigned) number
              2            no route to specified transit network
              3            no route to destination

           NOTE:  For this counter, RELEASE COMPLETE
           messages that are a reply to a previous RELEASE
           message and contain the same cause value, are
           redundant (for counting purposes) and should not
           be counted."

       ::= { atmSigStatEntry 5 }

   atmSigEmitUnavailRoutes    OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "Number of Route Unavailability transmitted from this
           interface.  This counter is incremented when a RELEASE,
           RELEASE COMPLETE (only when not preceded by a RELEASE
           message for the same call), ADD PARTY REJECT, or
           STATUS message that contains one of the following cause
           code values is transmitted (Note: These cause values apply
           to both UNI3.0 and UNI3.1):

           Cause Value            Meaning

              1            unallocated (unassigned) number
              2            no route to specified transit network
              3            no route to destination

           NOTE:  For this counter, RELEASE COMPLETE
           messages that are a reply to a previous RELEASE
           message and contain the same cause value, are
           redundant (for counting purposes) and should not
           be counted."
       ::= { atmSigStatEntry 6 }

   atmSigDetectUnavailResrcs     OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
           "Number of Resource Unavailability detected on this
           interface.  This counter is incremented when a RELEASE,
           RELEASE COMPLETE (only when not preceded by a RELEASE
           message for the same call), ADD PARTY REJECT, or
           STATUS message that contains one of the following





           cause code values is received (Note: These cause
           values apply to both UNI3.0 and UNI3.1 unless
           otherwise stated):

           Cause Value          Meaning

              35          requested VPCI/VCI not available
              37          user cell rate not available (UNI3.1
                          only)
              38          network out of order
              41          temporary failure
              45          no VPCI/VCI available
              47          resource unavailable, unspecified
              49          Quality of Service unavailable
              51          user cell rate not available (UNI3.0
                          only)
              58          bearer capability not presently
                          available
              63          Service or option not available,
                          unspecified
              92          too many pending add party requests

           NOTE:  For this counter, RELEASE COMPLETE
           messages that are a reply to a previous RELEASE
           message and contain the same cause value, are
           redundant (for counting purposes) and should not
           be counted."
       ::= { atmSigStatEntry 7 }

   atmSigEmitUnavailResrcs     OBJECT-TYPE
       SYNTAX       Counter32
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
          "Number of Resource Unavailability transmitted from this
          interface.  This counter is incremented when a RELEASE,
          RELEASE COMPLETE (only when not preceded by a RELEASE message
          for the same call), ADD PARTY REJECT, or STATUS message that
          contains one of the following cause code values is transmitted
          (Note: These cause values apply to both UNI3.0 and UNI3.1
          unless otherwise stated):

          Cause Value          Meaning

             35          requested VPCI/VCI not available
             37          user cell rate not available (UNI3.1
                         only)
             38          network out of order





             41          temporary failure
             45          no VPCI/VCI available
             47          resource unavailable, unspecified
             49          Quality of Service unavailable
             51          user cell rate not available (UNI3.0
                         only)
             58          bearer capability not presently
                         available
             63          Service or option not available,
                         unspecified
             92          too many pending add party requests

          NOTE:  For this counter, RELEASE COMPLETE messages that are a
          reply to a previous RELEASE message and contain the same cause
          value, are redundant (for counting purposes) and should not be
          counted."

      ::= { atmSigStatEntry 8 }

  atmSigDetectCldPtyEvents     OBJECT-TYPE
      SYNTAX       Counter32
      MAX-ACCESS   read-only
      STATUS       current
      DESCRIPTION
         "Number of Called Party Responsible For Unsuccessful Call
         detected on this interface.  This counter is incremented when a
         RELEASE, RELEASE COMPLETE (only when not preceded by a RELEASE
         message for the same call), ADD PARTY REJECT, or STATUS message
         that contains one of the following cause code values is
         received (Note: These cause values apply to both UNI3.0 and
         UNI3.1):

         Cause Value         Meaning

            17           user busy
            18           no user responding
            21           call rejected
            22           number changed
            23           user rejects all calls with calling
                         line identification restriction (CLIR)
            27           destination out of order
            31           normal, unspecified
            88           incompatible destination


         NOTE:  For this counter, RELEASE COMPLETE messages that are a
         reply to a previous RELEASE message and contain the same cause
         value, are redundant (for counting purposes) and should not be





         counted.

         Note: Cause Value #30 'response to STATUS ENQUIRY' was not
         included in this memo since it did not apply to a hard
         failure."

     ::= { atmSigStatEntry 9 }

 atmSigEmitCldPtyEvents     OBJECT-TYPE
     SYNTAX       Counter32
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION

        "Number of Called Party Responsible For Unsuccessful Call
        transmitted from this interface.  This counter is incremented
        when a RELEASE, RELEASE COMPLETE (only when not preceded by a
        RELEASE message for the same call), ADD PARTY REJECT, or STATUS
        message that contains one of the following cause code values is
        transmitted (Note: These cause values apply to both UNI3.0 and
        UNI3.1):

        Cause Value         Meaning

           17           user busy
           18           no user responding
           21           call rejected
           22           number changed
           23           user rejects all calls with calling
                        line identification restriction (CLIR)
           27           destination out of order
           31           normal, unspecified
           88           incompatible destination

        NOTE:  For this counter, RELEASE COMPLETE messages that are a
        reply to a previous RELEASE message and contain the same cause
        value, are redundant (for counting purposes) and should not be
        counted.

        Note: Cause Value #30 'response to STATUS ENQUIRY' was not
        included in this memo since it did not apply to a hard failure."

    ::= { atmSigStatEntry 10 }

atmSigDetectMsgErrors    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current





    DESCRIPTION
       "Number of Incorrect Messages detected on this interface.  The
       Incorrect Messages Counter reflects any sort of incorrect
       information in a message.  This includes:

       - RELEASE, RELEASE COMPLETE, ADD PARTY REJECT,
         and STATUS messages transmitted, that contain any of
         the Cause values listed below.

       - Ignored messages.  These messages are dropped
         because the message was so damaged that it could
         not be further processed.  A list of dropped
         messages is compiled below:

          1.  Message with invalid protocol discriminator

          2.  Message with errors in the call reference I.E.
               - Bits 5-8 of the first octet not equal to
                 '0000'
               - Bits 1-4 of the first octet indicating a
                 length other than 3 octets
               - RELEASE COMPLETE message received with a
                 call reference that does not relate to a
                 call active or in progress
               - SETUP message received with call reference
                 flag incorrectly set to 1
               - SETUP message received with a call
                 reference for a call that is already
                 active or in progress.

          3.  Message too short

       The following cause values are monitored by this counter (Note:
       These cause values apply to both UNI3.0 and UNI3.1 unless
       otherwise stated):

       Cause Value     Meaning

          10     VPCI/VCI unacceptable (UNI3.0 only)
          36     VPCI/VCI assignment failure (UNI3.1 only)
          81     invalid call reference value
          82     identified channel does not exist
          89     invalid endpoint reference
          96     mandatory information element is missing
          97     message type non-existent or not
                 implemented
          99     information element non-existent or not
                 implemented





          100    invalid information element contents
          101    message not compatible with call state
          104    incorrect message length
          111    protocol error, unspecified

          NOTE:  For this counter, RELEASE COMPLETE messages that are
          a reply to a previous RELEASE message and contain the same
          cause value, are redundant (for counting purposes) and
          should not be counted."

    ::= { atmSigStatEntry 11 }

atmSigEmitMsgErrors    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of Incorrect Messages transmitted on this interface.
       The Incorrect Messages Counter reflects any sort of incorrect
       information in a message.  This includes:

       - RELEASE, RELEASE COMPLETE, ADD PARTY REJECT,
         and STATUS messages transmitted or
         received, that contain any of the Cause values
         listed below.

       - Ignored messages.  These messages are dropped
         because the message was so damaged that it could
         not be further processed.  A list of dropped
         messages is compiled below:

          1.  Message with invalid protocol discriminator

          2.  Message with errors in the call reference I.E.
               - Bits 5-8 of the first octet not equal to
                 '0000'
               - Bits 1-4 of the first octet indicating a
                 length other than 3 octets
               - RELEASE COMPLETE message received with a
                 call reference that does not relate to a
                 call active or in progress
               - SETUP message received with call reference
                 flag incorrectly set to 1
               - SETUP message received with a call
                 reference for a call that is already
                 active or in progress.

          3.  Message too short





       The following cause values are monitored by this counter
       (Note: These cause values apply to both UNI3.0 and UNI3.1
       unless otherwise stated):

       Cause Value     Meaning

          10     VPCI/VCI unacceptable (UNI3.0 only)
          36     VPCI/VCI assignment failure (UNI3.1 only)
          81     invalid call reference value
          82     identified channel does not exist
          89     invalid endpoint reference
          96     mandatory information element is missing
          97     message type non-existent or not
                 implemented
          99     information element non-existent or not
                 implemented
          100    invalid information element contents
          101    message not compatible with call state
          104    incorrect message length
          111    protocol error, unspecified

          NOTE:  For this counter, RELEASE COMPLETE messages that are
          a reply to a previous RELEASE message and contain the same
          cause value, are redundant (for counting purposes) and
          should not be counted."

    ::= { atmSigStatEntry 12 }

atmSigDetectClgPtyEvents    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of Calling Party Events detected on this interface.
       This counter monitors error events that occur due to the
       originating user doing something wrong.  This counter is
       incremented when a RELEASE, RELEASE COMPLETE (only when not
       preceded by a RELEASE message for the same call), ADD PARTY
       REJECT, or STATUS message that contains one of the following
       cause code values is received (Note: These cause values
       apply to both UNI3.0 and UNI3.1):

       Cause Value     Meaning

          28     invalid number format (address incomplete)
          43     access information discarded
          57     bearer capability not authorized
          65     bearer capability not implemented





          73     unsupported combination of traffic
                 parameters
          78     AAL parameters cannot be supported (UNI3.1
                 only)
          91     invalid transit network selection
          93     AAL parameters cannot be supported (UNI3.0
                 only)

          NOTE:  For this counter, RELEASE COMPLETE messages that
          are a reply to a previous RELEASE message and contain
          the same cause value, are redundant (for counting purposes)
          and should not be counted."

    ::= { atmSigStatEntry 13 }

atmSigEmitClgPtyEvents    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of Calling Party Events transmitted from this interface.
       This counter monitors error events that occur due to the
       originating user doing something wrong.  This counter is
       incremented when a RELEASE, RELEASE COMPLETE (only when not
       preceded by a RELEASE message for the same call), ADD PARTY
       REJECT, or STATUS message that contains one of the following
       cause code values is transmitted (Note: These cause values
       apply to both UNI3.0 and UNI3.1):

       Cause Value     Meaning

          28     invalid number format (address incomplete)
          43     access information discarded
          57     bearer capability not authorized
          65     bearer capability not implemented
          73     unsupported combination of traffic
                 parameters
          78     AAL parameters cannot be supported (UNI3.1
                 only)
          91     invalid transit network selection
          93     AAL parameters cannot be supported (UNI3.0
                 only)

          NOTE:  For this counter, RELEASE COMPLETE messages that are
          a reply to a previous RELEASE message and contain the same
          cause value, are redundant (for counting purposes) and
          should not be counted."






    ::= { atmSigStatEntry 14 }

atmSigDetectTimerExpireds    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of Timer Expiries detected on this interface.  The Timer
       Expiries Counter provides a count of network timer expiries, and
       to some extent, host or switch timer expiries.  The conditions
       for incrementing this counter are:

          - Expiry of any network timer

          - Receipt of a RELEASE or RELEASE COMPLETE
            message with Cause #102, 'recovery on
            timer expiry'.

          NOTE:  For this counter, RELEASE COMPLETE messages that are
          a reply to a previous RELEASE message and contain the same
          cause value, are redundant (for counting purposes) and
          should not be counted."

    ::= { atmSigStatEntry 15 }

atmSigEmitTimerExpireds    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of Timer Expiries transmitted from this interface.
       The Timer Expiries Counter provides a count of network timer
       expiries, and to some extent, host or switch timer expiries.
       The conditions for incrementing this counter are:

          - Expiry of any network timer

          - Receipt of a RELEASE or RELEASE COMPLETE
            message with Cause #102, 'recovery on
            timer expiry'.

       NOTE:  For this counter, RELEASE COMPLETE messages that are a
       reply to a previous RELEASE message and contain the same cause
       value, are redundant (for counting purposes) and should not be
       counted."

    ::= { atmSigStatEntry 16 }






atmSigDetectRestarts    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of Restart Activity errors detected on this interface.
       The Restart Activity Counter provides a count of host, switch,
       or network restart activity.  This counter is incremented when
       receiving a RESTART message."

    ::= { atmSigStatEntry 17 }

atmSigEmitRestarts    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of Restart Activity errors transmitted from this
       interface.  The Restart Activity Counter provides a count of
       host, switch, or network restart activity.  This counter is
       incremented when transmitting a RESTART message."

    ::= { atmSigStatEntry 18 }

atmSigInEstabls    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of SVCs established at this signalling entity for
       incoming connections."
    ::= { atmSigStatEntry 19 }

atmSigOutEstabls    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of SVCs established at this signalling entity for
       outgoing connections."
    ::= { atmSigStatEntry 20 }

  -- 4. ATM Interface Signalling Support Table
  --
  -- This table provides information to support
  -- the signalling process which is used to establish
  -- ATM Switched Virtual Connections (SVCs).






atmSigSupportTable       OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmSigSupportEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This table contains ATM local interface configuration
       parameters, one entry per ATM signalling interface."
    ::= { atm2MIBObjects 4 }

atmSigSupportEntry         OBJECT-TYPE
    SYNTAX       AtmSigSupportEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This list contains signalling configuration parameters
       and state variables."
    INDEX { ifIndex }
    ::= { atmSigSupportTable  1}

AtmSigSupportEntry    ::= SEQUENCE  {
    atmSigSupportClgPtyNumDel       INTEGER,
    atmSigSupportClgPtySubAddr      INTEGER,
    atmSigSupportCldPtySubAddr      INTEGER,
    atmSigSupportHiLyrInfo          INTEGER,
    atmSigSupportLoLyrInfo          INTEGER,
    atmSigSupportBlliRepeatInd      INTEGER,
    atmSigSupportAALInfo            INTEGER,
    atmSigSupportPrefCarrier        OCTET STRING
}

atmSigSupportClgPtyNumDel     OBJECT-TYPE
    SYNTAX       INTEGER  { enabled(1), disabled(2) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "This object indicates whether the Calling Party Number
       Information Element is transferred to the called party
       address.  The value of this object can be:

         - enabled(1)  This Information Element is transferred
                       to the called party

         - disabled(2) This Information Element is NOT
                       transferred to the called party."

    ::= { atmSigSupportEntry 1 }

atmSigSupportClgPtySubAddr   OBJECT-TYPE





    SYNTAX       INTEGER  { enabled(1), disabled(2) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "This object indicates whether to accept and transfer the Calling
       Party Subaddress Information Element from the calling party to
       the called party.  Calling party subaddress information shall
       only be transferred to the called party if calling party number
       delivery is enabled (i.e., atmSigSupportClgPtyNumDel =
       'enabled(1)'.  The value of this object can be:

         - enabled(1)  This Information Element is transferred
                       to the called party

         - disabled(2) This Information Element is NOT
                       transferred to the called party."

    ::= { atmSigSupportEntry 2 }

atmSigSupportCldPtySubAddr    OBJECT-TYPE
    SYNTAX       INTEGER  { enabled(1), disabled(2) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "This object indicates whether to accept, transfer, and deliver
       the Called Party Subaddress Information Element from the calling
       party to the called party.  The value of this object can be:

         - enabled(1)  This Information Element is transferred
                       to the called party

         - disabled(2) This Information Element is NOT
                       transferred to the called party."

    ::= { atmSigSupportEntry 3 }

atmSigSupportHiLyrInfo     OBJECT-TYPE
    SYNTAX       INTEGER  { enabled(1), disabled(2) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "This object indicates whether to accept, transfer, and deliver
       the Broadband High Layer Information Element from the calling
       party to the called party.  The value of this object can be:

         - enabled(1)  This Information Element is transferred
                       to the called party






         - disabled(2) This Information Element is NOT
                       transferred to the called party."

    ::= { atmSigSupportEntry 4 }

atmSigSupportLoLyrInfo     OBJECT-TYPE
    SYNTAX       INTEGER  { enabled(1), disabled(2) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "This object indicates whether to accept, transfer, and deliver
       the Broadband Low Layer Information Element from the calling
       party to the called party.  The value of this object can be:

         - enabled(1)  This Information Element is transferred
                       to the called party

         - disabled(2) This Information Element is NOT
                       transferred to the called party."

    ::= { atmSigSupportEntry 5 }

atmSigSupportBlliRepeatInd      OBJECT-TYPE
    SYNTAX       INTEGER  { enabled(1), disabled(2) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
        "This object indicates whether to accept, transfer, and deliver
        the Broadband Repeat Indicator with two or three instances of
        the Broadband Low Layer Information Element for low layer
        information selection from the calling party to the called
        party.  This object's value should always be disabled(2) if
        the value of atmSigSupportLolyrInfo is disabled(2).

        The value of this object can be:

        - enabled(1)  This Information Element is transferred
              to the called party

        - disabled(2) This Information Element is NOT
              transferred to the called party."
    ::= { atmSigSupportEntry 6 }

atmSigSupportAALInfo     OBJECT-TYPE
    SYNTAX       INTEGER  { enabled(1), disabled(2) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION





       "This object indicates whether to accept, transfer, and deliver
       the ATM Adaptation Layer Parameters Information Element from the
       calling party to the called party.  The value of this object can
       be:

         - enabled(1)  This Information Element is transferred
                       to the called party

         - disabled(2) This Information Element is NOT
                       transferred to the called party."

    ::= { atmSigSupportEntry 7 }

atmSigSupportPrefCarrier     OBJECT-TYPE
    SYNTAX       OCTET STRING (SIZE(0|4))
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "This parameter identifies the carrier to which intercarrier
       calls originated from this interface are routed when transit
       network selection information is not provided by the calling
       party.  If a Carrier Identification Code (CIC) is used the
       parameter shall contain the CIC.  For three-digit CICs, the first
       octet shall be '0' and the CIC is contained in the three
       following octets.  If the preferred carrier feature is not
       supported the value is a zero-length string."

    ::= { atmSigSupportEntry 8 }

  -- 5. ATM Signalling Descriptor Parameter Table

    atmSigDescrParamTable     OBJECT-TYPE
        SYNTAX       SEQUENCE OF AtmSigDescrParamEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "A table contains signalling capabilities of VCLs except the
            Traffic Descriptor.  Traffic descriptors are described in
            the atmTrafficDescrParamTable."

        REFERENCE
            "ATM User-Network Interface Specification, Version 3.1 (UNI
            3.1), September 1994, Section 5.4.5 Variable Length
            Information Elements."

        ::= { atm2MIBObjects 5 }

    atmSigDescrParamEntry        OBJECT-TYPE





        SYNTAX       AtmSigDescrParamEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Each entry in this table represents a
            set of signalling capabilities that can
            be applied to a VCL.  There is no requirement
            for unique entries, except that the index must
            be unique."
        INDEX { atmSigDescrParamIndex }
        ::= { atmSigDescrParamTable 1 }

    AtmSigDescrParamEntry ::=
        SEQUENCE {
            atmSigDescrParamIndex
                                   AtmSigDescrParamIndex,
            atmSigDescrParamAalType         INTEGER,
            atmSigDescrParamAalSscsType     INTEGER,
            atmSigDescrParamBhliType        INTEGER,


            atmSigDescrParamBhliInfo        OCTET STRING,
            atmSigDescrParamBbcConnConf     INTEGER,
            atmSigDescrParamBlliLayer2      INTEGER,
            atmSigDescrParamBlliLayer3      INTEGER,
            atmSigDescrParamBlliPktSize     INTEGER,
            atmSigDescrParamBlliSnapId      INTEGER,
            atmSigDescrParamBlliOuiPid      OCTET STRING,
            atmSigDescrParamRowStatus       RowStatus
        }

    atmSigDescrParamIndex OBJECT-TYPE
        SYNTAX       AtmSigDescrParamIndex
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "The value of this object is used by the
            atmVclGenSigDescrIndex object in the atmVclGenTable to
            identify a row in this table."

        ::= { atmSigDescrParamEntry 1 }

     atmSigDescrParamAalType OBJECT-TYPE
         SYNTAX       INTEGER {
            other(1),       -- not defined
            aal1(2),        -- AAL type 1
            aal34(3),       -- AAL type 3/4
            aal5(4),        -- AAL type 5





            userDefined(5), -- User-Defined AAL
            aal2(6)         -- AAL type 2
            }
         MAX-ACCESS   read-create
         STATUS       current
         DESCRIPTION
            "The AAL type.  The value of this object is set to other(1)
            when not defined."

         DEFVAL { other }
         ::= { atmSigDescrParamEntry 2 }

     atmSigDescrParamAalSscsType OBJECT-TYPE
         SYNTAX       INTEGER {
            other(1),       -- other, or not used
            assured(2),     -- Data SSCS based on SSCOP
                            -- assured operation
            nonassured(3),  -- Data SSCS based on SSCOP
                            -- non-assured operation
            frameRelay(4),  -- frame relay SSCS
            null(5)         -- null

            }
         MAX-ACCESS   read-create
         STATUS       current
         DESCRIPTION
            "The SSCS type used by this entry."

         DEFVAL { other }
         ::= { atmSigDescrParamEntry 3 }

     atmSigDescrParamBhliType OBJECT-TYPE
         SYNTAX       INTEGER {
            other(1),         -- not defined
            iso(2),           -- ISO
            user(3),          -- User specific
            hiProfile(4),     -- Higher layer profile
                              -- this enum applicable to
                              -- UNI 3.0 only
            vendorSpecific(5) -- Vender specific
                              -- application identifier
            }
         MAX-ACCESS   read-create
         STATUS       current
         DESCRIPTION
            "The Broadband high layer type."

         DEFVAL { other }





         ::= { atmSigDescrParamEntry 4 }

     atmSigDescrParamBhliInfo OBJECT-TYPE
         SYNTAX     OCTET STRING (SIZE(0..8))
         MAX-ACCESS read-create
         STATUS     current
         DESCRIPTION
            "The Broadband high layer information.  When
            atmSigDescrParamBhliType is set to iso(2), the value of this
            object is a zero length string.  When
            atmSigDescrParamBhliType is set to user(3), the value of
            this object is an octet string with length ranging from 0 to
            8.  When atmSigDescrParamBhliType is set to hiProfile(4),
            the value of this object is a length of 4 octet string
            containing user to user profile identifier.  When
            atmSigDescrParamBhliType is set to vendorSpecific(5), the
            value of this object is a length of 7 octet string, where
            the most significant 3 octets consist of a globally-
            administered OUI, and the least significant 4 octets are the
            vender administered application OUI."

         DEFVAL { ''H }

         ::= { atmSigDescrParamEntry 5 }

     atmSigDescrParamBbcConnConf OBJECT-TYPE
         SYNTAX       INTEGER {
             ptp(1),   -- point-to-point
             ptmp(2)   -- point-to-multipoint
             }
         MAX-ACCESS   read-create
         STATUS       current
         DESCRIPTION
             "The Broadband bearer capability user plane connection
              configuration parameter."
         DEFVAL { ptp }
         ::= { atmSigDescrParamEntry 6 }

      atmSigDescrParamBlliLayer2 OBJECT-TYPE
          SYNTAX       INTEGER {
             other(1),        -- not specified
             iso1745(2),      -- Basic mode ISO 1745
             q921(3),         -- CCITT Recommendation Q.921
             x25linklayer(4), -- CCITT Recommendation X.25
                              -- Link Layer
             x25multilink(5), -- CCITT Recommendation X.25
                              -- Multilink
             lapb(6),         -- Extended LAPB; for half





                              -- duplex operation
             hdlcArm(7),      -- HDLC ARM (ISO 4335)
             hdlcNrm(8),      -- HDLC NRM (ISO 4335)
             hdlcAbm(9),      -- HDLC ABM (ISO 4335)
             iso88022(10),    -- LAN logical link control
                              -- (ISO 8802/2)
             x75slp(11),      -- CCITT Recommendation X.75,
                              -- single link
                              -- procedure (SLP)
             q922(12),        -- CCITT Recommendation Q.922
             userDef(13),     -- User specified
             iso7776(14)      -- ISO 7776 DTE-DTE operation
             }
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
            "The Broadband low layer information, protocol type of layer
            2.  The value of this object is other(1) if layer 2 protocol
            is not used."

          DEFVAL { other }
          ::= { atmSigDescrParamEntry 7 }

      atmSigDescrParamBlliLayer3 OBJECT-TYPE
          SYNTAX       INTEGER {
             other(1),       -- not specified
             x25pkt(2),      -- CCITT Recommendation X.25
                             -- packet layer
             isoiec8208(3),  -- ISO/IEC 8208 (X.25 packet
                             -- level protocol for data
                             -- terminal equipment)
             x223iso8878(4), -- X.223/ISO 8878
             isoiec8473(5),  -- ISO/IEC 8473 OSI
                             -- connectionless
                             -- mode protocol
             t70(6),         -- CCITT Recommendation T.70
                             -- minimum
                             -- network layer
             tr9577(7),      -- ISO/IEC TR 9577 Protocol
                             -- Identification in the
                             -- network layer
             userDef(8)      -- user specified

             }
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
            "The Broadband low layer information, protocol type of layer





            3.  The value of this object is other(1) if layer 3 protocol
            is not used."

          DEFVAL { other }
          ::= { atmSigDescrParamEntry 8 }

      atmSigDescrParamBlliPktSize OBJECT-TYPE
          SYNTAX       INTEGER {
             other(1),        -- not used
             s16(2),          -- 16 octets
             s32(3),          -- 32 octets
             s64(4),          -- 64 octets
             s128(5),         -- 128 octets
             s256(6),         -- 256 octets
             s512(7),         -- 512 octets
             s1024(8),        -- 1028 octets
             s2048(9),        -- 2048 octets
             s4096(10)        -- 4096 octets
          }
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
            "The default packet size defined in B-LLI."

          DEFVAL { other }
          ::= { atmSigDescrParamEntry 9 }

      atmSigDescrParamBlliSnapId OBJECT-TYPE
          SYNTAX       INTEGER {
             other(1),  -- not used
             true(2),   -- SNAP ID is 1
             false(3)   -- SNAP ID is 0
          }
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION
            "The SNAP ID used for Broadband low layer protocol layer 3.
            The value of this object is other(1) if
            atmSigDescrParamBlliLayer3 is set to other(1)."

          DEFVAL { other }
          ::= { atmSigDescrParamEntry 10 }

      atmSigDescrParamBlliOuiPid OBJECT-TYPE
          SYNTAX       OCTET STRING (SIZE(0|5))
          MAX-ACCESS   read-create
          STATUS       current
          DESCRIPTION





            "The OUI/PID encoding for Broadband low layer protocol layer
            3.  The value of this object is a zero length string if
            atmSigDescrParamBlliLayer3 is set to other(1).  When used,
            it is always 5 octets with the most significant octet as the
            OUI Octet 1 and the least significant octet as the PID Octet
            2."

          DEFVAL { ''H }
          ::= { atmSigDescrParamEntry 11 }

       atmSigDescrParamRowStatus OBJECT-TYPE
           SYNTAX       RowStatus
           MAX-ACCESS   read-create
           STATUS       current
           DESCRIPTION
            "This object is used to create and delete rows in the
            atmSigDescrParamTable."

           ::= { atmSigDescrParamEntry 12 }

  -- 6. ATM Interface Registered Address Table --

atmIfRegisteredAddrTable    OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmIfRegisteredAddrEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This table contains a list of ATM addresses that can be used for
       calls to and from a given interface by a switch or service.  The
       ATM addresses are either registered by the endsystem via ILMI or
       statically configured.  This table does not expose PNNI
       reachability information.  ILMI registered addresses cannot be
       deleted using this table.  This table only applies to switches
       and network services."
    ::= { atm2MIBObjects 6 }

atmIfRegisteredAddrEntry    OBJECT-TYPE
    SYNTAX       AtmIfRegisteredAddrEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "An entry in the ATM Interface Registered Address table."

    INDEX { ifIndex, atmIfRegAddrAddress }
    ::= { atmIfRegisteredAddrTable  1}

AtmIfRegisteredAddrEntry    ::= SEQUENCE  {
    atmIfRegAddrAddress             AtmAddr,





    atmIfRegAddrAddressSource       INTEGER,
    atmIfRegAddrOrgScope            INTEGER,
    atmIfRegAddrRowStatus           RowStatus
         }

atmIfRegAddrAddress   OBJECT-TYPE
    SYNTAX       AtmAddr
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "An address registered for a given switch or service interface."

    ::= { atmIfRegisteredAddrEntry 1}

atmIfRegAddrAddressSource  OBJECT-TYPE
    SYNTAX       INTEGER  {
       other(1),
       static(2),
       dynamic(3)
       }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The type of address source for a given ATM Address. The value
       dynamic(3) is indicated when ILMI is used."
    ::= { atmIfRegisteredAddrEntry 2}

atmIfRegAddrOrgScope  OBJECT-TYPE
    SYNTAX       INTEGER {
        localNetwork(1),
        localNetworkPlusOne(2),
        localNetworkPlusTwo(3),
        siteMinusOne(4),
        intraSite(5),
        sitePlusOne(6),
        organizationMinusOne(7),
        intraOrganization(8),
        organizationPlusOne(9),
        communityMinusOne(10),
        intraCommunity(11),
        communityPlusOne(12),
        regional(13),
        interRegional(14),
        global(15)
    }
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION





        "This object indicates the organizational scope for
        the referenced address.  The information of the
        referenced address shall not be distributed outside
        the indicated scope.   Refer to Annex 5.3 of ATM
        Forum UNI Signalling 4.0 for guidelines regarding
        the use of organizational scopes.

        This value cannot be configured for ILMI-registered
        addresses.

        The default values for organizational scope are
        localNetwork(1) for ATM group addresses, and
        global(15) for individual addresses."
    ::= { atmIfRegisteredAddrEntry 3}

atmIfRegAddrRowStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
       "This object is used to create and delete rows in the
       atmIfRegisteredAddrTable.  Rows created dynamically (e.g., ILMI-
       registered addresses) cannot be deleted using this object."

    ::= { atmIfRegisteredAddrEntry 4}

  -- 7. ATM VPI/VCI to Address Mapping Table

    atmVclAddrTable  OBJECT-TYPE
        SYNTAX       SEQUENCE OF AtmVclAddrEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "This table provides a mapping between the atmVclTable and
            the ATM called party/calling party address.  This table can
            be used to retrieve the calling party and called party ATM
            address pair for a given VCL.  Note that there can be more
            than one pair of calling party and called party ATM
            addresses for a VCL in a point to multi-point call."
        ::= { atm2MIBObjects 7 }

    atmVclAddrEntry    OBJECT-TYPE
        SYNTAX       AtmVclAddrEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Each entry in this table represents a binding between a VCL
            and an ATM address associated with this call.  This ATM





            address can be either the called party address or the
            calling party address.  There can be more than one pair of
            calling/called party ATM addresses associated with the VCL
            entry for point to multi-point calls.  Objects
            atmVclAddrType, and atmVclAddrRowStatus are
            required during row creation."
        INDEX  { ifIndex, atmVclVpi, atmVclVci,
                 atmVclAddrAddr }
        ::= { atmVclAddrTable 1 }

    AtmVclAddrEntry ::=
        SEQUENCE {
            atmVclAddrAddr          AtmAddr,
            atmVclAddrType          INTEGER,
            atmVclAddrRowStatus     RowStatus
        }

    atmVclAddrAddr     OBJECT-TYPE
        SYNTAX       AtmAddr
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "An ATM address on one end of the VCL.  For SVCs, the agent
            supplies the value of this object at creation time.  For PVC
            VCL, the manager can supply the value of this object during
            or after the PVC VCL creation."
        ::= { atmVclAddrEntry 1 }

   atmVclAddrType     OBJECT-TYPE
       SYNTAX       INTEGER {
           callingParty(1),
           calledParty(2)
       }
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
            "The type of ATM Address represented by the object
            atmVclAddrAddr.  Choices are either the calling party ATM
            address or the called party ATM address."
       ::= { atmVclAddrEntry 2 }

   atmVclAddrRowStatus     OBJECT-TYPE
       SYNTAX       RowStatus
       MAX-ACCESS   read-create
       STATUS       current
       DESCRIPTION
           "This object is used to create or destroy an
           entry from this table.  Note that the manager entity





           can only destroy the PVC VCLs."
       ::= { atmVclAddrEntry 3 }

  -- 8. ATM Address to VPI/VCI Mapping Table
  --
  -- This table provides an alternative way to access
  -- a row in the atmVclAddrTable by using
  -- an ATM address as an index, instead of
  -- the ifIndex

    atmAddrVclTable   OBJECT-TYPE
        SYNTAX       SEQUENCE OF AtmAddrVclEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "This table provides an alternative way to retrieve the
            atmVclTable.  This table can be used to retrieve the
            indexing to the atmVclTable by an ATM address."

        ::= { atm2MIBObjects 8 }

    atmAddrVclEntry    OBJECT-TYPE
        SYNTAX       AtmAddrVclEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Each entry in this table represents an entry in the
            atmVclTable of the ATM-MIB by its ATM address.  The ATM
            address is either the calling or called party ATM address
            of the call.  Entries in this table are read only.
            They show up when entries are created in the
            atmVclAddrTable."
        REFERENCE
            "Tesink, K., Editor, Definitions of Managed Objects
             for ATM Management, RFC 2515, Bell Communications
             Research, February, 1999."
        INDEX { atmVclAddrAddr, atmAddrVclAtmIfIndex,
                atmAddrVclVpi, atmAddrVclVci }
        ::= { atmAddrVclTable 1 }

    AtmAddrVclEntry ::=
        SEQUENCE {
            atmAddrVclAtmIfIndex    InterfaceIndex,
            atmAddrVclVpi           AtmVpIdentifier,
            atmAddrVclVci           AtmVcIdentifier,
            atmAddrVclAddrType      INTEGER
            }






    atmAddrVclAtmIfIndex     OBJECT-TYPE
        SYNTAX       InterfaceIndex
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "The interface index of the ATM interface to which this
             VCL pertains.  This object combined with the
             atmAddrVclVpi and atmAddrVclVci objects serves as an
             index to the atmVclTable."
        ::= { atmAddrVclEntry 1 }

    atmAddrVclVpi     OBJECT-TYPE
        SYNTAX       AtmVpIdentifier
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "The VPI value of the VCL.  This object combined with the
            atmAddrVclAtmIfIndex and atmAddrVclVci objects serves as
            an index to the atmVclTable."
        ::= { atmAddrVclEntry 2 }

    atmAddrVclVci     OBJECT-TYPE
        SYNTAX       AtmVcIdentifier
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "The VCI value of the VCL.  This object combined with the
            atmAddrVclAtmIfIndex and atmAddrVclVpi objects serves as
            an index to the atmVclTable."
        ::= { atmAddrVclEntry 3 }

   atmAddrVclAddrType     OBJECT-TYPE
       SYNTAX       INTEGER {
           callingParty(1),
           calledParty(2) }
       MAX-ACCESS   read-only
       STATUS       current
       DESCRIPTION
            "The type of ATM Address represented by the object
            atmVclAddrAddr.  Choices are either calling party address
            or called party address."
       ::= { atmAddrVclEntry 4 }

  -- 9. ATM VPL Statistics Table

    atmVplStatTable   OBJECT-TYPE
        SYNTAX       SEQUENCE OF AtmVplStatEntry
        MAX-ACCESS   not-accessible





        STATUS       current
        DESCRIPTION
            "This table contains all statistics counters per VPL.  It is
            used to monitor the usage of the VPL in terms of incoming
            cells and outgoing cells."
        ::= { atm2MIBObjects 9 }

    atmVplStatEntry    OBJECT-TYPE
        SYNTAX       AtmVplStatEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Each entry in this table represents a VPL."
        INDEX { ifIndex, atmVplVpi }
        ::= { atmVplStatTable 1 }

    AtmVplStatEntry ::=
        SEQUENCE {
            atmVplStatTotalCellIns      Counter32,
            atmVplStatClp0CellIns       Counter32,
            atmVplStatTotalDiscards     Counter32,
            atmVplStatClp0Discards      Counter32,
            atmVplStatTotalCellOuts     Counter32,
            atmVplStatClp0CellOuts      Counter32,
            atmVplStatClp0Tagged        Counter32
    }

    atmVplStatTotalCellIns OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells received by this VPL
            including both CLP=0 and CLP=1 cells.  The cells are
            counted prior to the application of the traffic policing."
        ::= { atmVplStatEntry 1 }

    atmVplStatClp0CellIns OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The number of valid ATM cells received by this VPL with
            CLP=0.  The cells are counted prior to the application of
            the traffic policing."
        ::= { atmVplStatEntry 2 }

    atmVplStatTotalDiscards OBJECT-TYPE





        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells discarded by the
            traffic policing entity.  This includes cells originally
            received with CLP=0 and CLP=1."
        ::= { atmVplStatEntry 3 }

    atmVplStatClp0Discards OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells received with CLP=0 and
            discarded by the traffic policing entity."
        ::= { atmVplStatEntry 4 }

    atmVplStatTotalCellOuts OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells transmitted  by this
            VPL.  This includes both CLP=0 and CLP=1 cells."
        ::= { atmVplStatEntry 5 }

    atmVplStatClp0CellOuts OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells transmitted with CLP=0
            by this VPL."
        ::= { atmVplStatEntry 6 }

    atmVplStatClp0Tagged OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells tagged by the traffic
            policing entity from CLP=0 to CLP=1."
        ::= { atmVplStatEntry 7 }

  -- 10. ATM Logical Port Configuration Table

    atmVplLogicalPortTable OBJECT-TYPE





        SYNTAX       SEQUENCE OF AtmVplLogicalPortEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Indicates whether the VPL is an ATM Logical Port interface
            (ifType=80)."
        ::= { atm2MIBObjects 10 }

    atmVplLogicalPortEntry OBJECT-TYPE
        SYNTAX       AtmVplLogicalPortEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "An entry with information about the ATM Logical Port
            interface."
        AUGMENTS { atmVplEntry }
        ::= { atmVplLogicalPortTable 1 }

    AtmVplLogicalPortEntry ::=
        SEQUENCE {
            atmVplLogicalPortDef        INTEGER,
            atmVplLogicalPortIndex      InterfaceIndexOrZero
            }

    atmVplLogicalPortDef   OBJECT-TYPE
        SYNTAX       INTEGER {
                        notLogicalIf(1),
                        isLogicalIf(2)
                        }
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "Indicates whether the VPC at this VPL interface is an ATM
            Logical Port interface."
        DEFVAL { notLogicalIf }
        ::= { atmVplLogicalPortEntry 1 }

    atmVplLogicalPortIndex OBJECT-TYPE
        SYNTAX       InterfaceIndexOrZero
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The ifTable index of the ATM logical port interface
            associated with this VPL. The distinguished value of zero
            indicates that the agent has not (yet) assigned such an
            ifTable Index. The zero value must be assigned by the agent
            if the value of atmVplLogicalPortDef is set to notLogicalIf,
            or if the VPL row is not active."





        ::= { atmVplLogicalPortEntry 2 }

  -- 11. ATM VCL Statistics Table

    atmVclStatTable   OBJECT-TYPE
        SYNTAX       SEQUENCE OF AtmVclStatEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "This table contains all statistics counters per VCL.  It is
            used to monitor the usage of the VCL in terms of incoming
            cells and outgoing cells."
        ::= { atm2MIBObjects 11 }

    atmVclStatEntry    OBJECT-TYPE
        SYNTAX       AtmVclStatEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Each entry in this table represents a VCL."
        INDEX { ifIndex, atmVclVpi, atmVclVci }
        ::= { atmVclStatTable 1 }

    AtmVclStatEntry ::=
        SEQUENCE {
            atmVclStatTotalCellIns      Counter32,
            atmVclStatClp0CellIns       Counter32,
            atmVclStatTotalDiscards     Counter32,
            atmVclStatClp0Discards      Counter32,
            atmVclStatTotalCellOuts     Counter32,
            atmVclStatClp0CellOuts      Counter32,
            atmVclStatClp0Tagged        Counter32
        }

    atmVclStatTotalCellIns OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells received by this VCL
            including both CLP=0 and CLP=1 cells.  The cells are counted
            prior to the application of the traffic policing."
        ::= { atmVclStatEntry 1 }

    atmVclStatClp0CellIns OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current





        DESCRIPTION
            "The number of valid ATM cells received by this VCL with
            CLP=0.  The cells are counted prior to the application of
            the traffic policing."
        ::= { atmVclStatEntry 2 }

    atmVclStatTotalDiscards OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells discarded by the
            traffic policing entity.  This includes cells originally
            received with CLP=0 and CLP=1."
        ::= { atmVclStatEntry 3 }

    atmVclStatClp0Discards OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells received with CLP=0
             and discarded by the traffic policing entity."
        ::= { atmVclStatEntry 4 }

    atmVclStatTotalCellOuts OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells transmitted  by this
            VCL.  This includes both CLP=0 and CLP=1 cells."
        ::= { atmVclStatEntry 5 }

    atmVclStatClp0CellOuts OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The total number of valid ATM cells transmitted with CLP=0
            by this VCL."
        ::= { atmVclStatEntry 6 }

    atmVclStatClp0Tagged OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION





            "The total number of valid ATM cells tagged by the traffic
            policing entity from CLP=0 to CLP=1."
        ::= { atmVclStatEntry 7 }

  -- 12. ATM AAL5 per-VCC Statistics Table

    atmAal5VclStatTable   OBJECT-TYPE
        SYNTAX       SEQUENCE OF AtmAal5VclStatEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "This table provides a collection of objects providing AAL5
            configuration and performance statistics of a VCL."
        ::= { atm2MIBObjects 12 }

    atmAal5VclStatEntry    OBJECT-TYPE
        SYNTAX       AtmAal5VclStatEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "Each entry in this table represents an AAL5 VCL, and
             is indexed by ifIndex values of AAL5 interfaces and
             the associated VPI/VCI values."
        INDEX { ifIndex, atmVclVpi, atmVclVci }
        ::= { atmAal5VclStatTable 1 }

    AtmAal5VclStatEntry ::=
        SEQUENCE {
           atmAal5VclInPkts        Counter32,
           atmAal5VclOutPkts       Counter32,
           atmAal5VclInOctets      Counter32,
           atmAal5VclOutOctets     Counter32
        }

    atmAal5VclInPkts      OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The number of AAL5 CPCS PDUs received on the AAL5 VCC at
            the interface identified by the ifIndex."
        ::= { atmAal5VclStatEntry 1 }

    atmAal5VclOutPkts   OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION





            "The number of AAL5 CPCS PDUs transmitted on the AAL5 VCC
             at the interface identified by the ifIndex."
        ::= { atmAal5VclStatEntry 2 }

    atmAal5VclInOctets   OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The number of octets contained in AAL5 CPCS PDUs received
            on the AAL5 VCC at the interface identified by the ifIndex."
        ::= { atmAal5VclStatEntry 3 }

    atmAal5VclOutOctets   OBJECT-TYPE
        SYNTAX       Counter32
        MAX-ACCESS   read-only
        STATUS       current
        DESCRIPTION
            "The number of octets contained in AAL5 CPCS PDUs
            transmitted on the AAL5 VCC at the interface identified by
            the ifIndex."
        ::= { atmAal5VclStatEntry 4 }

  -- 13. ATM VC General Information Table

    atmVclGenTable OBJECT-TYPE
        SYNTAX       SEQUENCE OF AtmVclGenEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "General Information for each VC."
        ::= { atm2MIBObjects 13 }

    atmVclGenEntry OBJECT-TYPE
        SYNTAX       AtmVclGenEntry
        MAX-ACCESS   not-accessible
        STATUS       current
        DESCRIPTION
            "An entry with general information about the ATM VC."

        AUGMENTS { atmVclEntry }
        ::= { atmVclGenTable 1 }

    AtmVclGenEntry ::=
        SEQUENCE {
          atmVclGenSigDescrIndex      AtmSigDescrParamIndex
        }






    atmVclGenSigDescrIndex   OBJECT-TYPE
        SYNTAX       AtmSigDescrParamIndex
        MAX-ACCESS   read-create
        STATUS       current
        DESCRIPTION
            "The value of this object identifies the row in the ATM
            Signalling Descriptor Parameter Table which applies to this
            VCL."
        ::= { atmVclGenEntry 1 }

  -- 14. ATM Interface Configuration Extension Table

atmInterfaceExtTable    OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmInterfaceExtEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This table contains ATM interface configuration and monitoring
       information not defined in the atmInterfaceConfTable from the
       ATM-MIB.  This includes the type of connection setup procedures,
       ILMI information, and information on the VPI/VCI range."
    REFERENCE
        "Tesink, K., Editor, Definitions of Managed Objects
         for ATM Management, RFC 2515, Bell Communications
         Research, February, 1999."
    ::= { atm2MIBObjects 14 }

atmInterfaceExtEntry    OBJECT-TYPE
    SYNTAX       AtmInterfaceExtEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "An entry extends the atmInterfaceConfEntry defined in the ATM-
       MIB.  Each entry corresponds to an ATM interface."
    REFERENCE
        "Tesink, K., Editor, Definitions of Managed Objects
         for ATM Management, RFC 2515, Bell Communications
         Research, February, 1999."
    AUGMENTS { atmInterfaceConfEntry }
    ::= { atmInterfaceExtTable 1 }

AtmInterfaceExtEntry    ::= SEQUENCE  {
        atmIntfConfigType                   AtmInterfaceType,
        atmIntfActualType                   AtmInterfaceType,
        atmIntfConfigSide                   INTEGER,
        atmIntfActualSide                   INTEGER,
        atmIntfIlmiAdminStatus              BITS,
        atmIntfIlmiOperStatus               BITS,





        atmIntfIlmiFsmState                 INTEGER,
        atmIntfIlmiEstablishConPollIntvl    Integer32,
        atmIntfIlmiCheckConPollIntvl        Integer32,
        atmIntfIlmiConPollInactFactor       Integer32,
        atmIntfIlmiPublicPrivateIndctr      INTEGER,
        atmInterfaceConfMaxSvpcVpi          INTEGER,
        atmInterfaceCurrentMaxSvpcVpi       INTEGER,
        atmInterfaceConfMaxSvccVpi          INTEGER,
        atmInterfaceCurrentMaxSvccVpi       INTEGER,
        atmInterfaceConfMinSvccVci          INTEGER,
        atmInterfaceCurrentMinSvccVci       INTEGER,
        atmIntfSigVccRxTrafficDescrIndex
                                   AtmTrafficDescrParamIndex,
        atmIntfSigVccTxTrafficDescrIndex
                                   AtmTrafficDescrParamIndex,
        atmIntfPvcFailures                  Counter32,
        atmIntfCurrentlyFailingPVpls        Gauge32,
        atmIntfCurrentlyFailingPVcls        Gauge32,
        atmIntfPvcFailuresTrapEnable        TruthValue,
        atmIntfPvcNotificationInterval      INTEGER,
        atmIntfLeafSetupFailures            Counter32,
        atmIntfLeafSetupRequests            Counter32 }

atmIntfConfigType     OBJECT-TYPE
    SYNTAX       AtmInterfaceType
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The type of connection setup procedures configured for the ATM
       interface.  Setting this variable to a value of 'other' is not
       allowed."
    DEFVAL { autoConfig }
    ::= { atmInterfaceExtEntry 1 }

atmIntfActualType     OBJECT-TYPE
    SYNTAX       AtmInterfaceType
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The type of connection setup procedures currently being used on
       the interface.  This may reflect a manually configured value for
       the interface type, or may be determined by other means such as
       auto-configuration.  A value of `autoConfig' indicates that
       auto-configuration was requested but has not yet been completed."
    ::= { atmInterfaceExtEntry 2 }

atmIntfConfigSide     OBJECT-TYPE
    SYNTAX       INTEGER  {





                     other(1),
                     user(2),
                     network(3) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The configured role of the managed entity as one side of the ATM
       interface.  This value does not apply when the object
       atmIntfConfigType is set to `autoConfig', `atmfPnni1Dot0', or
       `atmfBici2Dot0'."
    ::= { atmInterfaceExtEntry 3 }

atmIntfActualSide     OBJECT-TYPE
    SYNTAX       INTEGER  {
                     other(1),
                     user(2),
                     network(3),
                     symmetric(4) }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The current role used by the managed entity to represent one
       side of the ATM interface."
    ::= { atmInterfaceExtEntry 4 }

atmIntfIlmiAdminStatus    OBJECT-TYPE
    SYNTAX       BITS { ilmi(0),
                        ilmiAddressRegistration(1),
                        ilmiConnectivity(2),
                        ilmiPvcPvpMgmt(3),
                        ilmiSigVccParamNegotiation(4) }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "Indicates which components of ILMI are administratively enabled
       on this interface.  If the 'ilmi' bit is not set, then no ILMI
       components are operational.  ILMI components other than auto-
       configuration that are not represented in the value have their
       administrative status determined according to the 'ilmi' bit.
       The ILMI auto-configuration component is enabled/disabled by the
       atmIntfConfigType object."
    ::= { atmInterfaceExtEntry 5 }

atmIntfIlmiOperStatus    OBJECT-TYPE
    SYNTAX       BITS { ilmi(0),
                        ilmiAddressRegistration(1),
                        ilmiConnectivity(2),
                        ilmiPvcPvpMgmt(3),





                        ilmiSigVccParamNegotiation(4) }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Indicates which components of ILMI are operational on this
       interface."
    ::= { atmInterfaceExtEntry 6 }

atmIntfIlmiFsmState    OBJECT-TYPE
    SYNTAX       INTEGER { stopped(1),
                           linkFailing(2),
                           establishing(3),
                           configuring(4),
                           retrievingNetworkPrefixes(5),
                           registeringNetworkPrefixes(6),
                           retrievingAddresses(7),
                           registeringAddresses(8),
                           verifying(9) }
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Indicates the state of the ILMI Finite State Machine associated
       with this interface."

        REFERENCE
            "ATM Forum, Integrated Local Management Interface
             (ILMI) Specification, Version 4.0, af-ilmi-0065.000,
             September 1996, Appendix 1"
    ::= { atmInterfaceExtEntry 7 }

atmIntfIlmiEstablishConPollIntvl    OBJECT-TYPE
    SYNTAX       Integer32 (1..65535)
    UNITS        "seconds"
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The amount of time S between successive transmissions of ILMI
       messages on this interface for the purpose of detecting
       establishment of ILMI connectivity."
    REFERENCE
       "ATM Forum, Integrated Local Management Interface
        (ILMI) Specification, Version 4.0, af-ilmi-0065.000,
        September 1996, Section 8.3.1"
    DEFVAL { 1 }
    ::= { atmInterfaceExtEntry 8 }

atmIntfIlmiCheckConPollIntvl    OBJECT-TYPE
    SYNTAX       Integer32 (0..65535)





    UNITS        "seconds"
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The amount of time T between successive transmissions of ILMI
       messages on this interface for the purpose of detecting loss of
       ILMI connectivity.  The distinguished value zero disables ILMI
       connectivity procedures on this interface."
    REFERENCE
       "ATM Forum, Integrated Local Management Interface
        (ILMI) Specification, Version 4.0, af-ilmi-0065.000,
        September 1996, Section 8.3.1"
    DEFVAL { 5 }
    ::= { atmInterfaceExtEntry 9 }

atmIntfIlmiConPollInactFactor    OBJECT-TYPE
    SYNTAX       Integer32 (0..65535)
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The number K of consecutive polls on this interface for which no
       ILMI response message is received before ILMI connectivity is
       declared lost."
    REFERENCE
       "ATM Forum, Integrated Local Management Interface
        (ILMI) Specification, Version 4.0, af-ilmi-0065.000,
        September 1996, Section 8.3.1"
    DEFVAL { 4 }
    ::= { atmInterfaceExtEntry 10 }

atmIntfIlmiPublicPrivateIndctr    OBJECT-TYPE
    SYNTAX       INTEGER {
                           other(1),
                           public(2),
                           private(3)
                           }
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "Specifies whether this end of the interface is advertised in
       ILMI as a device of the `public' or `private' type."
    DEFVAL { private }
    ::= { atmInterfaceExtEntry 11 }

atmInterfaceConfMaxSvpcVpi    OBJECT-TYPE
    SYNTAX       INTEGER  (0..4095)
    MAX-ACCESS   read-write
    STATUS       current





    DESCRIPTION
       "The maximum VPI that the signalling stack on the ATM interface
       is configured to support for allocation to switched virtual path
       connections."
    ::= { atmInterfaceExtEntry 12 }

atmInterfaceCurrentMaxSvpcVpi    OBJECT-TYPE
    SYNTAX       INTEGER  (0..4095)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The maximum VPI that the signalling stack on the ATM interface
       may currently allocate to switched virtual path connections.
       This value is the minimum of atmInterfaceConfMaxSvpcVpi, and the
       atmInterfaceMaxSvpcVpi of the interface's UNI/NNI peer.

       If the interface does not negotiate with its peer to determine
       the maximum VPI that can be allocated to SVPCs on the interface,
       then the value of this object must equal
       atmInterfaceConfMaxSvpcVpi. "
    ::= { atmInterfaceExtEntry 13 }

atmInterfaceConfMaxSvccVpi    OBJECT-TYPE
    SYNTAX       INTEGER  (0..4095)
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The maximum VPI that the signalling stack on the ATM interface
       is configured to support for allocation to switched virtual
       channel connections."
    ::= { atmInterfaceExtEntry 14 }

atmInterfaceCurrentMaxSvccVpi    OBJECT-TYPE
    SYNTAX       INTEGER  (0..4095)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The maximum VPI that the signalling stack on the ATM interface
       may currently allocate to switched virtual channel connections.
       This value is the minimum of atmInterfaceConfMaxSvccVpi, and the
       atmInterfaceConfMaxSvccVpi of the interface's UNI/NNI peer.

       If the interface does not negotiate with its peer to determine
       the maximum VPI that can be allocated to SVCCs on the interface,
       then the value of this object must equal
       atmInterfaceConfMaxSvccVpi."
    ::= { atmInterfaceExtEntry 15 }






atmInterfaceConfMinSvccVci    OBJECT-TYPE
    SYNTAX       INTEGER  (0..65535)
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The minimum VCI that the signalling stack on the ATM interface
       is configured to support for allocation to switched virtual
       channel connections."
    ::= { atmInterfaceExtEntry 16 }

atmInterfaceCurrentMinSvccVci    OBJECT-TYPE
    SYNTAX       INTEGER  (0..65535)
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The minimum VCI that the signalling stack on the ATM interface
       may currently allocate to switched virtual channel connections.
       This value is the maximum of atmInterfaceConfMinSvccVci, and the
       atmInterfaceConfMinSvccVci of the interface's UNI/NNI peer.
       If the interface does not negotiate with its peer to determine
       the minimum VCI that can be allocated to SVCCs on the interface,
       then the value of this object must equal
       atmInterfaceConfMinSvccVci."
    ::= { atmInterfaceExtEntry 17 }

atmIntfSigVccRxTrafficDescrIndex    OBJECT-TYPE
    SYNTAX       AtmTrafficDescrParamIndex
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "This object identifies the row in the atmTrafficDescrParamTable
       used during ILMI auto-configuration to specify the advertised
       signalling VCC traffic parameters for the receive direction.
       The traffic descriptor resulting from ILMI auto-configuration of
       the signalling VCC is indicated in the atmVclTable."
    ::= { atmInterfaceExtEntry 18 }

atmIntfSigVccTxTrafficDescrIndex    OBJECT-TYPE
    SYNTAX       AtmTrafficDescrParamIndex
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "This object identifies the row in the atmTrafficDescrParamTable
       used during ILMI auto-configuration to specify the advertised
       signalling VCC traffic parameters for the transmit direction.
       The traffic descriptor resulting from ILMI auto-configuration of
       the signalling VCC is indicated in the atmVclTable."
    ::= { atmInterfaceExtEntry 19 }





atmIntfPvcFailures    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The number of times the operational status of a PVPL or PVCL on
       this interface has gone down."
    ::= { atmInterfaceExtEntry 20 }

atmIntfCurrentlyFailingPVpls    OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The current number of VPLs on this interface for which there is
       an active row in the atmVplTable having an atmVplConnKind value
       of `pvc' and an atmVplOperStatus with a value other than `up'."
    ::= { atmInterfaceExtEntry 21 }

atmIntfCurrentlyFailingPVcls    OBJECT-TYPE
    SYNTAX       Gauge32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The current number of VCLs on this interface for which there is
       an active row in the atmVclTable having an atmVclConnKind value
       of `pvc' and an atmVclOperStatus with a value other than `up'."
    ::= { atmInterfaceExtEntry 22 }

atmIntfPvcFailuresTrapEnable    OBJECT-TYPE
    SYNTAX       TruthValue
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "Allows the generation of traps in response to PVCL or PVPL
       failures on this interface."
    DEFVAL { false }
    ::= { atmInterfaceExtEntry 23 }

atmIntfPvcNotificationInterval    OBJECT-TYPE
    SYNTAX       INTEGER (1..3600)
    UNITS        "seconds"
    MAX-ACCESS   read-write
    STATUS       current
    DESCRIPTION
       "The minimum interval between the sending of
       atmIntfPvcFailuresTrap notifications for this interface."
    DEFVAL { 30 }





    ::= { atmInterfaceExtEntry 24 }

atmIntfLeafSetupFailures    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of setup failures.  For root, this is the number of
       rejected setup requests and for leaf, this is the number of setup
       failure received."
    ::= { atmInterfaceExtEntry 25 }

atmIntfLeafSetupRequests    OBJECT-TYPE
    SYNTAX       Counter32
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "Number of setup requests.  For root, this includes both incoming
       setup request and root intiated setup requests."
    ::= { atmInterfaceExtEntry 26 }

  -- 15. ATM ILMI Service Registry Table

atmIlmiSrvcRegTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmIlmiSrvcRegEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This table contains a list of all the ATM network services known
       by this device.

       The characteristics of these services are made available through
       the ILMI, using the ILMI general-purpose service registry MIB.
       These services may be made available to all ATM interfaces
       (atmIlmiSrvcRegIndex = 0) or to some specific ATM interfaces only
       (atmIlmiSrvcRegIndex = ATM interface index)."
    ::= { atm2MIBObjects 15 }

atmIlmiSrvcRegEntry OBJECT-TYPE
    SYNTAX       AtmIlmiSrvcRegEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "Information about a single service provider that is available to
       the user-side of an adjacent device through the ILMI.

       Implementors need to be aware that if the size of the
       atmIlmiSrvcRegServiceID exceeds 112 sub-identifiers then OIDs of





       column instances in this table will have more than 128 sub-
       identifiers and cannot be accessed using SNMPv1, SNMPv2, or
       SNMPv3."

    INDEX { atmIlmiSrvcRegIndex,
            atmIlmiSrvcRegServiceID,
            atmIlmiSrvcRegAddressIndex }
    ::= { atmIlmiSrvcRegTable 1 }

AtmIlmiSrvcRegEntry ::= SEQUENCE {
           atmIlmiSrvcRegIndex             InterfaceIndexOrZero,
           atmIlmiSrvcRegServiceID         OBJECT IDENTIFIER,
           atmIlmiSrvcRegAddressIndex      INTEGER,
           atmIlmiSrvcRegATMAddress        AtmAddr,
           atmIlmiSrvcRegParm1             OCTET STRING,
           atmIlmiSrvcRegRowStatus         RowStatus
           }

atmIlmiSrvcRegIndex OBJECT-TYPE
    SYNTAX       InterfaceIndexOrZero
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "The ATM interface where the service defined in this entry can be
       made available to an ATM device attached to this interface.

       The value of 0 has a special meaning: when an ATM service is
       defined in an entry whose atmIlmiSrvcRegIndex is zero, the ATM
       service is available to ATM devices connected to any ATM
       interface.  (default value(s)).

       When the user-side of an adjacent device queries the content of
       the ILMI service registry MIB (using the ILMI protocol), the
       local network-side responds with the ATM services defined in
       atmIlmiSrvcRegTable entries, provided that these entries are
       indexed by:

       - the corresponding ifIndex value (atmIlmiSrvcRegIndex
         equal to the ifIndex of the interface to which the
         adjacent device is connected) - zero (atmIlmiSrvcRegIndex=0)."
    ::= { atmIlmiSrvcRegEntry 1 }

atmIlmiSrvcRegServiceID OBJECT-TYPE
    SYNTAX       OBJECT IDENTIFIER
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This is the service identifier which uniquely identifies the





       type of service at the address provided in the table.  The object
       identifiers for the LAN Emulation Configuration Server (LECS) and
       the ATM Name Server (ANS) are defined in the ATM Forum ILMI
       Service Registry MIB.  The object identifiers for the ATMARP
       Server, the Multicast Address Resolution Server (MARS), and the
       NHRP Server (NHS) are defined in RFC 2601, RFC 2602, and RFC
       2603, respectively."
    ::= { atmIlmiSrvcRegEntry 2 }

atmIlmiSrvcRegAddressIndex OBJECT-TYPE
    SYNTAX       INTEGER (1..2147483647)
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "An arbitrary integer to differentiate multiple rows containing
       different ATM addresses for the same service on the same
       interface.  This number need NOT be the same as the corresponding
       ILMI atmfSrvcRegAddressIndex MIB object."
    ::= { atmIlmiSrvcRegEntry 3 }

atmIlmiSrvcRegATMAddress OBJECT-TYPE
    SYNTAX       AtmAddr
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
       "This is the full address of the service.  The user-side of the
       adjacent device may use this address to establish a connection
       with the service."
    ::= { atmIlmiSrvcRegEntry 4 }

atmIlmiSrvcRegParm1 OBJECT-TYPE
    SYNTAX       OCTET STRING (SIZE(1..255))
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
       "An octet string used according to the value of
       atmIlmiSrvcRegServiceID."
    ::= { atmIlmiSrvcRegEntry 5 }

atmIlmiSrvcRegRowStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
       "This object is used to create or destroy an entry from this
       table."
    ::= { atmIlmiSrvcRegEntry 6 }






  -- 16. ILMI Network Prefix Table

atmIlmiNetworkPrefixTable    OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmIlmiNetworkPrefixEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "A table specifying per-interface network prefix(es) supplied by
       the network side of the UNI during ILMI address registration.
       When no network prefixes are specified for a particular
       interface, one or more network prefixes based on the switch
       address(es) may be used for ILMI address registration."
    ::= { atm2MIBObjects 16 }

atmIlmiNetworkPrefixEntry OBJECT-TYPE
    SYNTAX       AtmIlmiNetworkPrefixEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "Information about a single network prefix supplied by the
       network side of the UNI during ILMI address registration.  Note
       that the index variable atmIlmiNetPrefixPrefix is a variable-
       length string, and as such the rule for variable-length strings
       in section 7.7 of RFC 2578 applies."
    INDEX   { ifIndex,
              atmIlmiNetPrefixPrefix }
    ::= { atmIlmiNetworkPrefixTable 1 }

AtmIlmiNetworkPrefixEntry ::=
    SEQUENCE {
           atmIlmiNetPrefixPrefix       AtmIlmiNetworkPrefix,
           atmIlmiNetPrefixRowStatus    RowStatus
    }

atmIlmiNetPrefixPrefix    OBJECT-TYPE
    SYNTAX       AtmIlmiNetworkPrefix
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "The network prefix specified for use in ILMI address
       registration."
    ::= { atmIlmiNetworkPrefixEntry 1 }

atmIlmiNetPrefixRowStatus    OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION





       "Used to create, delete, activate and de-activate network
       prefixes used in ILMI address registration."

    ::= { atmIlmiNetworkPrefixEntry 2 }

  -- 17. ATM Switch Address Table

atmSwitchAddressTable    OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmSwitchAddressEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This table contains one or more ATM endsystem addresses on a
       per-switch basis.  These addresses are used to identify the
       switch.  When no ILMI network prefixes are configured for certain
       interfaces, network prefixes based on the switch address(es) may
       be used for ILMI address registration."
    ::= { atm2MIBObjects 17 }

atmSwitchAddressEntry    OBJECT-TYPE
    SYNTAX       AtmSwitchAddressEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "An entry in the ATM Switch Address table."
    INDEX { atmSwitchAddressIndex }
    ::= { atmSwitchAddressTable 1 }

AtmSwitchAddressEntry ::=
    SEQUENCE {
               atmSwitchAddressIndex           Integer32,
               atmSwitchAddressAddress         OCTET STRING,
               atmSwitchAddressRowStatus       RowStatus
    }

atmSwitchAddressIndex   OBJECT-TYPE
    SYNTAX       Integer32 (1..65535)
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "An arbitrary index used to enumerate the ATM endsystem addresses
       for this switch."
    ::= { atmSwitchAddressEntry 1 }

atmSwitchAddressAddress   OBJECT-TYPE
    SYNTAX       OCTET STRING (SIZE(13|20))
    MAX-ACCESS   read-create
    STATUS       current





    DESCRIPTION
       "An ATM endsystem address or address prefix used to identify this
       switch.  When no ESI or SEL field is specified, the switch may
       generate the ESI and SEL fields automatically to obtain a
       complete 20-byte ATM endsystem address."
    ::= { atmSwitchAddressEntry 2 }

atmSwitchAddressRowStatus OBJECT-TYPE
    SYNTAX       RowStatus
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
       "Used to create, delete, activate, and de-activate addresses used
       to identify this switch."
    ::= { atmSwitchAddressEntry 3 }

  -- 18. ATM VP Cross-Connect Extension Table

atmVpCrossConnectXTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmVpCrossConnectXEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This table contains one row per VP Cross-Connect represented in
       the atmVpCrossConnectTable."
    ::= { atm2MIBObjects 18 }

atmVpCrossConnectXEntry       OBJECT-TYPE
    SYNTAX       AtmVpCrossConnectXEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "Information about a particular ATM VP Cross-Connect.
       Each entry provides an two objects that name the Cross-Connect.
       One is assigned by the Service User and the other by the Service
       Provider."
    AUGMENTS     { atmVpCrossConnectEntry }
    ::= { atmVpCrossConnectXTable 1 }

AtmVpCrossConnectXEntry ::= SEQUENCE {
      atmVpCrossConnectUserName       SnmpAdminString,
      atmVpCrossConnectProviderName   SnmpAdminString
}

atmVpCrossConnectUserName OBJECT-TYPE
    SYNTAX       SnmpAdminString (SIZE(0..255))
    MAX-ACCESS   read-create
    STATUS       current





    DESCRIPTION
       "This is a service user assigned textual representation of a VPC
       PVC."
    ::= { atmVpCrossConnectXEntry 1 }

atmVpCrossConnectProviderName OBJECT-TYPE
    SYNTAX       SnmpAdminString (SIZE(0..255))
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "This is a system supplied textual representation of VPC PVC.  It
       is assigned by the service provider."
    ::= { atmVpCrossConnectXEntry 2 }

  -- 19. ATM VC Cross-Connect Extension Table

atmVcCrossConnectXTable OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmVcCrossConnectXEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "This table contains one row per VC Cross-Connect represented in
       the atmVcCrossConnectTable."
    ::= { atm2MIBObjects 19 }

atmVcCrossConnectXEntry       OBJECT-TYPE
    SYNTAX       AtmVcCrossConnectXEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "Information about a particular ATM VC Cross-Connect.
       Each entry provides an two objects that name the Cross-Connect.
       One is assigned by the Service User and the other by the Service
       Provider."
    AUGMENTS   { atmVcCrossConnectEntry }
    ::= { atmVcCrossConnectXTable 1 }

AtmVcCrossConnectXEntry ::= SEQUENCE {
      atmVcCrossConnectUserName       SnmpAdminString,
      atmVcCrossConnectProviderName   SnmpAdminString
}

atmVcCrossConnectUserName OBJECT-TYPE
    SYNTAX       SnmpAdminString (SIZE(0..255))
    MAX-ACCESS   read-create
    STATUS       current
    DESCRIPTION
       "This is a service user assigned textual representation of a VCC





       PVC."
    ::= { atmVcCrossConnectXEntry 1 }

atmVcCrossConnectProviderName OBJECT-TYPE
    SYNTAX       SnmpAdminString (SIZE(0..255))
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "This is a system supplied textual representation of VCC PVC.  It
       is assigned by the service provider."
    ::= { atmVcCrossConnectXEntry 2 }


  -- 20. Currently Failing PVPL Table

atmCurrentlyFailingPVplTable    OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmCurrentlyFailingPVplEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "A table indicating all VPLs for which there is an active row in
       the atmVplTable having an atmVplConnKind value of `pvc' and an
       atmVplOperStatus with a value other than `up'."
    ::= { atm2MIBObjects 20 }

atmCurrentlyFailingPVplEntry    OBJECT-TYPE
    SYNTAX       AtmCurrentlyFailingPVplEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "Each entry in this table represents a VPL for which the
       atmVplRowStatus is `active', the atmVplConnKind is `pvc', and the
       atmVplOperStatus is other than `up'."
    INDEX   { ifIndex, atmVplVpi }
    ::= { atmCurrentlyFailingPVplTable 1 }

AtmCurrentlyFailingPVplEntry ::=
    SEQUENCE {
               atmCurrentlyFailingPVplTimeStamp    TimeStamp
    }

atmCurrentlyFailingPVplTimeStamp    OBJECT-TYPE
    SYNTAX       TimeStamp
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The time at which this PVPL began to fail."
    ::= { atmCurrentlyFailingPVplEntry 1 }





  -- 21. Currently Failing PVCL Table

atmCurrentlyFailingPVclTable    OBJECT-TYPE
    SYNTAX       SEQUENCE OF AtmCurrentlyFailingPVclEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "A table indicating all VCLs for which there is an active row in
       the atmVclTable having an atmVclConnKind value of `pvc' and an
       atmVclOperStatus with a value other than `up'."
    ::= { atm2MIBObjects 21 }

atmCurrentlyFailingPVclEntry    OBJECT-TYPE
    SYNTAX       AtmCurrentlyFailingPVclEntry
    MAX-ACCESS   not-accessible
    STATUS       current
    DESCRIPTION
       "Each entry in this table represents a VCL for which the
       atmVclRowStatus is `active', the atmVclConnKind is `pvc', and the
       atmVclOperStatus is other than `up'."
    INDEX        { ifIndex, atmVclVpi, atmVclVci }
    ::= { atmCurrentlyFailingPVclTable 1 }

AtmCurrentlyFailingPVclEntry ::=
    SEQUENCE {
               atmCurrentlyFailingPVclTimeStamp    TimeStamp
    }

atmCurrentlyFailingPVclTimeStamp    OBJECT-TYPE
    SYNTAX       TimeStamp
    MAX-ACCESS   read-only
    STATUS       current
    DESCRIPTION
       "The time at which this PVCL began to fail."
    ::= { atmCurrentlyFailingPVclEntry 1 }

  -- ATM PVC Traps

  atmPvcTraps    OBJECT IDENTIFIER ::= { atm2MIBTraps 1 }

  atmPvcTrapsPrefix    OBJECT IDENTIFIER ::= { atmPvcTraps 0 }

  atmIntfPvcFailuresTrap    NOTIFICATION-TYPE
    OBJECTS      { ifIndex, atmIntfPvcFailures,
                   atmIntfCurrentlyFailingPVpls,
                   atmIntfCurrentlyFailingPVcls }
    STATUS       current
    DESCRIPTION





       "A notification indicating that one or more PVPLs or PVCLs on
       this interface has failed since the last atmPvcFailuresTrap was
       sent.  If this trap has not been sent for the last
       atmIntfPvcNotificationInterval, then it will be sent on the next
       increment of atmIntfPvcFailures."
    ::= { atmPvcTrapsPrefix 1 }

  -- Conformance Information

atm2MIBConformance   OBJECT IDENTIFIER ::= {atm2MIB 3}

atm2MIBGroups        OBJECT IDENTIFIER ::= {atm2MIBConformance 1}

atm2MIBCompliances   OBJECT IDENTIFIER ::= {atm2MIBConformance 2}

  -- Compliance Statements

atm2MIBCompliance   MODULE-COMPLIANCE
    STATUS       current
    DESCRIPTION
        "The compliance statement for SNMP entities which represent ATM
         interfaces.  The compliance statements are used to determine
         if a particular group or object applies to hosts,
         networks/switches, or both.  The Common group is defined as
         applicable to all three."

    MODULE  -- this module
    MANDATORY-GROUPS  { atmCommonGroup }

  -- Objects in the ATM Switch/Service/Host Group

    GROUP       atmCommonStatsGroup
    DESCRIPTION
        "This group is mandatory for systems that are supporting
         per-VPC or per-VCC counters."

    OBJECT       atmVplLogicalPortDef
    MIN-ACCESS   read-only
    DESCRIPTION
        "This object is mandatory for systems support ATM Logical
         Port interfaces."

    OBJECT       atmIntfSigVccRxTrafficDescrIndex
    DESCRIPTION
        "This object is mandatory for systems that support negotiation
         of signalling VCC traffic parameters through ILMI."

    OBJECT       atmIntfSigVccTxTrafficDescrIndex





    DESCRIPTION
        "This object is mandatory for systems that support negotiation
         of signalling VCC traffic parameters through ILMI."

    OBJECT       atmCurrentlyFailingPVplTimeStamp
    DESCRIPTION
        "This object is optional."

    OBJECT       atmCurrentlyFailingPVclTimeStamp
    DESCRIPTION
        "This object is optional."

    OBJECT       atmIntfLeafSetupFailures
    DESCRIPTION
        "This object is optional."

    OBJECT       atmIntfLeafSetupRequests
    DESCRIPTION
        "This object is optional."

  -- Objects in the ATM Switch/Service Group

    GROUP        atmSwitchServcGroup
    DESCRIPTION
        "This group is mandatory for a Switch/Service that implements
         ATM interfaces."

    OBJECT       atmIfRegAddrRowStatus
    MIN-ACCESS   read-only
    DESCRIPTION
        "Write access is not required, and only one of the six
         enumerated values for the RowStatus textual convention need
         be supported, specifically: active(1)."

    OBJECT       atmSvcVpCrossConnectRowStatus
    MIN-ACCESS   read-only
    DESCRIPTION
        "Write access is not required, and only one of the six
         enumerated values for the RowStatus textual convention need
         be supported, specifically: active(1)"

    OBJECT       atmSvcVcCrossConnectRowStatus
    MIN-ACCESS   read-only
    DESCRIPTION
        "Write access is not required, and only one of the six
         enumerated values for the RowStatus textual convention need
         be supported, specifically: active(1)"






  -- Objects in the ATM Switch/Service Signalling Group

    GROUP       atmSwitchServcSigGroup
    DESCRIPTION
        "This group's write access is not required."

  -- Objects in the ATM Switch/Service Notifications Group

    GROUP        atmSwitchServcNotifGroup
    DESCRIPTION
        "This group is optional for systems implementing support for
         an ATM Switch or an ATM Network Service."

  -- Objects in the ATM Switch Group

    GROUP        atmSwitchGroup
    DESCRIPTION
        "This group is optional for a switch that implements ATM
         interfaces."

  -- Objects in the ATM Service Group

    GROUP        atmServcGroup
    DESCRIPTION
        "This group is mandatory for systems implementing support for
         an ATM Network Service."

  -- Objects in the ATM Host Group

    GROUP        atmHostGroup
    DESCRIPTION
        "This group is mandatory for a Host that implements ATM
         interfaces."

    OBJECT       atmVclAddrType
    MIN-ACCESS   read-only
    DESCRIPTION
        "Write access is not required."

    OBJECT       atmVclAddrRowStatus
    MIN-ACCESS   read-only
    DESCRIPTION
        "Write access is not required, and only one of the six
         enumerated values for the RowStatus textual convention need
         be supported, specifically:  active(1)."

  -- ATM Host Sig Descriptor Parameter Group






    GROUP        atmHostSigDescrGroup
    DESCRIPTION
        "This group is mandatory for a Host that implements ATM
         interfaces.  Write access is not required for this group."

    ::= { atm2MIBCompliances 1 }

  -- **********************************************

  -- Units of Conformance
  -- Mandatory for ATM hosts and switch/service providers

atmCommonGroup     OBJECT-GROUP

OBJECTS {
    atmSigSSCOPConEvents,
    atmSigSSCOPErrdPdus,
    atmSigDetectSetupAttempts,
    atmSigEmitSetupAttempts,
    atmSigDetectUnavailRoutes,
    atmSigEmitUnavailRoutes,
    atmSigDetectUnavailResrcs,
    atmSigEmitUnavailResrcs,
    atmSigDetectCldPtyEvents,
    atmSigEmitCldPtyEvents,
    atmSigDetectMsgErrors,
    atmSigEmitMsgErrors,
    atmSigDetectClgPtyEvents,
    atmSigEmitClgPtyEvents,
    atmSigDetectTimerExpireds,
    atmSigEmitTimerExpireds,
    atmSigDetectRestarts,
    atmSigEmitRestarts,
    atmSigInEstabls,
    atmSigOutEstabls,
    atmVplLogicalPortDef,
    atmVplLogicalPortIndex,
    atmInterfaceConfMaxSvpcVpi,
    atmInterfaceCurrentMaxSvpcVpi,
    atmInterfaceConfMaxSvccVpi,
    atmInterfaceCurrentMaxSvccVpi,
    atmInterfaceConfMinSvccVci,
    atmInterfaceCurrentMinSvccVci,
    atmIntfSigVccRxTrafficDescrIndex,
    atmIntfSigVccTxTrafficDescrIndex,
    atmIntfPvcFailures,
    atmIntfCurrentlyFailingPVpls,
    atmIntfCurrentlyFailingPVcls,





    atmIntfPvcNotificationInterval,
    atmIntfPvcFailuresTrapEnable,
    atmIntfLeafSetupFailures,
    atmIntfLeafSetupRequests,
    atmIntfConfigType,
    atmIntfActualType,
    atmIntfConfigSide,
    atmIntfActualSide,
    atmIntfIlmiAdminStatus,
    atmIntfIlmiOperStatus,
    atmIntfIlmiFsmState,
    atmIntfIlmiEstablishConPollIntvl,
    atmIntfIlmiCheckConPollIntvl,
    atmIntfIlmiConPollInactFactor,
    atmIntfIlmiPublicPrivateIndctr,
    atmCurrentlyFailingPVplTimeStamp,
    atmCurrentlyFailingPVclTimeStamp
}

  STATUS       current
  DESCRIPTION
    "A collection of objects providing information
    for a Switch/Service/Host that implements
    ATM interfaces."
  ::= { atm2MIBGroups 1 }

atmCommonStatsGroup     OBJECT-GROUP

OBJECTS {
    atmVclStatTotalCellIns,
    atmVclStatClp0CellIns,
    atmVclStatTotalDiscards,
    atmVclStatClp0Discards,
    atmVclStatTotalCellOuts,
    atmVclStatClp0CellOuts,
    atmVclStatClp0Tagged,
    atmVplStatTotalCellIns,
    atmVplStatClp0CellIns,
    atmVplStatTotalDiscards,
    atmVplStatClp0Discards,
    atmVplStatTotalCellOuts,
    atmVplStatClp0CellOuts,
    atmVplStatClp0Tagged
}

  STATUS       current
  DESCRIPTION
    "A collection of objects providing information





    for a Switch/Service/Host that implements
    ATM VCL and VPL Statistics"
  ::= { atm2MIBGroups 2 }

  atmSwitchServcGroup     OBJECT-GROUP

  OBJECTS {
    atmIlmiSrvcRegATMAddress,
    atmIlmiSrvcRegParm1,
    atmIlmiSrvcRegRowStatus,
    atmIlmiNetPrefixRowStatus,
    atmSvcVpCrossConnectCreationTime,
    atmSvcVpCrossConnectRowStatus,
    atmSvcVcCrossConnectCreationTime,
    atmSvcVcCrossConnectRowStatus,
    atmIfRegAddrAddressSource,
    atmIfRegAddrOrgScope,
    atmIfRegAddrRowStatus}
  STATUS       current
  DESCRIPTION
    "A collection of objects providing information
    for a Switch/Service that implements ATM interfaces."
  ::= { atm2MIBGroups 3 }

  atmSwitchServcSigGroup     OBJECT-GROUP

  OBJECTS {
    atmSigSupportClgPtyNumDel,
    atmSigSupportClgPtySubAddr,
    atmSigSupportCldPtySubAddr,
    atmSigSupportHiLyrInfo,
    atmSigSupportLoLyrInfo,
    atmSigSupportBlliRepeatInd,
    atmSigSupportAALInfo,
    atmSigSupportPrefCarrier}
  STATUS       current
  DESCRIPTION
    "A collection of objects providing information
    for a Switch/Service that implements ATM signalling."
  ::= { atm2MIBGroups 4 }

    atmSwitchServcNotifGroup     NOTIFICATION-GROUP

    NOTIFICATIONS { atmIntfPvcFailuresTrap }
    STATUS       current
    DESCRIPTION
        "A collection of notifications providing information
        for a Switch/Service that implements ATM interfaces."





    ::= { atm2MIBGroups 5 }

    atmSwitchGroup     OBJECT-GROUP
        OBJECTS {
            atmSwitchAddressAddress,
            atmSwitchAddressRowStatus }
        STATUS       current
        DESCRIPTION
          "A collection of objects providing information
          for an ATM switch."
        ::= { atm2MIBGroups 6 }

    atmServcGroup     OBJECT-GROUP

    OBJECTS {
        atmVpCrossConnectUserName,
        atmVpCrossConnectProviderName,
        atmVcCrossConnectUserName,
        atmVcCrossConnectProviderName }
    STATUS       current
    DESCRIPTION
        "A collection of objects providing information
        for an ATM Network Service."
    ::= { atm2MIBGroups 7 }

    atmHostGroup     OBJECT-GROUP

    OBJECTS {
        atmAal5VclInPkts,
        atmAal5VclOutPkts,
        atmAal5VclInOctets,
        atmAal5VclOutOctets,
        atmVclAddrType,
        atmVclAddrRowStatus,
        atmAddrVclAddrType,
        atmVclGenSigDescrIndex}
    STATUS       current
    DESCRIPTION
      "A collection of objects providing information
      for a Host that implements ATM interfaces."
    ::= { atm2MIBGroups 8 }

    atmHostSigDescrGroup     OBJECT-GROUP

    OBJECTS {
           atmSigDescrParamAalType,
           atmSigDescrParamAalSscsType,
           atmSigDescrParamBhliType,





           atmSigDescrParamBhliInfo,
           atmSigDescrParamBbcConnConf,
           atmSigDescrParamBlliLayer2,
           atmSigDescrParamBlliLayer3,
           atmSigDescrParamBlliPktSize,
           atmSigDescrParamBlliSnapId,
           atmSigDescrParamBlliOuiPid,
           atmSigDescrParamRowStatus}
    STATUS       current
    DESCRIPTION
      "A collection of objects providing information
      for a Host that implements ATM interfaces."
    ::= { atm2MIBGroups 9 }

END


