ETHER-CHIPSET-MIB DEFINITIONS ::= BEGIN


       IMPORTS
           MODULE-IDENTITY, OBJECT-IDENTITY, mib-2
               FROM SNMPv2-SMI
           dot3
               FROM EtherLike-MIB;

       etherChipsetMIB MODULE-IDENTITY
           LAST-UPDATED "9908240400Z"  -- August 24, 199
           ORGANIZATION "IETF 802.3 Hub MIB Working Group"
           CONTACT-INFO
               "WG E-mail: hubmib@hprnd.rose.hp.com
             To subscribe: hubmib-request@hprnd.rose.hp.com

                    Chair: Dan Romascanu
                   Postal: Lucent Technologies
                           Atidum Technology Park, Bldg. 3
                           Tel Aviv 61131
                           Israel
                      Tel: +972 3 645 8414
                   E-mail: dromasca@lucent.com

                  Editor: John Flick
                  Postal: Hewlett-Packard Company
                          8000 Foothills Blvd. M/S 5556
                          Roseville, CA 95747-5556
                          USA





                     Tel: +1 916 785 4018
                     Fax: +1 916 785 3583
                  E-mail: johnf@rose.hp.com"

           DESCRIPTION "This MIB module contains registered values for
                       use by the dot3StatsEtherChipSet object in
                       the EtherLike-MIB.  This object is used to
                       identify the MAC hardware used to communicate
                       on an interface.

                       Note that the dot3StatsEtherChipSet object
                       has been deprecated.  The primary purpose of
                       this module is to capture historic assignments
                       made by the various IETF working groups that
                       have been responsible for maintaining the
                       EtherLike-MIB.  Implementations which support
                       the dot3StatsEtherChipSet object for backwards
                       compatability may continue to use these values.
                       For those chipsets not represented in this
                       module, registration is required in other
                       documentation, e.g., assignment within that
                       part of the registration tree delegated to
                       individual enterprises (see RFC 1155 and RFC
                       1902)."

           REVISION    "9908240400Z"  -- August 24, 1999
           DESCRIPTION "Initial version of this module created by
                       splitting the chipset registration information
                       out from the EtherLike-MIB.
                       Version published as RFC 2666."
           ::= { mib-2 70 }

       dot3ChipSets          OBJECT IDENTIFIER ::= { dot3 8 }

       dot3ChipSetAMD        OBJECT IDENTIFIER ::= { dot3ChipSets 1 }

       dot3ChipSetAMD7990 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am7990 Local Area Network
                       Controller for Ethernet (LANCE)."
           ::= { dot3ChipSetAMD 1 }

       dot3ChipSetAMD79900 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79900 chip."
           ::= { dot3ChipSetAMD 2 }





       dot3ChipSetAMD79C940 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C940 Media Access Controller
                       for Ethernet (MACE)."
           ::= { dot3ChipSetAMD 3 }

       dot3ChipSetAMD79C90 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C90 CMOS Local Area Network
                       Controller for Ethernet (C-LANCE)."
           ::= { dot3ChipSetAMD 4 }

       dot3ChipSetAMD79C960 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C960 PCnet-ISA Single Chip
                       Ethernet Controller for ISA."
           ::= { dot3ChipSetAMD 5 }

       dot3ChipSetAMD79C961 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C961 PCnet-ISA+ Single Chip
                       Plug & Play Full-Duplex Ethernet Controller
                       for ISA."
           ::= { dot3ChipSetAMD 6 }

       dot3ChipSetAMD79C961A OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C961A PCnet-ISA II Single Chip
                       Plug & Play Full-Duplex Ethernet Controller
                       for ISA."
           ::= { dot3ChipSetAMD 7 }

       dot3ChipSetAMD79C965 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C965 PCnet-32 Single Chip
                       Ethernet Controller for PCI."
           ::= { dot3ChipSetAMD 8 }

       dot3ChipSetAMD79C970 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C970 PCnet PCI Single Chip





                       Ethernet Controller for PCI Local Bus."
           ::= { dot3ChipSetAMD 9 }

       dot3ChipSetAMD79C970A OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices AM79C970A PCnet PCI II Single Chip
                       Full-Duplex Ethernet Controller for PCI Local
                       Bus."
           ::= { dot3ChipSetAMD 10 }

       dot3ChipSetAMD79C971 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C971 PCnet-FAST Single Chip
                       Full-Duplex 10/100 Mbps Ethernet Controller for
                       PCI Local Bus."
           ::= { dot3ChipSetAMD 11 }

       dot3ChipSetAMD79C972 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Advanced
                       Micro Devices Am79C972 PCnet-FAST+ Enhanced
                       10/100 Mbps PCI Ethernet Controller with OnNow
                       Support."
           ::= { dot3ChipSetAMD 12 }

       dot3ChipSetIntel      OBJECT IDENTIFIER ::= { dot3ChipSets 2 }

       dot3ChipSetIntel82586 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Intel
                       82586 IEEE 802.3 Ethernet LAN Coprocessor."
           ::= { dot3ChipSetIntel 1 }

       dot3ChipSetIntel82596 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Intel
                       82596 High-Performance 32-Bit Local Area Network
                       Coprocessor."
           ::= { dot3ChipSetIntel 2 }

       dot3ChipSetIntel82595 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Intel
                       82595 High Integration Ethernet Controller."
           ::= { dot3ChipSetIntel 3 }






       dot3ChipSetIntel82557 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Intel
                       82557 Fast Ethernet PCI Bus Lan Controller."
           ::= { dot3ChipSetIntel 4 }

       dot3ChipSetIntel82558 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Intel
                       82558 Fast Ethernet PCI Bus LAN Controller with
                       Integrated PHY."
           ::= { dot3ChipSetIntel 5 }

       dot3ChipSetSeeq       OBJECT IDENTIFIER ::= { dot3ChipSets 3 }

       dot3ChipSetSeeq8003 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       8003 chip set."
           ::= { dot3ChipSetSeeq 1 }

       dot3ChipSetSeeq80C03 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       80C03 Full-Duplex CMOS Ethernet Data Link
                       Controller (MAC)."
           ::= { dot3ChipSetSeeq 2 }

       dot3ChipSetSeeq84C30 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       4-Port 84C30 Full-Duplex CMOS Ethernet 10
                       MBit/Sec Data Link Controller (MAC)."
           ::= { dot3ChipSetSeeq 3 }

       dot3ChipSetSeeq8431 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       4-Port 8431 Full-Duplex CMOS Ethernet 10
                       MBit/Sec Data Link Controller (MAC)."
           ::= { dot3ChipSetSeeq 4 }

       dot3ChipSetSeeq80C300 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       80C300 Full-Duplex CMOS Ethernet 10/100
                       Mbit/Sec Data Link Controller (MAC)."
           ::= { dot3ChipSetSeeq 5 }





       dot3ChipSetSeeq84C300 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       4-Port 84C300 Fast Ethernet Controller (MAC)."
           ::= { dot3ChipSetSeeq 6 }

       dot3ChipSetSeeq84301 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       4-Port 84301 Fast Ethernet Controller (MAC)."
           ::= { dot3ChipSetSeeq 7 }

       dot3ChipSetSeeq84302 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       4-Port 84302 Fast Ethernet Controller (MAC)."
           ::= { dot3ChipSetSeeq 8 }

       dot3ChipSetSeeq8100 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the SEEQ
                       8100 Gigabit Ethernet Controller (MAC & PCS)."
           ::= { dot3ChipSetSeeq 9 }

       dot3ChipSetNational   OBJECT IDENTIFIER ::= { dot3ChipSets 4 }

       dot3ChipSetNational8390 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP8390 Network Interface
                       Controller."
           ::= { dot3ChipSetNational 1 }

       dot3ChipSetNationalSonic OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP83932 Systems-Oriented Network
                       Interface Controller (SONIC)."
           ::= { dot3ChipSetNational 2 }

       dot3ChipSetNational83901 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP83901 Serial Network Interface
                       Controller (SNIC)."
           ::= { dot3ChipSetNational 3 }

       dot3ChipSetNational83902 OBJECT-IDENTITY





           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP83902 Serial Network Interface
                       Controller for Twisted Pair (ST-NIC)."
           ::= { dot3ChipSetNational 4 }

       dot3ChipSetNational83905 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP83905 AT Local Area Network
                       Twisted-Pair Interface (AT/LANTIC)."
           ::= { dot3ChipSetNational 5 }

       dot3ChipSetNational83907 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP83907 AT Twisted-Pair Enhanced
                       Coaxial Network Interface Controller
                       (AT/LANTIC II)."
           ::= { dot3ChipSetNational 6 }

       dot3ChipSetNational83916 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP83916 Systems-Oriented Network
                       Interface Controller (SONIC-16)."
           ::= { dot3ChipSetNational 7 }

       dot3ChipSetNational83934 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP83934 Systems-Oriented Network
                       Interface Controller with Twisted Pair Interface
                       (SONIC-T)."
           ::= { dot3ChipSetNational 8 }

       dot3ChipSetNational83936 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the National
                       Semiconductor DP83936AVUL Full-Duplex Systems-
                       Oriented Network Interface Controller with
                       Twisted Pair Interface (SONIC-T)."
           ::= { dot3ChipSetNational 9 }

       dot3ChipSetFujitsu    OBJECT IDENTIFIER ::= { dot3ChipSets 5 }

       dot3ChipSetFujitsu86950 OBJECT-IDENTITY
           STATUS      current





           DESCRIPTION "The authoritative identifier for the Fujitsu
                       86950 chip."
           ::= { dot3ChipSetFujitsu 1 }

       dot3ChipSetFujitsu86960 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Fujitsu
                       MB86960 Network Interface Controller with
                       Encoder/Decoder (NICE)."
           ::= { dot3ChipSetFujitsu 2 }

       dot3ChipSetFujitsu86964 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Fujitsu
                       MB86964 Ethernet Controller with 10BASE-T
                       Tranceiver."
           ::= { dot3ChipSetFujitsu 3 }

       dot3ChipSetFujitsu86965A OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Fujitsu
                       MB86965A EtherCoupler Single-Chip Ethernet
                       Controller."
           ::= { dot3ChipSetFujitsu 4 }

       dot3ChipSetFujitsu86965B OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Fujitsu
                       MB86965B EtherCoupler Single-Chip Ethernet
                       Controller (supports full-duplex)."
           ::= { dot3ChipSetFujitsu 5 }

       dot3ChipSetDigital    OBJECT IDENTIFIER ::= { dot3ChipSets 6 }

       dot3ChipSetDigitalDC21040 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Digital
                       Semiconductor DC21040 chip."
           ::= { dot3ChipSetDigital 1 }

       dot3ChipSetDigital21041 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Digital
                       Semiconductor 21041 PCI Ethernet LAN
                       Controller."
           ::= { dot3ChipSetDigital 2 }

       dot3ChipSetDigital21140 OBJECT-IDENTITY





           STATUS      current
           DESCRIPTION "The authoritative identifier for the Digital
                       Semiconductor 21140 PCI Fast Ethernet LAN
                       Controller."
           ::= { dot3ChipSetDigital 3 }

       dot3ChipSetDigital21143 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Digital
                       Semiconductor 21143 PCI/CardBus 10/100-Mb/s
                       Ethernet LAN Controller."
           ::= { dot3ChipSetDigital 4 }

       dot3ChipSetDigital21340 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Digital
                       Semiconductor 21340 10/100-MB/s managed buffered
                       port switch."
           ::= { dot3ChipSetDigital 5 }

       dot3ChipSetDigital21440 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Digital
                       Semiconductor 21440 Multiport 10/100Mbps
                       Ethernet Controller."
           ::= { dot3ChipSetDigital 6 }

       dot3ChipSetDigital21540 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Digital
                       Semiconductor 21540 PCI/CardBus Ethernet LAN
                       Controller with Modem Interface."
           ::= { dot3ChipSetDigital 7 }

       dot3ChipSetTI         OBJECT IDENTIFIER ::= { dot3ChipSets 7 }

       dot3ChipSetTIE100 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Texas
                       Instruments TNETE100 ThunderLAN PCI Fast
                       Ethernet Controller."
           ::= { dot3ChipSetTI 1 }

       dot3ChipSetTIE110 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Texas
                       Instruments TNETE110 ThunderLAN PCI 10BASE-T
                       Ethernet Adapter."





           ::= { dot3ChipSetTI 2 }

       dot3ChipSetTIX3100 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Texas
                       Instruments TNETX3100 Desktop ThunderSWITCH
                       8/2."
           ::= { dot3ChipSetTI 3 }

       dot3ChipSetTIX3150 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Texas
                       Instruments TNETX3150 ThunderSWITCH 12/3."
           ::= { dot3ChipSetTI 4 }

       dot3ChipSetTIX3270 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Texas
                       Instruments TNETX3270 ThunderSWITCH 24/3."
           ::= { dot3ChipSetTI 5 }

       dot3ChipSetToshiba    OBJECT IDENTIFIER ::= { dot3ChipSets 8 }

       dot3ChipSetToshibaTC35815F OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Toshiba
                       TC35815F PCI-Based 100/10Mbps Ethernet
                       Controller."
           ::= { dot3ChipSetToshiba 1 }

       dot3ChipSetLucent     OBJECT IDENTIFIER ::= { dot3ChipSets 9 }

       dot3ChipSetLucentATT1MX10 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Lucent
                       Technologies ATT1MX10 (Spinnaker) Quad MAC and
                       Tranceiver for Ethernet Frame Switching."
              ::= { dot3ChipSetLucent 1 }

       dot3ChipSetLucentLUC3M08 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Lucent
                       Technologies LUC3M08 Eight Ethernet MACs for
                       10/100 Mbits/s Frame Switching."
           ::= { dot3ChipSetLucent 2 }

       dot3ChipSetGalileo    OBJECT IDENTIFIER ::= { dot3ChipSets 10 }






       dot3ChipSetGalileoGT48001 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Galileo
                       Technology GT-48001A Switched Ethernet
                       Controller."
           ::= { dot3ChipSetGalileo 1 }

       dot3ChipSetGalileoGT48002 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Galileo
                       Technology GT-48002A Switched Fast Ethernet
                       Controller."
           ::= { dot3ChipSetGalileo 2 }

       dot3ChipSetGalileoGT48004 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Galileo
                       Technology GT-48004A Four Port Fast Ethernet
                       Switch for Multiport 10/100BASE-X Systems."
           ::= { dot3ChipSetGalileo 3 }

       dot3ChipSetGalileoGT48207 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Galileo
                       Technology GT-48207 Low-Cost 10 Port Switched
                       Ethernet Controller for 10+10/100BASE-X."
           ::= { dot3ChipSetGalileo 4 }

       dot3ChipSetGalileoGT48208 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Galileo
                       Technology GT-48208 Advanced 10 Port Switched
                       Ethernet Controller for 10+10/100BASE-X."
           ::= { dot3ChipSetGalileo 5 }

       dot3ChipSetGalileoGT48212 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Galileo
                       Technology GT-48212 Advanced 14 Port Switched
                       Ethernet Controller for 10+10/100BASE-X."
           ::= { dot3ChipSetGalileo 6 }

       dot3ChipSetJato       OBJECT IDENTIFIER ::= { dot3ChipSets 11 }

       dot3ChipSetJatoJT1001 OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the Jato
                       Technologies JT1001 GigEMAC Server





                       10/100/1000Mbps Ethernet Controller with PCI
                       interface."
           ::= { dot3ChipSetJato 1 }

       dot3ChipSetXaQti      OBJECT IDENTIFIER ::= { dot3ChipSets 12 }

       dot3ChipSetXaQtiXQ11800FP OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the XaQTI
                       XQ11800FP XMAC II Gigabit Ethernet Media Access
                       Controller."
           ::= { dot3ChipSetXaQti 1 }

       dot3ChipSetXaQtiXQ18110FP OBJECT-IDENTITY
           STATUS      current
           DESCRIPTION "The authoritative identifier for the XaQTI
                       XQ18110FP GigaPower Protocol Accelerator."
           ::= { dot3ChipSetXaQti 2 }

   END


