HC-ALARM-MIB DEFINITIONS ::= BEGIN


IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
        Integer32, Counter32, Unsigned32
                FROM SNMPv2-SMI
        MODULE-COMPLIANCE, OBJECT-GROUP,
        NOTIFICATION-GROUP
                FROM SNMPv2-CONF
        RowStatus, VariablePointer, StorageType,
        TEXTUAL-CONVENTION
                FROM SNMPv2-TC
        CounterBasedGauge64
                FROM HCNUM-TC
        rmon, OwnerString, rmonEventGroup
                FROM RMON-MIB;

hcAlarmMIB MODULE-IDENTITY
    LAST-UPDATED    "200212160000Z"
    ORGANIZATION    "IETF RMONMIB Working Group"
    CONTACT-INFO
            "        Andy Bierman
                     Cisco Systems, Inc.
                Tel: +1 408 527-3711





             E-mail: abierman@cisco.com
             Postal: 170 West Tasman Drive
                     San Jose, CA USA 95134

                     Keith McCloghrie
                     Cisco Systems, Inc.
                Tel: +1 408 526-5260
             E-mail: kzm@cisco.com
             Postal: 170 West Tasman Drive
                     San Jose, CA USA 95134

             Send comments to <rmonmib@ietf.org>
             Mailing list subscription info:
                 http://www.ietf.org/mailman/listinfo/rmonmib "
    DESCRIPTION
            "This module defines Remote Monitoring MIB extensions for
             High Capacity Alarms.

             Copyright (C) The Internet Society (2002). This version
             of this MIB module is part of RFC 3434; see the RFC
             itself for full legal notices."

    REVISION        "200212160000Z"
    DESCRIPTION
            "Initial version of the High Capacity Alarm MIB module.
             This version published as RFC 3434."
    ::= { rmon 29 }

hcAlarmObjects       OBJECT IDENTIFIER ::= { hcAlarmMIB 1 }
hcAlarmNotifications OBJECT IDENTIFIER ::= { hcAlarmMIB 2 }
hcAlarmConformance   OBJECT IDENTIFIER ::= { hcAlarmMIB 3 }

hcAlarmControlObjects OBJECT IDENTIFIER ::= { hcAlarmObjects 1 }
hcAlarmCapabilitiesObjects OBJECT IDENTIFIER
                                        ::= { hcAlarmObjects 2 }

--
-- Textual Conventions
--

HcValueStatus ::= TEXTUAL-CONVENTION
    STATUS current
    DESCRIPTION
            "This data type indicates the validity and sign of the data
            in associated object instances which represent the absolute
            value of a high capacity numeric quantity.  Such an object
            may be represented with one or more object instances. An
            object of type HcValueStatus MUST be defined within the same





            structure as the object(s) representing the high capacity
            absolute value.

            If the associated object instance(s) representing the high
            capacity absolute value could not be accessed during the
            sampling interval, and is therefore invalid, then the
            associated HcValueStatus object will contain the value
            'valueNotAvailable(1)'.

            If the associated object instance(s) representing the high
            capacity absolute value are valid and actual value of the
            sample is greater than or equal to zero, then the associated
            HcValueStatus object will contain the value
            'valuePositive(2)'.

            If the associated object instance(s) representing the high
            capacity absolute value are valid and the actual value of
            the sample is less than zero, then the associated
            HcValueStatus object will contain the value
            'valueNegative(3)'.  The associated absolute value should be
            multiplied by -1 to obtain the true sample value."
    SYNTAX INTEGER {
        valueNotAvailable(1),
        valuePositive(2),
        valueNegative(3)
    }

--
-- High Capacity Alarm Table
--

hcAlarmTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF HcAlarmEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A list of entries for the configuration of high capacity
            alarms."
    ::= { hcAlarmControlObjects 1 }

hcAlarmEntry OBJECT-TYPE
    SYNTAX      HcAlarmEntry
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A conceptual row in the hcAlarmTable. Entries are usually
            created in this table by management application action, but
            may also be created by agent action as well."





    INDEX { hcAlarmIndex }
    ::= { hcAlarmTable 1 }

HcAlarmEntry ::= SEQUENCE {
    hcAlarmIndex                     Integer32,
    hcAlarmInterval                  Integer32,
    hcAlarmVariable                  VariablePointer,
    hcAlarmSampleType                INTEGER,
    hcAlarmAbsValue                  CounterBasedGauge64,
    hcAlarmValueStatus               HcValueStatus,
    hcAlarmStartupAlarm              INTEGER,
    hcAlarmRisingThreshAbsValueLo    Unsigned32,
    hcAlarmRisingThreshAbsValueHi    Unsigned32,
    hcAlarmRisingThresholdValStatus  HcValueStatus,
    hcAlarmFallingThreshAbsValueLo   Unsigned32,
    hcAlarmFallingThreshAbsValueHi   Unsigned32,
    hcAlarmFallingThresholdValStatus HcValueStatus,
    hcAlarmRisingEventIndex          Integer32,
    hcAlarmFallingEventIndex         Integer32,
    hcAlarmValueFailedAttempts       Counter32,
    hcAlarmOwner                     OwnerString,
    hcAlarmStorageType               StorageType,
    hcAlarmStatus                    RowStatus }

hcAlarmIndex OBJECT-TYPE
    SYNTAX      Integer32 (1..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "An arbitrary integer index value used to uniquely identify
            this high capacity alarm entry."
    ::= { hcAlarmEntry 1 }

hcAlarmInterval OBJECT-TYPE
    SYNTAX      Integer32 (1..2147483647)
    UNITS      "seconds"
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The interval in seconds over which the data is sampled and
            compared with the rising and falling thresholds.  When
            setting this variable, care should be taken in the case of
            deltaValue sampling - the interval should be set short
            enough that the sampled variable is very unlikely to
            increase or decrease by more than 2^63 - 1 during a single
            sampling interval.







            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 2 }

hcAlarmVariable OBJECT-TYPE
    SYNTAX      VariablePointer
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The object identifier of the particular variable to be
            sampled.  Only variables that resolve to an ASN.1 primitive
            type of INTEGER (INTEGER, Integer32, Counter32, Counter64,
            Gauge, or TimeTicks) may be sampled.

            Because SNMP access control is articulated entirely in terms
            of the contents of MIB views, no access control mechanism
            exists that can restrict the value of this object to
            identify only those objects that exist in a particular MIB
            view.  Because there is thus no acceptable means of
            restricting the read access that could be obtained through
            the alarm mechanism, the probe must only grant write access
            to this object in those views that have read access to all
            objects on the probe.

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 3 }

hcAlarmSampleType OBJECT-TYPE
    SYNTAX INTEGER {
               absoluteValue(1),
               deltaValue(2)
           }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The method of sampling the selected variable and
            calculating the value to be compared against the thresholds.
            If the value of this object is absoluteValue(1), the value
            of the selected variable will be compared directly with the
            thresholds at the end of the sampling interval.  If the
            value of this object is deltaValue(2), the value of the
            selected variable at the last sample will be subtracted from
            the current value, and the difference compared with the
            thresholds.

            If the associated hcAlarmVariable instance could not be
            obtained at the previous sample interval, then a delta





            sample is not possible, and the value of the associated
            hcAlarmValueStatus object for this interval will be
            valueNotAvailable(1).

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 4 }

hcAlarmAbsValue OBJECT-TYPE
    SYNTAX      CounterBasedGauge64
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "The absolute value (i.e., unsigned value) of the
            hcAlarmVariable statistic during the last sampling period.
            The value during the current sampling period is not made
            available until the period is completed.

            To obtain the true value for this sampling interval, the
            associated instance of hcAlarmValueStatus must be checked,
            and the value of this object adjusted as necessary.

            If the MIB instance could not be accessed during the
            sampling interval, then this object will have a value of
            zero and the associated instance of hcAlarmValueStatus will
            be set to 'valueNotAvailable(1)'."
    ::= { hcAlarmEntry 5 }

hcAlarmValueStatus OBJECT-TYPE
    SYNTAX      HcValueStatus
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "This object indicates the validity and sign of the data for
            the hcAlarmAbsValue object, as described in the
            HcValueStatus textual convention."
    ::= { hcAlarmEntry 6 }

hcAlarmStartupAlarm OBJECT-TYPE
    SYNTAX     INTEGER {
                  risingAlarm(1),
                  fallingAlarm(2),
                  risingOrFallingAlarm(3)
               }
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The alarm that may be sent when this entry is first set to





            active.  If the first sample after this entry becomes active
            is greater than or equal to the rising threshold and this
            object is equal to risingAlarm(1) or
            risingOrFallingAlarm(3), then a single rising alarm will be
            generated.  If the first sample after this entry becomes
            valid is less than or equal to the falling threshold and
            this object is equal to fallingAlarm(2) or
            risingOrFallingAlarm(3), then a single falling alarm will be
            generated.

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 7 }

hcAlarmRisingThreshAbsValueLo OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The lower 32 bits of the absolute value for threshold for
            the sampled statistic.  The actual threshold value is
            determined by the associated instances of the
            hcAlarmRisingThreshAbsValueHi and
            hcAlarmRisingThresholdValStatus objects, as follows:

               ABS(threshold) = hcAlarmRisingThreshAbsValueLo +
                     (hcAlarmRisingThreshAbsValueHi * 2^^32)

            The absolute value of the threshold is adjusted as required,
            as described in the HcValueStatus textual convention.  These
            three object instances are conceptually combined to
            represent the rising threshold for this entry.

            When the current sampled value is greater than or equal to
            this threshold, and the value at the last sampling interval
            was less than this threshold, a single event will be
            generated.  A single event will also be generated if the
            first sample after this entry becomes valid is greater than
            or equal to this threshold and the associated
            hcAlarmStartupAlarm is equal to risingAlarm(1) or
            risingOrFallingAlarm(3).

            After a rising event is generated, another such event will
            not be generated until the sampled value falls below this
            threshold and reaches the threshold identified by the
            hcAlarmFallingThreshAbsValueLo,
            hcAlarmFallingThreshAbsValueHi, and
            hcAlarmFallingThresholdValStatus objects.





            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."

    ::= { hcAlarmEntry 8 }

hcAlarmRisingThreshAbsValueHi OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The upper 32 bits of the absolute value for threshold for
            the sampled statistic.  The actual threshold value is
            determined by the associated instances of the
            hcAlarmRisingThreshAbsValueLo and
            hcAlarmRisingThresholdValStatus objects, as follows:

               ABS(threshold) = hcAlarmRisingThreshAbsValueLo +
                     (hcAlarmRisingThreshAbsValueHi * 2^^32)

            The absolute value of the threshold is adjusted as required,
            as described in the HcValueStatus textual convention.  These
            three object instances are conceptually combined to
            represent the rising threshold for this entry.

            When the current sampled value is greater than or equal to
            this threshold, and the value at the last sampling interval
            was less than this threshold, a single event will be
            generated.  A single event will also be generated if the
            first sample after this entry becomes valid is greater than
            or equal to this threshold and the associated
            hcAlarmStartupAlarm is equal to risingAlarm(1) or
            risingOrFallingAlarm(3).

            After a rising event is generated, another such event will
            not be generated until the sampled value falls below this
            threshold and reaches the threshold identified by the
            hcAlarmFallingThreshAbsValueLo,
            hcAlarmFallingThreshAbsValueHi, and
            hcAlarmFallingThresholdValStatus objects.

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 9 }

hcAlarmRisingThresholdValStatus OBJECT-TYPE
    SYNTAX      HcValueStatus
    MAX-ACCESS  read-create
    STATUS      current





    DESCRIPTION
            "This object indicates the sign of the data for the rising
            threshold, as defined by the hcAlarmRisingThresAbsValueLo
            and hcAlarmRisingThresAbsValueHi objects, as described in
            the HcValueStatus textual convention.

            The enumeration 'valueNotAvailable(1)' is not allowed, and
            the associated hcAlarmStatus object cannot be equal to
            'active(1)' if this object is set to this value.

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 10 }

hcAlarmFallingThreshAbsValueLo OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The lower 32 bits of the absolute value for threshold for
            the sampled statistic.  The actual threshold value is
            determined by the associated instances of the
            hcAlarmFallingThreshAbsValueHi and
            hcAlarmFallingThresholdValStatus objects, as follows:

               ABS(threshold) = hcAlarmFallingThreshAbsValueLo +
                     (hcAlarmFallingThreshAbsValueHi * 2^^32)

            The absolute value of the threshold is adjusted as required,
            as described in the HcValueStatus textual convention.  These
            three object instances are conceptually combined to
            represent the falling threshold for this entry.

            When the current sampled value is less than or equal to this
            threshold, and the value at the last sampling interval was
            greater than this threshold, a single event will be
            generated.  A single event will also be generated if the
            first sample after this entry becomes valid is less than or
            equal to this threshold and the associated
            hcAlarmStartupAlarm is equal to fallingAlarm(2) or
            risingOrFallingAlarm(3).

            After a falling event is generated, another such event will
            not be generated until the sampled value rises above this
            threshold and reaches the threshold identified by the
            hcAlarmRisingThreshAbsValueLo,
            hcAlarmRisingThreshAbsValueHi, and
            hcAlarmRisingThresholdValStatus objects.





            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 11 }

hcAlarmFallingThreshAbsValueHi OBJECT-TYPE
    SYNTAX      Unsigned32
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The upper 32 bits of the absolute value for threshold for
            the sampled statistic.  The actual threshold value is
            determined by the associated instances of the
            hcAlarmFallingThreshAbsValueLo and
            hcAlarmFallingThresholdValStatus objects, as follows:

               ABS(threshold) = hcAlarmFallingThreshAbsValueLo +
                     (hcAlarmFallingThreshAbsValueHi * 2^^32)

            The absolute value of the threshold is adjusted as required,
            as described in the HcValueStatus textual convention.  These
            three object instances are conceptually combined to
            represent the falling threshold for this entry.

            When the current sampled value is less than or equal to this
            threshold, and the value at the last sampling interval was
            greater than this threshold, a single event will be
            generated.  A single event will also be generated if the
            first sample after this entry becomes valid is less than or
            equal to this threshold and the associated
            hcAlarmStartupAlarm is equal to fallingAlarm(2) or
            risingOrFallingAlarm(3).

            After a falling event is generated, another such event will
            not be generated until the sampled value rises above this
            threshold and reaches the threshold identified by the
            hcAlarmRisingThreshAbsValueLo,
            hcAlarmRisingThreshAbsValueHi, and
            hcAlarmRisingThresholdValStatus objects.

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 12 }

hcAlarmFallingThresholdValStatus OBJECT-TYPE
    SYNTAX      HcValueStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION





            "This object indicates the sign of the data for the falling
            threshold, as defined by the hcAlarmFallingThreshAbsValueLo
            and hcAlarmFallingThreshAbsValueHi objects, as described in
            the HcValueStatus textual convention.

            The enumeration 'valueNotAvailable(1)' is not allowed, and
            the associated hcAlarmStatus object cannot be equal to
            'active(1)' if this object is set to this value.

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 13 }

hcAlarmRisingEventIndex OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The index of the eventEntry that is used when a rising
            threshold is crossed.  The eventEntry identified by a
            particular value of this index is the same as identified by
            the same value of the eventIndex object.  If there is no
            corresponding entry in the eventTable, then no association
            exists.  In particular, if this value is zero, no associated
            event will be generated, as zero is not a valid event index.

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 14 }

hcAlarmFallingEventIndex OBJECT-TYPE
    SYNTAX      Integer32 (0..65535)
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The index of the eventEntry that is used when a falling
            threshold is crossed.  The eventEntry identified by a
            particular value of this index is the same as identified by
            the same value of the eventIndex object.  If there is no
            corresponding entry in the eventTable, then no association
            exists.  In particular, if this value is zero, no associated
            event will be generated, as zero is not a valid event index.

            This object may not be modified if the associated
            hcAlarmStatus object is equal to active(1)."
    ::= { hcAlarmEntry 15 }

hcAlarmValueFailedAttempts OBJECT-TYPE





    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
            "The number of times the associated hcAlarmVariable instance
            was polled on behalf of this hcAlarmEntry, (while in the
            active state) and the value was not available.  This counter
            may experience a discontinuity if the agent restarts,
            indicated by the value of sysUpTime."
    ::= { hcAlarmEntry 16 }

hcAlarmOwner OBJECT-TYPE
    SYNTAX     OwnerString
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The entity that configured this entry and is therefore
            using the resources assigned to it."
    ::= { hcAlarmEntry 17 }

hcAlarmStorageType OBJECT-TYPE
    SYNTAX     StorageType
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
            "The type of non-volatile storage configured for this entry.
            If this object is equal to 'permanent(4)', then the
            associated hcAlarmRisingEventIndex and
            hcAlarmFallingEventIndex objects must be writable."
    ::= { hcAlarmEntry 18 }

hcAlarmStatus OBJECT-TYPE
    SYNTAX      RowStatus
    MAX-ACCESS  read-create
    STATUS      current
    DESCRIPTION
            "The status of this row.

            An entry MUST NOT exist in the active state unless all
            objects in the entry have an appropriate value, as described
            in the description clause for each writable object.

            The hcAlarmStatus object may be modified if the associated
            instance of this object is equal to active(1),
            notInService(2), or notReady(3).  All other writable objects
            may be modified if the associated instance of this object is
            equal to notInService(2) or notReady(3)."
    ::= { hcAlarmEntry 19 }





--
-- Capabilities
--

hcAlarmCapabilities OBJECT-TYPE
    SYNTAX      BITS {
       hcAlarmCreation(0),
       hcAlarmNvStorage(1)
    }
    MAX-ACCESS  read-only
    STATUS      current
    DESCRIPTION
            "An indication of the high capacity alarm capabilities
            supported by this agent.

            If the 'hcAlarmCreation' BIT is set, then this agent allows
            NMS applications to create entries in the hcAlarmTable.

            If the 'hcAlarmNvStorage' BIT is set, then this agent allows
            entries in the hcAlarmTable which will be recreated after a
            system restart, as controlled by the hcAlarmStorageType
            object."
    ::= { hcAlarmCapabilitiesObjects 1 }

--
-- Notifications
--

hcAlarmNotifPrefix OBJECT IDENTIFIER
      ::= { hcAlarmNotifications 0 }

hcRisingAlarm NOTIFICATION-TYPE
    OBJECTS  { hcAlarmVariable,
               hcAlarmSampleType,
               hcAlarmAbsValue,
               hcAlarmValueStatus,
               hcAlarmRisingThreshAbsValueLo,
               hcAlarmRisingThreshAbsValueHi,
               hcAlarmRisingThresholdValStatus,
               hcAlarmRisingEventIndex }
    STATUS   current
    DESCRIPTION
            "The SNMP notification that is generated when a high
            capacity alarm entry crosses its rising threshold and
            generates an event that is configured for sending SNMP
            traps.

            The hcAlarmEntry object instances identified in the OBJECTS





            clause are from the entry that causes this notification to
            be generated."
     ::= { hcAlarmNotifPrefix 1 }

hcFallingAlarm NOTIFICATION-TYPE
    OBJECTS { hcAlarmVariable,
              hcAlarmSampleType,
              hcAlarmAbsValue,
              hcAlarmValueStatus,
              hcAlarmFallingThreshAbsValueLo,
              hcAlarmFallingThreshAbsValueHi,
              hcAlarmFallingThresholdValStatus,
              hcAlarmFallingEventIndex }
    STATUS    current
    DESCRIPTION
            "The SNMP notification that is generated when a high
            capacity alarm entry crosses its falling threshold and
            generates an event that is configured for sending SNMP
            traps.

            The hcAlarmEntry object instances identified in the OBJECTS
            clause are from the entry that causes this notification to
            be generated."
     ::= { hcAlarmNotifPrefix 2 }

--
-- Conformance Section
--

hcAlarmCompliances OBJECT IDENTIFIER ::= { hcAlarmConformance 1 }
hcAlarmGroups      OBJECT IDENTIFIER ::= { hcAlarmConformance 2 }

hcAlarmCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "Describes the requirements for conformance to the High
            Capacity Alarm MIB."
    MODULE  -- this module
        MANDATORY-GROUPS {
                           hcAlarmControlGroup,
                           hcAlarmCapabilitiesGroup,
                           hcAlarmNotificationsGroup
                         }

    MODULE RMON-MIB
        MANDATORY-GROUPS { rmonEventGroup }

    ::= { hcAlarmCompliances 1 }





-- Object Groups

hcAlarmControlGroup OBJECT-GROUP
    OBJECTS {
             hcAlarmInterval,
             hcAlarmVariable,
             hcAlarmSampleType,
             hcAlarmAbsValue,
             hcAlarmValueStatus,
             hcAlarmStartupAlarm,
             hcAlarmRisingThreshAbsValueLo,
             hcAlarmRisingThreshAbsValueHi,
             hcAlarmRisingThresholdValStatus,
             hcAlarmFallingThreshAbsValueLo,
             hcAlarmFallingThreshAbsValueHi,
             hcAlarmFallingThresholdValStatus,
             hcAlarmRisingEventIndex,
             hcAlarmFallingEventIndex,
             hcAlarmValueFailedAttempts,
             hcAlarmOwner,
             hcAlarmStorageType,
             hcAlarmStatus
    }
    STATUS  current
    DESCRIPTION
            "A collection of objects used to configure entries for high
            capacity alarm threshold monitoring purposes."
    ::= { hcAlarmGroups 1 }

hcAlarmCapabilitiesGroup OBJECT-GROUP
    OBJECTS {
             hcAlarmCapabilities
    }
    STATUS  current
    DESCRIPTION
            "A collection of objects used to indicate an agent's high
            capacity alarm threshold monitoring capabilities."
    ::= { hcAlarmGroups 2 }

hcAlarmNotificationsGroup NOTIFICATION-GROUP
    NOTIFICATIONS {
            hcRisingAlarm,
            hcFallingAlarm
    }
    STATUS  current
    DESCRIPTION
            "A collection of notifications to deliver information
            related to a high capacity rising or falling threshold event





            to a management application."
    ::= { hcAlarmGroups 3 }

END


