RADIUS-AUTH-CLIENT-MIB DEFINITIONS ::= BEGIN


   IMPORTS
          MODULE-IDENTITY, OBJECT-TYPE, OBJECT-IDENTITY,
          Counter32, Integer32, Gauge32,
          IpAddress, TimeTicks, mib-2      FROM SNMPv2-SMI
          SnmpAdminString                  FROM SNMP-FRAMEWORK-MIB
          InetAddressType, InetAddress,
          InetPortNumber                   FROM INET-ADDRESS-MIB
          MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF;


   radiusAuthClientMIB MODULE-IDENTITY
          LAST-UPDATED "200608210000Z" -- 21 August 2006
          ORGANIZATION "IETF RADIUS Extensions Working Group."
          CONTACT-INFO
                 " Bernard Aboba
                   Microsoft
                   One Microsoft Way
                   Redmond, WA  98052





                   US
                   Phone: +1 425 936 6605
                   EMail: bernarda@microsoft.com"
          DESCRIPTION
                "The MIB module for entities implementing the client
                 side of the Remote Authentication Dial-In User Service
                 (RADIUS) authentication protocol.  Copyright (C) The
                 Internet Society (2006).  This version of this MIB
                 module is part of RFC 4668; see the RFC itself for
                 full legal notices."
          REVISION "200608210000Z"  --  21 August 2006
          DESCRIPTION
                 "Revised version as published in RFC 4668.  This
                  version obsoletes that of RFC 2618 by deprecating
                  the MIB table containing IPv4-only address formats
                  and defining a new table to add support for version
                  neutral IP address formats.  The remaining MIB objects
                  from RFC 2618 are carried forward into this version."
          REVISION "199906110000Z"    -- 11 Jun 1999
          DESCRIPTION "Initial version as published in RFC 2618."
          ::= { radiusAuthentication 2 }

   radiusMIB OBJECT-IDENTITY
          STATUS  current
          DESCRIPTION
                "The OID assigned to RADIUS MIB work by the IANA."
           ::= { mib-2 67 }

   radiusAuthentication  OBJECT IDENTIFIER ::= {radiusMIB 1}

   radiusAuthClientMIBObjects  OBJECT IDENTIFIER
           ::= { radiusAuthClientMIB 1 }

   radiusAuthClient  OBJECT IDENTIFIER
           ::= { radiusAuthClientMIBObjects 1 }

   radiusAuthClientInvalidServerAddresses OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Response packets
                received from unknown addresses."
         ::= { radiusAuthClient 1 }

   radiusAuthClientIdentifier OBJECT-TYPE
         SYNTAX SnmpAdminString





         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
                "The NAS-Identifier of the RADIUS authentication client.
                 This is not necessarily the same as sysName in MIB II."
         REFERENCE "RFC 2865 section 5.32"
         ::= { radiusAuthClient 2 }

   radiusAuthServerTable OBJECT-TYPE
         SYNTAX     SEQUENCE OF RadiusAuthServerEntry
         MAX-ACCESS not-accessible
         STATUS     deprecated
         DESCRIPTION
               "The (conceptual) table listing the RADIUS authentication
                servers with which the client shares a secret."
         ::= { radiusAuthClient 3 }

   radiusAuthServerEntry OBJECT-TYPE
         SYNTAX     RadiusAuthServerEntry
         MAX-ACCESS not-accessible
         STATUS     deprecated
         DESCRIPTION
               "An entry (conceptual row) representing a RADIUS
                authentication server with which the client shares
                a secret."
         INDEX      { radiusAuthServerIndex }
         ::= { radiusAuthServerTable 1 }

   RadiusAuthServerEntry ::= SEQUENCE {
         radiusAuthServerIndex                           Integer32,
         radiusAuthServerAddress                         IpAddress,
         radiusAuthClientServerPortNumber                Integer32,
         radiusAuthClientRoundTripTime                   TimeTicks,
         radiusAuthClientAccessRequests                  Counter32,
         radiusAuthClientAccessRetransmissions           Counter32,
         radiusAuthClientAccessAccepts                   Counter32,
         radiusAuthClientAccessRejects                   Counter32,
         radiusAuthClientAccessChallenges                Counter32,
         radiusAuthClientMalformedAccessResponses        Counter32,
         radiusAuthClientBadAuthenticators               Counter32,
         radiusAuthClientPendingRequests                   Gauge32,
         radiusAuthClientTimeouts                        Counter32,
         radiusAuthClientUnknownTypes                    Counter32,
         radiusAuthClientPacketsDropped                  Counter32
   }

   radiusAuthServerIndex OBJECT-TYPE
         SYNTAX     Integer32 (1..2147483647)





         MAX-ACCESS not-accessible
         STATUS     deprecated
         DESCRIPTION
                "A number uniquely identifying each RADIUS
                Authentication server with which this client
                communicates."
         ::= { radiusAuthServerEntry 1 }

   radiusAuthServerAddress OBJECT-TYPE
         SYNTAX     IpAddress
         MAX-ACCESS read-only
         STATUS     deprecated
         DESCRIPTION
               "The IP address of the RADIUS authentication server
                referred to in this table entry."
         ::= { radiusAuthServerEntry 2 }

   radiusAuthClientServerPortNumber  OBJECT-TYPE
         SYNTAX Integer32 (0..65535)
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The UDP port the client is using to send requests to
                this server."
         REFERENCE "RFC 2865 section 3"
         ::= { radiusAuthServerEntry 3 }

   radiusAuthClientRoundTripTime  OBJECT-TYPE
         SYNTAX TimeTicks
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The time interval (in hundredths of a second) between
                the most recent Access-Reply/Access-Challenge and the
                Access-Request that matched it from this RADIUS
                authentication server."
         ::= { radiusAuthServerEntry 4 }

   -- Request/Response statistics
   --
   -- TotalIncomingPackets = Accepts + Rejects + Challenges +
   -- UnknownTypes
   --
   -- TotalIncomingPackets - MalformedResponses -
   -- BadAuthenticators - UnknownTypes - PacketsDropped =
   -- Successfully received
   --
   -- AccessRequests + PendingRequests + ClientTimeouts =





   -- Successfully received
   --
   --

   radiusAuthClientAccessRequests OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS Access-Request packets sent
                to this server.  This does not include retransmissions."
         REFERENCE "RFC 2865 section 4.1"
         ::= { radiusAuthServerEntry 5 }

   radiusAuthClientAccessRetransmissions OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS Access-Request packets
                retransmitted to this RADIUS authentication server."
         REFERENCE "RFC 2865 sections 2.5, 4.1"
         ::= { radiusAuthServerEntry 6 }

   radiusAuthClientAccessAccepts OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS Access-Accept packets
                (valid or invalid) received from this server."
         REFERENCE "RFC 2865 section 4.2"
         ::= { radiusAuthServerEntry 7 }

   radiusAuthClientAccessRejects OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS Access-Reject packets
                (valid or invalid) received from this server."
         REFERENCE "RFC 2865 section 4.3"
         ::= { radiusAuthServerEntry  8 }






   radiusAuthClientAccessChallenges OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS Access-Challenge packets
                (valid or invalid) received from this server."
         REFERENCE "RFC 2865 section 4.4"
         ::= { radiusAuthServerEntry 9 }

   -- "Access-Response" includes an Access-Accept, Access-Challenge
   -- or Access-Reject

   radiusAuthClientMalformedAccessResponses OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of malformed RADIUS Access-Response
                packets received from this server.
                Malformed packets include packets with
                an invalid length.  Bad authenticators or
                Message Authenticator attributes or unknown types
                are not included as malformed access responses."
         ::= { radiusAuthServerEntry 10 }

   radiusAuthClientBadAuthenticators OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS Access-Response packets
                containing invalid authenticators or Message
                Authenticator attributes received from this server."
         REFERENCE "RFC 2865 section 3, RFC 2869 section 5.14"
         ::= { radiusAuthServerEntry 11 }

   radiusAuthClientPendingRequests OBJECT-TYPE
         SYNTAX Gauge32
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS Access-Request packets
                destined for this server that have not yet timed out
                or received a response.  This variable is incremented





                when an Access-Request is sent and decremented due to
                receipt of an Access-Accept, Access-Reject,
                Access-Challenge, timeout, or retransmission."
         REFERENCE "RFC 2865 section 2"
         ::= { radiusAuthServerEntry 12 }

   radiusAuthClientTimeouts OBJECT-TYPE
        SYNTAX Counter32
        UNITS "timeouts"
        MAX-ACCESS read-only
        STATUS deprecated
        DESCRIPTION
               "The number of authentication timeouts to this server.
                After a timeout, the client may retry to the same
                server, send to a different server, or
                give up.  A retry to the same server is counted as a
                retransmit as well as a timeout.  A send to a different
                server is counted as a Request as well as a timeout."
                REFERENCE "RFC 2865 section 2, RFC 2869 section 2.3.2"
         ::= { radiusAuthServerEntry  13 }

   radiusAuthClientUnknownTypes OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS packets of unknown type that
                were received from this server on the authentication
                port."
         ::= { radiusAuthServerEntry  14 }

   radiusAuthClientPacketsDropped OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS deprecated
         DESCRIPTION
               "The number of RADIUS packets that were
                received from this server on the authentication port
                and dropped for some other reason."
         ::= { radiusAuthServerEntry  15 }


   -- New MIB Objects in this revision

   radiusAuthServerExtTable OBJECT-TYPE
         SYNTAX     SEQUENCE OF RadiusAuthServerExtEntry





         MAX-ACCESS not-accessible
         STATUS     current
         DESCRIPTION
               "The (conceptual) table listing the RADIUS authentication
                servers with which the client shares a secret."
         ::= { radiusAuthClient 4 }

   radiusAuthServerExtEntry OBJECT-TYPE
         SYNTAX     RadiusAuthServerExtEntry
         MAX-ACCESS not-accessible
         STATUS     current
         DESCRIPTION
               "An entry (conceptual row) representing a RADIUS
                authentication server with which the client shares
                a secret."
         INDEX      { radiusAuthServerExtIndex }
         ::= { radiusAuthServerExtTable 1 }

   RadiusAuthServerExtEntry ::= SEQUENCE {
         radiusAuthServerExtIndex                     Integer32,
         radiusAuthServerInetAddressType              InetAddressType,
         radiusAuthServerInetAddress                  InetAddress,
         radiusAuthClientServerInetPortNumber         InetPortNumber,
         radiusAuthClientExtRoundTripTime             TimeTicks,
         radiusAuthClientExtAccessRequests            Counter32,
         radiusAuthClientExtAccessRetransmissions     Counter32,
         radiusAuthClientExtAccessAccepts             Counter32,
         radiusAuthClientExtAccessRejects             Counter32,
         radiusAuthClientExtAccessChallenges          Counter32,
         radiusAuthClientExtMalformedAccessResponses  Counter32,
         radiusAuthClientExtBadAuthenticators         Counter32,
         radiusAuthClientExtPendingRequests           Gauge32,
         radiusAuthClientExtTimeouts                  Counter32,
         radiusAuthClientExtUnknownTypes              Counter32,
         radiusAuthClientExtPacketsDropped            Counter32,
         radiusAuthClientCounterDiscontinuity         TimeTicks
   }

   radiusAuthServerExtIndex OBJECT-TYPE
         SYNTAX     Integer32 (1..2147483647)
         MAX-ACCESS not-accessible
         STATUS     current
         DESCRIPTION
                "A number uniquely identifying each RADIUS
                Authentication server with which this client
                communicates."
         ::= { radiusAuthServerExtEntry 1 }






   radiusAuthServerInetAddressType OBJECT-TYPE
         SYNTAX     InetAddressType
         MAX-ACCESS read-only
         STATUS     current
         DESCRIPTION
               "The type of address format used for the
                radiusAuthServerInetAddress object."
         ::= { radiusAuthServerExtEntry 2 }

   radiusAuthServerInetAddress OBJECT-TYPE
         SYNTAX     InetAddress
         MAX-ACCESS read-only
         STATUS     current
         DESCRIPTION
               "The IP address of the RADIUS authentication
                server referred to in this table entry, using
                the version-neutral IP address format."
         ::= { radiusAuthServerExtEntry 3 }

   radiusAuthClientServerInetPortNumber  OBJECT-TYPE
         SYNTAX InetPortNumber ( 1..65535 )
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The UDP port the client is using to send requests
                to this server.  The value of zero (0) is invalid."
         REFERENCE "RFC 2865 section 3"
         ::= { radiusAuthServerExtEntry 4 }

   radiusAuthClientExtRoundTripTime  OBJECT-TYPE
         SYNTAX TimeTicks
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The time interval (in hundredths of a second) between
                the most recent Access-Reply/Access-Challenge and the
                Access-Request that matched it from this RADIUS
                authentication server."
         REFERENCE "RFC 2865 section 2"
         ::= { radiusAuthServerExtEntry 5 }

   -- Request/Response statistics
   --
   -- TotalIncomingPackets = Accepts + Rejects + Challenges +
   -- UnknownTypes
   --
   -- TotalIncomingPackets - MalformedResponses -
   -- BadAuthenticators - UnknownTypes - PacketsDropped =





   -- Successfully received
   --
   -- AccessRequests + PendingRequests + ClientTimeouts =
   -- Successfully received
   --
   --

   radiusAuthClientExtAccessRequests OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Request packets sent
                to this server.  This does not include retransmissions.
                This counter may experience a discontinuity when the
                RADIUS Client module within the managed entity is
                reinitialized, as indicated by the current value of
                radiusAuthClientCounterDiscontinuity."
         REFERENCE "RFC 2865 section 4.1"
         ::= { radiusAuthServerExtEntry 6 }

   radiusAuthClientExtAccessRetransmissions OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Request packets
                retransmitted to this RADIUS authentication server.
                This counter may experience a discontinuity when
                the RADIUS Client module within the managed entity
                is reinitialized, as indicated by the current value
                of radiusAuthClientCounterDiscontinuity."
         REFERENCE "RFC 2865 sections 2.5, 4.1"
         ::= { radiusAuthServerExtEntry 7 }

   radiusAuthClientExtAccessAccepts OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Accept packets
                (valid or invalid) received from this server.
                This counter may experience a discontinuity when
                the RADIUS Client module within the managed entity
                is reinitialized, as indicated by the current value





                of radiusAuthClientCounterDiscontinuity."
         REFERENCE "RFC 2865 section 4.2"
         ::= { radiusAuthServerExtEntry 8 }

   radiusAuthClientExtAccessRejects OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Reject packets
                (valid or invalid) received from this server.
                This counter may experience a discontinuity when
                the RADIUS Client module within the managed
                entity is reinitialized, as indicated by the
                current value of
                radiusAuthClientCounterDiscontinuity."
         REFERENCE "RFC 2865 section 4.3"
         ::= { radiusAuthServerExtEntry  9 }

   radiusAuthClientExtAccessChallenges OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Challenge packets
                (valid or invalid) received from this server.
                This counter may experience a discontinuity when
                the RADIUS Client module within the managed
                entity is reinitialized, as indicated by the
                current value of
                radiusAuthClientCounterDiscontinuity."
         REFERENCE "RFC 2865 section 4.4"
         ::= { radiusAuthServerExtEntry 10 }

   -- "Access-Response" includes an Access-Accept, Access-Challenge,
   -- or Access-Reject

   radiusAuthClientExtMalformedAccessResponses OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of malformed RADIUS Access-Response
                packets received from this server.
                Malformed packets include packets with





                an invalid length.  Bad authenticators or
                Message Authenticator attributes or unknown types
                are not included as malformed access responses.
                This counter may experience a discontinuity when
                the RADIUS Client module within the managed entity
                is reinitialized, as indicated by the current value
                of radiusAuthClientCounterDiscontinuity."
         REFERENCE "RFC 2865 sections 3, 4"
         ::= { radiusAuthServerExtEntry 11 }

   radiusAuthClientExtBadAuthenticators OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Response packets
                containing invalid authenticators or Message
                Authenticator attributes received from this server.
                This counter may experience a discontinuity when
                the RADIUS Client module within the managed entity
                is reinitialized, as indicated by the current value
                of radiusAuthClientCounterDiscontinuity."
         REFERENCE "RFC 2865 section 3"
         ::= { radiusAuthServerExtEntry 12 }

   radiusAuthClientExtPendingRequests OBJECT-TYPE
         SYNTAX Gauge32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS Access-Request packets
                destined for this server that have not yet timed out
                or received a response.  This variable is incremented
                when an Access-Request is sent and decremented due to
                receipt of an Access-Accept, Access-Reject,
                Access-Challenge, timeout, or retransmission."
         REFERENCE "RFC 2865 section 2"
         ::= { radiusAuthServerExtEntry 13 }

   radiusAuthClientExtTimeouts OBJECT-TYPE
        SYNTAX Counter32
        UNITS "timeouts"
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
               "The number of authentication timeouts to this server.





                After a timeout, the client may retry to the same
                server, send to a different server, or
                give up.  A retry to the same server is counted as a
                retransmit as well as a timeout.  A send to a different
                server is counted as a Request as well as a timeout.
                This counter may experience a discontinuity when the
                RADIUS Client module within the managed entity is
                reinitialized, as indicated by the current value of
                radiusAuthClientCounterDiscontinuity."
         REFERENCE "RFC 2865 sections 2.5, 4.1"
         ::= { radiusAuthServerExtEntry  14 }

   radiusAuthClientExtUnknownTypes OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS packets of unknown type that
                were received from this server on the authentication
                port.  This counter may experience a discontinuity
                when the RADIUS Client module within the managed
                entity is reinitialized, as indicated by the current
                value of radiusAuthClientCounterDiscontinuity."
                REFERENCE "RFC 2865 section 4"
         ::= { radiusAuthServerExtEntry  15 }

   radiusAuthClientExtPacketsDropped OBJECT-TYPE
         SYNTAX Counter32
         UNITS "packets"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION
               "The number of RADIUS packets that were
                received from this server on the authentication port
                and dropped for some other reason.  This counter may
                experience a discontinuity when the RADIUS Client
                module within the managed entity is reinitialized,
                as indicated by the current value of
                radiusAuthClientCounterDiscontinuity."
         ::= { radiusAuthServerExtEntry  16 }

   radiusAuthClientCounterDiscontinuity OBJECT-TYPE
         SYNTAX TimeTicks
         UNITS "centiseconds"
         MAX-ACCESS read-only
         STATUS current
         DESCRIPTION





               "The number of centiseconds since the last discontinuity
                in the RADIUS Client counters.  A discontinuity may
                be the result of a reinitialization of the RADIUS
                Client module within the managed entity."
         ::= { radiusAuthServerExtEntry 17 }


   -- conformance information

   radiusAuthClientMIBConformance OBJECT IDENTIFIER
           ::= { radiusAuthClientMIB 2 }

   radiusAuthClientMIBCompliances OBJECT IDENTIFIER
           ::= { radiusAuthClientMIBConformance 1 }

   radiusAuthClientMIBGroups OBJECT IDENTIFIER
           ::= { radiusAuthClientMIBConformance 2 }


   -- compliance statements

   radiusAuthClientMIBCompliance MODULE-COMPLIANCE
        STATUS  deprecated
        DESCRIPTION
              "The compliance statement for authentication clients
               implementing the RADIUS Authentication Client MIB.
               Implementation of this module is for IPv4-only
               entities, or for backwards compatibility use with
               entities that support both IPv4 and IPv6."
        MODULE  -- this module
               MANDATORY-GROUPS { radiusAuthClientMIBGroup }

        ::= { radiusAuthClientMIBCompliances 1 }

   radiusAuthClientExtMIBCompliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
              "The compliance statement for authentication
               clients implementing the RADIUS Authentication
               Client IPv6 Extensions MIB.  Implementation of
               this module is for entities that support IPv6,
               or support IPv4 and IPv6."
        MODULE  -- this module
               MANDATORY-GROUPS { radiusAuthClientExtMIBGroup }

        OBJECT radiusAuthServerInetAddressType
        SYNTAX InetAddressType { ipv4(1), ipv6(2) }
        DESCRIPTION





              "An implementation is only required to support
               IPv4 and globally unique IPv6 addresses."

        OBJECT radiusAuthServerInetAddress
        SYNTAX InetAddress ( SIZE (4|16) )
        DESCRIPTION
              "An implementation is only required to support
               IPv4 and globally unique IPv6 addresses."
        ::= { radiusAuthClientMIBCompliances 2 }


   -- units of conformance

   radiusAuthClientMIBGroup OBJECT-GROUP
        OBJECTS { radiusAuthClientIdentifier,
                  radiusAuthClientInvalidServerAddresses,
                  radiusAuthServerAddress,
                  radiusAuthClientServerPortNumber,
                  radiusAuthClientRoundTripTime,
                  radiusAuthClientAccessRequests,
                  radiusAuthClientAccessRetransmissions,
                  radiusAuthClientAccessAccepts,
                  radiusAuthClientAccessRejects,
                  radiusAuthClientAccessChallenges,
                  radiusAuthClientMalformedAccessResponses,
                  radiusAuthClientBadAuthenticators,
                  radiusAuthClientPendingRequests,
                  radiusAuthClientTimeouts,
                  radiusAuthClientUnknownTypes,
                  radiusAuthClientPacketsDropped
               }
        STATUS  deprecated
        DESCRIPTION
              "The basic collection of objects providing management of
               RADIUS Authentication Clients."
        ::= { radiusAuthClientMIBGroups 1 }


   radiusAuthClientExtMIBGroup OBJECT-GROUP
        OBJECTS { radiusAuthClientIdentifier,
                  radiusAuthClientInvalidServerAddresses,
                  radiusAuthServerInetAddressType,
                  radiusAuthServerInetAddress,
                  radiusAuthClientServerInetPortNumber,
                  radiusAuthClientExtRoundTripTime,
                  radiusAuthClientExtAccessRequests,
                  radiusAuthClientExtAccessRetransmissions,
                  radiusAuthClientExtAccessAccepts,





                  radiusAuthClientExtAccessRejects,
                  radiusAuthClientExtAccessChallenges,
                  radiusAuthClientExtMalformedAccessResponses,
                  radiusAuthClientExtBadAuthenticators,
                  radiusAuthClientExtPendingRequests,
                  radiusAuthClientExtTimeouts,
                  radiusAuthClientExtUnknownTypes,
                  radiusAuthClientExtPacketsDropped,
                  radiusAuthClientCounterDiscontinuity
               }
        STATUS  current
        DESCRIPTION
              "The collection of extended objects providing
               management of RADIUS Authentication Clients
               using version-neutral IP address format."
        ::= { radiusAuthClientMIBGroups 2 }

   END


