ATM-ACCOUNTING-INFORMATION-MIB DEFINITIONS ::= BEGIN


IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, OBJECT-IDENTITY,
    mib-2, Integer32, Counter64                   FROM SNMPv2-SMI
    DisplayString, DateAndTime                    FROM SNMPv2-TC
    AtmAddr                                       FROM ATM-TC-MIB;


atmAccountingInformationMIB MODULE-IDENTITY
    LAST-UPDATED "9611052000Z"
    ORGANIZATION "IETF AToM MIB Working Group"
    CONTACT-INFO "
                  Keith McCloghrie
                  Cisco Systems, Inc.
                  170 West Tasman Drive,
                  San Jose CA 95134-1706.
                  Phone: +1 408 526 5260
                  Email: kzm@cisco.com"





    DESCRIPTION
            "The MIB module for identifying items of accounting
            information which are applicable to ATM connections."
    ::= { mib-2 59 }


atmAcctngMIBObjects OBJECT IDENTIFIER ::=
                                        { atmAccountingInformationMIB 1 }


-- Definitions of objects for use in specifying ATM accounting
-- data to be collected

atmAcctngDataObjects OBJECT-IDENTITY
    STATUS      current
    DESCRIPTION
            "This identifier defines a subtree under which various
            objects are defined such that a set of objects to be
            collected as ATM accounting data can be specified as a
            (subtree, list) tuple using this identifier as the subtree."
    ::= { atmAcctngMIBObjects 1 }

-- Objects defined under the atmAcctngDataObjects subtree
--
-- In each case the semantics of the object are interpreted with
-- respect to the creation/storage of an accounting record for a
-- particular connection on a particular interface.

atmAcctngConnectionType OBJECT-TYPE
    SYNTAX      INTEGER { pvc(1),
                          pvp(2),
                          svcIncoming(3),
                          svcOutgoing(4),
                          svpIncoming(5),
                          svpOutgoing(6),
                          spvcInitiator(7),
                          spvcTarget(8),
                          spvpInitiator(9),
                          spvpTarget(10) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The type of connection."
    ::= { atmAcctngDataObjects 1 }

atmAcctngCastType OBJECT-TYPE
    SYNTAX      INTEGER { p2p(1), p2mp(2) }
    MAX-ACCESS  not-accessible





    STATUS      current
    DESCRIPTION
            "An indication of whether the connection is point-to-point
            or point-to-multipoint."
    ::= { atmAcctngDataObjects 2 }

atmAcctngIfName OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "A textual name for the interface on which the data for the
            connection was collected.  If the local SNMP agent supports
            the object ifName, the value of this object must be
            identical to that of ifName in the conceptual row of the
            ifTable corresponding to this interface."
    ::= { atmAcctngDataObjects 3 }

atmAcctngIfAlias OBJECT-TYPE
    SYNTAX      DisplayString
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The 'alias' name for the interface as specified by a
            network manager, e.g., via a management set operation to
            modify the relevant instance of the ifAlias object.  Note
            that in contrast to ifIndex, ifAlias provides a non-volatile
            'handle' for the interface, the value of which is retained
            across agent reboots."
    ::= { atmAcctngDataObjects 4 }

atmAcctngVpi OBJECT-TYPE
    SYNTAX      INTEGER (0..4095)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The VPI used for the connection."
    ::= { atmAcctngDataObjects 5 }

atmAcctngVci OBJECT-TYPE
    SYNTAX      INTEGER (0..65535)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The VCI used for the connection."
    ::= { atmAcctngDataObjects 6 }

atmAcctngCallingParty OBJECT-TYPE





    SYNTAX      AtmAddr
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The connection's calling party.  If unknown (e.g., for a
            PVC), then the value of this object is the zero-length
            string."
    ::= { atmAcctngDataObjects 7 }

atmAcctngCalledParty OBJECT-TYPE
    SYNTAX      AtmAddr
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The connection's called party.  If unknown (e.g., for a
            PVC), then the value of this object is the zero-length
            string."
    ::= { atmAcctngDataObjects 8 }

atmAcctngCallReference OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(0..3))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The connection's call reference value (e.g., from Q.2931).
            If unknown (e.g., for a PVC), then the value of this object
            is the zero-length string."
    ::= { atmAcctngDataObjects 9 }

atmAcctngStartTime OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The time when the connection was established."
    ::= { atmAcctngDataObjects 10 }

atmAcctngCollectionTime OBJECT-TYPE
    SYNTAX      DateAndTime
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The time at which the data in this record was collected."
    ::= { atmAcctngDataObjects 11 }

atmAcctngCollectMode OBJECT-TYPE
    SYNTAX      INTEGER { onRelease(1),
                          periodically(2),





                          onCommand(3) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The reason why this connection data was collected."
    ::= { atmAcctngDataObjects 12 }

atmAcctngReleaseCause OBJECT-TYPE
    SYNTAX      Integer32
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "If the connection data was collected because of the release
            of an SVC, then this is the cause code in the Release
            message for the connection; otherwise, this object has the
            value zero."
    ::= { atmAcctngDataObjects 13 }

atmAcctngServiceCategory OBJECT-TYPE
    SYNTAX      INTEGER { other(1), cbr(2), vbrRt(3), vbrNrt(4),
                          abr(5), ubr(6), unknown(7) }
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The connection's service category."
    ::= { atmAcctngDataObjects 14 }

atmAcctngTransmittedCells OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The number of cells, including OAM cells, transmitted by
            this switch on this connection."
    ::= { atmAcctngDataObjects 15 }

atmAcctngTransmittedClp0Cells OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The number of cells with CLP=0, including OAM cells,
            transmitted by this switch on this connection."
    ::= { atmAcctngDataObjects 16 }

atmAcctngReceivedCells OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  not-accessible





    STATUS      current
    DESCRIPTION
            "The number of cells, including OAM cells, received by this
            switch on this connection."
    ::= { atmAcctngDataObjects 17 }

atmAcctngReceivedClp0Cells OBJECT-TYPE
    SYNTAX      Counter64
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The number of cells with CLP=0, including OAM cells,
            received by this switch on this connection."
    ::= { atmAcctngDataObjects 18 }

atmAcctngTransmitTrafficDescriptorType OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The traffic descriptor type (as defined in RFC 1695 and its
            successors) in the direction in which the switch transmits
            cells on the connection."
    REFERENCE
            "See atmTrafficDescriptorTypes in ATM-MIB.my in RFC 1695 and
            its successors."
    ::= { atmAcctngDataObjects 19 }

atmAcctngTransmitTrafficDescriptorParam1 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The first traffic descriptor parameter in the direction in
            which this switch transmits cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngTransmitTrafficDescriptorType."
    ::= { atmAcctngDataObjects 20 }

atmAcctngTransmitTrafficDescriptorParam2 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The second traffic descriptor parameter in the direction in
            which this switch transmits cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngTransmitTrafficDescriptorType."





    ::= { atmAcctngDataObjects 21 }

atmAcctngTransmitTrafficDescriptorParam3 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The third traffic descriptor parameter in the direction in
            which this switch transmits cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngTransmitTrafficDescriptorType."
    ::= { atmAcctngDataObjects 22 }

atmAcctngTransmitTrafficDescriptorParam4 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The fourth traffic descriptor parameter in the direction in
            which this switch transmits cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngTransmitTrafficDescriptorType."
    ::= { atmAcctngDataObjects 23 }

atmAcctngTransmitTrafficDescriptorParam5 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The fifth traffic descriptor parameter in the direction in
            which this switch transmits cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngTransmitTrafficDescriptorType."
    ::= { atmAcctngDataObjects 24 }

atmAcctngReceiveTrafficDescriptorType OBJECT-TYPE
    SYNTAX      OBJECT IDENTIFIER
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The traffic descriptor type (as defined in RFC 1695 and its
            successors) in the direction in which this switch receives
            cells on this connection."
    REFERENCE
            "See atmTrafficDescriptorTypes in ATM-MIB.my in RFC 1695 and
            its successors."
    ::= { atmAcctngDataObjects 25 }






atmAcctngReceiveTrafficDescriptorParam1 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The first traffic descriptor parameter in the direction in
            which this switch receives cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngReceiveTrafficDescriptorType."
    ::= { atmAcctngDataObjects 26 }

atmAcctngReceiveTrafficDescriptorParam2 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The second traffic descriptor parameter in the direction in
            which this switch receives cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngReceiveTrafficDescriptorType."
    ::= { atmAcctngDataObjects 27 }

atmAcctngReceiveTrafficDescriptorParam3 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The third traffic descriptor parameter in the direction in
            which this switch receives cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngReceiveTrafficDescriptorType."
    ::= { atmAcctngDataObjects 28 }

atmAcctngReceiveTrafficDescriptorParam4 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The fourth traffic descriptor parameter in the direction in
            which this switch receives cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngReceiveTrafficDescriptorType."
    ::= { atmAcctngDataObjects 29 }

atmAcctngReceiveTrafficDescriptorParam5 OBJECT-TYPE
    SYNTAX      INTEGER (0..2147483647)
    MAX-ACCESS  not-accessible
    STATUS      current





    DESCRIPTION
            "The fifth traffic descriptor parameter in the direction in
            which this switch receives cells on this connection.
            Interpretation of this parameter is dependent on the value
            of atmAcctngReceiveTrafficDescriptorType."
    ::= { atmAcctngDataObjects 30 }

atmAcctngCallingPartySubAddress OBJECT-TYPE
    SYNTAX      AtmAddr
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The connection's calling party sub-address.  If the
            connection has no calling party sub-address, or it's value
            is unknown, then the value of this object is the zero-length
            string."
    ::= { atmAcctngDataObjects 31 }

atmAcctngCalledPartySubAddress OBJECT-TYPE
    SYNTAX      AtmAddr
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The connection's called party sub-address.  If the
            connection has no called party sub-address, or it's value is
            unknown, then the value of this object is the zero-length
            string."
    ::= { atmAcctngDataObjects 32 }

atmAcctngRecordCrc16 OBJECT-TYPE
    SYNTAX      OCTET STRING (SIZE(2))
    MAX-ACCESS  not-accessible
    STATUS      current
    DESCRIPTION
            "The value of the CRC-16 checksum (as defined by ISO 3309
            (HDLC) and/or ITU X.25) calculated over the accounting
            record containing this object.

            While the mechanism for calculating/encoding the checksum
            value is specific to the method of encoding the accounting
            record, an accounting record containing this object is
            typically generated by initializing the value of this object
            to the all-zeros string ('0000'H), with the location of
            these zeros being saved.  After generating the record, the
            checksum is calculated over the whole connection record and
            then the all-zeros value is overwritten (at the saved
            location) by the calculated value of the checksum."
    ::= { atmAcctngDataObjects 33 }





END


