FRNETSERV-MIB DEFINITIONS ::= BEGIN


 IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
    Counter32, Integer32,
    TimeTicks                                FROM SNMPv2-SMI
    DisplayString, PhysAddress,
    TimeStamp, RowStatus                     FROM SNMPv2-TC
    MODULE-COMPLIANCE, OBJECT-GROUP          FROM SNMPv2-CONF
    ifIndex, transmission                    FROM RFC-1213;

 frnetservMIB MODULE-IDENTITY
      LAST-UPDATED "9311161200Z"
      ORGANIZATION "IETF Frame Relay Network MIB Working Group"
      CONTACT-INFO
            "   Tracy A. Brown
                Bellcore
                331 Newman Springs Rd.
                Red Bank, NJ 07701 USA

                Tel: 1-908-758-2107
                Fax: 1-908-758-4177
                E-mail: tacox@mail.bellcore.com."
      DESCRIPTION
               "The MIB module to describe generic objects for
               Frame Relay Network Service."
      ::= { transmission 44 }

      IfIndex ::= TEXTUAL-CONVENTION
            STATUS  current
            DESCRIPTION
               "The value of this object identifies the
               interface for which this entry contains
               management information.  The value of this
               object for a particular interface has the same
               value as the ifIndex object, defined in RFC
               1213, for the same interface."
            SYNTAX Integer32

      frnetservObjects  OBJECT IDENTIFIER ::= { frnetservMIB 1 }
      frnetservTraps    OBJECT IDENTIFIER ::= { frnetservMIB 2 }


 -- The Frame Relay Service Logical Port Group

 --  the Frame Relay Logical Port Group





 --  This table is an interface specific addendum
 --  to the generic ifTable from MIB-II.

frLportTable OBJECT-TYPE
 SYNTAX  SEQUENCE OF FrLportEntry
 MAX-ACCESS  not-accessible
 STATUS  current
 DESCRIPTION
         "The Frame Relay Logical Port Information table."
 ::= { frnetservObjects 1 }

frLportEntry OBJECT-TYPE
 SYNTAX  FrLportEntry
 MAX-ACCESS  not-accessible
 STATUS  current
 DESCRIPTION
          "An entry in the Frame Relay Logical Port
          Information table."
 INDEX   { ifIndex }
 ::= { frLportTable 1 }

FrLportEntry ::=
  SEQUENCE {
      frLportNumPlan
          INTEGER,
      frLportContact
          DisplayString,
      frLportLocation
          DisplayString,
      frLportType
          INTEGER,
      frLportAddrDLCILen
          INTEGER,
      frLportVCSigProtocol
          INTEGER,
      frLportVCSigPointer
          OBJECT IDENTIFIER
 }


 frLportNumPlan OBJECT-TYPE
     SYNTAX  INTEGER {
               other(1),
               e164(2),
               x121(3),
               none(4)
             }
     MAX-ACCESS  read-only





     STATUS  current
     DESCRIPTION
             "The value of this object identifies the network
             address numbering plan for this UNI/NNI logical
             port. The network address is the object
             ifPhysAddress. The value none implies that there
             is no ifPhysAddress.  The SNMP proxy-agent will
             return an octet string of zero length for
             ifPhysAddress. The value other means that an
             address has been assigned to this interface, but
             the numbering plan is not enumerated here."
     ::= { frLportEntry 1 }

 frLportContact OBJECT-TYPE
     SYNTAX  DisplayString (SIZE(0..255))
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the network
             contact for this UNI/NNI logical port."
     ::= { frLportEntry 2 }

 frLportLocation OBJECT-TYPE
     SYNTAX  DisplayString (SIZE(0..255))
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the Frame
             Relay network location for this UNI/NNI logical
             port."
     ::= { frLportEntry 3 }

 frLportType OBJECT-TYPE
     SYNTAX  INTEGER {
               uni(1),
               nni(2)
             }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the type of
             network interface for this logical port."
     ::= { frLportEntry 4 }

 frLportAddrDLCILen OBJECT-TYPE
     SYNTAX  INTEGER {
      twoOctets10Bits(1),
      threeOctets10Bits(2),





      threeOctets16Bits(3),
      fourOctets17Bits(4),
      fourOctets23Bits(5)
    }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the Q.922
             Address field length and DLCI length for this
             UNI/NNI logical port."
     ::= { frLportEntry 5 }

 frLportVCSigProtocol OBJECT-TYPE
     SYNTAX  INTEGER {
               none(1),
               lmi(2),
               ansiT1617D(3),
               ansiT1617B(4),
               ccittQ933A(5)
             }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the Local
             In-Channel Signaling Protocol that is used for
             this frame relay UNI/NNI logical port."
     ::= { frLportEntry 6 }

 frLportVCSigPointer OBJECT-TYPE
     SYNTAX  OBJECT IDENTIFIER
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object is used as a pointer to
             the table that contains the Local In-Channel
             Signaling Protocol parameters and errors for this
             UNI/NNI logical port.  See the Frame Relay
             Management VC Signaling Parameters and Errors
             Group."
     ::= { frLportEntry 7 }


 -- the Frame Relay Management VC Signaling Group

 -- This Group contains managed objects for the
 -- Local In-Channel Signaling Parameters and
 -- for signaling errors.






 frMgtVCSigTable OBJECT-TYPE
     SYNTAX  SEQUENCE OF FrMgtVCSigEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The Frame Relay Management VC Signaling
             Parameters and Errors table."
     ::= { frnetservObjects 2 }

 frMgtVCSigEntry OBJECT-TYPE
     SYNTAX  FrMgtVCSigEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "An entry in the Frame Relay Management VC
             Signaling Parameters Errors table."
     INDEX   { ifIndex }
     ::= { frMgtVCSigTable 1 }

 FrMgtVCSigEntry ::=
     SEQUENCE {
         frMgtVCSigProced
             INTEGER,
         frMgtVCSigUserN391
             INTEGER,
         frMgtVCSigUserN392
             INTEGER,
         frMgtVCSigUserN393
             INTEGER,
         frMgtVCSigUserT391
             INTEGER,
         frMgtVCSigNetN392
             INTEGER,
         frMgtVCSigNetN393
             INTEGER,
         frMgtVCSigNetT392
             INTEGER,
         frMgtVCSigNetnN4
             INTEGER,
         frMgtVCSigNetnT3
             INTEGER,
         frMgtVCSigUserLinkRelErrors
             Counter32,
         frMgtVCSigUserProtErrors
             Counter32,
         frMgtVCSigUserChanInactive
             Counter32,
         frMgtVCSigNetLinkRelErrors





             Counter32,
         frMgtVCSigNetProtErrors
             Counter32,
         frMgtVCSigNetChanInactive
             Counter32
 }


 frMgtVCSigProced OBJECT-TYPE
     SYNTAX  INTEGER {
               u2nnet(1),
               bidirect(2)
             }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the Local
             In-Channel Signaling Procedure that is used for
             this UNI/NNI logical port.  The UNI/NNI logical
             port can be performing only user-to-network
             network-side procedures or bidirectional
             procedures."
     ::= { frMgtVCSigEntry 1 }

 frMgtVCSigUserN391 OBJECT-TYPE
     SYNTAX  INTEGER (1..255)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the User-side
             N391 full status polling cycle value for this
             UNI/NNI logical port.  If the logical port is not
             performing user-side procedures, then this value
             is equal to noSuchName. This object applies to
             Q.933 Annex A and T1.617 Annex D."
     DEFVAL { 6 }
     ::= { frMgtVCSigEntry 2 }

 frMgtVCSigUserN392 OBJECT-TYPE
     SYNTAX  INTEGER (1..10)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the User-side
             N392 error threshold value for this UNI/NNI
             logical port.  If the logical port is not
             performing user-side procedures, then this value
             is equal to noSuchName. This object applies to





             Q.933 Annex A and T1.617 Annex D."
     DEFVAL { 3 }
     ::= { frMgtVCSigEntry 3 }

 frMgtVCSigUserN393 OBJECT-TYPE
     SYNTAX  INTEGER (1..10)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the User-side
             N393 monitored events count value for this UNI/NNI
             logical port.  If the logical port is not
             performing user-side procedures, then this value
             is equal to noSuchName. This object applies to
             Q.933 Annex A and T1.617 Annex D."
     DEFVAL { 4 }
     ::= { frMgtVCSigEntry 4 }

 frMgtVCSigUserT391 OBJECT-TYPE
     SYNTAX  INTEGER (5..30)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the User-side
             T391 link integrity verification polling timer
             value for this UNI/NNI logical port.  If the
             logical port is not performing user-side
             procedures, then this value is equal to
             noSuchName. This object applies to Q.933 Annex A
             and T1.617 Annex D."
     DEFVAL { 10 }
     ::= { frMgtVCSigEntry 5 }

 frMgtVCSigNetN392 OBJECT-TYPE
     SYNTAX  INTEGER (1..10)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the Network-
             side N392 error threshold value (nN2 for LMI) for
             this UNI/NNI logical port.  If the logical port is
             not performing network-side procedures, then this
             value is equal to noSuchName. This object applies
             to Q.933 Annex A, T1.617 Annex D and LMI."
     DEFVAL { 3 }
     ::= { frMgtVCSigEntry 6 }

 frMgtVCSigNetN393 OBJECT-TYPE





     SYNTAX  INTEGER (1..10)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the Network-
             side N393 monitored events count value (nN3 for
             LMI) for this UNI/NNI logical port.  If the
             logical port is not performing network-side
             procedures, then this value is equal to
             noSuchName. This object applies to Q.933 Annex A,
             T1.617 Annex D and LMI."
     DEFVAL { 4 }
     ::= { frMgtVCSigEntry 7 }

 frMgtVCSigNetT392 OBJECT-TYPE
     SYNTAX  INTEGER (5..30)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the Network-
             side T392 polling verification timer value (nT2
             for LMI)  for this UNI/NNI logical port.  If the
             logical port is not performing network-side
             procedures, then this value is equal to
             noSuchName. This object applies to Q.933 Annex A,
             T1.617 Annex D and LMI."
     DEFVAL { 15 }
     ::= { frMgtVCSigEntry 8 }

 frMgtVCSigNetnN4 OBJECT-TYPE
     SYNTAX  INTEGER (5..5)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the Network-
             side nN4 maximum status enquires received value
             for this UNI/NNI logical port.  If the logical
             port is not performing network-side procedures or
             is not performing LMI procedures, then this value
             is equal to noSuchName. This object applies only
             to LMI and always has a value of 5."
     ::= { frMgtVCSigEntry 9 }

 frMgtVCSigNetnT3 OBJECT-TYPE
     SYNTAX  INTEGER (5 | 10 | 15 | 20 | 25 | 30)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION





             "The value of this object identifies the Network-
             side nT3 timer (for nN4 status enquires received)
             value for this UNI/NNI logical port.  If the
             logical port is not performing network-side
             procedures or is not performing LMI procedures,
             then this value is equal to noSuchName. This
             object applies only to LMI."
     DEFVAL { 20 }
     ::= { frMgtVCSigEntry 10 }

 frMgtVCSigUserLinkRelErrors OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of user-side local in-channel
             signaling link reliability errors (i.e., non-
             receipt of Status/Status Enquiry messages or
             invalid sequence numbers in a Link Integrity
             Verification Information Element) for this UNI/NNI
             logical port.  If the logical port is not
             performing user-side procedures, then this value
             is equal to noSuchName."
     ::= { frMgtVCSigEntry 11 }

 frMgtVCSigUserProtErrors OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of user-side local in-channel
             signaling protocol errors (i.e., protocol
             discriminator, message type, call reference, and
             mandatory information element errors) for this
             UNI/NNI logical port.  If the logical port is not
             performing user-side procedures, then this value
             is equal to noSuchName."
     ::= { frMgtVCSigEntry 12 }

 frMgtVCSigUserChanInactive OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of times the user-side channel was
             declared inactive (i.e., N392 errors in N393
             events) for this UNI/NNI logical port. If the
             logical port is not performing user-side





             procedures, then this value is equal to
             noSuchName."
     ::= { frMgtVCSigEntry 13 }

 frMgtVCSigNetLinkRelErrors OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of network-side local in-channel
             signaling link reliability errors (i.e., non-
             receipt of Status/Status Enquiry messages or
             invalid sequence numbers in a Link Integrity
             Verification Information Element) for this UNI/NNI
             logical port.  If the logical port is not
             performing network-side procedures, then this
             value is equal to noSuchName."
     ::= { frMgtVCSigEntry 14 }

 frMgtVCSigNetProtErrors OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of network-side local in-channel
             signaling protocol errors (i.e., protocol
             discriminator, message type, call reference, and
             mandatory information element errors) for this
             UNI/NNI logical port.  If the logical port is not
             performing network-side procedures, then this
             value is equal to noSuchName."
     ::= { frMgtVCSigEntry 15 }

 frMgtVCSigNetChanInactive OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of times the network-side channel was
             declared inactive (i.e., N392 errors in N393
             events) for this UNI/NNI logical port.  If the
             logical port is not performing network-side
             procedures, then this value is equal to
             noSuchName."
     ::= { frMgtVCSigEntry 16 }








 -- The PVC End-Point Group

 -- This table is used to identify the traffic parameters
 -- for a bi-directional PVC segment end-point, and it also
 -- provides statistics for a PVC segment
 -- end-point.

 -- A PVC segment end-point is identified by a UNI/NNI
 -- logical port index value and DLCI index value.

 -- If the Frame Relay service provider allows
 -- the Frame Relay CNM subscriber to create, modify
 -- or delete PVCs using SNMP, then this table is used to identify
 -- and reserve
 -- the requested traffic parameters of each
 -- PVC segment end-point.  The Connection table
 -- is used to "connect" the end-points together.
 -- Not all implementations will support the
 -- capability of creating/modifying/deleting
 -- PVCs using SNMP as a feature of Frame Relay
 -- CNM service.

 -- Uni-directional PVCs are modeled with zero
 -- valued traffic parameters in one of the
 -- directions (In or Out direction) in this table.

 -- To create a PVC, the following procedures
 -- shall be followed:
 -- 1). Create the entries for the PVC segment endpoints in the
 --     frPVCEndptTable by specifying the traffic parameters
 --     for the bi-directional PVC segment endpoints.
 --     As shown in the figure, a point-to-point PVC has
 --     two endpoints, thus two entries in this table.
 --     Uni-directional PVCs are modeled
 --     with zero valued traffic parameters in one
 --     direction; all the `In' direction parameters
 --     for one Frame Relay PVC End-point or
 --     all the `Out' direction
 --     parameters for the other Frame Relay PVC
 --     End-point.













 --     In    ____________________________________ Out
 --    >>>>>>|                                   |>>>>>>>>
 --    ______| Frame Relay Network               |__________
 --     Out  |                                   |  In
 --    <<<<<<|                                   |<<<<<<<<
 --          |___________________________________|
 --  Frame Relay PVC                            Frame Relay
 --   End-point                                 PVC  End-point

 -- 2). Go to the Frame Relay Connection Group.
 --

 -- The Frame Relay PVC End-point Table

 frPVCEndptTable OBJECT-TYPE
     SYNTAX  SEQUENCE OF FrPVCEndptEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The Frame Relay PVC End-Point table.  This table
             is used to model a PVC end-point.  This table
             contains the traffic parameters and statistics for
             a PVC end-point."
     ::= { frnetservObjects 3 }

 frPVCEndptEntry OBJECT-TYPE
     SYNTAX  FrPVCEndptEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "An entry in the Frame Relay PVC Endpoint table."
     INDEX   { ifIndex, frPVCEndptDLCIIndex }
     ::= { frPVCEndptTable 1 }

 FrPVCEndptEntry ::=
     SEQUENCE {
         frPVCEndptDLCIIndex
             Integer32,
         frPVCEndptInMaxFrameSize
             Integer32,
         frPVCEndptInBc
             Integer32,
         frPVCEndptInBe
             Integer32,
         frPVCEndptInCIR
            Integer32,
         frPVCEndptOutMaxFrameSize
             Integer32,





         frPVCEndptOutBc
             Integer32,
         frPVCEndptOutBe
             Integer32,
         frPVCEndptOutCIR
             Integer32,
         frPVCEndptConnectIdentifier
             Integer32,
         frPVCEndptRowStatus
             RowStatus,
         frPVCEndptRcvdSigStatus
             INTEGER,
         frPVCEndptInFrames
             Counter32,
         frPVCEndptOutFrames
             Counter32,
         frPVCEndptInDEFrames
             Counter32,
         frPVCEndptInExcessFrames
             Counter32,
         frPVCEndptOutExcessFrames
             Counter32,
         frPVCEndptInDiscards
             Counter32,
         frPVCEndptInOctets
             Counter32,
         frPVCEndptOutOctets
             Counter32
     }


 frPVCEndptDLCIIndex OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the DLCI
             value for this PVC end-point."
     ::= { frPVCEndptEntry 1 }

 frPVCEndptInMaxFrameSize OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object is the size in octets of
             the largest frame relay information field for this
             PVC end-point in the ingress direction (into the





             frame relay network).  The value of
             frPVCEndptInMaxFrameSize must be less than or
             equal to the corresponding ifMtu for this Frame
             Relay UNI/NNI logical port."
     ::= { frPVCEndptEntry 2 }

 frPVCEndptInBc OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the
             committed burst size (Bc) parameter (measured in
             bits) for this PVC end-point in the ingress
             direction (into the frame relay network)."
     ::= { frPVCEndptEntry 3 }

 frPVCEndptInBe OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the excess
             burst size (Be) parameter (measured in bits) for
             this PVC end-point in the ingress direction (into
             the frame relay network)."
     ::= { frPVCEndptEntry 4 }

 frPVCEndptInCIR OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the
             committed information rate (CIR) parameter
             (measured in bits per second) for this PVC end-
             point in the ingress direction (into the frame
             relay network)."
     ::= { frPVCEndptEntry 5 }

 frPVCEndptOutMaxFrameSize OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object is the size in octets of
             the largest frame relay information field for this
             PVC end-point in the egress direction (out of the





             frame relay network).  The value of
             frPVCEndptOutMaxFrameSize must be less than or
             equal to the corresponding ifMtu for this Frame
             Relay UNI/NNI logical port."
     ::= { frPVCEndptEntry 6 }

 frPVCEndptOutBc OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the
             committed burst size (Bc) parameter (measured in
             bits) for this PVC end-point in the egress
             direction (out of the frame relay network)."
     ::= { frPVCEndptEntry 7 }

 frPVCEndptOutBe OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the excess
             burst size (Be) parameter (measured in bits) for
             this PVC end-point in the egress direction (out of
             the frame relay network)."
     ::= { frPVCEndptEntry 8 }

 frPVCEndptOutCIR OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the
             committed information rate (CIR) parameter
             (measured in bits per second) for this PVC end-
             point in the egress direction (out of the frame
             relay network)."
     ::= { frPVCEndptEntry 9 }

 frPVCEndptConnectIdentifier OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "This object is used to associate PVC end-points
             as being part of one PVC segment connection.  This
             value of this object is equal to the value of





             frPVCConnectIndex, which is used as one of the
             indices into the frPVCConnectTable.  The value of
             this object is provided by the agent, after the
             associated entries in the frPVCConnectTable have
             been created."
     ::= { frPVCEndptEntry 10 }

 frPVCEndptRowStatus OBJECT-TYPE
     SYNTAX  RowStatus
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "This object is used to create new rows in this
             table, modify existing rows, and to delete
             existing rows.  To create a new PVC, the entries
             for the PVC segment end-points in the
             frPVCEndptTable must first be created.  Next, the
             frPVCConnectTable is used to associate the Frame
             Relay PVC segment end-points.  In order for the
             manager to have the necessary error diagnostics,
             the frPVCEndptRowStatus object must initially be
             set to `createAndWait'.  While the
             frPVCEndptRowStatus object is in the
             `createAndWait' state, the manager can set each
             columnar object and get the necessary error
             diagnostics.  The frPVCEndptRowStatus object may
             not be set to `active' unless the following
             columnar objects exist in this row:
             frPVCEndptInMaxFrameSize, frPVCEndptInBc,
             frPVCEndptInBe, frPVCEndptInCIR,
             frPVCEndptOutMaxFrameSize, frPVCEndptOutBc,
             frPVCEndptOutBe, and frPVCEndptOutCIR."
     ::= { frPVCEndptEntry 11 }

 frPVCEndptRcvdSigStatus OBJECT-TYPE
     SYNTAX  INTEGER {
               deleted(1),
               active(2),
               inactive(3),
               none(4)
             }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the PVC
             status received via the local in-channel signaling
             procedures for this PVC end-point.  This object is
             only pertinent for interfaces that perform the





             bidirectional procedures.  For user-to-network
             network side procedures, the value of this object
             should be none."
     ::= { frPVCEndptEntry 12 }

 frPVCEndptInFrames OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of frames received by the network
             (ingress) for this PVC end-point. This includes
             any frames discarded by the network due to
             submitting more than Bc + Be data or due to any
             network congestion recovery procedures."
     ::= { frPVCEndptEntry 13 }

 frPVCEndptOutFrames OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of frames sent by the network (egress)
             regardless of whether they are Bc or Be frames for
             this PVC end-point."
     ::= { frPVCEndptEntry 14 }

 frPVCEndptInDEFrames OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of frames received by the network
             (ingress) with the DE bit set to (1) for this PVC
             end-point."
     ::= { frPVCEndptEntry 15 }

 frPVCEndptInExcessFrames OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of frames received by the network
             (ingress) for this PVC end-point which were
             treated as excess traffic.  Frames which are sent
             to the network with DE set to zero are treated as
             excess when more than Bc bits are submitted to the
             network during the Committed Information Rate





             Measurement Interval (Tc).  Excess traffic may or
             may not be discarded at the ingress if more than
             Bc + Be bits are submitted to the network during
             Tc.  Traffic discarded at the ingress is not
             recorded in frPVCEndptInExcessFrames.  Frames
             which are sent to the network with DE set to one
             are also treated as excess traffic."
     ::= { frPVCEndptEntry 16 }

 frPVCEndptOutExcessFrames OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of frames sent by the network (egress)
             for this PVC end-point which were treated as
             excess traffic.  (The DE bit may be set to one.)"
     ::= { frPVCEndptEntry 17 }

 frPVCEndptInDiscards OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of frames received by the the network
             (ingress) that were discarded due to traffic
             enforcement for this PVC end-point."
     ::= { frPVCEndptEntry 18 }

 frPVCEndptInOctets OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The number of octets received by the network
             (ingress) for this PVC end-point.  This counter
             should only count octets from the beginning of the
             frame relay header field to the end of user data.
             If the network supporting Frame Relay can not
             count octets, then this count should be an
             approximation."
     ::= { frPVCEndptEntry 19 }

 frPVCEndptOutOctets OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION





             "The number of octets sent by the network (egress)
             for this PVC end-point.  This counter should only
             count octets from the beginning of the frame relay
             header field to the end of user data.  If the
             network supporting Frame Relay can not count
             octets, then this count should be an
             approximation."
     ::= { frPVCEndptEntry 20 }


 -- The Frame Relay PVC Connection Group

 -- The Frame Relay PVC Connection Group
 -- is used to model the bi-directional
 -- PVC segment flows;
 -- point-to-point PVCs, point-to-multipoint
 -- PVCs, and multipoint-to-multipoint
 -- PVCs.

 -- This table has read-create access and
 -- is used to associate PVC end-points
 -- together as belonging to one connection.
 -- The frPVCConnectIndex is used to associate
 -- all the bi-directional flows.
 -- Not all implementations will support the
 -- capability of creating/modifying/deleting
 -- PVCs using SNMP as a feature of Frame Relay
 -- CNM service.

 -- Once the entries in the frPVCEndptTable
 -- are created, the following step are used
 -- to associate the PVC end-points as belonging
 -- to one PVC connection:
 -- 1). Obtain a unique frPVCConnectIndex
 --     using the frPVCConnectIndexValue object.
 -- 2). Connect the PVC segment endpoints together
 --     with the applicable frPVCConnectIndex value
 --     obtained via
 --     frPVCConnectIndexValue.
 --     The entries in this table are created by using
 --     the frPVCConnectRowStatus object.
 -- 3). The agent will provide the value of the
 --     corresponding instances of
 --     frPVCEndptConnectIdentifier with the
 --     the frPVCConnectIndex value.
 -- 4). Set frPVCConnectAdminStatus to `active' in all
 --     rows for this PVC segment to
 --     turn the PVC on.





 -- For example, the Frame Relay PVC Connection Group
 -- models a bi-directional, point-to-point PVC segment
 -- as one entry in this table.

 -- Frame Relay Network                  Frame Relay Network
 --  Low Port ____________________________________ High Port
 --          |                                   |
 --    ______| >> from low to high PVC flow   >> |____________
 --          | << from high to low PVC flow   << |
 --          |___________________________________|
 --

 -- The terms low and high are chosen to represent numerical
 -- ordering of a PVC segment's endpoints for representation
 -- in this table.  That is, the endpoint with the lower value
 -- of ifIndex is termed 'low', while the opposite endpoint
 -- of the segment is termed 'high'.
 -- This terminology is to provide directional information;
 -- for example the frPVCConnectL2hOperStatus and
 -- frPVCConnectH2lOperStatus as illustrated above.

 -- If the Frame Relay Connection table is used to model
 -- a unidirectional PVC, then one direction (either from low to high
 -- or from high to low) has its Operational Status equal to down.

 -- A PVC segment is a portion of a PVC
 -- that traverses one Frame Relay Network, and
 -- a PVC segment is identified
 -- by its two end-points (UNI/NNI logical port index
 -- value and DLCI index value)
 -- through one Frame Relay Network.


 frPVCConnectIndexValue OBJECT-TYPE
     SYNTAX  INTEGER (0..2147483647)
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "This object contains an appropriate value to be
             used for frPVCConnectIndex when creating entries
             in the frPVCConnectTable.  The value 0 indicates
             that no unassigned entries are available.  To
             obtain the frPVCConnectIndex value for a new
             entry, the manager issues a management protocol
             retrieval operation to obtain the current value of
             this object.  After each retrieval, the agent
             should modify the value to the next unassigned
             index."





     ::= { frnetservObjects 4 }

 --  The Frame Relay PVC Connection Table

 frPVCConnectTable OBJECT-TYPE
     SYNTAX  SEQUENCE OF FrPVCConnectEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The Frame Relay PVC Connect table.  A bi-
             directional PVC segment is modeled as one entry in
             this table."
     ::= { frnetservObjects 5 }

 frPVCConnectEntry OBJECT-TYPE
     SYNTAX  FrPVCConnectEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "An entry in the Frame Relay PVC Connect table.
             This entry is used to model a PVC segment in two
             directions."
     INDEX { frPVCConnectIndex,
             frPVCConnectLowIfIndex, frPVCConnectLowDLCIIndex,
             frPVCConnectHighIfIndex, frPVCConnectHighDLCIIndex }
     ::= { frPVCConnectTable 1 }

 FrPVCConnectEntry ::=
     SEQUENCE {
         frPVCConnectIndex
             Integer32,
         frPVCConnectLowIfIndex
             IfIndex,
         frPVCConnectLowDLCIIndex
             Integer32,
         frPVCConnectHighIfIndex
             IfIndex,
         frPVCConnectHighDLCIIndex
             Integer32,
         frPVCConnectAdminStatus
             INTEGER,
         frPVCConnectL2hOperStatus
             INTEGER,
         frPVCConnectH2lOperStatus
             INTEGER,
         frPVCConnectL2hLastChange
             TimeStamp,
         frPVCConnectH2lLastChange





             TimeStamp,
         frPVCConnectRowStatus
             RowStatus
 }

 frPVCConnectIndex OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the
             frPVCConnectIndexValue obtained to uniquely
             identify this PVC segment connection."
     ::= { frPVCConnectEntry 1 }

 frPVCConnectLowIfIndex OBJECT-TYPE
     SYNTAX  IfIndex
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to MIB II's
             ifIndex value of the UNI/NNI logical port for this
             PVC segment.  The term low implies that this PVC
             segment end-point has the numerically lower
             ifIndex value than the connected/associated PVC
             segment end-point.  If the value is equal to zero,
             then this logical port is not a Frame Relay
             UNI/NNI logical port."
     ::= { frPVCConnectEntry 2 }

 frPVCConnectLowDLCIIndex OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the DLCI
             value for this end-point of the PVC segment.  If
             the value is equal to zero, then this endpoint of
             the PVC segment is not a Frame Relay connection."
     ::= { frPVCConnectEntry 3 }

 frPVCConnectHighIfIndex OBJECT-TYPE
     SYNTAX  IfIndex
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to MIB II's
             ifIndex value for the UNI/NNI logical port for





             this PVC segment.  The term high implies that this
             PVC segment end-point has the numerically higher
             ifIndex value than the connected/associated PVC
             segment end-point."
     ::= { frPVCConnectEntry 4 }

 frPVCConnectHighDLCIIndex OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the egress
             DLCI value for this end-point of the PVC segment."
     ::= { frPVCConnectEntry 5 }

 frPVCConnectAdminStatus OBJECT-TYPE
     SYNTAX  INTEGER {
               active(1),
               inactive(2),
               testing(3)
             }
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the desired
             administrative status of this bi-directional PVC
             segment.  The active state means the PVC segment
             is currently operational; the inactive state means
             the PVC segment is currently not operational; the
             testing state means the PVC segment is currently
             undergoing a test.  This state is set by an
             administrative entity.  This value affects the PVC
             status indicated across the ingress NNI/UNI of
             both end-points of the bi-directional PVC segment.
             When a PVC segment connection is created using
             this table, this object is initially set to
             `inactive'.  After the frPVCConnectRowStatus
             object is set to `active' (and the
             corresponding/associated entries in the
             frPVCEndptTable have their frPVCEndptRowStatus
             object set to `active'), the
             frPVCConnectAdminStatus object may be set to
             `active' to turn on the PVC segment connection."
     ::= { frPVCConnectEntry 6 }

 frPVCConnectL2hOperStatus OBJECT-TYPE
     SYNTAX  INTEGER {
               active(1),





               inactive(2),
               testing(3),
               unknown(4)
             }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the current
             operational status of the PVC segment connection
             in one direction; (i.e., in the low to high
             direction).  The active state means it is
             currently operational; the inactive state means it
             is currently not operational; the testing state
             means it is currently undergoing a test; the
             unknown state means the status of it currently can
             not be determined.  This value affects the PVC
             status indicated across the ingress NNI/UNI (low
             side) of the PVC segment."
     ::= { frPVCConnectEntry 7 }

 frPVCConnectH2lOperStatus OBJECT-TYPE
     SYNTAX  INTEGER {
               active(1),
               inactive(2),
               testing(3),
               unknown(4)
             }
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object identifies the current
             operational status of the PVC segment connection
             in one direction; (i.e., in the high to low
             direction).  The active state means it is
             currently operational; the inactive state means it
             is currently not operational; the testing state
             means it is currently undergoing a test; the
             unknown state means the status of it currently can
             not be determined.  This value affects the PVC
             status indicated across the ingress NNI/UNI (high
             side) of the PVC segment."
     ::= { frPVCConnectEntry 8 }

 frPVCConnectL2hLastChange OBJECT-TYPE
     SYNTAX  TimeStamp
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION





             "The value of MIB II's sysUpTime object at the
             time this PVC segment entered its current
             operational state in the low to high direction.
             If the current state was entered prior to the last
             re-initialization of the proxy-agent, then this
             object contains a zero value."
     ::= { frPVCConnectEntry 9 }

 frPVCConnectH2lLastChange OBJECT-TYPE
     SYNTAX  TimeStamp
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of MIB II's sysUpTime object at the
             time this PVC segment entered its current
             operational state in the high to low direction.
             If the current state was entered prior to the last
             re-initialization of the proxy-agent, then this
             object contains a zero value."
     ::= { frPVCConnectEntry 10 }

 frPVCConnectRowStatus OBJECT-TYPE
     SYNTAX  RowStatus
     MAX-ACCESS  read-create
     STATUS  current
     DESCRIPTION
             "The status of this entry in the
             frPVCConnectTable.  This variable is used to
             create new connections for the PVC end-points and
             to change existing connections of the PVC end-
             points.  This object must be initially set to
             `createAndWait'.  In this state, the agent checks
             the parameters in the associated entries in the
             frPVCEndptTable to verify that the PVC end-points
             can be connected (i.e., the In parameters for one
             PVC end-point are equal to the Out parameters for
             the other PVC end-point).  This object can not be
             set to `active' unless the following columnar
             objects exist in this row: frPVCConnectAdminStatus
             and frPVCConnectGenericPointer.  The agent also
             supplies the associated value of frPVCConnectIndex
             for the frPVCEndptConnectIdentifier instances.  To
             turn on a PVC segment connection, the
             frPVCConnectAdminStatus is set to `active'."
     ::= { frPVCConnectEntry 11 }








 -- The Frame Relay Accounting Groups

 -- The groups are the following:
 --  Accounting on a PVC basis
 --  Accounting on an Interface/Logical Port basis

 -- The Accounting on a Frame Relay PVC basis Group

 -- The accounting information is collected for a PVC
 -- segment end-point.

 frAccountPVCTable OBJECT-TYPE
     SYNTAX  SEQUENCE OF FrAccountPVCEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The Frame Relay Accounting PVC table.  This table
             is used to perform accounting on a PVC segment
             end-point basis."
     ::= { frnetservObjects 6 }

 frAccountPVCEntry OBJECT-TYPE
     SYNTAX  FrAccountPVCEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "An entry in the Frame Relay Accounting PVC
             table."
     INDEX   { ifIndex, frAccountPVCDLCIIndex }
     ::= { frAccountPVCTable 1 }

 FrAccountPVCEntry ::=
     SEQUENCE {
         frAccountPVCDLCIIndex
             Integer32,
         frAccountPVCSegmentSize
             Integer32,
         frAccountPVCInSegments
             Counter32,
         frAccountPVCOutSegments
             Counter32
     }


 frAccountPVCDLCIIndex OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  not-accessible
     STATUS  current





     DESCRIPTION
             "The value of this object is equal to the DLCI
             value for this PVC segment end-point."
     ::= { frAccountPVCEntry 1 }

 frAccountPVCSegmentSize OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the Segment
             Size for this PVC segment end-point."
     ::= { frAccountPVCEntry 2 }

 frAccountPVCInSegments OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the number
             of segments received by this PVC segment end-
             point."
     ::= { frAccountPVCEntry 3 }

  frAccountPVCOutSegments OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the number
             of segments sent by this PVC segment end-point."
     ::= { frAccountPVCEntry 4 }


 -- The Accounting on a Frame Relay Logical Port basis Group


 frAccountLportTable OBJECT-TYPE
     SYNTAX  SEQUENCE OF FrAccountLportEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "The Frame Relay Accounting Logical Port table.
             This table is used to perform accounting on a
             UNI/NNI Logical Port basis."
     ::= { frnetservObjects 7 }

 frAccountLportEntry OBJECT-TYPE





     SYNTAX  FrAccountLportEntry
     MAX-ACCESS  not-accessible
     STATUS  current
     DESCRIPTION
             "An entry in the Frame Relay Accounting Logical
             Port table."
     INDEX   { ifIndex }
     ::= { frAccountLportTable 1 }

 FrAccountLportEntry ::=
     SEQUENCE {
         frAccountLportSegmentSize
             Integer32,
         frAccountLportInSegments
             Counter32,
         frAccountLportOutSegments
             Counter32
     }


 frAccountLportSegmentSize OBJECT-TYPE
     SYNTAX  Integer32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the Segment
             Size for this UNI/NNI logical port."
     ::= { frAccountLportEntry 1 }

 frAccountLportInSegments OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the number
             of segments received by this UNI/NNI logical
             port."
     ::= { frAccountLportEntry 2 }

 frAccountLportOutSegments OBJECT-TYPE
     SYNTAX  Counter32
     MAX-ACCESS  read-only
     STATUS  current
     DESCRIPTION
             "The value of this object is equal to the number
             of segments sent by this UNI/NNI logical port."
     ::= { frAccountLportEntry 3 }






 -- Frame Relay Network Service TRAPS

 frPVCConnectStatusChange  NOTIFICATION-TYPE
     OBJECTS { frPVCConnectIndex,
               frPVCConnectLowIfIndex, frPVCConnectLowDLCIIndex,
               frPVCConnectHighIfIndex, frPVCConnectHighDLCIIndex,
               frPVCConnectL2hOperStatus, frPVCConnectH2lOperStatus,
               frPVCEndptRcvdSigStatus }
     STATUS  current
     DESCRIPTION
             "This trap indicates that the indicated PVC has
             changed state.  This trap is not sent if an FR-UNI
             changes state; a linkDown or linkUp trap should be
             sent instead."
     ::= { frnetservTraps 1 }


 -- Conformance Information

 frnetservConformance  OBJECT IDENTIFIER ::= { frnetservMIB 3 }

 frnetservGroups       OBJECT IDENTIFIER ::= { frnetservConformance 1 }
 frnetservCompliances  OBJECT IDENTIFIER ::= { frnetservConformance 2 }

 -- Compliance Statements

 frnetservCompliance MODULE-COMPLIANCE
       STATUS  current
       DESCRIPTION
         "The compliance statement for SNMPv2 entities
         which have Frame Relay Network Service Interfaces."

       MODULE -- this module
           MANDATORY-GROUPS { frnetservLportGroup,
                              frnetservMgtVCSigGroup,
                              frnetservPVCEndptGroup,
                              frnetservPVCConnectGroup }

           GROUP       frnetservAccountPVCGroup
           DESCRIPTION
                 "This group is optional for Frame Relay interfaces.
                 It is
                 mandatory if and only if accounting is performed
                 on a PVC
                 basis this
                 Frame Relay interface."

           GROUP       frnetservAccountLportGroup





           DESCRIPTION
                 "This group is optional for Frame Relay interfaces.
                 It is
                 mandatory if and only if accounting is
                 performed on a
                 logical port basis this
                 Frame Relay interface."

           OBJECT      frPVCEndptInMaxFrameSize
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCEndptInBc
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCEndptInBe
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCEndptInCIR
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCEndptOutMaxFrameSize
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCEndptOutBc
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCEndptOutBe
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION





                 "Write access is not required."

           OBJECT      frPVCEndptOutCIR
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCEndptConnectIdentifier
           SYNTAX      Integer32
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCEndptRowStatus
           SYNTAX      INTEGER { active(1) }  -- subset of RowStatus
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required, and only one of the
                 six enumerated values for the RowStatus textual
                 convention need be supported, specifically:
                 active(1)."

           OBJECT      frPVCConnectAdminStatus
           SYNTAX      INTEGER {
                         active(1),
                         inactive(2),
                         testing(3)
                        }
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCConnectGenericPointer
           SYNTAX      OBJECT IDENTIFIER
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required."

           OBJECT      frPVCConnectRowStatus
           SYNTAX      INTEGER { active(1) }  -- subset of RowStatus
           MIN-ACCESS  read-only
           DESCRIPTION
                 "Write access is not required, and only one of the
                 six enumerated values for the RowStatus textual
                 convention need be supported, specifically:
                 active(1)."
       ::= { frnetservCompliances 1 }





 -- Units of Conformance

 frnetservLportGroup  OBJECT-GROUP
       OBJECTS { frLportNumPlan, frLportContact, frLportLocation,
                 frLportType,
                 frLportAddrDLCILen, frLportVCSigProtocol,
                 frLportVCSigPointer }
       STATUS  current
       DESCRIPTION
             "A collection of objects providing information applicable
             to a Frame Relay Logical Port."
       ::= { frnetservGroups 1 }

 frnetservMgtVCSigGroup  OBJECT-GROUP
       OBJECTS { frMgtVCSigProced,
                 frMgtVCSigUserN391,
                 frMgtVCSigUserN392,
                 frMgtVCSigUserN393,
                 frMgtVCSigUserT391,
                 frMgtVCSigNetN392,
                 frMgtVCSigNetN393,
                 frMgtVCSigNetT392,
                 frMgtVCSigNetnN4,
                 frMgtVCSigNetnT3,
                 frMgtVCSigUserLinkRelErrors,
                 frMgtVCSigUserProtErrors,
                 frMgtVCSigUserChanInactive,
                 frMgtVCSigNetLinkRelErrors,
                 frMgtVCSigNetProtErrors,
                 frMgtVCSigNetChanInactive }
       STATUS  current
       DESCRIPTION
             "A collection of objects providing information
             applicable to the
             Local In-Channel Signaling Procedures used for a
             UNI/NNI logical port."
       ::= { frnetservGroups 2 }

 frnetservPVCEndptGroup  OBJECT-GROUP
       OBJECTS { frPVCConnectIndexValue,
                 frPVCEndptInMaxFrameSize, frPVCEndptInBc,
                 frPVCEndptInBe, frPVCEndptInCIR,
                 frPVCEndptOutMaxFrameSize, frPVCEndptOutBc,
                 frPVCEndptOutBe, frPVCEndptOutCIR,
                 frPVCEndptConnectIdentifier, frPVCEndptRowStatus,
                 frPVCEndptRcvdSigStatus, frPVCEndptInFrames,
                 frPVCEndptOutFrames, frPVCEndptInDEFrames,
                 frPVCEndptInExcessFrames, frPVCEndptOutExcessFrames,





                 frPVCEndptInDiscards,
                 frPVCEndptInOctets, frPVCEndptOutOctets }
       STATUS  current
       DESCRIPTION
             "A collection of objects providing information application
             to a Frame Relay PVC end-point."
       ::= { frnetservGroups 3 }

 frnetservPVCConnectGroup  OBJECT-GROUP
       OBJECTS { frPVCConnectAdminStatus, frPVCConnectL2hOperStatus,
                 frPVCConnectH2lOperStatus, frPVCConnectL2hLastChange,
                 frPVCConnectH2lLastChange,
                 frPVCConnectGenericPointer, frPVCConnectRowStatus }
       STATUS  current
       DESCRIPTION
             "A collection of objects providing information applicable
             to a Frame Relay PVC connection."
       ::= { frnetservGroups 4 }

 frnetservAccountPVCGroup  OBJECT-GROUP
       OBJECTS { frAccountPVCSegmentSize, frAccountPVCInSegments,
                 frAccountPVCOutSegments }
       STATUS  current
       DESCRIPTION
             "A collection of objects providing accounting
             information application
             to a Frame Relay PVC end-point."
       ::= { frnetservGroups 5 }

 frnetservAccountLportGroup  OBJECT-GROUP
       OBJECTS { frAccountLportSegmentSize, frAccountLportInSegments,
                 frAccountLportOutSegments }
       STATUS  current
       DESCRIPTION
             "A collection of objects providing accounting
             information application
             to a Frame Relay logical port."
       ::= { frnetservGroups 6 }


 END











