RFC1298-MIB DEFINITIONS ::= BEGIN


    IMPORTS
      enterprises         FROM RFC1155-SMI;

      novell              OBJECT IDENTIFIER ::= { enterprises 23 }
      transportDomains    OBJECT IDENTIFIER ::= { novell 7 }

      ipxTransportDomain  OBJECT IDENTIFIER ::= { transportDomains 1 }

    -- Authoritatively names the IPX Transport Domain

    IpxTransportAddress ::= OCTET STRING (SIZE (12))

    -- A textual convention denoting a transport service address in
    -- the ipxTransportDomain.  An IpxTransportAddress is 12 octets
    -- long and comprises 3 fields, each in network-byte (high-low)
    -- order.

    -- The first field is 4 octets long and contains the network
    -- number.

    -- The next field is 6 octets long and contains the physical
    -- address of the node.  Since IPX can run over a variety of
    -- subnet architectures, the physical node address may not
    -- require all 6 octets.  As specified in [2], the physical
    -- node address will occupy the least significant portion of
    -- the field and the most significant octets should be set
    -- to zero.

    -- The last field is 2 octets long and contains the socket
    -- number.

 END


