PW-ATM-MIB DEFINITIONS ::= BEGIN


    IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Counter32, Unsigned32, mib-2
          FROM SNMPv2-SMI

    MODULE-COMPLIANCE, OBJECT-GROUP
          FROM SNMPv2-CONF

    TruthValue, RowStatus, RowPointer
          FROM SNMPv2-TC

    PerfCurrentCount, PerfIntervalCount
          FROM PerfHist-TC-MIB

    InterfaceIndex
          FROM IF-MIB

    pwIndex
          FROM PW-STD-MIB

    AtmVpIdentifier, AtmVcIdentifier
          FROM ATM-TC-MIB;

      pwAtmMIB MODULE-IDENTITY
      LAST-UPDATED "200906160000Z"  -- 16 June 2009
      ORGANIZATION "Pseudowire Emulation Edge-to-Edge (PWE3)
                    Working Group"
      CONTACT-INFO
          "Thomas D. Nadeau
           Postal: BT
                   BT Centre
                   81 Newgate Street
                   London  EC1A 7AJ
                   United Kingdom





           Email:  tom.nadeau@bt.com

           Orly Nicklass
           Postal: RADVISION Ltd.
                  24 Raul Wallenberg
                  Tel Aviv, Israel
           Email: orlyn@radvision.com

           Discussion and general questions should be posed to
           the PWE3 Working Group (pwe3@ietf.org)."

      DESCRIPTION
          "This MIB contains managed object definitions for
           pseudowire emulation of ATM over Packet Switched
           Networks (PSNs).

           This MIB supplements the PW-STD-MIB module.
           The PW-STD-MIB contains structures and MIB associations
           generic to pseudowire (PW) emulation.  PW-specific
           MIBs (such as this) contain config and stats for specific
           PW types.

           Copyright (c) 2009 IETF Trust and the persons identified as
           authors of the code.  All rights reserved.

           Redistribution and use in source and binary forms, with or
           without modification, are permitted provided that the
           following conditions are met:

           - Redistributions of source code must retain the above
             copyright notice, this list of conditions and the
             following disclaimer.

           - Redistributions in binary form must reproduce the above
             copyright notice, this list of conditions and the
             following disclaimer in the documentation and/or other
             materials provided with the distribution.

           - Neither the name of Internet Society, IETF or IETF Trust,
             nor the names of specific contributors, may be used to
             endorse or promote products derived from this software
             without specific prior written permission.

           THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
           CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED WARRANTIES,
           INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF
           MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
           DISCLAIMED.  IN NO EVENT SHALL THE COPYRIGHT OWNER OR





           CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL,
           SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT
           NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES;
           LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION)
           HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN
           CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE
           OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS
           SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

           This version of this MIB module is part of RFC 5605;
           see the RFC itself for full legal notices.
           "

      -- Revision history.

      REVISION "200906160000Z"  -- 16 June 2009
      DESCRIPTION "Initial version published as RFC 5605."

         ::= { mib-2 183 }

    -- Top-level components of this MIB

    pwAtmNotifications OBJECT IDENTIFIER ::= { pwAtmMIB 0 }
    pwAtmObjects       OBJECT IDENTIFIER ::= { pwAtmMIB 1 }
    pwAtmConformance   OBJECT IDENTIFIER ::= { pwAtmMIB 2 }

-- ATM PW PSN Bound(Outbound) Table for 1 to 1 connection

pwAtmOutboundTable OBJECT-TYPE
    SYNTAX    SEQUENCE OF PwAtmOutboundEntry
    MAX-ACCESS        not-accessible
    STATUS            current
    DESCRIPTION
        "This table specifies the information for an ATM PW to
        be carried over the PSN in the outbound direction.  An
        entry is created in this table for every entry in
        the pwTable with a pwType equal to one of the following:
        atmAal5SduVcc(2), atmCell1to1Vcc(12), atmCell1to1Vpc(13)
        or atmAal5PduVcc(14), or atmTransparent(3)."
    ::= { pwAtmObjects 1 }

pwAtmOutboundEntry OBJECT-TYPE
    SYNTAX        PwAtmOutboundEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A row in this table represents an ATM PW that needs to be
         adapted and carried over the PSN.  This table is indexed by





         pwIndex from pwTable.  Unless otherwise specified, all
         writeable objects in this table MUST NOT be changed after
         row activation in the generic pwTable, and values must
         persist after reboot."
    REFERENCE
      "See [PWMIB]."

    INDEX { pwIndex }
    ::= { pwAtmOutboundTable 1 }

PwAtmOutboundEntry ::= SEQUENCE {
      pwAtmOutboundAtmIf                InterfaceIndex,
      pwAtmOutboundVpi                  AtmVpIdentifier,
      pwAtmOutboundVci                  AtmVcIdentifier,
      pwAtmOutboundTrafficParamDescr    RowPointer,
      pwAtmOutboundRowStatus            RowStatus
      }

pwAtmOutboundAtmIf OBJECT-TYPE
    SYNTAX        InterfaceIndex
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The ATM Interface that receives cells from the ATM
        network."
    ::= { pwAtmOutboundEntry 1 }

pwAtmOutboundVpi OBJECT-TYPE
    SYNTAX        AtmVpIdentifier
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "VPI value of this ATM PW.  The value may indicate the
        translated value when egress generates new VPI."
    ::= { pwAtmOutboundEntry 2 }

pwAtmOutboundVci OBJECT-TYPE
    SYNTAX        AtmVcIdentifier
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "VCI value of this ATM PW.  The value may indicate the
        translated value when egress generates new VCI."
    ::= { pwAtmOutboundEntry 3 }

pwAtmOutboundTrafficParamDescr OBJECT-TYPE
    SYNTAX        RowPointer
    MAX-ACCESS    read-create





    STATUS        current
    DESCRIPTION
        "This object represents a pointer to an ATM
         traffic-parameter-specific row in either a private or
         standard table that will be employed while receiving
         cells from the ATM network.  This row should contain a
         set of self-consistent ATM traffic parameters including
         the ATM traffic service category.
         A value of 0.0 indicates Best Effort."
     ::= { pwAtmOutboundEntry 4 }

pwAtmOutboundRowStatus OBJECT-TYPE
    SYNTAX        RowStatus
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "This object is used to create, modify, or delete a row in
         this table.  Unless otherwise specified, all writeable
         objects in this table MUST NOT be changed after row
         activation as explained in the pwAtmOutboundEntry. "
    ::= { pwAtmOutboundEntry 5 }

-- End of ATM PW Outbound Table

-- ATM PW CE Bound(Inbound) Table for 1 to 1 mode

pwAtmInboundTable OBJECT-TYPE
    SYNTAX    SEQUENCE OF PwAtmInboundEntry
    MAX-ACCESS        not-accessible
    STATUS            current
    DESCRIPTION
        "This table specifies the information for an ATM PW in the
         inbound direction."
    ::= { pwAtmObjects 3 }

pwAtmInboundEntry OBJECT-TYPE
    SYNTAX    PwAtmInboundEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A row in this table represents an ATM PW that needs to be
         sent into the ATM network after reconstructing cells from
         packets received from a PSN.  This table is indexed by
         pwIndex from pwTable.  An entry is created in this table
         for every entry in the pwTable with a
         pwType equal to one of the following:
         atmAal5SduVcc(2), atmCell1to1Vcc(12), atmCell1to1Vpc(13),
         atmAal5PduVcc(14), or atmTransparent(3).  Unless otherwise





         specified, all writeable objects in this table MUST NOT
         be changed after row activation in the generic pwTable,
         and values must persist after reboot."
    REFERENCE
      "See [PWMIB]."

    INDEX { pwIndex }
    ::= { pwAtmInboundTable 1 }

PwAtmInboundEntry ::= SEQUENCE {
      pwAtmInboundAtmIf                 InterfaceIndex,
      pwAtmInboundVpi                   AtmVpIdentifier,
      pwAtmInboundVci                   AtmVcIdentifier,
      pwAtmInboundTrafficParamDescr     RowPointer,
      pwAtmInboundRowStatus             RowStatus
          }

pwAtmInboundAtmIf OBJECT-TYPE
    SYNTAX        InterfaceIndex
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The ATM Interface that sends cells into the ATM network
        after reconstructing cells from packets received from
        a PSN."
    ::= { pwAtmInboundEntry 1 }

pwAtmInboundVpi OBJECT-TYPE
    SYNTAX        AtmVpIdentifier
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "VPI value of this ATM PW.
         If the pwType is atmTransparent, then the value will
         be set to zero."
        ::= { pwAtmInboundEntry 2 }

pwAtmInboundVci OBJECT-TYPE
    SYNTAX        AtmVcIdentifier
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "VCI value of this ATM PW.
         If the pwType is atmTransparent, atmCell1to1Vpc, or
         atmCellNto1Vpc, then the value will be set to zero."
        ::= { pwAtmInboundEntry 3 }

pwAtmInboundTrafficParamDescr OBJECT-TYPE





    SYNTAX        RowPointer
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "This object represents a pointer to an ATM traffic-parameter-
         specific row in either a private or standard table that will
         be employed while transmitting into the ATM network.  This
         table contains a set of self-consistent ATM traffic parameters
         including the ATM traffic service category.  A value of 0.0
         indicates Best Effort."

        ::= { pwAtmInboundEntry 4 }

pwAtmInboundRowStatus OBJECT-TYPE
    SYNTAX        RowStatus
    MAX-ACCESS    read-create
    STATUS        current
        DESCRIPTION
        "This object is used to create, modify, or delete a row in
         this table.  Unless otherwise specified, all writeable
         objects in this table MUST NOT be changed after row
         activation as explained in the pwAtmInboundEntry. "
        ::= { pwAtmInboundEntry 5 }

-- End of ATM PW Inbound Table

--Generic ATM PW table for all types of ATM PW connection.

pwAtmCfgTable OBJECT-TYPE
    SYNTAX    SEQUENCE OF PwAtmCfgEntry
    MAX-ACCESS        not-accessible
    STATUS            current
    DESCRIPTION
        "This table specifies generic information for an ATM PW
         to be carried over PSN in any mode."
    ::= { pwAtmObjects 5 }

    pwAtmCfgEntry OBJECT-TYPE
    SYNTAX        PwAtmCfgEntry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
         "This table contains a set of parameters for
         the ATM PW that needs to be adapted and carried
         over the PSN.  This table is indexed by pwIndex from
         pwTable.  An entry is created for every new ATM
         type associated pwIndex in the pwTable.  Unless
         otherwise specified, all read-write objects in





         this table MAY be changed when the PW is defined
         as not active, and all RW objects values must
         persist after reboot."
    REFERENCE
      "See [PWMIB]."

    INDEX { pwIndex }
    ::= { pwAtmCfgTable 1 }

PwAtmCfgEntry ::= SEQUENCE {
        pwAtmCfgMaxCellConcatenation       Unsigned32,
        pwAtmCfgFarEndMaxCellConcatenation Unsigned32,
        pwAtmCfgTimeoutMode                INTEGER,
        pwAtmClpQosMapping                 TruthValue
                }

pwAtmCfgMaxCellConcatenation OBJECT-TYPE
     SYNTAX        Unsigned32 (1..29)
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION
         "The maximum number of ATM cells that can be
          concatenated into one PW packet towards the PSN.
          In a non-LDP or other signaling protocol environment,
          this object MAY be changed at anytime, but traffic
          might be interrupted; otherwise, it may be changed
          when PW is not active."
    ::= { pwAtmCfgEntry 1 }

pwAtmCfgFarEndMaxCellConcatenation OBJECT-TYPE
     SYNTAX        Unsigned32 (1..29)
     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION
         "The maximum number of ATM cells that can be
          concatenated into one PW packet towards PSN as reported by
          the far end.  If there is no LDP in use, the object will
          either return a value of 0 or allow setting it for calculating
          protocol overhead."
    ::= { pwAtmCfgEntry 2 }

pwAtmCfgTimeoutMode OBJECT-TYPE
     SYNTAX        INTEGER
                        {
                         notApplicable (1),
                         disabled      (2),
                         enabled       (3)
                        }





     MAX-ACCESS    read-write
     STATUS        current
     DESCRIPTION
         "This object determines whether or not a packet can be
          transmitted to the PSN based on timeout expiration
          for collecting cells.  The actual handling of the
          timeout is implementation-specific; as such,
          this object may be changed at any time under proper
          consideration of the traffic interruption effect."
    ::= { pwAtmCfgEntry 3 }

pwAtmClpQosMapping OBJECT-TYPE
    SYNTAX        TruthValue
    MAX-ACCESS    read-write
    STATUS        current
    DESCRIPTION
        "This object indicates whether the Cell Loss Priority
         (CLP) bits should be considered when setting the
         value in the Quality-of-Service fields of the
         encapsulating protocol (e.g., EXP fields of the
         MPLS Label Stack).  Selecting True allows the drop
         precedence to be preserved across the PSN.  In
         transparent cell transport, the value of this object
         MUST be false(2); in other cases, it can be changed
         at any time."
    REFERENCE
      "See section 12 of [ATMENCAP]."
    ::= { pwAtmCfgEntry 4 }

-- Device capable of implementing N:1, 1:1, and transparent cell
-- mode assumes to support the N:1 table for all
-- modes with respective applicable setting.
-- In such implementation, user can create an entry for either
-- 1:1 or transparent cell transport modes only
-- in pwAtmInboundNto1Table. The side effect of such
-- will be an automatic create of the respective line in the
-- pwAtmOutboundNto1Table.

-- ATM PW Outbound Table for N to 1 connection

pwAtmOutboundNto1Table OBJECT-TYPE
    SYNTAX    SEQUENCE OF PwAtmOutboundNto1Entry
    MAX-ACCESS        not-accessible
    STATUS            current
    DESCRIPTION
        "This table specifies the information for an ATM PW to
        be carried over the PSN in the outbound direction.  Up to
        N entries can be created in this table for every





        entry in the pwTable with a pwType equal to:
        atmCellNto1Vcc(9) or atmCellNto1Vpc(10).
        An entry can be created only when the VP/VC are known.
        A single entry will be created in this table for every
        entry in the pwTable with a pwType equal to
        one of the following: atmCell1to1Vcc(12),
        atmCell1to1Vpc(13), atmAal5PduVcc(14),
        atmAal5SduVcc(2), or atmTransparent(3).
        "
    ::= { pwAtmObjects 6 }

pwAtmOutboundNto1Entry OBJECT-TYPE
    SYNTAX        PwAtmOutboundNto1Entry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A row in this table represents an ATM PW that needs to be
         adapted and carried over PSN.  This table is indexed by
         pwIndex from pwTable and the ATM interface with VPL/VCLs.
         In atmTransparent(3), Vpi and VCi will be 0xFFFF
         during set operation.
         Unless otherwise specified, all read-create objects in this
         table MUST NOT be changed after row activation
         and SHOULD remain unchanged after reboot."
    INDEX { pwIndex, pwAtmOutboundNto1AtmIf ,
                        pwAtmOutboundNto1Vpi,
                        pwAtmOutboundNto1Vci  }
    ::= { pwAtmOutboundNto1Table 1 }

PwAtmOutboundNto1Entry ::= SEQUENCE {
      pwAtmOutboundNto1AtmIf                    InterfaceIndex,
      pwAtmOutboundNto1Vpi                      AtmVpIdentifier,
      pwAtmOutboundNto1Vci                      AtmVcIdentifier,
      pwAtmOutboundNto1RowStatus                RowStatus,
      pwAtmOutboundNto1TrafficParamDescr        RowPointer,
      pwAtmOutboundNto1MappedVpi                AtmVpIdentifier,
      pwAtmOutboundNto1MappedVci                AtmVcIdentifier
     }

pwAtmOutboundNto1AtmIf OBJECT-TYPE
    SYNTAX        InterfaceIndex
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The ATM Interface that receives cells from the ATM network."
    ::= { pwAtmOutboundNto1Entry 1 }

pwAtmOutboundNto1Vpi OBJECT-TYPE





    SYNTAX        AtmVpIdentifier
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "VPI value of this ATM PW.  In atmTransparent(3),
         Vpi will be the equivalent of 0xFFFF."
    ::= { pwAtmOutboundNto1Entry 2 }

pwAtmOutboundNto1Vci OBJECT-TYPE
    SYNTAX        AtmVcIdentifier
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "VCI value of this ATM PW.  In atmTransparent(3), or
         the VP case, the value will be the equivalent of
         0xFFFF."
    ::= { pwAtmOutboundNto1Entry 3 }

pwAtmOutboundNto1RowStatus OBJECT-TYPE
    SYNTAX        RowStatus
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "This object is used to create, modify or delete a row in
         this table."
    ::= { pwAtmOutboundNto1Entry 4 }

pwAtmOutboundNto1TrafficParamDescr OBJECT-TYPE
    SYNTAX        RowPointer
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "This object represents a pointer to an ATM traffic-parameter-
         specific row in either private or standard table that will
         be employed while receiving cells from the ATM network.
         This table should contain a set
         of self-consistent ATM traffic parameters including the ATM
         traffic service category.  A value of 0.0 indicates Best
         Effort."

    ::= { pwAtmOutboundNto1Entry 5 }

pwAtmOutboundNto1MappedVpi         OBJECT-TYPE
    SYNTAX        AtmVpIdentifier
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The egress-generated VPI value of this ATM PW.  The





        entry is valid for PW type of atmCellNto1Vcc(9),
        atmCellNto1Vpc(10), atmCell1to1Vcc(12), or
        atmCell1to1Vpc(13).  In other types, the value will be the
        equivalent of 0xFFFF.  Value MAY be changed when the
        PW is defined as not active. "
    ::= { pwAtmOutboundNto1Entry 6 }

pwAtmOutboundNto1MappedVci      OBJECT-TYPE
    SYNTAX        AtmVcIdentifier
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The egress-generated VCI value of this ATM PW.  The
        entry is valid for PW type of atmCellNto1Vcc(9),
        atmCellNto1Vpc(10), atmCell1to1Vcc(12), or
        atmCell1to1Vpc(13.  In the VP case or other types, the
        value will be the equivalent of 0xFFFF.
        Value MAY be changed when the PW is defined
        as not active."
    ::= { pwAtmOutboundNto1Entry 7 }

-- ATM PW Inbound Table for N to 1 connection

pwAtmInboundNto1Table OBJECT-TYPE
    SYNTAX    SEQUENCE OF PwAtmInboundNto1Entry
    MAX-ACCESS        not-accessible
    STATUS            current
    DESCRIPTION
        "This table specifies the information for an ATM PW to
        be carried over PSN in the Inbound direction.  Up to
        N entries can be created in this table for every
        entry in the pwTable with a pwType equal to:
        atmCellNto1Vcc(9) or atmCellNto1Vpc(10).
        An entry can be created only when the VP/VC are known.
        A single entry will be created in this table for every
        entry in the pwTable with a pwType equal to
        one of the following: atmCell1to1Vcc(12),
        atmCell1to1Vpc(13), atmAal5PduVcc(14),
        atmAal5SduVcc(2), or atmTransparent(3)."
    ::= { pwAtmObjects 7 }

pwAtmInboundNto1Entry OBJECT-TYPE
    SYNTAX        PwAtmInboundNto1Entry
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "A row in this table represents an ATM PW that needs to be
         adapted and carried over PSN.  This table is indexed by





         pwIndex from pwTable and the ATM interface with VPL/VCLs.
         In atmTransparent(3), Vpi and VCi will be 0xFFFF
         during set operation.
         Unless otherwise specified, all Read-Create objects in this
         table MUST NOT be changed after row activation
         and SHOULD remain unchanged after reboot."
    INDEX { pwIndex, pwAtmInboundNto1AtmIf ,
                        pwAtmInboundNto1Vpi,
                        pwAtmInboundNto1Vci
                        }
    ::= { pwAtmInboundNto1Table 1 }

PwAtmInboundNto1Entry ::= SEQUENCE {
      pwAtmInboundNto1AtmIf                InterfaceIndex,
      pwAtmInboundNto1Vpi                  AtmVpIdentifier,
      pwAtmInboundNto1Vci                  AtmVcIdentifier,
      pwAtmInboundNto1RowStatus            RowStatus,
      pwAtmInboundNto1TrafficParamDescr    RowPointer,
      pwAtmInboundNto1MappedVpi            AtmVpIdentifier,
      pwAtmInboundNto1MappedVci            AtmVcIdentifier
    }

pwAtmInboundNto1AtmIf OBJECT-TYPE
    SYNTAX        InterfaceIndex
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "The ATM Interface that receives cells from the ATM network."
    ::= { pwAtmInboundNto1Entry 1 }

pwAtmInboundNto1Vpi OBJECT-TYPE
    SYNTAX        AtmVpIdentifier
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "VPI value of this ATM PW.  In atmTransparent(3),
         Vpi will be the equivalent of 0xFFFF."
    ::= { pwAtmInboundNto1Entry 2 }

pwAtmInboundNto1Vci OBJECT-TYPE
    SYNTAX        AtmVcIdentifier
    MAX-ACCESS    not-accessible
    STATUS        current
    DESCRIPTION
        "VCI value of this ATM PW.  In atmTransparent(3), or
         the VP case, the value will be the equivalent of
         0xFFFF."
    ::= { pwAtmInboundNto1Entry 3 }





pwAtmInboundNto1RowStatus OBJECT-TYPE
    SYNTAX        RowStatus
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "This object is used to create, modify, or delete a row in
        this table."
    ::= { pwAtmInboundNto1Entry 4 }

pwAtmInboundNto1TrafficParamDescr OBJECT-TYPE
    SYNTAX        RowPointer
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "This object represents a pointer to an ATM traffic-parameter-
         specific row in either a private or standard table that will
         be employed while receiving cells from the ATM network.
         This table should contain a set
         of self-consistent ATM traffic parameters including the ATM
         traffic service category.  A value of 0.0 indicates Best
         Effort."

    ::= { pwAtmInboundNto1Entry 5 }

pwAtmInboundNto1MappedVpi    OBJECT-TYPE
    SYNTAX        AtmVpIdentifier
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The generated VPI value of this ATM PW.  The
        entry is valid for PW type of atmCellNto1Vcc(9),
        atmCellNto1Vpc(10), atmCell1to1Vcc(12), or
        atmCell1to1Vpc(13).  In other types, the value will be the
        equivalent of 0xFFFF.  Value MAY be changed when the
        PW is defined as not active."
    ::= { pwAtmInboundNto1Entry 6 }

pwAtmInboundNto1MappedVci     OBJECT-TYPE
    SYNTAX        AtmVcIdentifier
    MAX-ACCESS    read-create
    STATUS        current
    DESCRIPTION
        "The generated VCI value of this ATM PW.  The
        entry is valid for PW type of atmCellNto1Vcc(9),
        atmCellNto1Vpc(10), atmCell1to1Vcc(12), or
        atmCell1to1Vpc(13.  In the VP case or other types, the
        value will be the equivalent of 0xFFFF.
        Value MAY be changed when the





        PW is defined as not active."
    ::= { pwAtmInboundNto1Entry 7 }

-- ATM PW Outbound Perf Table

-- The following supplement the counters presented in the
-- PW generic MIB

-- ATM PW Performance Current Table.

pwAtmPerfCurrentTable OBJECT-TYPE
  SYNTAX        SEQUENCE OF PwAtmPerfCurrentEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
      "The current 15-minute interval counts are in
       this table.
       This table provides performance information per ATM PW."
  ::= { pwAtmObjects 8 }

pwAtmPerfCurrentEntry OBJECT-TYPE
  SYNTAX        PwAtmPerfCurrentEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
      "An entry in this table is created by the agent for every
       pwAtmCfgTable entry.  After 15 minutes, the contents of this
       table entry are copied to a new entry in the
       pwAtmPerfInterval table and the counts in this entry
       are reset to zero."
  INDEX  { pwIndex }
  ::= { pwAtmPerfCurrentTable 1 }

PwAtmPerfCurrentEntry ::= SEQUENCE {
     pwAtmPerfCurrentMissingPkts    PerfCurrentCount,
     pwAtmPerfCurrentPktsReOrder    PerfCurrentCount,
     pwAtmPerfCurrentPktsMisOrder   PerfCurrentCount,
     pwAtmPerfCurrentPktsTimeout    PerfCurrentCount,
     pwAtmPerfCurrentCellsXmit      PerfCurrentCount,
     pwAtmPerfCurrentCellsDropped   PerfCurrentCount,
     pwAtmPerfCurrentCellsReceived  PerfCurrentCount,
     pwAtmPerfCurrentUnknownCells   PerfCurrentCount
  }

pwAtmPerfCurrentMissingPkts OBJECT-TYPE
  SYNTAX        PerfCurrentCount
  MAX-ACCESS    read-only
  STATUS        current





  DESCRIPTION
      "Number of missing packets (as detected via control word
       sequence number gaps)."
  ::= { pwAtmPerfCurrentEntry 1 }

pwAtmPerfCurrentPktsReOrder OBJECT-TYPE
  SYNTAX        PerfCurrentCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets detected out of sequence (via control
       word sequence number), but successfully re-ordered.
       Note: some implementations may not support this feature."
  ::= { pwAtmPerfCurrentEntry 2 }

pwAtmPerfCurrentPktsMisOrder OBJECT-TYPE
  SYNTAX        PerfCurrentCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets detected out of order (via control word
       sequence numbers)."
   ::= { pwAtmPerfCurrentEntry 3 }

pwAtmPerfCurrentPktsTimeout OBJECT-TYPE
  SYNTAX        PerfCurrentCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets transmitted due to timeout expiration
       while attempting to collect cells."
   ::= { pwAtmPerfCurrentEntry 4 }

pwAtmPerfCurrentCellsXmit OBJECT-TYPE
  SYNTAX        PerfCurrentCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of transmitted cells."
   ::= { pwAtmPerfCurrentEntry 5 }

pwAtmPerfCurrentCellsDropped OBJECT-TYPE
  SYNTAX        PerfCurrentCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of dropped cells."
   ::= { pwAtmPerfCurrentEntry 6 }





pwAtmPerfCurrentCellsReceived OBJECT-TYPE
  SYNTAX        PerfCurrentCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of received cells."
   ::= { pwAtmPerfCurrentEntry 7 }

pwAtmPerfCurrentUnknownCells OBJECT-TYPE
  SYNTAX        PerfCurrentCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of cells received from the PSN with unknown VPI or
      VCI values.  This object is relevant only in N:1 mode."
   ::= { pwAtmPerfCurrentEntry 8 }

-- End ATM PW Performance Current Interval Table

-- ATM PW Performance Interval Table.

pwAtmPerfIntervalTable OBJECT-TYPE
  SYNTAX        SEQUENCE OF PwAtmPerfIntervalEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
      "This table provides performance information per ATM PW
       similar to the pwAtmPerfCurrentTable above.  However,
       these counts represent historical 15 minute intervals.
       Typically, this table will have a maximum of 96 entries
       for a 24 hour period. "
  ::= { pwAtmObjects 9 }

pwAtmPerfIntervalEntry OBJECT-TYPE
  SYNTAX        PwAtmPerfIntervalEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
      "An entry in this table is created by the agent for
       every pwAtmPerfCurrentEntry that is 15 minutes old.
       The contents of the Current entry are copied to the new
       entry here.  The Current entry then resets its counts
       to zero for the next current 15 minute interval. "
  INDEX  { pwIndex, pwAtmPerfIntervalNumber }
  ::= { pwAtmPerfIntervalTable 1 }

PwAtmPerfIntervalEntry ::= SEQUENCE {
     pwAtmPerfIntervalNumber         Unsigned32,





     pwAtmPerfIntervalValidData      TruthValue,
     pwAtmPerfIntervalDuration       Unsigned32,
     pwAtmPerfIntervalMissingPkts    PerfIntervalCount,
     pwAtmPerfIntervalPktsReOrder    PerfIntervalCount,
     pwAtmPerfIntervalPktsMisOrder   PerfIntervalCount,
     pwAtmPerfIntervalPktsTimeout    PerfIntervalCount,
     pwAtmPerfIntervalCellsXmit      PerfIntervalCount,
     pwAtmPerfIntervalCellsDropped   PerfIntervalCount,
     pwAtmPerfIntervalCellsReceived  PerfIntervalCount,
     pwAtmPerfIntervalUnknownCells   PerfIntervalCount
     }

pwAtmPerfIntervalNumber OBJECT-TYPE
  SYNTAX        Unsigned32 (1..96)
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
      "A number (normally between 1 and 96 to cover a 24 hour
       period) that identifies the interval for which the set
       of statistics is available.  The interval identified by 1
       is the most recently completed 15 minute interval, and
       the interval identified by N is the interval immediately
       preceding the one identified by N-1.  The minimum range of
       N is 1 through 4.  The default range is 1 through 32.  The
       maximum value of N is 96."
  ::= { pwAtmPerfIntervalEntry 1 }

pwAtmPerfIntervalValidData OBJECT-TYPE
  SYNTAX        TruthValue
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "This variable indicates if the data for this interval
       is valid."
  ::= { pwAtmPerfIntervalEntry 2 }

pwAtmPerfIntervalDuration OBJECT-TYPE
   SYNTAX      Unsigned32
   MAX-ACCESS  read-only
   STATUS      current
   DESCRIPTION
     "The duration of a particular interval in seconds.
      Adjustments in the system's time-of-day clock, may
      cause the interval to be greater or less than the
      normal value.  Therefore, this actual interval value
      is provided."
   ::= { pwAtmPerfIntervalEntry 3 }






pwAtmPerfIntervalMissingPkts OBJECT-TYPE
  SYNTAX        PerfIntervalCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of missing packets (as detected via control
       word sequence number gaps)."
  ::= { pwAtmPerfIntervalEntry 4 }

pwAtmPerfIntervalPktsReOrder OBJECT-TYPE
  SYNTAX        PerfIntervalCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets detected out of sequence (via control
       word sequence number), but successfully re-ordered.
       Note: some implementations may not support this
       feature."
  ::= { pwAtmPerfIntervalEntry 5 }

 pwAtmPerfIntervalPktsMisOrder OBJECT-TYPE
  SYNTAX        PerfIntervalCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets detected out of order (via control word
       sequence numbers)."
  ::= { pwAtmPerfIntervalEntry 6 }

pwAtmPerfIntervalPktsTimeout OBJECT-TYPE
  SYNTAX        PerfIntervalCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets transmitted due to timeout expiration."
   ::= { pwAtmPerfIntervalEntry 7 }

pwAtmPerfIntervalCellsXmit OBJECT-TYPE
  SYNTAX        PerfIntervalCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of transmitted cells."
   ::= { pwAtmPerfIntervalEntry 8 }

pwAtmPerfIntervalCellsDropped OBJECT-TYPE
  SYNTAX        PerfIntervalCount
  MAX-ACCESS    read-only





  STATUS        current
  DESCRIPTION
      "Number of dropped cells."
   ::= { pwAtmPerfIntervalEntry 9 }

pwAtmPerfIntervalCellsReceived OBJECT-TYPE
  SYNTAX        PerfIntervalCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of received cells."
   ::= { pwAtmPerfIntervalEntry 10 }

pwAtmPerfIntervalUnknownCells OBJECT-TYPE
  SYNTAX        PerfIntervalCount
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of cells received from the PSN with unknown VPI or
      VCI values.  This object is relevant only in N:1 mode."
   ::= { pwAtmPerfIntervalEntry 11 }

-- End ATM PW Performance Interval Table

-- ATM PW 1day Performance Table

pwAtmPerf1DayIntervalTable OBJECT-TYPE
  SYNTAX        SEQUENCE OF PwAtmPerf1DayIntervalEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
      "This table provides performance information per ATM PW
       similar to the pwAtmPerfIntervalTable above.  However,
       these counters represent historical one-day intervals up to
       one full month."
  ::= { pwAtmObjects 10 }

pwAtmPerf1DayIntervalEntry OBJECT-TYPE
  SYNTAX        PwAtmPerf1DayIntervalEntry
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
      "An entry is created in this table by the agent
       for every entry in the pwAtmCfgTable table."
  INDEX  { pwIndex,pwAtmPerf1DayIntervalNumber }
     ::= { pwAtmPerf1DayIntervalTable 1 }

PwAtmPerf1DayIntervalEntry ::= SEQUENCE {





     pwAtmPerf1DayIntervalNumber          Unsigned32,
     pwAtmPerf1DayIntervalValidData       TruthValue,
     pwAtmPerf1DayIntervalDuration        Unsigned32,
     pwAtmPerf1DayIntervalMissingPkts     Counter32,
     pwAtmPerf1DayIntervalPktsReOrder     Counter32,
     pwAtmPerf1DayIntervalPktsMisOrder    Counter32,
     pwAtmPerf1DayIntervalPktsTimeout     Counter32,
     pwAtmPerf1DayIntervalCellsXmit       Counter32,
     pwAtmPerf1DayIntervalCellsDropped    Counter32,
     pwAtmPerf1DayIntervalCellsReceived   Counter32,
     pwAtmPerf1DayIntervalUnknownCells    Counter32
     }

pwAtmPerf1DayIntervalNumber OBJECT-TYPE
  SYNTAX        Unsigned32 (1..365)
  MAX-ACCESS    not-accessible
  STATUS        current
  DESCRIPTION
      "The number of intervals, where 1 indicates current day
       measured period and 2 and above indicate previous days,
       respectively."
  ::= { pwAtmPerf1DayIntervalEntry 1 }

pwAtmPerf1DayIntervalValidData OBJECT-TYPE
  SYNTAX        TruthValue
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "This object indicates if the data for this interval
       is valid."
  ::= { pwAtmPerf1DayIntervalEntry 2 }

pwAtmPerf1DayIntervalDuration OBJECT-TYPE
  SYNTAX      Unsigned32
  MAX-ACCESS  read-only
  STATUS      current
  DESCRIPTION
    "The duration of a particular interval in seconds.
     Adjustments in the system's time-of-day clock may
     cause the interval to be greater or less than the
     normal value.  Therefore, this actual interval value
     is provided."
  ::= { pwAtmPerf1DayIntervalEntry 3 }

pwAtmPerf1DayIntervalMissingPkts OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current





  DESCRIPTION
    "Number of missing packets (as detected via control word
     sequence number gaps)."
  ::= { pwAtmPerf1DayIntervalEntry 4 }

pwAtmPerf1DayIntervalPktsReOrder OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets detected out of sequence (via control
       word sequence number), but successfully re-ordered.
       Note: some implementations may not support this
       feature."
  ::= { pwAtmPerf1DayIntervalEntry 5 }

pwAtmPerf1DayIntervalPktsMisOrder OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets detected out of order (via control word
       sequence numbers) and that could not be re-ordered."
  ::= { pwAtmPerf1DayIntervalEntry 6 }

pwAtmPerf1DayIntervalPktsTimeout OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of packets transmitted due to timeout expiration."
   ::= { pwAtmPerf1DayIntervalEntry 7 }

pwAtmPerf1DayIntervalCellsXmit OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of transmitted cells."
   ::= { pwAtmPerf1DayIntervalEntry 8 }

pwAtmPerf1DayIntervalCellsDropped OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of dropped cells."
   ::= { pwAtmPerf1DayIntervalEntry 9 }





pwAtmPerf1DayIntervalCellsReceived OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of received cells."
   ::= { pwAtmPerf1DayIntervalEntry 10 }

pwAtmPerf1DayIntervalUnknownCells OBJECT-TYPE
  SYNTAX        Counter32
  MAX-ACCESS    read-only
  STATUS        current
  DESCRIPTION
      "Number of cells received from the PSN with unknown VPI
      or VCI values.  This object is relevant only in N:1 mode."
   ::= { pwAtmPerf1DayIntervalEntry 11 }

-- End of ATM PW Performance table

    pwAtmCompliances OBJECT IDENTIFIER ::= { pwAtmConformance 1 }
    pwAtmGroups      OBJECT IDENTIFIER ::= { pwAtmConformance 2 }
    pwAtmCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
            "The compliance statement for agents that support
             ATM PW."
    MODULE  -- this module
        MANDATORY-GROUPS { pwAtmCfgGroup,
                           pwAtmPerfGroup
                         }

       OBJECT pwAtmCfgFarEndMaxCellConcatenation
       MIN-ACCESS read-only
       DESCRIPTION
        "The ability to set this object
        is not required."

       GROUP        pwAtmOutbound1to1Group
       DESCRIPTION "This group is mandatory only for implementations
                    that support the ATM PW 1:1 mode and not using
                    the Nto1 table."

       GROUP        pwAtmInbound1to1Group
       DESCRIPTION "This group is mandatory only for implementations
                    that support the ATM PW 1:1 mode and not using
                    the Nto1 table."

       GROUP        pwAtmOutboundNto1Group





       DESCRIPTION "This group is mandatory only for implementations
                    that support the ATM PW N:1 and transparent mode."

       GROUP        pwAtmInboundNto1Group
       DESCRIPTION "This group is mandatory only for implementations
                    that support the ATM PW N:1 and transparent mode."

    ::= { pwAtmCompliances 2 }

-- Units of conformance.

    pwAtmCfgGroup OBJECT-GROUP
    OBJECTS {pwAtmCfgMaxCellConcatenation,
             pwAtmCfgFarEndMaxCellConcatenation,
             pwAtmCfgTimeoutMode,
             pwAtmClpQosMapping
                     }

    STATUS  current
    DESCRIPTION
              "Collection of objects for basic ATM PW
               configuration."
    ::= { pwAtmGroups 5 }

    pwAtmPerfGroup OBJECT-GROUP
    OBJECTS {pwAtmPerfCurrentMissingPkts,
             pwAtmPerfCurrentPktsReOrder,
             pwAtmPerfCurrentPktsMisOrder,
             pwAtmPerfCurrentPktsTimeout,
             pwAtmPerfCurrentCellsXmit,
             pwAtmPerfCurrentCellsDropped,
             pwAtmPerfCurrentCellsReceived,
             pwAtmPerfCurrentUnknownCells,
             pwAtmPerfIntervalValidData,
             pwAtmPerfIntervalDuration,
             pwAtmPerfIntervalMissingPkts,
             pwAtmPerfIntervalPktsReOrder,
             pwAtmPerfIntervalPktsMisOrder,
             pwAtmPerfIntervalPktsTimeout,
             pwAtmPerfIntervalCellsXmit,
             pwAtmPerfIntervalCellsDropped,
             pwAtmPerfIntervalCellsReceived,
             pwAtmPerfIntervalUnknownCells,
             pwAtmPerf1DayIntervalValidData,
             pwAtmPerf1DayIntervalDuration,
             pwAtmPerf1DayIntervalMissingPkts,
             pwAtmPerf1DayIntervalPktsReOrder,
             pwAtmPerf1DayIntervalPktsMisOrder,





             pwAtmPerf1DayIntervalPktsTimeout,
             pwAtmPerf1DayIntervalCellsXmit,
             pwAtmPerf1DayIntervalCellsDropped,
             pwAtmPerf1DayIntervalCellsReceived,
             pwAtmPerf1DayIntervalUnknownCells
                         }
    STATUS current
    DESCRIPTION
              "Collection of objects for basic ATM PW Performance."
    ::= { pwAtmGroups 6 }

    pwAtmOutbound1to1Group OBJECT-GROUP
    OBJECTS {pwAtmOutboundAtmIf,
             pwAtmOutboundVpi,
             pwAtmOutboundVci,
             pwAtmOutboundTrafficParamDescr,
             pwAtmOutboundRowStatus
             }
    STATUS  current
    DESCRIPTION
              "Collection of objects for basic 1:1 ATM PW outbound
               configuration."
    ::= { pwAtmGroups 7 }

    pwAtmInbound1to1Group OBJECT-GROUP
    OBJECTS {pwAtmInboundAtmIf,
             pwAtmInboundVpi,
             pwAtmInboundVci,
             pwAtmInboundTrafficParamDescr,
             pwAtmInboundRowStatus
             }
    STATUS  current
    DESCRIPTION
          "Collection of objects for basic 1:1 ATM PW inbound
           configuration."
    ::= { pwAtmGroups 8 }

    pwAtmOutboundNto1Group OBJECT-GROUP
    OBJECTS {pwAtmOutboundNto1RowStatus,
             pwAtmOutboundNto1TrafficParamDescr,
             pwAtmOutboundNto1MappedVpi,
             pwAtmOutboundNto1MappedVci
                         }
    STATUS  current
    DESCRIPTION
          "Collection of objects for N:1, 1:1, or transparent
          ATM PW outbound configuration."
    ::= { pwAtmGroups 9 }





    pwAtmInboundNto1Group OBJECT-GROUP
    OBJECTS {pwAtmInboundNto1RowStatus,
             pwAtmInboundNto1TrafficParamDescr,
             pwAtmInboundNto1MappedVpi,
             pwAtmInboundNto1MappedVci
                 }
    STATUS current
    DESCRIPTION
          "Collection of objects for N:1, 1:1, or transparent
           ATM PW inbound configuration."
    ::= { pwAtmGroups 10 }

END


