VDSL2-LINE-TC-MIB DEFINITIONS ::= BEGIN


IMPORTS
   MODULE-IDENTITY,
   transmission
      FROM SNMPv2-SMI

   TEXTUAL-CONVENTION
      FROM SNMPv2-TC;

vdsl2TCMIB MODULE-IDENTITY
   LAST-UPDATED "200909300000Z" -- September 30, 2009
   ORGANIZATION "ADSLMIB Working Group"
   CONTACT-INFO "WG-email:  adslmib@ietf.org
   Info:      https://www1.ietf.org/mailman/listinfo/adslmib

             Chair:     Mike Sneed
                        Sand Channel Systems
             Postal:    P.O. Box 37324
                        Raleigh NC 27627-732
             Email:     sneedmike@hotmail.com
             Phone:     +1 206 600 7022

             Co-Chair:  Menachem Dodge





                        ECI Telecom Ltd.
             Postal:    30 Hasivim St.
                        Petach Tikva 49517,
                        Israel.
             Email:     mbdodge@ieee.org
             Phone:     +972 3 926 8421

             Co-editor: Moti Morgenstern
                        ECI Telecom Ltd.
             Postal:    30 Hasivim St.
                        Petach Tikva 49517,
                        Israel.
             Email:     moti.morgenstern@ecitele.com
             Phone:     +972 3 926 6258

             Co-editor: Scott Baillie
                        NEC Australia
             Postal:    649-655 Springvale Road,
                        Mulgrave, Victoria 3170,
                        Australia.
             Email:     scott.baillie@nec.com.au
             Phone:     +61 3 9264 3986

             Co-editor: Umberto Bonollo
                        NEC Australia
             Postal:    649-655 Springvale Road,
                        Mulgrave, Victoria 3170,
                        Australia.
             Email:     umberto.bonollo@nec.com.au
             Phone:     +61 3 9264 3385
            "
   DESCRIPTION
        "This MIB Module provides Textual Conventions to be
         used by the VDSL2-LINE-MIB module for the purpose of
         managing VDSL2, ADSL, ADSL2, and ADSL2+ lines.

         Copyright (c) 2009 IETF Trust and the persons
         identified as authors of the code.  All rights
         reserved.

         Redistribution and use in source and binary
         forms, with or without modification, are
         permitted provided that the following
         conditions are met:

         - Redistributions of source code must retain the
           above copyright notice, this list of conditions
           and the following disclaimer.





         - Redistributions in binary form must reproduce
           the above copyright notice, this list of
           conditions and the following disclaimer in
           the documentation and/or other materials provided
           with the distribution.

         - Neither the name of Internet Society, IETF or
           IETF Trust, nor the names of specific contributors,
           may be used to endorse or promote products derived
           from this software without specific prior written
           permission.

         THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND
         CONTRIBUTORS 'AS IS' AND ANY EXPRESS OR IMPLIED
         WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED
         WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A
         PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL
         THE COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY
         DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR
         CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO,
         PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE,
         DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED
         AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
         LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE)
         ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF
         ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.

         This version of this MIB module is part of RFC 5650;
         see the RFC itself for full legal notices."

   REVISION "200909300000Z" -- September 30, 2009
   DESCRIPTION "Initial version, published as RFC 5650."
      ::= { transmission 251 3} -- vdsl2MIB 3

------------------------------------------------
--          Textual Conventions               --
------------------------------------------------

Xdsl2Unit ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Identifies a transceiver as being either xTU-C or xTU-R.
       A VDSL2/ADSL/ADSL2 or ADSL2+ line consists of two
       transceivers: an xTU-C and an xTU-R.
       In the case of ADSL/ADSL2 and ADSL2+, those two transceivers are
       also called atuc and atur.
       In the case of VDSL2, those two transceivers are also called
       vtuc and vtur.





       Specified as an INTEGER, the two values are:
        xtuc(1)  -- central office transceiver
        xtur(2)  -- remote site transceiver"
   SYNTAX      INTEGER {
                  xtuc(1),
                  xtur(2)
               }

Xdsl2Direction ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "Identifies the direction of a band in a VDSL2/ADSL/ADSL2/
         ADSL2+ link.
         The upstream direction is a transmission from the remote end
         (xTU-R) towards the central office end (xTU-C).  The downstream
         direction is a transmission from the xTU-C towards the xTU-R.
         Specified as an INTEGER, the values are defined as
         follows:"
     SYNTAX INTEGER {
        upstream(1),   -- Transmission from the xTU-R to the xTU-C.
        downstream(2)  -- Transmission from the xTU-C to the xTU-R.
            }

Xdsl2Band ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "Identifies a band in a VDSL2/ADSL/ADSL2/ADSL2+ link.
         For a band in the upstream direction, transmission is from the
         remote end (xTU-R) towards the central office end (xTU-C).
         For a band in the downstream direction, transmission is from
         the xTU-C towards the xTU-R.
         For ADSL, ADSL2 and ADSL2+, which use a single band in the
         upstream direction and a single band
         in the downstream direction,
         the only relevant values are upstream(1) and downstream(2).
         For VDSL2, which uses multiple bands in each transmission
         direction, a band in the upstream direction is indicated by any
         of us0(3), us1(5), us2(7), us3(9), or us4(11), and a band in
         the downstream direction is indicated by any of ds1(4),
         ds2(6), ds3(8), or ds4(10).
         For VDSL2, the values upstream(1) and downstream(2) may be used
         when there is a need to refer to the whole upstream or
         downstream traffic (e.g., report the average signal-to-noise
         ratio on any transmission direction).
         Specified as an INTEGER, the values are defined as
         follows:"
     SYNTAX INTEGER {
        upstream(1),   -- Transmission from the xTU-R to the xTU-C





                       -- (refers to the single upstream band for
                       -- ADSL/ADSL2/ADSL2+ or to the whole
                       -- upstream traffic for VDSL2).
        downstream(2), -- Transmission from the xTU-C to the xTU-R
                       -- (refers to the single downstream band
                       -- for ADSL/ADSL2/ADSL2+ or to the whole
                       -- downstream traffic for VDSL2).
        us0(3),        -- Upstream band number 0   (US0) (VDSL2).
        ds1(4),        -- Downstream band number 1 (DS1) (VDSL2).
        us1(5),        -- Upstream band number 1   (US1) (VDSL2).
        ds2(6),        -- Downstream band number 2 (DS2) (VDSL2).
        us2(7),        -- Upstream band number 2   (US2) (VDSL2).
        ds3(8),        -- Downstream band number 3 (DS3) (VDSL2).
        us3(9),        -- Upstream band number 3   (US3) (VDSL2).
        ds4(10),       -- Downstream band number 4 (DS4) (VDSL2).
        us4(11)        -- Upstream band number 4   (US4) (VDSL2).
            }

Xdsl2TransmissionModeType ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "A set of xDSL line transmission modes, with one bit
       per mode.  The notes (F) and (L) denote Full-Rate and
       Lite/splitterless, respectively:
          Bit 00 : Regional Std. (ANSI T1.413) (F)
          Bit 01 : Regional Std. (ETSI DTS/TM06006) (F)
          Bit 02 : G.992.1 POTS non-overlapped (F)
          Bit 03 : G.992.1 POTS overlapped (F)
          Bit 04 : G.992.1 ISDN non-overlapped (F)
          Bit 05 : G.992.1 ISDN overlapped (F)
          Bit 06 : G.992.1 TCM-ISDN non-overlapped (F)
          Bit 07 : G.992.1 TCM-ISDN overlapped (F)
          Bit 08 : G.992.2 POTS non-overlapped (L)
          Bit 09 : G.992.2 POTS overlapped (L)
          Bit 10 : G.992.2 with TCM-ISDN non-overlapped (L)
          Bit 11 : G.992.2 with TCM-ISDN overlapped (L)
          Bit 12 : G.992.1 TCM-ISDN symmetric (F) --- not in G.997.1
          Bit 13-17: Reserved
          Bit 18 : G.992.3 POTS non-overlapped (F)
          Bit 19 : G.992.3 POTS overlapped (F)
          Bit 20 : G.992.3 ISDN non-overlapped (F)
          Bit 21 : G.992.3 ISDN overlapped (F)
          Bit 22-23: Reserved
          Bit 24 : G.992.4 POTS non-overlapped (L)
          Bit 25 : G.992.4 POTS overlapped (L)
          Bit 26-27: Reserved
          Bit 28 : G.992.3 Annex I All-Digital non-overlapped (F)
          Bit 29 : G.992.3 Annex I All-Digital overlapped (F)





          Bit 30 : G.992.3 Annex J All-Digital non-overlapped (F)
          Bit 31 : G.992.3 Annex J All-Digital overlapped (F)
          Bit 32 : G.992.4 Annex I All-Digital non-overlapped (L)
          Bit 33 : G.992.4 Annex I All-Digital overlapped (L)
          Bit 34 : G.992.3 Annex L POTS non-overlapped, mode 1,
                                   wide U/S (F)
          Bit 35 : G.992.3 Annex L POTS non-overlapped, mode 2,
                                   narrow U/S(F)
          Bit 36 : G.992.3 Annex L POTS overlapped, mode 3,
                                   wide U/S (F)
          Bit 37 : G.992.3 Annex L POTS overlapped, mode 4,
                                   narrow U/S (F)
          Bit 38 : G.992.3 Annex M POTS non-overlapped (F)
          Bit 39 : G.992.3 Annex M POTS overlapped (F)
          Bit 40 : G.992.5 POTS non-overlapped (F)
          Bit 41 : G.992.5 POTS overlapped (F)
          Bit 42 : G.992.5 ISDN non-overlapped (F)
          Bit 43 : G.992.5 ISDN overlapped (F)
          Bit 44-45: Reserved
          Bit 46 : G.992.5 Annex I All-Digital non-overlapped (F)
          Bit 47 : G.992.5 Annex I All-Digital overlapped (F)
          Bit 48 : G.992.5 Annex J All-Digital non-overlapped (F)
          Bit 49 : G.992.5 Annex J All-Digital overlapped (F)
          Bit 50 : G.992.5 Annex M POTS non-overlapped (F)
          Bit 51 : G.992.5 Annex M POTS overlapped (F)
          Bit 52-55: Reserved
          Bit 56 : G.993.2 Annex A
          Bit 57 : G.993.2 Annex B
          Bit 58 : G.993.2 Annex C
          Bit 59-63: Reserved"

   SYNTAX      BITS {
                  ansit1413(0),
                  etsi(1),
                  g9921PotsNonOverlapped(2),
                  g9921PotsOverlapped(3),
                  g9921IsdnNonOverlapped(4),
                  g9921isdnOverlapped(5),
                  g9921tcmIsdnNonOverlapped(6),
                  g9921tcmIsdnOverlapped(7),
                  g9922potsNonOverlapped(8),
                  g9922potsOverlapped(9),
                  g9922tcmIsdnNonOverlapped(10),
                  g9922tcmIsdnOverlapped(11),
                  g9921tcmIsdnSymmetric(12),
                  reserved1(13),
                  reserved2(14),
                  reserved3(15),





                  reserved4(16),
                  reserved5(17),
                  g9923PotsNonOverlapped(18),
                  g9923PotsOverlapped(19),
                  g9923IsdnNonOverlapped(20),
                  g9923isdnOverlapped(21),
                  reserved6(22),
                  reserved7(23),
                  g9924potsNonOverlapped(24),
                  g9924potsOverlapped(25),
                  reserved8(26),
                  reserved9(27),
                  g9923AnnexIAllDigNonOverlapped(28),
                  g9923AnnexIAllDigOverlapped(29),
                  g9923AnnexJAllDigNonOverlapped(30),
                  g9923AnnexJAllDigOverlapped(31),
                  g9924AnnexIAllDigNonOverlapped(32),
                  g9924AnnexIAllDigOverlapped(33),
                  g9923AnnexLMode1NonOverlapped(34),
                  g9923AnnexLMode2NonOverlapped(35),
                  g9923AnnexLMode3Overlapped(36),
                  g9923AnnexLMode4Overlapped(37),
                  g9923AnnexMPotsNonOverlapped(38),
                  g9923AnnexMPotsOverlapped(39),
                  g9925PotsNonOverlapped(40),
                  g9925PotsOverlapped(41),
                  g9925IsdnNonOverlapped(42),
                  g9925isdnOverlapped(43),
                  reserved10(44),
                  reserved11(45),
                  g9925AnnexIAllDigNonOverlapped(46),
                  g9925AnnexIAllDigOverlapped(47),
                  g9925AnnexJAllDigNonOverlapped(48),
                  g9925AnnexJAllDigOverlapped(49),
                  g9925AnnexMPotsNonOverlapped(50),
                  g9925AnnexMPotsOverlapped(51),
                  reserved12(52),
                  reserved13(53),
                  reserved14(54),
                  reserved15(55),
                  g9932AnnexA(56),
                  g9932AnnexB(57),
                  g9932AnnexC(58),
                  reserved16(59),
                  reserved17(60),
                  reserved18(61),
                  reserved19(62),
                  reserved20(63)





               }

Xdsl2RaMode ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Specifies the rate adaptation behavior for the line.
       The three possible behaviors are:
        manual (1)   - No Rate-Adaptation.  The initialization
                       process attempts to synchronize to a
                       specified rate.
        raInit (2)   - Rate-Adaptation during initialization process
                       only, which attempts to synchronize to a rate
                       between minimum and maximum specified values.
        dynamicRa (3)- Dynamic Rate-Adaptation during initialization
                       process as well as during Showtime."
   SYNTAX      INTEGER {
                  manual(1),
                  raInit(2),
                  dynamicRa(3)
               }

Xdsl2InitResult ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Specifies the result of full initialization attempt; the
       six possible result values are:
        noFail (0)            - Successful initialization
        configError (1)       - Configuration failure
        configNotFeasible (2) - Configuration details not supported
        commFail (3)          - Communication failure
        noPeerAtu (4)         - Peer ATU not detected
        otherCause (5)        - Other initialization failure reason"

   SYNTAX      INTEGER {
                  noFail(0),
                  configError(1),
                  configNotFeasible(2),
                  commFail(3),
                  noPeerAtu(4),
                  otherCause(5)
               }

Xdsl2OperationModes ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "The VDSL2 management model specified includes an xDSL Mode
       object that identifies an instance of xDSL Mode-Specific
       PSD Configuration object in the xDSL Line Profile.  The





       following classes of xDSL operating mode are defined.
       The notes (F) and (L) denote Full-Rate and Lite/splitterless,
       respectively:
       +-------+--------------------------------------------------+
       | Value |         xDSL operation mode description          |
       +-------+--------------------------------------------------+
           1   - The default/generic PSD configuration.  Default
                 configuration will be used when no other matching
                 mode-specific configuration can be found.
           2   - Regional Std. (ANSI T1.413) (F)
           3   - Regional Std. (ETSI DTS/TM06006) (F)
           4   - G.992.1 POTS non-overlapped (F)
           5   - G.992.1 POTS overlapped (F)
           6   - G.992.1 ISDN non-overlapped (F)
           7   - G.992.1 ISDN overlapped (F)
           8   - G.992.1 TCM-ISDN non-overlapped (F)
           9   - G.992.1 TCM-ISDN overlapped (F)
          10   - G.992.2 POTS non-overlapped (L)
          11   - G.992.2 POTS overlapped (L)
          12   - G.992.2 with TCM-ISDN non-overlapped (L)
          13   - G.992.2 with TCM-ISDN overlapped (L)
          14   - G.992.1 TCM-ISDN symmetric (F) --- not in G.997.1
        15-19  - Unused. Reserved for future ITU-T specification.
          20   - G.992.3 POTS non-overlapped (F)
          21   - G.992.3 POTS overlapped (F)
          22   - G.992.3 ISDN non-overlapped (F)
          23   - G.992.3 ISDN overlapped (F)
        24-25  - Unused. Reserved for future ITU-T specification.
          26   - G.992.4 POTS non-overlapped (L)
          27   - G.992.4 POTS overlapped (L)
        28-29  - Unused. Reserved for future ITU-T specification.
          30   - G.992.3 Annex I All-Digital non-overlapped (F)
          31   - G.992.3 Annex I All-Digital overlapped (F)
          32   - G.992.3 Annex J All-Digital non-overlapped (F)
          33   - G.992.3 Annex J All-Digital overlapped (F)
          34   - G.992.4 Annex I All-Digital non-overlapped (L)
          35   - G.992.4 Annex I All-Digital overlapped (L)
          36   - G.992.3 Annex L POTS non-overlapped, mode 1,
                 wide U/S (F)
          37   - G.992.3 Annex L POTS non-overlapped, mode 2,
                 narrow U/S(F)
          38   - G.992.3 Annex L POTS overlapped, mode 3,
                 wide U/S (F)
          39   - G.992.3 Annex L POTS overlapped, mode 4,
                 narrow U/S (F)
          40   - G.992.3 Annex M POTS non-overlapped (F)
          41   - G.992.3 Annex M POTS overlapped (F)
          42   - G.992.5 POTS non-overlapped (F)





          43   - G.992.5 POTS overlapped (F)
          44   - G.992.5 ISDN non-overlapped (F)
          45   - G.992.5 ISDN overlapped (F)
        46-47  - Unused. Reserved for future ITU-T specification.
          48   - G.992.5 Annex I All-Digital non-overlapped (F)
          49   - G.992.5 Annex I All-Digital overlapped (F)
          50   - G.992.5 Annex J All-Digital non-overlapped (F)
          51   - G.992.5 Annex J All-Digital overlapped (F)
          52   - G.992.5 Annex M POTS non-overlapped (F)
          53   - G.992.5 Annex M POTS overlapped (F)
        54-57  - Unused. Reserved for future ITU-T specification.
          58   - G.993.2 Annex A
          59   - G.993.2 Annex B
          60   - G.993.2 Annex C
      "
   SYNTAX      INTEGER {
                  defMode(1),
                  ansit1413(2),
                  etsi(3),
                  g9921PotsNonOverlapped(4),
                  g9921PotsOverlapped(5),
                  g9921IsdnNonOverlapped(6),
                  g9921isdnOverlapped(7),
                  g9921tcmIsdnNonOverlapped(8),
                  g9921tcmIsdnOverlapped(9),
                  g9922potsNonOverlapped(10),
                  g9922potsOverlapped(11),
                  g9922tcmIsdnNonOverlapped(12),
                  g9922tcmIsdnOverlapped(13),
                  g9921tcmIsdnSymmetric(14),
                  g9923PotsNonOverlapped(20),
                  g9923PotsOverlapped(21),
                  g9923IsdnNonOverlapped(22),
                  g9923isdnOverlapped(23),
                  g9924potsNonOverlapped(26),
                  g9924potsOverlapped(27),
                  g9923AnnexIAllDigNonOverlapped(30),
                  g9923AnnexIAllDigOverlapped(31),
                  g9923AnnexJAllDigNonOverlapped(32),
                  g9923AnnexJAllDigOverlapped(33),
                  g9924AnnexIAllDigNonOverlapped(34),
                  g9924AnnexIAllDigOverlapped(35),
                  g9923AnnexLMode1NonOverlapped(36),
                  g9923AnnexLMode2NonOverlapped(37),
                  g9923AnnexLMode3Overlapped(38),
                  g9923AnnexLMode4Overlapped(39),
                  g9923AnnexMPotsNonOverlapped(40),
                  g9923AnnexMPotsOverlapped(41),





                  g9925PotsNonOverlapped(42),
                  g9925PotsOverlapped(43),
                  g9925IsdnNonOverlapped(44),
                  g9925isdnOverlapped(45),
                  g9925AnnexIAllDigNonOverlapped(48),
                  g9925AnnexIAllDigOverlapped(49),
                  g9925AnnexJAllDigNonOverlapped(50),
                  g9925AnnexJAllDigOverlapped(51),
                  g9925AnnexMPotsNonOverlapped(52),
                  g9925AnnexMPotsOverlapped(53),
                  g9932AnnexA(58),
                  g9932AnnexB(59),
                  g9932AnnexC(60)
               }

Xdsl2PowerMngState ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Objects with this syntax uniquely identify each power
       management state defined for the VDSL2/ADSL/ADSL2 or ADSL2+
       link.
       In VDSL2, only L0 and L3 states are defined.
       The possible values are:
         l0(1)              - L0: Full power.  Synchronized and
                                  full transmission (i.e., Showtime).
         l1(2)              - L1: Low power with reduced net data rate
                                  (for G.992.2 only).
         l2(3)              - L2: Low power with reduced net data rate
                                  (for G.992.3, G.992.4 and G.992.5).
         l3(4)              - L3: Idle power management state / No
         power."

   SYNTAX      INTEGER {
                  l0(1),
                  l1(2),
                  l2(3),
                  l3(4)
               }

Xdsl2ConfPmsForce ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Objects with this syntax are configuration parameters
       that specify the desired power management state transition
       for the VDSL2/ADSL/ADSL2 or ADSL2+ link.
       In VDSL2, only L0 and L3 states are defined:
         l3toL0 (0)         - Perform a transition from L3 to L0
                              (Full power management state).





         l0toL2 (2)         - Perform a transition from L0 to L2
                              (Low power management state).
         l0orL2toL3 (3)     - Perform a transition into L3 (Idle
                              power management state)."

   SYNTAX      INTEGER {
                  l3toL0 (0),
                  l0toL2 (2),
                  l0orL2toL3 (3)
               }

Xdsl2LinePmMode ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "Objects with this syntax are configuration parameters
       that reference the power modes/states into which the xTU-C or
       xTU-R may autonomously transit.

       It is a BITS structure that allows control of the following
       transit options:
        allowTransitionsToIdle (0)    - xTU may autonomously transit
                                        to idle (L3) state.
        allowTransitionsToLowPower (1)- xTU may autonomously transit
                                        to low-power (L1/L2)
                                        state."

   SYNTAX BITS {
       allowTransitionsToIdle(0),
       allowTransitionsToLowPower(1)
     }

Xdsl2LineLdsf ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "Objects with this syntax are configuration parameters
       that control the Loop Diagnostic mode for a VDSL2/ADSL/ADSL2
       or ADSL2+ link.  The possible values are:
         inhibit (0)  - Inhibit Loop Diagnostic mode
         force   (1)  - Force/Initiate Loop Diagnostic mode"

   SYNTAX INTEGER {
       inhibit(0),
       force(1)
     }

Xdsl2LdsfResult ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION





        "Possible failure reasons associated with performing
         Dual Ended Loop Test (DELT) on a DSL line.
         Possible values are:
          none        (1) - The default value in case LDSF was never
                            requested for the associated line.
          success     (2) - The recent command completed
                            successfully.
          inProgress  (3) - The Loop Diagnostics process is in
                            progress.
          unsupported (4) - The NE or the line card doesn't support
                            LDSF.
          cannotRun   (5) - The NE cannot initiate the command, due
                            to a nonspecific reason.
          aborted     (6) - The Loop Diagnostics process aborted.
          failed      (7) - The Loop Diagnostics process failed.
          illegalMode (8) - The NE cannot initiate the command, due
                            to the specific mode of the relevant
                            line.
          adminUp     (9) - The NE cannot initiate the command, as
                            the relevant line is administratively
                            'Up'.
          tableFull   (10)- The NE cannot initiate the command, due
                            to reaching the maximum number of rows
                            in the results table.
          noResources (11)- The NE cannot initiate the command, due
                            to lack of internal memory resources."
     SYNTAX INTEGER {
          none (1),
          success (2),
          inProgress (3),
          unsupported (4),
          cannotRun (5),
          aborted (6),
          failed (7),
          illegalMode (8),
          adminUp (9),
          tableFull (10),
          noResources (11)
     }

Xdsl2LineBpsc ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "Objects with this syntax are configuration parameters
       that control the bits per subcarrier measurement for a
       VDSL2/ADSL/ADSL2 or ADSL2+ link.  The possible values are:
         idle    (1)  - Idle state
         measure (2)  - Measure the bits per subcarrier"





   SYNTAX INTEGER {
       idle(1),
       measure(2)
     }

Xdsl2BpscResult ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "Possible failure reasons associated with performing
         a bits per subcarrier measurement on a DSL line.
         Possible values are:

          none        (1) - The default value, in case a measurement
                            was never requested for the associated
                            line.
          success     (2) - The recent measurement request completed
                            successfully.
          inProgress  (3) - The bits per subcarrier measurement is
                            in progress.
          unsupported (4) - The bits per subcarrier request
                            mechanism is not supported.
          failed      (5) - The measurement request has failed and no
                            results are available.
          noResources (6) - The NE cannot initiate the command, due
                            to lack of internal memory resources."
     SYNTAX INTEGER {
          none(1),
          success(2),
          inProgress(3),
          unsupported(4),
          failed(5),
          noResources(6)
     }

Xdsl2LineReset ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "This type is used to request a line reset to occur.
          idle        (1) - This state indicates that there is
                            currently no request for a line reset.
          reset       (2) - This state indicates that a line reset
                            request has been issued."
   SYNTAX INTEGER {
       idle(1),
       reset(2)
     }

Xdsl2LineProfiles ::= TEXTUAL-CONVENTION





   STATUS current
   DESCRIPTION
     "Objects with this syntax reference the list of
      ITU-T G.993.2 implementation profiles supported by an
      xTU, enabled on the VDSL2 line or active on that line."

      SYNTAX BITS {
          profile8a(0),
          profile8b(1),
          profile8c(2),
          profile8d(3),
          profile12a(4),
          profile12b(5),
          profile17a(6),
          profile30a(7)
     }

Xdsl2LineClassMask ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "VDSL2 PSD Mask Class.
       The limit Power Spectral Density masks are grouped in
       the following PSD mask classes:

       Class 998     Annex A: D-32, D-48, D-64, D-128.
       Class 997-M1c Annex B: 997-M1c-A-7.
       Class 997-M1x Annex B: 997-M1x-M-8, 997-M1x-M.
       Class 997-M2x Annex B: 997-M2x-M-8, 997-M2x-A, 997-M2x-M,
                              997E17-M2x-NUS0, 997E30-M2x-NUS0.
       Class 998-M1x Annex B: 998-M1x-A, 998-M1x-B, 998-M1x-NUS0.
       Class 998-M2x Annex B: 998-M2x-A, 998-M2x-M, 998-M2x-B,
                              998-M2x-NUS0, 998E17-M2x-NUS0,
                              998E17-M2x-NUS0-M, 998E30-M2x-NUS0,
                              998E30-M2x-NUS0-M.
       Class 998ADE-M2x Annex B: Annex B: 998-M2x-A, 998-M2x-M,
                              998-M2x-B, 998-M2x-NUS0,
                              998ADE17-M2x-A, 998ADE17-M2x-B,
                              998ADE17-M2x-NUS0-M,
                              998ADE30-M2x-NUS0-A,
                              998ADE30-M2x-NUS0-M.
       Class 998-B   Annex C: POTS-138b, POTS-276b per C.2.1.1
                              in G.993.2, TCM-ISDN per C.2.1.2
                              in G.993.2.
       Class 998-CO  Annex C: POTS-138co, POTS-276co per C.2.1.1
                              in G.993.2.
       Class HPE-M1  Annex B: HPE17-M1-NUS0, HPE30-M1-NUS0."

   SYNTAX      INTEGER {





                  none(1),
                  a998ORb997M1cORc998B(2),
                  b997M1xOR998co(3),
                  b997M2x(4),
                  b998M1x(5),
                  b998M2x(6),
                  b998AdeM2x(7),
                  bHpeM1(8)
               }

Xdsl2LineLimitMask ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "The G.993.2 limit PSD mask for each class of profile.
      The profiles are grouped in following profile classes:
      - Class 8: Profiles 8a, 8b, 8c, 8d.
      - Class 12: Profiles 12a, 12b.
      - Class 17: Profile 17a.
      - Class 30: Profile 30a."

      SYNTAX BITS {
          profile8Limit1(0),
          profile8Limit2(1),
          profile8Limit3(2),
          profile8Limit4(3),
          profile8Limit5(4),
          profile8Limit6(5),
          profile8Limit7(6),
          profile8Limit8(7),
          profile8Limit9(8),
          profile8Limit10(9),
          profile8Limit11(10),
          profile8Limit12(11),
          profile8Limit13(12),
          profile8Limit14(13),
          profile8Limit15(14),
          profile8Limit16(15),
          --
          profile12Limit1(16),
          profile12Limit2(17),
          profile12Limit3(18),
          profile12Limit4(19),
          profile12Limit5(20),
          profile12Limit6(21),
          profile12Limit7(22),
          profile12Limit8(23),
          profile12Limit9(24),
          profile12Limit10(25),





          profile12Limit11(26),
          profile12Limit12(27),
          profile12Limit13(28),
          profile12Limit14(29),
          profile12Limit15(30),
          profile12Limit16(31),
          --
          profile17Limit1(32),
          profile17Limit2(33),
          profile17Limit3(34),
          profile17Limit4(35),
          profile17Limit5(36),
          profile17Limit6(37),
          profile17Limit7(38),
          profile17Limit8(39),
          profile17Limit9(40),
          profile17Limit10(41),
          profile17Limit11(42),
          profile17Limit12(43),
          profile17Limit13(44),
          profile17Limit14(45),
          profile17Limit15(46),
          profile17Limit16(47),
          --
          profile30Limit1(48),
          profile30Limit2(49),
          profile30Limit3(50),
          profile30Limit4(51),
          profile30Limit5(52),
          profile30Limit6(53),
          profile30Limit7(54),
          profile30Limit8(55),
          profile30Limit9(56),
          profile30Limit10(57),
          profile30Limit11(58),
          profile30Limit12(59),
          profile30Limit13(60),
          profile30Limit14(61),
          profile30Limit15(62),
          profile30Limit16(63)
     }

Xdsl2LineUs0Disable ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "Indicates if US0 is disabled for each limit PSD mask.
      The profiles are grouped in following profile classes:
      - Class 8: Profiles 8a, 8b, 8c, 8d.





      - Class 12: Profiles 12a, 12b.
      - Class 17: Profile 17a.
      - Class 30: Profile 30a."

      SYNTAX BITS {
          profile8Us0Disable1(0),
          profile8Us0Disable2(1),
          profile8Us0Disable3(2),
          profile8Us0Disable4(3),
          profile8Us0Disable5(4),
          profile8Us0Disable6(5),
          profile8Us0Disable7(6),
          profile8Us0Disable8(7),
          profile8Us0Disable9(8),
          profile8Us0Disable10(9),
          profile8Us0Disable11(10),
          profile8Us0Disable12(11),
          profile8Us0Disable13(12),
          profile8Us0Disable14(13),
          profile8Us0Disable15(14),
          profile8Us0Disable16(15),
          --
          profile12Us0Disable1(16),
          profile12Us0Disable2(17),
          profile12Us0Disable3(18),
          profile12Us0Disable4(19),
          profile12Us0Disable5(20),
          profile12Us0Disable6(21),
          profile12Us0Disable7(22),
          profile12Us0Disable8(23),
          profile12Us0Disable9(24),
          profile12Us0Disable10(25),
          profile12Us0Disable11(26),
          profile12Us0Disable12(27),
          profile12Us0Disable13(28),
          profile12Us0Disable14(29),
          profile12Us0Disable15(30),
          profile12Us0Disable16(31),
          --
          profile17Us0Disable1(32),
          profile17Us0Disable2(33),
          profile17Us0Disable3(34),
          profile17Us0Disable4(35),
          profile17Us0Disable5(36),
          profile17Us0Disable6(37),
          profile17Us0Disable7(38),
          profile17Us0Disable8(39),
          profile17Us0Disable9(40),





          profile17Us0Disable10(41),
          profile17Us0Disable11(42),
          profile17Us0Disable12(43),
          profile17Us0Disable13(44),
          profile17Us0Disable14(45),
          profile17Us0Disable15(46),
          profile17Us0Disable16(47),
          --
          profile30Us0Disable1(48),
          profile30Us0Disable2(49),
          profile30Us0Disable3(50),
          profile30Us0Disable4(51),
          profile30Us0Disable5(52),
          profile30Us0Disable6(53),
          profile30Us0Disable7(54),
          profile30Us0Disable8(55),
          profile30Us0Disable9(56),
          profile30Us0Disable10(57),
          profile30Us0Disable11(58),
          profile30Us0Disable12(59),
          profile30Us0Disable13(60),
          profile30Us0Disable14(61),
          profile30Us0Disable15(62),
          profile30Us0Disable16(63)
     }

Xdsl2LineUs0Mask ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "The US0 PSD masks to be allowed by the near-end xTU on
      the line.  This parameter is only defined for G.993.2 Annex A.
      It is represented as a bitmap (0 if not allowed and 1 if
      allowed) with the following definitions."

      SYNTAX BITS {
          eu32(0),
          eu36(1),
          eu40(2),
          eu44(3),
          eu48(4),
          eu52(5),
          eu56(6),
          eu60(7),
          --
          eu64(8),
          eu128(9),
          reserved1(10),
          reserved2(11),





          reserved3(12),
          reserved4(13),
          reserved5(14),
          reserved6(15),
          --
          adlu32(16),
          adlu36(17),
          adlu40(18),
          adlu44(19),
          adlu48(20),
          adlu52(21),
          adlu56(22),
          adlu60(23),
          --
          adlu64(24),
          adlu128(25),
          reserved7(26),
          reserved8(27),
          reserved9(28),
          reserved10(29),
          reserved11(30),
          reserved12(31)
     }

Xdsl2SymbolProtection ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type specifies the minimum impulse noise protection
       for the bearer channel if it is transported over DMT symbols
       with a subcarrier spacing of 4.3125 kHz.
       The possible values are:
       'noProtection' (i.e., INP not required), 'halfSymbol' (i.e., INP
       length is 1/2 symbol), and 1-16 symbols in steps of 1
       symbol."

   SYNTAX      INTEGER {
               noProtection (1),
               halfSymbol (2),
               singleSymbol (3),
               twoSymbols (4),
               threeSymbols (5),
               fourSymbols (6),
               fiveSymbols (7),
               sixSymbols (8),
               sevenSymbols (9),
               eightSymbols (10),
               nineSymbols (11),
               tenSymbols (12),





               elevenSymbols (13),
               twelveSymbols (14),
               thirteeSymbols (15),
               fourteenSymbols (16),
               fifteenSymbols (17),
               sixteenSymbols (18)
             }

Xdsl2SymbolProtection8 ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type specifies the minimum impulse noise protection
       for the bearer channel if it is transported over DMT symbols
       with a subcarrier spacing of 8.625 kHz.
       The possible values are:
       'noProtection' (i.e., INP not required) and 1-16 symbols in
       steps of 1 symbol."

   SYNTAX      INTEGER {
               noProtection (1),
               singleSymbol (2),
               twoSymbols (3),
               threeSymbols (4),
               fourSymbols (5),
               fiveSymbols (6),
               sixSymbols (7),
               sevenSymbols (8),
               eightSymbols (9),
               nineSymbols (10),
               tenSymbols (11),
               elevenSymbols (12),
               twelveSymbols (13),
               thirteeSymbols (14),
               fourteenSymbols (15),
               fifteenSymbols (16),
               sixteenSymbols (17)
             }

Xdsl2MaxBer ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Objects with this syntax are configuration parameters
       that reference the maximum Bit Error Rate (BER).
       The possible values are:
         eminus3 (1)  - Maximum BER=E^-3
         eminus5 (2)  - Maximum BER=E^-5
         eminus7 (3)  - Maximum BER=E^-7"
   SYNTAX      INTEGER {





                  eminus3(1),
                  eminus5(2),
                  eminus7(3)
               }

Xdsl2ChInitPolicy ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This syntax serves for channel configuration parameters
       that reference the channel initialization policy.
       The possible values are:
         policy0 (1) - Policy 0 according to the applicable standard.
         policy1 (2) - Policy 1 according to the applicable
                       standard."
   SYNTAX      INTEGER {
                  policy0(1),
                  policy1(2)
               }

Xdsl2ScMaskDs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Each one of the 4096 bits in this OCTET STRING array
       represents the corresponding subcarrier in the downstream
       direction.
       A bit value of one indicates that a subcarrier is masked."
   SYNTAX      OCTET STRING (SIZE(0..512))

Xdsl2ScMaskUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Each one of the 4096 bits in this OCTET STRING array
       represents the corresponding subcarrier in the upstream
       direction.  A bit value of one indicates that a subcarrier
       is masked."
   SYNTAX      OCTET STRING (SIZE(0..512))

Xdsl2CarMask ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type defines an array of bands.  Each band is
       represented by 4 octets and there is a maximum of 32 bands
       allowed.
       Each band consists of a 16-bit start subcarrier index followed by
       a 16-bit stop subcarrier index.
       The subcarrier index is an unsigned number in the range 0 to
       NSC-1."
   SYNTAX      OCTET STRING (SIZE(0..128))





Xdsl2RfiBands ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type defines a subset of downstream PSD mask
       breakpoints used to notch radio frequency interference (RFI)
       bands.
       Each RFI band is represented by 4 octets: a 16-bit start
       subcarrier index followed by a 16-bit stop subcarrier
       index.
       There is a maximum of 16 RFI bands allowed.
       The subcarrier index is an unsigned number in the range 0 to
       NSC-1."
   SYNTAX      OCTET STRING (SIZE(0..64))

Xdsl2PsdMaskDs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 32 PSD mask
       breakpoints.
       Each breakpoint occupies 3 octets: The first
       two octets hold the index of the subcarrier associated with the
       breakpoint.  The third octet holds the PSD reduction at the
       breakpoint from 0 (0 dBm/Hz) to 255 (-127.5 dBm/Hz) using units
       of 0.5 dBm/Hz.
       The subcarrier index is an unsigned number in the range 0 to
       NSCds-1."
   SYNTAX      OCTET STRING (SIZE(0..96))

Xdsl2PsdMaskUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 16 PSD mask
       breakpoints.
       Each breakpoint occupies 3 octets: The first two octets hold the
       index of the subcarrier associated with the breakpoint.  The
       third octet holds the PSD reduction at the breakpoint from 0
       (0 dBm/Hz) to 255 (-127.5 dBm/Hz) using units of
       0.5 dBm/Hz.
       The subcarrier index is an unsigned number in the range 0 to
       NSCus-1."
   SYNTAX      OCTET STRING (SIZE(0..48))

Xdsl2Tssi ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 32 transmit
       spectrum shaping (TSSi) breakpoints.
       Each breakpoint is a pair of values occupying 3 octets with the





       following structure:
       First 2 octets - Index of the subcarrier used in the context of
                        the breakpoint.
       Third octet    - The shaping parameter at the breakpoint.
       The shaping parameter value is in the range 0 to 126 (units of
       -0.5 dB).  The special value 127 indicates that the subcarrier is
       not transmitted.
       The subcarrier index is an unsigned number in the range 0 to
       NSC-1."
   SYNTAX      OCTET STRING (SIZE(0..96))

Xdsl2LastTransmittedState ::= TEXTUAL-CONVENTION
     STATUS current
     DESCRIPTION
        "This parameter represents the last successful transmitted
         initialization state in the last full initialization performed
         on the line.  States are per the specific xDSL technology and
         are numbered from 0 (if G.994.1 is used) or 1 (if G.994.1 is
         not used) up to Showtime."
     SYNTAX      INTEGER {
       -- ADSL family ATU-C side --
       atucG9941(0),
       atucQuiet1(1),
       atucComb1(2),
       atucQuiet2(3),
       atucComb2(4),
       atucIcomb1(5),
       atucLineprob(6),
       atucQuiet3(7),
       atucComb3(8),
       atucIComb2(9),
       atucMsgfmt(10),
       atucMsgpcb(11),
       atucQuiet4(12),
       atucReverb1(13),
       atucTref1(14),
       atucReverb2(15),
       atucEct(16),
       atucReverb3(17),
       atucTref2(18),
       atucReverb4(19),
       atucSegue1(20),
       atucMsg1(21),
       atucReverb5(22),
       atucSegue2(23),
       atucMedley(24),
       atucExchmarker(25),
       atucMsg2(26),





       atucReverb6(27),
       atucSegue3(28),
       atucParams(29),
       atucReverb7(30),
       atucSegue4(31),
       atucShowtime(32),
       -- ADSL family ATU-R side --
       aturG9941(100),
       aturQuiet1(101),
       aturComb1(102),
       aturQuiet2(103),
       aturComb2(104),
       aturIcomb1(105),
       aturLineprob(106),
       aturQuiet3(107),
       aturComb3(108),
       aturIcomb2(109),
       aturMsgfmt(110),
       aturMsgpcb(111),
       aturReverb1(112),
       aturQuiet4(113),
       aturReverb2(114),
       aturQuiet5(115),
       aturReverb3(116),
       aturEct(117),
       aturReverb4(118),
       aturSegue1(119),
       aturReverb5(120),
       aturSegue2(121),
       aturMsg1(122),
       aturMedley(123),
       aturExchmarker(124),
       aturMsg2(125),
       aturReverb6(126),
       aturSegue3(127),
       aturParams(128),
       aturReverb7(129),
       aturSegue4(130),
       aturShowtime(131),
       -- VDSL2 VTU-C side --
       vtucG9941(200),
       vtucQuiet1(201),
       vtucChDiscov1(202),
       vtucSynchro1(203),
       vtucPilot1(204),
       vtucQuiet2(205),
       vtucPeriodic1(206),
       vtucSynchro2(207),





       vtucChDiscov2(208),
       vtucSynchro3(209),
       vtucTraining1(210),
       vtucSynchro4(211),
       vtucPilot2(212),
       vtucTeq(213),
       vtucEct(214),
       vtucPilot3(215),
       vtucPeriodic2(216),
       vtucTraining2(217),
       vtucSynchro5(218),
       vtucMedley(219),
       vtucSynchro6(220),
       vtucShowtime(221),
       -- VDSL2 VTU-R side --
       vturG9941(300),
       vturQuiet1(301),
       vturChDiscov1(302),
       vturSynchro1(303),
       vturLineprobe(304),
       vturPeriodic1(305),
       vturSynchro2(306),
       vturChDiscov2(307),
       vturSynchro3(308),
       vturQuiet2(309),
       vturTraining1(310),
       vturSynchro4(311),
       vturTeq(312),
       vturQuiet3(313),
       vturEct(314),
       vturPeriodic2(315),
       vturTraining2(316),
       vturSynchro5(317),
       vturMedley(318),
       vturSynchro6(319),
       vturShowtime(320)
     }

Xdsl2LineStatus ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
      "Objects with this syntax are status parameters
       that reflect the failure status for a given endpoint of a
       VDSL2/ADSL/ADSL2 or ADSL2+ link.

       This BITS structure can report the following failures:

        noDefect (0)      - This bit position positively reports





                            that no defect or failure exist.
        lossOfFraming (1) - Loss of frame synchronization.
        lossOfSignal (2)  - Loss of signal.
        lossOfPower (3)   - Loss of power.  Usually this failure may
                            be reported for CPE units only.
        initFailure (4)   - Recent initialization process failed.
                            Never active on xTU-R."
   SYNTAX BITS {
       noDefect(0),
       lossOfFraming(1),
       lossOfSignal(2),
       lossOfPower(3),
        initFailure(4)
     }

Xdsl2ChInpReport ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type is used to indicate the method used to compute the
       Actual Impulse Noise Protection (ACTINP).  If set to
       'inpComputedUsingFormula', the ACTINP is computed
       according to the INP_no_erasure formula (9.6/G.993.2).
       If set to 'inpEstimatedByXtur', the ACTINP is the value
       estimated by the xTU receiver.
        inpComputedUsingFormula (1) - ACTINP computed using
                                      INP_no_erasure formula.
        inpEstimatedByXtur (2)      - ACTINP estimated by
                                      the xTU receiver."
   SYNTAX      INTEGER {
                  inpComputedUsingFormula(1),
                  inpEstimatedByXtur(2)
               }

Xdsl2ChAtmStatus ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "Objects with this syntax are status parameters that
      reflect the failure status for the Transmission Convergence (TC)
      layer of a given ATM interface (data path over a VDSL2/ADSL/
      ADSL2 or ADSL2+ link).

      This BITS structure can report the following failures:
       noDefect (0)             - This bit position positively
                                  reports that no defect or failure
                                  exists.
       noCellDelineation (1)    - The link was successfully
                                  initialized, but cell delineation
                                  was never acquired on the





                                  associated ATM data path.
       lossOfCellDelineation (2)- Loss of cell delineation on the
                                  associated ATM data path."
   SYNTAX BITS {
       noDefect(0),
       noCellDelineation(1),
       lossOfCellDelineation(2)
     }

Xdsl2ChPtmStatus ::= TEXTUAL-CONVENTION
   STATUS current
   DESCRIPTION
     "Objects with this syntax are status parameters that
      reflect the failure status for a given PTM interface (packet
      data path over a VDSL2/ADSL/ADSL2 or ADSL2+ link).

      This BITS structure can report the following failures:
          noDefect (0)    - This bit position positively
                            reports that no defect or failure exists.
          outOfSync (1)   - Out of synchronization."
   SYNTAX BITS {
          noDefect(0),
          outOfSync(1)
     }

Xdsl2UpboKLF ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Defines the upstream power backoff force mode (UPBOKLF).
       The three possible mode values are:
          auto(1)         - The VDSL Transceiver Unit (VTUs) will
                            autonomously determine the
                            electrical length.
          override(2)     - Forces the VTU-R to use the electrical
                            length, kl0, of the CO-MIB (UPBOKL) to
                            compute the UPBO.
          disableUpbo(3)  - Disables UPBO such that UPBO is not
                            utilized."
   SYNTAX INTEGER {
     auto(1),
     override(2),
     disableUpbo(3)
     }

Xdsl2BandUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Each value identifies a specific band in the upstream





       transmission direction (excluding the US0 band.).
       The possible values that identify a band are as follows:
          us1(5)          - Upstream band number 1 (US1).
          us2(7)          - Upstream band number 2 (US2).
          us3(9)          - Upstream band number 3 (US3).
          us4(11)         - Upstream band number 4 (US4)."
   SYNTAX        INTEGER {
     us1(5),
     us2(7),
     us3(9),
     us4(11)
     }

Xdsl2LinePsdMaskSelectUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type is used to define which upstream PSD mask is
       enabled.  This type is used only for Annexes J and M of ITU-T
       Recommendations G.992.3 and G.992.5.

       adlu32Eu32 (1),   - ADLU-32 / EU-32
       adlu36Eu36 (2),   - ADLU-36 / EU-36
       adlu40Eu40 (3),   - ADLU-40 / EU-40
       adlu44Eu44 (4),   - ADLU-44 / EU-44
       adlu48Eu48 (5),   - ADLU-48 / EU-48
       adlu52Eu52 (6),   - ADLU-52 / EU-52
       adlu56Eu56 (7),   - ADLU-56 / EU-56
       adlu60Eu60 (8),   - ADLU-60 / EU-60
       adlu64Eu64 (9)    - ADLU-64 / EU-64"
   SYNTAX        INTEGER {
     adlu32Eu32(1),
     adlu36Eu36(2),
     adlu40Eu40(3),
     adlu44Eu44(4),
     adlu48Eu48(5),
     adlu52Eu52(6),
     adlu56Eu56(7),
     adlu60Eu60(8),
     adlu64Eu64(9)
     }

Xdsl2LineCeFlag ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type is used to enable the use of the optional
       cyclic extension values.  If the bit is set to '1', the optional
       cyclic extension values may be used.  Otherwise, the cyclic
       extension shall be forced to the mandatory length (5N/32).





       enableCyclicExtension (0) - Enable use of optional
                                   Cyclic Extension values."
   SYNTAX        BITS {
     enableCyclicExtension(0)
     }

Xdsl2LineSnrMode ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type is used to enable the transmitter-referred
       virtual noise.  The value of 1, indicates that virtual
       noise is disabled.  The value of 2, indicates that virtual
       noise is enabled.

      virtualNoiseDisabled (1) - virtual noise is disabled.
      virtualNoiseEnabled (2)  - virtual noise is enabled."
   SYNTAX        INTEGER {
     virtualNoiseDisabled(1),
     virtualNoiseEnabled(2)
     }

Xdsl2LineTxRefVnDs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 32 PSD mask
       breakpoints.
       Each breakpoint occupies 3 octets: The first two octets hold the
       index of the subcarrier associated with the breakpoint.  The
       third octet holds the PSD reduction at the breakpoint from 0
       (-140 dBm/Hz) to 200 (-40 dBm/Hz) using units of 0.5 dBm/Hz.
       A special value of 255 indicates a noise level of 0 W/Hz.
       The subcarrier index is an unsigned number in the range 0 to
       NSCds-1."
   SYNTAX      OCTET STRING (SIZE(0..96))

Xdsl2LineTxRefVnUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This is a structure that represents up to 16 PSD mask
       breakpoints.
       Each breakpoint occupies 3 octets: The first two octets hold the
       index of the subcarrier associated with the breakpoint.  The
       third octet holds the PSD reduction at the breakpoint from 0
       (-140 dBm/Hz) to 200 (-40 dBm/Hz) using units of 0.5 dBm/Hz.
       A special value of 255 indicates a noise level of 0 W/Hz.
       The subcarrier index is an unsigned number in the range 0 to
       NSCus-1."
   SYNTAX      OCTET STRING (SIZE(0..48))





Xdsl2BitsAlloc ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "This type specifies an array of nibbles, where each nibble
       indicates the bits allocation for a subcarrier.
       Each nibble has a value in the range 0 to 15 to indicate
       the bits allocation."
   SYNTAX      OCTET STRING (SIZE(0..256))

Xdsl2MrefPsdDs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Objects with this syntax are MEDLEY Reference PSD status
       parameters in the downstream direction.  This is expressed as
       the set of
       breakpoints exchanged at initialization.
       The OCTET STRING contains up to 48 pairs of values in the
       following structure:
       Octets 0-1 -- Index of the first subcarrier used in the
                   context of a first breakpoint.
       Octets 2-3 -- The PSD level for the subcarrier indicated
                   in octets 0-1.
       Octets 4-7 -- Same, for a second breakpoint
       Octets 8-11 -- Same, for a third breakpoint
       And so on until
       Octets 188-191 -- Same, for a 48th breakpoint.
       The subcarrier index is an unsigned number in the range 0
       to NSCds-1.
       The PSD level is an integer value in the 0 to 4095 range.  It is
       represented in units of 0.1 dB offset from -140 dBm/Hz."
   SYNTAX      OCTET STRING (SIZE(0..192))

Xdsl2MrefPsdUs ::= TEXTUAL-CONVENTION
   STATUS      current
   DESCRIPTION
      "Objects with this syntax are MEDLEY Reference PSD status
       parameters in the upstream direction.  This is expressed
       as the set of
       breakpoints exchanged at initialization.
       The OCTET STRING contains up to 32 pairs of values in the
       following structure:
       Octets 0-1 -- Index of the first subcarrier used in the
                   context of a first breakpoint.
       Octets 2-3 -- The PSD level for the subcarrier indicated
                   in octets 0-1.
       Octets 4-7 -- Same, for a second breakpoint
       Octets 8-11 -- Same, for a third breakpoint
       And so on until





       Octets 124-127 -- Same, for a 32nd breakpoint.
       The subcarrier index is an unsigned number in the range 0
       to NSCus-1.
       The PSD level is an integer value in the 0 to 4095 range.  It is
       represented in units of 0.1 dB offset from -140 dBm/Hz."
   SYNTAX      OCTET STRING (SIZE(0..128))

END



