DLSW-MIB DEFINITIONS ::= BEGIN


IMPORTS
        DisplayString, RowStatus,
        RowPointer, TruthValue,
        TEXTUAL-CONVENTION                FROM SNMPv2-TC





        Counter32, Gauge32, TimeTicks,
        OBJECT-TYPE, MODULE-IDENTITY,
        NOTIFICATION-TYPE                 FROM SNMPv2-SMI
        MODULE-COMPLIANCE, OBJECT-GROUP,
        NOTIFICATION-GROUP                FROM SNMPv2-CONF
        ifIndex                           FROM IF-MIB
        sdlcLSAddress                     FROM SNA-SDLC-MIB;

dlsw MODULE-IDENTITY
    LAST-UPDATED  "9606040900Z"
    ORGANIZATION  "AIW DLSw MIB RIGLET and IETF DLSw MIB Working Group"
    CONTACT-INFO
                  "David D. Chen
                   IBM Corporation
                   800 Park, Highway 54
                   Research Triangle Park, NC 27709-9990
                   Tel:    1 919 254 6182
                   E-mail: dchen@vnet.ibm.com"
   DESCRIPTION
        "This MIB module contains objects to manage Data Link
         Switches."
::= { mib-2 46 }

dlswMIB         OBJECT IDENTIFIER ::= { dlsw 1 }
dlswDomains     OBJECT IDENTIFIER ::= { dlsw 2 }

-- *******************************************************************
-- Textual convention definitions
-- *******************************************************************

NBName ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
       "Represents a single qualified NetBIOS name, which can include
        `don't care' and `wildcard' characters to represent a number
        of real NetBIOS names.  If an individual character position in
        the qualified name contains a `?', the corresponding character
        position in a real NetBIOS name is a `don't care'.  If the
        qualified name ends in `*', the remainder of a real NetBIOS
        name is a `don't care'. `*' is only considered a wildcard if it
        appears at the end of a name."
    SYNTAX  OCTET STRING (SIZE (0..16))

MacAddressNC ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "1x:"
    STATUS       current
    DESCRIPTION
       "Represents an 802 MAC address represented in





        non-canonical format.  That is, the most significant
        bit will be transmitted first.  If this information
        is not available, the value is a zero length string."
    SYNTAX       OCTET STRING (SIZE (0 | 6))

TAddress ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
       "Denotes a transport service address.
        For dlswTCPDomain, a TAddress is 4 octets long,
        containing the IP-address in network-byte order."
    SYNTAX  OCTET STRING (SIZE (0..255))

EndStationLocation ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
       "Representing the location of an end station related
        to the managed DLSw node."
    SYNTAX  INTEGER  {
                other          (1),
                internal       (2),  -- local virtual MAC address
                remote         (3),  -- via DLSw partner
                local          (4)   -- locally attached
            }

DlcType ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
       "Representing the type of DLC of an end station, if
        applicable."
    SYNTAX  INTEGER  {
                other          (1),  -- not assigned yet
                na             (2),  -- not applicable
                llc            (3),  -- 802.2 Logical Link Control
                sdlc           (4),  -- SDLC
                qllc           (5)   -- QLLC
            }

LFSize  ::= TEXTUAL-CONVENTION
    STATUS  current
    DESCRIPTION
       "The largest size of the INFO field (including DLC header,
        not including any MAC-level or framing octets).
        64 valid values as defined by the IEEE 802.1D
        Addendum are acceptable."
    SYNTAX  INTEGER  {
               lfs516(516), lfs635(635), lfs754(754), lfs873(873),
               lfs993(993), lfs1112(1112), lfs1231(1231),





               lfs1350(1350), lfs1470(1470), lfs1542(1542),
               lfs1615(1615), lfs1688(1688), lfs1761(1761),
               lfs1833(1833), lfs1906(1906), lfs1979(1979),
               lfs2052(2052), lfs2345(2345), lfs2638(2638),
               lfs2932(2932), lfs3225(3225), lfs3518(3518),
               lfs3812(3812), lfs4105(4105), lfs4399(4399),
               lfs4865(4865), lfs5331(5331), lfs5798(5798),
               lfs6264(6264), lfs6730(6730), lfs7197(7197),
               lfs7663(7663), lfs8130(8130), lfs8539(8539),
               lfs8949(8949), lfs9358(9358), lfs9768(9768),
               lfs10178(10178), lfs10587(10587), lfs10997(10997),
               lfs11407(11407), lfs12199(12199), lfs12992(12992),
               lfs13785(13785), lfs14578(14578), lfs15370(15370),
               lfs16163(16163), lfs16956(16956), lfs17749(17749),
               lfs20730(20730), lfs23711(23711), lfs26693(26693),
               lfs29674(29674), lfs32655(32655), lfs38618(38618),
               lfs41600(41600), lfs44591(44591), lfs47583(47583),
               lfs50575(50575), lfs53567(53567), lfs56559(56559),
               lfs59551(59551), lfs65535(65535)
            }

null OBJECT IDENTIFIER ::= { 0 0 }


-- *******************************************************************
-- DLSw Transport Domain definitions
-- *******************************************************************

-- DLSw over TCP
dlswTCPDomain  OBJECT IDENTIFIER ::= { dlswDomains 1 }
-- for an IP address of length 4:
--
-- octets   contents        encoding
--  1-4     IP-address      network-byte order
--
DlswTCPAddress ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "1d.1d.1d.1d"
    STATUS       current
    DESCRIPTION
            "Represents the IP address of a DLSw which uses
             TCP as a transport protocol."
    SYNTAX       OCTET STRING (SIZE (4))


-- *******************************************************************
-- DLSw MIB Definition
-- *******************************************************************






-- The DLSw MIB module contains an object part and a conformance part.
-- Object part is organized in the following groups:
-- (1) dlswNode      -- information about this DLSw
-- (2) dlswTConn     -- about adjacent DLSw partners
-- (3) dlswInterface -- about which interfaces DLSw is active on
-- (4) dlswDirectory -- about any directory of local/remote resources
-- (5) dlswCircuit   -- about established circuits.
-- (6) dlswSdlc      -- about SDLC data link switched devices

dlswNode        OBJECT IDENTIFIER ::= { dlswMIB 1 }
dlswTConn       OBJECT IDENTIFIER ::= { dlswMIB 2 }
dlswInterface   OBJECT IDENTIFIER ::= { dlswMIB 3 }
dlswDirectory   OBJECT IDENTIFIER ::= { dlswMIB 4 }
dlswCircuit     OBJECT IDENTIFIER ::= { dlswMIB 5 }
dlswSdlc        OBJECT IDENTIFIER ::= { dlswMIB 6 }  -- SDLC

-- *******************************************************************
-- THE NODE GROUP
-- *******************************************************************

-- -------------------------------------------------------------------
-- DLSw Node Identity
-- -------------------------------------------------------------------
dlswNodeVersion  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (2))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This value identifies the particular version of the DLSw
        standard supported by this DLSw.  The first octet is a
        hexadecimal value representing the DLSw standard Version
        number of this DLSw, and the second is a hexadecimal value
        representing the DLSw standard Release number. This
        information is reported in DLSw Capabilities Exchange."
    REFERENCE
       "DLSW: Switch-to-Switch Protocol RFC 1795"
    ::= { dlswNode 1 }

dlswNodeVendorID  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (3))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The value identifies the manufacturer's IEEE-assigned
        organizationally Unique Identifier (OUI) of this DLSw.
        This information is reported in DLSw Capabilities
        Exchange."
    REFERENCE





       "DLSW: Switch-to-Switch Protocol RFC 1795"
    ::= { dlswNode 2 }

dlswNodeVersionString  OBJECT-TYPE
    SYNTAX     DisplayString
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This string gives product-specific information about
        this DLSw (e.g., product name, code release and fix level).
        This flows in Capabilities Exchange messages."
    REFERENCE
       "DLSW: Switch-to-Switch Protocol RFC 1795"
    ::= { dlswNode 3 }

-- -------------------------------------------------------------------
-- DLSw Code Capability
-- -------------------------------------------------------------------
dlswNodeStdPacingSupport  OBJECT-TYPE
    SYNTAX     INTEGER  {
       none              (1),  -- does not support DLSw
                               -- Standard pacing scheme
       adaptiveRcvWindow (2),  -- the receive window size
                               -- varies
       fixedRcvWindow    (3)   -- the receive window size
                               -- remains constant
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "Circuit pacing, as defined in the DLSw Standard, allows each
        of the two DLSw nodes on a circuit to control the amount
        of data the other is permitted to send to them.  This object
        reflects the level of support the DLSw node has for this
        protocol.  (1) means the node has no support for the standard
        circuit pacing flows;  it may use RFC 1434+ methods only, or
        a proprietary flow control scheme.  (2) means the node supports
        the standard scheme and can vary the window sizes it grants as
        a data receiver.  (3) means the node supports the standard
        scheme but never varies its receive window size."
    ::= { dlswNode 4 }

-- -------------------------------------------------------------------
-- DLSw Node Operational Objects
-- -------------------------------------------------------------------
dlswNodeStatus  OBJECT-TYPE
    SYNTAX     INTEGER  {
        active        (1),





        inactive      (2)
    }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "The status of the DLSw part of the system.  Changing the
        value from active to inactive causes DLSw to take
        the following actions - (1) it disconnects all circuits
        through all DLSw partners, (2) it disconnects all
        transport connections to all DLSw partners, (3) it
        disconnects all local DLC connections, and (4) it stops
        processing all DLC connection set-up traffic.
        Since these are destructive actions, the user should
        query the circuit and transport connection tables in
        advance to understand the effect this action will have.
        Changing the value from inactive to active causes DLSw
        to come up in its initial state, i.e., transport
        connections established and ready to bring up circuits."
    ::= { dlswNode 5 }

dlswNodeUpTime  OBJECT-TYPE
    SYNTAX     TimeTicks
    UNITS      "hundredths of a second"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The amount of time (in hundredths of a second) since
        the DLSw portion of the system was last re-initialized.
        That is, if dlswState is in the active state,
        the time the dlswState entered the active state.
        It will remain zero if dlswState is in the
        inactive state."
    ::= { dlswNode 6 }

dlswNodeVirtualSegmentLFSize  OBJECT-TYPE
    SYNTAX     LFSize
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "The largest frame size (including DLC header and info field
        but not any MAC-level or framing octets) this DLSw can forward
        on any path through itself.  This object can represent any box-
        level frame size forwarding restriction (e.g., from the use
        of fixed-size buffers).  Some DLSw implementations will have
        no such restriction.

        This value will affect the LF size of circuits during circuit
        creation.  The LF size of an existing circuit can be found in





        the RIF (Routing Information Field)."
    DEFVAL  { lfs65535 }
    ::= { dlswNode 7 }

-- ...................................................................
-- NETBIOS Resources
-- ...................................................................

dlswNodeResourceNBExclusivity  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "The value of true indicates that the NetBIOS Names
        configured in dlswDirNBTable are the only ones accessible
        via this DLSw.

        If a node supports sending run-time capabilities exchange
        messages, changes to this object should cause that action.
        It is up to the implementation exactly when to start the
        run-time capabilities exchange."
    ::= { dlswNode 8 }

-- ...................................................................
-- MAC Address List
-- ...................................................................

dlswNodeResourceMacExclusivity  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "The value of true indicates that the MAC addresses
        configured in the dlswDirMacTable are the only ones
        accessible via this DLSw.

        If a node supports sending run-time capabilities exchange
        messages, changes to this object should cause that action.
        It is up to the implementation exactly when to start the
        run-time capabilities exchange."
    ::= { dlswNode 9 }


-- *******************************************************************
-- TRANSPORT CONNECTION (aka: PARTNER DLSW)
-- *******************************************************************

-- -------------------------------------------------------------------





-- Transport Connection Statistics Objects
-- -------------------------------------------------------------------
dlswTConnStat    OBJECT IDENTIFIER ::= { dlswTConn 1 }

dlswTConnStatActiveConnections  OBJECT-TYPE
    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of transport connections that are not in
        `disconnected' state."
    ::= { dlswTConnStat 1 }

dlswTConnStatCloseIdles  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of times transport connections in this node
        exited the connected state with zero active circuits on
        the transport connection."
    ::= { dlswTConnStat 2 }

dlswTConnStatCloseBusys  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of times transport connections in this node
        exited the connected state with some non-zero number
        of active circuits on the transport connection.  Normally
        this means the transport connection failed unexpectedly."
    ::= { dlswTConnStat 3 }

-- -------------------------------------------------------------------
-- Transport Connection Configuration Table
-- -------------------------------------------------------------------
dlswTConnConfigTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswTConnConfigEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "This table defines the transport connections
        that will be initiated or accepted by this
        DLSw.  Structure of masks allows wildcard
        definition for a collection of transport
        connections by a conceptual row.  For a
        specific transport connection, there may





        be multiple of conceptual rows match the
        transport address.  The `best' match will
        the one to determine the characteristics
        of the transport connection."
    ::= { dlswTConn 2 }

dlswTConnConfigEntry  OBJECT-TYPE
    SYNTAX     DlswTConnConfigEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "Each conceptual row defines a collection of
        transport connections."
    INDEX   { dlswTConnConfigIndex }
    ::= { dlswTConnConfigTable 1 }

DlswTConnConfigEntry ::= SEQUENCE {
    dlswTConnConfigIndex              INTEGER,
    dlswTConnConfigTDomain            OBJECT IDENTIFIER,
    dlswTConnConfigLocalTAddr         TAddress,
    dlswTConnConfigRemoteTAddr        TAddress,
    dlswTConnConfigLastModifyTime     TimeTicks,
    dlswTConnConfigEntryType          INTEGER,
    dlswTConnConfigGroupDefinition    RowPointer,
    dlswTConnConfigSetupType          INTEGER,
    dlswTConnConfigSapList            OCTET STRING,
    dlswTConnConfigAdvertiseMacNB     TruthValue,
    dlswTConnConfigInitCirRecvWndw    INTEGER,
    dlswTConnConfigOpens              Counter32,
    dlswTConnConfigRowStatus          RowStatus
    }

dlswTConnConfigIndex  OBJECT-TYPE
    SYNTAX     INTEGER (0..2147483647)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The index to the conceptual row of the table.
        Negative numbers are not allowed.  There
        are objects defined that point to conceptual
        rows of this table with this index value.
        Zero is used to denote that no corresponding
        row exists.

        Index values are assigned by the agent, and
        should not be reused but should continue to
        increase in value."
    ::= { dlswTConnConfigEntry 1 }





dlswTConnConfigTDomain  OBJECT-TYPE
    SYNTAX     OBJECT IDENTIFIER
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The object identifier which indicates the transport
        domain of this conceptual row."
    ::= { dlswTConnConfigEntry 2 }

dlswTConnConfigLocalTAddr  OBJECT-TYPE
    SYNTAX     TAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The local transport address for this conceptual row
        of the transport connection definition."
    ::= { dlswTConnConfigEntry 3 }

dlswTConnConfigRemoteTAddr  OBJECT-TYPE
    SYNTAX     TAddress
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The remote transport address.  Together with
        dlswTConnConfigEntryType and dlswTConnConfigGroupDefinition,
        the object instance of this conceptual row identifies a
        collection of the transport connections that will be
        either initiated by this DLSw or initiated by a partner
        DLSw and accepted by this DLSw."
    ::= { dlswTConnConfigEntry 4 }

dlswTConnConfigLastModifyTime  OBJECT-TYPE
    SYNTAX     TimeTicks
    UNITS      "hundredths of a second"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The time (in hundredths of a second) since the value of
        any object in this conceptual row except for
        dlswTConnConfigOpens was last changed.  This value
        may be compared to dlswTConnOperConnectTime to
        determine whether values in this row are completely
        valid for a transport connection created using
        this row definition."
    ::= { dlswTConnConfigEntry 5 }

dlswTConnConfigEntryType  OBJECT-TYPE
    SYNTAX     INTEGER  {





        individual     (1),
        global         (2),
        group          (3)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The object instance signifies the type of entry in the
        associated conceptual row.  The value of `individual'
        means that the entry applies to a specific partner DLSw
        node as identified by dlswTConnConfigRemoteTAddr and
        dlswTConnConfigTDomain.  The value of `global'
        means that the entry applies to all partner DLSw nodes
        of the TDomain.  The value of 'group' means that the entry
        applies to a specific set of DLSw nodes in the TDomain.
        Any group definitions are enterprise-specific and are pointed
        to by dlswTConnConfigGroupDefinition.  In the cases of
        `global' and `group', the value in dlswTConnConfigRemoteTAddr
        may not have any significance."
    ::= { dlswTConnConfigEntry 6 }

dlswTConnConfigGroupDefinition OBJECT-TYPE
    SYNTAX     RowPointer
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "For conceptual rows of `individual' and `global' as
        specified in dlswTConnConfigEntryType, the instance
        of this object is  `0.0'.  For conceptual rows of
        `group', the instance points to the specific
        group definition."
    ::= { dlswTConnConfigEntry 7 }

dlswTConnConfigSetupType  OBJECT-TYPE

    SYNTAX     INTEGER  {
        other              (1),
        activePersistent   (2),
        activeOnDemand     (3),
        passive            (4),
        excluded           (5)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This value of the instance of a conceptual row
        identifies the behavior of the collection of
        transport connections that this conceptual row





        defines.  The value of activePersistent, activeOnDemand
        and passive means this DLSw will accept any transport
        connections, initiated by partner DLSw nodes, which
        are defined by this conceptual row.  The value of
        activePersistent means this DLSw will also initiate
        the transport connections of this conceptual row and
        retry periodically if necessary.  The value of
        activeOnDemand means this DLSw will initiate a
        transport connection of this conceptual row, if
        there is a directory cache hits.  The value of
        other is implementation specific.  The value of exclude
        means that the specified node is not allowed to be
        a partner to this DLSw node.  To take a certain
        conceptual row definition out of service, a value of
        notInService for dlswTConnConfigRowStatus should be
        used."
    DEFVAL  { passive }
    ::= { dlswTConnConfigEntry 8 }

dlswTConnConfigSapList  OBJECT-TYPE
    SYNTAX     OCTET STRING  (SIZE(16))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The SAP list indicates which SAPs are advertised to
        the transport connection defined by this conceptual
        row.  Only SAPs with even numbers are represented,
        in the form of the most significant bit of the first
        octet representing the SAP 0, the next most significant
        bit representing the SAP 2, to the least significant
        bit of the last octet representing the SAP 254.  Data
        link switching is allowed for those SAPs which have
        one in its corresponding bit, not allowed otherwise.
        The whole SAP list has to be changed together.  Changing
        the SAP list affects only new circuit establishments
        and has no effect on established circuits.

        This list can be used to restrict specific partners
        from knowing about all the SAPs used by DLSw on all its
        interfaces (these are represented in dlswIfSapList for
        each interface).  For instance, one may want to run NetBIOS
        with some partners but not others.

        If a node supports sending run-time capabilities exchange
        messages, changes to this object should cause that action.
        When to start the run-time capabilities exchange is
        implementation-specific.






        The DEFVAL below indicates support for SAPs 0, 4, 8, and C."
    DEFVAL  { 'AA000000000000000000000000000000'H }
    ::= { dlswTConnConfigEntry 9 }

dlswTConnConfigAdvertiseMacNB  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The value of true indicates that any defined local MAC
         addresses and NetBIOS names will be advertised to a
         partner node via initial and (if supported) run-time
         capabilities exchange messages.  The DLSw node should send
         the appropriate exclusivity control vector to accompany
         each list it sends, or to represent that the node is
         explicitly configured to have a null list.

         The value of false indicates that the DLSw node should not
         send a MAC address list or NetBIOS name list, and should
         also not send their corresponding exclusivity control
         vectors."
    DEFVAL  { true }
    ::= { dlswTConnConfigEntry 10 }

dlswTConnConfigInitCirRecvWndw  OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    UNITS      "SSP messages"
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The initial circuit receive pacing window size, in the unit
        of SSP messages, to be used for future transport connections
        activated using this table row.  The managed node sends this
        value as its initial receive pacing window in its initial
        capabilities exchange message.  Changing this value does not
        affect the initial circuit receive pacing window size of
        currently active transport connections.  If the standard window
        pacing scheme is not supported, the value is zero.

        A larger receive window value may be appropriate for partners
        that are reachable only via physical paths that have longer
        network delays."
    DEFVAL  { 1 }
    ::= { dlswTConnConfigEntry 11 }

dlswTConnConfigOpens  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only





    STATUS     current
    DESCRIPTION
       "Number of times transport connections entered
        connected state according to the definition of
        this conceptual row."
    ::= { dlswTConnConfigEntry 12 }

dlswTConnConfigRowStatus  OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This object is used by the manager to create
        or delete the row entry in the dlswTConnConfigTable
        following the RowStatus textual convention.  The value
        of notInService will be used to take a conceptual
        row definition out of use."
    ::= { dlswTConnConfigEntry 13 }

-- -------------------------------------------------------------------
-- Transport Connection Operation Table
-- -------------------------------------------------------------------
-- (1) At most one transport connection can be connected between
--     this DLSw and one of its DLSw partners at a given time.
-- (2) Multiple transport types are supported.
-- (3) Since the entries may be reused, dlswTConnOperEntryTime
--     needs to be consulted for the possibility of counter reset.
-- -------------------------------------------------------------------

dlswTConnOperTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswTConnOperEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "A list of transport connections.   It is optional but
        desirable for the agent to keep an entry for some
        period of time after the transport connection is
        disconnected.  This allows the manager to capture
        additional useful information about the connection, in
        particular, statistical information and the cause of the
        disconnection."
    ::= { dlswTConn 3 }

dlswTConnOperEntry  OBJECT-TYPE
    SYNTAX     DlswTConnOperEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION





       ""
    INDEX   { dlswTConnOperTDomain, dlswTConnOperRemoteTAddr }
    ::= { dlswTConnOperTable 1 }

DlswTConnOperEntry ::= SEQUENCE {
    dlswTConnOperTDomain                  OBJECT IDENTIFIER,
    dlswTConnOperLocalTAddr               TAddress,
    dlswTConnOperRemoteTAddr              TAddress,

    dlswTConnOperEntryTime                TimeTicks,
    dlswTConnOperConnectTime              TimeTicks,
    dlswTConnOperState                    INTEGER,
    dlswTConnOperConfigIndex              INTEGER,
    dlswTConnOperFlowCntlMode             INTEGER,

    dlswTConnOperPartnerVersion           OCTET STRING,
    dlswTConnOperPartnerVendorID          OCTET STRING,
    dlswTConnOperPartnerVersionStr        DisplayString,
    dlswTConnOperPartnerInitPacingWndw    INTEGER,

    dlswTConnOperPartnerSapList           OCTET STRING,
    dlswTConnOperPartnerNBExcl            TruthValue,
    dlswTConnOperPartnerMacExcl           TruthValue,
    dlswTConnOperPartnerNBInfo            INTEGER,
    dlswTConnOperPartnerMacInfo           INTEGER,

    dlswTConnOperDiscTime                 TimeTicks,
    dlswTConnOperDiscReason               INTEGER,
    dlswTConnOperDiscActiveCir            INTEGER,

    dlswTConnOperInDataPkts               Counter32,
    dlswTConnOperOutDataPkts              Counter32,
    dlswTConnOperInDataOctets             Counter32,
    dlswTConnOperOutDataOctets            Counter32,

    dlswTConnOperInCntlPkts               Counter32,
    dlswTConnOperOutCntlPkts              Counter32,

    dlswTConnOperCURexSents               Counter32,
    dlswTConnOperICRexRcvds               Counter32,
    dlswTConnOperCURexRcvds               Counter32,
    dlswTConnOperICRexSents               Counter32,

    dlswTConnOperNQexSents                Counter32,
    dlswTConnOperNRexRcvds                Counter32,
    dlswTConnOperNQexRcvds                Counter32,
    dlswTConnOperNRexSents                Counter32,






    dlswTConnOperCirCreates               Counter32,
    dlswTConnOperCircuits                 Gauge32
    }

dlswTConnOperTDomain  OBJECT-TYPE
    SYNTAX     OBJECT IDENTIFIER
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The object identifier indicates the transport domain
        of this transport connection."
    ::= { dlswTConnOperEntry 1 }

dlswTConnOperLocalTAddr  OBJECT-TYPE
    SYNTAX     TAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The local transport address for this transport connection.
        This value could be different from dlswTConnConfigLocalAddr,
        if the value of the latter were changed after this transport
        connection was established."
    ::= { dlswTConnOperEntry 2 }

dlswTConnOperRemoteTAddr  OBJECT-TYPE
    SYNTAX     TAddress
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The remote transport address of this transport connection."
    ::= { dlswTConnOperEntry 3 }

dlswTConnOperEntryTime  OBJECT-TYPE
    SYNTAX     TimeTicks
    UNITS      "hundredths of a second"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The amount of time (in hundredths of a second) since this
        transport connection conceptual row was created."
    ::= { dlswTConnOperEntry 4 }

-- ...................................................................
-- DLSw Transport Connection Operational Objects
-- ...................................................................

dlswTConnOperConnectTime  OBJECT-TYPE
    SYNTAX     TimeTicks





    UNITS      "hundredths of a second"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The amount of time (in hundredths of a second) since this
        transport connection last entered the 'connected' state.
        A value of zero means this transport connection has never
        been established."
    ::= { dlswTConnOperEntry 5 }

dlswTConnOperState  OBJECT-TYPE
    SYNTAX     INTEGER  {
        connecting         (1),
        initCapExchange    (2),
        connected          (3),
        quiescing          (4),
        disconnecting      (5),
        disconnected       (6)
    }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "The state of this transport connection.  The transport
        connection enters `connecting' state when DLSw makes
        a connection request to the transport layer.  Once initial
        Capabilities Exchange is sent, the transport connection
        enters enters `initCapExchange' state.  When partner
        capabilities have been determined and the transport
        connection is ready for sending CanUReach (CUR) messages,
        it moves to the `connected' state.  When DLSw is in the
        process of bringing down the connection, it is in the
        `disconnecting' state.  When the transport layer
        indicates one of its connections is disconnected, the
        transport connection moves to the `disconnected' state.

        Whereas all of the values will be returned in response
        to a management protocol retrieval operation, only two
        values may be specified in a management protocol set
        operation: `quiescing' and `disconnecting'.  Changing
        the value to `quiescing' prevents new circuits from being
        established, and will cause a transport disconnect when
        the last circuit on the connection goes away.  Changing
        the value to `disconnecting' will force off all circuits
        immediately and bring the connection to `disconnected'
        state."
    ::= { dlswTConnOperEntry 6 }

dlswTConnOperConfigIndex  OBJECT-TYPE





    SYNTAX     INTEGER (0..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The value of dlswTConnConfigIndex of the dlswTConnConfigEntry
        that governs the configuration information used by this
        dlswTConnOperEntry.  The manager can therefore normally
        examine both configured and operational information
        for this transport connection.

        This value is zero if the corresponding dlswTConnConfigEntry
        was deleted after the creation of this dlswTConnOperEntry.
        If some fields in the former were changed but the conceptual
        row was not deleted, some configuration information may not
        be valid for this operational transport connection.  The
        manager can compare dlswTConnOperConnectTime and
        dlswTConnConfigLastModifyTime to determine if this condition
        exists."
    ::= { dlswTConnOperEntry 7 }

-- ...................................................................
-- Transport Connection Characteristics
-- ...................................................................

dlswTConnOperFlowCntlMode  OBJECT-TYPE
    SYNTAX     INTEGER  {
       undetermined   (1),
       pacing         (2),   -- DLSw standard flow control
       other          (3)    -- non-DLSw standard flow control
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The flow control mechanism in use on this transport connection.
        This value is undetermined (1) before the mode of flow control
        can be established on a new transport connection (i.e., after
        CapEx is sent but before Capex or other SSP control messages
        have been received).  Pacing (2) indicates that the standard
        RFC 1795 pacing mechanism is in use.  Other (3) may be either
        the RFC 1434+ xBusy mechanism operating to a back-level DLSw,
        or a vendor-specific flow control method.  Whether it is xBusy
        or not can be inferred from dlswTConnOperPartnerVersion."
    ::= { dlswTConnOperEntry 8 }

-- ...................................................................

dlswTConnOperPartnerVersion  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0 | 2))





    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This value identifies which version (first octet) and release
        (second octet) of the DLSw standard is supported by this
        partner DLSw. This information is obtained from a DLSw
        capabilities exchange message received from the partner DLSw.
        A string of zero length is returned before a Capabilities
        Exchange message is received, or if one is never received.
        A conceptual row with a dlswTConnOperState of `connected' but
        a zero length partner version indicates that the partner is
        a non-standard DLSw partner.

        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    REFERENCE
       "DLSW: Switch-to-Switch Protocol RFC 1795"
    ::= { dlswTConnOperEntry 9 }

dlswTConnOperPartnerVendorID  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0 | 3))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This value identifies the IEEE-assigned organizationally
        Unique Identifier (OUI) of the maker of this partner
        DLSw.  This information is obtained from a DLSw
        capabilities exchange message received from the partner DLSw.
        A string of zero length is returned before a Capabilities
        Exchange message is received, or if one is never received.

        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    ::= { dlswTConnOperEntry 10 }

dlswTConnOperPartnerVersionStr  OBJECT-TYPE
    SYNTAX     DisplayString (SIZE (0..253))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This value identifies the particular product version (e.g.,
        product name, code level, fix level) of this partner DLSw.
        The format of the actual version string is vendor-specific.
        This information is obtained from a DLSw capabilities exchange
        message received from the partner DLSw.
        A string of zero length is returned before a Capabilities
        Exchange message is received, if one is never received, or
        if one is received but it does not contain a version string.





        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    REFERENCE
       "DLSW: Switch-to-Switch Protocol RFC 1795"
    ::= { dlswTConnOperEntry 11 }

dlswTConnOperPartnerInitPacingWndw  OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The value of the partner initial receive pacing window.  This
        is our initial send pacing window for all new circuits on this
        transport connection, as modified and granted by the first flow
        control indication the partner sends on each circuit.
        This information is obtained from a DLSw capabilities exchange
        message received from the partner DLSw.
        A value of zero is returned before a Capabilities
        Exchange message is received, or if one is never received.

        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    REFERENCE
       "DLSW: Switch-to-Switch Protocol RFC 1795"
    ::= { dlswTConnOperEntry 12 }

-- ...................................................................

dlswTConnOperPartnerSapList  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0 | 16))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The Supported SAP List received in the capabilities
        exchange message from the partner DLSw.  This list has
        the same format described for dlswTConnConfigSapList.
        A string of zero length is returned before a Capabilities
        Exchange message is received, or if one is never received.

        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    ::= { dlswTConnOperEntry 13 }

dlswTConnOperPartnerNBExcl  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION





       "The value of true signifies that the NetBIOS names received
        from this partner in the NetBIOS name list in its capabilities
        exchange message are the only NetBIOS names reachable by
        that partner.  `False' indicates that other NetBIOS names may
        be reachable.  `False' should be returned before a Capabilities
        Exchange message is received, if one is never received, or if
        one is received without a NB Name Exclusivity CV.

        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    ::= { dlswTConnOperEntry 14 }

dlswTConnOperPartnerMacExcl  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The value of true signifies that the MAC addresses received
        from this partner in the MAC address list in its capabilities
        exchange message are the only MAC addresses reachable by
        that partner.  `False' indicates that other MAC addresses may
        be reachable.  `False' should be returned before a Capabilities
        Exchange message is received, if one is never received, or if
        one is received without a MAC Address Exclusivity CV.

        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    ::= { dlswTConnOperEntry 15 }

dlswTConnOperPartnerNBInfo  OBJECT-TYPE
    SYNTAX     INTEGER  {
       none           (1),  -- none is kept
       partial        (2),  -- partial list is kept
       complete       (3),  -- complete list is kept
       notApplicable  (4)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "It is up to this DSLw whether to keep either none, some,
        or all of the NetBIOS name list that was received in
        the capabilities exchange message sent by this partner DLSw.
        This object identifies how much information was kept by
        this DLSw.  These names are stored as userConfigured
        remote entries in dlswDirNBTable.
        A value of (4), notApplicable, should be returned before
        a Capabilities Exchange message is received, or if one is
        never received.





        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    ::= { dlswTConnOperEntry 16 }

dlswTConnOperPartnerMacInfo  OBJECT-TYPE
    SYNTAX     INTEGER  {
       none           (1),  -- none is kept
       partial        (2),  -- partial list is kept
       complete       (3),  -- complete list is kept
       notApplicable  (4)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "It is up to this DLSw whether to keep either none, some,
        or all of the MAC address list that was received in the
        capabilities exchange message sent by this partner DLSw.
        This object identifies how much information was kept by
        this DLSw.  These names are stored as userConfigured
        remote entries in dlswDirMACTable.
        A value of (4), notApplicable, should be returned before
        a Capabilities Exchange message is received, or if one is
        never received.

        If an implementation chooses to keep dlswTConnOperEntrys in
        the `disconnected' state, this value should remain unchanged."
    ::= { dlswTConnOperEntry 17 }

-- ...................................................................
-- Information about the last disconnect of this transport connection.
--   These objects make sense only for implementations that keep
--   transport connection information around after disconnection.
-- ...................................................................
dlswTConnOperDiscTime  OBJECT-TYPE
    SYNTAX     TimeTicks
    UNITS      "hundredths of a second"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The amount of time (in hundredths of a second) since the
        dlswTConnOperState last entered `disconnected' state."
    ::= { dlswTConnOperEntry 18 }

dlswTConnOperDiscReason  OBJECT-TYPE
    SYNTAX     INTEGER  {
        other              (1),
        capExFailed        (2),
        transportLayerDisc (3),





        operatorCommand    (4),
        lastCircuitDiscd   (5),
        protocolError      (6)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This object signifies the reason that either prevented the
        transport connection from entering the connected state, or
        caused the transport connection to enter the disconnected
        state."
    ::= { dlswTConnOperEntry 19 }

dlswTConnOperDiscActiveCir  OBJECT-TYPE
    SYNTAX     INTEGER (0..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of circuits active (not in DISCONNECTED state)
        at the time the transport connection was last disconnected.
        This value is zero if the transport connection has never
        been connected."
    ::= { dlswTConnOperEntry 20 }

-- ...................................................................
-- Transport Connection Statistics
-- (1) Traffic counts
-- ...................................................................
dlswTConnOperInDataPkts  OBJECT-TYPE
    SYNTAX     Counter32
    UNITS      "SSP messages"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of Switch-to-Switch Protocol (SSP) messages of
        type DGRMFRAME, DATAFRAME, or INFOFRAME received on this
        transport connection."
    ::= { dlswTConnOperEntry 21 }

dlswTConnOperOutDataPkts  OBJECT-TYPE
    SYNTAX     Counter32
    UNITS      "SSP messages"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of Switch-to-Switch Protocol (SSP) messages of
        type DGRMFRAME, DATAFRAME, or INFOFRAME transmitted on this
        transport connection."





    ::= { dlswTConnOperEntry 22 }

dlswTConnOperInDataOctets  OBJECT-TYPE
    SYNTAX     Counter32
    UNITS      "octets"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number octets in Switch-to-Switch Protocol (SSP) messages
        of type DGRMFRAME, DATAFRAME, or INFOFRAME received on this
        transport connection.  Each message is counted starting with
        the first octet following the SSP message header."
    ::= { dlswTConnOperEntry 23 }

dlswTConnOperOutDataOctets  OBJECT-TYPE
    SYNTAX     Counter32
    UNITS      "octets"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number octets in Switch-to-Switch Protocol (SSP) messages
        of type DGRMFRAME, DATAFRAME, or INFOFRAME transmitted on this
        transport connection.  Each message is counted starting with
        the first octet following the SSP message header."
    ::= { dlswTConnOperEntry 24 }

dlswTConnOperInCntlPkts  OBJECT-TYPE
    SYNTAX     Counter32
    UNITS      "SSP messages"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of Switch-to-Switch Protocol (SSP) messages
        received on this transport connection which were not of
        type DGRMFRAME, DATAFRAME, or INFOFRAME."
    ::= { dlswTConnOperEntry 25 }

dlswTConnOperOutCntlPkts  OBJECT-TYPE
    SYNTAX     Counter32
    UNITS      "SSP messages"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of Switch-to-Switch Protocol (SSP) messages of
        transmitted on this transport connection which were not of
        type DGRMFRAME, DATAFRAME, or INFOFRAME."
    ::= { dlswTConnOperEntry 26 }






-- ...................................................................
-- (2) Directory activities (Explorer messages)
-- ...................................................................

dlswTConnOperCURexSents  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of CanUReach_ex messages sent on this transport
        connection."
    ::= { dlswTConnOperEntry 27 }

dlswTConnOperICRexRcvds  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of ICanReach_ex messages received on this transport
        connection."
    ::= { dlswTConnOperEntry 28 }

dlswTConnOperCURexRcvds  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of CanUReach_ex messages received on this transport
        connection."
    ::= { dlswTConnOperEntry 29 }

dlswTConnOperICRexSents  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of ICanReach_ex messages sent on this transport
        connection."
    ::= { dlswTConnOperEntry 30 }

-- ...................................................................

dlswTConnOperNQexSents  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of NetBIOS_NQ_ex (NetBIOS Name Query-explorer)





        messages sent on this transport connection."
    ::= { dlswTConnOperEntry 31 }

dlswTConnOperNRexRcvds  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of NETBIOS_NR_ex (NetBIOS Name Recognized-explorer)
        messages received on this transport connection."
    ::= { dlswTConnOperEntry 32 }

dlswTConnOperNQexRcvds  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of NETBIOS_NQ_ex messages received on this
        transport connection."
    ::= { dlswTConnOperEntry 33 }

dlswTConnOperNRexSents  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of NETBIOS_NR_ex messages sent on this transport
        connection."
    ::= { dlswTConnOperEntry 34 }

-- ...................................................................
-- (3) Circuit activities on each transport connection
-- ...................................................................
dlswTConnOperCirCreates  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of times that circuits entered `circuit_established'
        state (not counting transitions from `circuit_restart')."
    ::= { dlswTConnOperEntry 35 }

dlswTConnOperCircuits  OBJECT-TYPE
    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of currently active circuits on this transport





        connection, where `active' means not in `disconnected' state."
    ::= { dlswTConnOperEntry 36 }


-- -------------------------------------------------------------------
-- Transport Connection Specific
-- -------------------------------------------------------------------
dlswTConnSpecific OBJECT IDENTIFIER ::= { dlswTConn 4 }
dlswTConnTcp      OBJECT IDENTIFIER ::= { dlswTConnSpecific 1 }

-- ...................................................................
-- TCP Transport Connection Specific -- Configuration
-- ...................................................................
dlswTConnTcpConfigTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswTConnTcpConfigEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "This table defines the TCP transport connections that
        will be either initiated by or accepted by this DSLw.
        It augments the entries in dlswTConnConfigTable whose domain
        is dlswTCPDomain."
    ::= { dlswTConnTcp 1 }

dlswTConnTcpConfigEntry  OBJECT-TYPE
    SYNTAX     DlswTConnTcpConfigEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "Each conceptual row defines parameters that are
        specific to dlswTCPDomain transport connections."
    INDEX   { dlswTConnConfigIndex }
    ::= { dlswTConnTcpConfigTable 1 }

DlswTConnTcpConfigEntry ::= SEQUENCE {
    dlswTConnTcpConfigKeepAliveInt       INTEGER,
    dlswTConnTcpConfigTcpConnections     INTEGER,
    dlswTConnTcpConfigMaxSegmentSize     INTEGER
    }

dlswTConnTcpConfigKeepAliveInt  OBJECT-TYPE
    SYNTAX     INTEGER (0..1800)
    UNITS      "seconds"
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The time in seconds between TCP keepAlive messages when
        no traffic is flowing.  Zero signifies no keepAlive protocol.





        Changes take effect only for new TCP connections."
    DEFVAL  { 0 }
    ::= { dlswTConnTcpConfigEntry 1 }

dlswTConnTcpConfigTcpConnections  OBJECT-TYPE
    SYNTAX     INTEGER (1..16)
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This is our preferred number of TCP connections within a
        TCP transport connection.  The actual number used is negotiated
        at capabilities exchange time. Changes take effect only
        for new transport connections."
    DEFVAL  { 2 }
    ::= { dlswTConnTcpConfigEntry 2 }

dlswTConnTcpConfigMaxSegmentSize  OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    UNITS      "packets"
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This is the number of bytes that this node is
        willing to receive over the read TCP connection(s).
        Changes take effect for new transport connections."
    DEFVAL  { 4096 }
    ::= { dlswTConnTcpConfigEntry 3 }


-- ...................................................................
-- TCP Transport Connection Specific -- Operation
-- ...................................................................
dlswTConnTcpOperTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswTConnTcpOperEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "A list of TCP transport connections.   It is optional
        but desirable for the agent to keep an entry for some
        period of time after the transport connection is
        disconnected.  This allows the manager to capture
        additional useful information about the connection, in
        particular, statistical information and the cause of the
        disconnection."
    ::= { dlswTConnTcp 2 }

dlswTConnTcpOperEntry  OBJECT-TYPE
    SYNTAX     DlswTConnTcpOperEntry





    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       ""
    INDEX   { dlswTConnOperTDomain, dlswTConnOperRemoteTAddr }
    ::= { dlswTConnTcpOperTable 1 }

DlswTConnTcpOperEntry ::= SEQUENCE {
    dlswTConnTcpOperKeepAliveInt             INTEGER,
    dlswTConnTcpOperPrefTcpConnections       INTEGER,
    dlswTConnTcpOperTcpConnections           INTEGER
    }

dlswTConnTcpOperKeepAliveInt  OBJECT-TYPE
    SYNTAX     INTEGER (0..1800)
    UNITS      "seconds"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The time in seconds between TCP keepAlive messages when
        no traffic is flowing.  Zero signifies no keepAlive protocol is
        operating."
    ::= { dlswTConnTcpOperEntry 1 }

dlswTConnTcpOperPrefTcpConnections  OBJECT-TYPE
    SYNTAX     INTEGER (1..16)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This is the number of TCP connections preferred by this DLSw
        partner, as received in its capabilities exchange message."
    ::= { dlswTConnTcpOperEntry 2 }


dlswTConnTcpOperTcpConnections  OBJECT-TYPE
    SYNTAX     INTEGER (1..16)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This is the actual current number of TCP connections within
        this transport connection."
    ::= { dlswTConnTcpOperEntry 3 }

-- *******************************************************************
-- DLSW INTERFACE GROUP
-- *******************************************************************

dlswIfTable  OBJECT-TYPE





    SYNTAX     SEQUENCE OF DlswIfEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The list of interfaces on which DLSw is active."
    ::= { dlswInterface 1 }

dlswIfEntry  OBJECT-TYPE
    SYNTAX     DlswIfEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       ""
    INDEX   { ifIndex }
    ::= { dlswIfTable 1 }

DlswIfEntry ::= SEQUENCE {
    dlswIfRowStatus      RowStatus,
    dlswIfVirtualSegment INTEGER,
    dlswIfSapList        OCTET STRING
    }

dlswIfRowStatus  OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This object is used by the manager to create
        or delete the row entry in the dlswIfTable
        following the RowStatus textual convention."
    ::= { dlswIfEntry 1 }

dlswIfVirtualSegment  OBJECT-TYPE
    SYNTAX     INTEGER (0..4095 | 65535)
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The segment number that uniquely identifies the virtual
        segment to which this DLSw interface is connected.
        Current source routing protocols limit this value to
        the range 0 - 4095. (The value 0 is used by some
        management applications for special test cases.)
        A value of 65535 signifies that no virtual segment
        is assigned to this interface.  For instance,
        in a non-source routing environment, segment number
        assignment is not required."
    DEFVAL { 65535 }
    ::= { dlswIfEntry 2 }





dlswIfSapList  OBJECT-TYPE
    SYNTAX     OCTET STRING  (SIZE(16))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The SAP list indicates which SAPs are allowed to be
        data link switched through this interface.  This list
        has the same format described for dlswTConnConfigSapList.

        When changes to this object take effect is implementation-
        specific.  Turning off a particular SAP can destroy
        active circuits that are using that SAP.  An agent
        implementation may reject such changes until there are no
        active circuits if it so chooses.  In this case, it is up
        to the manager to close the circuits first, using
        dlswCircuitState.

        The DEFVAL below indicates support for SAPs 0, 4, 8, and C."
    DEFVAL  { 'AA000000000000000000000000000000'H }
    ::= { dlswIfEntry 3 }


-- *******************************************************************
-- DIRECTORY
-- Directory services caches the locations of MAC addresses
-- and NetBIOS names.  For resources which are attached via
-- local interfaces, the ifIndex may be cached, and for
-- resources which are reachable via a DLSw partner, the
-- transport address of the DLSw partner is cached.
-- *******************************************************************

-- -------------------------------------------------------------------
-- Directory Related Statistical Objects
-- -------------------------------------------------------------------
dlswDirStat     OBJECT IDENTIFIER ::= { dlswDirectory 1 }

dlswDirMacEntries  OBJECT-TYPE
    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The current total number of entries in the dlswDirMacTable."
    ::= { dlswDirStat 1 }

dlswDirMacCacheHits  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current





    DESCRIPTION
       "The number of times a cache search for a particular MAC address
        resulted in success."
    ::= { dlswDirStat 2 }

dlswDirMacCacheMisses  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of times a cache search for a particular MAC address
        resulted in failure."
    ::= { dlswDirStat 3 }

dlswDirMacCacheNextIndex  OBJECT-TYPE
    SYNTAX     INTEGER (0..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The next value of dlswDirMacIndex to be assigned by
        the agent.  A retrieval of this object atomically reserves
        the returned value for use by the manager to create a row
        in dlswDirMacTable.  This makes it possible for the agent
        to control the index space of the MAC address cache, yet
        allows the manager to administratively create new rows."
    ::= { dlswDirStat 4 }

dlswDirNBEntries  OBJECT-TYPE
    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The current total number of entries in the dlswDirNBTable."
    ::= { dlswDirStat 5 }

dlswDirNBCacheHits  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of times a cache search for a particular NetBIOS
        name resulted in success."
    ::= { dlswDirStat 6 }

dlswDirNBCacheMisses  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current





    DESCRIPTION
       "The number of times a cache search for a particular NetBIOS
        name resulted in failure."
    ::= { dlswDirStat 7 }

dlswDirNBCacheNextIndex  OBJECT-TYPE
    SYNTAX     INTEGER (0..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The next value of dlswDirNBIndex to be assigned by the
        agent.  A retrieval of this object atomically reserves
        the returned value for use by the manager to create
        a row in dlswDirNBTable.  This makes it possible for the
        agent to control the index space for the NetBIOS name
        cache, yet allows the manager to administratively
        create new rows."
    ::= { dlswDirStat 8 }

-- -------------------------------------------------------------------
-- Directory Cache
-- -------------------------------------------------------------------
dlswDirCache     OBJECT IDENTIFIER ::= { dlswDirectory 2 }

-- ...................................................................
-- Directory for MAC Addresses.
-- All Possible combinations of values of these objects.
--
--     EntryType   LocationType       Location        Status
--  -------------- ------------ ------------------ --------------
--  userConfigured    local     ifEntry or 0.0     reachable, or
--                                                 notReachable, or
--                                                 unknown
--  userConfigured    remote    TConnConfigEntry   reachable, or
--                                                 notReachable, or
--                                                 unknown
--  partnerCapExMsg   remote    TConnOperEntry     unknown
--  dynamic           local     ifEntry or 0.0     reachable
--  dynamic           remote    TConnOperEntry     reachable
--
-- ...................................................................
dlswDirMacTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswDirMacEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "This table contains locations of MAC addresses.
        They could be either verified or not verified,





        local or remote, and configured locally or learned
        from either Capabilities Exchange messages or
        directory searches."
    ::= { dlswDirCache 1 }

dlswDirMacEntry  OBJECT-TYPE
    SYNTAX     DlswDirMacEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "Indexed by dlswDirMacIndex."
    INDEX   { dlswDirMacIndex }
    ::= { dlswDirMacTable 1 }

DlswDirMacEntry ::= SEQUENCE {
    dlswDirMacIndex          INTEGER,
    dlswDirMacMac            MacAddressNC,
    dlswDirMacMask           MacAddressNC,
    dlswDirMacEntryType      INTEGER,
    dlswDirMacLocationType   INTEGER,
    dlswDirMacLocation       RowPointer,
    dlswDirMacStatus         INTEGER,
    dlswDirMacLFSize         LFSize,
    dlswDirMacRowStatus      RowStatus
    }

dlswDirMacIndex  OBJECT-TYPE
    SYNTAX     INTEGER (0..2147483647)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "Uniquely identifies a conceptual row of this table."
    ::= { dlswDirMacEntry 1 }

dlswDirMacMac  OBJECT-TYPE
    SYNTAX     MacAddressNC
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The MAC address, together with the dlswDirMacMask,
        specifies a set of MAC addresses that are defined or
        discovered through an interface or partner DLSw nodes."
    ::= { dlswDirMacEntry 2 }

dlswDirMacMask  OBJECT-TYPE
    SYNTAX     MacAddressNC
    MAX-ACCESS read-create
    STATUS     current





    DESCRIPTION
       "The MAC address mask, together with the dlswDirMacMac,
        specifies a set of MAC addresses that are defined or
        discovered through an interface or partner DLSw nodes."
    DEFVAL { 'FFFFFFFFFFFF'H }
    ::= { dlswDirMacEntry 3 }

dlswDirMacEntryType  OBJECT-TYPE
    SYNTAX     INTEGER  {
        other                    (1),
        userConfiguredPublic     (2),
        userConfiguredPrivate    (3),
        partnerCapExMsg          (4),
        dynamic                  (5)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The cause of the creation of this conceptual row.
        It could be one of the three methods: (1) user
        configured, including via management protocol
        set operations, configuration file, command line
        or equivalent methods; (2) learned from the
        partner DLSw Capabilities Exchange messages;
        and (3) dynamic, e.g., learned from ICanReach
        messages, or LAN explorer frames.  Since only
        individual MAC addresses can be dynamically learned,
        dynamic entries will all have a mask of all FFs.

        The public versus private distinction for user-
        configured resources applies only to local resources
        (UC remote resources are private), and indicates
        whether that resource should be advertised in
        capabilities exchange messages sent by this node."
    DEFVAL { userConfiguredPublic }
    ::= { dlswDirMacEntry 4 }

dlswDirMacLocationType  OBJECT-TYPE
    SYNTAX     INTEGER  {
        other                 (1),
        local                 (2),
        remote                (3)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The location of the resource (or a collection of
        resources using a mask) of this conceptual row





        is either (1) local - the resource is reachable
        via an interface, or (2) remote - the resource
        is reachable via a partner DLSw node (or a set
        of partner DLSw nodes)."
    DEFVAL { local }
    ::= { dlswDirMacEntry 5 }

dlswDirMacLocation  OBJECT-TYPE
    SYNTAX     RowPointer
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "Points to either the ifEntry, dlswTConnConfigEntry,
        dlswTConnOperEntry, 0.0, or something that is implementation
        specific.  It identifies the location of the MAC address
        (or the collection of MAC addresses.)"
    DEFVAL { null }
    ::= { dlswDirMacEntry 6 }

dlswDirMacStatus  OBJECT-TYPE
    SYNTAX     INTEGER  {
        unknown               (1),
        reachable             (2),
        notReachable          (3)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This object specifies whether DLSw currently believes
        the MAC address to be accessible at the specified location.
        The value `notReachable' allows a configured resource
        definition to be taken out of service when a search to
        that resource fails (avoiding a repeat of the search)."
    DEFVAL { unknown }
    ::= { dlswDirMacEntry 7 }

dlswDirMacLFSize  OBJECT-TYPE
    SYNTAX     LFSize
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The largest size of the MAC INFO field (LLC header and data)
        that a circuit to the MAC address can carry through this path."
    DEFVAL { lfs65535 }
    ::= { dlswDirMacEntry 8 }

dlswDirMacRowStatus  OBJECT-TYPE
    SYNTAX     RowStatus





    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This object is used by the manager to create
        or delete the row entry in the dlswDirMacTable
        following the RowStatus textual convention."
    ::= { dlswDirMacEntry 9 }

-- ...................................................................
-- Directory for NetBIOS Names
-- All Possible combinations of values of these objects.
--
--     EntryType   LocationType       Location        Status
--  -------------- ------------ ------------------ --------------
--  userConfigured    local     ifEntry or 0.0     reachable, or
--                                                 notReachable, or
--                                                 unknown
--  userConfigured    remote    TConnConfigEntry   reachable, or
--                                                 notReachable, or
--                                                 unknown
--  partnerCapExMsg   remote    TConnOperEntry     unknown
--  dynamic           local     ifEntry or 0.0     reachable
--  dynamic           remote    TConnOperEntry     reachable
--
-- ...................................................................
dlswDirNBTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswDirNBEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "This table contains locations of NetBIOS names.
        They could be either verified or not verified,
        local or remote, and configured locally or learned
        from either Capabilities Exchange messages or
        directory searches."
    ::= { dlswDirCache 2 }

dlswDirNBEntry  OBJECT-TYPE
    SYNTAX     DlswDirNBEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "Indexed by dlswDirNBIndex."
    INDEX   { dlswDirNBIndex }
    ::= { dlswDirNBTable 1 }

DlswDirNBEntry ::= SEQUENCE {
    dlswDirNBIndex           INTEGER,





    dlswDirNBName            NBName,
    dlswDirNBNameType        INTEGER,
    dlswDirNBEntryType       INTEGER,
    dlswDirNBLocationType    INTEGER,
    dlswDirNBLocation        RowPointer,
    dlswDirNBStatus          INTEGER,
    dlswDirNBLFSize          LFSize,
    dlswDirNBRowStatus       RowStatus
    }

dlswDirNBIndex  OBJECT-TYPE
    SYNTAX     INTEGER (0..2147483647)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "Uniquely identifies a conceptual row of this table."
    ::= { dlswDirNBEntry 1 }

dlswDirNBName  OBJECT-TYPE
    SYNTAX     NBName
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The NetBIOS name (including `any char' and `wildcard'
        characters) specifies a set of NetBIOS names that are
        defined or discovered through an interface or partner
        DLSw nodes."
    ::= { dlswDirNBEntry 2 }

dlswDirNBNameType  OBJECT-TYPE
    SYNTAX     INTEGER  {
        unknown       (1),
        individual    (2),
        group         (3)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "Whether dlswDirNBName represents an (or a set of) individual
        or group NetBIOS name(s)."
    DEFVAL { unknown }
    ::= { dlswDirNBEntry 3 }

dlswDirNBEntryType  OBJECT-TYPE
    SYNTAX     INTEGER  {
        other                    (1),
        userConfiguredPublic     (2),
        userConfiguredPrivate    (3),





        partnerCapExMsg          (4),
        dynamic                  (5)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The cause of the creation of this conceptual row.
        It could be one of the three methods: (1) user
        configured, including via management protocol
        set operations, configuration file, command line,
        or equivalent methods; (2) learned from the
        partner DLSw Capabilities Exchange messages;
        and (3) dynamic, e.g., learned from ICanReach
        messages, or test frames.  Since only actual
        NetBIOS names can be dynamically learned, dynamic
        entries will not contain any char or wildcard
        characters.

        The public versus private distinction for user-
        configured resources applies only to local resources
        (UC remote resources are private), and indicates
        whether that resource should be advertised in
        capabilities exchange messages sent by this node."
    DEFVAL { userConfiguredPublic }
    ::= { dlswDirNBEntry 4 }

dlswDirNBLocationType  OBJECT-TYPE
    SYNTAX     INTEGER  {
        other                 (1),
        local                 (2),
        remote                (3)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The location of the resource (or a collection of resources
        using any char/wildcard characters) of this conceptual row
        is either (1) local - the resource is reachable via an
        interface, or (2) remote - the resource is reachable via a
        a partner DLSw node (or a set of partner DLSw nodes)."
    DEFVAL { local }
    ::= { dlswDirNBEntry 5 }

dlswDirNBLocation  OBJECT-TYPE
    SYNTAX     RowPointer
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION





       "Points to either the ifEntry, dlswTConnConfigEntry,
        dlswTConnOperEntry, 0.0, or something that is implementation
        specific.  It identifies the location of the NetBIOS name
        or the set of NetBIOS names."
    DEFVAL { null }
    ::= { dlswDirNBEntry 6 }

dlswDirNBStatus  OBJECT-TYPE
    SYNTAX     INTEGER  {
        unknown               (1),
        reachable             (2),
        notReachable          (3)
    }
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This object specifies whether DLSw currently believes
        the NetBIOS name to be accessible at the specified location.
        The value `notReachable' allows a configured resource
        definition to be taken out of service when a search to
        that resource fails (avoiding a repeat of the search)."
    DEFVAL { unknown }
    ::= { dlswDirNBEntry 7 }

dlswDirNBLFSize  OBJECT-TYPE
    SYNTAX     LFSize
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The largest size of the MAC INFO field (LLC header and data)
        that a circuit to the NB name can carry through this path."
    DEFVAL { lfs65535 }
    ::= { dlswDirNBEntry 8 }

dlswDirNBRowStatus  OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This object is used by manager to create
        or delete the row entry in the dlswDirNBTable
        following the RowStatus textual convention."
    ::= { dlswDirNBEntry 9 }


-- -------------------------------------------------------------------
-- Resource Locations
-- -------------------------------------------------------------------





dlswDirLocate       OBJECT IDENTIFIER ::= { dlswDirectory 3 }

-- ...................................................................
-- Locate Entries in the dlswDirMacTable for a given MAC address
-- ...................................................................
dlswDirLocateMacTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswDirLocateMacEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "This table is used to retrieve all entries in the
        dlswDirMacTable that match a given MAC address,
        in the order of the best matched first, the
        second best matched second, and so on, till
        no more entries match the given MAC address."
    ::= { dlswDirLocate 1 }

dlswDirLocateMacEntry  OBJECT-TYPE
    SYNTAX     DlswDirLocateMacEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "Indexed by dlswDirLocateMacMac and dlswDirLocateMacMatch.
        The first object is the MAC address of interest, and
        the second object is the order in the list of all
        entries that match the MAC address."
    INDEX   { dlswDirLocateMacMac, dlswDirLocateMacMatch }
    ::= { dlswDirLocateMacTable 1 }

DlswDirLocateMacEntry ::= SEQUENCE {
    dlswDirLocateMacMac            MacAddressNC,
    dlswDirLocateMacMatch          INTEGER,
    dlswDirLocateMacLocation       RowPointer
    }

dlswDirLocateMacMac  OBJECT-TYPE
    SYNTAX     MacAddressNC
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The MAC address to be located."
    ::= { dlswDirLocateMacEntry 1 }

dlswDirLocateMacMatch  OBJECT-TYPE
    SYNTAX     INTEGER (1..255)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION





       "The order of the entries of dlswDirMacTable
        that match dlswDirLocateMacMac.  A value of
        one represents the entry that best matches the
        MAC address.  A value of two represents the second
        best matched entry, and so on."
    ::= { dlswDirLocateMacEntry 2 }

dlswDirLocateMacLocation  OBJECT-TYPE
    SYNTAX     RowPointer
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "Points to the dlswDirMacEntry."
    ::= { dlswDirLocateMacEntry 3 }

-- ...................................................................
-- Locate Entries in the dlswDirNBTable for a given NetBIOS name
-- ...................................................................
dlswDirLocateNBTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswDirLocateNBEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "This table is used to retrieve all entries in the
        dlswDirNBTable that match a given NetBIOS name,
        in the order of the best matched first, the
        second best matched second, and so on, till
        no more entries match the given NetBIOS name."
    ::= { dlswDirLocate 2 }

dlswDirLocateNBEntry  OBJECT-TYPE
    SYNTAX     DlswDirLocateNBEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "Indexed by dlswDirLocateNBName and dlswDirLocateNBMatch.
        The first object is the NetBIOS name of interest, and
        the second object is the order in the list of all
        entries that match the NetBIOS name."
    INDEX   { dlswDirLocateNBName, dlswDirLocateNBMatch }
    ::= { dlswDirLocateNBTable 1 }

DlswDirLocateNBEntry ::= SEQUENCE {
    dlswDirLocateNBName           NBName,
    dlswDirLocateNBMatch          INTEGER,
    dlswDirLocateNBLocation       RowPointer
    }






dlswDirLocateNBName  OBJECT-TYPE
    SYNTAX     NBName
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The NetBIOS name to be located (no any char or wildcards)."
    ::= { dlswDirLocateNBEntry 1 }

dlswDirLocateNBMatch  OBJECT-TYPE
    SYNTAX     INTEGER (1..255)
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The order of the entries of dlswDirNBTable
        that match dlswDirLocateNBName.  A value of
        one represents the entry that best matches the
        NetBIOS name.  A value of two represents the second
        best matched entry, and so on."
    ::= { dlswDirLocateNBEntry 2 }

dlswDirLocateNBLocation  OBJECT-TYPE
    SYNTAX     RowPointer
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "Points to the dlswDirNBEntry."
    ::= { dlswDirLocateNBEntry 3 }


-- *******************************************************************
-- CIRCUIT
-- A circuit is the end-to-end association of two DLSw entities
-- through one or two DLSw nodes.  It is the concatenation of
-- two "data links", optionally with an intervening transport
-- connection. The origin of the circuit is the end station that
-- initiates the circuit.  The target of the circuit is the end
-- station that receives the initiation.
-- *******************************************************************

-- -------------------------------------------------------------------
-- Statistics Related to Circuits
-- -------------------------------------------------------------------
dlswCircuitStat      OBJECT IDENTIFIER ::= { dlswCircuit 1 }

dlswCircuitStatActives  OBJECT-TYPE
    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current





    DESCRIPTION
       "The current number of circuits in dlswCircuitTable that are
        not in the disconnected state."
    ::= { dlswCircuitStat 1 }

dlswCircuitStatCreates  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The total number of entries ever added to dlswCircuitTable,
        or reactivated upon exiting `disconnected' state."
    ::= { dlswCircuitStat 2 }


-- -------------------------------------------------------------------
-- Circuit Table
--
-- This table is the DLSw entity's view of circuits.  There will be
-- a conceptual row in the table associated with each data link.
--
-- The chart below lists the various possible combinations of
-- origin and target MAC locations and the number of entries in
-- this Circuit Table:
--
--           number of       |    Origin End Station Location
--         entries in the    |--------------------------------------
--         Circuit Table     |  internal     local       remote
--    -----------------------|--------------------------------------
--     Target    |  internal |     NA          2           1
--     End       |  local    |     2           2           1
--     Station   |  remote   |     1           1           NA
--     Location  |           |
--
--     NA: Not applicable
--
--  Note:
--  (a) IfIndex and RouteInfo are applied only if location is local.
--  (b) TDomain and TAddr are applied only if location is remote.
--
-- Most of statistics related to circuits can be collected
-- from LLC-2 Link Station Table.
-- -------------------------------------------------------------------
dlswCircuitTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswCircuitEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION





       "This table is the circuit representation in the DLSw
        entity. Virtual data links are used to represent any internal
        end stations.  There is a conceptual row associated with
        each data link.  Thus, for circuits without an intervening
        transport connection, there are two conceptual rows
        for each circuit.

        The table consists of the circuits being established,
        established, and as an implementation option, circuits that
        have been disconnected.  For circuits carried over
        transport connections, an entry is created after
        the CUR_cs was sent or received.  For circuits between
        two locally attached devices, or internal virtual MAC
        addresses, an entry is created when the equivalent of
        CUR_cs sent/received status is reached.

        End station 1 (S1) and End station 2 (S2) are used to
        represent the two end stations of the circuit.
        S1 is always an end station which is locally attached.
        S2 may be locally attached or remote.  If it is locally
        attached, the circuit will be represented by two rows indexed
        by (A, B) and (B, A) where A & B are the relevant MACs/SAPs.

        The table may be used to store the causes of disconnection of
        circuits.  It is recommended that the oldest disconnected
        circuit entry be removed from this table when the memory
        space of disconnected circuits is needed."
    ::= { dlswCircuit 2 }

dlswCircuitEntry  OBJECT-TYPE
    SYNTAX     DlswCircuitEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       ""
    INDEX   { dlswCircuitS1Mac,
              dlswCircuitS1Sap,
              dlswCircuitS2Mac,
              dlswCircuitS2Sap }
    ::= { dlswCircuitTable 1 }

DlswCircuitEntry ::= SEQUENCE {
    dlswCircuitS1Mac                MacAddressNC,
    dlswCircuitS1Sap                OCTET STRING,
    dlswCircuitS1IfIndex            INTEGER,
    dlswCircuitS1DlcType            DlcType,
    dlswCircuitS1RouteInfo          OCTET STRING,
    dlswCircuitS1CircuitId          OCTET STRING,





    dlswCircuitS1Dlc                RowPointer,

    dlswCircuitS2Mac                MacAddressNC,
    dlswCircuitS2Sap                OCTET STRING,
    dlswCircuitS2Location           EndStationLocation,
    dlswCircuitS2TDomain            OBJECT IDENTIFIER,
    dlswCircuitS2TAddress           TAddress,
    dlswCircuitS2CircuitId          OCTET STRING,

    dlswCircuitOrigin               INTEGER,

    dlswCircuitEntryTime            TimeTicks,
    dlswCircuitStateTime            TimeTicks,
    dlswCircuitState                INTEGER,

    dlswCircuitPriority             INTEGER,

    dlswCircuitFCSendGrantedUnits   INTEGER,
    dlswCircuitFCSendCurrentWndw    INTEGER,
    dlswCircuitFCRecvGrantedUnits   INTEGER,
    dlswCircuitFCRecvCurrentWndw    INTEGER,
    dlswCircuitFCLargestRecvGranted Gauge32,
    dlswCircuitFCLargestSendGranted Gauge32,
    dlswCircuitFCHalveWndwSents     Counter32,
    dlswCircuitFCResetOpSents       Counter32,
    dlswCircuitFCHalveWndwRcvds     Counter32,
    dlswCircuitFCResetOpRcvds       Counter32,
    dlswCircuitDiscReasonLocal      INTEGER,
    dlswCircuitDiscReasonRemote     INTEGER,
    dlswCircuitDiscReasonRemoteData OCTET STRING
    }

-- ...................................................................
-- Information related to the End Station 1 (S1).
-- ...................................................................
dlswCircuitS1Mac  OBJECT-TYPE
    SYNTAX     MacAddressNC
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The MAC Address of End Station 1 (S1) used for this circuit."
    ::= { dlswCircuitEntry 1 }

dlswCircuitS1Sap  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(1))
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION





       "The SAP at End Station 1 (S1) used for this circuit."
    ::= { dlswCircuitEntry 2 }

dlswCircuitS1IfIndex  OBJECT-TYPE
    SYNTAX     INTEGER (0..2147483647)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The ifEntry index of the local interface through which S1
        can be reached."
    ::= { dlswCircuitEntry 3 }

dlswCircuitS1DlcType  OBJECT-TYPE
    SYNTAX     DlcType
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The DLC protocol in use between the DLSw node and S1."
    ::= { dlswCircuitEntry 4 }

dlswCircuitS1RouteInfo  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0..30))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "If source-route bridging is in use between the DLSw
        node and S1, this is the routing information field
        describing the path between the two devices.
        Otherwise the value will be an OCTET STRING of
        zero length."
    ::= { dlswCircuitEntry 5 }

dlswCircuitS1CircuitId  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0 | 8))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The Circuit ID assigned by this DLSw node to this circuit.
        The first four octets are the DLC port Id, and
        the second four octets are the Data Link Correlator.
        If the DLSw SSP was not used to establish this circuit,
        the value will be a string of zero length."
    ::= { dlswCircuitEntry 6 }

dlswCircuitS1Dlc  OBJECT-TYPE
    SYNTAX     RowPointer
    MAX-ACCESS read-only
    STATUS     current





    DESCRIPTION
       "Points to a conceptual row of the underlying DLC MIB,
        which could either be the standard MIBs (e.g., the SDLC),
        or an enterprise-specific DLC MIB."
    ::= { dlswCircuitEntry 7 }

-- ...................................................................
-- Information related to the End Station 2 (S2).
-- ...................................................................
dlswCircuitS2Mac  OBJECT-TYPE
    SYNTAX     MacAddressNC
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The MAC Address of End Station 2 (S2) used for this circuit."
    ::= { dlswCircuitEntry 8 }

dlswCircuitS2Sap  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(1))
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The SAP at End Station 2 (S2) used for this circuit."
    ::= { dlswCircuitEntry 9 }

dlswCircuitS2Location  OBJECT-TYPE
    SYNTAX     EndStationLocation
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The location of End Station 2 (S2).
        If the location of End Station 2 is local, the
        interface information will be available in the
        conceptual row whose S1 and S2 are the S2 and
        the S1 of this conceptual row, respectively."
    ::= { dlswCircuitEntry 10 }

dlswCircuitS2TDomain  OBJECT-TYPE
    SYNTAX     OBJECT IDENTIFIER
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "If the location of End Station 2 is remote,
        this value is the transport domain of the
        transport protocol the circuit is running
        over.  Otherwise, the value is 0.0."
    ::= { dlswCircuitEntry 11 }






dlswCircuitS2TAddress  OBJECT-TYPE
    SYNTAX     TAddress
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "If the location of End Station 2 is remote,
        this object contains the address of the partner
        DLSw, else it will be an OCTET STRING of zero length."
    ::= { dlswCircuitEntry 12 }

dlswCircuitS2CircuitId  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0 | 8))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The Circuit ID assigned to this circuit by the partner
        DLSw node.  The first four octets are the DLC port Id, and
        the second four octets are the Data Link Correlator.
        If the DLSw SSP was not used to establish this circuit,
        the value will be a string of zero length."
    ::= { dlswCircuitEntry 13 }

-- ...................................................................
dlswCircuitOrigin  OBJECT-TYPE
    SYNTAX     INTEGER  {
        s1             (1),
        s2             (2)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "This object specifies which of the two end stations
        initiated the establishment of this circuit."
    ::= { dlswCircuitEntry 14 }

-- ...................................................................
-- Operational information related to this circuit.
-- ...................................................................
dlswCircuitEntryTime  OBJECT-TYPE
    SYNTAX     TimeTicks
    UNITS      "hundredths of a second"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The amount of time (in hundredths of a second) since this
        circuit table conceptual row was created."
    ::= { dlswCircuitEntry 15 }






dlswCircuitStateTime  OBJECT-TYPE
    SYNTAX     TimeTicks
    UNITS      "hundredths of a second"
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The amount of time (in hundredths of a second) since this
        circuit entered the current state."
    ::= { dlswCircuitEntry 16 }

dlswCircuitState  OBJECT-TYPE
    SYNTAX     INTEGER  {
        disconnected           (1),
        circuitStart           (2),
        resolvePending         (3),
        circuitPending         (4),
        circuitEstablished     (5),
        connectPending         (6),
        contactPending         (7),
        connected              (8),
        disconnectPending      (9),
        haltPending            (10),
        haltPendingNoack       (11),
        circuitRestart         (12),
        restartPending         (13)
    }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "The current state of this circuit.  The agent, implementation
        specific, may choose to keep entries for some period of time
        after circuit disconnect, so the manager can gather the time
        and cause of disconnection.

        While all of the specified values may be returned from a GET
        operation, the only SETable value is `disconnectPending'.
        When this value is set, DLSw should perform the appropriate
        action given its previous state (e.g., send HALT_DL if the
        state was `connected') to bring the circuit down to the
        `disconnected' state.  Both the partner DLSw and local end
        station(s) should be notified as appropriate.

        This MIB provides no facility to re-establish a disconnected
        circuit, because in DLSw this should be an end station-driven
        function."
    ::= { dlswCircuitEntry 17 }

dlswCircuitPriority  OBJECT-TYPE





    SYNTAX     INTEGER  {
        unsupported     (1),
        low             (2),
        medium          (3),
        high            (4),
        highest         (5)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The transmission priority of this circuit as understood by
        this DLSw node.  This value is determined by the two DLSw
        nodes at circuit startup time.  If this DLSw node does not
        support DLSw circuit priority, the value `unsupported' should
        be returned."
    ::= { dlswCircuitEntry 18 }

-- ...................................................................
-- Pacing Objects:
-- These objects are applicable if DLSw is using the SSP circuit
-- pacing protocol to control the flow between the two data links
-- in this circuit.
-- ...................................................................
dlswCircuitFCSendGrantedUnits  OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of paced SSP messages that this DLSw is currently
        authorized to send on this circuit before it must stop and
        wait for an additional flow control indication from the
        partner DLSw.

        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 19 }

dlswCircuitFCSendCurrentWndw  OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The current window size that this DLSw is using in its role
        as a data sender.  This is the value by which this DLSw would
        increase the number of messages it is authorized to send, if
        it were to receive a flow control indication with the bits
        specifying `repeat window'.






        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 20 }

dlswCircuitFCRecvGrantedUnits  OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The current number of paced SSP messages that this DLSw has
        authorized the partner DLSw to send on this circuit before
        the partner DLSw must stop and wait for an additional flow
        control indication from this DLSw.

        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 21 }

dlswCircuitFCRecvCurrentWndw  OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The current window size that this DLSw is using in its role
        as a data receiver.  This is the number of additional paced
        SSP messages that this DLSw would be authorizing its DLSw
        partner to send, if this DLSw were to send a flow control
        indication with the bits specifying `repeat window'.

        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 22 }

dlswCircuitFCLargestRecvGranted  OBJECT-TYPE
    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The largest receive window size granted by this DLSw during
        the current activation of this circuit.  This is not the
        largest number of messages granted at any time, but the
        largest window size as represented by FCIND operator bits.

        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 23 }

dlswCircuitFCLargestSendGranted  OBJECT-TYPE





    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The largest send (with respect to this DLSw) window size
        granted by the partner DLSw during the current activation of
        this circuit.

        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 24 }

dlswCircuitFCHalveWndwSents  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of Halve Window operations this DLSw has sent on
        this circuit, in its role as a data receiver.

        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 25 }

dlswCircuitFCResetOpSents  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of Reset Window operations this DLSw has sent on
        this circuit, in its role as a data receiver.

        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 26 }

dlswCircuitFCHalveWndwRcvds  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of Halve Window operations this DLSw has received on
        this circuit, in its role as a data sender.

        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 27 }






dlswCircuitFCResetOpRcvds  OBJECT-TYPE
    SYNTAX     Counter32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of Reset Window operations this DLSw has received on
        this circuit, in its role as a data sender.
        The value zero should be returned if this circuit is not
        running the DLSw pacing protocol."
    ::= { dlswCircuitEntry 28 }


-- ...................................................................
-- Information about the circuit disconnection
-- ...................................................................
dlswCircuitDiscReasonLocal  OBJECT-TYPE
    SYNTAX     INTEGER  {
        endStationDiscRcvd           (1),
        endStationDlcError           (2),
        protocolError                (3),
        operatorCommand              (4),
        haltDlRcvd                   (5),
        haltDlNoAckRcvd              (6),
        transportConnClosed          (7)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The reason why this circuit was last disconnected, as seen
        by this DLSw node.

        This object is present only if the agent keeps circuit
        table entries around for some period after circuit disconnect."
    ::= { dlswCircuitEntry 29 }

dlswCircuitDiscReasonRemote  OBJECT-TYPE
    SYNTAX     INTEGER  {
        unknown                      (1),
        endStationDiscRcvd           (2),
        endStationDlcError           (3),
        protocolError                (4),
        operatorCommand              (5)
    }
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The generic reason code why this circuit was last
        disconnected, as reported by the DLSw partner in a HALT_DL





        or HALT_DL_NOACK.  If the partner does not send a reason
        code in these messages, or the DLSw implementation does
        not report receiving one, the value `unknown' is returned.

        This object is present only if the agent keeps circuit table
        entries around for some period after circuit disconnect."
    ::= { dlswCircuitEntry 30 }

dlswCircuitDiscReasonRemoteData  OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0 | 4))
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "Implementation-specific data reported by the DLSw partner in
        a HALT_DL or HALT_DL_NOACK, to help specify how and why this
        circuit was last disconnected.  If the partner does not send
        this data in these messages, or the DLSw implementation does
        not report receiving it, a string of zero length is returned.

        This object is present only if the agent keeps circuit table
        entries around for some period after circuit disconnect."
    ::= { dlswCircuitEntry 31 }


-- ...................................................................
-- Statistics related to this circuit.
-- All statistics are in LLC-2 Link Station Statistical Table.
-- All SDLC statistics are in SDLC MIB
-- ...................................................................


-- *******************************************************************
-- DLSW SDLC EXTENSION
-- *******************************************************************
dlswSdlcLsEntries  OBJECT-TYPE
    SYNTAX     Gauge32
    MAX-ACCESS read-only
    STATUS     current
    DESCRIPTION
       "The number of entries in dlswSdlcLsTable."
    ::= { dlswSdlc 1 }

-- ...................................................................
dlswSdlcLsTable  OBJECT-TYPE
    SYNTAX     SEQUENCE OF DlswSdlcLsEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION





       "The table defines the virtual MAC addresses for those
        SDLC link stations that participate in data link switching."
    ::= { dlswSdlc 2 }

dlswSdlcLsEntry  OBJECT-TYPE
    SYNTAX     DlswSdlcLsEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
       "The index of this table is the ifIndex value for the
        SDLC port which owns this link station and the poll
        address of the particular SDLC link station."
    INDEX  { ifIndex, sdlcLSAddress }
    ::= { dlswSdlcLsTable 1 }

DlswSdlcLsEntry ::= SEQUENCE {
    dlswSdlcLsLocalMac           MacAddressNC,
    dlswSdlcLsLocalSap           OCTET STRING,
    dlswSdlcLsLocalIdBlock       DisplayString,
    dlswSdlcLsLocalIdNum         DisplayString,
    dlswSdlcLsRemoteMac          MacAddressNC,
    dlswSdlcLsRemoteSap          OCTET STRING,
    dlswSdlcLsRowStatus          RowStatus
    }

dlswSdlcLsLocalMac    OBJECT-TYPE
    SYNTAX     MacAddressNC
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The virtual MAC address used to represent the SDLC-attached
        link station to the rest of the DLSw network."
    ::= { dlswSdlcLsEntry 1 }

dlswSdlcLsLocalSap    OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE(1))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The SAP used to represent this link station."
    ::= { dlswSdlcLsEntry 2 }

dlswSdlcLsLocalIdBlock OBJECT-TYPE
    SYNTAX     DisplayString  (SIZE (0 | 3))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The block number is the first three digits of the node_id,





        if available.  These 3 hexadecimal digits identify the
        product."
    DEFVAL { ''H }
    ::= { dlswSdlcLsEntry 3 }

dlswSdlcLsLocalIdNum OBJECT-TYPE
    SYNTAX     DisplayString  (SIZE (0 | 5))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The ID number is the last 5 digits of the node_id, if
        available.  These 5 hexadecimal digits are
        administratively defined and combined with the 3 digit
        block number form the node_id.  This node_id is used to
        identify the local node and is included in SNA XIDs."
    DEFVAL { ''H }
    ::= { dlswSdlcLsEntry 4 }

dlswSdlcLsRemoteMac    OBJECT-TYPE
    SYNTAX     MacAddressNC
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The MAC address to which DLSw should attempt to connect
        this link station. If this information is not available,
        a length of zero for this object should be returned."
    DEFVAL { ''H }
    ::= { dlswSdlcLsEntry 5 }

dlswSdlcLsRemoteSap    OBJECT-TYPE
    SYNTAX     OCTET STRING (SIZE (0 | 1))
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "The SAP of the remote station to which this link
        station should be connected.  If this information
        is not available, a length of zero for this object
        should be returned."
    DEFVAL { ''H }
    ::= { dlswSdlcLsEntry 6 }

dlswSdlcLsRowStatus    OBJECT-TYPE
    SYNTAX     RowStatus
    MAX-ACCESS read-create
    STATUS     current
    DESCRIPTION
       "This object is used by the manager to create
        or delete the row entry in the dlswSdlcLsTable





        following the RowStatus textual convention."
    ::= { dlswSdlcLsEntry 7 }


-- *******************************************************************
-- TRAP GENERATION CONTROL
-- *******************************************************************
dlswTrapControl OBJECT IDENTIFIER  ::= { dlswNode 10}

dlswTrapCntlTConnPartnerReject  OBJECT-TYPE
    SYNTAX     INTEGER  {
        enabled     (1),
        disabled    (2),
        partial     (3)
    }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "Indicates whether the DLSw is permitted to emit partner
        reject related traps.  With the value of `enabled'
        the DLSw will emit all partner reject related traps.
        With the value of `disabled' the DLSw will not emit
        any partner reject related traps.  With the value
        of `partial' the DLSw will only emits partner reject
        traps for CapEx reject.  The changes take effect
        immediately."
    ::= { dlswTrapControl 1 }

dlswTrapCntlTConnProtViolation  OBJECT-TYPE
    SYNTAX     TruthValue
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "Indicates whether the DLSw is permitted to generate
        protocol-violation traps on the events such as
        window size violation.  The changes take effect
        immediately."
    ::= { dlswTrapControl 2 }

dlswTrapCntlTConn  OBJECT-TYPE
    SYNTAX     INTEGER {
        enabled     (1),
        disabled    (2),
        partial     (3)
    }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION





       "Indicates whether the DLSw is permitted to emit transport
        connection up and down traps.  With the value of `enabled'
        the DLSw will emit traps when connections enter `connected'
        and `disconnected' states.  With the value of `disabled'
        the DLSw will not emit traps when connections enter of
        `connected' and `disconnected' states.  With the value
        of `partial' the DLSw will only emits transport connection
        down traps when the connection is closed with busy.
        The changes take effect immediately."
    ::= { dlswTrapControl 3 }

dlswTrapCntlCircuit  OBJECT-TYPE
    SYNTAX     INTEGER {
        enabled     (1),
        disabled    (2),
        partial     (3)
    }
    MAX-ACCESS read-write
    STATUS     current
    DESCRIPTION
       "Indicates whether the DLSw is permitted to generate
        circuit up and down traps.  With the value of `enabled'
        the DLSw will emit traps when circuits enter `connected'
        and `disconnected' states.  With the value of `disabled'
        the DLSw will not emit traps when circuits enter of
        `connected' and `disconnected' states.  With the value
        of `partial' the DLSw will emit traps only for those
        circuits that are initiated by this DLSw, e.g.,
        originating the CUR_CS message.  The changes take effect
        immediately."
    ::= { dlswTrapControl 4 }

-- *******************************************************************
-- NOTIFICATIONS, i.e., TRAP DEFINITIONS
-- *******************************************************************
dlswTraps              OBJECT IDENTIFIER ::= { dlswMIB 0 }

-- -------------------------------------------------------------------
-- This section defines the well-known notifications sent by
-- DLSW agents.
-- Care must be taken to insure that no particular notification
-- is sent to a single receiving entity more often than once
-- every five seconds.
--
-- Traps includes:
-- (1) Partner rejected (capEx rejection, not in partner list, etc.)
-- (2) DLSw protocol violation (e.g., window size violation, etc.)
-- (3) Transport connection up/down





-- (4) Circuit up/down
-- -------------------------------------------------------------------
--

dlswTrapTConnPartnerReject NOTIFICATION-TYPE
    OBJECTS { dlswTConnOperTDomain, dlswTConnOperRemoteTAddr
    }
    STATUS     current
    DESCRIPTION
       "This trap is sent each time a transport connection
        is rejected by a partner DLSw during Capabilities
        Exchanges.  The emission of this trap is controlled
        by dlswTrapCntlTConnPartnerReject."
    ::= { dlswTraps 1 }

dlswTrapTConnProtViolation NOTIFICATION-TYPE
    OBJECTS { dlswTConnOperTDomain, dlswTConnOperRemoteTAddr
    }
    STATUS     current
    DESCRIPTION
       "This trap is sent each time a protocol violation is
        detected for a transport connection.  The emission of this
        trap is controlled by dlswTrapCntlTConnProtViolation."
    ::= { dlswTraps 2 }

dlswTrapTConnUp NOTIFICATION-TYPE
    OBJECTS { dlswTConnOperTDomain, dlswTConnOperRemoteTAddr
    }
    STATUS     current
    DESCRIPTION
       "This trap is sent each time a transport connection
        enters `connected' state.  The emission of this trap
        is controlled by dlswTrapCntlTConn."
    ::= { dlswTraps 3 }

dlswTrapTConnDown NOTIFICATION-TYPE
    OBJECTS { dlswTConnOperTDomain, dlswTConnOperRemoteTAddr
    }
    STATUS     current
    DESCRIPTION
       "This trap is sent each time a transport connection
        enters `disconnected' state.  The emission of this trap
        is controlled by dlswTrapCntlTConn."
    ::= { dlswTraps 4 }

dlswTrapCircuitUp NOTIFICATION-TYPE
    OBJECTS { dlswCircuitS1Mac, dlswCircuitS1Sap,
              dlswCircuitS2Mac, dlswCircuitS2Sap





    }
    STATUS     current
    DESCRIPTION
       "This trap is sent each time a circuit enters `connected'
        state.  The emission of this trap is controlled by
        dlswTrapCntlCircuit."
    ::= { dlswTraps 5 }

dlswTrapCircuitDown NOTIFICATION-TYPE
    OBJECTS { dlswCircuitS1Mac, dlswCircuitS1Sap,
              dlswCircuitS2Mac, dlswCircuitS2Sap
    }
    STATUS     current
    DESCRIPTION
       "This trap is sent each time a circuit enters `disconnected'
        state.  The emission of this trap is controlled by
        dlswTrapCntlCircuit."
    ::= { dlswTraps 6 }


-- *******************************************************************
-- CONFORMANCE INFORMATION
-- *******************************************************************
dlswConformance        OBJECT IDENTIFIER ::= { dlsw 3 }

dlswCompliances        OBJECT IDENTIFIER ::= { dlswConformance 1 }
dlswGroups             OBJECT IDENTIFIER ::= { dlswConformance 2 }

-- -------------------------------------------------------------------
-- COMPLIANCE STATEMENTS
-- -------------------------------------------------------------------

-- ...................................................................
-- Core compliance for all DLSw entities
-- ...................................................................
dlswCoreCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
       "The core compliance statement for all DLSw nodes."
    MODULE
        MANDATORY-GROUPS  {
                dlswNodeGroup,
                dlswTConnStatGroup,
                dlswTConnConfigGroup,
                dlswTConnOperGroup,
                dlswInterfaceGroup,
                dlswCircuitGroup,
                dlswCircuitStatGroup,





                dlswNotificationGroup }

        GROUP dlswNodeNBGroup
            DESCRIPTION
               "The DLSw NetBIOS Node group is mandatory only for
                those DLSw entities that implement NetBIOS."

        GROUP dlswTConnNBGroup
            DESCRIPTION
               "The DLSw NetBIOS Transport Connection group is
                mandatory only for those DLSw entities that
                implement NetBIOS."

        OBJECT  dlswNodeStatus
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswNodeVirtualSegmentLFSize
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswNodeResourceNBExclusivity
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswNodeResourceMacExclusivity
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTrapCntlTConnPartnerReject
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTrapCntlTConnProtViolation
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTrapCntlTConn
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."






        OBJECT  dlswTrapCntlCircuit
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigTDomain
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigLocalTAddr
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigRemoteTAddr
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigEntryType
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigGroupDefinition
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigSetupType
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigSapList
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigAdvertiseMacNB
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnConfigInitCirRecvWndw
            MIN-ACCESS  read-only
            DESCRIPTION





                "Write access is not required."

        OBJECT  dlswTConnConfigRowStatus
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnOperState
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswIfRowStatus
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswIfVirtualSegment
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswIfSapList
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswCircuitState
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

    ::= { dlswCompliances 1 }

-- ...................................................................
-- Compliance for all DLSw entities that provide TCP transport.
-- ...................................................................
dlswTConnTcpCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
       "Compliance for DLSw nodes that use TCP as a
        transport connection protocol."
    MODULE
        MANDATORY-GROUPS  {
                dlswTConnTcpConfigGroup,
                dlswTConnTcpOperGroup }

        OBJECT  dlswTConnTcpConfigKeepAliveInt





            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnTcpConfigTcpConnections
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswTConnTcpConfigMaxSegmentSize
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

    ::= { dlswCompliances 2 }

-- ...................................................................
-- Compliance for all DLSw Entities that implement a directory
-- ...................................................................
dlswDirCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
       "Compliance for DLSw nodes that provide a directory
        function."
    MODULE
        MANDATORY-GROUPS  {
                dlswDirGroup }

        GROUP dlswDirNBGroup
            DESCRIPTION
               "The DLSw NetBIOS group is mandatory only for
                those DLSw entities that implement NetBIOS."

        OBJECT  dlswDirMacMac
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirMacMask
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirMacEntryType
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."






        OBJECT  dlswDirMacLocationType
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirMacLocation
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirMacStatus
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirMacLFSize
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirMacRowStatus
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirNBName
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirNBNameType
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirNBEntryType
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirNBLocationType
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirNBLocation
            MIN-ACCESS  read-only
            DESCRIPTION





                "Write access is not required."

        OBJECT  dlswDirNBStatus
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirNBLFSize
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

        OBJECT  dlswDirNBRowStatus
            MIN-ACCESS  read-only
            DESCRIPTION
                "Write access is not required."

    ::= { dlswCompliances 3 }

-- ...................................................................
-- Compliance for all DLSw entities that provide an ordered
-- list of directory entries that match a resource
-- ...................................................................
dlswDirLocateCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
       "Compliance for DLSw nodes that provide an ordered
        list of directory entries for a given resource."
    MODULE
        MANDATORY-GROUPS  {
                dlswDirLocateGroup }

        GROUP dlswDirLocateNBGroup
            DESCRIPTION
               "The DLSw NetBIOS group is mandatory only for
                those DLSw entities that implement NetBIOS."

    ::= { dlswCompliances 4 }

-- ...................................................................
-- Compliance for all DLSw entities that support SDLC end stations
-- ...................................................................
dlswSdlcCompliance MODULE-COMPLIANCE
    STATUS current
    DESCRIPTION
       "Compliance for DLSw nodes that support SDLC."
    MODULE
        MANDATORY-GROUPS  {





                dlswSdlcGroup }

        OBJECT  dlswSdlcLsLocalMac
            MIN-ACCESS  read-only
            DESCRIPTION
               "Write access is not required."

        OBJECT  dlswSdlcLsLocalSap
            MIN-ACCESS  read-only
            DESCRIPTION
               "Write access is not required."

        OBJECT  dlswSdlcLsLocalIdBlock
            MIN-ACCESS  read-only
            DESCRIPTION
               "Write access is not required."

        OBJECT  dlswSdlcLsLocalIdNum
            MIN-ACCESS  read-only
            DESCRIPTION
               "Write access is not required."

        OBJECT  dlswSdlcLsRemoteMac
            MIN-ACCESS  read-only
            DESCRIPTION
               "Write access is not required."

        OBJECT  dlswSdlcLsRemoteSap
            MIN-ACCESS  read-only
            DESCRIPTION
               "Write access is not required."

        OBJECT  dlswSdlcLsRowStatus
            MIN-ACCESS  read-only
            DESCRIPTION
               "Write access is not required."

    ::= { dlswCompliances 5 }

-- -------------------------------------------------------------------
-- CONFORMANCE GROUPS
-- -------------------------------------------------------------------

-- ...................................................................
-- Node Conformance Group
-- ...................................................................
dlswNodeGroup  OBJECT-GROUP
    OBJECTS  {





        dlswNodeVersion,
        dlswNodeVendorID,
        dlswNodeVersionString,
        dlswNodeStdPacingSupport,
        dlswNodeStatus,
        dlswNodeUpTime,
        dlswNodeVirtualSegmentLFSize,
        dlswNodeResourceMacExclusivity,
        dlswTrapCntlTConnPartnerReject,
        dlswTrapCntlTConnProtViolation,
        dlswTrapCntlTConn,
        dlswTrapCntlCircuit
        }
    STATUS current
    DESCRIPTION
       "Conformance group for DLSw node general information."
    ::= { dlswGroups 1 }

-- ...................................................................
dlswNodeNBGroup  OBJECT-GROUP
    OBJECTS  {
        dlswNodeResourceNBExclusivity
        }
    STATUS current
    DESCRIPTION
       "Conformance group for DLSw node general information
        specifically for nodes that support NetBIOS."
    ::= { dlswGroups 2 }

-- ...................................................................
dlswTConnStatGroup  OBJECT-GROUP
    OBJECTS  {
        dlswTConnStatActiveConnections,
        dlswTConnStatCloseIdles,
        dlswTConnStatCloseBusys
        }
    STATUS current
    DESCRIPTION
       "Conformance group for statistics for transport
        connections."
    ::= { dlswGroups 3 }

-- ...................................................................
dlswTConnConfigGroup  OBJECT-GROUP
    OBJECTS  {
        dlswTConnConfigTDomain,
        dlswTConnConfigLocalTAddr,
        dlswTConnConfigRemoteTAddr,





        dlswTConnConfigLastModifyTime,
        dlswTConnConfigEntryType,
        dlswTConnConfigGroupDefinition,
        dlswTConnConfigSetupType,
        dlswTConnConfigSapList,
        dlswTConnConfigAdvertiseMacNB,
        dlswTConnConfigInitCirRecvWndw,
        dlswTConnConfigOpens,
        dlswTConnConfigRowStatus
        }
    STATUS current
    DESCRIPTION
       "Conformance group for the configuration of
        transport connections."
    ::= { dlswGroups 4 }

-- ...................................................................
dlswTConnOperGroup  OBJECT-GROUP
    OBJECTS  {
        dlswTConnOperLocalTAddr,
        dlswTConnOperEntryTime,
        dlswTConnOperConnectTime,
        dlswTConnOperState,
        dlswTConnOperConfigIndex,
        dlswTConnOperFlowCntlMode,
        dlswTConnOperPartnerVersion,
        dlswTConnOperPartnerVendorID,
        dlswTConnOperPartnerVersionStr,
        dlswTConnOperPartnerInitPacingWndw,
        dlswTConnOperPartnerSapList,
        dlswTConnOperPartnerMacExcl,
        dlswTConnOperPartnerMacInfo,
        dlswTConnOperDiscTime,
        dlswTConnOperDiscReason,
        dlswTConnOperDiscActiveCir,
        dlswTConnOperInDataPkts,
        dlswTConnOperOutDataPkts,
        dlswTConnOperInDataOctets,
        dlswTConnOperOutDataOctets,
        dlswTConnOperInCntlPkts,
        dlswTConnOperOutCntlPkts,
        dlswTConnOperCURexSents,
        dlswTConnOperICRexRcvds,
        dlswTConnOperCURexRcvds,
        dlswTConnOperICRexSents,
        dlswTConnOperCirCreates,
        dlswTConnOperCircuits
        }





    STATUS current
    DESCRIPTION
       "Conformance group for operation information for
        transport connections."
    ::= { dlswGroups 5 }
-- ...................................................................
dlswTConnNBGroup  OBJECT-GROUP
    OBJECTS  {
        dlswTConnOperPartnerNBExcl,
        dlswTConnOperPartnerNBInfo,
        dlswTConnOperNQexSents,
        dlswTConnOperNRexRcvds,
        dlswTConnOperNQexRcvds,
        dlswTConnOperNRexSents
        }
    STATUS current
    DESCRIPTION
       "Conformance group for operation information for
        transport connections, specifically for nodes
        that support NetBIOS."
    ::= { dlswGroups 6 }

-- ...................................................................
dlswTConnTcpConfigGroup  OBJECT-GROUP
    OBJECTS  {
        dlswTConnTcpConfigKeepAliveInt,
        dlswTConnTcpConfigTcpConnections,
        dlswTConnTcpConfigMaxSegmentSize
        }
    STATUS current
    DESCRIPTION
       "Conformance group for configuration information for
        transport connections using TCP."
    ::= { dlswGroups 7 }

-- ...................................................................
dlswTConnTcpOperGroup  OBJECT-GROUP
    OBJECTS  {
        dlswTConnTcpOperKeepAliveInt,
        dlswTConnTcpOperPrefTcpConnections,
        dlswTConnTcpOperTcpConnections
        }
    STATUS current
    DESCRIPTION
       "Conformance group for operation information for
        transport connections using TCP."
    ::= { dlswGroups 8 }






-- ...................................................................
dlswInterfaceGroup  OBJECT-GROUP
    OBJECTS  {
        dlswIfRowStatus,
        dlswIfVirtualSegment,
        dlswIfSapList
        }
    STATUS current
    DESCRIPTION
       "Conformance group for DLSw interfaces."
    ::= { dlswGroups 9 }

-- ...................................................................
dlswDirGroup  OBJECT-GROUP
    OBJECTS  {
        dlswDirMacEntries,
        dlswDirMacCacheHits,
        dlswDirMacCacheMisses,
        dlswDirMacCacheNextIndex,
        dlswDirMacMac,
        dlswDirMacMask,
        dlswDirMacEntryType,
        dlswDirMacLocationType,
        dlswDirMacLocation,
        dlswDirMacStatus,
        dlswDirMacLFSize,
        dlswDirMacRowStatus
        }
    STATUS current
    DESCRIPTION
       "Conformance group for DLSw directory using MAC
        addresses."
    ::= { dlswGroups 10 }

-- ...................................................................
dlswDirNBGroup  OBJECT-GROUP
    OBJECTS  {
        dlswDirNBEntries,
        dlswDirNBCacheHits,
        dlswDirNBCacheMisses,
        dlswDirNBCacheNextIndex,
        dlswDirNBName,
        dlswDirNBNameType,
        dlswDirNBEntryType,
        dlswDirNBLocationType,
        dlswDirNBLocation,
        dlswDirNBStatus,
        dlswDirNBLFSize,





        dlswDirNBRowStatus
        }
    STATUS current
    DESCRIPTION
       "Conformance group for DLSw directory using NetBIOS
        names."
    ::= { dlswGroups 11 }

-- ...................................................................
dlswDirLocateGroup  OBJECT-GROUP
    OBJECTS  {
        dlswDirLocateMacLocation
        }
    STATUS current
    DESCRIPTION
       "Conformance group for a node that can return directory
        entry order for a given MAC address."
    ::= { dlswGroups 12 }

-- ...................................................................
dlswDirLocateNBGroup  OBJECT-GROUP
    OBJECTS  {
        dlswDirLocateNBLocation
        }
    STATUS current
    DESCRIPTION
       "Conformance group for a node that can return directory
        entry order for a given NetBIOS name."
    ::= { dlswGroups 13 }

-- ...................................................................
dlswCircuitStatGroup  OBJECT-GROUP
    OBJECTS  {
        dlswCircuitStatActives,
        dlswCircuitStatCreates
        }
    STATUS current
    DESCRIPTION
       "Conformance group for statistics about circuits."
    ::= { dlswGroups 14 }

-- ...................................................................
dlswCircuitGroup  OBJECT-GROUP
    OBJECTS  {
        dlswCircuitS1IfIndex,
        dlswCircuitS1DlcType,
        dlswCircuitS1RouteInfo,
        dlswCircuitS1CircuitId,





        dlswCircuitS1Dlc,
        dlswCircuitS2Location,
        dlswCircuitS2TDomain,
        dlswCircuitS2TAddress,
        dlswCircuitS2CircuitId,
        dlswCircuitOrigin,
        dlswCircuitEntryTime,
        dlswCircuitStateTime,
        dlswCircuitState,
        dlswCircuitPriority,
        dlswCircuitFCSendGrantedUnits,
        dlswCircuitFCSendCurrentWndw,
        dlswCircuitFCRecvGrantedUnits,
        dlswCircuitFCRecvCurrentWndw,
        dlswCircuitFCLargestRecvGranted,
        dlswCircuitFCLargestSendGranted,
        dlswCircuitFCHalveWndwSents,
        dlswCircuitFCResetOpSents,
        dlswCircuitFCHalveWndwRcvds,
        dlswCircuitFCResetOpRcvds,
        dlswCircuitDiscReasonLocal,
        dlswCircuitDiscReasonRemote,
        dlswCircuitDiscReasonRemoteData
        }
    STATUS current
    DESCRIPTION
       "Conformance group for DLSw circuits."
    ::= { dlswGroups 15 }

-- ...................................................................
dlswSdlcGroup  OBJECT-GROUP
    OBJECTS  {
        dlswSdlcLsEntries,
        dlswSdlcLsLocalMac,
        dlswSdlcLsLocalSap,
        dlswSdlcLsLocalIdBlock,
        dlswSdlcLsLocalIdNum,
        dlswSdlcLsRemoteMac,
        dlswSdlcLsRemoteSap,
        dlswSdlcLsRowStatus
        }
    STATUS current
    DESCRIPTION
       "Conformance group for DLSw SDLC support."
    ::= { dlswGroups 16 }

-- ...................................................................
dlswNotificationGroup  NOTIFICATION-GROUP





    NOTIFICATIONS  {
        dlswTrapTConnPartnerReject,
        dlswTrapTConnProtViolation,
        dlswTrapTConnUp,
        dlswTrapTConnDown,
        dlswTrapCircuitUp,
        dlswTrapCircuitDown
        }
    STATUS current
    DESCRIPTION
       "Conformance group for DLSw notifications."
    ::= { dlswGroups 17 }

END






































