TE-LINK-STD-MIB DEFINITIONS ::= BEGIN


   IMPORTS
      MODULE-IDENTITY, OBJECT-TYPE, transmission, Integer32, Unsigned32
         FROM SNMPv2-SMI

      MODULE-COMPLIANCE, OBJECT-GROUP
         FROM SNMPv2-CONF

      TEXTUAL-CONVENTION, RowStatus, StorageType
         FROM SNMPv2-TC

      InterfaceIndexOrZero, ifIndex
         FROM IF-MIB

      InetAddressType, InetAddress
         FROM INET-ADDRESS-MIB;


   teLinkStdMIB MODULE-IDENTITY
      LAST-UPDATED "200510110000Z"  -- 11 October 2005
      ORGANIZATION "Multiprotocol Label Switching (MPLS) Working Group"
      CONTACT-INFO
          "        Martin Dubuc
           Email:  mdubuc@ncf.ca

                   Thomas D. Nadeau
           Email:  tnadeau@cisco.com






                   Jonathan P. Lang
           Email:  jplang@ieee.org

           Comments about this document should be emailed directly to
           the MPLS working group mailing list at mpls@uu.net."

      DESCRIPTION
          "Copyright (C) 2005 The Internet Society.  This version of
           this MIB module is part of RFC 4220; see the RFC
           itself for full legal notices.

           This MIB module contains managed object definitions for
           MPLS traffic engineering links as defined in
           'Link Bundling in MPLS Traffic Engineering (TE)'."

      -- Revision history.
      REVISION
          "200510110000Z"  -- 11 October 2005
      DESCRIPTION
          "Initial version published as RFC 4220."
      ::= { transmission 200 }

   -- Textual Conventions

   TeLinkBandwidth ::= TEXTUAL-CONVENTION
      STATUS       current
      DESCRIPTION
          "This type is used to represent link bandwidth in bps.  This
           value is represented using a 4 octet IEEE floating point
           format [IEEE].  The floating point representation is not
           used to represent fractional value but rather to allow
           specification of large numbers that cannot be expressed
           with 32-bit integers."
      REFERENCE
          "IEEE Standard for Binary Floating-Point Arithmetic,
           Standard 754-1985"
      SYNTAX       OCTET STRING (SIZE(4))

   TeLinkPriority ::= TEXTUAL-CONVENTION
      DISPLAY-HINT "d"
      STATUS       current
      DESCRIPTION
          "This type is used to represent a priority.  Each connection
           is assigned a priority.  This priority is used when
           accounting for bandwidth on TE links or component
           links, for resource allocation and for rerouting purposes.
           Value 0 is the highest priority.  Value 7 is the lowest
           priority."





      SYNTAX       Unsigned32 (0..7)

   TeLinkProtection ::= TEXTUAL-CONVENTION
      STATUS       current
      DESCRIPTION
          "Link protection."
      SYNTAX       INTEGER {
                       primary(1),
                       secondary(2)
                   }

   TeLinkSwitchingCapability ::= TEXTUAL-CONVENTION
      STATUS       current
      DESCRIPTION
          "Switching capability as specified in the 'OSPF Extensions in
           Support of Generalized Multi-Protocol Label Switching
           (GMPLS)' document.  The values specified in this document
           are not contiguous."
      SYNTAX       INTEGER {
                       packetSwitch1(1),
                       packetSwitch2(2),
                       packetSwitch3(3),
                       packetSwitch4(4),
                       layer2Switch(51),
                       tdm(100),
                       lambdaSwitch(150),
                       fiberSwitch(200)
                   }

   TeLinkEncodingType ::= TEXTUAL-CONVENTION
      STATUS       current
      DESCRIPTION
          "Link encoding type as specified in 'Generalized
           Multi-Protocol Label Switching (GMPLS) Signaling
           Functional Description' document.  The values
           specified in this document are not contiguous."
      SYNTAX       INTEGER {
                       packet(1),
                       ethernet(2),
                       ansiEtsiPdh(3),
                       sdhItuSonetAnsi(5),
                       digitalWrapper(7),
                       lambda(8),
                       fiber(9),
                       fiberChannel(11)
                   }

   TeLinkSonetSdhIndication ::= TEXTUAL-CONVENTION





      STATUS       current
      DESCRIPTION
          "This convention is used to indicate whether the interface
           supports Standard or Arbitrary SONET/SDH.  To simplify the
           mapping process, the values used in this textual convention
           match the values specified in the interface switching
           capability specific information field, i.e., 0 for Standard
           SONET/SDH and 1 for Arbitrary SONET/SDH."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      SYNTAX       INTEGER {
                       standard(0),
                       arbitrary(1)
                   }

   -- Top level components of this MIB module

   -- Notifications
   teLinkNotifications OBJECT IDENTIFIER ::= { teLinkStdMIB 0 }
   -- Tables, Scalars
   teLinkObjects       OBJECT IDENTIFIER ::= { teLinkStdMIB 1 }
   -- Conformance
   teLinkConformance   OBJECT IDENTIFIER ::= { teLinkStdMIB 2 }

   -- TE Link Table

   teLinkTable OBJECT-TYPE
      SYNTAX        SEQUENCE OF TeLinkEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This table specifies the grouping of component links into
           TE links and the grouping of TE links into bundled links."
      ::= { teLinkObjects 1 }

   teLinkEntry OBJECT-TYPE
      SYNTAX        TeLinkEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "An entry in this table exists for each ifEntry with an
           ifType of teLink(200), i.e., for every TE link.  An ifEntry
           in the ifTable must exist before a teLinkEntry is created
           with the corresponding ifIndex.  If a TE link entry in the
           ifTable is destroyed, then so is the corresponding entry
           in the teLinkTable.  The administrative and operational
           status values are controlled from the ifEntry."





      INDEX         { ifIndex }
      ::= { teLinkTable 1 }

   TeLinkEntry ::= SEQUENCE {
     teLinkAddressType                 InetAddressType,
     teLinkLocalIpAddr                 InetAddress,
     teLinkRemoteIpAddr                InetAddress,
     teLinkMetric                      Unsigned32,
     teLinkMaximumReservableBandwidth  TeLinkBandwidth,
     teLinkProtectionType              INTEGER,
     teLinkWorkingPriority             TeLinkPriority,
     teLinkResourceClass               Unsigned32,
     teLinkIncomingIfId                Integer32,
     teLinkOutgoingIfId                InterfaceIndexOrZero,
     teLinkRowStatus                   RowStatus,
     teLinkStorageType                 StorageType
   }

   teLinkAddressType OBJECT-TYPE
      SYNTAX        InetAddressType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The type of Internet address for the TE link."
      ::= { teLinkEntry 1 }

   teLinkLocalIpAddr OBJECT-TYPE
      SYNTAX        InetAddress
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The local Internet address for numbered links.  The type of
           this address is determined by the value of the
           teLinkAddressType object.

           For IPv4 and IPv6 numbered links, this object represents the
           local IP address associated with the TE link.  For an
           unnumbered link, the local address is of type unknown, this
           object is set to the zero length string, and the
           teLinkOutgoingIfId object then identifies the unnumbered
           address.

           If the TE link is a Forwarding Adjacency (FA), the local
           IP address is set to the head-end address of the FA-LSP.

           If ipAddrTable is implemented, this object must have the
           same value as the ipAdEntAddr object that belongs to the
           row in ipAddrTable where ipAdEntIfIndex is equal to





           ifIndex."
      ::= { teLinkEntry 2 }

   teLinkRemoteIpAddr OBJECT-TYPE
      SYNTAX        InetAddress
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The remote Internet address for numbered links.  The type of
           this address is determined by the value of the
           teLinkAddressType object.

           The remote IP address associated with the TE link (IPv4 and
           IPv6 numbered links).  For an unnumbered link, the remote
           address is of type unknown, this object is set to the
           zero length string, and the teLinkIncomingIfId object then
           identifies the unnumbered address.

           If the TE link is a Forwarding Adjacency, the remote IP
           address is set to the tail-end address of the FA-LSP."
      ::= { teLinkEntry 3 }

   teLinkMetric OBJECT-TYPE
      SYNTAX        Unsigned32
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The traffic engineering metric for the TE link is
           derived from its component links.  All component links
           within the TE link must have the same traffic
           engineering metric."
      REFERENCE
          "Link Bundling in MPLS Traffic Engineering (TE), RFC 4201"
      ::= { teLinkEntry 4 }

   teLinkMaximumReservableBandwidth OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum reservable bandwidth on
           the TE link.  This is the union of the maximum reservable
           bandwidth of all the component links within the
           TE link that can be used to carry live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"





      ::= { teLinkEntry 5 }

   teLinkProtectionType OBJECT-TYPE
      SYNTAX        INTEGER {
                        extraTraffic(1),
                        unprotected(2),
                        shared(3),
                        dedicated1For1(4),
                        dedicated1Plus1(5),
                        enhanced(6)
                    }
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the link protection type of the
           TE link.  Descriptions of the different protection types can
           be found in the 'Routing Extensions in Support of
           Generalized Multi-Protocol Label Switching (GMPLS)'
           document."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203 and
           Routing Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4202"
      ::= { teLinkEntry 6 }

   teLinkWorkingPriority OBJECT-TYPE
      SYNTAX        TeLinkPriority
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This object represents a priority value such that a new
           connection with a higher priority, i.e., numerically lower
           than this value, is guaranteed to be setup on a primary
           link and not on a secondary link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkEntry 7 }

   teLinkResourceClass OBJECT-TYPE
      SYNTAX        Unsigned32
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the TE link resource class.
           The resource class is a 32 bit bitfield.  The resource class
           for a link bundle is derived from the resource class of its





           TE links.  All TE links within a link bundle must have the
           same resource class.  Encoding of the resource class is
           described in the 'Traffic Engineering (TE) Extensions to
           OSPF Version 2' document."
      REFERENCE
          "Link Bundling in MPLS Traffic Engineering (TE), RFC 4201
           and Traffic Engineering (TE) Extensions to OSPF Version 2,
           RFC 3630"
      ::= { teLinkEntry 8 }

   teLinkIncomingIfId OBJECT-TYPE
      SYNTAX        Integer32 (0..2147483647)
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "For unnumbered links, the incoming interface is set to the
           outgoing interface identifier chosen by the neighboring LSR
           for the reverse link corresponding to this TE link.  If the
           link is numbered, the value of this object is 0 and the
           address is stored in the teLinkRemoteIpAddr instead."
      REFERENCE
          "Link Bundling in MPLS Traffic Engineering (TE), RFC 4201"
      ::= { teLinkEntry 9 }

   teLinkOutgoingIfId OBJECT-TYPE
      SYNTAX        InterfaceIndexOrZero
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "If the link is unnumbered, the outgoing interface identifier
           is set to the outgoing interface identifier chosen for the
           TE link by the advertising LSR.  If the link is numbered, the
           value of this object is 0 and the address is stored in the
           teLinkLocalIpAddr instead."
      REFERENCE
          "Link Bundling in MPLS Traffic Engineering (TE), RFC 4201"
      ::= { teLinkEntry 10 }

   teLinkRowStatus OBJECT-TYPE
      SYNTAX        RowStatus
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This variable is used to create, modify, and/or
           delete a row in this table.  None of the writable objects in
           a row can be changed if status is active(1)."
      ::= { teLinkEntry 11 }






   teLinkStorageType OBJECT-TYPE
      SYNTAX        StorageType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The storage type for this conceptual row in the
           teLinkTable.  Conceptual rows having the value
           'permanent' need not allow write-access to any
           columnar object in the row."
      ::= { teLinkEntry 12 }

   -- End of teLinkTable


   -- TE Link Descriptor Table

   teLinkDescriptorTable OBJECT-TYPE
      SYNTAX        SEQUENCE OF TeLinkDescriptorEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This table specifies the interface switching capability
           descriptors associated with the TE links."
      ::= { teLinkObjects 2 }

   teLinkDescriptorEntry OBJECT-TYPE
      SYNTAX        TeLinkDescriptorEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "An entry in this table is created for every TE link interface
           switching capability descriptor.  An ifEntry in the ifTable
           must exist before a teLinkDescriptorEntry using the same
           ifIndex is created.  ifType of ifEntry must be teLink(200).
           If a TE link entry in the ifTable is destroyed, then so are
           all of the entries in the teLinkDescriptorTable that use the
           ifIndex of this TE link."
      INDEX         { ifIndex, teLinkDescriptorId }
      ::= { teLinkDescriptorTable 1 }

   TeLinkDescriptorEntry ::= SEQUENCE {
     teLinkDescriptorId               Unsigned32,
     teLinkDescrSwitchingCapability   TeLinkSwitchingCapability,
     teLinkDescrEncodingType          TeLinkEncodingType,
     teLinkDescrMinLspBandwidth       TeLinkBandwidth,
     teLinkDescrMaxLspBandwidthPrio0  TeLinkBandwidth,
     teLinkDescrMaxLspBandwidthPrio1  TeLinkBandwidth,
     teLinkDescrMaxLspBandwidthPrio2  TeLinkBandwidth,





     teLinkDescrMaxLspBandwidthPrio3  TeLinkBandwidth,
     teLinkDescrMaxLspBandwidthPrio4  TeLinkBandwidth,
     teLinkDescrMaxLspBandwidthPrio5  TeLinkBandwidth,
     teLinkDescrMaxLspBandwidthPrio6  TeLinkBandwidth,
     teLinkDescrMaxLspBandwidthPrio7  TeLinkBandwidth,
     teLinkDescrInterfaceMtu          Unsigned32,
     teLinkDescrIndication            TeLinkSonetSdhIndication,
     teLinkDescrRowStatus             RowStatus,
     teLinkDescrStorageType           StorageType
   }

   teLinkDescriptorId OBJECT-TYPE
      SYNTAX        Unsigned32 (1..4294967295)
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This object specifies the link descriptor identifier."
      ::= { teLinkDescriptorEntry 1 }

   teLinkDescrSwitchingCapability OBJECT-TYPE
      SYNTAX        TeLinkSwitchingCapability
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies interface switching capability of
           the TE link, which is derived from its component links."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 2 }

   teLinkDescrEncodingType OBJECT-TYPE
      SYNTAX        TeLinkEncodingType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the TE link encoding type."
      REFERENCE
          "Generalized Multi-Protocol Label Switching (GMPLS)
           Signaling Functional Description, RFC 3471"
      ::= { teLinkDescriptorEntry 3 }

   teLinkDescrMinLspBandwidth OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION





          "This attribute specifies the minimum LSP bandwidth on
           the TE link.  This is derived from the union of the
           minimum LSP bandwidth of all the component links
           associated with the TE link that can be used to carry
           live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 4 }

   teLinkDescrMaxLspBandwidthPrio0 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 0 on the TE link.  This is the union of the maximum
           LSP bandwidth at priority 0 of all the component links within
           the TE link that can be used to carry live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 5 }

   teLinkDescrMaxLspBandwidthPrio1 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 1 on the TE link.  This is the union of the maximum
           LSP bandwidth at priority 1 of all the component links within
           the TE link that can be used to carry live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 6 }

   teLinkDescrMaxLspBandwidthPrio2 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 2 on the TE link.  This is the union of the maximum





           LSP bandwidth at priority 2 of all the component links within
           the TE link that can be used to carry live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 7 }

   teLinkDescrMaxLspBandwidthPrio3 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 3 on the TE link.  This is the union of the maximum
           LSP bandwidth at priority 3 of all the component links within
           the TE link that can be used to carry live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 8 }

   teLinkDescrMaxLspBandwidthPrio4 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 4 on the TE link.  This is the union of the maximum
           LSP bandwidth at priority 4 of all the component links within
           the TE link that can be used to carry live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 9 }

   teLinkDescrMaxLspBandwidthPrio5 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 5 on the TE link.  This is the union of the maximum
           LSP bandwidth at priority 5 of all the component links within
           the TE link that can be used to carry live traffic."
      REFERENCE





          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 10 }

   teLinkDescrMaxLspBandwidthPrio6 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 6 on the TE link.  This is the union of the maximum
           LSP bandwidth at priority 6 of all the component links within
           the TE link that can be used to carry live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 11 }

   teLinkDescrMaxLspBandwidthPrio7 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 7 on the TE link.  This is the union of the maximum
           LSP bandwidth at priority 7 of all the component links within
           the TE link that can be used to carry live traffic."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 12 }

   teLinkDescrInterfaceMtu OBJECT-TYPE
      SYNTAX        Unsigned32 (1..65535)
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the interface MTU for the TE
           link descriptor."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 13 }

   teLinkDescrIndication OBJECT-TYPE
      SYNTAX        TeLinkSonetSdhIndication





      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies whether this interface supports
           Standard or Arbitrary SONET/SDH."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkDescriptorEntry 14 }

   teLinkDescrRowStatus OBJECT-TYPE
      SYNTAX        RowStatus
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This variable is used to create, modify, and/or
           delete a row in this table.  No read-create object
           can be changed if teLinkDescrRowStatus is in the active(1)
           state."
      ::= { teLinkDescriptorEntry 15 }

   teLinkDescrStorageType OBJECT-TYPE
      SYNTAX        StorageType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The storage type for this conceptual row in the
           teLinkDescriptorTable.  Conceptual rows having the value
           'permanent' need not allow write-access to any
           columnar object in the row."
      ::= { teLinkDescriptorEntry 16 }

   -- End of teLinkDescriptorTable


   -- TE Link Shared Risk Link Group Table

   teLinkSrlgTable OBJECT-TYPE
      SYNTAX        SEQUENCE OF TeLinkSrlgEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This table specifies the SRLGs associated with TE links."
      ::= { teLinkObjects 3 }

   teLinkSrlgEntry OBJECT-TYPE
      SYNTAX        TeLinkSrlgEntry
      MAX-ACCESS    not-accessible





      STATUS        current
      DESCRIPTION
          "An entry in this table contains information about an
           SRLG associated with a TE link.
           An ifEntry in the ifTable must exist before a
           teLinkSrlgEntry using the same ifIndex is created.
           The ifType of ifEntry must be teLink(200).
           If a TE link entry in the ifTable is destroyed, then so
           are all of the entries in the teLinkSrlgTable that use the
           ifIndex of this TE link."
      INDEX         { ifIndex, teLinkSrlg }
      ::= { teLinkSrlgTable 1 }

   TeLinkSrlgEntry ::= SEQUENCE {
     teLinkSrlg            Unsigned32,
     teLinkSrlgRowStatus   RowStatus,
     teLinkSrlgStorageType StorageType
   }

   teLinkSrlg OBJECT-TYPE
      SYNTAX        Unsigned32 (0..4294967295)
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This identifies an SRLG supported by the TE link.  An SRLG is
           identified with a 32-bit number that is unique within an IGP
           domain.  Zero is a valid SRLG number."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { teLinkSrlgEntry 1 }

   teLinkSrlgRowStatus OBJECT-TYPE
      SYNTAX        RowStatus
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This variable is used to create, modify, and/or
           delete a row in this table.  No read-create object can
           be modified if teLinkSrlgRowStatus is active(1)."
      ::= { teLinkSrlgEntry 2 }

   teLinkSrlgStorageType OBJECT-TYPE
      SYNTAX        StorageType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The storage type for this conceptual row in the





           teLinkSrlgTable.  Conceptual rows having the value
           'permanent' need not allow write-access to any
           columnar object in the row."
      ::= { teLinkSrlgEntry 3 }

   -- End of teLinkSrlgTable


   -- TE Link Bandwidth Table

   teLinkBandwidthTable OBJECT-TYPE
      SYNTAX        SEQUENCE OF TeLinkBandwidthEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This table specifies the priority-based bandwidth table
           for TE links."
      ::= { teLinkObjects 4 }

   teLinkBandwidthEntry OBJECT-TYPE
      SYNTAX        TeLinkBandwidthEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "An entry in this table contains information about
           the priority-based bandwidth of TE links.  An ifEntry in the
           ifTable must exist before a teLinkBandwidthEntry using the
           same ifIndex is created.  The ifType of ifEntry must be
           teLink(200).  If a TE link entry in the ifTable is destroyed,
           then so are all of the entries in the teLinkBandwidthTable
           that use the ifIndex of this TE link."
      INDEX         { ifIndex, teLinkBandwidthPriority }
      ::= { teLinkBandwidthTable 1 }

   TeLinkBandwidthEntry ::= SEQUENCE {
     teLinkBandwidthPriority    TeLinkPriority,
     teLinkBandwidthUnreserved  TeLinkBandwidth,
     teLinkBandwidthRowStatus   RowStatus,
     teLinkBandwidthStorageType StorageType
   }

   teLinkBandwidthPriority OBJECT-TYPE
      SYNTAX        TeLinkPriority
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This attribute specifies the priority.  A value of 0 is valid
           as specified in the 'Traffic Engineering (TE) Extensions to





           OSPF Version 2' document."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203 and
           Traffic Engineering (TE) Extensions to OSPF Version 2,
           RFC 3630"
      ::= { teLinkBandwidthEntry 1 }

   teLinkBandwidthUnreserved OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
          "This attribute specifies the TE link unreserved
           bandwidth at priority p.  It is the sum of the unreserved
           bandwidths at priority p of all component links associated
           with the TE link (excluding all links that are strictly
           used as protecting links)."
      REFERENCE
          "Link Bundling in MPLS Traffic Engineering (TE), RFC 4201"
      ::= { teLinkBandwidthEntry 2 }

   teLinkBandwidthRowStatus OBJECT-TYPE
      SYNTAX        RowStatus
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This variable is used to create, modify, and/or
           delete a row in this table.  No read-create object
           can be modified when teLinkBandwidthRowStatus is active(1)."
      ::= { teLinkBandwidthEntry 3 }

   teLinkBandwidthStorageType OBJECT-TYPE
      SYNTAX        StorageType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The storage type for this conceptual row in the
           teLinkBandwidthTable.  Conceptual rows having the value
           'permanent' need not allow write-access to any
           columnar object in the row."
      ::= { teLinkBandwidthEntry 4 }

   -- End of teLinkBandwidthTable


   -- Component Link Table





   componentLinkTable  OBJECT-TYPE
      SYNTAX        SEQUENCE OF ComponentLinkEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This table specifies the component link parameters."
      ::= { teLinkObjects 5 }

   componentLinkEntry  OBJECT-TYPE
      SYNTAX        ComponentLinkEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "An entry in this table exists for each ifEntry that
           represents a component link.  An ifEntry must exist in
           the ifTable before a componentLinkEntry is created with
           the corresponding ifIndex.  ifEntry's ifType can be
           of any interface type that has been defined for TE Link
           interworking.  Examples include ATM, Frame Relay, Ethernet,
           etc.  If an entry representing a component link is destroyed
           in the ifTable, then so is the corresponding entry in the
           componentLinkTable.  The administrative and operational
           status values are controlled from the ifEntry."
      INDEX         { ifIndex }
      ::= { componentLinkTable 1 }

   ComponentLinkEntry ::= SEQUENCE {
     componentLinkMaxResBandwidth     TeLinkBandwidth,
     componentLinkPreferredProtection TeLinkProtection,
     componentLinkCurrentProtection   TeLinkProtection,
     componentLinkRowStatus           RowStatus,
     componentLinkStorageType         StorageType
   }

   componentLinkMaxResBandwidth OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum reservable bandwidth on
           the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkEntry 1 }

   componentLinkPreferredProtection OBJECT-TYPE





      SYNTAX        TeLinkProtection
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies whether this component link is
           a primary or secondary entity."
      ::= { componentLinkEntry 2 }

   componentLinkCurrentProtection OBJECT-TYPE
      SYNTAX        TeLinkProtection
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
          "This attribute specifies whether this component link is
           currently used as primary or secondary link."
      ::= { componentLinkEntry 3 }

   componentLinkRowStatus OBJECT-TYPE
      SYNTAX        RowStatus
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This variable is used to create, modify, and/or
           delete a row in this table.  No read-create object
           can be modified when componentLinkRowStatus is active(1)."
      ::= { componentLinkEntry 4 }

   componentLinkStorageType OBJECT-TYPE
      SYNTAX        StorageType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The storage type for this conceptual row in the
           componentLinkTable.  Conceptual rows having the value
           'permanent' need not allow write-access to any
           columnar object in the row."
      ::= { componentLinkEntry 5 }

   -- End of componentLinkTable


   -- Component Link Descriptor Table

   componentLinkDescriptorTable OBJECT-TYPE
      SYNTAX        SEQUENCE OF ComponentLinkDescriptorEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION





          "This table specifies the interface switching capability
           descriptors associated with the component links."
      ::= { teLinkObjects 6 }

   componentLinkDescriptorEntry OBJECT-TYPE
      SYNTAX        ComponentLinkDescriptorEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "An entry in this table is created for every component link
           descriptor.  An ifEntry in the ifTable must exist before a
           componentLinkDescriptorEntry using the same ifIndex is
           created.  ifEntry's ifType can be of any interface type that
           has been defined for TE Link interworking.  Examples include
           ATM, Frame Relay, Ethernet, etc.  If a component link entry
           in the ifTable is destroyed, then so are all entries in the
           componentLinkDescriptorTable that use the ifIndex of this
           component link."
      INDEX         { ifIndex, componentLinkDescrId }
      ::= { componentLinkDescriptorTable 1 }

   ComponentLinkDescriptorEntry ::= SEQUENCE {
     componentLinkDescrId                    Unsigned32,
     componentLinkDescrSwitchingCapability   TeLinkSwitchingCapability,
     componentLinkDescrEncodingType          TeLinkEncodingType,
     componentLinkDescrMinLspBandwidth       TeLinkBandwidth,
     componentLinkDescrMaxLspBandwidthPrio0  TeLinkBandwidth,
     componentLinkDescrMaxLspBandwidthPrio1  TeLinkBandwidth,
     componentLinkDescrMaxLspBandwidthPrio2  TeLinkBandwidth,
     componentLinkDescrMaxLspBandwidthPrio3  TeLinkBandwidth,
     componentLinkDescrMaxLspBandwidthPrio4  TeLinkBandwidth,
     componentLinkDescrMaxLspBandwidthPrio5  TeLinkBandwidth,
     componentLinkDescrMaxLspBandwidthPrio6  TeLinkBandwidth,
     componentLinkDescrMaxLspBandwidthPrio7  TeLinkBandwidth,
     componentLinkDescrInterfaceMtu          Unsigned32,
     componentLinkDescrIndication            TeLinkSonetSdhIndication,
     componentLinkDescrRowStatus             RowStatus,
     componentLinkDescrStorageType           StorageType
   }

   componentLinkDescrId OBJECT-TYPE
      SYNTAX        Unsigned32 (1..4294967295)
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This object specifies the link descriptor identifier."
      ::= { componentLinkDescriptorEntry 1 }






   componentLinkDescrSwitchingCapability OBJECT-TYPE
      SYNTAX        TeLinkSwitchingCapability
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies link multiplexing capabilities of
           the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 2 }

   componentLinkDescrEncodingType OBJECT-TYPE
      SYNTAX        TeLinkEncodingType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the component link encoding type."
      REFERENCE
          "Generalized Multi-Protocol Label Switching (GMPLS) Signaling
           Functional Description, RFC 3471"
      ::= { componentLinkDescriptorEntry 3 }

   componentLinkDescrMinLspBandwidth OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the minimum LSP bandwidth on
           the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 4 }

   componentLinkDescrMaxLspBandwidthPrio0 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 0 on the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 5 }





   componentLinkDescrMaxLspBandwidthPrio1 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 1 on the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 6 }

   componentLinkDescrMaxLspBandwidthPrio2 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 2 on the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 7 }

   componentLinkDescrMaxLspBandwidthPrio3 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 3 on the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 8 }

   componentLinkDescrMaxLspBandwidthPrio4 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 4 on the component link."
      REFERENCE





          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 9 }

   componentLinkDescrMaxLspBandwidthPrio5 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "thousand bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 5 on the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 10 }

   componentLinkDescrMaxLspBandwidthPrio6 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 6 on the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 11 }

   componentLinkDescrMaxLspBandwidthPrio7 OBJECT-TYPE
      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies the maximum LSP bandwidth at
           priority 7 on the component link."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 12 }

   componentLinkDescrInterfaceMtu OBJECT-TYPE
      SYNTAX        Unsigned32 (1..65535)
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION





          "This attribute specifies the interface MTU for the component
           link descriptor."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 13 }

   componentLinkDescrIndication OBJECT-TYPE
      SYNTAX        TeLinkSonetSdhIndication
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This attribute specifies whether this interface supports
           Standard or Arbitrary SONET/SDH."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkDescriptorEntry 14 }

   componentLinkDescrRowStatus OBJECT-TYPE
      SYNTAX        RowStatus
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This variable is used to create, modify, and/or
           delete a row in this table.  No read-create object
           can be modified when componentLinkDescrRowStatus
           is active(1)."
      ::= { componentLinkDescriptorEntry 15 }

   componentLinkDescrStorageType OBJECT-TYPE
      SYNTAX        StorageType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The storage type for this conceptual row in the
           componentLinkDescriptorTable.  Conceptual rows
           having the value 'permanent' need not allow write-access
           to any columnar object in the row."
      ::= { componentLinkDescriptorEntry 16 }

   -- End of componentLinkDescriptorTable


   -- Component Link Bandwidth Table

   componentLinkBandwidthTable OBJECT-TYPE
      SYNTAX        SEQUENCE OF ComponentLinkBandwidthEntry





      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This table specifies the priority-based bandwidth
           for component links."
      ::= { teLinkObjects 7 }

   componentLinkBandwidthEntry OBJECT-TYPE
      SYNTAX        ComponentLinkBandwidthEntry
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "An entry in this table contains information about
           the priority-based bandwidth on component links.
           An ifEntry in the ifTable must exist before a
           componentLinkBandwidthEntry using the same ifIndex is
           created.  ifEntry's ifType can be of any interface type that
           has been defined for TE Link interworking.  Examples
           include ATM, Frame Relay, Ethernet, etc.  If a component link
           entry in the ifTable is destroyed, then so are all entries
           in the componentLinkBandwidthTable that use the ifIndex of
           this component link."
      INDEX         { ifIndex, componentLinkBandwidthPriority }
      ::= { componentLinkBandwidthTable 1 }

   ComponentLinkBandwidthEntry ::= SEQUENCE {
     componentLinkBandwidthPriority    TeLinkPriority,
     componentLinkBandwidthUnreserved  TeLinkBandwidth,
     componentLinkBandwidthRowStatus   RowStatus,
     componentLinkBandwidthStorageType StorageType
   }

   componentLinkBandwidthPriority OBJECT-TYPE
      SYNTAX        TeLinkPriority
      MAX-ACCESS    not-accessible
      STATUS        current
      DESCRIPTION
          "This attribute specifies the priority.  A value of 0 is valid
           as specified in the 'Traffic Engineering (TE) Extensions to
            OSPF Version 2' document."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203 and
           Traffic Engineering (TE) Extensions to OSPF Version 2,
           RFC 3630"
      ::= { componentLinkBandwidthEntry 1 }

   componentLinkBandwidthUnreserved OBJECT-TYPE





      SYNTAX        TeLinkBandwidth
      UNITS         "bps"
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
          "This attribute specifies the component link unreserved
           bandwidth at priority p."
      REFERENCE
          "OSPF Extensions in Support of Generalized Multi-Protocol
           Label Switching (GMPLS), RFC 4203"
      ::= { componentLinkBandwidthEntry 2 }

   componentLinkBandwidthRowStatus OBJECT-TYPE
      SYNTAX        RowStatus
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "This variable is used to create, modify, and/or
           delete a row in this table.  No read-create object can
           be modified when componentLinkBandwidthRowStatus is
           active(1)."
      ::= { componentLinkBandwidthEntry 3 }

   componentLinkBandwidthStorageType OBJECT-TYPE
      SYNTAX        StorageType
      MAX-ACCESS    read-create
      STATUS        current
      DESCRIPTION
          "The storage type for this conceptual row in the
           componentLinkBandwidthTable.  Conceptual rows
           having the value 'permanent' need not allow write-access
           to any columnar object in the row."
      ::= { componentLinkBandwidthEntry 4 }

   -- End of componentLinkBandwidthTable


   -- Module compliance

   teLinkCompliances
      OBJECT IDENTIFIER ::= { teLinkConformance 1 }

   teLinkGroups
      OBJECT IDENTIFIER ::= { teLinkConformance 2 }

   teLinkModuleFullCompliance MODULE-COMPLIANCE
      STATUS current
      DESCRIPTION





          "Compliance statement for agents that support read-create
           so that both configuration and monitoring of TE links can
           be accomplished via this MIB module."
      MODULE -- this module

         MANDATORY-GROUPS    { teLinkGroup,
                               teLinkBandwidthGroup,
                               componentLinkBandwidthGroup }

         GROUP teLinkSrlgGroup
         DESCRIPTION
             "This group is mandatory for GMPLS enabled devices."

         GROUP teLinkPscGroup
         DESCRIPTION
             "This group is mandatory for devices that support the
              packet switching capability."

         GROUP teLinkTdmGroup
         DESCRIPTION
             "This group is mandatory for devices that support the TDM
              switching capability."

         -- teLinkTable

         OBJECT      teLinkAddressType
         SYNTAX      INTEGER { unknown(0), ipv4(1), ipv6(2) }
         DESCRIPTION
             "Only ipv4(1) and ipv6(2) address types need to be
              supported for numbered links.  For unnumbered links, the
              unknown(0) address type needs to be supported."

         OBJECT      teLinkLocalIpAddr
         SYNTAX      InetAddress (SIZE(0|4|16))
         DESCRIPTION
             "Size of TE link IP address depends on type of TE link.
              TE link IP address size is zero if the link is unnumbered,
              four if the link IP address is IPv4, and sixteen if the
              link IP address is IPv6."

         OBJECT      teLinkRemoteIpAddr
         SYNTAX      InetAddress (SIZE(0|4|16))
         DESCRIPTION
             "Size of TE link IP address depends on type of TE link.
              TE link IP address size is zero if the link is unnumbered,
              four if the link IP address is IPv4, and sixteen if the
              link IP address is IPv6."






         OBJECT      teLinkRowStatus
         SYNTAX      RowStatus { active(1), notInService(2) }
         WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                  createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for notReady(3) and createAndWait(5) is
              not required."

         -- teLinkDescriptorTable

         OBJECT      teLinkDescrRowStatus
         SYNTAX      RowStatus { active(1), notInService(2) }
         WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                  createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for notReady(3) and createAndWait(5) is
              not required."

         -- teLinkSrlgTable

         OBJECT      teLinkSrlgRowStatus
         SYNTAX      RowStatus { active(1), notInService(2) }
         WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                  createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for notReady(3) and createAndWait(5) is
              not required."

         -- teLinkBandwidthTable

         OBJECT      teLinkBandwidthRowStatus
         SYNTAX      RowStatus { active(1), notInService(2) }
         WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                  createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for notReady(3) and createAndWait(5) is
              not required."

         -- componentLinkTable

         OBJECT      componentLinkRowStatus
         SYNTAX      RowStatus { active(1), notInService(2) }
         WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                  createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for notReady(3) and createAndWait(5) is
              not required."






         -- componentLinkDescriptorTable

         OBJECT      componentLinkDescrRowStatus
         SYNTAX      RowStatus { active(1), notInService(2) }
         WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                  createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for notReady(3) and createAndWait(5) is
              not required."

         -- componentLinkBandwidthTable

         OBJECT      componentLinkBandwidthRowStatus
         SYNTAX      RowStatus { active(1), notInService(2) }
         WRITE-SYNTAX RowStatus { active(1), notInService(2),
                                  createAndGo(4), destroy(6) }
         DESCRIPTION
             "Support for notReady(3) and createAndWait(5) is
              not required."

      ::= { teLinkCompliances 1 }

   teLinkModuleReadOnlyCompliance MODULE-COMPLIANCE
      STATUS current
      DESCRIPTION
          "Compliance statement for agents that support the
           monitoring of the TE link MIB module."
      MODULE -- this module

         MANDATORY-GROUPS    { teLinkGroup,
                               teLinkBandwidthGroup,
                               componentLinkBandwidthGroup }

         GROUP teLinkSrlgGroup
         DESCRIPTION
             "This group is mandatory for GMPLS enabled devices."

         GROUP teLinkPscGroup
         DESCRIPTION
             "This group is mandatory for devices that support the
              packet switching capability."

         GROUP teLinkTdmGroup
         DESCRIPTION
             "This group is mandatory for devices that support the TDM
              switching capability."

         -- teLinkTable





         OBJECT      teLinkAddressType
         SYNTAX      INTEGER { unknown(0), ipv4(1), ipv6(2) }
         MIN-ACCESS  read-only
         DESCRIPTION
             "Only ipv4(1) and ipv6(2) address types need to be
              supported for numbered links.  For unnumbered links, the
              unknown(0) address type needs to be supported."

         OBJECT      teLinkLocalIpAddr
         SYNTAX      InetAddress (SIZE(0|4|16))
         MIN-ACCESS  read-only
         DESCRIPTION
             "Size of TE link IP address depends on type of TE link.
              TE link IP address size is zero if the link is unnumbered,
              four if the link IP address is IPv4, and sixteen if the
              link IP address is IPv6."

         OBJECT      teLinkRemoteIpAddr
         SYNTAX      InetAddress (SIZE(0|4|16))
         MIN-ACCESS  read-only
         DESCRIPTION
             "Size of TE link IP address depends on type of TE link.
              TE link IP address size is zero if the link is unnumbered,
              four if the link IP address is IPv4, and sixteen if the
              link IP address is IPv6."

         OBJECT      teLinkProtectionType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkWorkingPriority
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkRowStatus
         SYNTAX      RowStatus { active(1) }
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required and active(1) is the
              only status that needs to be supported."

         OBJECT      teLinkStorageType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."






         -- teLinkDescriptorTable

         OBJECT      teLinkDescrSwitchingCapability
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrEncodingType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMinLspBandwidth
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMaxLspBandwidthPrio0
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMaxLspBandwidthPrio1
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMaxLspBandwidthPrio2
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMaxLspBandwidthPrio3
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMaxLspBandwidthPrio4
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMaxLspBandwidthPrio5
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMaxLspBandwidthPrio6





         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrMaxLspBandwidthPrio7
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      teLinkDescrRowStatus
         SYNTAX      RowStatus { active(1) }
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required and active(1) is the
              only status that needs to be supported."

         OBJECT      teLinkDescrStorageType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         -- teLinkSrlgTable

         OBJECT      teLinkSrlgRowStatus
         SYNTAX      RowStatus { active(1) }
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required and active(1) is the
              only status that needs to be supported."

         OBJECT      teLinkSrlgStorageType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         -- teLinkBandwidthTable

         OBJECT      teLinkBandwidthRowStatus
         SYNTAX      RowStatus { active(1) }
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required and active(1) is the
              only status that needs to be supported."

         OBJECT      teLinkBandwidthStorageType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."





         -- componentLinkTable

         OBJECT      componentLinkMaxResBandwidth
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkPreferredProtection
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkRowStatus
         SYNTAX      RowStatus { active(1) }
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required and active(1) is the
              only status that needs to be supported."

         OBJECT      componentLinkStorageType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         -- componentLinkDescriptorTable

         OBJECT      componentLinkDescrSwitchingCapability
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrEncodingType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMinLspBandwidth
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMaxLspBandwidthPrio0
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMaxLspBandwidthPrio1
         MIN-ACCESS  read-only





         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMaxLspBandwidthPrio2
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMaxLspBandwidthPrio3
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMaxLspBandwidthPrio4
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMaxLspBandwidthPrio5
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMaxLspBandwidthPrio6
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrMaxLspBandwidthPrio7
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrInterfaceMtu
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrIndication
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         OBJECT      componentLinkDescrRowStatus
         SYNTAX      RowStatus { active(1) }
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required and active(1) is the





              only status that needs to be supported."

         OBJECT      componentLinkDescrStorageType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

         -- componentLinkBandwidthTable

         OBJECT      componentLinkBandwidthRowStatus
         SYNTAX      RowStatus { active(1) }
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required and active(1) is the
              only status that needs to be supported."

         OBJECT      componentLinkBandwidthStorageType
         MIN-ACCESS  read-only
         DESCRIPTION
             "Write access is not required."

      ::= { teLinkCompliances 2 }

   -- Units of conformance

   teLinkGroup OBJECT-GROUP
      OBJECTS { teLinkAddressType,
                teLinkLocalIpAddr,
                teLinkRemoteIpAddr,
                teLinkMetric,
                teLinkProtectionType,
                teLinkWorkingPriority,
                teLinkResourceClass,
                teLinkIncomingIfId,
                teLinkOutgoingIfId,
                teLinkRowStatus,
                teLinkStorageType,
                teLinkDescrSwitchingCapability,
                teLinkDescrEncodingType,
                teLinkDescrRowStatus,
                teLinkDescrStorageType,
                componentLinkPreferredProtection,
                componentLinkCurrentProtection,
                componentLinkRowStatus,
                componentLinkStorageType,
                componentLinkDescrSwitchingCapability,
                componentLinkDescrEncodingType,
                componentLinkDescrRowStatus,





                componentLinkDescrStorageType
              }

      STATUS  current
      DESCRIPTION
             "Collection of objects needed for the management of
              resources associated with TE links."
      ::= { teLinkGroups 1 }

   teLinkSrlgGroup OBJECT-GROUP
      OBJECTS { teLinkSrlgRowStatus,
                teLinkSrlgStorageType
              }

      STATUS  current
      DESCRIPTION
             "Collection of objects needed for the management of
              SRLG resources associated with TE links."
      ::= { teLinkGroups 2 }

   teLinkBandwidthGroup OBJECT-GROUP
      OBJECTS { teLinkMaximumReservableBandwidth,
                teLinkDescrMaxLspBandwidthPrio0,
                teLinkDescrMaxLspBandwidthPrio1,
                teLinkDescrMaxLspBandwidthPrio2,
                teLinkDescrMaxLspBandwidthPrio3,
                teLinkDescrMaxLspBandwidthPrio4,
                teLinkDescrMaxLspBandwidthPrio5,
                teLinkDescrMaxLspBandwidthPrio6,
                teLinkDescrMaxLspBandwidthPrio7,
                teLinkBandwidthUnreserved,
                teLinkBandwidthRowStatus,
                teLinkBandwidthStorageType
              }

      STATUS  current
      DESCRIPTION
             "Collection of objects needed for the management of
              the bandwidth resources associated with TE links and
              component links."
      ::= { teLinkGroups 3 }

   componentLinkBandwidthGroup OBJECT-GROUP
      OBJECTS { componentLinkMaxResBandwidth,
                componentLinkDescrMaxLspBandwidthPrio0,
                componentLinkDescrMaxLspBandwidthPrio1,
                componentLinkDescrMaxLspBandwidthPrio2,
                componentLinkDescrMaxLspBandwidthPrio3,





                componentLinkDescrMaxLspBandwidthPrio4,
                componentLinkDescrMaxLspBandwidthPrio5,
                componentLinkDescrMaxLspBandwidthPrio6,
                componentLinkDescrMaxLspBandwidthPrio7,
                componentLinkBandwidthUnreserved,
                componentLinkBandwidthRowStatus,
                componentLinkBandwidthStorageType
              }

      STATUS  current
      DESCRIPTION
             "Collection of objects needed for the management of the
              bandwidth parameters associated with component links."
      ::= { teLinkGroups 4 }

   teLinkPscGroup OBJECT-GROUP
      OBJECTS { teLinkDescrMinLspBandwidth,
                teLinkDescrInterfaceMtu,
                componentLinkDescrMinLspBandwidth,
                componentLinkDescrInterfaceMtu
              }

      STATUS  current
      DESCRIPTION
             "Collection of objects needed for devices that are
              packet switch capable."
      ::= { teLinkGroups 5 }

   teLinkTdmGroup OBJECT-GROUP
      OBJECTS { teLinkDescrMinLspBandwidth,
                teLinkDescrIndication,
                componentLinkDescrMinLspBandwidth,
                componentLinkDescrIndication
              }

      STATUS  current
      DESCRIPTION
             "Collection of objects needed for devices that are
              TDM switching capable."
      ::= { teLinkGroups 6 }

   -- End of TE-LINK-STD-MIB
   END









