SNMP-USM-HMAC-SHA2-MIB DEFINITIONS ::= BEGIN

       IMPORTS
           MODULE-IDENTITY, OBJECT-IDENTITY,
       snmpModules             FROM SNMPv2-SMI          -- [RFC2578]
       snmpAuthProtocols       FROM SNMP-FRAMEWORK-MIB; -- [RFC3411]

   snmpUsmHmacSha2MIB MODULE-IDENTITY
       LAST-UPDATED    "201508130000Z"       -- 13 August 2015, midnight
       ORGANIZATION    "SNMPv3 Working Group"
       CONTACT-INFO    "WG email: OPSAWG@ietf.org
                       Subscribe:
                           https://www.ietf.org/mailman/listinfo/opsawg
                       Editor:    Johannes Merkle
                                  secunet Security Networks
                       Postal:    Mergenthaler Allee 77
                                  D-65760 Eschborn
                                  Germany
                       Phone:     +49 20154543091
                       Email:     johannes.merkle@secunet.com

                       Co-Editor: Manfred Lochter
                                  Bundesamt fuer Sicherheit in der





                                  Informationstechnik (BSI)
                       Postal:    Postfach 200363
                                  D-53133 Bonn
                                  Germany
                       Phone:     +49 228 9582 5643
                       Email:     manfred.lochter@bsi.bund.de"

       DESCRIPTION     "Definitions of Object Identities needed
                       for the use of HMAC-SHA2 by SNMP's User-based
                       Security Model.

             Copyright (c) 2015 IETF Trust and the persons identified
             as authors of the code.  All rights reserved.

             Redistribution and use in source and binary forms, with
             or without modification, is permitted pursuant to, and
             subject to the license terms contained in, the Simplified
             BSD License set forth in Section 4.c of the IETF Trust's
             Legal Provisions Relating to IETF Documents
             (http://trustee.ietf.org/license-info)."

       REVISION    "201508130000Z"       -- 13 August 2015, midnight
       DESCRIPTION "Initial version, published as RFC 7630"
   ::= { snmpModules 235 }

   usmHMAC128SHA224AuthProtocol OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "The Authentication Protocol
                   usmHMAC128SHA224AuthProtocol uses HMAC-SHA-224 and
                   truncates output to 128 bits."
       REFERENCE   "- Krawczyk, H., Bellare, M., and R. Canetti, HMAC:
                   Keyed-Hashing for Message Authentication, RFC 2104.
                   - National Institute of Standards and Technology,
                   Secure Hash Standard (SHS), FIPS PUB 180-4, 2012."
       ::= { snmpAuthProtocols 4 }

   usmHMAC192SHA256AuthProtocol OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "The Authentication Protocol
                   usmHMAC192SHA256AuthProtocol uses HMAC-SHA-256 and
                   truncates output to 192 bits."
       REFERENCE   "- Krawczyk, H., Bellare, M., and R. Canetti, HMAC:
                   Keyed-Hashing for Message Authentication, RFC 2104.
                   - National Institute of Standards and Technology,
                   Secure Hash Standard (SHS), FIPS PUB 180-4, 2012."
       ::= { snmpAuthProtocols 5 }

   usmHMAC256SHA384AuthProtocol OBJECT-IDENTITY





       STATUS      current
       DESCRIPTION "The Authentication Protocol
                   usmHMAC256SHA384AuthProtocol uses HMAC-SHA-384 and
                   truncates output to 256 bits."
       REFERENCE   "- Krawczyk, H., Bellare, M., and R. Canetti, HMAC:
                   Keyed-Hashing for Message Authentication, RFC 2104.
                   - National Institute of Standards and Technology,
                   Secure Hash Standard (SHS), FIPS PUB 180-4, 2012."
       ::= { snmpAuthProtocols 6 }

   usmHMAC384SHA512AuthProtocol OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "The Authentication Protocol
                   usmHMAC384SHA512AuthProtocol uses HMAC-SHA-512 and
                   truncates output to 384 bits."
       REFERENCE   "- Krawczyk, H., Bellare, M., and R. Canetti, HMAC:
                   Keyed-Hashing for Message Authentication, RFC 2104.
                   - National Institute of Standards and Technology,
                   Secure Hash Standard (SHS), FIPS PUB 180-4, 2012."
       ::= { snmpAuthProtocols 7 }

   END


