WWW-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, mib-2,
       Counter32, Counter64, Integer32, Unsigned32, TimeTicks
           FROM SNMPv2-SMI




       TEXTUAL-CONVENTION, DisplayString, DateAndTime, TimeInterval
           FROM SNMPv2-TC

       MODULE-COMPLIANCE, OBJECT-GROUP
           FROM SNMPv2-CONF

       Utf8String
           FROM SYSAPPL-MIB;

   wwwMIB MODULE-IDENTITY
       LAST-UPDATED "9902251400Z"
       ORGANIZATION "IETF Application MIB Working Group"
       CONTACT-INFO
           "        Harrie Hazewinkel

            Postal: Joint Research Centre of the E.C.
                    via Fermi - Ispra 21020 (VA)
                    Italy

               Tel: +39+(0)332 786322
               Fax: +39+(0)332 785641
            E-mail: harrie.hazewinkel@jrc.it

                    Carl W. Kalbfleisch

            Postal: Verio, Inc.
                    1950 Stemmons Freeway
                    Suite 2006
                    Dallas, TX 75207
                    US

               Tel: +1 214 290-8653
               Fax: +1 214 744-0742
            E-mail: cwk@verio.net

                    Juergen Schoenwaelder

            Postal: TU Braunschweig
                    Bueltenweg 74/75
                    38106 Braunschweig
                    Germany

               Tel: +49 531 391-3683
               Fax: +49 531 489-5936
            E-mail: schoenw@ibr.cs.tu-bs.de"
       DESCRIPTION
           "This WWW service MIB module is applicable to services
            realized by a family of 'Document Transfer Protocols'
            (DTP). Examples of DTPs are HTTP and FTP."




          -- revision history

          REVISION    "9902251400Z"
          DESCRIPTION "Initial version, published as RFC2594."

          ::= { mib-2 65 }

   --
   --  Object Identifier Assignments
   --

   wwwMIBObjects     OBJECT IDENTIFIER ::= { wwwMIB 1 }
   wwwMIBConformance OBJECT IDENTIFIER ::= { wwwMIB 2 }

   --
   -- Textual Conventions
   --

   WwwRequestType ::= TEXTUAL-CONVENTION
       STATUS      current
       DESCRIPTION
           "The WwwRequestType defines the textual identification of
            request types used by a document transfer protocol. For
            the proper values for a given DTP, refer to the protocol
            mappings for that DTP."
       SYNTAX      OCTET STRING (SIZE (1..40))

   WwwResponseType ::= TEXTUAL-CONVENTION
       STATUS      current
       DESCRIPTION
           "The WwwResponseType defines the different response values
            used by document transfer protocols. For the proper values
            for a given DTP, refer to the protocol mappings for that
            DTP."
       SYNTAX      Integer32 (0..2147483647)

   WwwOperStatus ::= TEXTUAL-CONVENTION
       STATUS      current
       DESCRIPTION
           "The operational status of a WWW service. 'down' indicates
            that the service is not available. 'running' indicates
            that the service is operational and available. 'halted'
            indicates that the service is operational but not
            available. 'congested' indicates that the service is
            operational but no additional inbound associations can be
            accommodated. 'restarting' indicates that the service is
            currently unavailable but is in the process of restarting
            and will be available soon."
       SYNTAX      INTEGER {
                       down(1),




                       running(2),
                       halted(3),
                       congested(4),
                       restarting(5)
                   }

   WwwDocName ::= TEXTUAL-CONVENTION
       DISPLAY-HINT "255a"
       STATUS      current
       DESCRIPTION
           "The server relative name of a document. If the URL were
            http://www.x.org/standards/search/search.cgi?string=test
            then the value of this textual convention would resolve
            to '/standards/search/search.cgi'. This textual convention
            uses the character set for URIs as defined in RFC 2396
            section 2."
       SYNTAX      OCTET STRING (SIZE (0..255))


   -- The WWW Service Information Group
   --
   -- The WWW service information group contains information about
   -- the WWW services known by the SNMP agent.

   wwwService OBJECT IDENTIFIER ::= { wwwMIBObjects 1 }

   wwwServiceTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwServiceEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table of the WWW services known by the SNMP agent."
       ::= { wwwService 1 }

   wwwServiceEntry OBJECT-TYPE
       SYNTAX      WwwServiceEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Details about a particular WWW service."
       INDEX       { wwwServiceIndex }
       ::= { wwwServiceTable 1 }

   WwwServiceEntry ::= SEQUENCE {
       wwwServiceIndex             Unsigned32,
       wwwServiceDescription       Utf8String,
       wwwServiceContact           Utf8String,
       wwwServiceProtocol          OBJECT IDENTIFIER,
       wwwServiceName              DisplayString,
       wwwServiceType              INTEGER,




       wwwServiceStartTime         DateAndTime,
       wwwServiceOperStatus        WwwOperStatus,
       wwwServiceLastChange        DateAndTime
   }

   wwwServiceIndex OBJECT-TYPE
       SYNTAX      Unsigned32 (1..4294967295)
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An integer used to uniquely identify a WWW service. The
            value must be the same as the corresponding value of the
            applSrvIndex defined in the Application Management MIB
            (APPLICATION-MIB) if the applSrvIndex object is available.
            It might be necessary to manually configure sub-agents in
            order to meet this requirement."
       ::= { wwwServiceEntry 1 }

   wwwServiceDescription OBJECT-TYPE
       SYNTAX      Utf8String
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Textual description of the WWW service. This shall include
            at least the vendor and version number of the application
            realizing the WWW service. In a minimal case, this might
            be the Product Token (see RFC 2068) for the application."
       ::= { wwwServiceEntry 2 }

   wwwServiceContact OBJECT-TYPE
       SYNTAX      Utf8String
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The textual identification of the contact person for this
            service, together with information on how to contact this
            person. For instance, this might be a string containing an
            email address, e.g. '<webmaster@domain.name>'."
       ::= { wwwServiceEntry 3 }

   wwwServiceProtocol OBJECT-TYPE
       SYNTAX      OBJECT IDENTIFIER
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "An identification of the primary protocol in use by this
            service. For Internet applications, the IANA maintains
            a registry of the OIDs which correspond to well-known
            application protocols.  If the application protocol is not
            listed in the registry, an OID value of the form




            {applTCPProtoID port} or {applUDPProtoID port} are used for
            TCP-based and UDP-based protocols, respectively. In either
            case 'port' corresponds to the primary port number being
            used by the protocol."
       REFERENCE
           "The OID values applTCPProtoID and applUDPProtoID are
            defined in the NETWORK-SERVICES-MIB (RFC 2248)."
       ::= { wwwServiceEntry 4 }

   wwwServiceName OBJECT-TYPE
       SYNTAX      DisplayString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The fully qualified domain name by which this service is
            known. This object must contain the virtual host name if
            the service is realized for a virtual host."
       ::= { wwwServiceEntry 5 }

   wwwServiceType OBJECT-TYPE
       SYNTAX      INTEGER {
                       wwwOther(1),
                       wwwServer(2),
                       wwwClient(3),
                       wwwProxy(4),
                       wwwCachingProxy(5)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The application type using or realizing this WWW service."
       ::= { wwwServiceEntry 6 }

   wwwServiceStartTime OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time when this WWW service was last started.
            The value SHALL be '0000000000000000'H if the last start
            time of this WWW service is not known."
       ::= { wwwServiceEntry 7 }

   wwwServiceOperStatus OBJECT-TYPE
       SYNTAX      WwwOperStatus
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "Indicates the operational status of the WWW service."
       ::= { wwwServiceEntry 8 }




   wwwServiceLastChange OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time when this WWW service entered its current
            operational state. The value SHALL be '0000000000000000'H if
            the time of the last state change is not known."
       ::= { wwwServiceEntry 9 }


   -- The WWW Protocol Statistics Group
   --
   -- The WWW protocol statistics group contains statistics about
   -- the DTP requests and responses sent or received.

   wwwProtocolStatistics OBJECT IDENTIFIER ::= { wwwMIBObjects 2 }

   wwwSummaryTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwSummaryEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table providing overview statistics for the
            WWW services on this system."
       ::= { wwwProtocolStatistics 1 }

   wwwSummaryEntry OBJECT-TYPE
       SYNTAX      WwwSummaryEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Overview statistics for an individual service."
       INDEX       { wwwServiceIndex }
       ::= { wwwSummaryTable 1 }

   WwwSummaryEntry ::= SEQUENCE {
       wwwSummaryInRequests        Counter32,
       wwwSummaryOutRequests       Counter32,
       wwwSummaryInResponses       Counter32,
       wwwSummaryOutResponses      Counter32,
       wwwSummaryInBytes           Counter64,
       wwwSummaryInLowBytes        Counter32,
       wwwSummaryOutBytes          Counter64,
       wwwSummaryOutLowBytes       Counter32
   }

   wwwSummaryInRequests OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only




       STATUS      current
       DESCRIPTION
           "The number of requests successfully received."
       ::= { wwwSummaryEntry 1 }

   wwwSummaryOutRequests OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests generated."
       ::= { wwwSummaryEntry 2 }

   wwwSummaryInResponses OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of responses successfully received."
       ::= { wwwSummaryEntry 3 }

   wwwSummaryOutResponses OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of responses generated."
       ::= { wwwSummaryEntry 4 }

   wwwSummaryInBytes OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of content bytes received."
       ::= { wwwSummaryEntry 5 }

   wwwSummaryInLowBytes OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The lowest thirty-two bits of wwwSummaryInBytes."
       ::= { wwwSummaryEntry 6 }

   wwwSummaryOutBytes OBJECT-TYPE
       SYNTAX      Counter64
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION




           "The number of content bytes transmitted."
       ::= { wwwSummaryEntry 7 }

   wwwSummaryOutLowBytes OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The lowest thirty-two bits of wwwSummaryOutBytes."
       ::= { wwwSummaryEntry 8 }

   -- The WWW request tables contain detailed information about
   -- requests send or received by WWW services.

   wwwRequestInTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwRequestInEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table providing detailed statistics for requests
            received by WWW services on this system."
       ::= { wwwProtocolStatistics 2 }

   wwwRequestInEntry OBJECT-TYPE
       SYNTAX      WwwRequestInEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Request statistics for an individual service."
       INDEX       { wwwServiceIndex, wwwRequestInIndex }
       ::= { wwwRequestInTable 1 }

   WwwRequestInEntry ::= SEQUENCE {
       wwwRequestInIndex           WwwRequestType,
       wwwRequestInRequests        Counter32,
       wwwRequestInBytes           Counter32,
       wwwRequestInLastTime        DateAndTime
   }

   wwwRequestInIndex OBJECT-TYPE
       SYNTAX      WwwRequestType
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The particular request type the statistics apply to."
       ::= { wwwRequestInEntry 1 }

   wwwRequestInRequests OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only




       STATUS      current
       DESCRIPTION
           "The number of requests of this type received by this
            WWW service."
       ::= { wwwRequestInEntry 2 }

   wwwRequestInBytes OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of content bytes per request type received
            by this WWW service."
       ::= { wwwRequestInEntry 3 }

   wwwRequestInLastTime OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time when the last byte of the last complete
            request of this type was received by this WWW service. The
            value SHALL be '0000000000000000'H if no request of this
            type has been received yet."
       ::= { wwwRequestInEntry 4 }

   wwwRequestOutTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwRequestOutEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table providing detailed statistics for requests
            generated by the services on this system."
       ::= { wwwProtocolStatistics 3 }

   wwwRequestOutEntry OBJECT-TYPE
       SYNTAX      WwwRequestOutEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Request statistics for an individual service."
       INDEX       { wwwServiceIndex, wwwRequestOutIndex }
       ::= { wwwRequestOutTable 1 }

   WwwRequestOutEntry ::= SEQUENCE {
       wwwRequestOutIndex          WwwRequestType,
       wwwRequestOutRequests       Counter32,
       wwwRequestOutBytes          Counter32,
       wwwRequestOutLastTime       DateAndTime
   }




   wwwRequestOutIndex OBJECT-TYPE
       SYNTAX      WwwRequestType
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The particular request type the statistics apply to."
       ::= { wwwRequestOutEntry 1 }

   wwwRequestOutRequests OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of requests of this type generated by this
            WWW service."
       ::= { wwwRequestOutEntry 2 }

   wwwRequestOutBytes OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of content bytes per requests type generated
            by this WWW service."
       ::= { wwwRequestOutEntry 3 }

   wwwRequestOutLastTime OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time when the first byte of the last request
            of this type was send by this WWW service. The value SHALL
            be '0000000000000000'H if no request of this type has been
            send yet."
       ::= { wwwRequestOutEntry 4 }

   -- The WWW response tables contain detailed information about
   -- responses sent or received by WWW services.

   wwwResponseInTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwResponseInEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table providing detailed statistics for responses
            received by WWW services on this system."
       ::= { wwwProtocolStatistics 4 }

   wwwResponseInEntry OBJECT-TYPE




       SYNTAX      WwwResponseInEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Response statistics for an individual service."
       INDEX       { wwwServiceIndex, wwwResponseInIndex }
       ::= { wwwResponseInTable 1 }

   WwwResponseInEntry ::= SEQUENCE {
       wwwResponseInIndex          WwwResponseType,
       wwwResponseInResponses      Counter32,
       wwwResponseInBytes          Counter32,
       wwwResponseInLastTime       DateAndTime
   }

   wwwResponseInIndex OBJECT-TYPE
       SYNTAX      WwwResponseType
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The particular response type the statistics apply to."
       ::= { wwwResponseInEntry 1 }

   wwwResponseInResponses OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of responses of this type received by this
            WWW service."
       ::= { wwwResponseInEntry 2 }

   wwwResponseInBytes OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of content bytes per response type received
            by this WWW service."
       ::= { wwwResponseInEntry 3 }

   wwwResponseInLastTime OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time when the last byte of the last complete
            response of this type was received by this WWW service. The
            value SHALL be '0000000000000000'H if no response of this
            type has been received yet."




       ::= { wwwResponseInEntry 4 }

   wwwResponseOutTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwResponseOutEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table providing detailed statistics for responses
            generated by services on this system."
       ::= { wwwProtocolStatistics 5 }

   wwwResponseOutEntry OBJECT-TYPE
       SYNTAX      WwwResponseOutEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "Response statistics for an individual service."
       INDEX       { wwwServiceIndex, wwwResponseOutIndex }
       ::= { wwwResponseOutTable 1 }

   WwwResponseOutEntry ::= SEQUENCE {
       wwwResponseOutIndex         WwwResponseType,
       wwwResponseOutResponses     Counter32,
       wwwResponseOutBytes         Counter32,
       wwwResponseOutLastTime      DateAndTime
   }

   wwwResponseOutIndex OBJECT-TYPE
       SYNTAX      WwwResponseType
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The particular response type the statistics apply to."
       ::= { wwwResponseOutEntry 1 }

   wwwResponseOutResponses OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of responses of this type generated by this
            WWW service."
       ::= { wwwResponseOutEntry 2 }

   wwwResponseOutBytes OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of content bytes per response type generated




            by this WWW service."
       ::= { wwwResponseOutEntry 3 }

   wwwResponseOutLastTime OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time when the first byte of the last response of
            this type was sent by this WWW service. The value SHALL be
            '0000000000000000'H if response of this type has been send
            yet."
       ::= { wwwResponseOutEntry 4 }


   -- The WWW Document Statistics Group
   --
   -- The WWW document statistics group contains statistics about
   -- document read attempts.

   wwwDocumentStatistics OBJECT IDENTIFIER ::= { wwwMIBObjects 3 }

   wwwDocCtrlTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwDocCtrlEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "A table which controls how the MIB implementation
            collects and maintains document statistics."
       ::= { wwwDocumentStatistics 1 }

   wwwDocCtrlEntry OBJECT-TYPE
       SYNTAX      WwwDocCtrlEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry used to configure the wwwDocLastNTable,
            the wwwDocBucketTable, the wwwDocAccessTopNTable,
            and the wwwDocBytesTopNTable."
       INDEX       { wwwServiceIndex }
       ::= { wwwDocCtrlTable 1 }

   WwwDocCtrlEntry ::= SEQUENCE {
       wwwDocCtrlLastNSize           Unsigned32,
       wwwDocCtrlLastNLock           TimeTicks,
       wwwDocCtrlBuckets             Unsigned32,
       wwwDocCtrlBucketTimeInterval  TimeInterval,
       wwwDocCtrlTopNSize            Unsigned32
   }




   wwwDocCtrlLastNSize OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The maximum number of entries in the wwwDocLastNTable."
       DEFVAL { 25 }
       ::= { wwwDocCtrlEntry 1 }

   wwwDocCtrlLastNLock OBJECT-TYPE
       SYNTAX      TimeTicks
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "This object allows a manager to lock the wwwDocLastNTable
            in order to retrieve the wwwDocLastNTable in a consistent
            state. The agent is expected to take a snapshot of the
            wwwDocLastNTable when it is locked and to continue updating
            the real wwwDocLastNTable table so that recent information is
            available as soon as the wwwDocLastNTable is unlocked again.

            Setting this object to a value greater than 0 will lock
            the table. The timer ticks backwards until it reaches 0.
            The table unlocks automatically once the timer reaches 0
            and the timer stops ticking.

            A manager can increase the timer to request more time to
            read the table. However, any attempt to decrease the timer
            will fail with an inconsistentValue error. This rule ensures
            that multiple managers can simultaneously lock and retrieve
            the wwwDocLastNTable. Note that managers must cooperate in
            using wwwDocCtrlLastNLock. In particular, a manager MUST not
            keep the wwwDocLastNTable locked when it is not necessary to
            finish a retrieval operation."
       ::= { wwwDocCtrlEntry 2 }

   wwwDocCtrlBuckets OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The maximum number of buckets maintained by the agent
            before the oldest bucket is deleted. The buckets are
            used to populate the wwwDocAccessTopNTable and the
            wwwDocBytesTopNTable. The time interval captured in
            each bucket can be configured by setting the
            wwwDocCtrlBucketTimeInterval object."
       DEFVAL { 4 }        -- 4 buckets times 15 minutes = 1 hour
       ::= { wwwDocCtrlEntry 3 }




   wwwDocCtrlBucketTimeInterval OBJECT-TYPE
       SYNTAX      TimeInterval
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The time interval after which a new bucket is created.
            Changing this object has no effect on existing buckets."
       DEFVAL { 90000 }    -- 15 minutes (resolution .01 s)
       ::= { wwwDocCtrlEntry 4 }

   wwwDocCtrlTopNSize OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
           "The maximum number of entries shown in the
            wwwDocAccessTopNTable and the wwwDocBytesTopNTable.
            Changing this object has no effect on existing buckets."
       DEFVAL { 25 }
       ::= { wwwDocCtrlEntry 5 }


   wwwDocLastNTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwDocLastNEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table which logs the last N access attempts."
       ::= { wwwDocumentStatistics 2 }

   wwwDocLastNEntry OBJECT-TYPE
       SYNTAX      WwwDocLastNEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry which describes a recent access attempt."
       INDEX       { wwwServiceIndex, wwwDocLastNIndex }
       ::= { wwwDocLastNTable 1 }

   WwwDocLastNEntry ::= SEQUENCE {
       wwwDocLastNIndex            Unsigned32,
       wwwDocLastNName             WwwDocName,
       wwwDocLastNTimeStamp        DateAndTime,
       wwwDocLastNRequestType      WwwRequestType,
       wwwDocLastNResponseType     WwwResponseType,
       wwwDocLastNStatusMsg        Utf8String,
       wwwDocLastNBytes            Unsigned32
   }

   wwwDocLastNIndex OBJECT-TYPE




       SYNTAX      Unsigned32 (1..4294967295)
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An arbitrary monotonically increasing integer number used
            for indexing the wwwDocLastNTable. The first document
            accessed appears in the table with this index value equal
            to one. Each subsequent document is indexed with the next
            sequential index value. The Nth document accessed will be
            indexed by N. This table presents a sliding window of the
            last wwwDocCtrlLastNSize documents accessed. Thus, entries
            in this table will be indexed by N-wwwDocCtrlLastNSize
            thru N if N > wwwDocCtrlLastNSize and 1 thru N if
            N <= wwwDocCtrlLastNSize.

            The wwwDocCtrlLastNLock attribute can be used to lock
            this table to allow the manager to read its contents."
       ::= { wwwDocLastNEntry 1 }

   wwwDocLastNName OBJECT-TYPE
       SYNTAX      WwwDocName
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The name of the document for which access was attempted."
       ::= { wwwDocLastNEntry 2 }

   wwwDocLastNTimeStamp OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time of the last attempt to access this
            document."
       ::= { wwwDocLastNEntry 3 }

   wwwDocLastNRequestType OBJECT-TYPE
       SYNTAX      WwwRequestType
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The protocol request type which was received by the
            server when this document access was attempted."
       ::= { wwwDocLastNEntry 4 }

   wwwDocLastNResponseType OBJECT-TYPE
       SYNTAX      WwwResponseType
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION




           "The protocol response type which was sent to the client
            as a result of this attempt to access a document. This
            object contains the type of the primary response if
            there were multiple responses to a single request."
       ::= { wwwDocLastNEntry 5 }

   wwwDocLastNStatusMsg OBJECT-TYPE
       SYNTAX      Utf8String
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "This object contains a human readable description of the
            reason why the wwwDocLastNResponseType was returned to the
            client. This object defines the implementation-specific
            reason if the value of wwwDocLastNResponseType indicates
            an error. For example, this object can indicate that the
            requested document could not be transferred due to a
            timeout condition or the document could not be transferred
            because a 'soft link' pointing to the document could not be
            resolved."
       ::= { wwwDocLastNEntry 6 }

   wwwDocLastNBytes OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The number of content bytes that were returned as a
            result of this attempt to access a document."
       ::= { wwwDocLastNEntry 7 }


   wwwDocBucketTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwDocBucketEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "This table provides administrative summary information for
            the buckets maintained per WWW service."
       ::= { wwwDocumentStatistics 3 }

   wwwDocBucketEntry OBJECT-TYPE
       SYNTAX      WwwDocBucketEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry which describes the parameters associated with a
            particular bucket."
       INDEX       { wwwServiceIndex, wwwDocBucketIndex }
       ::= { wwwDocBucketTable 1 }




   WwwDocBucketEntry ::= SEQUENCE {
       wwwDocBucketIndex           Unsigned32,
       wwwDocBucketTimeStamp       DateAndTime,
       wwwDocBucketAccesses        Unsigned32,
       wwwDocBucketDocuments       Unsigned32,
       wwwDocBucketBytes           Unsigned32
   }

   wwwDocBucketIndex OBJECT-TYPE
       SYNTAX      Unsigned32 (1..4294967295)
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An arbitrary monotonically increasing integer number
            used for indexing the wwwDocBucketTable. The index number
            wraps to 1 whenever the maximum value is reached."
       ::= { wwwDocBucketEntry 1 }

   wwwDocBucketTimeStamp OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time when the bucket was made available."
       ::= { wwwDocBucketEntry 2 }

   wwwDocBucketAccesses OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The total number of access attempts for any document
            provided by this WWW service during the time interval
            over which this bucket was created."
       ::= { wwwDocBucketEntry 3 }

   wwwDocBucketDocuments OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The total number of different documents for which access
            was attempted this this WWW service during the time interval
            over which this bucket was created."
       ::= { wwwDocBucketEntry 4 }

   wwwDocBucketBytes OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current




       DESCRIPTION
           "The total number of content bytes which were transferred
            from this WWW service during the time interval over which
            this bucket was created."
       ::= { wwwDocBucketEntry 5 }


   wwwDocAccessTopNTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwDocAccessTopNEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table of the most frequently accessed documents in a
            given bucket. This table is sorted by the column
            wwwDocAccessTopNAccesses. Entries having the same number
            of accesses are secondarily sorted by wwwDocAccessTopNBytes.
            Entries with the same number of accesses and the same
            number of bytes will have an arbitrary order."
       ::= { wwwDocumentStatistics 4 }

   wwwDocAccessTopNEntry OBJECT-TYPE
       SYNTAX      WwwDocAccessTopNEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry in the top N table sorted by document accesses."
       INDEX       { wwwServiceIndex, wwwDocBucketIndex,
                     wwwDocAccessTopNIndex }
       ::= { wwwDocAccessTopNTable 1 }

   WwwDocAccessTopNEntry ::= SEQUENCE {
       wwwDocAccessTopNIndex             Unsigned32,
       wwwDocAccessTopNName              WwwDocName,
       wwwDocAccessTopNAccesses          Unsigned32,
       wwwDocAccessTopNBytes             Unsigned32,
       wwwDocAccessTopNLastResponseType  WwwResponseType
   }

   wwwDocAccessTopNIndex OBJECT-TYPE
       SYNTAX      Unsigned32 (1..4294967295)
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An arbitrary monotonically increasing integer number
            used for indexing the wwwDocAccessTopNTable. The index is
            inversely correlated to the sorting order of the table. The
            document with the highest access count will get the index
            value 1."
       ::= { wwwDocAccessTopNEntry 1 }




   wwwDocAccessTopNName OBJECT-TYPE
       SYNTAX      WwwDocName
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The name of the document for which access was attempted."
       ::= { wwwDocAccessTopNEntry 2 }

   wwwDocAccessTopNAccesses OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The total number of access attempts for this document."
       ::= { wwwDocAccessTopNEntry 3 }

   wwwDocAccessTopNBytes OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The total number of content bytes that were transmitted
            as a result of attempts to access this document."
       ::= { wwwDocAccessTopNEntry 4 }

   wwwDocAccessTopNLastResponseType OBJECT-TYPE
       SYNTAX      WwwResponseType
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The protocol response type which was sent to the client
            as a result of the last attempt to access this document.
            This object contains the type of the primary response if
            there were multiple responses to a single request."
       ::= { wwwDocAccessTopNEntry 5 }


   wwwDocBytesTopNTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF WwwDocBytesTopNEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The table of the documents which caused most network
            traffic in a given bucket. This table is sorted by the
            column wwwDocBytesTopNBytes. Entries having the same number
            bytes are secondarily sorted by wwwDocBytesTopNAccesses.
            Entries with the same number of accesses and the same
            number of bytes will have an arbitrary order."
       ::= { wwwDocumentStatistics 5 }




   wwwDocBytesTopNEntry OBJECT-TYPE
       SYNTAX      WwwDocBytesTopNEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry in the top N table sorted by network traffic."
       INDEX       { wwwServiceIndex, wwwDocBucketIndex,
                     wwwDocBytesTopNIndex }
       ::= { wwwDocBytesTopNTable 1 }

   WwwDocBytesTopNEntry ::= SEQUENCE {
       wwwDocBytesTopNIndex             Unsigned32,
       wwwDocBytesTopNName              WwwDocName,
       wwwDocBytesTopNAccesses          Unsigned32,
       wwwDocBytesTopNBytes             Unsigned32,
       wwwDocBytesTopNLastResponseType  WwwResponseType
   }

   wwwDocBytesTopNIndex OBJECT-TYPE
       SYNTAX      Unsigned32 (1..4294967295)
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An arbitrary monotonically increasing integer number
            used for indexing the wwwDocBytesTopNTable. The index is
            inversely correlated to the sorting order of the table. The
            document with the highest byte count will get the index
            value 1."
       ::= { wwwDocBytesTopNEntry 1 }

   wwwDocBytesTopNName OBJECT-TYPE
       SYNTAX      WwwDocName
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The name of the document for which access was attempted."
       ::= { wwwDocBytesTopNEntry 2 }

   wwwDocBytesTopNAccesses OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The total number of access attempts for this document."
       ::= { wwwDocBytesTopNEntry 3 }

   wwwDocBytesTopNBytes OBJECT-TYPE
       SYNTAX      Unsigned32
       MAX-ACCESS  read-only
       STATUS      current




       DESCRIPTION
           "The total number of content bytes that were transmitted
            as a result of attempts to access this document."
       ::= { wwwDocBytesTopNEntry 4 }

   wwwDocBytesTopNLastResponseType OBJECT-TYPE
       SYNTAX      WwwResponseType
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The protocol response type which was sent to the client
            as a result of the last attempt to access this document.
            This object contains the type of the primary response if
            there were multiple responses to a single request."
       ::= { wwwDocBytesTopNEntry 5 }

   --
   -- Conformance Definitions
   --

   wwwMIBCompliances OBJECT IDENTIFIER ::= { wwwMIBConformance 1 }
   wwwMIBGroups      OBJECT IDENTIFIER ::= { wwwMIBConformance 2 }

   wwwMinimalCompliance MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "The compliance statement for SNMP agents which implement
            the minimal subset of the WWW-MIB. Implementors might
            choose this subset for high-performance server where
            full compliance might be to expensive."
       MODULE  -- this module
       MANDATORY-GROUPS {
           wwwServiceGroup,
           wwwSummaryGroup
       }
       OBJECT wwwSummaryOutRequests
       DESCRIPTION
           "Instances of wwwSummaryOutRequests do not exist on pure
            WWW server implementations."
       OBJECT wwwSummaryInResponses
       DESCRIPTION
           "Instances of wwwSummaryOutRequests do not exist on pure
            WWW server implementations."
       OBJECT wwwSummaryInRequests
       DESCRIPTION
           "Instances of wwwSummaryInRequests do not exist on pure
            WWW client implementations."
       OBJECT wwwSummaryOutResponses
       DESCRIPTION
           "Instances of wwwSummaryOutResponses do not exist on pure




            WWW client implementations."
       ::= { wwwMIBCompliances 1 }

   wwwFullCompliance MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "The compliance statement for SNMP agents which implement
            the full WWW-MIB."
       MODULE  -- this module
       MANDATORY-GROUPS {
           wwwServiceGroup,
           wwwSummaryGroup
       }
       GROUP  wwwRequestInGroup
       DESCRIPTION
           "The wwwRequestInGroup is mandatory only for WWW server
            or proxy server implementations."
       GROUP wwwResponseOutGroup
       DESCRIPTION
           "The wwwResponseOutGroup is mandatory only for WWW server
            or proxy server implementations."
       GROUP wwwRequestOutGroup
       DESCRIPTION
           "The wwwRequestOutGroup is mandatory only for WWW client
            or proxy server implementations."
       GROUP wwwResponseInGroup
       DESCRIPTION
           "The wwwRequestOutGroup is mandatory only for WWW client
            or proxy server implementations."
       GROUP wwwDocumentGroup
       DESCRIPTION
           "The wwwDocumentGroup is mandatory only for WWW server
            or proxy server implementations."
       OBJECT wwwSummaryOutRequests
       DESCRIPTION
           "Instances of wwwSummaryOutRequests do not exist on pure
            WWW server implementations."
       OBJECT wwwSummaryInResponses
       DESCRIPTION
           "Instances of wwwSummaryOutRequests do not exist on pure
            WWW server implementations."
       OBJECT wwwSummaryInRequests
       DESCRIPTION
           "Instances of wwwSummaryInRequests do not exist on pure
            WWW client implementations."
       OBJECT wwwSummaryOutResponses
       DESCRIPTION
           "Instances of wwwSummaryOutResponses do not exist on pure
            WWW client implementations."
       ::= { wwwMIBCompliances 2 }




   wwwServiceGroup OBJECT-GROUP
       OBJECTS {
           wwwServiceDescription,
           wwwServiceContact,
           wwwServiceProtocol,
           wwwServiceName,
           wwwServiceType,
           wwwServiceStartTime,
           wwwServiceOperStatus,
           wwwServiceLastChange
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing information about
            the WWW services known by the SNMP agent."
       ::= { wwwMIBGroups 1 }

   wwwSummaryGroup OBJECT-GROUP
       OBJECTS {
           wwwSummaryInRequests,
           wwwSummaryOutRequests,
           wwwSummaryInResponses,
           wwwSummaryOutResponses,
           wwwSummaryInBytes,
           wwwSummaryInLowBytes,
           wwwSummaryOutBytes,
           wwwSummaryOutLowBytes
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing summary statistics
            about requests and responses generated and received
            by a WWW service."
       ::= { wwwMIBGroups 2 }

   wwwRequestInGroup OBJECT-GROUP
       OBJECTS {
           wwwRequestInRequests,
           wwwRequestInBytes,
           wwwRequestInLastTime
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing detailed statistics
            about requests received by a WWW service."
       ::= { wwwMIBGroups 3 }

   wwwRequestOutGroup OBJECT-GROUP
       OBJECTS {
           wwwRequestOutRequests,




           wwwRequestOutBytes,
           wwwRequestOutLastTime
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing detailed statistics
            about requests generated by a WWW service."
       ::= { wwwMIBGroups 4 }

   wwwResponseInGroup OBJECT-GROUP
       OBJECTS {
           wwwResponseInResponses,
           wwwResponseInBytes,
           wwwResponseInLastTime
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing detailed statistics
            about responses received by a WWW service."
       ::= { wwwMIBGroups 5 }

   wwwResponseOutGroup OBJECT-GROUP
       OBJECTS {
           wwwResponseOutResponses,
           wwwResponseOutBytes,
           wwwResponseOutLastTime
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing detailed statistics
            about responses generated by a WWW service."
       ::= { wwwMIBGroups 6 }

   wwwDocumentGroup OBJECT-GROUP
       OBJECTS {
           wwwDocCtrlLastNSize,
           wwwDocCtrlLastNLock,
           wwwDocCtrlBuckets,
           wwwDocCtrlBucketTimeInterval,
           wwwDocCtrlTopNSize,
           wwwDocLastNName,
           wwwDocLastNTimeStamp,
           wwwDocLastNRequestType,
           wwwDocLastNResponseType,
           wwwDocLastNStatusMsg,
           wwwDocLastNBytes,
           wwwDocBucketTimeStamp,
           wwwDocBucketAccesses,
           wwwDocBucketDocuments,
           wwwDocBucketBytes,




           wwwDocAccessTopNName,
           wwwDocAccessTopNAccesses,
           wwwDocAccessTopNBytes,
           wwwDocAccessTopNLastResponseType,
           wwwDocBytesTopNName,
           wwwDocBytesTopNAccesses,
           wwwDocBytesTopNBytes,
           wwwDocBytesTopNLastResponseType
       }
       STATUS  current
       DESCRIPTION
           "A collection of objects providing information about
            accesses to documents."
       ::= { wwwMIBGroups 7 }

   END



