MIXER-MAPPINGS DEFINITIONS ::= BEGIN

   EXPORTS -- everything --;

   IMPORTS

      mixer -- { iso(1) org(3) dod(6) internet(1) mail(7) mixer(1) }
           FROM MIXER --Companion RFC--;

   mixer-headings OBJECT IDENTIFIER ::=
           { mixer 1 } -- called mime-mhs-headings in RFC 1495 --

   mixer-bodies OBJECT IDENTIFIER ::=
           { mixer 2 } -- called mime-mhs-bodies in RFC 1495 --

   -- mixer-core is defined as { mixer core(3) } in [MIXER]

   mixer-bp-data OBJECT IDENTIFIER ::=
           { mixer-bodies 1 }; -- called mime-mhs-bp-data in RFC 1494 --

   mixer-bp-parameter OBJECT IDENTIFIER ::=
           { mixer-bodies 2 };

   id-mime-bp-data OBJECT IDENTIFIER ::=
           { mixer-bp-data 1 };
   -- for debugging: mixer-bp-data is 1.3.6.1.7.1.2.1.1

   id-mime-bp-parameters OBJECT IDENTIFIER ::=
           { mixer-bp-parameter 1 };

   -- the following assignments were done in RFC 1494, using
   -- slightly different names, but the same numbers.
   -- their defining text is now is now in other documents
      id-mime-postscript-body OBJECT IDENTIFIER ::=
                     { mixer-bp-data 2 }

      id-mime-jpeg-body OBJECT IDENTIFIER ::=
                     { mixer-bp-data 3 }

      id-mime-gif-body OBJECT IDENTIFIER ::=
                     { mixer-bp-data 4 }

   -- This is a new definition, and defines an FTAM application
   reference,
   -- not a BP15 data OID.
   id-mime-ftbp-data OBJECT IDENTIFIER ::=
                      { mixer-bp-data 5 }





   -- The following heading extensions are defined
   id-hex-partial-message OBJECT IDENTIFIER ::=
              { mixer-headings 1 }

   id-hex-multipart-message OBJECT IDENTIFIER ::=
              { mixer-headings 2 } -- from RFC 1495; obsolete

   id-hex-multipart-message-v2 OBJECT IDENTIFIER ::=
           { mixer-headings 3 }

   END









































