IANA-FINISHER-MIB DEFINITIONS ::= BEGIN

 -- http://www.iana.org/assignments/ianafinisher-mib

IMPORTS
    MODULE-IDENTITY,
        mib-2
            FROM SNMPv2-SMI                              -- [RFC2578]
    TEXTUAL-CONVENTION
            FROM SNMPv2-TC;                              -- [RFC2579]

ianafinisherMIB MODULE-IDENTITY
    LAST-UPDATED  "200406020000Z" -- June 2, 2004
    ORGANIZATION  "IANA"
    CONTACT-INFO  "Internet Assigned Numbers Authority

                  Postal: ICANN
                          4676 Admiralty Way, Suite 330
                          Marina del Rey, CA 90292

                  Tel:    +1 310 823 9358
                  E-Mail: iana@iana.org"

    DESCRIPTION   "This MIB module defines a set of finishing-related
                  TEXTUAL-CONVENTIONs for use in Finisher MIB (RFC 3806)
                  and other MIBs which need to specify finishing
                  mechanism details.

                  Any additions or changes to the contents of this MIB
                  module require either publication of an RFC, or
                  Designated Expert Review as defined in RFC 2434,
                  Guidelines for Writing an IANA Considerations Section
                  in RFCs.  The Designated Expert will be selected by
                  the IESG Area Director(s) of the Applications Area.

                  Copyright (C) The Internet Society (2004). The





                  initial version of this MIB module was published
                  in RFC 3806. For full legal notices see the RFC
                  itself or see:
                  http://www.ietf.org/copyrights/ianamib.html"

    REVISION      "200406020000Z"  -- June 2, 2004
    DESCRIPTION   "Original version, published in coordination
                  with Finisher MIB (RFC 3806)."

    ::= { mib-2 110 }

-- TEXTUAL-CONVENTIONs for this MIB module

FinDeviceTypeTC ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
      "The defined finishing device subunit process
       enumerations."
    SYNTAX       INTEGER {
         other(1),
         unknown(2),
         stitcher(3),
         folder(4),
         binder(5),
         trimmer(6),
         dieCutter(7),
         puncher(8),
         perforater(9),
         slitter(10),
         separationCutter(11),
         imprinter(12),
         wrapper(13),
         bander(14),
         makeEnvelope(15),
         stacker(16),
         sheetRotator(17),
         inserter(18)
        }

FinAttributeTypeTC  ::= TEXTUAL-CONVENTION
    STATUS     current
    DESCRIPTION
        "This TEXTUAL-CONVENTION defines the set of enums for use in
         the finDeviceAttributeTable.  See section 5.7 for the complete
         specification of each attribute."
    SYNTAX       INTEGER {
         other(1),
         deviceName(3),





         deviceVendorName(4),
         deviceModel(5),
         deviceVersion(6),
         deviceSerialNumber(7),
         maximumSheets(8),
         finProcessOffsetUnits(9),
         finReferenceEdge(10),
         finAxisOffset(11),
         finJogEdge(12),
         finHeadLocation(13),
         finOperationRestrictions(14),
         finNumberOfPositions(15),
         namedConfiguration(16),
         finMediaTypeRestriction(17),
         finPrinterInputTraySupported(18),
         finPreviousFinishingOperation(19),
         finNextFinishingOperation(20),
         stitchingType(30),
         stitchingDirection(31),
         foldingType(40),
         bindingType(50),
         punchHoleType(80),
         punchHoleSizeLongDim(81),
         punchHoleSizeShortDim(82),
         punchPattern(83),
         slittingType(100),
         wrappingType(130),
         stackOutputType(160),
         stackOffset(161),
         stackRotation(162)
        }

FinEdgeTC ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
      "Specifies an edge for a Finishing Process."
    SYNTAX       INTEGER {
         topEdge(3),
         bottomEdge(4),
         leftEdge(5),
         rightEdge(6)
        }

FinStitchingTypeTC ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
      "The defined stitching type enumerations.  For the edgeStitch and
       stapleDual enums, the finReferenceEdge attribute is recommended





       to define the edge to which the operation applies."
    SYNTAX       INTEGER {
         other(1),         -- More information in other attributes
         unknown(2),
         stapleTopLeft(4),
         stapleBottomLeft(5),
         stapleTopRight(6),
         stapleBottomRight(7),
         saddleStitch(8),
         edgeStitch(9),
         stapleDual(10)
        }

FinStitchingDirTypeTC ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
      "Defines the direction, relative to the top sheet in the output
       subunit, that the stitching operation was performed.  For a
       topDown(3) process, the staple will be clinched on the bottom
       of the stack.  This parameter can be used to determine what
       order the pages of a booklet are to be printed such that the
       staple clinch will be on the inside of the resulting booklet."
    SYNTAX       INTEGER {
         unknown(2),
         topDown(3),
         bottomUp(4)
        }

FinStitchingAngleTypeTC ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
      "This enumeration provides a description of the angular
       orientation of each stitch in a single or multiple stitching
       operation, relative to the 'X' axis.  As with all finishing
       operations, the 'X' axis is always relative to the portrait
       orientation of the document regardless of the orientation
       of the printed image.  This enum is primarily applicable to
       corner stitching operations."
    SYNTAX       INTEGER {
         unknown(2),
         horizontal(3),
         vertical(4),
         slanted(5)
        }

FinFoldingTypeTC ::= TEXTUAL-CONVENTION
   STATUS       current
   DESCRIPTION





     "The defined folding device process enumerations."
   SYNTAX       INTEGER {
         other(1),        -- More information in other attributes
         unknown(2),
         zFold(3),
         halfFold(4),
         letterFold(5)
        }

FinBindingTypeTC ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
      "The defined binding type enumerations."
    SYNTAX       INTEGER {
         other(1),          -- More information in other attributes
         unknown(2),
         tape(4),
         plastic(5),
         velo(6),
         perfect(7),
         spiral(8),
         adhesive(9),
         comb(10),
         padding(11)
        }

FinPunchHoleTypeTC ::= TEXTUAL-CONVENTION
   STATUS       current
   DESCRIPTION
     "The defined hole type punch process enumerations."
   SYNTAX       INTEGER {
         other(1),        -- More information in other attributes
         unknown(2),
         round(3),
         oblong(4),
         square(5),
         rectangular(6),
         star(7)
        }

FinPunchPatternTC ::= TEXTUAL-CONVENTION
   STATUS       current
   DESCRIPTION
     "The defined hole pattern punch process enumerations."
   SYNTAX       INTEGER {
         other(1),           --Pattern to be defined in other attributes
         unknown(2),
         twoHoleUSTop(4),    --Letter/legal, 8.5 inch edge





         threeHoleUS(5),     --Letter/ledger, 11 inch edge
         twoHoleDIN(6),      --A4/A3, 297 mm edge
         fourHoleDIN(7),     --A4/A3, 297 mm edge
         twentyTwoHoleUS(8), --Letter/ledger, 11 inch edge
         nineteenHoleUS(9),  --Letter/ledger, 11 inch edge
         twoHoleMetric(10),  --B5/B4, 257 mm edge
         swedish4Hole(11),   --A4/A3, 297 mm edge
         twoHoleUSSide(12),  --Letter/ledger, 11 inch edge
         fiveHoleUS(13),     --Letter/ledger, 11 inch edge
         sevenHoleUS(14),    --Letter/ledger, 11 inch edge
         mixed7H4S(15),      --A4/A3, 297 mm edge
         norweg6Hole(16),    --A4/A3, 297 mm edge
         metric26Hole(17),   --B5/B4, 257 mm edge
         metric30Hole(18)    --A4/A3, 297 mm edge
        }

FinSlittingTypeTC ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
      "The defined slitting type enumerations."
    SYNTAX       INTEGER {
         other(1),         -- More information in other attributes
         unknown(2),
         slitAndSeparate(4),
         slitAndMerge(5)
        }

FinWrappingTypeTC ::= TEXTUAL-CONVENTION
   STATUS       current
   DESCRIPTION
     "The defined wrapping device process enumerations."
   SYNTAX       INTEGER {
         other(1),        -- More information in other attributes
         unknown(2),
         shrinkWrap(4),
         paperWrap(5)
        }

FinStackOutputTypeTC ::= TEXTUAL-CONVENTION
   STATUS       current
   DESCRIPTION
     "The defined stack output type enumerations."
   SYNTAX       INTEGER {
         other(1),        -- More information in other attributes
         unknown(2),
         straight(4),     -- No offset, one on top of another
         offset(5),
         crissCross(6)    -- Rotated





        }
END


