IPV6-TCP-MIB DEFINITIONS ::= BEGIN


 IMPORTS
    MODULE-COMPLIANCE, OBJECT-GROUP      FROM SNMPv2-CONF
    MODULE-IDENTITY, OBJECT-TYPE,
    mib-2, experimental                  FROM SNMPv2-SMI
    Ipv6Address, Ipv6IfIndexOrZero       FROM IPV6-TC;

 ipv6TcpMIB MODULE-IDENTITY
    LAST-UPDATED "201702220000Z"
    ORGANIZATION "IETF IPv6 MIB Working Group"
    CONTACT-INFO
         "       Mike Daniele

                 Postal: Compaq Computer Corporation
                         110 Spitbrook Rd
                         Nashua, NH 03062.
                         US

                 Phone:  +1 603 884 1423
                 Email:  daniele@zk3.dec.com"
    DESCRIPTION
         "The obsolete MIB module for entities implementing TCP
         over IPv6.  Use the TCP-MIB instead.

         Copyright (c) 2017 IETF Trust and the persons identified
         as authors of the code.  All rights reserved.

         Redistribution and use in source and binary forms, with
         or without modification, is permitted pursuant to, and
         subject to the license terms contained in, the Simplified
         BSD License set forth in Section 4.c of the IETF Trust's
         Legal Provisions Relating to IETF Documents
         (http://trustee.ietf.org/license-info)."
    REVISION "201702220000Z"
    DESCRIPTION
         "Obsoleting this MIB module; it has been replaced by
         the revised TCP-MIB (RFC 4022)."
    REVISION "9801290000Z"
    DESCRIPTION
         "First revision, published as RFC 2452"
    ::= { experimental 86 }

 -- objects specific to TCP for IPv6

 tcp      OBJECT IDENTIFIER ::= { mib-2 6 }





 -- the TCP over IPv6 Connection table

 -- This connection table contains information about this
 -- entity's existing TCP connections between IPv6 endpoints.
 -- Only connections between IPv6 addresses are contained in
 -- this table.  This entity's connections between IPv4
 -- endpoints are contained in tcpConnTable.

 ipv6TcpConnTable OBJECT-TYPE
    SYNTAX      SEQUENCE OF Ipv6TcpConnEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
         "A table containing TCP connection-specific information,
          for only those connections whose endpoints are IPv6 addresses.

          This table is obsoleted by TCP-MIB::tcpConnectionTable."
    ::= { tcp 16 }

 ipv6TcpConnEntry OBJECT-TYPE
    SYNTAX      Ipv6TcpConnEntry
    MAX-ACCESS  not-accessible
    STATUS      obsolete
    DESCRIPTION
         "A conceptual row of the ipv6TcpConnTable containing
          information about a particular current TCP connection.
          Each row of this table is transient, in that it ceases to
          exist when (or soon after) the connection makes the transition
          to the CLOSED state.

          Note that conceptual rows in this table require an additional
          index object compared to tcpConnTable, since IPv6 addresses
          are not guaranteed to be unique on the managed node.

          This entry is obsoleted by TCP-MIB::tcpConnectionEntry."
    INDEX   { ipv6TcpConnLocalAddress,
              ipv6TcpConnLocalPort,
              ipv6TcpConnRemAddress,
              ipv6TcpConnRemPort,
              ipv6TcpConnIfIndex }
    ::= { ipv6TcpConnTable 1 }

 Ipv6TcpConnEntry ::=
    SEQUENCE { ipv6TcpConnLocalAddress    Ipv6Address,
               ipv6TcpConnLocalPort       INTEGER,
               ipv6TcpConnRemAddress      Ipv6Address,
               ipv6TcpConnRemPort         INTEGER,
               ipv6TcpConnIfIndex         Ipv6IfIndexOrZero,





               ipv6TcpConnState           INTEGER }

 ipv6TcpConnLocalAddress OBJECT-TYPE
    SYNTAX     Ipv6Address
    MAX-ACCESS not-accessible
    STATUS     obsolete
    DESCRIPTION
         "The local IPv6 address for this TCP connection.  In
          the case of a connection in the listen state which
          is willing to accept connections for any IPv6
          address associated with the managed node, the value
          ::0 is used.

          This object is obsoleted by
          TCP-MIB::tcpConnectionLocalAddressType."
    ::= { ipv6TcpConnEntry 1 }

 ipv6TcpConnLocalPort OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    MAX-ACCESS not-accessible
    STATUS     obsolete
    DESCRIPTION
         "The local port number for this TCP connection.

         This object is obsoleted by TCP-MIB::tcpConnectionLocalPort."
    ::= { ipv6TcpConnEntry 2 }

 ipv6TcpConnRemAddress OBJECT-TYPE
    SYNTAX     Ipv6Address
    MAX-ACCESS not-accessible
    STATUS     obsolete
    DESCRIPTION
         "The remote IPv6 address for this TCP connection.

         This object is obsoleted by TCP-MIB::tcpConnectionRemAddress."
    ::= { ipv6TcpConnEntry 3 }

 ipv6TcpConnRemPort OBJECT-TYPE
    SYNTAX     INTEGER (0..65535)
    MAX-ACCESS not-accessible
    STATUS     obsolete
    DESCRIPTION
         "The remote port number for this TCP connection.

         This object is obsoleted by TCP-MIB::tcpConnectionRemPort."
    ::= { ipv6TcpConnEntry 4 }

 ipv6TcpConnIfIndex OBJECT-TYPE





    SYNTAX     Ipv6IfIndexOrZero
    MAX-ACCESS not-accessible
    STATUS     obsolete
    DESCRIPTION
         "An index object used to disambiguate conceptual rows in
          the table, since the connection 4-tuple may not be unique.

          If the connection's remote address (ipv6TcpConnRemAddress)
          is a link-local address and the connection's local address
          (ipv6TcpConnLocalAddress) is not a link-local address, this
          object identifies a local interface on the same link as
          the connection's remote link-local address.

          Otherwise, this object identifies the local interface that
          is associated with the ipv6TcpConnLocalAddress for this
          TCP connection.  If such a local interface cannot be
          determined, this object should take on the value 0.
          (A possible example of this would be if the value of
          ipv6TcpConnLocalAddress is ::0.)

          The interface identified by a particular non-0 value of this
          index is the same interface as identified by the same value
          of ipv6IfIndex.

          The value of this object must remain constant during the life
          of the TCP connection.

          This object is obsoleted by the zone identifier in
          an InetAddressIPv6z address in either
          TCP-MIB::tcpConnectionLocalAddress or
          TCP-MIB::tcpConnectionRemAddress."
    ::= { ipv6TcpConnEntry 5 }

 ipv6TcpConnState OBJECT-TYPE
    SYNTAX     INTEGER {
         closed(1),
         listen(2),
         synSent(3),
         synReceived(4),
         established(5),
         finWait1(6),
         finWait2(7),
         closeWait(8),
         lastAck(9),
         closing(10),
         timeWait(11),
         deleteTCB(12) }
    MAX-ACCESS read-write





    STATUS     obsolete
    DESCRIPTION
         "The state of this TCP connection.

          The only value which may be set by a management station is
          deleteTCB(12).  Accordingly, it is appropriate for an agent
          to return an error response ('badValue' for SNMPv1,
          'wrongValue' for SNMPv2) if a management station attempts
          to set this object to any other value.

          If a management station sets this object to the value
          deleteTCB(12), then this has the effect of deleting the TCB
          (as defined in RFC 793) of the corresponding connection on
          the managed node, resulting in immediate termination of the
          connection.

          As an implementation-specific option, a RST segment may be
          sent from the managed node to the other TCP endpoint (note
          however that RST segments are not sent reliably).

          This object is obsoleted by TCP-MIB::tcpConnectionState."
    ::= { ipv6TcpConnEntry 6 }

 --
 -- conformance information
 --

 ipv6TcpConformance OBJECT IDENTIFIER ::= { ipv6TcpMIB 2 }

 ipv6TcpCompliances OBJECT IDENTIFIER ::= { ipv6TcpConformance 1 }
 ipv6TcpGroups      OBJECT IDENTIFIER ::= { ipv6TcpConformance 2 }

 -- compliance statements

 ipv6TcpCompliance MODULE-COMPLIANCE
    STATUS  obsolete
    DESCRIPTION
         "The compliance statement for SNMPv2 entities which
          implement TCP over IPv6.

          This compliance statement is obsoleted by
          TCP-MIB::tcpMIBCompliance2."
    MODULE  -- this module
    MANDATORY-GROUPS { ipv6TcpGroup }
    ::= { ipv6TcpCompliances 1 }

 ipv6TcpGroup OBJECT-GROUP
    OBJECTS   { -- these are defined in this module





                -- ipv6TcpConnLocalAddress (not-accessible)
                -- ipv6TcpConnLocalPort (not-accessible)
                -- ipv6TcpConnRemAddress (not-accessible)
                -- ipv6TcpConnRemPort (not-accessible)
                -- ipv6TcpConnIfIndex (not-accessible)
                ipv6TcpConnState }
    STATUS    obsolete
    DESCRIPTION
         "The group of objects providing management of
          TCP over IPv6.

          This group is obsoleted by several groups in TCP-MIB."
    ::= { ipv6TcpGroups 1 }

 END


