DISMAN-SCHEDULE-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, NOTIFICATION-TYPE,
       Integer32, Unsigned32, Counter32, mib-2, zeroDotZero
           FROM SNMPv2-SMI

       TEXTUAL-CONVENTION,
       DateAndTime, RowStatus, StorageType, VariablePointer
           FROM SNMPv2-TC

       MODULE-COMPLIANCE, OBJECT-GROUP, NOTIFICATION-GROUP
           FROM SNMPv2-CONF

       SnmpAdminString
           FROM SNMP-FRAMEWORK-MIB;

   schedMIB MODULE-IDENTITY
       LAST-UPDATED "200201070000Z"
       ORGANIZATION "IETF Distributed Management Working Group"
       CONTACT-INFO
           "WG EMail:  disman@dorothy.bmc.com
            Subscribe: disman-request@dorothy.bmc.com

            Chair:     Randy Presuhn
                       BMC Software, Inc.
            Postal:    Office 1-3141
                       2141 North First Street
                       San Jose,  California 95131
                       USA
            EMail:     rpresuhn@bmc.com
            Phone:     +1 408 546-1006

            Editor:    David B. Levi
                       Nortel Networks
            Postal:    4401 Great America Parkway
                       Santa Clara, CA 95052-8185
                       USA
            EMail:     dlevi@nortelnetworks.com
            Phone:     +1 865 686 0432






            Editor:    Juergen Schoenwaelder
                       TU Braunschweig
            Postal:    Bueltenweg 74/75
                       38106 Braunschweig
                       Germany
            EMail:     schoenw@ibr.cs.tu-bs.de
            Phone:     +49 531 391-3283"
       DESCRIPTION
           "This MIB module defines a MIB which provides mechanisms to
            schedule SNMP set operations periodically or at specific
            points in time."
       REVISION    "200201070000Z"
       DESCRIPTION
           "Revised version, published as RFC 3231.

            This revision introduces a new object type called
            schedTriggers.  Created new conformance and compliance
            statements that take care of the new schedTriggers object.

            Several clarifications have been added to remove ambiguities
            that were discovered and reported by implementors."
       REVISION    "199811171800Z"
       DESCRIPTION
           "Initial version, published as RFC 2591."
       ::= { mib-2 63 }

   --
   -- The various groups defined within this MIB definition:
   --

   schedObjects       OBJECT IDENTIFIER ::= { schedMIB 1 }
   schedNotifications OBJECT IDENTIFIER ::= { schedMIB 2 }
   schedConformance   OBJECT IDENTIFIER ::= { schedMIB 3 }

   --
   -- Textual Conventions:
   --

   SnmpPduErrorStatus ::= TEXTUAL-CONVENTION
       STATUS       current
       DESCRIPTION
           "This TC enumerates the SNMPv1 and SNMPv2 PDU error status
            codes as defined in RFC 1157 and RFC 1905.  It also adds a
            pseudo error status code `noResponse' which indicates a
            timeout condition."
       SYNTAX      INTEGER {
                       noResponse(-1),
                       noError(0),





                       tooBig(1),
                       noSuchName(2),
                       badValue(3),
                       readOnly(4),
                       genErr(5),
                       noAccess(6),
                       wrongType(7),
                       wrongLength(8),
                       wrongEncoding(9),
                       wrongValue(10),
                       noCreation(11),
                       inconsistentValue(12),
                       resourceUnavailable(13),
                       commitFailed(14),
                       undoFailed(15),
                       authorizationError(16),
                       notWritable(17),
                       inconsistentName(18)
                   }

   --
   -- Some scalars which provide information about the local time zone.
   --

   schedLocalTime OBJECT-TYPE
       SYNTAX      DateAndTime (SIZE (11))
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The local time used by the scheduler.  Schedules which
            refer to calendar time will use the local time indicated
            by this object.  An implementation MUST return all 11 bytes
            of the DateAndTime textual-convention so that a manager
            may retrieve the offset from GMT time."
       ::= { schedObjects 1 }

   --
   -- The schedule table which controls the scheduler.
   --

   schedTable OBJECT-TYPE
       SYNTAX      SEQUENCE OF SchedEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "This table defines scheduled actions triggered by
            SNMP set operations."
       ::= { schedObjects 2 }





   schedEntry OBJECT-TYPE
       SYNTAX      SchedEntry
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "An entry describing a particular scheduled action.

            Unless noted otherwise, writable objects of this row
            can be modified independent of the current value of
            schedRowStatus, schedAdminStatus and schedOperStatus.
            In particular, it is legal to modify schedInterval
            and the objects in the schedCalendarGroup when
            schedRowStatus is active and schedAdminStatus and
            schedOperStatus are both enabled."
       INDEX { schedOwner, schedName }
       ::= { schedTable 1 }

   SchedEntry ::= SEQUENCE {
       schedOwner          SnmpAdminString,
       schedName           SnmpAdminString,
       schedDescr          SnmpAdminString,
       schedInterval       Unsigned32,
       schedWeekDay        BITS,
       schedMonth          BITS,
       schedDay            BITS,
       schedHour           BITS,
       schedMinute         BITS,
       schedContextName    SnmpAdminString,
       schedVariable       VariablePointer,
       schedValue          Integer32,
       schedType           INTEGER,
       schedAdminStatus    INTEGER,
       schedOperStatus     INTEGER,
       schedFailures       Counter32,
       schedLastFailure    SnmpPduErrorStatus,
       schedLastFailed     DateAndTime,
       schedStorageType    StorageType,
       schedRowStatus      RowStatus,
       schedTriggers       Counter32
   }

   schedOwner OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE(0..32))
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The owner of this scheduling entry.  The exact semantics of
            this string are subject to the security policy defined by





            the security administrator."
       ::= { schedEntry 1 }

   schedName OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE(1..32))
       MAX-ACCESS  not-accessible
       STATUS      current
       DESCRIPTION
           "The locally-unique, administratively assigned name for this
            scheduling entry.  This object allows a schedOwner to have
            multiple entries in the schedTable."
       ::= { schedEntry 2 }

   schedDescr OBJECT-TYPE
       SYNTAX      SnmpAdminString
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The human readable description of the purpose of this
            scheduling entry."
       DEFVAL      { "" }
       ::= { schedEntry 3 }

   schedInterval OBJECT-TYPE
       SYNTAX      Unsigned32
       UNITS       "seconds"
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The number of seconds between two action invocations of
            a periodic scheduler.  Implementations must guarantee
            that action invocations will not occur before at least
            schedInterval seconds have passed.

            The scheduler must ignore all periodic schedules that
            have a schedInterval value of 0.  A periodic schedule
            with a scheduling interval of 0 seconds will therefore
            never invoke an action.

            Implementations may be forced to delay invocations in the
            face of local constraints.  A scheduled management function
            should therefore not rely on the accuracy provided by the
            scheduler implementation.

            Note that implementations which maintain a list of pending
            activations must re-calculate them when this object is
            changed."
       DEFVAL      { 0 }





       ::= { schedEntry 4 }

   schedWeekDay OBJECT-TYPE
       SYNTAX      BITS {
                       sunday(0),
                       monday(1),
                       tuesday(2),
                       wednesday(3),
                       thursday(4),
                       friday(5),
                       saturday(6)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The set of weekdays on which the scheduled action should
            take place.  Setting multiple bits will include several
            weekdays in the set of possible weekdays for this schedule.
            Setting all bits will cause the scheduler to ignore the
            weekday.

            Note that implementations which maintain a list of pending
            activations must re-calculate them when this object is
            changed."
       DEFVAL      { {} }
       ::= { schedEntry 5 }

   schedMonth OBJECT-TYPE
       SYNTAX      BITS {
                       january(0),
                       february(1),
                       march(2),
                       april(3),
                       may(4),
                       june(5),
                       july(6),
                       august(7),
                       september(8),
                       october(9),
                       november(10),
                       december(11)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The set of months during which the scheduled action should
            take place.  Setting multiple bits will include several
            months in the set of possible months for this schedule.





            Setting all bits will cause the scheduler to ignore the
            month.

            Note that implementations which maintain a list of pending
            activations must re-calculate them when this object is
            changed."
       DEFVAL      { {} }
       ::= { schedEntry 6 }

   schedDay OBJECT-TYPE
       SYNTAX      BITS {
                       d1(0),   d2(1),   d3(2),   d4(3),   d5(4),
                       d6(5),   d7(6),   d8(7),   d9(8),   d10(9),
                       d11(10), d12(11), d13(12), d14(13), d15(14),
                       d16(15), d17(16), d18(17), d19(18), d20(19),
                       d21(20), d22(21), d23(22), d24(23), d25(24),
                       d26(25), d27(26), d28(27), d29(28), d30(29),
                       d31(30),
                       r1(31),  r2(32),  r3(33),  r4(34),  r5(35),
                       r6(36),  r7(37),  r8(38),  r9(39),  r10(40),
                       r11(41), r12(42), r13(43), r14(44), r15(45),
                       r16(46), r17(47), r18(48), r19(49), r20(50),
                       r21(51), r22(52), r23(53), r24(54), r25(55),
                       r26(56), r27(57), r28(58), r29(59), r30(60),
                       r31(61)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The set of days in a month on which a scheduled action
            should take place.  There are two sets of bits one can
            use to define the day within a month:

            Enumerations starting with the letter 'd' indicate a
            day in a month relative to the first day of a month.
            The first day of the month can therefore be specified
            by setting the bit d1(0) and d31(30) means the last
            day of a month with 31 days.

            Enumerations starting with the letter 'r' indicate a
            day in a month in reverse order, relative to the last
            day of a month.  The last day in the month can therefore
            be specified by setting the bit r1(31) and r31(61) means
            the first day of a month with 31 days.

            Setting multiple bits will include several days in the set
            of possible days for this schedule.  Setting all bits will
            cause the scheduler to ignore the day within a month.





            Setting all bits starting with the letter 'd' or the
            letter 'r' will also cause the scheduler to ignore the
            day within a month.

            Note that implementations which maintain a list of pending
            activations must re-calculate them when this object is
            changed."
       DEFVAL      { {} }
       ::= { schedEntry 7 }

   schedHour OBJECT-TYPE
       SYNTAX      BITS {
                       h0(0),   h1(1),   h2(2),   h3(3),   h4(4),
                       h5(5),   h6(6),   h7(7),   h8(8),   h9(9),
                       h10(10), h11(11), h12(12), h13(13), h14(14),
                       h15(15), h16(16), h17(17), h18(18), h19(19),
                       h20(20), h21(21), h22(22), h23(23)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The set of hours within a day during which the scheduled
            action should take place.

            Note that implementations which maintain a list of pending
            activations must re-calculate them when this object is
            changed."
       DEFVAL      { {} }
       ::= { schedEntry 8 }

   schedMinute OBJECT-TYPE
       SYNTAX      BITS {
                       m0(0),   m1(1),   m2(2),   m3(3),   m4(4),
                       m5(5),   m6(6),   m7(7),   m8(8),   m9(9),
                       m10(10), m11(11), m12(12), m13(13), m14(14),
                       m15(15), m16(16), m17(17), m18(18), m19(19),
                       m20(20), m21(21), m22(22), m23(23), m24(24),
                       m25(25), m26(26), m27(27), m28(28), m29(29),
                       m30(30), m31(31), m32(32), m33(33), m34(34),
                       m35(35), m36(36), m37(37), m38(38), m39(39),
                       m40(40), m41(41), m42(42), m43(43), m44(44),
                       m45(45), m46(46), m47(47), m48(48), m49(49),
                       m50(50), m51(51), m52(52), m53(53), m54(54),
                       m55(55), m56(56), m57(57), m58(58), m59(59)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION





           "The set of minutes within an hour when the scheduled action
            should take place.

            Note that implementations which maintain a list of pending
            activations must re-calculate them when this object is
            changed."
       DEFVAL      { {} }
       ::= { schedEntry 9 }

   schedContextName OBJECT-TYPE
       SYNTAX      SnmpAdminString (SIZE(0..32))
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The context which contains the local MIB variable pointed
            to by schedVariable."
       DEFVAL      { "" }
       ::= { schedEntry 10 }

   schedVariable OBJECT-TYPE
       SYNTAX      VariablePointer
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "An object identifier pointing to a local MIB variable
            which resolves to an ASN.1 primitive type of INTEGER."
       DEFVAL      { zeroDotZero }
       ::= { schedEntry 11 }

   schedValue OBJECT-TYPE
       SYNTAX      Integer32
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The value which is written to the MIB object pointed to by
            schedVariable when the scheduler invokes an action.  The
            implementation shall enforce the use of access control
            rules when performing the set operation on schedVariable.
            This is accomplished by calling the isAccessAllowed abstract
            service interface as defined in RFC 2571.

            Note that an implementation may choose to issue an SNMP Set
            message to the SNMP engine and leave the access control
            decision to the normal message processing procedure."
       DEFVAL      { 0 }
       ::= { schedEntry 12 }

   schedType OBJECT-TYPE





       SYNTAX      INTEGER {
                       periodic(1),
                       calendar(2),
                       oneshot(3)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The type of this schedule.  The value periodic(1) indicates
            that this entry specifies a periodic schedule.  A periodic
            schedule is defined by the value of schedInterval.  The
            values of schedWeekDay, schedMonth, schedDay, schedHour
            and schedMinute are ignored.

            The value calendar(2) indicates that this entry describes a
            calendar schedule.  A calendar schedule is defined by the
            values of schedWeekDay, schedMonth, schedDay, schedHour and
            schedMinute.  The value of schedInterval is ignored.  A
            calendar schedule will trigger on all local times that
            satisfy the bits set in schedWeekDay, schedMonth, schedDay,
            schedHour and schedMinute.

            The value oneshot(3) indicates that this entry describes a
            one-shot schedule.  A one-shot schedule is similar to a
            calendar schedule with the additional feature that it
            disables itself by changing in the `finished'
            schedOperStatus once the schedule triggers an action.

            Note that implementations which maintain a list of pending
            activations must re-calculate them when this object is
            changed."
       DEFVAL      { periodic }
       ::= { schedEntry 13 }

   schedAdminStatus OBJECT-TYPE
       SYNTAX      INTEGER {
                       enabled(1),
                       disabled(2)
                   }
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The desired state of the schedule."
       DEFVAL      { disabled }
       ::= { schedEntry 14 }

   schedOperStatus OBJECT-TYPE
       SYNTAX      INTEGER {





                       enabled(1),
                       disabled(2),
                       finished(3)
                   }
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The current operational state of this schedule.  The state
            enabled(1) indicates this entry is active and that the
            scheduler will invoke actions at appropriate times.  The
            disabled(2) state indicates that this entry is currently
            inactive and ignored by the scheduler.  The finished(3)
            state indicates that the schedule has ended.  Schedules
            in the finished(3) state are ignored by the scheduler.
            A one-shot schedule enters the finished(3) state when it
            deactivates itself.

            Note that the operational state must not be enabled(1)
            when the schedRowStatus is not active."
       ::= { schedEntry 15 }

   schedFailures OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "This variable counts the number of failures while invoking
            the scheduled action.  This counter at most increments once
            for a triggered action."
       ::= { schedEntry 16 }

   schedLastFailure OBJECT-TYPE
       SYNTAX      SnmpPduErrorStatus
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The most recent error that occurred during the invocation of
            a scheduled action.  The value noError(0) is returned
            if no errors have occurred yet."
       DEFVAL      { noError }
       ::= { schedEntry 17 }

   schedLastFailed OBJECT-TYPE
       SYNTAX      DateAndTime
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
           "The date and time when the most recent failure occurred.





            The value '0000000000000000'H is returned if no failure
            occurred since the last re-initialization of the scheduler."
       DEFVAL      { '0000000000000000'H }
       ::= { schedEntry 18 }

   schedStorageType OBJECT-TYPE
       SYNTAX      StorageType
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "This object defines whether this scheduled action is kept
            in volatile storage and lost upon reboot or if this row is
            backed up by non-volatile or permanent storage.

            Conceptual rows having the value `permanent' must allow
            write access to the columnar objects schedDescr,
            schedInterval, schedContextName, schedVariable, schedValue,
            and schedAdminStatus.  If an implementation supports the
            schedCalendarGroup, write access must be also allowed to
            the columnar objects schedWeekDay, schedMonth, schedDay,
            schedHour, schedMinute."
       DEFVAL      { volatile }
       ::= { schedEntry 19 }

   schedRowStatus OBJECT-TYPE
       SYNTAX      RowStatus
       MAX-ACCESS  read-create
       STATUS      current
       DESCRIPTION
           "The status of this scheduled action.  A control that allows
            entries to be added and removed from this table.

            Note that the operational state must change to enabled
            when the administrative state is enabled and the row
            status changes to active(1).

            Attempts to destroy(6) a row or to set a row
            notInService(2) while the operational state is enabled
            result in inconsistentValue errors.

            The value of this object has no effect on whether other
            objects in this conceptual row can be modified."
       ::= { schedEntry 20 }

   schedTriggers OBJECT-TYPE
       SYNTAX      Counter32
       MAX-ACCESS  read-only
       STATUS      current





       DESCRIPTION
           "This variable counts the number of attempts (either
            successful or failed) to invoke the scheduled action."
       ::= { schedEntry 21 }

   --
   -- Notifications that are emitted to indicate failures.  The
   -- definition of schedTraps makes notification registrations
   -- reversible (see STD 58, RFC 2578).
   --

   schedTraps OBJECT IDENTIFIER ::= { schedNotifications 0 }

   schedActionFailure NOTIFICATION-TYPE
       OBJECTS     { schedLastFailure, schedLastFailed }
       STATUS      current
       DESCRIPTION
           "This notification is generated whenever the invocation of a
            scheduled action fails."
       ::= { schedTraps 1 }

   -- conformance information

   schedCompliances OBJECT IDENTIFIER ::= { schedConformance 1 }
   schedGroups      OBJECT IDENTIFIER ::= { schedConformance 2 }

   -- compliance statements

   schedCompliance2 MODULE-COMPLIANCE
       STATUS      current
       DESCRIPTION
           "The compliance statement for SNMP entities which implement
            the scheduling MIB."
       MODULE      -- this module
       MANDATORY-GROUPS {
              schedGroup2, schedNotificationsGroup
       }
       GROUP  schedCalendarGroup
       DESCRIPTION
           "The schedCalendarGroup is mandatory only for those
            implementations that support calendar based schedules."
       OBJECT schedType
       DESCRIPTION
           "The values calendar(2) or oneshot(3) are not valid for
            implementations that do not implement the
            schedCalendarGroup.  Such an implementation must return
            inconsistentValue error responses for attempts to set
            schedAdminStatus to calendar(2) or oneshot(3)."





       ::= { schedCompliances 2 }

   schedGroup2 OBJECT-GROUP
       OBJECTS {
           schedDescr, schedInterval, schedContextName,
           schedVariable, schedValue, schedType,
           schedAdminStatus, schedOperStatus, schedFailures,
           schedLastFailure, schedLastFailed, schedStorageType,
           schedRowStatus, schedTriggers
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing scheduling capabilities."
       ::= { schedGroups 4 }

   schedCalendarGroup OBJECT-GROUP
       OBJECTS {
           schedLocalTime, schedWeekDay, schedMonth,
           schedDay, schedHour, schedMinute
       }
       STATUS      current
       DESCRIPTION
           "A collection of objects providing calendar based schedules."
       ::= { schedGroups 2 }

   schedNotificationsGroup NOTIFICATION-GROUP
       NOTIFICATIONS {
           schedActionFailure
       }
       STATUS      current
       DESCRIPTION
           "The notifications emitted by the scheduler."
       ::= { schedGroups 3 }

   --
   -- Deprecated compliance and conformance group definitions
   -- from RFC 2591.
   --

   schedCompliance MODULE-COMPLIANCE
       STATUS      deprecated
       DESCRIPTION
           "The compliance statement for SNMP entities which implement
            the scheduling MIB."
       MODULE      -- this module
       MANDATORY-GROUPS {
              schedGroup, schedNotificationsGroup
       }





       GROUP  schedCalendarGroup
       DESCRIPTION
           "The schedCalendarGroup is mandatory only for those
            implementations that support calendar based schedules."
       OBJECT schedType
       DESCRIPTION
           "The values calendar(2) or oneshot(3) are not valid for
            implementations that do not implement the
            schedCalendarGroup.  Such an implementation must return
            inconsistentValue error responses for attempts to set
            schedAdminStatus to calendar(2) or oneshot(3)."
       ::= { schedCompliances 1 }

   schedGroup OBJECT-GROUP
       OBJECTS {
           schedDescr, schedInterval, schedContextName,
           schedVariable, schedValue, schedType,
           schedAdminStatus, schedOperStatus, schedFailures,
           schedLastFailure, schedLastFailed, schedStorageType,
           schedRowStatus
       }
       STATUS      deprecated
       DESCRIPTION
           "A collection of objects providing scheduling capabilities."
       ::= { schedGroups 1 }

   END


