SNMP-IEEE802-TM-MIB DEFINITIONS ::= BEGIN


   IMPORTS
       MODULE-IDENTITY, OBJECT-IDENTITY, snmpModules, snmpDomains
           FROM SNMPv2-SMI;

       snmpIeee802TmMib MODULE-IDENTITY
           LAST-UPDATED "200611210000Z"
           ORGANIZATION "IETF Operations and Management Area"
           CONTACT-INFO
               "Juergen Schoenwaelder (Editor)
                International University Bremen
                P.O. Box 750 561
                28725 Bremen, Germany

                Phone: +49 421 200-3587
                EMail: j.schoenwaelder@iu-bremen.de

                Send comments to <ietfmibs@ops.ietf.org>."
           DESCRIPTION
               "This MIB module defines the SNMP over IEEE 802
                transport mapping.

                Copyright (C) The IETF Trust (2006).  This version
                of this MIB module is part of RFC 4789; see the RFC
                itself for full legal notices."
           REVISION "200611210000Z"
           DESCRIPTION
               "The initial version, published as RFC 4789."
           ::= { snmpModules 21 }

       snmpIeee802Domain OBJECT-IDENTITY
           STATUS  current
           DESCRIPTION
               "The SNMP over IEEE 802 networks transport domain.  The
                corresponding transport address is of type MacAddress
                as defined in the SNMPv2-TC module (RFC 2579)."
           REFERENCE "RFC 2579"
           ::= { snmpDomains 6 }
   END










