RADIUS-AUTH-SERVER-MIB DEFINITIONS ::= BEGIN


IMPORTS
       MODULE-IDENTITY, OBJECT-TYPE, OBJECT-IDENTITY,
       Counter32, Integer32,
       IpAddress, TimeTicks, mib-2      FROM SNMPv2-SMI
       SnmpAdminString                  FROM SNMP-FRAMEWORK-MIB
       MODULE-COMPLIANCE, OBJECT-GROUP  FROM SNMPv2-CONF;

radiusAuthServMIB MODULE-IDENTITY
       LAST-UPDATED "9906110000Z"
       ORGANIZATION "IETF RADIUS Working Group."
       CONTACT-INFO
              " Bernard Aboba
                Microsoft





                One Microsoft Way
                Redmond, WA  98052
                US

                Phone: +1 425 936 6605
                EMail: bernarda@microsoft.com"
       DESCRIPTION
             "The MIB module for entities implementing the server
              side of the Remote Access Dialin User Service (RADIUS)
              authentication protocol."
       REVISION "9906110000Z"    --  11 Jun 1999
       DESCRIPTION "Initial version as published in RFC 2619"
       ::= { radiusAuthentication 1 }

radiusMIB OBJECT-IDENTITY
       STATUS  current
       DESCRIPTION
             "The OID assigned to RADIUS MIB work by the IANA."
        ::= { mib-2 67 }

radiusAuthentication  OBJECT IDENTIFIER ::= {radiusMIB 1}

radiusAuthServMIBObjects     OBJECT IDENTIFIER ::=
                                                 { radiusAuthServMIB 1 }

radiusAuthServ      OBJECT IDENTIFIER ::= { radiusAuthServMIBObjects 1 }

radiusAuthServIdent OBJECT-TYPE
       SYNTAX      SnmpAdminString
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
             "The implementation identification string for the
              RADIUS authentication server software in use on the
              system, for example; `FNS-2.1'"
       ::= {radiusAuthServ 1}

radiusAuthServUpTime OBJECT-TYPE
       SYNTAX      TimeTicks
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
             "If the server has a persistent state (e.g., a process),
              this value will be the time elapsed (in hundredths of a
              seco) since the server process was started.
              For software without persistent state, this value will
              be zero."
       ::= {radiusAuthServ 2}





radiusAuthServResetTime OBJECT-TYPE
       SYNTAX      TimeTicks
       MAX-ACCESS  read-only
       STATUS      current
       DESCRIPTION
             "If the server has a persistent state (e.g., a process)
              and supports a `reset' operation (e.g., can be told to
              re-read configuration files), this value will be the
              time elapsed (in hundredths of a second) since the
              server was `reset.'  For software that does not
              have persistence or does not support a `reset' operation,
              this value will be zero."
       ::= {radiusAuthServ 3}

radiusAuthServConfigReset OBJECT-TYPE
       SYNTAX INTEGER { other(1),
                        reset(2),
                        initializing(3),
                        running(4)}
       MAX-ACCESS  read-write
       STATUS      current
       DESCRIPTION
              "Status/action object to reinitialize any persistent
               server state.  When set to reset(2), any persistent
               server state (such as a process) is reinitialized as if
               the server had just been started.  This value will
               never be returned by a read operation.  When read, one of
               the following values will be returned:
                   other(1) - server in some unknown state;
                   initializing(3) - server (re)initializing;
                   running(4) - server currently running."
       ::= {radiusAuthServ 4}

-- New Stats proposed by Dale E. Reed Jr (daler@iea-software.com)

radiusAuthServTotalAccessRequests OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
               "The number of packets received on the
                authentication port."
        ::= { radiusAuthServ 5}

radiusAuthServTotalInvalidRequests OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current





        DESCRIPTION
              "The number of RADIUS Access-Request packets
               received from unknown addresses."
        ::= { radiusAuthServ 6 }

radiusAuthServTotalDupAccessRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of duplicate RADIUS Access-Request
              packets received."
       ::= { radiusAuthServ 7 }

radiusAuthServTotalAccessAccepts OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Access-Accept packets sent."
       ::= { radiusAuthServ 8 }

radiusAuthServTotalAccessRejects OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of RADIUS Access-Reject packets sent."
      ::= { radiusAuthServ 9 }

radiusAuthServTotalAccessChallenges OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of RADIUS Access-Challenge packets sent."
      ::= { radiusAuthServ 10 }

radiusAuthServTotalMalformedAccessRequests OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of malformed RADIUS Access-Request
             packets received. Bad authenticators
             and unknown types are not included as
             malformed Access-Requests."
      ::= { radiusAuthServ 11 }





radiusAuthServTotalBadAuthenticators OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of RADIUS Authentication-Request packets
             which contained invalid Signature attributes received."
      ::= { radiusAuthServ 12 }

radiusAuthServTotalPacketsDropped OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of incoming packets
             silently discarded for some reason other
             than malformed, bad authenticators or
             unknown types."
      ::= { radiusAuthServ 13 }

radiusAuthServTotalUnknownTypes OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
            "The number of RADIUS packets of unknown type which
             were received."
      ::= { radiusAuthServ 14 }

-- End of new

radiusAuthClientTable OBJECT-TYPE
       SYNTAX     SEQUENCE OF RadiusAuthClientEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
             "The (conceptual) table listing the RADIUS authentication
              clients with which the server shares a secret."
       ::= { radiusAuthServ 15 }

radiusAuthClientEntry OBJECT-TYPE
       SYNTAX     RadiusAuthClientEntry
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
             "An entry (conceptual row) representing a RADIUS
              authentication client with which the server shares a
              secret."





       INDEX      { radiusAuthClientIndex }
       ::= { radiusAuthClientTable 1 }

RadiusAuthClientEntry ::= SEQUENCE {
       radiusAuthClientIndex                           Integer32,
       radiusAuthClientAddress                         IpAddress,
       radiusAuthClientID                        SnmpAdminString,
       radiusAuthServAccessRequests                    Counter32,
       radiusAuthServDupAccessRequests                 Counter32,
       radiusAuthServAccessAccepts                     Counter32,
       radiusAuthServAccessRejects                     Counter32,
       radiusAuthServAccessChallenges                  Counter32,
       radiusAuthServMalformedAccessRequests           Counter32,
       radiusAuthServBadAuthenticators                 Counter32,
       radiusAuthServPacketsDropped                    Counter32,
       radiusAuthServUnknownTypes                      Counter32
}

radiusAuthClientIndex OBJECT-TYPE
       SYNTAX     Integer32 (1..2147483647)
       MAX-ACCESS not-accessible
       STATUS     current
       DESCRIPTION
             "A number uniquely identifying each RADIUS
              authentication client with which this server
              communicates."
       ::= { radiusAuthClientEntry 1 }

radiusAuthClientAddress OBJECT-TYPE
       SYNTAX     IpAddress
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The NAS-IP-Address of the RADIUS authentication client
              referred to in this table entry."
       ::= { radiusAuthClientEntry 2 }

radiusAuthClientID OBJECT-TYPE
       SYNTAX     SnmpAdminString
       MAX-ACCESS read-only
       STATUS     current
       DESCRIPTION
             "The NAS-Identifier of the RADIUS authentication client
              referred to in this table entry. This is not necessarily
              the same as sysName in MIB II."
       ::= { radiusAuthClientEntry 3 }

-- Server Counters





--
-- Responses = AccessAccepts + AccessRejects + AccessChallenges
--
-- Requests - DupRequests - BadAuthenticators - MalformedRequests -
-- UnknownTypes -  PacketsDropped - Responses = Pending
--
-- Requests - DupRequests - BadAuthenticators - MalformedRequests -
-- UnknownTypes - PacketsDropped = entries logged

radiusAuthServAccessRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of packets received on the authentication
              port from this client."
       ::= { radiusAuthClientEntry  4 }

radiusAuthServDupAccessRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of duplicate RADIUS Access-Request
              packets received from this client."
       ::= { radiusAuthClientEntry  5 }

radiusAuthServAccessAccepts OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Access-Accept packets
              sent to this client."
       ::= { radiusAuthClientEntry  6 }

radiusAuthServAccessRejects OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
             "The number of RADIUS Access-Reject packets
              sent to this client."
       ::= { radiusAuthClientEntry  7 }

radiusAuthServAccessChallenges OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only





       STATUS current
       DESCRIPTION
             "The number of RADIUS Access-Challenge packets
              sent to this client."
       ::= { radiusAuthClientEntry  8 }

radiusAuthServMalformedAccessRequests OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of malformed RADIUS Access-Request
              packets received from this client.
              Bad authenticators and unknown types are not included as
              malformed Access-Requests."
       ::= { radiusAuthClientEntry  9 }

radiusAuthServBadAuthenticators OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS Authentication-Request packets
              which contained invalid Signature attributes received
              from this client."
       ::= { radiusAuthClientEntry  10 }

radiusAuthServPacketsDropped OBJECT-TYPE
      SYNTAX Counter32
      MAX-ACCESS read-only
      STATUS current
      DESCRIPTION
              "The number of incoming packets from this
               client silently discarded for some reason other
               than malformed, bad authenticators or
               unknown types."
       ::= { radiusAuthClientEntry  11 }

radiusAuthServUnknownTypes OBJECT-TYPE
       SYNTAX Counter32
       MAX-ACCESS read-only
       STATUS current
       DESCRIPTION
             "The number of RADIUS packets of unknown type which
              were received from this client."
       ::= { radiusAuthClientEntry  12 }







-- conformance information

radiusAuthServMIBConformance
              OBJECT IDENTIFIER ::= { radiusAuthServMIB 2 }
radiusAuthServMIBCompliances
              OBJECT IDENTIFIER ::= { radiusAuthServMIBConformance 1 }
radiusAuthServMIBGroups
              OBJECT IDENTIFIER ::= { radiusAuthServMIBConformance 2 }


-- compliance statements

radiusAuthServMIBCompliance MODULE-COMPLIANCE
            STATUS  current
            DESCRIPTION
                  "The compliance statement for authentication servers
                   implementing the RADIUS Authentication Server MIB."
            MODULE  -- this module
            MANDATORY-GROUPS { radiusAuthServMIBGroup }

            OBJECT        radiusAuthServConfigReset
            WRITE-SYNTAX  INTEGER { reset(2) }
            DESCRIPTION  "The only SETable value is 'reset' (2)."

            ::= { radiusAuthServMIBCompliances 1 }

-- units of conformance

radiusAuthServMIBGroup OBJECT-GROUP
      OBJECTS {radiusAuthServIdent,
               radiusAuthServUpTime,
               radiusAuthServResetTime,
               radiusAuthServConfigReset,
               radiusAuthServTotalAccessRequests,
               radiusAuthServTotalInvalidRequests,
               radiusAuthServTotalDupAccessRequests,
               radiusAuthServTotalAccessAccepts,
               radiusAuthServTotalAccessRejects,
               radiusAuthServTotalAccessChallenges,
               radiusAuthServTotalMalformedAccessRequests,
               radiusAuthServTotalBadAuthenticators,
               radiusAuthServTotalPacketsDropped,
               radiusAuthServTotalUnknownTypes,
               radiusAuthClientAddress,
               radiusAuthClientID,
               radiusAuthServAccessRequests,
               radiusAuthServDupAccessRequests,
               radiusAuthServAccessAccepts,





               radiusAuthServAccessRejects,
               radiusAuthServAccessChallenges,
               radiusAuthServMalformedAccessRequests,
               radiusAuthServBadAuthenticators,
               radiusAuthServPacketsDropped,
               radiusAuthServUnknownTypes
              }
      STATUS  current
      DESCRIPTION
            "The collection of objects providing management of
             a RADIUS Authentication Server."
      ::= { radiusAuthServMIBGroups 1 }

END


