UUID-TC-MIB DEFINITIONS ::= BEGIN


        IMPORTS
          MODULE-IDENTITY, mib-2
            FROM SNMPv2-SMI             -- RFC 2578
          TEXTUAL-CONVENTION
            FROM SNMPv2-TC              -- RFC 2579
          ;

        uuidTCMIB MODULE-IDENTITY





          LAST-UPDATED "201304050000Z"  -- April 5, 2013
          ORGANIZATION "IETF Energy Management Working Group"
          CONTACT-INFO "WG Email: eman@ietf.org
                        Mailing list subscription info:
                        http://www.ietf.org/mailman/listinfo/eman

                        Dan Romascanu
                        Avaya
                        Park Atidim, Bldg. #3
                        Tel Aviv, 61581
                        Israel
                        Phone: +972-3-6458414
                        Email: dromasca@avaya.com

                        Juergen Quittek
                        NEC Europe Ltd.
                        Network Research Division
                        Kurfuersten-Anlage 36
                        Heidelberg  69115
                        Germany
                        Phone: +49 6221 4342-115
                        Email: quittek@neclab.eu

                        Mouli Chandramouli
                        Cisco Systems, Inc.
                        Sarjapur Outer Ring Road
                        Bangalore 560103
                        India
                        Phone: +91 80 4429 2409
                        Email: moulchan@cisco.com"

          DESCRIPTION
                     "This MIB module defines TEXTUAL-CONVENTIONs
                      representing Universally Unique IDentifiers
                      (UUIDs).

                      Copyright (c) 2013 IETF Trust and the persons
                      identified as authors of the code.  All rights
                      reserved.

                      Redistribution and use in source and binary forms,
                      with or without modification, is permitted
                      pursuant to, and subject to the license terms
                      contained in, the Simplified BSD License set forth
                      in Section 4.c of the IETF Trust's Legal
                      Provisions Relating to IETF Documents
                      (http://trustee.ietf.org/license-info)."






          REVISION     "201304050000Z"  -- April 5, 2013
          DESCRIPTION  "Initial version of this MIB as published in
                        RFC 6933."

          ::= { mib-2 217 }

        -- Textual Conventions

   UUID ::= TEXTUAL-CONVENTION
       DISPLAY-HINT    "4x-2x-2x-1x1x-6x"
       STATUS          current
       DESCRIPTION
            "Universally Unique Identifier information.  The syntax must
             conform to RFC 4122, Section 4.1."

           SYNTAX      OCTET STRING (SIZE (16))

   UUIDorZero ::= TEXTUAL-CONVENTION
       DISPLAY-HINT    "4x-2x-2x-1x1x-6x"
       STATUS          current
       DESCRIPTION
            "Universally Unique Identifier information.  The syntax must
             conform to RFC 4122, Section 4.1.

             The semantics of the value zero-length OCTET STRING are
             object-specific and must therefore be defined as part of
             the description of any object that uses this syntax."

           SYNTAX      OCTET STRING (SIZE (0|16))

   END


