RFC1158-MIB

               DEFINITIONS ::= BEGIN


               IMPORTS
                       mgmt, OBJECT-TYPE, NetworkAddress, IpAddress,
                       Counter, Gauge, TimeTicks
                           FROM RFC1155-SMI;

               mib-2      OBJECT IDENTIFIER ::= { mgmt 1 }    -- MIB-II
                          -- (same prefix as MIB-I)

               system     OBJECT IDENTIFIER ::= { mib-2 1 }
               interfaces OBJECT IDENTIFIER ::= { mib-2 2 }
               at         OBJECT IDENTIFIER ::= { mib-2 3 }





               ip         OBJECT IDENTIFIER ::= { mib-2 4 }
               icmp       OBJECT IDENTIFIER ::= { mib-2 5 }
               tcp        OBJECT IDENTIFIER ::= { mib-2 6 }
               udp        OBJECT IDENTIFIER ::= { mib-2 7 }
               egp        OBJECT IDENTIFIER ::= { mib-2 8 }
               -- cmot    OBJECT IDENTIFIER ::= { mib-2 9 }
               transmission OBJECT IDENTIFIER ::= { mib-2 10 }
               snmp       OBJECT IDENTIFIER ::= { mib-2 11 }


               -- object types

               -- the System group

               sysDescr OBJECT-TYPE
                       SYNTAX  DisplayString (SIZE (0..255))
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { system 1 }

               sysObjectID OBJECT-TYPE
                       SYNTAX  OBJECT IDENTIFIER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { system 2 }

               sysUpTime OBJECT-TYPE
                       SYNTAX  TimeTicks
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { system 3 }

               sysContact OBJECT-TYPE
                       SYNTAX  DisplayString (SIZE (0..255))
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { system 4 }

               sysName OBJECT-TYPE
                       SYNTAX  DisplayString (SIZE (0..255))
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { system 5 }

               sysLocation OBJECT-TYPE
                       SYNTAX  DisplayString (SIZE (0..255))
                       ACCESS  read-only
                       STATUS  mandatory





                       ::= { system 6 }

               sysServices OBJECT-TYPE
                       SYNTAX  INTEGER (0..127)
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { system 7 }


               -- the Interfaces group

               ifNumber OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { interfaces 1 }

               -- the Interfaces table

               ifTable OBJECT-TYPE
                       SYNTAX  SEQUENCE OF IfEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { interfaces 2 }

               ifEntry OBJECT-TYPE
                       SYNTAX  IfEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifTable 1 }

               IfEntry ::= SEQUENCE {
                   ifIndex
                       INTEGER,
                   ifDescr
                       DisplayString,
                   ifType
                       INTEGER,
                   ifMtu
                       INTEGER,
                   ifSpeed
                       Gauge,
                   ifPhysAddress
                       OCTET STRING,
                   ifAdminStatus
                       INTEGER,
                   ifOperStatus
                       INTEGER,





                   ifLastChange
                       TimeTicks,
                   ifInOctets
                       Counter,
                   ifInUcastPkts
                       Counter,
                   ifInNUcastPkts
                       Counter,
                   ifInDiscards
                       Counter,
                   ifInErrors
                       Counter,
                   ifInUnknownProtos
                       Counter,
                   ifOutOctets
                       Counter,
                   ifOutUcastPkts
                       Counter,
                   ifOutNUcastPkts
                       Counter,
                   ifOutDiscards
                       Counter,
                   ifOutErrors
                       Counter,
                   ifOutQLen
                       Gauge,
                   ifSpecific
                       OBJECT IDENTIFIER
               }

               ifIndex OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 1 }

               ifDescr OBJECT-TYPE
                       SYNTAX  DisplayString (SIZE (0..255))
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 2 }

               ifType OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   other(1),             -- none of the
                                                         -- following
                                   regular1822(2),
                                   hdh1822(3),





                                   ddn-x25(4),
                                   rfc877-x25(5),
                                   ethernet-csmacd(6),
                                   iso88023-csmacd(7),
                                   iso88024-tokenBus(8),
                                   iso88025-tokenRing(9),
                                   iso88026-man(10),
                                   starLan(11),
                                   proteon-10Mbit(12),
                                   proteon-80Mbit(13),
                                   hyperchannel(14),
                                   fddi(15),
                                   lapb(16),
                                   sdlc(17),
                                   t1-carrier(18),
                                   cept(19),        -- european
                                                    --equivalent of T-1
                                   basicISDN(20),
                                   primaryISDN(21),
                                                         -- proprietary
                                                         -- serial
                                   propPointToPointSerial(22),
                                   terminalServer-asyncPort(23),
                                   softwareLoopback(24),
                                   eon(25),              -- CLNP over IP
                                   ethernet-3Mbit(26),
                                   nsip(27),             -- XNS over IP
                                   slip(28)              -- generic SLIP
                           }
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 3 }

               ifMtu OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 4 }

               ifSpeed OBJECT-TYPE
                       SYNTAX  Gauge
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 5 }

               ifPhysAddress OBJECT-TYPE
                       SYNTAX  OCTET STRING
                       ACCESS  read-only





                       STATUS  mandatory
                       ::= { ifEntry 6 }

               ifAdminStatus OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   up(1),     -- ready to pass packets
                                   down(2),
                                   testing(3) -- in some test mode
                               }
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ifEntry 7 }

               ifOperStatus OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   up(1),     -- ready to pass packets
                                   down(2),
                                   testing(3) -- in some test mode
                               }
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 8 }

               ifLastChange OBJECT-TYPE
                       SYNTAX  TimeTicks
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 9 }

               ifInOctets OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 10 }

               ifInUcastPkts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { ifEntry 11 }

               ifInNUcastPkts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 12 }

               ifInDiscards OBJECT-TYPE





                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 13 }

               ifInErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 14 }

               ifInUnknownProtos OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 15 }

               ifOutOctets OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 16 }

               ifOutUcastPkts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 17 }

               ifOutNUcastPkts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 18 }

               ifOutDiscards OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 19 }

               ifOutErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 20 }

               ifOutQLen OBJECT-TYPE





                       SYNTAX  Gauge
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 21 }

               ifSpecific OBJECT-TYPE
                       SYNTAX  OBJECT IDENTIFIER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ifEntry 22 }

               nullSpecific OBJECT IDENTIFIER ::= { 0 0 }

               -- the Address Translation group (deprecated)

               atTable OBJECT-TYPE
                       SYNTAX  SEQUENCE OF AtEntry
                       ACCESS  read-write
                       STATUS  deprecated
                       ::= { at 1 }

               atEntry OBJECT-TYPE
                       SYNTAX  AtEntry
                       ACCESS  read-write
                       STATUS  deprecated
                       ::= { atTable 1 }

               AtEntry ::= SEQUENCE {
                   atIfIndex
                       INTEGER,
                   atPhysAddress
                       OCTET STRING,
                   atNetAddress
                       NetworkAddress
               }

               atIfIndex OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  deprecated
                       ::= { atEntry 1 }

               atPhysAddress OBJECT-TYPE
                       SYNTAX  OCTET STRING
                       ACCESS  read-write
                       STATUS  deprecated
                       ::= { atEntry 2 }






               atNetAddress OBJECT-TYPE
                       SYNTAX  NetworkAddress
                       ACCESS  read-write
                       STATUS  deprecated
                       ::= { atEntry 3 }


               -- the IP group

               ipForwarding OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   gateway(1), -- entity forwards
                                               -- datagrams
                                   host(2)     -- entity does NOT
                                               -- forward datagrams
                               }
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ip 1 }

               ipDefaultTTL OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ip 2 }

               ipInReceives OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 3 }

               ipInHdrErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 4 }

               ipInAddrErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 5 }

               ipForwDatagrams OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory





                       ::= { ip 6 }

               ipInUnknownProtos OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 7 }

               ipInDiscards OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 8 }

               ipInDelivers OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 9 }

               ipOutRequests OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 10 }

               ipOutDiscards OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 11 }

               ipOutNoRoutes OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 12 }

               ipReasmTimeout OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 13 }

               ipReasmReqds OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory





                       ::= { ip 14 }

               ipReasmOKs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 15 }

               ipReasmFails OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 16 }

               ipFragOKs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 17 }

               ipFragFails OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 18 }

               ipFragCreates OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 19 }

               -- the IP Interface table

               ipAddrTable OBJECT-TYPE
                       SYNTAX  SEQUENCE OF IpAddrEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ip 20 }

               ipAddrEntry OBJECT-TYPE
                       SYNTAX  IpAddrEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ipAddrTable 1 }

               IpAddrEntry ::= SEQUENCE {
                   ipAdEntAddr





                       IpAddress,
                   ipAdEntIfIndex
                       INTEGER,
                   ipAdEntNetMask
                       IpAddress,
                   ipAdEntBcastAddr
                       INTEGER,
                   ipAdEntReasmMaxSize
                       INTEGER (0..65535)
               }

               ipAdEntAddr OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { ipAddrEntry 1 }

               ipAdEntIfIndex OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { ipAddrEntry 2 }

               ipAdEntNetMask OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { ipAddrEntry 3 }

               ipAdEntBcastAddr OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ipAddrEntry 4 }

               ipAdEntReasmMaxSiz OBJECT-TYPE
                       SYNTAX  INTEGER (0..65535)
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ipAddrEntry 5 }

               -- the IP Routing table

               ipRoutingTable OBJECT-TYPE
                       SYNTAX  SEQUENCE OF IpRouteEntry
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ip 21 }





               ipRouteEntry OBJECT-TYPE
                       SYNTAX  IpRouteEntry
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRoutingTable 1 }

               IpRouteEntry ::= SEQUENCE {
                   ipRouteDest
                       IpAddress,
                   ipRouteIfIndex
                       INTEGER,
                   ipRouteMetric1
                       INTEGER,
                   ipRouteMetric2
                       INTEGER,
                   ipRouteMetric3
                       INTEGER,
                   ipRouteMetric4
                       INTEGER,
                   ipRouteNextHop
                       IpAddress,
                   ipRouteType
                       INTEGER,
                   ipRouteProto
                       INTEGER,
                   ipRouteAge
                       INTEGER,
                   ipRouteMask
                       IpAddress
               }

               ipRouteDest OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 1 }

               ipRouteIfIndex  OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 2 }

               ipRouteMetric1 OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 3 }





               ipRouteMetric2 OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 4 }

               ipRouteMetric3 OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 5 }

               ipRouteMetric4 OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 6 }

               ipRouteNextHop OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 7 }

               ipRouteType OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   other(1),    -- none of the following

                                   invalid(2),  -- an invalidated route

                                                -- route to directly
                                   direct(3),   -- connected
                                                -- (sub-)network

                                                -- route to a non-local
                                   remote(4)    -- host/network/
                                                -- sub-network
                           }
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 8 }

               ipRouteProto OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   other(1),    -- none of the following

                                                -- non-protocol
                                                -- information





                                                --   e.g., manually
                                   local(2),    --   configured entries

                                                -- set via a network
                                   netmgmt(3),  --   management protocol

                                                -- obtained via ICMP,
                                   icmp(4),     --   e.g., Redirect

                                                -- the following are
                                                -- gateway routing
                                                -- protocols
                                   egp(5),
                                   ggp(6),
                                   hello(7),
                                   rip(8),
                                   is-is(9),
                                   es-is(10),
                                   ciscoIgrp(11),
                                   bbnSpfIgp(12),
                                   ospf(13)
                                   bgp(14)
                           }
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { ipRouteEntry 9 }

               ipRouteAge OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 10 }

               ipRouteMask OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipRouteEntry 11 }

               -- the IP Address Translation tables

               ipNetToMediaTable OBJECT-TYPE
                       SYNTAX  SEQUENCE OF IpNetToMediaEntry
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ip 22 }

               ipNetToMediaEntry OBJECT-TYPE





                       SYNTAX  IpNetToMediaEntry
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipNetToMediaTable 1 }

               IpNetToMediaEntry ::= SEQUENCE {
                   ipNetToMediaIfIndex
                       INTEGER,
                   ipNetToMediaPhysAddress
                       OCTET STRING,
                   ipNetToMediaNetAddress
                       IpAddress,
                   ipNetoToMediaType
                       INTEGER
               }

               ipNetToMediaIfIndex OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipNetToMediaEntry 1 }

               ipNetToMediaPhysAddress OBJECT-TYPE
                       SYNTAX  OCTET STRING
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipNetToMediaEntry 2 }

               ipNetToMediaNetAddress OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipNetToMediaEntry 3 }

               ipNetToMediaType OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   other(1),   -- none of the following

                                   invalid(2), -- an invalidated mapping
                                   dynamic(3), -- connected (sub-)network

                                   static(4)
                           }
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { ipNetToMediaEntry 4 }







               -- the ICMP group

               icmpInMsgs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 1 }

               icmpInErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 2 }

               icmpInDestUnreachs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 3 }

               icmpInTimeExcds OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 4 }

               icmpInParmProbs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 5 }

               icmpInSrcQuenchs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 6 }

               icmpInRedirects OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 7 }

               icmpInEchos OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory





                       ::= { icmp 8 }

               icmpInEchoReps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 9 }

               icmpInTimestamps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 10 }

               icmpInTimestampReps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 11 }

               icmpInAddrMasks OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 12 }

               icmpInAddrMaskReps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 13 }

               icmpOutMsgs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 14 }

               icmpOutErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 15 }

               icmpOutDestUnreachs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory





                       ::= { icmp 16 }

               icmpOutTimeExcds OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 17 }

               icmpOutParmProbs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 18 }

               icmpOutSrcQuenchs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 19 }

               icmpOutRedirects OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 20 }

               icmpOutEchos OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 21 }

               icmpOutEchoReps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 22 }

               icmpOutTimestamps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 23 }

               icmpOutTimestampReps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory





                       ::= { icmp 24 }

               icmpOutAddrMasks OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 25 }

               icmpOutAddrMaskReps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { icmp 26 }


               -- the TCP group

               tcpRtoAlgorithm OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   other(1),    -- none of the following
                                   constant(2), -- a constant rto
                                   rsre(3),     -- MIL-STD-1778,
                                                -- Appendix B
                                   vanj(4)      -- Van Jacobson's
                                                -- algorithm
                               }
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 1 }

               tcpRtoMin OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 2 }

               tcpRtoMax OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 3 }

               tcpMaxConn OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 4 }






               tcpActiveOpens OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 5 }

               tcpPassiveOpens OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 6 }

               tcpAttemptFails OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 7 }

               tcpEstabResets OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 8 }

               tcpCurrEstab OBJECT-TYPE
                       SYNTAX  Gauge
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 9 }

               tcpInSegs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 10 }

               tcpOutSegs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 11 }

               tcpRetransSegs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 12 }






               -- the TCP connections table

               tcpConnTable OBJECT-TYPE
                       SYNTAX  SEQUENCE OF TcpConnEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 13 }

               tcpConnEntry OBJECT-TYPE
                       SYNTAX  TcpConnEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcpConnTable 1 }

               TcpConnEntry ::= SEQUENCE {
                   tcpConnState
                       INTEGER,
                   tcpConnLocalAddress
                       IpAddress,
                   tcpConnLocalPort
                       INTEGER (0..65535),
                   tcpConnRemAddress
                       IpAddress,
                   tcpConnRemPort
                       INTEGER (0..65535)
               }

               tcpConnState OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   closed(1),
                                   listen(2),
                                   synSent(3),
                                   synReceived(4),
                                   established(5),
                                   finWait1(6),
                                   finWait2(7),
                                   closeWait(8),
                                   lastAck(9),
                                   closing(10),
                                   timeWait(11)
                               }
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcpConnEntry 1 }

               tcpConnLocalAddress OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-only





                       STATUS  mandatory
                       ::= { tcpConnEntry 2 }

               tcpConnLocalPort OBJECT-TYPE
                       SYNTAX  INTEGER (0..65535)
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcpConnEntry 3 }

               tcpConnRemAddress OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcpConnEntry 4 }

               tcpConnRemPort OBJECT-TYPE
                       SYNTAX  INTEGER (0..65535)
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcpConnEntry 5 }

               -- additional TCP variables

               tcpInErrs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 14 }

               tcpOutRsts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { tcp 15 }


               -- the UDP group

               udpInDatagrams OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { udp 1 }

               udpNoPorts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory





                       ::= { udp 2 }

               udpInErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { udp 3 }

               udpOutDatagrams OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { udp 4 }

               -- the UDP listener table

               udpTable OBJECT-TYPE
                       SYNTAX  SEQUENCE OF UdpEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { udp 5 }

               udpEntry OBJECT-TYPE
                       SYNTAX  UdpEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { udpTable 1 }

               UdpEntry ::= SEQUENCE {
                   udpLocalAddress
                       IpAddress,
                   udpLocalPort
                       INTEGER (0..65535)
               }

               udpLocalAddress OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { udpEntry 1 }

               udpLocalPort OBJECT-TYPE
                       SYNTAX  INTEGER (0..65535)
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { udpEntry 2 }







               -- the EGP group

               egpInMsgs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egp 1 }

               egpInErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egp 2 }

               egpOutMsgs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egp 3 }

               egpOutErrors OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egp 4 }

               -- the EGP Neighbor table

               egpNeighTable OBJECT-TYPE
                       SYNTAX  SEQUENCE OF EgpNeighEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egp 5 }

               egpNeighEntry OBJECT-TYPE
                       SYNTAX  EgpNeighEntry
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighTable 1 }

               EgpNeighEntry ::= SEQUENCE {
                   egpNeighState
                       INTEGER,
                   egpNeighAddr
                       IpAddress,
                   egpNeighAs
                       INTEGER,
                   egpNeighInMsgs





                       Counter,
                   egpNeighInErrs
                       Counter,
                   egpNeighOutMsgs
                       Counter,
                   egpNeighOutErrs
                       Counter,
                   egpNeighInErrMsgs
                       Counter,
                   egpNeighOutErrMsgs
                       Counter,
                   egpNeighStateUps
                       Counter,
                   egpNeighStateDowns
                       Counter,
                   egpNeighIntervalHello
                       INTEGER,
                   egpNeighIntervalPoll
                       INTEGER,
                   egpNeighMode
                       INTEGER,
                   egpNeighEventTrigger
                       INTEGER
               }

               egpNeighState OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   idle(1),
                                   acquisition(2),
                                   down(3),
                                   up(4),
                                   cease(5)
                               }
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 1 }

               egpNeighAddr OBJECT-TYPE
                       SYNTAX  IpAddress
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 2 }

               egpNeighAs OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 3 }





               egpNeighInMsgs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 4 }

               egpNeighInErrs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 5 }

               egpNeighOutMsgs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 6 }

               egpNeighOutErrs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 7 }

               egpNeighInErrMsgs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 8 }

               egpNeighOutErrMsgs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 9 }

               egpNeighStateUps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 10 }

               egpNeighStateDowns OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 11 }






               egpNeighIntervalHello OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 12 }

               egpNeighIntervalPoll OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 13 }

               egpNeighMode OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   active(1),
                                   passive(2)
                               }
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egpNeighEntry 14 }

               egpNeighEventTrigger OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   start(1),
                                   stop(2)
                               }
                       ACCESS  read-write
                       STATUS  mandatory
                       ::= { egpNeighEntry 15 }

               -- additional EGP variables

               egpAs OBJECT-TYPE
                       SYNTAX  INTEGER
                       ACCESS  read-only
                       STATUS  mandatory
                       ::= { egp 6 }


               -- the Transmission group (empty at present)

               -- the SNMP group

               snmpInPkts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 1 }





               snmpOutPkts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 2 }

               snmpInBadVersions OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 3 }

               snmpInBadCommunityNames OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 4 }

               snmpInBadCommunityUses OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 5 }

               snmpInASNParseErrs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 6 }

               snmpInBadTypes OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 7 }

               snmpInTooBigs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 8 }

               snmpInNoSuchNames OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 9 }






               snmpInBadValues OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 10 }

               snmpInReadOnlys OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 11 }

               snmpInGenErrs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 12 }

               snmpInTotalReqVars OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 13 }

               snmpInTotalSetVars OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 14 }

               snmpInGetRequests OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 15 }

               snmpInGetNexts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 16 }

               snmpInSetRequests OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 17 }






               snmpInGetResponses OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 18 }

               snmpInTraps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 19 }

               snmpOutTooBigs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 20 }

               snmpOutNoSuchNames OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 21 }

               snmpOutBadValues OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 22 }

               snmpOutReadOnlys OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 23 }

               snmpOutGenErrs OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 24 }

               snmpOutGetRequests OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 25 }






               snmpOutGetNexts OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 26 }

               snmpOutSetRequests OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 27 }

               snmpOutGetResponses OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 28 }

               snmpOutTraps OBJECT-TYPE
                       SYNTAX  Counter
                       ACCESS  read-only
                       STATUS  mandatory
                       ::=  { snmp 29 }

               snmpEnableAuthTraps OBJECT-TYPE
                       SYNTAX  INTEGER {
                                   enabled(1),
                                   disabled(2)
                               }
                       ACCESS  read-write
                       STATUS  mandatory
                       ::=  { snmp 30 }

               END


